{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Auswahl","Zwischenwerte","Matrix-Material","Klimazonen","Translation","Preisliste","Ausdruck"],"not_rendered":{"charts":4,"images":148,"macros":1,"external_links":1,"defined_names":11,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Auswahl","index":0,"n_rows":474,"n_cols":37,"rows_kept":474,"cut":false,"hidden":false,"merged":[[247,4,247,6],[247,7,247,9],[245,4,245,6],[245,7,245,9],[246,4,246,6],[244,4,244,6],[244,7,244,9],[244,19,244,21],[244,22,244,24],[245,19,245,21],[245,22,245,24],[248,4,248,6],[246,7,246,9],[243,19,243,21],[243,22,243,24],[241,22,241,24],[242,19,242,21],[234,22,234,24],[198,22,198,24],[199,22,199,24],[200,22,200,24],[201,22,201,24],[202,22,202,24],[203,22,203,24],[204,22,204,24],[205,22,205,24],[224,22,224,24],[225,22,225,24],[226,22,226,24],[235,19,235,21],[206,22,206,24],[241,7,241,9],[242,4,242,6],[235,22,235,24],[222,22,222,24],[233,32,233,34],[234,32,234,34],[235,32,235,34],[236,32,236,34],[237,32,237,34],[224,32,224,34],[65,4,65,9],[53,4,53,17],[59,4,59,17],[67,4,67,17],[223,22,223,24],[219,19,219,21],[220,19,220,21],[221,19,221,21],[222,19,222,21],[225,32,225,34],[226,32,226,34],[227,32,227,34],[228,32,228,34],[229,32,229,34],[230,32,230,34],[231,32,231,34],[232,32,232,34],[214,32,214,34],[243,4,243,6],[243,7,243,9],[242,7,242,9],[241,19,241,21],[221,22,221,24],[216,22,216,24],[217,22,217,24],[218,22,218,24],[219,22,219,24],[220,22,220,24],[240,7,240,9],[242,22,242,24],[240,22,240,24],[241,4,241,6],[236,19,236,21],[225,19,225,21],[226,19,226,21],[227,19,227,21],[228,19,228,21],[229,19,229,21],[230,19,230,21],[227,22,227,24],[228,22,228,24],[229,22,229,24],[215,32,215,34],[216,32,216,34],[217,32,217,34],[218,32,218,34],[219,32,219,34],[220,32,220,34],[221,32,221,34],[222,32,222,34],[223,32,223,34],[206,32,206,34],[207,32,207,34],[208,32,208,34],[209,32,209,34],[210,32,210,34],[211,32,211,34],[212,32,212,34],[213,32,213,34],[197,32,197,34],[199,32,199,34],[200,32,200,34],[201,32,201,34],[202,32,202,34],[203,32,203,34],[204,32,204,34],[205,32,205,34],[471,11,471,21],[473,11,473,21],[71,10,71,17],[107,3,107,7],[109,3,109,7],[111,3,111,7],[330,6,330,11],[332,6,332,11],[113,3,113,7],[115,3,115,7],[328,6,328,11],[275,6,275,14],[279,6,279,14],[233,2,233,3],[233,10,233,13],[234,10,234,13],[233,14,233,17],[453,9,453,21],[455,11,455,21],[467,11,467,21],[469,11,469,21],[198,10,198,13],[198,14,198,17],[459,11,459,21],[465,11,465,21],[461,11,461,21],[463,11,463,21],[457,11,457,21],[271,16,271,24],[273,16,273,24],[275,16,275,24],[352,5,352,14],[353,5,353,14],[354,5,354,14],[355,5,355,14],[356,5,356,14],[357,5,357,14],[358,5,358,14],[379,5,379,14],[380,5,380,14],[381,5,381,14],[369,5,369,14],[370,5,370,14],[371,5,371,14],[372,5,372,14],[405,21,405,26],[350,26,350,29],[400,26,400,29],[350,31,350,34],[400,1,400,4],[263,6,263,14],[267,6,267,14],[269,6,269,14],[255,16,255,24],[400,11,400,14],[400,16,400,19],[400,21,400,24],[362,18,362,28],[350,1,350,4],[350,6,350,9],[350,11,350,14],[350,16,350,19],[350,21,350,24],[386,18,386,28],[387,18,387,28],[388,18,388,28],[389,18,389,28],[384,5,384,14],[361,18,361,28],[365,18,365,28],[366,18,366,28],[367,18,367,28],[250,31,250,34],[250,21,250,24],[297,2,297,16],[281,6,281,14],[283,6,283,14],[285,6,285,14],[287,6,287,14],[279,16,279,24],[281,16,281,24],[250,11,250,14],[250,16,250,19],[250,1,250,4],[250,6,250,9],[253,6,253,24],[249,4,249,6],[249,7,249,9],[257,16,257,24],[249,19,249,21],[249,22,249,24],[269,16,269,24],[265,6,265,24],[261,6,261,14],[259,6,259,14],[257,6,257,14],[255,6,255,14],[100,36,100,39],[246,19,246,21],[246,22,246,24],[247,19,247,21],[247,22,247,24],[248,19,248,21],[248,22,248,24],[237,4,237,6],[237,7,237,9],[238,4,238,6],[238,7,238,9],[239,4,239,6],[239,7,239,9],[240,4,240,6],[237,22,237,24],[238,19,238,21],[238,22,238,24],[239,19,239,21],[239,22,239,24],[236,10,236,13],[235,14,235,17],[235,4,235,6],[235,7,235,9],[248,7,248,9],[230,22,230,24],[231,22,231,24],[236,22,236,24],[233,22,233,24],[232,22,232,24],[207,22,207,24],[208,22,208,24],[209,22,209,24],[210,22,210,24],[211,22,211,24],[212,22,212,24],[213,22,213,24],[214,22,214,24],[215,22,215,24],[234,14,234,17],[235,10,235,13],[202,19,202,21],[203,19,203,21],[204,19,204,21],[205,19,205,21],[206,19,206,21],[207,19,207,21],[208,19,208,21],[209,19,209,21],[202,14,202,17],[211,19,211,21],[212,19,212,21],[213,19,213,21],[214,19,214,21],[215,19,215,21],[216,19,216,21],[210,19,210,21],[234,19,234,21],[231,19,231,21],[223,19,223,21],[224,19,224,21],[217,19,217,21],[218,19,218,21],[240,19,240,21],[233,4,233,6],[233,7,233,9],[234,4,234,6],[236,2,236,3],[236,4,236,6],[236,7,236,9],[231,2,231,3],[231,4,231,6],[231,7,231,9],[232,2,232,3],[232,4,232,6],[232,7,232,9],[235,2,235,3],[234,2,234,3],[234,7,234,9],[237,19,237,21],[236,14,236,17],[231,10,231,13],[232,10,232,13],[231,14,231,17],[232,14,232,17],[232,19,232,21],[233,19,233,21],[229,2,229,3],[229,4,229,6],[229,7,229,9],[230,2,230,3],[230,4,230,6],[230,7,230,9],[229,10,229,13],[230,10,230,13],[229,14,229,17],[230,14,230,17],[227,2,227,3],[227,4,227,6],[227,7,227,9],[228,2,228,3],[228,4,228,6],[228,7,228,9],[227,10,227,13],[228,10,228,13],[227,14,227,17],[228,14,228,17],[225,2,225,3],[225,4,225,6],[225,7,225,9],[226,2,226,3],[226,4,226,6],[226,7,226,9],[225,10,225,13],[226,10,226,13],[225,14,225,17],[226,14,226,17],[223,2,223,3],[223,4,223,6],[223,7,223,9],[224,2,224,3],[224,4,224,6],[224,7,224,9],[223,10,223,13],[224,10,224,13],[223,14,223,17],[224,14,224,17],[221,2,221,3],[221,4,221,6],[221,7,221,9],[222,2,222,3],[222,4,222,6],[222,7,222,9],[221,10,221,13],[222,10,222,13],[221,14,221,17],[222,14,222,17],[219,2,219,3],[219,4,219,6],[219,7,219,9],[220,2,220,3],[220,4,220,6],[220,7,220,9],[219,10,219,13],[220,10,220,13],[219,14,219,17],[220,14,220,17],[217,2,217,3],[217,4,217,6],[217,7,217,9],[218,2,218,3],[218,4,218,6],[218,7,218,9],[217,10,217,13],[218,10,218,13],[217,14,217,17],[218,14,218,17],[215,2,215,3],[215,4,215,6],[215,7,215,9],[216,2,216,3],[216,4,216,6],[216,7,216,9],[215,10,215,13],[216,10,216,13],[215,14,215,17],[216,14,216,17],[213,2,213,3],[213,4,213,6],[213,7,213,9],[214,2,214,3],[214,4,214,6],[214,7,214,9],[213,14,213,17],[214,14,214,17],[211,2,211,3],[211,4,211,6],[211,7,211,9],[212,2,212,3],[212,4,212,6],[212,7,212,9],[211,14,211,17],[212,14,212,17],[211,10,211,13],[212,10,212,13],[213,10,213,13],[214,10,214,13],[209,2,209,3],[209,4,209,6],[209,7,209,9],[210,2,210,3],[210,4,210,6],[210,7,210,9],[209,14,209,17],[210,14,210,17],[207,2,207,3],[207,4,207,6],[207,7,207,9],[208,2,208,3],[208,4,208,6],[208,7,208,9],[207,14,207,17],[208,14,208,17],[207,10,207,13],[208,10,208,13],[209,10,209,13],[210,10,210,13],[205,2,205,3],[205,4,205,6],[205,7,205,9],[206,2,206,3],[206,4,206,6],[206,7,206,9],[205,14,205,17],[206,14,206,17],[203,2,203,3],[203,4,203,6],[203,7,203,9],[204,2,204,3],[204,4,204,6],[204,7,204,9],[203,14,203,17],[204,14,204,17],[206,10,206,13],[203,10,203,13],[204,10,204,13],[205,10,205,13],[199,2,199,3],[199,4,199,6],[199,7,199,9],[200,2,200,3],[200,4,200,6],[200,7,200,9],[199,14,199,17],[200,14,200,17],[199,10,199,13],[200,10,200,13],[201,10,201,13],[202,10,202,13],[202,2,202,3],[202,4,202,6],[202,7,202,9],[166,2,166,3],[167,2,167,3],[167,4,167,6],[167,7,167,9],[201,2,201,3],[201,4,201,6],[201,7,201,9],[168,10,168,20],[170,10,170,20],[174,2,174,3],[174,4,174,6],[174,7,174,9],[174,10,174,20],[179,2,179,3],[179,4,179,6],[179,7,179,9],[179,10,179,20],[188,2,188,3],[188,4,188,6],[159,2,159,3],[161,2,161,3],[162,2,162,3],[163,7,163,9],[164,7,164,9],[169,2,169,3],[169,4,169,6],[169,7,169,9],[165,2,165,3],[165,4,165,6],[163,2,163,3],[164,2,164,3],[168,2,168,3],[168,4,168,6],[168,7,168,9],[162,4,162,6],[160,7,160,9],[161,7,161,9],[166,4,166,6],[160,4,160,6],[161,4,161,6],[162,7,162,9],[199,19,199,21],[200,19,200,21],[201,19,201,21],[198,2,198,3],[198,4,198,6],[198,7,198,9],[201,14,201,17],[198,19,198,21],[4,31,4,34],[150,1,150,4],[150,6,150,9],[150,11,150,14],[150,16,150,19],[150,21,150,24],[150,26,150,29],[150,31,150,34],[50,1,50,4],[50,6,50,9],[50,11,50,14],[50,16,50,19],[50,21,50,24],[50,26,50,29],[50,31,50,34],[100,26,100,29],[105,3,105,7],[103,3,103,15],[100,31,100,34],[4,26,4,29],[100,6,100,9],[159,7,159,9],[159,10,159,20],[154,2,154,3],[155,2,155,3],[156,2,156,3],[100,21,100,24],[4,1,4,4],[4,6,4,9],[100,11,100,14],[100,16,100,19],[4,11,4,14],[4,16,4,19],[4,21,4,24],[100,1,100,4],[123,6,123,7],[154,4,154,6],[19,3,19,8],[19,9,19,16],[159,4,159,6],[165,21,165,23],[164,24,164,27],[158,21,158,23],[159,21,159,23],[159,24,159,27],[162,24,162,27],[163,24,163,27],[158,24,158,27],[152,2,152,3],[153,2,153,3],[152,4,152,6],[153,4,153,6],[152,7,152,9],[154,7,154,9],[155,7,155,9],[158,7,158,9],[158,10,158,20],[154,10,154,20],[155,10,155,20],[157,2,157,3],[158,2,158,3],[160,2,160,3],[155,4,155,6],[156,4,156,6],[160,24,160,27],[160,21,160,23],[161,21,161,23],[162,21,162,23],[163,21,163,23],[162,10,162,20],[163,10,163,20],[164,10,164,20],[160,10,160,20],[161,10,161,20],[164,21,164,23],[168,21,168,23],[168,24,168,27],[167,10,167,20],[152,24,152,27],[154,24,154,27],[155,24,155,27],[153,7,153,9],[153,24,153,27],[157,21,157,23],[156,24,156,27],[157,24,157,27],[157,10,157,20],[156,7,156,9],[157,7,157,9],[152,21,152,23],[153,21,153,23],[154,21,154,23],[155,21,155,23],[156,21,156,23],[153,10,153,20],[167,21,167,23],[167,24,167,27],[156,10,156,20],[165,24,165,27],[170,24,170,27],[169,10,169,20],[169,21,169,23],[169,24,169,27],[172,2,172,3],[172,4,172,6],[172,7,172,9],[172,10,172,20],[172,21,172,23],[172,24,172,27],[171,10,171,20],[171,21,171,23],[171,24,171,27],[171,2,171,3],[171,4,171,6],[171,7,171,9],[170,2,170,3],[170,4,170,6],[170,7,170,9],[170,21,170,23],[174,24,174,27],[173,2,173,3],[173,4,173,6],[173,7,173,9],[173,10,173,20],[173,21,173,23],[173,24,173,27],[176,2,176,3],[176,4,176,6],[176,7,176,9],[176,10,176,20],[176,21,176,23],[176,24,176,27],[175,2,175,3],[175,4,175,6],[175,7,175,9],[175,10,175,20],[175,21,175,23],[175,24,175,27],[174,21,174,23],[186,24,186,27],[184,2,184,3],[185,21,185,23],[179,21,179,23],[179,24,179,27],[178,2,178,3],[178,4,178,6],[178,7,178,9],[178,10,178,20],[178,21,178,23],[178,24,178,27],[182,2,182,3],[182,4,182,6],[182,7,182,9],[182,10,182,20],[182,21,182,23],[182,24,182,27],[181,2,181,3],[181,4,181,6],[181,7,181,9],[181,10,181,20],[181,21,181,23],[181,24,181,27],[180,21,180,23],[190,2,190,3],[190,4,190,6],[190,7,190,9],[190,10,190,20],[185,2,185,3],[185,4,185,6],[185,7,185,9],[185,10,185,20],[184,4,184,6],[184,7,184,9],[184,10,184,20],[189,2,189,3],[189,4,189,6],[188,7,188,9],[188,10,188,20],[187,2,187,3],[187,4,187,6],[187,7,187,9],[187,10,187,20],[186,2,186,3],[186,4,186,6],[186,7,186,9],[186,10,186,20],[150,36,150,39],[250,36,250,39],[350,36,350,39],[400,36,400,39],[297,18,297,32],[152,10,152,20],[191,24,191,27],[185,24,185,27],[190,24,190,27],[189,24,189,27],[188,24,188,27],[166,24,166,27],[188,21,188,23],[166,21,166,23],[161,24,161,27],[373,5,373,14],[374,5,374,14],[157,4,157,6],[158,4,158,6],[180,24,180,27],[177,4,177,6],[177,7,177,9],[166,10,166,20],[165,7,165,9],[450,26,450,29],[390,18,390,28],[391,18,391,28],[392,18,392,28],[393,18,393,28],[394,18,394,28],[419,27,419,35],[421,27,421,35],[423,27,423,35],[400,31,400,34],[419,21,419,26],[421,21,421,26],[423,4,423,9],[403,4,403,17],[450,31,450,34],[450,1,450,4],[450,6,450,9],[450,11,450,14],[417,4,417,9],[413,21,414,38],[407,21,407,26],[450,36,450,39],[413,4,413,9],[415,4,415,9],[407,4,407,9],[409,4,409,9],[411,4,411,9],[427,6,427,9],[423,21,423,26],[405,27,405,35],[407,27,407,35],[409,27,409,35],[411,27,411,35],[417,27,417,35],[450,16,450,19],[450,21,450,24],[392,5,392,14],[393,5,393,14],[391,5,391,14],[400,6,400,9],[403,21,403,35],[415,21,415,35],[419,4,419,9],[421,4,421,9],[405,4,405,9],[4,36,4,39],[50,36,50,39],[387,5,387,14],[388,5,388,14],[389,5,389,14],[394,5,394,14],[409,21,409,26],[411,21,411,26],[417,21,417,26],[390,5,390,14],[177,21,177,23],[177,24,177,27],[363,18,363,28],[364,18,364,28],[382,5,382,14],[360,18,360,28],[308,2,308,5],[361,5,361,14],[362,5,362,14],[363,5,363,14],[364,5,364,14],[365,5,365,14],[366,5,366,14],[367,5,367,14],[352,18,352,28],[353,18,353,28],[354,18,354,28],[355,18,355,28],[356,18,356,28],[357,18,357,28],[250,26,250,29],[285,16,285,24],[287,16,287,24],[277,6,277,24],[271,6,271,14],[273,6,273,14],[259,16,259,24],[261,16,261,24],[263,16,263,24],[267,16,267,24],[283,16,283,24],[336,6,336,11],[334,6,334,11],[326,6,326,18],[183,2,183,3],[183,4,183,6],[183,7,183,9],[17,3,17,16],[7,3,7,16],[9,9,9,16],[11,9,11,16],[13,9,13,16],[9,3,9,8],[11,3,11,8],[13,3,13,8],[15,3,15,8],[15,9,15,16],[21,3,21,8],[21,9,21,16],[23,3,23,8],[23,9,23,16],[25,3,25,8],[25,9,25,16],[29,3,29,8],[55,4,55,9],[31,3,31,8],[27,3,27,16],[180,2,180,3],[180,4,180,6],[180,7,180,9],[180,10,180,20],[177,2,177,3],[163,4,163,6],[164,4,164,6],[166,7,166,9],[165,10,165,20],[177,10,177,20],[380,18,380,28],[381,18,381,28],[382,18,382,28],[383,18,383,28],[190,21,190,23],[189,7,189,9],[189,10,189,20],[189,21,189,23],[183,21,183,23],[183,24,183,27],[359,5,359,14],[360,5,360,14],[377,5,377,14],[378,5,378,14],[375,5,375,14],[376,5,376,14],[368,5,368,14],[377,18,377,28],[183,10,183,20],[184,21,184,23],[184,24,184,27],[187,21,187,23],[187,24,187,27],[186,21,186,23],[1,41,1,44],[386,5,386,14],[368,18,368,28],[370,18,370,28],[371,18,371,28],[372,18,372,28],[373,18,373,28],[374,18,374,28],[375,18,375,28],[376,18,376,28],[383,5,383,14],[57,4,57,9],[61,4,61,9],[63,4,63,9],[69,4,69,9],[71,4,71,9],[358,18,358,28],[359,18,359,28],[385,5,385,14],[369,18,369,28],[378,18,378,28],[379,18,379,28],[384,18,384,28],[385,18,385,28]]}
[]
[null,{"$f":"Translation!A4&\" \"&Translation!A5","v":"Engineering tool Solar system"}]
[null,"v2.36"]
[]
[null,{"$f":"Translation!A9","v":"Project data"},null,null,null,null,{"$f":"Translation!A42","v":"System selection"},null,null,null,null,{"$f":"Translation!A65","v":"Collector details"},null,null,null,null,{"$f":"Translation!A95","v":"Material composition"},null,null,null,null,{"$f":"Translation!A135","v":"Solar yield"},null,null,null,null,{"$f":"Translation!A175","v":"Hydraulical scetch"},null,null,null,null,{"$f":"Translation!A273","v":"Expansion vessel"},null,null,null,null,{"$f":"Translation!A298","v":"Printout"}]
[]
[]
[null,null,null,{"$f":"Translation!$A$10","v":"Project"}]
[]
[null,null,null,{"$f":"Translation!$A$11","v":"Name"},null,null,null,null,null,"Beispielprojekt"]
[null,null,null,null,null,null,null,null,null," "]
[null,null,null,{"$f":"Translation!$A$12","v":"Street"}]
[]
[null,null,null,{"$f":"Translation!$A$13","v":"Postcode/Town"}]
[]
[null,null,null,{"$f":"Translation!$A$14","v":"Phone"}]
[]
[null,null,null,{"$f":"Translation!$A$15","v":"Customer"}]
[]
[null,null,null,{"$f":"Translation!$A$11","v":"Name"},null,null,null,null,null,"Stiebel Eltron GmbH & Co. KG"]
[]
[null,null,null,{"$f":"Translation!$A$12","v":"Street"},null,null,null,null,null,"Dr.-Stiebel-Straße"]
[]
[null,null,null,{"$f":"Translation!$A$13","v":"Postcode/Town"},null,null,null,null,null,"37603 Holzminden"]
[]
[null,null,null,{"$f":"Translation!$A$14","v":"Phone"},null,null,null,null,null,"05531 / 702 110"]
[]
[null,null,null,{"$f":"Translation!A16","v":"Climate zone"}]
[]
[null,null,null,{"$f":"Translation!A17","v":"Country selection"}]
[]
[null,null,null,{"$f":"Translation!A18","v":"City/region selection"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"$B$5","v":"Project data"},null,null,null,null,{"$f":"$G$5","v":"System selection"},null,null,null,null,{"$f":"$L$5","v":"Collector details"},null,null,null,null,{"$f":"$Q$5","v":"Material composition"},null,null,null,null,{"$f":"$V$5","v":"Solar yield"},null,null,null,null,{"$f":"$AA$5","v":"Hydraulical scetch"},null,null,null,null,{"$f":"$AF$5","v":"Expansion vessel"},null,null,null,null,{"$f":"$AK$5","v":"Printout"}]
[]
[]
[null,null,null,null,{"$f":"Translation!A43","v":"Solar DHW heating"}]
[]
[null,null,null,null,{"$f":"Translation!$A$44","v":"Number of occupants"},null,null,null,null,null,{"$f":"Zwischenwerte!C14","v":true}]
[]
[null,null,null,null,{"$f":"Translation!$A$45","v":"DHW demand"}]
[]
[null,null,null,null,{"$f":"Translation!A51","v":"Solar central heating backup"}]
[]
[null,null,null,null,{"$f":"Translation!$A$52","v":"Heat demand building"},null,null,null,null,null,{"$f":"Zwischenwerte!D14","v":false}]
[]
[null,null,null,null,{"$f":"Translation!A170","v":"Standard outside temperature"}]
[]
[null,null,null,null,{"$f":"Translation!$A$53","v":"Cylinder type"}]
[]
[null,null,null,null,{"$f":"Translation!A57","v":"Solar swimming pool heating"}]
[]
[null,null,null,null,{"$f":"Translation!$A$58","v":"Swimming pool type"}]
[]
[null,null,null,null,{"$f":"Translation!$A$63","v":"Volume in m³"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"$B$5","v":"Project data"},null,null,null,null,{"$f":"$G$5","v":"System selection"},null,null,null,null,{"$f":"$L$5","v":"Collector details"},null,null,null,null,{"$f":"$Q$5","v":"Material composition"},null,null,null,null,{"$f":"$V$5","v":"Solar yield"},null,null,null,null,{"$f":"$AA$5","v":"Hydraulical scetch"},null,null,null,null,{"$f":"$AF$5","v":"Expansion vessel"},null,null,null,null,{"$f":"$AK$5","v":"Printout"}]
[]
[]
[null,null,null,{"$f":"Translation!A65","v":"Collector details"}]
[]
[null,null,null,{"$f":"Translation!A66","v":"Collector type"},null,null,null,null,null,null,null,null,null,null,null,null," [i]"]
[]
[null,null,null,{"$f":"Translation!A69","v":"Collector number"}]
[]
[null,null,null,{"$f":"Translation!A71","v":"Collector inclination"}]
[]
[null,null,null,{"$f":"Translation!A72","v":"Collector orientation"}]
[]
[null,null,null,{"$f":"IF(Zwischenwerte!L14<4,Translation!A83,\"\")","v":"Shape of roof"}]
[]
[null,null,null,{"$f":"IF(Zwischenwerte!L14<4,Translation!A86,\"\")","v":"Fixing type"}]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A93","v":"Click at desired collector arrangement"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>",{"$f":"Zwischenwerte!M14","v":"On end next to each other"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"$B$5","v":"Project data"},null,null,null,null,{"$f":"$G$5","v":"System selection"},null,null,null,null,{"$f":"$L$5","v":"Collector details"},null,null,null,null,{"$f":"$Q$5","v":"Material composition"},null,null,null,null,{"$f":"$V$5","v":"Solar yield"},null,null,null,null,{"$f":"$AA$5","v":"Hydraulical scetch"},null,null,null,null,{"$f":"$AF$5","v":"Expansion vessel"},null,null,null,null,{"$f":"$AK$5","v":"Printout"}]
[]
[null,null,{"$f":"Translation!A96","v":"Position"},null,{"$f":"Translation!A97","v":"Number"},null,null,{"$f":"Translation!A98","v":"ID"},null,null,{"$f":"Translation!A99","v":"Description"},null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A100","v":"Price each"},null,null,{"$f":"Translation!A101","v":"Total price"}]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H154),TRUE,FALSE)","v":false},1,null,2,null,null,230016,null,null,{"$f":"IF(H154=\"\",\"\",IF(VLOOKUP(H154,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H154,Preisliste!$B:$C,2,FALSE)))","v":"Solar flat-plate collector SOL 27 premium S"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H154=\"\",\"\",IF(VLOOKUP(H154,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H154,Preisliste!$B:$D,3,FALSE)))","v":809},null,null,{"$f":"IF(ISERROR(E154*V154),\"\",E154*V154)","v":1618},null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H155),TRUE,FALSE)","v":false},2,null,1,null,null,230170,null,null,{"$f":"IF(H155=\"\",\"\",IF(VLOOKUP(H155,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H155,Preisliste!$B:$C,2,FALSE)))","v":"Mounting frame SOL R2"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H155=\"\",\"\",IF(VLOOKUP(H155,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H155,Preisliste!$B:$D,3,FALSE)))","v":160},null,null,{"$f":"IF(ISERROR(E155*V155),\"\",E155*V155)","v":160},null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H156),TRUE,FALSE)","v":false},3,null,2,null,null,230175,null,null,{"$f":"IF(H156=\"\",\"\",IF(VLOOKUP(H156,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H156,Preisliste!$B:$C,2,FALSE)))","v":"Fixing Kit - tiled roof SOL BP"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H156=\"\",\"\",IF(VLOOKUP(H156,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H156,Preisliste!$B:$D,3,FALSE)))","v":80},null,null,160,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H157),TRUE,FALSE)","v":false},4,null,1,null,null,230185,null,null,{"$f":"IF(H157=\"\",\"\",IF(VLOOKUP(H157,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H157,Preisliste!$B:$C,2,FALSE)))","v":"Push-fit connection SOL SV-A"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H157=\"\",\"\",IF(VLOOKUP(H157,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H157,Preisliste!$B:$D,3,FALSE)))","v":49},null,null,49,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H158),TRUE,FALSE)","v":false},5,null,1,null,null,230186,null,null,{"$f":"IF(H158=\"\",\"\",IF(VLOOKUP(H158,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H158,Preisliste!$B:$C,2,FALSE)))","v":"Push-fit connection SOL SV-D"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H158=\"\",\"\",IF(VLOOKUP(H158,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H158,Preisliste!$B:$D,3,FALSE)))","v":299},null,null,299,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H159),TRUE,FALSE)","v":false},6,null,1,null,null,232945,null,null,{"$f":"IF(H159=\"\",\"\",IF(VLOOKUP(H159,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H159,Preisliste!$B:$C,2,FALSE)))","v":"Flexible solar pipe SFR 15, DN 20 15m"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H159=\"\",\"\",IF(VLOOKUP(H159,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H159,Preisliste!$B:$D,3,FALSE)))","v":585},null,null,585,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H160),TRUE,FALSE)","v":false},7,null,1,null,null,234784,null,null,{"$f":"IF(H160=\"\",\"\",IF(VLOOKUP(H160,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H160,Preisliste!$B:$C,2,FALSE)))","v":"Solar compact installation SOKI 7 E trend"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H160=\"\",\"\",IF(VLOOKUP(H160,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H160,Preisliste!$B:$D,3,FALSE)))","v":540},null,null,540,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H161),TRUE,FALSE)","v":false},8,null,1,null,null,187873,null,null,{"$f":"IF(H161=\"\",\"\",IF(VLOOKUP(H161,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H161,Preisliste!$B:$C,2,FALSE)))","v":"Warm water cylinder SBB 300 plus"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H161=\"\",\"\",IF(VLOOKUP(H161,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H161,Preisliste!$B:$D,3,FALSE)))","v":1692},null,null,1692,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H162),TRUE,FALSE)","v":false},9,null,1,null,null,73222,null,null,{"$f":"IF(H162=\"\",\"\",IF(VLOOKUP(H162,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H162,Preisliste!$B:$C,2,FALSE)))","v":"Heat transfer liquid H30-L, 20 l"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H162=\"\",\"\",IF(VLOOKUP(H162,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H162,Preisliste!$B:$D,3,FALSE)))","v":79},null,null,79,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H163),TRUE,FALSE)","v":false},10,null,1,null,null,74031,null,null,{"$f":"IF(H163=\"\",\"\",IF(VLOOKUP(H163,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H163,Preisliste!$B:$C,2,FALSE)))","v":"Solar expansion vessel 25 l"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H163=\"\",\"\",IF(VLOOKUP(H163,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H163,Preisliste!$B:$D,3,FALSE)))","v":80},null,null,80,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H164),TRUE,FALSE)","v":false},11,null,1,null,null,231905,null,null,{"$f":"IF(H164=\"\",\"\",IF(VLOOKUP(H164,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H164,Preisliste!$B:$C,2,FALSE)))","v":"DEV connection set AGWH"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H164=\"\",\"\",IF(VLOOKUP(H164,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H164,Preisliste!$B:$D,3,FALSE)))","v":46},null,null,46,null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H165),TRUE,FALSE)","v":false},12,null,null,null,null,null,null,null,{"$f":"IF(H165=\"\",\"\",IF(VLOOKUP(H165,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H165,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H165=\"\",\"\",IF(VLOOKUP(H165,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H165,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,{"$f":"IF(ISERROR(E165*V165),\"\",E165*V165)","v":""},null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H166),TRUE,FALSE)","v":false},13,null,null,null,null,null,null,null,{"$f":"IF(H166=\"\",\"\",IF(VLOOKUP(H166,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H166,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H166=\"\",\"\",IF(VLOOKUP(H166,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H166,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H167),TRUE,FALSE)","v":false},14,null,null,null,null,null,null,null,{"$f":"IF(H167=\"\",\"\",IF(VLOOKUP(H167,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H167,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H167=\"\",\"\",IF(VLOOKUP(H167,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H167,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H168),TRUE,FALSE)","v":false},15,null,null,null,null,null,null,null,{"$f":"IF(H168=\"\",\"\",IF(VLOOKUP(H168,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H168,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H168=\"\",\"\",IF(VLOOKUP(H168,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H168,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H169),TRUE,FALSE)","v":false},16,null,null,null,null,null,null,null,{"$f":"IF(H169=\"\",\"\",IF(VLOOKUP(H169,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H169,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H169=\"\",\"\",IF(VLOOKUP(H169,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H169,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H170),TRUE,FALSE)","v":false},17,null,null,null,null,null,null,null,{"$f":"IF(H170=\"\",\"\",IF(VLOOKUP(H170,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H170,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H170=\"\",\"\",IF(VLOOKUP(H170,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H170,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H171),TRUE,FALSE)","v":false},18,null,null,null,null,null,null,null,{"$f":"IF(H171=\"\",\"\",IF(VLOOKUP(H171,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H171,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H171=\"\",\"\",IF(VLOOKUP(H171,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H171,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H172),TRUE,FALSE)","v":false},19,null,null,null,null,null,null,null,{"$f":"IF(H172=\"\",\"\",IF(VLOOKUP(H172,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H172,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H172=\"\",\"\",IF(VLOOKUP(H172,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H172,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H173),TRUE,FALSE)","v":false},20,null,null,null,null,null,null,null,{"$f":"IF(H173=\"\",\"\",IF(VLOOKUP(H173,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H173,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H173=\"\",\"\",IF(VLOOKUP(H173,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H173,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H174),TRUE,FALSE)","v":false},21,null,null,null,null,null,null,null,{"$f":"IF(H174=\"\",\"\",IF(VLOOKUP(H174,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H174,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H174=\"\",\"\",IF(VLOOKUP(H174,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H174,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H175),TRUE,FALSE)","v":false},22,null,null,null,null,null,null,null,{"$f":"IF(H175=\"\",\"\",IF(VLOOKUP(H175,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H175,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H175=\"\",\"\",IF(VLOOKUP(H175,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H175,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H176),TRUE,FALSE)","v":false},23,null,null,null,null,null,null,null,{"$f":"IF(H176=\"\",\"\",IF(VLOOKUP(H176,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H176,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H176=\"\",\"\",IF(VLOOKUP(H176,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H176,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H177),TRUE,FALSE)","v":false},24,null,null,null,null,null,null,null,{"$f":"IF(H177=\"\",\"\",IF(VLOOKUP(H177,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H177,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H177=\"\",\"\",IF(VLOOKUP(H177,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H177,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H178),TRUE,FALSE)","v":false},25,null,null,null,null,null,null,null,{"$f":"IF(H178=\"\",\"\",IF(VLOOKUP(H178,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H178,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H178=\"\",\"\",IF(VLOOKUP(H178,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H178,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H179),TRUE,FALSE)","v":false},26,null,null,null,null,null,null,null,{"$f":"IF(H179=\"\",\"\",IF(VLOOKUP(H179,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H179,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H179=\"\",\"\",IF(VLOOKUP(H179,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H179,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H180),TRUE,FALSE)","v":false},27,null,null,null,null,null,null,null,{"$f":"IF(H180=\"\",\"\",IF(VLOOKUP(H180,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H180,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H180=\"\",\"\",IF(VLOOKUP(H180,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H180,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H181),TRUE,FALSE)","v":false},28,null,null,null,null,null,null,null,{"$f":"IF(H181=\"\",\"\",IF(VLOOKUP(H181,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H181,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H181=\"\",\"\",IF(VLOOKUP(H181,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H181,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H182),TRUE,FALSE)","v":false},29,null,null,null,null,null,null,null,{"$f":"IF(H182=\"\",\"\",IF(VLOOKUP(H182,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H182,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H182=\"\",\"\",IF(VLOOKUP(H182,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H182,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H183),TRUE,FALSE)","v":false},30,null,null,null,null,null,null,null,{"$f":"IF(H183=\"\",\"\",IF(VLOOKUP(H183,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H183,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H183=\"\",\"\",IF(VLOOKUP(H183,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H183,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H184),TRUE,FALSE)","v":false},31,null,null,null,null,null,null,null,{"$f":"IF(H184=\"\",\"\",IF(VLOOKUP(H184,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H184,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H184=\"\",\"\",IF(VLOOKUP(H184,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H184,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H185),TRUE,FALSE)","v":false},32,null,null,null,null,null,null,null,{"$f":"IF(H185=\"\",\"\",IF(VLOOKUP(H185,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H185,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H185=\"\",\"\",IF(VLOOKUP(H185,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H185,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H186),TRUE,FALSE)","v":false},33,null,null,null,null,null,null,null,{"$f":"IF(H186=\"\",\"\",IF(VLOOKUP(H186,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H186,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H186=\"\",\"\",IF(VLOOKUP(H186,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H186,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H187),TRUE,FALSE)","v":false},34,null,null,null,null,null,null,null,{"$f":"IF(H187=\"\",\"\",IF(VLOOKUP(H187,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H187,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H187=\"\",\"\",IF(VLOOKUP(H187,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H187,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H188),TRUE,FALSE)","v":false},35,null,null,null,null,null,null,null,{"$f":"IF(H188=\"\",\"\",IF(VLOOKUP(H188,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H188,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H188=\"\",\"\",IF(VLOOKUP(H188,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H188,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H189),TRUE,FALSE)","v":false},36,null,null,null,null,null,null,null,{"$f":"IF(H189=\"\",\"\",IF(VLOOKUP(H189,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H189,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H189=\"\",\"\",IF(VLOOKUP(H189,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H189,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H190),TRUE,FALSE)","v":false},37,null,null,null,null,null,null,null,{"$f":"IF(H190=\"\",\"\",IF(VLOOKUP(H190,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H190,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H190=\"\",\"\",IF(VLOOKUP(H190,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H190,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,{"$f":"IF(AND(Zwischenwerte!$G$225=FALSE,Zwischenwerte!$D$225=H191),TRUE,FALSE)","v":false},38,null,null,null,null,null,null,null,{"$f":"IF(H191=\"\",\"\",IF(VLOOKUP(H191,Preisliste!$B:$C,2,FALSE)=\"\",\"No Description entered. Please edit pricelist.\",VLOOKUP(H191,Preisliste!$B:$C,2,FALSE)))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H191=\"\",\"\",IF(VLOOKUP(H191,Preisliste!$B:$D,3,FALSE)=\"--- \",\"No price entered\",VLOOKUP(H191,Preisliste!$B:$D,3,FALSE)))","v":""},null,null,"",null,null,null,"x"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A102","v":"Recommended retail price excl. VAT"},{"$f":"SUM(Y154:AB191)","v":5308}]
[]
[]
[]
[]
[]
[null,null,"Zwischenwerte Standard (unbearbeitete Liste aus Matrix)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Manuell hinzugefügte Positionen (über Preisliste)",null,null,null,null,null,null,null,null,null,null,null,null,"Geändert ?"]
[null,null,"Position",null,"Anzahl",null,null,"Ident.-Nr.",null,null,"Anzahl (Original)",null,null,null,"Ident.-Nr.(Original)"]
[null,null,1,null,2,null,null,230016,null,null,2,null,null,null,230016,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(E200=K200,H200=O200),FALSE,TRUE)","v":false}]
[null,null,2,null,1,null,null,230170,null,null,1,null,null,null,230170,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(E201=K201,H201=O201),FALSE,TRUE)","v":false}]
[null,null,3,null,2,null,null,230175,null,null,2,null,null,null,230175,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,4,null,1,null,null,230185,null,null,1,null,null,null,230185,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,5,null,1,null,null,230186,null,null,1,null,null,null,230186,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,6,null,1,null,null,232945,null,null,1,null,null,null,232945,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,7,null,1,null,null,234784,null,null,1,null,null,null,234784,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,8,null,1,null,null,187873,null,null,1,null,null,null,187873,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,9,null,1,null,null,73222,null,null,1,null,null,null,73222,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,10,null,1,null,null,74031,null,null,1,null,null,null,74031,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,11,null,1,null,null,231905,null,null,1,null,null,null,231905,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,26,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,29,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,38,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(COUNTIF(AG200:AI237,TRUE)>0,TRUE,IF(T200<>\"\",TRUE,FALSE))","v":false}]
[]
[]
[]
[null,"formatierung"]
[null,"so lassen !!"]
[null,"sonst vba-fehler"]
[]
[]
[]
[]
[]
[]
[null,{"$f":"$B$5","v":"Project data"},null,null,null,null,{"$f":"$G$5","v":"System selection"},null,null,null,null,{"$f":"$L$5","v":"Collector details"},null,null,null,null,{"$f":"$Q$5","v":"Material composition"},null,null,null,null,{"$f":"$V$5","v":"Solar yield"},null,null,null,null,{"$f":"$AA$5","v":"Hydraulical scetch"},null,null,null,null,{"$f":"$AF$5","v":"Expansion vessel"},null,null,null,null,{"$f":"$AK$5","v":"Printout"}]
[]
[]
[null,null,null,null,null,null,{"$f":"Translation!A43","v":"Solar DHW heating"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A45","v":"DHW demand"},null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!F14&\" \"&Translation!A136&\" x \"&Zwischenwerte!B100&\" \"&Translation!A137","v":"4 Occupants x 40 l/day"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A138","v":"Recommended cylinder"},null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!E225","v":"SBB 300 Plus"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A139","v":"Heat demand"},null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!F6=6,FIXED(Zwischenwerte!B112*365,0)&\" kWh/r\",FIXED(Zwischenwerte!B112*365,0)&\" kWh/a\")","v":"2.853 kWh/a"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A135","v":"Solar yield"},null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$6=6,FIXED(Zwischenwerte!E319,0)&\" kWh/r\",FIXED(Zwischenwerte!E319,0)&\" kWh/a\")","v":"2.013 kWh/a"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A140","v":"Solar coverage DHW heating"},null,null,null,null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!D319*100,1)&\" %\"","v":"70,6 %"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A51","v":"Solar central heating backup"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A52","v":"Heat demand building"},null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!H14","v":""}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A141","v":"Annual heat demand"},null,null,null,null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!K319,0)&IF(Zwischenwerte!$F$6=6,\" kWh/r\",\" kWh/a\")","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A142","v":"Heating water buffer cylinder"},null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!I14=Zwischenwerte!I17,Zwischenwerte!B123,Zwischenwerte!E225)","v":"SBB 300 Plus"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A143","v":"Solar yield heating backup"},null,null,null,null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!M319,0)&IF(Zwischenwerte!$F$6=6,\" kWh/r\",\" kWh/a\")","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A144","v":"Coverage DHW | Heating backup"},null,null,null,null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!N319*100,1)&\" %\"","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A57","v":"Solar swimming pool heating"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A145","v":"Swimming pool type | Volume"},null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!J14&\"  |  \"&Zwischenwerte!K14&\" m³\"","v":"  |  0 m³"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A146","v":"Duration of use | Cooling"},null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B118&IF(Zwischenwerte!$F$6=6,\" d/r\",\" d/a\")&\"  |  \"&Zwischenwerte!B120&\" K/d\"","v":{"$error":"#N/A"}}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A147","v":"Heat demand for reheating"},null,null,null,null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!B121,1)&\" kWh/d\"","v":{"$error":"#N/A"}}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A148","v":"Solar yield swimming pool"},null,null,null,null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!G319,0)&IF(Zwischenwerte!$F$6=6,\" kWh/r\",\" kWh/a\")","v":{"$error":"#N/A"}}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A149","v":"Coverage heat loss swimming pool"},null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!D25=3,MIN(100,(FIXED(Zwischenwerte!H319*100,1))),MIN(100,(FIXED(Zwischenwerte!F319*100,1))))&\" %\"","v":{"$error":"#N/A"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"Translation!A135&\" \"&Translation!A164&\" [kWh/d]\"","v":"Solar yield DHW heating [kWh/d]"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A165&\" \"&Translation!A164&\" [%]\"","v":"Solar coverage DHW heating [%]"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,{"$f":"Translation!A166","v":"Extended settings"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A167","v":"Cold water temperature"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A168","v":"Cylinder temperature"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A169","v":"System losses DHW"}]
[]
[null,null,null,null,null,null,{"$f":"Translation!A171","v":"Heating limit temperature"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"$B$5","v":"Project data"},null,null,null,null,{"$f":"$G$5","v":"System selection"},null,null,null,null,{"$f":"$L$5","v":"Collector details"},null,null,null,null,{"$f":"$Q$5","v":"Material composition"},null,null,null,null,{"$f":"$V$5","v":"Solar yield"},null,null,null,null,{"$f":"$AA$5","v":"Hydraulical scetch"},null,null,null,null,{"$f":"$AF$5","v":"Expansion vessel"},null,null,null,null,{"$f":"$AK$5","v":"Printout"}]
[]
[null,null,null,null,1,{"$f":"Translation!A187","v":"Heat pump"},null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"Translation!A230","v":"Fill & drain valve"}]
[null,null,null,null,"1-1",{"$f":"Translation!A188","v":"Exhaust air module: LWM 250"},null,null,null,null,null,null,null,null,null,null,null,11,{"$f":"Translation!A231","v":"Oil fired boiler / Gas fired boiler"}]
[null,null,null,null,"1-2",{"$f":"Translation!A189","v":"Cooling module: WPAC"},null,null,null,null,null,null,null,null,null,null,null,12,{"$f":"Translation!A232","v":"Electric central heating"}]
[null,null,null,null,2,{"$f":"Translation!A190","v":"Control unit: WPMW"},null,null,null,null,null,null,null,null,null,null,null,13,{"$f":"Translation!A233","v":"Mixing valve"}]
[null,null,null,null,"2-1",{"$f":"Translation!A191","v":"Swimming pool module: MSMW"},null,null,null,null,null,null,null,null,null,null,null,14,{"$f":"Translation!A234","v":"Mixing valve actuator"}]
[null,null,null,null,"2-2",{"$f":"Translation!A192","v":"Remote control: FE 7"},null,null,null,null,null,null,null,null,null,null,null,15,{"$f":"Translation!A235","v":"Heating control unit"}]
[null,null,null,null,"2-3",{"$f":"Translation!A193","v":"Remote control cooling: FEK"},null,null,null,null,null,null,null,null,null,null,null,16,{"$f":"Translation!A236","v":"Remote set value selector"}]
[null,null,null,null,"2 a",{"$f":"Translation!A194","v":"Temperature sensor: Outside temperature"},null,null,null,null,null,null,null,null,null,null,null,17,{"$f":"Translation!A237","v":"Temperature sensor: Outside temperature"}]
[null,null,null,null,"2 b",{"$f":"Translation!A195","v":"Temperature sensor: Return temperature"},null,null,null,null,null,null,null,null,null,null,null,18,{"$f":"Translation!A238","v":"Temperature sensor: Flow temperature"}]
[null,null,null,null,"2 c",{"$f":"Translation!A196","v":"Temperature sensor: Flow temperature, DHW \"off\""},null,null,null,null,null,null,null,null,null,null,null,19,{"$f":"Translation!A239","v":"Air vent valve"}]
[null,null,null,null,"2 d",{"$f":"Translation!A197","v":"Temperature sensor: Flow temperature, DHW \"on\""},null,null,null,null,null,null,null,null,null,null,null,20,{"$f":"Translation!A240","v":"Solid fuel boiler"}]
[null,null,null,null,"2 e",{"$f":"Translation!A198","v":"Temperature sensor: Mixer control"},null,null,null,null,null,null,null,null,null,null,null,21,{"$f":"Translation!A241","v":"Motorised valve / Solenoid valve"}]
[null,null,null,null,"2 f",{"$f":"Translation!A199","v":"Temperature sensor: Heat source 2"},null,null,null,null,null,null,null,null,null,null,null,22,{"$f":"Translation!A242","v":"Diverter valve"}]
[null,null,null,null,"2 g",{"$f":"Translation!A200","v":"Temperature sensor: Heat source "},null,null,null,null,null,null,null,null,null,null,null,23,{"$f":"Translation!A243","v":"Threaded immersion heater"}]
[null,null,null,null,"2 h",{"$f":"Translation!A201","v":"Temperature sensor: Swimming pool water heating"},null,null,null,null,null,null,null,null,null,null,null,24,{"$f":"Translation!A244","v":"Heat exchanger"}]
[null,null,null,null,"2 k",{"$f":"Translation!A202","v":"Temperature sensor: solar panel"},null,null,null,null,null,null,null,null,null,null,null,25,{"$f":"Translation!A245","v":"Combi cylinder"}]
[null,null,null,null,"2 ko",{"$f":"Translation!A203","v":"Temperature sensor: solar panel East"},null,null,null,null,null,null,null,null,null,null,null,26,{"$f":"Translation!A246","v":"DHW cylinder"}]
[null,null,null,null,"2 kw",{"$f":"Translation!A204","v":"Temperature sensor: solar panel West"},null,null,null,null,null,null,null,null,null,null,null,27,{"$f":"Translation!A247","v":"Central control thermostat"}]
[null,null,null,null,"2 l",{"$f":"Translation!A205","v":"Temperature sensor 1:  return flow temperature increase"},null,null,null,null,null,null,null,null,null,null,null,28,{"$f":"Translation!A248","v":"Cold water - safety equipment assembly"}]
[null,null,null,null,"2 m",{"$f":"Translation!A206","v":"Temperature sensor 2:  return flow temperature increase"},null,null,null,null,null,null,null,null,null,null,null,29,{"$f":"Translation!A249","v":"Controller: Swimming pool water"}]
[null,null,null,null,"2 p",{"$f":"Translation!A207","v":"Temperature sensor: solar buffer cylinder"},null,null,null,null,null,null,null,null,null,null,null,30,{"$f":"Translation!A250","v":"Control thermostat"}]
[null,null,null,null,"2 r",{"$f":"Translation!A208","v":"Temperature sensor: additional solar buffer cylinder"},null,null,null,null,null,null,null,null,null,null,null,31,{"$f":"Translation!A251","v":"Overflow valve"}]
[null,null,null,null,"2 s",{"$f":"Translation!A209","v":"Temperature sensor: solar system hot water/ cooling"},null,null,null,null,null,null,null,null,null,null,null,32,{"$f":"Translation!A252","v":"cap valve"}]
[null,null,null,null,3,{"$f":"Translation!A210","v":"Circulation pump: Heat pump - heat source"},null,null,null,null,null,null,null,null,null,null,null,33,{"$f":"Translation!A253","v":"Line regulating valve"}]
[null,null,null,null,"3 a",{"$f":"Translation!A211","v":"Circulation pump: Heat pump - heating side"},null,null,null,null,null,null,null,null,null,null,null,34,{"$f":"Translation!A254","v":"Temperature differential controller"}]
[null,null,null,null,"3 b",{"$f":"Translation!A212","v":"Circulation pump: DHW heating"},null,null,null,null,null,null,null,null,null,null,null,35,{"$f":"Translation!A255","v":"Flow limiter"}]
[null,null,null,null,"3 c",{"$f":"Translation!A213","v":"Circulation pump: Heating circuit 1"},null,null,null,null,null,null,null,null,null,null,null,36,{"$f":"Translation!A256","v":"High limit thermostat - underfloor heating system "}]
[null,null,null,null,"3 d ",{"$f":"Translation!A214","v":"Circulation pump: Heating circuit 2"},null,null,null,null,null,null,null,null,null,null,null,37,{"$f":"Translation!A257","v":"Zone valve"}]
[null,null,null,null,"3 e",{"$f":"Translation!A215","v":"Circulation pump: Swimming pool"},null,null,null,null,null,null,null,null,null,null,null,38,{"$f":"Translation!A258","v":"Inflow tube"}]
[null,null,null,null,"3 f",{"$f":"Translation!A216","v":"Circulation pump: Solar DHE heating"},null,null,null,null,null,null,null,null,null,null,null,39,{"$f":"Translation!A259","v":"Filter / strainer"}]
[null,null,null,null,"3 f.1",{"$f":"Translation!A217","v":"Circulation pump: Solar heating system"},null,null,null,null,null,null,null,null,null,null,null,40,{"$f":"Translation!A260","v":"Fancoil "}]
[null,null,null,null,"3 f.2",{"$f":"Translation!A218","v":"Circulation pump: Solar Swimming pool"},null,null,null,null,null,null,null,null,null,null,null,41,{"$f":"Translation!A261","v":"Instantaneous water heater DHE"}]
[null,null,null,null,"3 fo",{"$f":"Translation!A219","v":"Circulation pump: Solar panel East"},null,null,null,null,null,null,null,null,null,null,null,42,{"$f":"Translation!A262","v":"Solar panel"}]
[null,null,null,null,"3 fw",{"$f":"Translation!A220","v":"Circulation pump: Solar panel West"},null,null,null,null,null,null,null,null,null,null,null,43,{"$f":"Translation!A263","v":"Electrical heating flang"}]
[null,null,null,null,"3 g",{"$f":"Translation!A221","v":"Circulation pump: Solid fuel boiler"}]
[null,null,null,null,"3 x",{"$f":"Translation!A222","v":"Circulation pump: Cooling - hest source"},null,null,null,null,null,null,null,null,null,null,null,"I",{"$f":"Translation!A264","v":"Heat utilisation system"}]
[null,null,null,null,"3 y",{"$f":"Translation!A223","v":"Circulation pump: Heat pump - heat source"},null,null,null,null,null,null,null,null,null,null,null,"II",{"$f":"Translation!A265","v":"Heat source system "}]
[null,null,null,null,4,{"$f":"Translation!A224","v":"Compact installation: WPKI"},null,null,null,null,null,null,null,null,null,null,null,"III",{"$f":"Translation!A266","v":"Solar panel"}]
[null,null,null,null,5,{"$f":"Translation!A225","v":"Safety valve"},null,null,null,null,null,null,null,null,null,null,null,"IV",{"$f":"Translation!A267","v":"Cooling system"}]
[null,null,null,null,6,{"$f":"Translation!A226","v":"Expansion vessel"},null,null,null,null,null,null,null,null,null,null,null,"V",{"$f":"Translation!A268","v":"Radiator heating system "}]
[null,null,null,null,7,{"$f":"Translation!A227","v":"Buffer cylinder/ low loss header"},null,null,null,null,null,null,null,null,null,null,null,"VI",{"$f":"Translation!A269","v":"Underfloor heating system"}]
[null,null,null,null,8,{"$f":"Translation!A228","v":"Anti-vibration mount"},null,null,null,null,null,null,null,null,null,null,null,"VII",{"$f":"Translation!A270","v":"DHW"}]
[null,null,null,null,9,{"$f":"Translation!A229","v":"Non-return valve"},null,null,null,null,null,null,null,null,null,null,null,"VIII",{"$f":"Translation!A271","v":"Swimming pool water "}]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!B367=FALSE,Translation!A176,\"\")","v":""}]
[null,{"$f":"$B$5","v":"Project data"},null,null,null,null,{"$f":"$G$5","v":"System selection"},null,null,null,null,{"$f":"$L$5","v":"Collector details"},null,null,null,null,{"$f":"$Q$5","v":"Material composition"},null,null,null,null,{"$f":"$V$5","v":"Solar yield"},null,null,null,null,{"$f":"$AA$5","v":"Hydraulical scetch"},null,null,null,null,{"$f":"$AF$5","v":"Expansion vessel"},null,null,null,null,{"$f":"$AK$5","v":"Printout"}]
[]
[]
[null,null,null,null,{"$f":"Translation!A274","v":"Components solar system"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A273","v":"Expansion vessel"}]
[]
[null,null,null,null,{"$f":"Translation!A275","v":"Collector"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A286","v":"Expansion volume"},null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C459,1)&\" \"&Translation!$A$287","v":"7,3 Litres"}]
[]
[null,null,null,null,{"$f":"Translation!A276","v":"DHW cylinder"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A288","v":"Pressure factor"},null,null,null,null,null,0.38500000000000001]
[]
[null,null,null,null,{"$f":"Translation!A277","v":"Buffer cylinder"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A289","v":"Minimum size"},null,null,null,null,null,{"$f":"Zwischenwerte!C472","v":"19 Litres"}]
[]
[null,null,null,null,{"$f":"Translation!A278","v":"Heat exchanger"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A291","v":"Recommendation"},null,null,null,null,null,{"$f":"Zwischenwerte!C473","v":"AG 25"},null,null,null,null,null,null,null,null," [i]"]
[]
[null,null,null,null,{"$f":"Translation!A279","v":"Flexible solar pipe"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A296","v":"Applicable for up to 20 m height differential (collector - DEV), safety valve response pressure 6 bar"}]
[]
[null,null,null,null,{"$f":"Translation!A280","v":"Copper pipe 18 x 1.0"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A292","v":"Heat transfer medium"}]
[]
[null,null,null,null,{"$f":"Translation!A281","v":"Copper pipe 22 x 1.0"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A293","v":"System volume"},null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C454,1)&\" \"&Translation!$A$287","v":"13,2 Litres"}]
[]
[null,null,null,null,{"$f":"Translation!A282","v":"Copper pipe 28 x 1.5"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A294","v":"Liquid seal (min. 3 l)"},null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C455,1)&\" \"&Translation!$A$287","v":"3,0 Litres"}]
[]
[null,null,null,null,{"$f":"Translation!A283","v":"Copper pipe 35 x 1.5"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A295","v":"Total volume"},null,null,null,null,null,{"$f":"Zwischenwerte!C475","v":"16 Litres"}]
[]
[null,null,null,null,{"$f":"Translation!A284","v":"Other installations"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A291&\" H-30 L\"","v":"Recommendation H-30 L"},null,null,null,null,null,{"$f":"Zwischenwerte!C478","v":"1 x 20 Litres H-30L"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"$B$5","v":"Project data"},null,null,null,null,{"$f":"$G$5","v":"System selection"},null,null,null,null,{"$f":"$L$5","v":"Collector details"},null,null,null,null,{"$f":"$Q$5","v":"Material composition"},null,null,null,null,{"$f":"$V$5","v":"Solar yield"},null,null,null,null,{"$f":"$AA$5","v":"Hydraulical scetch"},null,null,null,null,{"$f":"$AF$5","v":"Expansion vessel"},null,null,null,null,{"$f":"$AK$5","v":"Printout"}]
[]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"Translation!A299","v":"Select printout"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A300","v":"Project"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A301","v":"Description solar system"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A302","v":"Type of utilisation"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A303","v":"Material composition"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A135","v":"Solar yield"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A304","v":"Hydraulic/wiring diagrams"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A305","v":"Pipework installation"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A273","v":"Expansion vessel"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A65","v":"Collector details"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translation!A306","v":"Installation information"}]

{"sheet":"Zwischenwerte","index":1,"n_rows":533,"n_cols":32,"rows_kept":533,"cut":false,"hidden":true,"merged":[[453,8,453,9],[460,8,460,9],[385,13,385,14],[385,10,385,12],[385,7,385,9],[385,4,385,6],[511,12,512,12],[510,8,510,11],[510,12,510,15],[511,9,512,9],[511,11,512,11],[511,8,512,8],[511,10,512,10],[511,13,512,13],[511,15,512,15],[511,14,512,14],[468,11,469,11],[468,10,469,10],[468,8,469,8],[468,9,469,9],[463,8,463,9],[462,8,462,9],[461,8,461,9],[511,7,512,7],[473,0,473,1],[468,7,469,7],[461,0,461,1],[511,1,512,1],[511,3,512,3],[511,2,512,2],[511,4,512,4],[511,5,512,5],[471,0,471,1],[472,0,472,1],[474,0,474,1],[470,0,470,1],[468,0,469,1],[511,0,512,0],[510,0,510,3],[510,4,510,7],[511,6,512,6],[464,8,464,9],[468,2,469,2],[4,2,4,3],[4,4,4,5],[459,0,459,1],[456,0,456,1],[454,0,454,1],[457,0,457,1],[458,0,458,1],[364,2,364,6],[362,2,362,6],[434,1,435,1],[434,2,435,2],[451,0,452,1],[434,3,435,3],[434,4,435,4],[434,5,435,5],[434,0,435,0],[455,0,455,1],[460,0,460,1],[385,0,385,3],[355,0,356,0],[386,5,387,5],[456,8,456,9],[355,1,356,1],[355,2,356,6],[360,2,360,6],[361,2,361,6],[357,2,357,6],[359,2,359,6],[349,2,349,6],[343,2,343,6],[344,2,344,6],[345,2,345,6],[346,2,346,6],[347,2,347,6],[348,2,348,6],[11,43,11,44],[432,2,433,2],[432,3,433,3],[11,11,11,12],[386,13,387,13],[386,14,387,14],[303,9,303,14],[109,9,110,9],[165,0,165,3],[432,1,433,1],[386,12,387,12],[165,4,165,8],[165,9,165,12],[230,0,231,0],[386,7,387,7],[303,0,303,2],[221,1,222,1],[221,0,222,0],[432,0,433,0],[221,2,222,2],[221,3,222,3],[109,8,110,8],[111,8,112,8],[111,9,112,9],[453,0,453,1],[451,2,452,2],[386,6,387,6],[459,8,459,9],[455,8,455,9],[386,1,387,1],[386,0,387,0],[386,2,387,2],[386,3,387,3],[386,4,387,4],[451,8,452,9],[432,4,433,4],[432,5,433,5],[451,7,452,7],[386,8,387,8],[386,9,387,9],[436,0,437,0],[436,1,437,1],[436,2,437,2],[436,3,437,3],[436,4,437,4],[436,5,437,5],[454,8,454,9],[457,8,457,9],[11,25,11,26],[303,3,303,4],[230,5,231,5],[230,6,231,6],[230,7,231,7],[221,4,222,4],[74,2,74,6],[75,2,75,6],[76,2,76,6],[77,2,77,6],[78,2,78,6],[80,2,80,6],[303,5,303,6],[81,2,81,6],[121,2,121,6],[230,4,231,4],[230,8,231,8],[4,12,4,13],[4,14,4,15],[4,16,4,17],[4,18,4,19],[4,6,4,7],[109,11,110,11],[111,11,112,11],[325,2,325,6],[341,2,342,6],[82,2,82,6],[11,30,11,31],[458,8,458,9],[465,8,465,9],[4,20,4,21],[341,0,342,0],[341,1,342,1],[230,2,231,2],[230,1,231,1],[230,3,231,3],[4,0,4,1],[72,2,72,6],[73,2,73,6],[111,10,112,10],[324,2,324,6],[322,2,322,6],[323,2,323,6],[303,7,303,8],[221,5,222,5],[221,6,222,6],[386,10,387,10],[386,11,387,11],[363,2,363,6],[4,8,4,9],[4,10,4,11]]}
["Berechnungsblatt Zwischenwerte"]
[]
[]
["Kopfdaten"]
["Bauvorhaben",null,"Fachhandwerker",null,"Sonstiges I",null,"Sonstiges II",null,"Übersetzungen für Comboboxen I",null,"Übersetzungen ChkOptionalesZubehör I",null,"Übersetzungen ChkOptionalesZubehör I",null,"Übersetzungen frmPreisliste",null,"Übersetzungen frmPreisliste II",null,"Übersetzung MsgBox Anderer Speicher",null,"Übersetzung MsgBox Standradwerte Material"]
["Name",{"$f":"IF(Auswahl!$J$10=\"\",\"\",Auswahl!$J$10)","v":"Beispielprojekt"},"Name",{"$f":"IF(Auswahl!$J$20=\"\",\"\",Auswahl!$J$20)","v":"Stiebel Eltron GmbH & Co. KG"},"Sprache",2,"Stadt Gewählt","Hamburg","chkSomIntegriert","Aachen","chkSomIntegriert",{"$f":"Translation!A106","v":"SOKI with integral control unit"},"chkBGC",{"$f":"Translation!A110","v":"Threaded immersion heater BGC"},"Überschrift",{"$f":"Translation!A103","v":"Add product"},"btnEintragLöschen",{"$f":"Translation!A116","v":"Remove from material list"},"Term 1",{"$f":"Translation!A118","v":"The DHW cylinder determined by reference to collector number is not sufficient for the specified DHW demand. This cylinder is recommended:"},"Term 1",{"$f":"Translation!A125","v":"There were changes made to the selected solar system. The material list will be rebuilt (reset of  manual changes)."}]
["Straße",{"$f":"IF(Auswahl!$J$12=\"\",\"\",Auswahl!$J$12)","v":""},"Straße",{"$f":"IF(Auswahl!$J$22=\"\",\"\",Auswahl!$J$22)","v":"Dr.-Stiebel-Straße"},"Haken bei Koll. automatisch?",false,null,null,"chkSAS",null,"chkSAS",{"$f":"Translation!A107","v":"SOKI installation at the SBB...Plus"},"chkZTA",{"$f":"Translation!A111","v":"Central thermostatic valve"},"Beschreibung",{"$f":"Translation!A113","v":"Please enter product number and description."},"btnFertig",{"$f":"Translation!A117","v":"Close window"},"Term 2",{"$f":"Translation!A98","v":"ID"},"Term 2",{"$f":"Translation!A126","v":"All changes and items manually added will be resetted. Continue ?"}]
["PLZ/Ort",{"$f":"IF(Auswahl!$J$14=\"\",\"\",Auswahl!$J$14)","v":""},"PLZ/Ort",{"$f":"IF(Auswahl!$J$24=\"\",\"\",Auswahl!$J$24)","v":"37603 Holzminden"},"Währung","€",null,null,"chKWMZ",null,"chKWMZ",{"$f":"Translation!A108","v":"Heat metering"},"chkWärmeträger",{"$f":"Translation!A112","v":"Heat transfer medium H-30 LS"},"btnSuchen",{"$f":"Translation!A114","v":"Search..."},"btnStandard wiederherstellen",{"$f":"Translation!A104","v":"Reset standard values"},"Term 3",{"$f":"Translation!A119","v":"Do you want to replace DHW cylinder ?"},"Überschrift",{"$f":"Translation!A104","v":"Reset standard values"}]
["Telefon",{"$f":"IF(Auswahl!$J$16=\"\",\"\",Auswahl!$J$16)","v":""},"Telefon",{"$f":"IF(Auswahl!$J$26=\"\",\"\",Auswahl!$J$26)","v":"05531 / 702 110"},"Preise Materialliste anzeigen ?",true,null,null,"chkHUV",null,"chkHUV",{"$f":"Translation!A109","v":"Heating diverter valve"},null,null,"btnInMaterialliste",{"$f":"Translation!A115","v":"Add to material list"}]
[]
["Eingabe/Ausgabewerte Comboboxen Eingabemaske"]
["Klimazone - Land","Stadt","Solare WWB ?","Solare HU ?","Pool Solar ?","Personenzahl","WW-Bedarf","Heizlast","Speicherart","Schwimmbadart","Schwimmbadvolumen","Kollektoranordnung",null,"Kollektorart","Kollektoranzahl","Kollektorneigung","Kollektorausrichtung","Dachform","Befestigungsart","2. Wärmeerzeuger","Kaltwassertemperatur","Speichertemperatur","Systemverluste WWB","Normaußentemperatur","Heizgrenztemperatur","Ausdruck",null,"Sprache","Beschriftung Buttons","Beschriftung Auftraggeber","Währung"]
[]
["Germany","Aachen",true,false,false,"4","Standard demand (40 litres)","","","",{"$f":"IF(E14=FALSE,0,Auswahl!K72)","v":0},1,{"$f":"VLOOKUP(L14,L16:M39,2,FALSE)","v":"On end next to each other"},"Rooftop SOL 27 Premium","Determine the optimum number","45 °","South","Tiled roof","Standard fixings","Heat pump","10 °C","45 °C","20 %","-14 °C","15 °C","Alles gewählt ?",{"$f":"COUNTIF(AA16:AA39,TRUE)","v":7},"English",null,null,1,{"$f":"VLOOKUP(AE14,AE17:AF39,2,FALSE)","v":"Euro €"}]
[]
[]
[{"$f":"Translation!A19","v":"Germany"},null,null,null,null,1,{"$f":"Translation!A46","v":"Very low demand (15 litres)"},"3 kW",{"$f":"Translation!A54","v":"Two cylinder system (SBB+SBP)"},{"$f":"Translation!A59","v":"Open air swimming pool with cover"},0.7,1,{"$f":"Translation!A79","v":"On end next to each other"},{"$f":"Translation!A67&\" SOL 27 Premium\"","v":"Rooftop SOL 27 Premium"},{"$f":"Translation!$A$70","v":"Determine the optimum number"},"0 °",{"$f":"Translation!A73","v":"South"},{"$f":"Translation!A84","v":"Tiled roof"},{"$f":"Translation!A87","v":"Standard fixings"},{"$f":"Translation!A178","v":"None"},"5 °C","45 °C","0 %","0 °C","10 °C",{"$f":"Auswahl!L456","v":"Project"},true,"Deutsch",{"$f":"\"|  \"&Translation!A103","v":"|  Add product"},{"$f":"Translation!A361","v":"Beispielprojekt"},1,"Euro €"]
[{"$f":"Translation!A20","v":"France"},null,null,"Bild Systemhaus:",null,2,{"$f":"Translation!A47","v":"Low demand (30 litres)"},"4 kW",{"$f":"Translation!A55","v":"Instantaneous water heater (SBS)"},{"$f":"Translation!A60","v":"Open air pool without cover"},1,2,{"$f":"Translation!A80","v":"Across above each other"},{"$f":"Translation!A67&\" SOL 27 Basic\"","v":"Rooftop SOL 27 Basic"},1,"15 °",{"$f":"Translation!A74","v":"Southeast"},{"$f":"Translation!A85","v":"Corrugated roof"},{"$f":"Translation!A88","v":"Support stands 15°- 30°"},{"$f":"Translation!A179","v":"Heat pump"},"6 °C","50 °C","5 %","-2 °C","12 °C",{"$f":"Auswahl!L458","v":"Description solar system"},true,"English",{"$f":"\"|  \"&Translation!A104","v":"|  Reset standard values"},{"$f":"Translation!A362","v":"Stiebel Eltron GmbH & Co. KG"},2,"Pounds £"]
[{"$f":"Translation!A21","v":"Switzerland"},null,null,{"$f":"IF(E14=FALSE,IF(OR(I14=I18,I14=I19),3,IF(I14=I17,2,IF(C14=TRUE,1,0))),IF(OR(I14=I18,I14=I19),6,IF(I14=I17,5,IF(C14=TRUE,4,7))))","v":1},null,3,{"$f":"Translation!A48","v":"Standard demand (40 litres)"},"5 kW",{"$f":"Translation!A56","v":"Combi cylinder (SBK)"},{"$f":"Translation!A61","v":"Indoor pool with cover"},0.5,3,{"$f":"Translation!A81","v":"Across next to each other"},{"$f":"Translation!A68&\" SOL 23 Premium\"","v":"Roof integration SOL 23 Premium"},2,"30 °",{"$f":"Translation!A75","v":"Southwest"},{"$f":"Translation!A90","v":"Slate roof"},{"$f":"Translation!A89","v":"Quick assembly fixings"},{"$f":"Translation!A180","v":"Instantaneous water heater"},"7 °C","55 °C","10 %","-4 °C","15 °C",{"$f":"Auswahl!L460","v":"Type of utilisation"},true,"Francais",{"$f":"\"|  \"&Translation!A105","v":"|  Optional accessories"},{"$f":"Translation!A363","v":"Dr.-Stiebel-Straße"},3,"Dollar $"]
[{"$f":"Translation!A22","v":"USA"},null,null,null,null,4,{"$f":"Translation!A49","v":"High demand (60 litres)"},"6 kW",null,{"$f":"Translation!A62","v":"Indoor pool without cover"},1,4,{"$f":"Translation!A79","v":"On end next to each other"},null,3,"45 °",{"$f":"Translation!A76","v":"East"},{"$f":"Translation!A91","v":"Shingle roof"},null,{"$f":"Translation!A181","v":"Oil/gas boiler"},"8 °C","60 °C","15 %","-6 °C","20 °C",{"$f":"Auswahl!L462","v":"Material composition"},true,"Italiano",{"$f":"\"|  \"&Translation!A120","v":"|  Print material list"},{"$f":"Translation!A364","v":"37603 Holzminden"},4,"Koruna Kc"]
[{"$f":"Translation!A23","v":"Great Britain"},null,null,"Anzahl 'Wahr\"",null,5,{"$f":"Translation!A50","v":"Very high demand (80 litres)"},"7 kW",null,null,null,5,{"$f":"Translation!A81","v":"Across next to each other"},null,4,"60 °",{"$f":"Translation!A77","v":"West"},{"$f":"Translation!A92","v":"Plain tile roof"},null,{"$f":"Translation!A182","v":"Solid fuel boiler"},"9 °C","65 °C","20 %","-8 °C",null,{"$f":"Auswahl!L464","v":"Solar yield"},true,"Nederlands",{"$f":"IF(F9=TRUE,\"|  \"&Translation!A121,\"|  \"&Translation!A122)","v":"|  Printout with prices"},{"$f":"Translation!A365","v":"05531 / 702 110"},5,"Krone DKK"]
[{"$f":"Translation!A24","v":"Czech Republic"},null,null,{"$f":"C14+D14+E14","v":1},null,6,null,"8 kW",null,null,null,6,{"$f":"Translation!A79","v":"On end next to each other"},null,5,"75 °",null,{"$f":"Translation!A92&\"-CU\"","v":"Plain tile roof-CU"},{"$f":"Translation!A87","v":"Standard fixings"},null,"10 °C","70 °C","25 %","-10 °C",null,{"$f":"Auswahl!L466","v":"Hydraulic/wiring diagrams"},false,"čeština",{"$f":"\"|  \"&Translation!A123","v":"|  Export material-list"}]
[{"$f":"Translation!A25","v":"Poland"},null,null,null,null,7,null,"9 kW",null,null,null,7,{"$f":"Translation!A81","v":"Across next to each other"},null,6,"90 °",null,null,{"$f":"Translation!A89","v":"Quick assembly fixings"},null,"11 °C","75 °C","30 %","-12 °C",null,{"$f":"Auswahl!L468","v":"Pipework installation"},false,"Slovenčina",{"$f":"\"|  \"&Translation!A124","v":"|  Edit pricelist"}]
[{"$f":"Translation!A26","v":"Austria"},null,null,"Nutzungsart",null,8,null,"10 kW",null,null,null,8,{"$f":"Translation!A82","v":"On end above each other"},null,8,null,null,null,null,null,"12 °C","80 °C","35 %","-14 °C",null,{"$f":"Auswahl!L470","v":"Expansion vessel"},false,"Polski",{"$f":"\"|  \"&Translation!A150","v":"|  Show list of results"}]
[{"$f":"Translation!A27","v":"Sweden"},null,null,{"$f":"IF(D22=0,0,IF(D22=3,4,(IF(D22=1,(IF(C14=TRUE,1,5)),IF(E14=TRUE,3,2)))))","v":1},null,9,null,"11 kW",null,null,null,9,{"$f":"Translation!A79","v":"On end next to each other"},null,10,null,null,null,null,null,"13 °C","85 °C","40 %","-16 °C",null,{"$f":"Auswahl!L472","v":"Collector details"},true,"Magyar",{"$f":"\"|  \"&Translation!A151","v":"|  Show graph"}]
[{"$f":"Translation!A28","v":"Ireland"},null,null,null,null,10,null,"12 kW",null,null,null,null,null,null,12,null,null,null,null,null,"14 °C","90 °C",null,"-18 °C",null,{"$f":"Auswahl!L474","v":"Installation information"},true,"Suomi",{"$f":"\"|  \"&Translation!A166","v":"|  Extended settings"}]
[{"$f":"Translation!A29","v":"Italy"},null,null,null,null,11,null,"13 kW",null,null,null,null,null,null,15,null,null,null,null,null,"15 °C",null,null,"-20 °C",null,{"$f":"Auswahl!L476","v":0},false,"Dansk",{"$f":"\"|  \"&Translation!A172","v":"|  Accept"}]
[{"$f":"Translation!A30","v":"Hungary"},null,null,null,null,12,null,"14 kW",null,null,null,null,null,null,16,null,null,null,null,null,"16 °C",null,null,"-22 °C",null,{"$f":"Auswahl!L478","v":0},false,null,{"$f":"\"|  \"&Translation!A173","v":"|  Standard values"}]
[{"$f":"Translation!A31","v":"Belgium"},null,null,"1=WWB, 2=WWB+HU, 3=WWB+Pool, 4=WWB+HU+Pool, 5=Nur Pool",null,13,null,"15 kW",null,null,null,null,null,null,null,null,null,null,null,null,"17 °C",null,null,"-24 °C",null,null,false,null,{"$f":"\"|  \"&Translation!A186","v":"|  Show pipework installation"}]
[{"$f":"Translation!A32","v":"Netherlands"},null,null,null,null,14,null,"16 kW",null,null,null,null,null,null,null,null,null,null,null,null,"18 °C",null,null,"-26 °C",null,null,false,null,{"$f":"\"|  \"&Translation!A183","v":"|  Show hydraulic scetch"}]
[{"$f":"Translation!A33","v":"Slovakia"},null,null,null,null,15,null,"17 kW",null,null,null,null,null,null,null,null,null,null,null,null,"19 °C",null,null,"-28 °C",null,null,false,null,{"$f":"\"|  \"&Translation!A184","v":"|  Show electrical scetch"}]
[{"$f":"Translation!A34","v":"Finland"},null,null,null,null,null,null,"18 kW",null,null,null,null,null,null,null,null,null,null,null,null,"20 °C",null,null,"-30 °C",null,null,false,null,{"$f":"\"|  \"&Translation!A185","v":"|  Show description"}]
[{"$f":"Translation!A35","v":"Bosnia-Herzegovina"},null,null,null,null,null,null,"19 kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-32 °C",null,null,false,null,{"$f":"\"|  \"&Translation!A285","v":"|  Get components from material list"}]
[{"$f":"Translation!A36","v":"Denmark"},null,null,null,null,null,null,"20 kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-34 °C",null,null,false,null,{"$f":"Translation!A308","v":"Print selection"}]
[{"$f":"Translation!A37","v":"Morocco"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-36 °C",null,null,false,null,{"$f":"Translation!A307","v":"Select all"}]
[{"$f":"Translation!A38","v":"Europe"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-38 °C",null,null,false,null,{"$f":"\"|  \"&Translation!A130","v":"|  Back to main window"}]
["---",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 °C",null,null,false,null,{"$f":"\"|  \"&Translation!A131","v":"|  Show values changed"}]
["Land gewählt ?",null,null,null,null,null,null,null,null,null,null,null,null,null,"Optimale Kollektorzahl",null,null,"Gewählte Dachform (Ausdruck)","Andere Dachhaken möglich ?",null,null,null,null,null,null,null,false,null,{"$f":"\"|  \"&Translation!A133","v":"|  Import pricelist"}]
[{"$f":"IF(A14=A37,FALSE,TRUE)","v":true},null,null,null,null,null,null,null,null,null,null,null,null,null,"2",null,null,{"$f":"IF(OR(L14=L20,L14=L21),Translation!A355,IF(OR(L14=L22,L14=L23),Translation!A356,R14))","v":"Tiled roof"},{"$f":"IF(OR(L14>3,N14=N19,R14=R18),FALSE,TRUE)","v":true}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Materialauswahl (Zum Durchsuchen der Material-Matrix)",null,null,null,null,null,null,null,"Kollektordaten"]
["Kollektortyp:",{"$f":"IF(N14=N17,1,IF(N14=N18,2,IF(N14=N19,3,0)))","v":1},"1=Sol 27 Premium, 2=Sol 27 Basic, 3=Sol 23 Plus",null,null,null,null,null,"Kollektortyptyp","Konversionsfaktor","Wärmeverlust alpha0","Wärmeverlust alpha1","Kollektorfläche"]
["Nutzungsart:",{"$f":"D25","v":1},"1=WWB, 2=WWB+HU, 3=WWB+SB, 4=WWB+HU+SB, 5=Nur SB",null,null,null,null,"Nutzung"]
["Speicherart",{"$f":"IF(D25=5,0,IF(OR(I14=\"\",I14=I17),1,IF(I14=I18,3,2)))","v":1},"0=KeinSpeicher, 1=SBB, 2=SBK, 3=SBS",null,null,null,null,"Kollektortyp",{"$f":"N17","v":"Rooftop SOL 27 Premium"},0.83,3.46,1.5299999999999999E-2,2.4]
["Dachart",{"$f":"IF(N14=N19,1,IF(L14>3,3,IF(R14=R18,2,1)))","v":1},"1=Pfannendach, 2=Welldach, 3=Flachdach/Wand",null,null,null,null,"Speicher",{"$f":"N18","v":"Rooftop SOL 27 Basic"},0.79,3.42,1.4200000000000001E-2,2.4]
["Kollektoranordnung",{"$f":"IF(L14=L24,4,IF(L14=L18,3,IF(OR(L14=L19,L14=L21,L14=L23),2,1)))","v":1},"1=senkrecht nebeneinander, 2= waagerecht nebeneinander, 3=waagerecht übereinader, 4 = senkrecht übereinander",null,null,null,null,"HUV","Roof integration SOL 23 Premium",0.83,3.46,1.5299999999999999E-2,2]
["Kollektorbefestigung",{"$f":"IF(L14>3,1,IF(S14=S19,2,IF(S14=S18,3,1)))","v":1},"1=Standardbefestigung, 2=Schnellbefestigung, 3=Aufständerung 15°-30°",null,null,null,null,"Dachform"]
["Solarregelung",1,"1 = Regelung in SOKI integriert, 2 = Regelung & SOKI separat",null,null,null,null,"Anordnung"]
["Umschaltventil",1,"1=mit Umschaltventil, 2=separate Pumpen Heizung/WWB",null,null,null,null,"Befestigung"]
["Kollektoranzahl",{"$f":"IF(O14=O17,O39*1,O14*1)","v":2},"1 - 16",null,null,null,null,"Regelung"]
["Schlüssel Suchzeile",{"$f":"B74&B73&B75&B80&B76&B77&B78&B79&B81","v":"111111112"},null,null,null,null,null,"Kollektorzahl"]
["Suchzeile",{"$f":"MATCH(B82,'Matrix-Material'!J:J,0)","v":4}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Eingabewerte für Berechnung Deckungsanteil",null,null,null,null,null,null,null,"Südabweichung | Kollektorneigung (nach DIN 4701-10)"]
["Personenzahl",{"$f":"IF(F14=\"\",0,F14*1)","v":4},"Eingabewert",null,null,null,null,null,"Kollektorneigung",{"$f":"Translation!A73","v":"South"},{"$f":"Translation!A74","v":"Southeast"},{"$f":"Translation!A75","v":"Southwest"},{"$f":"Translation!A76","v":"East"},{"$f":"Translation!A77","v":"West"}]
["WW-Verbrauch",{"$f":"IF(G14=G17,15,IF(G14=G18,30,IF(G14=G19,40,IF(G14=G20,60,80))))","v":40},"Eingabewert",null,null,null,null,null,{"$f":"P17","v":"0 °"},0.81,0.81,0.81,0.81,0.81]
["Liter/Tag",{"$f":"ROUND(((B99*B100)/((B110-B109)/(45-B109))),0)","v":160},"Volumen bei Speichertemperatur (gemäß EN 15450)",null,null,null,null,null,"15 °",0.91100000000000003,0.88300000000000001,0.89500000000000002,0.79900000000000004,0.81299999999999994]
["Kollektoranzahl",{"$f":"B81","v":2},"Eingabewert",null,null,null,null,null,"30 °",0.97599999999999998,0.92700000000000005,0.95199999999999996,0.78700000000000003,0.83]
["Koll.-Gesamtfläche",{"$f":"B102*VLOOKUP(N14,I74:M83,5,FALSE)","v":4.8},"Kollektorfläche x Anzahl",null,null,null,null,null,"45 °",1,0.94,0.97099999999999997,0.76300000000000001,0.82]
["Konversionsfaktor",{"$f":"VLOOKUP(N14,I74:M83,2,FALSE)","v":0.83},"Kollektorkennwert",null,null,null,null,null,"60 °",0.97799999999999998,0.90900000000000003,0.95199999999999996,0.71799999999999997,0.78600000000000003]
["Wärmeverlust",{"$f":"VLOOKUP(N14,I74:M83,3,FALSE)","v":3.46},"Kollektorkennwert",null,null,null,null,null,"75 °",0.88700000000000001,0.80500000000000005,0.88300000000000001,0.64600000000000002,0.72399999999999998]
["Faktor Neigung/Azimut",{"$f":"INDEX(J100:N108,MATCH(P14,I100:I108,0),MATCH(Q14,J99:N99,0))","v":1},"Abschwächungsfaktor aus Tabelle für abweichende Neigung und Ausrichtung, nach DIN 4701-10",null,null,null,null,null,"90 °",0.70599999999999996,0.68200000000000005,0.749,0.54200000000000004,0.63100000000000001]
["Neigungswinkel",{"$f":"IF(P14=P17,0,IF(P14=P18,15,IF(P14=P19,30,IF(P14=P20,45,IF(P14=P21,60,IF(P14=P22,75,90))))))","v":45},"Eingabewert"]
["Breitengrad",{"$f":"Klimazonen!C2","v":50.77},"aus Eingabewert für Land/Stadt"]
["Kaltwassertemperatur",{"$f":"LEFT(U14,FIND(\" \",U14)-1)*1","v":10},"Eingabewert"]
["Speichertemperatur",{"$f":"LEFT(V14,FIND(\" \",V14)-1)*1","v":45},"Eingabewert",null,null,null,null,null,"Globalstrahlung","Klimazone Zahlenwert","Faktor","Klimazone Ausdruck"]
["Faktor Südabweichung",{"$f":"HLOOKUP(Q14,J99:N108,5,FALSE)","v":1},"aus Tabelle für 45° Kollektorneigung (f-Chart rechnet zwar Neigungswinkel ein, aber nicht Südabweichung)",null,null,null,null,null,null,null,"Speichervergrößerung"]
["Wärmebedarf WWB",{"$f":"(B101*1.163*(45-B109)*(1+(LEFT(W14,FIND(\" \",W14)-1)*1)/100)/1000)*1","v":7.8153600000000001},"kWh/d ( x Systemverlustfaktor)",null,null,null,null,null,{"$f":"Klimazonen!C16*365","v":1032.95},1,{"$f":"VLOOKUP(J112,J114:K128,2,FALSE)","v":1},{"$f":"VLOOKUP(J112,J114:L128,3,FALSE)","v":"I"}]
["Volumen pro m²/Fläche",{"$f":"ROUND(40*B106*K112,0)","v":40},"Mind. 40 l Speichervolumen pro m² Kollektorfläche * Faktor Klimazone * Faktor Südabweichung/Neigung"]
["Heizlast in KW",{"$f":"LEFT(H14,FIND(\" \",H14)-1)*1","v":{"$error":"#VALUE!"}},"Eingabewert"]
["Normaußentemp",{"$f":"LEFT(X14,FIND(\" \",X14)-1)*1","v":-14},"Eingabewert",null,null,null,null,null,0,1,1,"I"]
["Heizgrenze",{"$f":"LEFT(Y14,FIND(\" \",Y14)-1)*1","v":15},"Eingabewert",null,null,null,null,null,1040,2,1,"II"]
["Schwimmbadart",{"$f":"IF(J14=J17,1,IF(J14=J18,2,IF(J14=J19,3,4)))","v":4},"1=Freibad mit Abdeckung | 2=Freibad ohne Abdeckung | 3=Hallenbad mit Abdeckung | 4=Hallenbad ohne Abdeckung",null,null,null,null,null,1140,3,1.1000000000000001,"III"]
["Schwimbadnutzung",{"$f":"IF(B117<3,122,365)","v":365},"Freibad 122,5 Tage (Mitte Mai bis Mitte September) | Hallenbad 365 Tage",null,null,null,null,null,1250,4,1.2,"IV"]
["Schwimmbadvolumen",{"$f":"IF(K14*1=0,0.1,K14*1)","v":0.1},"Eingabewert",null,null,null,null,null,1350,5,1.333,"V"]
["Abkühlung K/Tag",{"$f":"VLOOKUP(J14,J16:K39,2,FALSE)","v":{"$error":"#N/A"}},"0,7=Freibad mit Abdeckung | 1=Freibad ohne Abdeckung | 0,5 = Hallenbad mit Abdeckung | 1 = Hallenbad ohne Abdeckung",null,null,null,null,null,1450,6,1.4330000000000001,"VI"]
["Wärmebedarf Pool",{"$f":"B119*1.163*B120","v":{"$error":"#N/A"}},"kWh/d (Volumen * 1,163 * Abkühlung)",null,null,null,null,null,1550,7,1.4666999999999999,"VII"]
["Nutzungsart:",{"$f":"D25","v":1},"1=WWB, 2=WWB+HU, 3=WWB+SB, 4=WWB+HU+SB, 5=Nur SB",null,null,null,null,null,1650,8,1.5,"VIII"]
["Gewählter Pufferspeicher",{"$f":"IF(B102>8,G235,G234)","v":"SBP 700 E SOL"},null,null,null,null,null,null,100000,9,null,"XI"]
["Puffervolumen",{"$f":"IF(B102>8,1000,700)","v":700}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Auswahl Speicher nach Verbrauch"]
[null,"Berechnung","Typ SBB","Typ SBS","Typ SBK"]
["Berechnungsart","Volumen benötigt","Volumen gewählt","Volumen gewählt","Volumen gewählt"]
[]
["nach Verbrauch",{"$f":"IF(B101>200,B101*1.18,IF(B101>400,B101*1.16,IF(B101>600,B101*1.14,IF(B101>800,B101*1.12,IF(B101>1000,B101*1.1,B101*1.2)))))","v":192},{"$f":"INDEX(A169:A184,IF(ISNA(MATCH(B147,A169:A184,0)),MATCH(B147,A169:A184,1)+1,MATCH(B147,A169:A184,0)))","v":305},{"$f":"VLOOKUP(INDEX(E169:E184,IF(ISNA(MATCH(B147,E169:E184,0)),MATCH(B147,E169:E184,1)+1,MATCH(B147,E169:E184,0))),E169:F184,2,FALSE)","v":600},{"$f":"ROUNDUP(B147/250,0)*250","v":250}]
["nach Kollektorfläche",{"$f":"IF(OR(D25=3,D25=4,D25=5),0,IF(B102>1,MAX(150,B113*B103*0.97),B113*B103*0.97))","v":186.24},{"$f":"IF(D25=1,INDEX(A169:A184,IF(ISNA(MATCH(B148,A169:A184,0)),MATCH(B148,A169:A184,1)+1,MATCH(B148,A169:A184,0))),A171)","v":305},{"$f":"INDEX(F169:F184,IF(ISNA(MATCH(B148,F169:F184,0)),MATCH(B148,F169:F184,1)+1,MATCH(B148,F169:F184,0)))","v":600},{"$f":"ROUNDUP(B148/750,0)*250","v":250}]
["Maximale Speichergröße",null,{"$f":"MAX(C147,C148)","v":305},{"$f":"MAX(D147,D148)","v":600},{"$f":"MAX(E147,E148)","v":250}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Hilfstabelle Speicherauswahl nach Verbrauch"]
["Typ SBB",null,null,null,"Typ SBS",null,null,null,null,"Typ SBK"]
["Speichervolumen","Anzahl","Ident.Nr","Bezeichnung","l/Tag Warmwasser","Gesamtinhalt SBS","Anzahl","Ident.Nr","Bezeichnung","Speichervolumen","Anzahl","Ident.Nr","Bezeichnung"]
[{"$f":"C149","v":305},{"$f":"VLOOKUP($A$168,$A$169:$D$190,2,FALSE)","v":1},{"$f":"VLOOKUP($A$168,$A$169:$D$190,3,FALSE)","v":187873},{"$f":"VLOOKUP($A$168,$A$169:$D$190,4,FALSE)","v":"SBB 300 Plus/trend"},{"$f":"INDEX(E169:E190,MATCH(F168,F169:F190,0))","v":275},{"$f":"D149","v":600},{"$f":"VLOOKUP($F$168,$F$169:$I$190,2,FALSE)","v":1},{"$f":"VLOOKUP($F$168,$F$169:$I$190,3,FALSE)","v":229984},{"$f":"VLOOKUP($F$168,$F$169:$I$190,4,FALSE)","v":"SBS 601 W SOL"},{"$f":"E149","v":250},{"$f":"VLOOKUP($J$168,$J$169:$M$190,2,FALSE)","v":1},{"$f":"VLOOKUP($J$168,$J$169:$M$190,3,FALSE)","v":74067},{"$f":"VLOOKUP($J$168,$J$169:$M$190,4,FALSE)","v":"SBK 600 / 150"}]
[0,0,0,"Kein Speicher",0,0,0,null,"Kein Speicher",0,0,null,"Kein Speicher"]
[146,1,74098,"KS 150 SOL",275,600,1,229984,"SBS 601 W SOL",250,1,74067,"SBK 600 / 150"]
[305,1,{"$f":"IF(N14=N18,233490,187873)","v":187873},"SBB 300 Plus/trend",350,800,1,229985,"SBS 801 W SOL",500,2,74067,"2 x SBK 600 / 150"]
[410,1,{"$f":"IF(N14=N18,233491,187874)","v":187874},"SBB 400 Plus/trend",475,1000,1,229986,"SBS 1001 W SOL",750,3,74067,"3 x SBK 600 / 150"]
[500,1,233492,"SBB 500 Trend",600,1500,1,229987,"SBS 1501 W SOL",1000,4,74067,"4 x SBK 600 / 150"]
[600,1,187875,"SBB 600 Plus",700,1600,2,229985,"2 x SBS 801 W SOL",1250,5,74067,"5 x SBK 600 / 150"]
[750,1,229294,"SBB 751 SOL",950,2000,2,229986,"2 x SBS 1001 W SOL",1500,6,74067,"6 x SBK 600 / 150"]
[1000,1,229295,"SBB 1001 SOL",1200,3000,2,229987,"2 x SBS 1501 W SOL",1750,7,74067,"7 x SBK 600 / 150"]
[1200,2,187875,"2 x SBB 600 Plus",1800,4500,3,229987,"3 x SBS 1501 W SOL"]
[1500,2,229294,"2 x SBB 751 SOL",2400,6000,4,229987,"4 x SBS 1501 W SOL"]
[2000,2,229295,"2 x SBB 1001 SOL",3000,7500,5,229987,"5 x SBS 1501 W SOL"]
[3000,3,229295,"3 x SBB 1001 SOL",3600,9000,6,229987,"6 x SBS 1501 W SOL"]
[4000,4,229295,"4 x SBB 1001 SOL",4200,10500,7,229987,"7 x SBS 1501 W SOL"]
[9999999999,null,null,null,9999999999,9999999999]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Vergleich Speicher nach Matrix <> Speicher nach Verbrauch"]
["Name","Speicher gefunden ?","Anzahl","Ident-Nr.","Bezeichnung","Gesamtvolumen","Reicht Volumen aus?"]
[]
[]
["Speicher in Matrix-Material",{"$f":"IF(COUNTIF(A233:A257,TRUE)=0,FALSE,TRUE)","v":true},{"$f":"IF(B225=FALSE,1,INDEX(Auswahl!E154:E191,MATCH(D225,Auswahl!H154:H191,0)))","v":1},{"$f":"IF(B225=FALSE,0,VLOOKUP(TRUE,A233:B257,2,FALSE))","v":187873},{"$f":"IF(B225=FALSE,0,VLOOKUP(TRUE,A233:C257,3,FALSE))","v":"SBB 300 Plus"},{"$f":"IF(B225=FALSE,100000,C225*VLOOKUP(TRUE,A233:D257,4,FALSE))","v":305},{"$f":"IF(D225*1=D226*1,TRUE,IF(F225<F226,FALSE,TRUE))","v":true}]
["Speicher nach Verbrauch",true,{"$f":"IF($B$75=1,B168,IF($B$75=2,K168,G168))","v":1},{"$f":"IF($B$75=1,C168,IF($B$75=2,L168,H168))","v":187873},{"$f":"IF($B$75=1,D168,IF($B$75=2,M168,I168))","v":"SBB 300 Plus/trend"},{"$f":"IF($B$75=1,A168,IF($B$75=2,J168,E168))","v":305}]
["Wärmedämmung",null,{"$f":"C226","v":1},{"$f":"VLOOKUP(D226,B233:E257,4,FALSE)","v":false},{"$f":"VLOOKUP(D225,B233:E257,4,FALSE)","v":false}]
[]
[]
["Liste aller WW-Speicher in der Matrix",null,null,null,null,"Liste Pufferspeicher"]
["In Materialliste vorhanden?","Ident.-Nr","Name Speicher","Volumen","Dämmung","Ident.-Nr","Name Speicher","Volumen","Dämmung"]
[]
[]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B234)>0,TRUE,FALSE)","v":false},74098,"KS 150 SOL",146,false,185460,"SBP 700 E SOL",700,false]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B235)>0,TRUE,FALSE)","v":true},187873,"SBB 300 Plus",305,false,227566,"SBP 1000 E SOL",1000,231929]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B236)>0,TRUE,FALSE)","v":false},187874,"SBB 400 Plus",410,false,227567,"SBP 1500 E SOL",1500,231930]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B237)>0,TRUE,FALSE)","v":false},233490,"SBB 300 Trend",300,false]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B238)>0,TRUE,FALSE)","v":false},233491,"SBB 400 Trend",400,false]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B239)>0,TRUE,FALSE)","v":false},233492,"SBB 500 Trend",500,false]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B240)>0,TRUE,FALSE)","v":false},227534,"SBB 501 WP SOL",500,false]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B241)>0,TRUE,FALSE)","v":false},187875,"SBB 600 Plus",600,false]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B242)>0,TRUE,FALSE)","v":false},229294,"SBB 751 SOL",750,231923]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B243)>0,TRUE,FALSE)","v":false},229295,"SBB 1001 SOL",1000,231924]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B244)>0,TRUE,FALSE)","v":false},74067,"SBK 600 / 150",250,false]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B245)>0,TRUE,FALSE)","v":false},229984,"SBS 601 W SOL",275,231925]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B246)>0,TRUE,FALSE)","v":false},229985,"SBS 801 W SOL",350,231926]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B247)>0,TRUE,FALSE)","v":false},229986,"SBS 1001 W SOL",475,231927]
[{"$f":"IF(COUNTIF(Auswahl!$H$154:$H$191,B248)>0,TRUE,FALSE)","v":false},229987,"SBS 1501 W SOL",600,231928]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["f-Chart (Berechnung Strahlung auf Kollektorebenen / Deckungsanteil WWB)"]
["Monat","Tag Nr.","Tage","Gg,Mittel   ","Gdiff,Mittel ","ta,mittel","d","wS","w","RS","R","Gg,Fläche","DeltaT","x","y","R"]
[null,null,null,"[kWh/m²d]","[kWh/m²d]","[°C]","[°]","[°]","[°]",null,null,"[Wh/m²d]","[K]"]
["Jan",17,31,{"$f":"Klimazonen!C4","v":0.72},{"$f":"Klimazonen!D4","v":0.44},{"$f":"Klimazonen!E4","v":2.8},{"$f":"23.45*SIN(RADIANS(360*(284+B288)/365))","v":-20.916962574476418},{"$f":"ACOS(-(TAN(RADIANS($B$108)))*TAN(RADIANS(G288)))*180/PI()","v":62.087315621201917},{"$f":"IF(ACOS(-(TAN(RADIANS($B$108-$B$107)))*TAN(RADIANS(G288)))*180/PI()>H288,H288,ACOS(-(TAN(RADIANS($B$108-$B$107)))*TAN(RADIANS(G288)))*180/PI())","v":62.087315621201917},{"$f":"(COS(RADIANS($B$108-$B$107))*COS(RADIANS(G288))*SIN(RADIANS(I288))+PI()*I288/180*SIN(RADIANS($B$108-$B$107))*SIN(RADIANS(G288)))/(COS(RADIANS($B$108))*COS(RADIANS(G288))*SIN(RADIANS(H288))+PI()*H288/180*SIN(RADIANS($B$108))*SIN(RADIANS(G288)))","v":3.5184974242052478},{"$f":"((1-E288/D288)*J288)+(E288/D288*(1+COS(RADIANS($B$107)))/2)+(0.2*(1-COS(RADIANS($B$107)))/2)","v":1.9192098366570531},{"$f":"D288*K288*$B$111*1000","v":1381.8310823930781},{"$f":"11.6+1.18*$B$110+3.86*$B$109-2.32*F288","v":96.803999999999988},{"$f":"($B$105*$B$103*M288*0.9*24/($B$112*1000))*($F$225/75/$B$103)^-0.25","v":4.6314402742351728},{"$f":"$B$104*$B$103*L288*0.9/($B$112*1000)","v":0.63396868845819276},{"$f":"1.029*O288-0.065*N288-0.245*O288^2+0.0018*N288^2+0.0215*O288^3","v":0.29692935031441031}]
["Feb",47,28,{"$f":"Klimazonen!C5","v":1.36},{"$f":"Klimazonen!D5","v":0.9},{"$f":"Klimazonen!E5","v":4},{"$f":"23.45*SIN(RADIANS(360*(284+B289)/365))","v":-12.954608093780696},73.635436957924767,73.635436957924767,2.4480630783887944,1.4221621656995744,1934.1405453514212,94.019999999999982,4.4982440248707798,0.88736210992354236,{"$f":"1.029*O289-0.065*N289-0.245*O289^2+0.0018*N289^2+0.0215*O289^3","v":0.47923794885141363}]
["Mrz",75,31,{"$f":"Klimazonen!C6","v":2.38},{"$f":"Klimazonen!D6","v":1.55},{"$f":"Klimazonen!E6","v":6.7},-2.4177348051423611,{"$f":"ACOS(-(TAN(RADIANS($B$108)))*TAN(RADIANS(G290)))*180/PI()","v":87.035650091600445},87.035650091600445,1.6964142440211341,1.176781581527192,2800.7401640347166,87.755999999999986,4.1985524638008949,{"$f":"$B$104*$B$103*L290*0.9/($B$112*1000)","v":1.2849483494250911},0.72213217248169848]
["Apr",105,30,{"$f":"Klimazonen!C7","v":3.84},{"$f":"Klimazonen!D7","v":1.75},{"$f":"Klimazonen!E7","v":9.6},{"$f":"23.45*SIN(RADIANS(360*(284+B291)/365))","v":9.4148933468800724},101.71790516909785,{"$f":"IF(ACOS(-(TAN(RADIANS($B$108-$B$107)))*TAN(RADIANS(G291)))*180/PI()>H291,H291,ACOS(-(TAN(RADIANS($B$108-$B$107)))*TAN(RADIANS(G291)))*180/PI())","v":90.96005077071645},{"$f":"(COS(RADIANS($B$108-$B$107))*COS(RADIANS(G291))*SIN(RADIANS(I291))+PI()*I291/180*SIN(RADIANS($B$108-$B$107))*SIN(RADIANS(G291)))/(COS(RADIANS($B$108))*COS(RADIANS(G291))*SIN(RADIANS(H291))+PI()*H291/180*SIN(RADIANS($B$108))*SIN(RADIANS(G291)))","v":1.2053358285067932},1.0743076331098418,4125.3413111417922,{"$f":"11.6+1.18*$B$110+3.86*$B$109-2.32*F291","v":81.027999999999992},3.8766615278369447,1.8926605818836251,0.99075199466505248]
["Mai",135,31,{"$f":"Klimazonen!C8","v":4.99},{"$f":"Klimazonen!D8","v":2.79},{"$f":"Klimazonen!E8","v":13.8},18.791917517696167,114.63063951102752,91.970412599316475,0.95194252359854858,0.92622068694588244,4621.8412278599535,71.283999999999992,3.4104746550615688,2.1204492060013416,1.0845881024185307]
["Jun",162,30,{"$f":"Klimazonen!C9","v":5.07},{"$f":"Klimazonen!D9","v":2.56},{"$f":"Klimazonen!E9","v":16.8},23.085911002836561,121.47122711353381,92.468548477348705,0.85780871840720718,0.88494939350281876,{"$f":"D293*K293*$B$111*1000","v":4486.6934250592913},64.323999999999984,3.0774840316505845,2.0584449014367339,1.0845618156506474]
["Jul",198,31,{"$f":"Klimazonen!C10","v":5.12},{"$f":"Klimazonen!D10","v":2.4700000000000002},{"$f":"Klimazonen!E10","v":17.8},{"$f":"23.45*SIN(RADIANS(360*(284+B294)/365))","v":21.183693564513842},118.3379948802246,92.244310545448812,0.89820859627317717,{"$f":"((1-E294/D294)*J294)+(E294/D294*(1+COS(RADIANS($B$107)))/2)+(0.2*(1-COS(RADIANS($B$107)))/2)","v":0.9059552701019129},4638.4909829217941,62.003999999999984,2.9664871571802571,2.1280879279219875,{"$f":"1.029*O294-0.065*N294-0.245*O294^2+0.0018*N294^2+0.0215*O294^3","v":1.1104834372988752}]
["Aug",228,31,{"$f":"Klimazonen!C11","v":4.45},{"$f":"Klimazonen!D11","v":2.25},{"$f":"Klimazonen!E11","v":18.7},13.454959682356431,107.03962650368048,91.385278754078413,1.0863523952290624,0.99793435521590768,4440.8078807107895,59.91599999999999,2.866589970156963,2.0373931254704334,1.0897814775680741]
["Sep",258,30,{"$f":"Klimazonen!C12","v":2.91},{"$f":"Klimazonen!D12","v":1.71},{"$f":"Klimazonen!E12","v":15.1},2.2168867832133041,92.717642492159882,90.224122899231844,1.4716013826250707,1.1377078638279374,3310.7298837392982,68.267999999999986,3.2661787182501421,1.5189259446955261,0.87997104481175215]
["Okt",288,31,{"$f":"Klimazonen!C13","v":1.76},{"$f":"Klimazonen!D13","v":1.1100000000000001},{"$f":"Klimazonen!E13","v":10.9},-9.5993972342263003,78.044726753131869,{"$f":"IF(ACOS(-(TAN(RADIANS($B$108-$B$107)))*TAN(RADIANS(G297)))*180/PI()>H297,H297,ACOS(-(TAN(RADIANS($B$108-$B$107)))*TAN(RADIANS(G297)))*180/PI())","v":78.044726753131869},2.1582195236907125,1.364679636629923,2401.8361604686643,78.011999999999986,3.7323655910255185,1.1019356417332589,0.64763661146207541]
["Nov",318,30,{"$f":"Klimazonen!C14","v":0.87},{"$f":"Klimazonen!D14","v":0.55000000000000004},{"$f":"Klimazonen!E14","v":6.2},-18.911954741226136,65.188634696442577,65.188634696442577,3.174860085879712,1.7366566693615848,1510.8913023445787,88.915999999999983,4.2540509010360594,0.6931800779089794,0.3587823874533751]
["Dez",344,31,{"$f":"Klimazonen!C15","v":0.47},{"$f":"Klimazonen!D15","v":0.35},{"$f":"Klimazonen!E15","v":3.4},-23.049627643930584,58.590307474913132,58.590307474913132,3.9730036733784777,1.6792981038240329,789.27010879729539,95.411999999999978,4.5648421495529758,0.36210832285442796,8.2298569551536763E-2]
["Jahr",null,365,{"$f":"Klimazonen!C16","v":2.83},{"$f":"Klimazonen!D16","v":1.54},{"$f":"Klimazonen!E16","v":10.5},null,null,null,null,null,{"$f":"SUMPRODUCT(L288:L299,C288:C299)","v":1110484.9587611635},null,null,509.47811337341176]
[]
[]
["Berechnung Deckungsanteil/Wärmemengen"]
[null,null,null,"Nur Warmwasserbereitung",null,"Nur Schwimmbadbeheizung",null,"Warmwasser + Schwimmbad",null,"Warmwasser + Heizung",null,null,null,null,null,"WWB+Heizung+Pool"]
["Monat","Tage","Solarer Ertrag","Deckungsanteil","Q-WWB","Deckungsanteil","Q-Pool","Deckungsanteil","Q-WWB + Q-Pool","Heizlast","Heizwärmebedarf","Deckungsanteil","Q-Hzg","Deckungsanteil","Q-Hzg+WWB"]
[null,null,"KWh/d","WWB","[kWh/d]","Pool","[kWh/d]","Pool","[kWh/d]","KW","kWh/d","Heizung","[kWh/d]","Heizung+WWB","[kWh/d]"]
[{"$f":"Translation!A152","v":"Jan"},31,{"$f":"L288*$B$103/1000","v":6.6327891954867741},{"$f":"IF(P288<0,0,MIN(P288,1))","v":0.29692935031441031},{"$f":"D307*$B$112","v":2.32060976727323},{"$f":"MIN(1,C307/$B$121)","v":{"$error":"#N/A"}},{"$f":"IF($B$117<3,0,F307*$B$121)","v":{"$error":"#N/A"}},{"$f":"MAX(MIN(1,(C307-E307)/$B$121),0)","v":{"$error":"#N/A"}},{"$f":"IF($B$117<3,E307,E307+H307*$B$121)","v":{"$error":"#N/A"}},{"$f":"MAX(0,(($B$116-F288)*$B$114)/($B$116-$B$115))","v":{"$error":"#VALUE!"}},{"$f":"J307*24","v":{"$error":"#VALUE!"}},{"$f":"IF(K307=0,0,MAX(MIN(1,(C307*0.25-E307)/K307),0))","v":{"$error":"#VALUE!"}},{"$f":"K307*L307","v":{"$error":"#VALUE!"}},{"$f":"(E307+M307)/($B$112+K307)","v":{"$error":"#VALUE!"}},{"$f":"M307+E307","v":{"$error":"#VALUE!"}}]
[{"$f":"Translation!A153","v":"Feb"},28,{"$f":"L289*$B$103/1000","v":9.2838746176868217},{"$f":"IF(P289<0,0,MIN(P289,1))","v":0.47923794885141363},3.7454170959353839,{"$error":"#N/A"},{"$f":"IF($B$117<3,0,F308*$B$121)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF($B$117<3,E308,E308+H308*$B$121)","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$f":"J308*24","v":{"$error":"#VALUE!"}},{"$f":"IF(K308=0,0,MAX(MIN(1,(C308*0.25-E308)/K308),0))","v":{"$error":"#VALUE!"}},{"$f":"K308*L308","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"M308+E308","v":{"$error":"#VALUE!"}}]
[{"$f":"Translation!A154","v":"Mar"},31,13.44355278736664,0.72213217248169848,5.643722895526567,{"$error":"#N/A"},{"$f":"IF($B$117<3,0,F309*$B$121)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF($B$117<3,E309,E309+H309*$B$121)","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A155","v":"Apr"},30,{"$f":"L291*$B$103/1000","v":19.801638293480604},0.99075199466505248,7.7430835090254648,{"$error":"#N/A"},{"$f":"IF($B$117<3,0,F310*$B$121)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF($B$117<3,E310,E310+H310*$B$121)","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A156","v":"May"},31,22.184837893727778,1,{"$f":"D311*$B$112","v":7.8153600000000001},{"$f":"MIN(1,C311/$B$121)","v":{"$error":"#N/A"}},{"$f":"F311*$B$121","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"E311+H311*$B$121","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A157","v":"Jun"},30,21.536128440284596,1,7.8153600000000001,{"$error":"#N/A"},{"$f":"F312*$B$121","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"E312+H312*$B$121","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A158","v":"Jul"},31,22.264756718024611,1,7.8153600000000001,{"$error":"#N/A"},{"$f":"F313*$B$121","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"E313+H313*$B$121","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A159","v":"Aug"},31,21.315877827411789,1,7.8153600000000001,{"$error":"#N/A"},{"$f":"F314*$B$121","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"E314+H314*$B$121","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A160","v":"Sep"},30,15.891503441948631,0.87997104481175215,6.8772905047799755,{"$error":"#N/A"},{"$f":"F315*$B$121","v":{"$error":"#N/A"}},{"$f":"MAX(MIN(1,(C315-E315)/$B$121),0)","v":{"$error":"#N/A"}},{"$f":"E315+H315*$B$121","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A161","v":"Oct"},31,11.528813570249588,0.64763661146207541,5.0615132677562453,{"$error":"#N/A"},{"$f":"IF($B$117<3,0,F316*$B$121)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF($B$117<3,E316,E316+H316*$B$121)","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A162","v":"Nov"},30,7.2522782512539772,0.3587823874533751,2.8040135196076097,{"$error":"#N/A"},{"$f":"IF($B$117<3,0,F317*$B$121)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF($B$117<3,E317,E317+H317*$B$121)","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$f":"Translation!A163","v":"Dec"},31,3.7884965222270175,8.2298569551536763E-2,0.6431929485302984,{"$error":"#N/A"},{"$f":"IF($B$117<3,0,F318*$B$121)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF($B$117<3,E318,E318+H318*$B$121)","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Jahr",365,{"$f":"SUMPRODUCT(C307:C318,B307:B318)","v":5330.3278020535845},{"$f":"SUMPRODUCT(D307:D318,B307:B318)/365","v":0.70554170738040078},{"$f":"SUMPRODUCT(B307:B318,E307:E318)","v":2012.6327899402588},{"$f":"IF(B117<3,(SUMPRODUCT(B312:B314,F312:F314)+0.5*B311*F311+0.5*B315*F315)/B118,SUMPRODUCT(B307:B318,F307:F318)/B118)","v":{"$error":"#N/A"}},{"$f":"IF(B117<3,SUMPRODUCT(B312:B314,G312:G314)+0.5*B311*G311+0.5*B315*G315,SUMPRODUCT(B307:B318,G307:G318))","v":{"$error":"#N/A"}},{"$f":"IF(B117<3,(SUMPRODUCT(B312:B314,H312:H314)+0.5*B311*H311+0.5*B315*H315)/B118,SUMPRODUCT(B307:B318,H307:H318)/B118)","v":{"$error":"#N/A"}},{"$f":"IF(B117<3,SUMPRODUCT(B312:B314,I312:I314)+0.5*B311*I311+0.5*B315*I315,SUMPRODUCT(B307:B318,I307:I318))","v":{"$error":"#N/A"}},{"$f":"B114","v":{"$error":"#VALUE!"}},{"$f":"SUMPRODUCT(K307:K318,B307:B318)","v":{"$error":"#VALUE!"}},{"$f":"SUMPRODUCT(B307:B318,L307:L318)/B319","v":{"$error":"#VALUE!"}},{"$f":"SUMPRODUCT(M307:M318,B307:B318)","v":{"$error":"#VALUE!"}},{"$f":"(E319+M319)/(B112*365+K319)","v":{"$error":"#VALUE!"}},{"$f":"SUMPRODUCT(O307:O318,D307:D318)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(D319>=D320,F319>=F320,L319>=L320,N319>=N320),TRUE,FALSE)","v":{"$error":"#N/A"}}]
["Sollwert",null,null,0.57999999999999996,null,{"$f":"IF(B117>2,0.6,1)","v":0.6},null,{"$f":"IF(B117>2,0.6,1)","v":0.6},null,null,null,{"$f":"IF(D319>0.95,0.02,0)","v":0},null,{"$f":"IF(D319<=0.95,IF(B114<=10,0.12,IF(B114<=15,0.11,0.1)),IF(L319<0.02,0,IF(B114<=10,0.12,IF(B114<=15,0.11,0.1))))","v":{"$error":"#VALUE!"}},null,true]
[]
["Soll-/Istwerte Deckungsgrad"]
["Nutzungsart Solar:",{"$f":"B74","v":1},"1=WWB, 2=WWB+HU, 3=WWB+SB, 4=WWB+HU+SB, 5=Nur SB"]
["Sollwert Deckung:",{"$f":"IF(B323=1,D320,IF(B323=2,N320,IF(B323=3,H320,IF(B323=5,F320,P320))))","v":0.57999999999999996},"aus Festlegung in Zeile 332"]
["Istwert Deckung",{"$f":"IF(B323=1,D319,IF(B323=2,N319,IF(B323=3,H319,IF(B323=5,F319,P319))))","v":0.70554170738040078},"aus Ergebnis Berechnung in Zeile 331"]
["Istwert >= Sollwert ?",{"$f":"IF(B323=2,(IF(AND(D319>=D320,L319>=L320,N319>=N320),TRUE,FALSE)),IF(B325>=B324,TRUE,FALSE))","v":true},"Boolescher Ausdruck für Schleife zur Bestimmung der optimalen Kollektoranzahl"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Hydraulikzeichnungen"]
["Schlüssel",{"$f":"B344&\"-\"&B345&\"-\"&B346","v":"1-1-1"}]
[]
["Nutzungsart",{"$f":"D25","v":1},"1=WWB, 2=WWB+HU, 3=WWB+Pool, 4=WWB+HU+Pool, 5=Nur Pool"]
["Speicherart",{"$f":"IF(AND(B74=1,B81=1),4,B75)","v":1},"0=Kein Speicher, 1=SBB, 2=SBK, 3=SBS, 4=KS 150"]
["2. WE",{"$f":"IF(T14=T17,0,IF(T14=T18,1,IF(T14=T19,2,IF(T14=T20,3,4))))","v":1},"0=Keiner, 1=Wärmepumpe, 2=Durchlauferhitzer, 3=Öl-/Gaskessel, 4=Feststoffkessel"]
[]
[]
[]
[]
[]
[]
[]
[]
["Zeichnungen Rohrinstallation"]
["Schlüssel",{"$f":"\"BildRohr-\"&B358&B359&B360","v":"BildRohr-121"}]
[]
["Kollektortyp",{"$f":"IF(N14=N19,2,1)","v":1},"1=SOL 27 Premium/Basic, 2= SOL 23 Premium"]
["Kollektoranzahl",{"$f":"B81","v":2},"1-16"]
["Anordnung",{"$f":"B77","v":1},"1=senkrecht nebeneinander, 2= waagerecht nebeneinander, 3=waagerecht übereinader, 4 = senkrecht übereinander"]
[]
[]
[]
[]
[]
[]
["Gefunden?",true]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Wasserinhalt Komponenten"]
["Kollektoren",null,null,null,"Warmwasserspeicher",null,null,"Pufferspeicher",null,null,"Wärmetauscher",null,null,"Sonstige Einbauten"]
["Typ","Anzahl","Wasserinhalt","Kollektorgruppe","Typ","Wasserinhalt","Anzahl","Typ","Wasserinhalt","Anzahl","Typ","Wasserinhalt","Anzahl","Auswahl","Wasserinhalt"]
[]
[]
["Rooftop SOL 27 Premium S","2",{"$f":"VLOOKUP(A390,A393:C413,3,FALSE)*B390","v":3},{"$f":"VLOOKUP(B390*1,B392:D412,3,FALSE)*0.13","v":0.13},"SBB 300 Plus",{"$f":"IF(G390=G393,0,VLOOKUP(E390,E392:F413,2,FALSE)*G390)","v":10.1},"1","SBP 700 E SOL",{"$f":"IF(J390=J393,0,VLOOKUP(H390,H392:I413,2,FALSE)*J390)","v":0},"---","WT 10",{"$f":"IF(M390=M393,0,VLOOKUP(K390,K392:L413,2,FALSE)*M390)","v":0},"---","---",{"$f":"IF(N390=E453,0,LEFT(N390,FIND(\" \",N390)-1)*1)","v":0}]
[]
[]
[{"$f":"N17&\" S\"","v":"Rooftop SOL 27 Premium S"},{"$f":"O18","v":1},1.5,0,"KS 150 SOL",3.2,"---","SBP 700 E SOL",14.2,"---","WT 10",0.9,"---"]
[{"$f":"N17&\" W\"","v":"Rooftop SOL 27 Premium W"},2,1.83,1,"SBB 300 Plus",10.1,1,"SBP 1000 E SOL",26,1,"WT 20",1.7,1]
[{"$f":"N18&\" S\"","v":"Rooftop SOL 27 Basic S"},3,1.3,2,"SBB 400 Plus",11.3,2,"SBP 1500 E SOL",31,2,"WT 30",2.5,2]
[{"$f":"N18&\" W\"","v":"Rooftop SOL 27 Basic W"},4,1.7,3,"SBB 600 Plus",21.1,3,null,null,3,"WT 40",4,3]
[{"$f":"N19","v":"Roof integration SOL 23 Premium"},5,1.2,4,"SBB 300 Trend",9.1999999999999993,4,null,null,4,null,null,4]
[null,6,null,4,"SBB 400 Trend",10.7,5,null,null,5,null,null,5]
[null,8,null,6,"SBB 500 Trend",16.399999999999999,6,null,null,6,null,null,6]
[null,10,null,8,"SBB 401 WP SOL",8.6999999999999993,7,null,null,7,null,null,7]
[null,12,null,9,"SBB 501 WP SOL",8.6999999999999993,8,null,null,8,null,null,8]
[null,15,null,12,"SBB 751 SOL",28.2,9,null,null,9,null,null,9]
[null,16,null,12,"SBB 1001 SOL",37.6,10,null,null,10,null,null,10]
[null,18,null,12,"SBS 601 W SOL",11.9]
[null,20,null,16,"SBS 801 W SOL",21.2]
[null,21,null,14,"SBS 1001 W SOL",25.9]
[null,24,null,20,"SBS 1501 W SOL",31.2]
[null,25,null,20,"SBK 600/150",15.2]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Wasserinhalt Kollektoren/Speicher"]
["Rohrtyp",{"$f":"Translation!A279","v":"Flexible solar pipe"},{"$f":"Translation!A280","v":"Copper pipe 18 x 1.0"},{"$f":"Translation!A281","v":"Copper pipe 22 x 1.0"},{"$f":"Translation!A282","v":"Copper pipe 28 x 1.5"},{"$f":"Translation!A283","v":"Copper pipe 35 x 1.5"}]
["Länge","---","---","---","---","---"]
[]
["Inhalt (Liter)",{"$f":"IF(B433=$F$453,0,LEFT(B433,FIND(\" \",B433)-1)*B437)","v":0},{"$f":"IF(C433=$F$453,0,LEFT(C433,FIND(\" \",C433)-1)*C437)","v":0},{"$f":"IF(D433=$F$453,0,LEFT(D433,FIND(\" \",D433)-1)*D437)","v":0},{"$f":"IF(E433=$F$453,0,LEFT(E433,FIND(\" \",E433)-1)*E437)","v":0},{"$f":"IF(F433=$F$453,0,LEFT(F433,FIND(\" \",F433)-1)*F437)","v":0}]
[]
["Inhalt (Liter/m)",0.30499999999999999,0.20100000000000001,0.314,0.49099999999999999,0.80400000000000005]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Berechnung MAG",null,null,null,"Listbox Sonstige","Listbox Rohre",null,"Nebenrechnung Auswahl MAG"]
["Berechnungsgröße",null,"Wert",null,null,null,null,"Mindestgröße","Auswahl MAG"]
[null,null,null,null,"---","---"]
["Summe Wasserinhalt Komponenten",null,{"$f":"C390+D390+F390+I390+L390+O390+SUM(B435:F436)","v":13.23},null,{"$f":"1&\" \"&Translation!$A$287","v":"1 Litres"},"1 m",null,0,"AG 12"]
["Flüssigkeitsvorlage 5% (mind. 3 l)",null,{"$f":"MAX(C454*0.005,3)","v":3},null,{"$f":"2&\" \"&Translation!$A$287","v":"2 Litres"},"2 m",null,13,"AG 18"]
["Gesamtinhalt ",null,{"$f":"C454+C455","v":16.23},null,{"$f":"3&\" \"&Translation!$A$287","v":"3 Litres"},"3 m",null,19,"AG 25"]
["Ausdehnungsvolumen",null,{"$f":"(C456-C390)*0.0849","v":1.123227},null,{"$f":"4&\" \"&Translation!$A$287","v":"4 Litres"},"4 m",null,26,"AG 50"]
["Verdampfungsvolumen",null,{"$f":"C390+D390","v":3.13},null,{"$f":"5&\" \"&Translation!$A$287","v":"5 Litres"},"5 m",null,51,"AG 80"]
["Summe Ausdehnungsvolumen",null,{"$f":"C455+C457+C458","v":7.2532269999999999},null,{"$f":"6&\" \"&Translation!$A$287","v":"6 Litres"},"6 m",null,81,"2 x AG 50"]
["Mindestgröße MAG",null,{"$f":"ROUND(C459/0.385,0)","v":19},null,{"$f":"7&\" \"&Translation!$A$287","v":"7 Litres"},"7 m",null,101,"2 x AG 80"]
[null,null,null,null,{"$f":"8&\" \"&Translation!$A$287","v":"8 Litres"},"8 m",null,161,{"$f":"\"AG 200 \"&Translation!$A$287&\" (\"&Translation!$A$290&\")\"","v":"AG 200 Litres (on site)"}]
[null,null,null,null,{"$f":"9&\" \"&Translation!$A$287","v":"9 Litres"},"9 m",null,201,{"$f":"\"AG 250 \"&Translation!$A$287&\" (\"&Translation!$A$290&\")\"","v":"AG 250 Litres (on site)"}]
[null,null,null,null,{"$f":"10&\" \"&Translation!$A$287","v":"10 Litres"},"10 m",null,251,{"$f":"\"AG 300 \"&Translation!$A$287&\" (\"&Translation!$A$290&\")\"","v":"AG 300 Litres (on site)"}]
[null,null,null,null,{"$f":"11&\" \"&Translation!$A$287","v":"11 Litres"},"11 m",null,301,{"$f":"\"AG 400 \"&Translation!$A$287&\" (\"&Translation!$A$290&\")\"","v":"AG 400 Litres (on site)"}]
[null,null,null,null,{"$f":"12&\" \"&Translation!$A$287","v":"12 Litres"},"12 m",null,401,{"$f":"\"AG 500 \"&Translation!$A$287&\" (\"&Translation!$A$290&\")\"","v":"AG 500 Litres (on site)"}]
[null,null,null,null,{"$f":"13&\" \"&Translation!$A$287","v":"13 Litres"},"13 m",null,501,{"$f":"\"AG 1000 \"&Translation!$A$287&\" (\"&Translation!$A$290&\")\"","v":"AG 1000 Litres (on site)"}]
[null,null,null,null,{"$f":"14&\" \"&Translation!$A$287","v":"14 Litres"},"14 m"]
["Ergebnisübergabe MAG",null,null,null,{"$f":"15&\" \"&Translation!$A$287","v":"15 Litres"},"15 m",null,"Gewählte Komponenten aus Materialliste finden"]
["Textbox",null,"Wert",null,{"$f":"16&\" \"&Translation!$A$287","v":"16 Litres"},"16 m",null,"Kategorie","Gefunden ?","Artikelnummer","Typ","Anzahl"]
[null,null,null,null,{"$f":"17&\" \"&Translation!$A$287","v":"17 Litres"},"17 m"]
["Anzahl & Typ Kollektoren",null,{"$f":"B390&\" x \"&A390","v":"2 x Rooftop SOL 27 Premium S"},null,{"$f":"18&\" \"&Translation!$A$287","v":"18 Litres"},"18 m",null,"Kollektor"]
["Mindestgröße MAG",null,{"$f":"ROUND(C460,0)&\" \"&Translation!A287","v":"19 Litres"},null,{"$f":"19&\" \"&Translation!$A$287","v":"19 Litres"},"19 m"]
["Empfehlung MAG",null,{"$f":"VLOOKUP(C460,H454:J466,2)","v":"AG 25"},null,{"$f":"20&\" \"&Translation!$A$287","v":"20 Litres"},"20 m"]
["Mindestgröße | Empfehlung MAG",null,{"$f":"C472&\"  |  \"&C473","v":"19 Litres  |  AG 25"},null,{"$f":"21&\" \"&Translation!$A$287","v":"21 Litres"},"21 m"]
["Wärmeträger-Flüssigkeit",null,{"$f":"ROUND(C456,0)&\" \"&Translation!A287","v":"16 Litres"},null,{"$f":"22&\" \"&Translation!$A$287","v":"22 Litres"},"22 m"]
["20-Liter Kanister",null,{"$f":"ROUNDDOWN(ROUNDUP(ROUND(C456,0),-1)/20,0)","v":1},null,{"$f":"23&\" \"&Translation!$A$287","v":"23 Litres"},"23 m"]
["10-Liter Kanister",null,{"$f":"(ROUNDUP(ROUND(C456,0),-1)-C476*20)/10","v":0},null,{"$f":"24&\" \"&Translation!$A$287","v":"24 Litres"},"24 m"]
["Empfehlung Kanister",null,{"$f":"IF(ROUND(C456,0)<11,\"1 x 10 \"&Translation!A287&\" H-30L\",IF(C477=0,C476&\" x 20 \"&Translation!A287&\" H-30L\",C476&\" x 20 \"&Translation!A287&\" H-30L | \"&C477&\" x 10 \"&Translation!A287&\" H-30L\"))","v":"1 x 20 Litres H-30L"},null,{"$f":"25&\" \"&Translation!$A$287","v":"25 Litres"},"25 m"]
[null,null,null,null,{"$f":"26&\" \"&Translation!$A$287","v":"26 Litres"},"26 m"]
[null,null,null,null,{"$f":"27&\" \"&Translation!$A$287","v":"27 Litres"},"27 m"]
[null,null,null,null,{"$f":"28&\" \"&Translation!$A$287","v":"28 Litres"},"28 m"]
[null,null,null,null,{"$f":"29&\" \"&Translation!$A$287","v":"29 Litres"},"29 m"]
[null,null,null,null,{"$f":"30&\" \"&Translation!$A$287","v":"30 Litres"},"30 m"]
[null,null,null,null,{"$f":"31&\" \"&Translation!$A$287","v":"31 Litres"},"31 m"]
[null,null,null,null,{"$f":"32&\" \"&Translation!$A$287","v":"32 Litres"},"32 m"]
[null,null,null,null,{"$f":"33&\" \"&Translation!$A$287","v":"33 Litres"},"33 m"]
[null,null,null,null,{"$f":"34&\" \"&Translation!$A$287","v":"34 Litres"},"34 m"]
[null,null,null,null,{"$f":"35&\" \"&Translation!$A$287","v":"35 Litres"},"35 m"]
[null,null,null,null,{"$f":"36&\" \"&Translation!$A$287","v":"36 Litres"},"36 m"]
[null,null,null,null,{"$f":"37&\" \"&Translation!$A$287","v":"37 Litres"},"37 m"]
[null,null,null,null,{"$f":"38&\" \"&Translation!$A$287","v":"38 Litres"},"38 m"]
[null,null,null,null,{"$f":"39&\" \"&Translation!$A$287","v":"39 Litres"},"39 m"]
[null,null,null,null,{"$f":"40&\" \"&Translation!$A$287","v":"40 Litres"},"40 m"]
[null,null,null,null,{"$f":"41&\" \"&Translation!$A$287","v":"41 Litres"},"41 m"]
[null,null,null,null,{"$f":"42&\" \"&Translation!$A$287","v":"42 Litres"},"42 m"]
[null,null,null,null,{"$f":"43&\" \"&Translation!$A$287","v":"43 Litres"},"43 m"]
[null,null,null,null,{"$f":"44&\" \"&Translation!$A$287","v":"44 Litres"},"44 m"]
[null,null,null,null,{"$f":"45&\" \"&Translation!$A$287","v":"45 Litres"},"45 m"]
[null,null,null,null,{"$f":"46&\" \"&Translation!$A$287","v":"46 Litres"},"46 m"]
[null,null,null,null,{"$f":"47&\" \"&Translation!$A$287","v":"47 Litres"},"47 m"]
[null,null,null,null,{"$f":"48&\" \"&Translation!$A$287","v":"48 Litres"},"48 m"]
[null,null,null,null,{"$f":"49&\" \"&Translation!$A$287","v":"49 Litres"},"49 m"]
[null,null,null,null,{"$f":"50&\" \"&Translation!$A$287","v":"50 Litres"},"50 m"]
[]
[]
[]
[]
[]
[]
["Vorgabewerte für Comboboxen MAG aus Materialliste bestimmen"]
["Kollektoren",null,null,null,"Warmwasserspeicher",null,null,null,"Pufferspeicher",null,null,null,"Wärmetauscher"]
["Ident-Nr. in Materialliste ?","Ident.-Nr.","Anzahl","Bezeichnung","Ident-Nr. in Materialliste ?","Ident.-Nr.","Anzahl","Bezeichnung","Ident-Nr. in Materialliste ?","Ident.-Nr.","Anzahl","Bezeichnung","Ident-Nr. in Materialliste ?","Ident.-Nr.","Anzahl","Bezeichnung"]
[]
[]
[{"$f":"IF(COUNTIF(A517:A538,TRUE)>0,TRUE,FALSE)","v":true},{"$f":"IF(A515=FALSE,B518,VLOOKUP(TRUE,A517:B538,2,FALSE))","v":230016},{"$f":"IF(A515=FALSE,2,INDEX(Auswahl!$E$154:$E$191,MATCH(B515,Auswahl!$H$154:$H$191,0)))","v":2},{"$f":"IF(A515=FALSE,D518,VLOOKUP(TRUE,A517:D538,4,FALSE))","v":"Rooftop SOL 27 Premium S"},{"$f":"IF(COUNTIF(E517:E538,TRUE)>0,TRUE,FALSE)","v":true},{"$f":"IF(E515=FALSE,F519,VLOOKUP(TRUE,E517:F538,2,FALSE))","v":187873},{"$f":"IF(E515=FALSE,G393,INDEX(Auswahl!$E$154:$E$191,MATCH(F515,Auswahl!$H$154:$H$191,0)))","v":1},{"$f":"IF(E515=FALSE,H519,VLOOKUP(TRUE,E517:H538,4,FALSE))","v":"SBB 300 Plus"},{"$f":"IF(COUNTIF(I517:I538,TRUE)>0,TRUE,FALSE)","v":false},{"$f":"IF(I515=FALSE,J518,VLOOKUP(TRUE,I517:J538,2,FALSE))","v":185460},{"$f":"IF(I515=FALSE,M393,INDEX(Auswahl!$E$154:$E$191,MATCH(J515,Auswahl!$H$154:$H$191,0)))","v":"---"},{"$f":"IF(I515=FALSE,L518,VLOOKUP(TRUE,I517:L538,4,FALSE))","v":"SBP 700 E SOL"},{"$f":"IF(COUNTIF(M517:M538,TRUE)>0,TRUE,FALSE)","v":false},{"$f":"IF(M515=FALSE,N518,VLOOKUP(TRUE,M517:N538,2,FALSE))","v":70633},{"$f":"IF(M515=FALSE,M393,INDEX(Auswahl!$E$154:$E$191,MATCH(N515,Auswahl!$H$154:$H$191,0)))","v":"---"},{"$f":"IF(M515=FALSE,P518,VLOOKUP(TRUE,M517:P538,4,FALSE))","v":"WT 10"}]
[]
[]
[{"$f":"IF(ISERROR(VLOOKUP(B518,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":true},230016,null,{"$f":"A393","v":"Rooftop SOL 27 Premium S"},{"$f":"IF(ISERROR(VLOOKUP(F518,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},74098,null,{"$f":"E393","v":"KS 150 SOL"},{"$f":"IF(ISERROR(VLOOKUP(J518,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},185460,null,{"$f":"H393","v":"SBP 700 E SOL"},{"$f":"IF(ISERROR(VLOOKUP(N518,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},70633,null,"WT 10"]
[{"$f":"IF(ISERROR(VLOOKUP(B519,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},230017,null,{"$f":"A394","v":"Rooftop SOL 27 Premium W"},{"$f":"IF(ISERROR(VLOOKUP(F519,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":true},187873,null,{"$f":"E394","v":"SBB 300 Plus"},{"$f":"IF(ISERROR(VLOOKUP(J519,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},227566,null,{"$f":"H394","v":"SBP 1000 E SOL"},{"$f":"IF(ISERROR(VLOOKUP(N519,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},706634,null,"WT 20"]
[{"$f":"IF(ISERROR(VLOOKUP(B520,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},228927,null,"Rooftop SOL 27 Basic S",{"$f":"IF(ISERROR(VLOOKUP(F520,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},187874,null,"SBB 400 Plus",{"$f":"IF(ISERROR(VLOOKUP(J520,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},227567,null,"SBP 1500 E SOL",{"$f":"IF(ISERROR(VLOOKUP(N520,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},71091,null,"WT 30"]
[{"$f":"IF(ISERROR(VLOOKUP(B521,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},230912,null,{"$f":"A396","v":"Rooftop SOL 27 Basic W"},{"$f":"IF(ISERROR(VLOOKUP(F521,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},187875,null,"SBB 600 Plus",null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(N521,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},229338,null,"WT 40"]
[{"$f":"IF(ISERROR(VLOOKUP(B522,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},230020,null,{"$f":"A397","v":"Roof integration SOL 23 Premium"},{"$f":"IF(ISERROR(VLOOKUP(F522,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},230338,null,"SBB 300 Trend"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F523,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},230339,null,"SBB 400 Trend"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F524,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},230340,null,"SBB 500 Trend"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F525,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},221362,null,"SBB 401 WP SOL"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F526,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},227534,null,"SBB 501 WP SOL"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F527,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},229294,null,"SBB 751 SOL"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F528,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},229295,null,"SBB 1001 SOL"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F529,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},229984,null,"SBS 601 W SOL"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F530,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},229985,null,"SBS 801 W SOL"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F531,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},229986,null,"SBS 1001 W SOL"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F532,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},229987,null,"SBS 1501 W SOL"]
[null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(F533,Auswahl!$H$154:$H$191,1,FALSE)),FALSE,TRUE)","v":false},74067,null,"SBK 600/150"]

{"sheet":"Matrix-Material","index":2,"n_rows":7163,"n_cols":116,"rows_kept":562,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":250,"rows_last":62,"rows_between":250,"halvings":3}}
["1=WWB | 2=WWB+HU | 3=WWB+SB | 4=WWB+HU+SB | 5= Nur SB","1=SOL 27 Premium S/W | 2=SOL 27 basic S/W | 3=SOL 23 premium ","0=Kein Speicher | 1=SBB | 2=SBK | 3=SBS","1=Mit HUV  | 2=Mit Pumpen","1= Pfannendach | 2 = Welldach | 3 = Flachdach/Wand","1=senkr. nebeneinander | 2=waag. nebeneinander | 3=waag. Übereinander | 4=senkr. übereinander","1=Standard | 2=Schnellbefestigung I 3=mit Aufständerung","1=Regelung integriert  |  2=Pumpengruppe Regelung getrennt"," 1 - 16",null,{"$f":"VLOOKUP(K2,Preisliste!$B:$C,2,FALSE)","v":"Solar flat-plate collector SOL 27 premium S"},{"$f":"VLOOKUP(L2,Preisliste!$B:$C,2,FALSE)","v":"Solar flat-plate collector SOL 27 premium W"},{"$f":"VLOOKUP(M2,Preisliste!$B:$C,2,FALSE)","v":"Quick-connector SOL SBP-S"},{"$f":"VLOOKUP(N2,Preisliste!$B:$C,2,FALSE)","v":"Quick-connector SOL SBP-W"},{"$f":"VLOOKUP(O2,Preisliste!$B:$C,2,FALSE)","v":"Quick-connector SOL SBP-WE"},{"$f":"VLOOKUP(P2,Preisliste!$B:$C,2,FALSE)","v":"Mounting frame SOL R1"},{"$f":"VLOOKUP(Q2,Preisliste!$B:$C,2,FALSE)","v":"Mounting frame SOL R2"},{"$f":"VLOOKUP(R2,Preisliste!$B:$C,2,FALSE)","v":"Mounting frame SOL R1 W"},{"$f":"VLOOKUP(S2,Preisliste!$B:$C,2,FALSE)","v":"Frame connection set SOL RV"},{"$f":"VLOOKUP(T2,Preisliste!$B:$C,2,FALSE)","v":"Frame connection set SOL RV-W"},{"$f":"VLOOKUP(U2,Preisliste!$B:$C,2,FALSE)","v":"Fixing Kit - tiled roof SOL BP"},{"$f":"VLOOKUP(V2,Preisliste!$B:$C,2,FALSE)","v":"Frame support SOL RA"},{"$f":"VLOOKUP(W2,Preisliste!$B:$C,2,FALSE)","v":"Frame connection set SOL RV-W"},{"$f":"VLOOKUP(X2,Preisliste!$B:$C,2,FALSE)","v":"Fixing Kit - corrugated roof SOL BW"},{"$f":"VLOOKUP(Y2,Preisliste!$B:$C,2,FALSE)","v":"Mounting kit flat roof SOL BF-S"},{"$f":"VLOOKUP(Z2,Preisliste!$B:$C,2,FALSE)","v":"Mounting kit flat roof SOL BF-W"},{"$f":"VLOOKUP(AA2,Preisliste!$B:$C,2,FALSE)","v":"Fixing kit - shingle roof SOL BS"},{"$f":"VLOOKUP(AB2,Preisliste!$B:$C,2,FALSE)","v":"Fixing kit - plain tile roof SOL BB"},{"$f":"VLOOKUP(AC2,Preisliste!$B:$C,2,FALSE)","v":"Fixing kit - plain tile roof SOL BB-Cu"},{"$f":"VLOOKUP(AD2,Preisliste!$B:$C,2,FALSE)","v":"Push-fit connection SOL SV-A"},{"$f":"VLOOKUP(AE2,Preisliste!$B:$C,2,FALSE)","v":"Push-fit connection SOL SV-A50"},{"$f":"VLOOKUP(AF2,Preisliste!$B:$C,2,FALSE)","v":"Push-fit connection SOL SV-F"},{"$f":"VLOOKUP(AG2,Preisliste!$B:$C,2,FALSE)","v":"Push-fit connection SOL SV-D"},{"$f":"VLOOKUP(AH2,Preisliste!$B:$C,2,FALSE)","v":"Solar flat-plate collector SOL 27 Basic S"},{"$f":"VLOOKUP(AI2,Preisliste!$B:$C,2,FALSE)","v":"Solar flat-plate collector SOL 27 Basic W"},{"$f":"VLOOKUP(AJ2,Preisliste!$B:$C,2,FALSE)","v":"Quick-connector SOL SBP-S"},{"$f":"VLOOKUP(AK2,Preisliste!$B:$C,2,FALSE)","v":"Quick-connector SOL SBP-W"},{"$f":"VLOOKUP(AL2,Preisliste!$B:$C,2,FALSE)","v":"Quick-connector SOL SBP-WE"},{"$f":"VLOOKUP(AM2,Preisliste!$B:$C,2,FALSE)","v":"Mounting frame SOL R1"},{"$f":"VLOOKUP(AN2,Preisliste!$B:$C,2,FALSE)","v":"Mounting frame SOL R2"},{"$f":"VLOOKUP(AO2,Preisliste!$B:$C,2,FALSE)","v":"Mounting frame SOL R1 W"},{"$f":"VLOOKUP(AP2,Preisliste!$B:$C,2,FALSE)","v":"Frame connection set SOL RV"},{"$f":"VLOOKUP(AQ2,Preisliste!$B:$C,2,FALSE)","v":"Fixing Kit - tiled roof SOL BP"},{"$f":"VLOOKUP(AR2,Preisliste!$B:$C,2,FALSE)","v":"Frame support SOL RA"},{"$f":"VLOOKUP(AS2,Preisliste!$B:$C,2,FALSE)","v":"Frame connection set SOL RV-W"},{"$f":"VLOOKUP(AT2,Preisliste!$B:$C,2,FALSE)","v":"Fixing Kit - corrugated roof SOL BW"},{"$f":"VLOOKUP(AU2,Preisliste!$B:$C,2,FALSE)","v":"Mounting kit flat roof SOL BF-S"},{"$f":"VLOOKUP(AV2,Preisliste!$B:$C,2,FALSE)","v":"Mounting kit flat roof SOL BF-W"},{"$f":"VLOOKUP(AW2,Preisliste!$B:$C,2,FALSE)","v":"Fixing kit - shingle roof SOL BS"},{"$f":"VLOOKUP(AX2,Preisliste!$B:$C,2,FALSE)","v":"Fixing kit - plain tile roof SOL BB"},{"$f":"VLOOKUP(AY2,Preisliste!$B:$C,2,FALSE)","v":"Fixing kit - plain tile roof SOL BB-Cu"},{"$f":"VLOOKUP(AZ2,Preisliste!$B:$C,2,FALSE)","v":"Push-fit connection SOL SV-A"},{"$f":"VLOOKUP(BA2,Preisliste!$B:$C,2,FALSE)","v":"Push-fit connection SOL SV-D"},{"$f":"VLOOKUP(BB2,Preisliste!$B:$C,2,FALSE)","v":"Collector sensor pocket KTH basic"},{"$f":"VLOOKUP(BC2,Preisliste!$B:$C,2,FALSE)","v":"Corrugated stainless steel hose"},{"$f":"VLOOKUP(BD2,Preisliste!$B:$C,2,FALSE)","v":"Quick-action air vent valve SOL SE"},{"$f":"VLOOKUP(BE2,Preisliste!$B:$C,2,FALSE)","v":"Solar flat-plate collector SOL 23 premium"},{"$f":"VLOOKUP(BF2,Preisliste!$B:$C,2,FALSE)","v":"Side cover set SOL AS"},{"$f":"VLOOKUP(BG2,Preisliste!$B:$C,2,FALSE)","v":"Push-fit connection SOL SV-I"},{"$f":"VLOOKUP(BH2,Preisliste!$B:$C,2,FALSE)","v":"Push-fit connection SOL SV-R"},{"$f":"VLOOKUP(BI2,Preisliste!$B:$C,2,FALSE)","v":"Side flashing SOL AZ"},{"$f":"VLOOKUP(BJ2,Preisliste!$B:$C,2,FALSE)","v":"Corrugated stainless steel hose"},{"$f":"VLOOKUP(BK2,Preisliste!$B:$C,2,FALSE)","v":"Flexible solar pipe SFR 15, DN 20 15m"},{"$f":"VLOOKUP(BL2,Preisliste!$B:$C,2,FALSE)","v":"Solar compact installation SOKI E trend"},{"$f":"VLOOKUP(BM2,Preisliste!$B:$C,2,FALSE)","v":"Solar compact installation SOKI 7 E trend"},{"$f":"VLOOKUP(BN2,Preisliste!$B:$C,2,FALSE)","v":"Solar compact installation SOKI 7 E trend"},{"$f":"VLOOKUP(BO2,Preisliste!$B:$C,2,FALSE)","v":"Solar compact installation SOKI E premium"},{"$f":"VLOOKUP(BP2,Preisliste!$B:$C,2,FALSE)","v":"Solar control unit SOM 7 E Plus"},{"$f":"VLOOKUP(BQ2,Preisliste!$B:$C,2,FALSE)","v":"Solar control unit SOM 7 E Plus"},{"$f":"VLOOKUP(BR2,Preisliste!$B:$C,2,FALSE)","v":"Solar control unit SOM 8 plus"},{"$f":"VLOOKUP(BS2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder KS 150 SOL"},{"$f":"VLOOKUP(BT2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 300 plus"},{"$f":"VLOOKUP(BU2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 400 plus"},{"$f":"VLOOKUP(BV2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 600 plus"},{"$f":"VLOOKUP(BW2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 300 Trend"},{"$f":"VLOOKUP(BX2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 400 Trend"},{"$f":"VLOOKUP(BY2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 500 Trend"},{"$f":"VLOOKUP(BZ2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 751 SOL"},{"$f":"VLOOKUP(CA2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 1001 SOL"},{"$f":"VLOOKUP(CB2,Preisliste!$B:$C,2,FALSE)","v":"Thermal insulation WDH 751 SBB"},{"$f":"VLOOKUP(CC2,Preisliste!$B:$C,2,FALSE)","v":"Thermal insulation WDH 1001 SBB"},{"$f":"VLOOKUP(CD2,Preisliste!$B:$C,2,FALSE)","v":"Loading station WTS 30 E"},{"$f":"VLOOKUP(CE2,Preisliste!$B:$C,2,FALSE)","v":"Loading station WTS 40 E"},{"$f":"VLOOKUP(CF2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 401 WP SOL"},{"$f":"VLOOKUP(CG2,Preisliste!$B:$C,2,FALSE)","v":"Warm water cylinder SBB 501 WP SOL"},{"$f":"VLOOKUP(CH2,Preisliste!$B:$C,2,FALSE)","v":"Buffer cylinder SBP 700 E SOL"},{"$f":"VLOOKUP(CI2,Preisliste!$B:$C,2,FALSE)","v":"Buffer cylinder SBP 1000 E SOL"},{"$f":"VLOOKUP(CJ2,Preisliste!$B:$C,2,FALSE)","v":"Thermal insulation WDH 1000 SBP"},{"$f":"VLOOKUP(CK2,Preisliste!$B:$C,2,FALSE)","v":"Buffer cylinder SBP 1500 E SOL"},{"$f":"VLOOKUP(CL2,Preisliste!$B:$C,2,FALSE)","v":"Thermal insulation WDH 1500 SBP"},{"$f":"VLOOKUP(CM2,Preisliste!$B:$C,2,FALSE)","v":"Combi cylinder SBK 600/150"},{"$f":"VLOOKUP(CN2,Preisliste!$B:$C,2,FALSE)","v":"Instantaneous cylinder SBS 601 W SOL"},{"$f":"VLOOKUP(CO2,Preisliste!$B:$C,2,FALSE)","v":"Instantaneous cylinder SBS 801 W SOL"},{"$f":"VLOOKUP(CP2,Preisliste!$B:$C,2,FALSE)","v":"Instantaneous cylinder SBS 1001 W SOL"},{"$f":"VLOOKUP(CQ2,Preisliste!$B:$C,2,FALSE)","v":"Instantaneous cylinder SBS 1501 W SOL"},{"$f":"VLOOKUP(CR2,Preisliste!$B:$C,2,FALSE)","v":"Thermal insulation WDH 601 SBS"},{"$f":"VLOOKUP(CS2,Preisliste!$B:$C,2,FALSE)","v":"Thermal insulation WDH 801 SBS"},{"$f":"VLOOKUP(CT2,Preisliste!$B:$C,2,FALSE)","v":"Thermal insulation WDH 1001 SBS"},{"$f":"VLOOKUP(CU2,Preisliste!$B:$C,2,FALSE)","v":"Thermal insulation WDH 1501 SBS"},{"$f":"VLOOKUP(CV2,Preisliste!$B:$C,2,FALSE)","v":"Heat exchanger WT 10"},{"$f":"VLOOKUP(CW2,Preisliste!$B:$C,2,FALSE)","v":"Heat exchanger WT 20"},{"$f":"VLOOKUP(CX2,Preisliste!$B:$C,2,FALSE)","v":"Heat exchanger WT 30"},{"$f":"VLOOKUP(CY2,Preisliste!$B:$C,2,FALSE)","v":"Heat exchanger WT 40"},{"$f":"VLOOKUP(CZ2,Preisliste!$B:$C,2,FALSE)","v":"Heat transfer liquid H30-L, 10 l"},{"$f":"VLOOKUP(DA2,Preisliste!$B:$C,2,FALSE)","v":"Heat transfer liquid H30-L, 20 l"},{"$f":"VLOOKUP(DB2,Preisliste!$B:$C,2,FALSE)","v":"Heat transfer liquid H30-LS, 10 l"},{"$f":"VLOOKUP(DC2,Preisliste!$B:$C,2,FALSE)","v":"Heat transfer liquid H30-LS, 20 l"},{"$f":"VLOOKUP(DD2,Preisliste!$B:$C,2,FALSE)","v":"Three-way diverter valve SUV"},{"$f":"VLOOKUP(DE2,Preisliste!$B:$C,2,FALSE)","v":"Regulating valve with flowmeter"},{"$f":"VLOOKUP(DF2,Preisliste!$B:$C,2,FALSE)","v":"Solar expansion vessel 12 l"},{"$f":"VLOOKUP(DG2,Preisliste!$B:$C,2,FALSE)","v":"Solar expansion vessel 18 l"},{"$f":"VLOOKUP(DH2,Preisliste!$B:$C,2,FALSE)","v":"Solar expansion vessel 25 l"},{"$f":"VLOOKUP(DI2,Preisliste!$B:$C,2,FALSE)","v":"Solar expansion vessel 50 l"},{"$f":"VLOOKUP(DJ2,Preisliste!$B:$C,2,FALSE)","v":"Solar expansion vessel 80 l"},{"$f":"VLOOKUP(DK2,Preisliste!$B:$C,2,FALSE)","v":"DEV connection set AGWH"},{"$f":"VLOOKUP(DL2,Preisliste!$B:$C,2,FALSE)","v":"Heating diverter valve (on side)"}]
["Nutzung","Kollektortyp","Speicher","HUV","Dachform","Anordnung","Befestigung","Regelung","Kollektorzahl","Suchschlüssel",230016,230017,231980,231981,231982,230169,230170,230920,230171,230172,230175,230173,230172,231998,230177,230178,230189,230190,230191,230185,231322,230913,230186,228927,230912,231980,231981,231982,230169,230170,230920,230171,230175,230173,230172,231998,230177,230178,230189,230190,230191,230185,230186,229322,73469,231898,230020,230184,230187,230188,230183,73469,232945,234783,234784,234784,231014,234785,234785,230933,74098,187873,187874,187875,233490,233491,233492,229294,229295,231923,231924,232907,232908,221362,227534,185460,227566,231929,227567,231930,74067,229984,229985,229986,229987,231925,231926,231927,231928,70633,70634,71091,229338,73221,73222,74099,74100,231900,74244,74029,74030,74031,187868,231899,231905,"------"]
[1,1,1,1,1,1,1,1,1,{"$f":"A3&B3&C3&D3&E3&F3&G3&H3&I3","v":"111111111"},1,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,1,1,1,2,{"$f":"A4&B4&C4&D4&E4&F4&G4&H4&I4","v":"111111112"},2,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,1,1,3,"111111113",3,null,null,null,null,1,1,null,1,null,3,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null," ",1,null,null,1]
[1,1,1,1,1,1,1,1,4,"111111114",4,null,null,null,null,null,2,null,1,null,4,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,1,5,"111111115",5,null,null,null,null,1,2,null,2,null,5,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,1,6,"111111116",6,null,null,null,null,2,2,null,2,null,6,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,1,8,"111111118",8,null,null,null,null,null,4,null,2,null,8,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,1,10,"1111111110",10,null,null,null,null,2,4,null,4,null,10,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,1,12,"1111111112",12,null,null,null,null,null,6,null,3,null,12,null,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,1,15,"1111111115",15,null,null,null,null,3,6,null,6,null,15,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,1,16,"1111111116",16,null,null,null,null,null,8,null,4,null,16,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,2,1,"111111121",1,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,1,1,2,2,"111111122",2,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,1,2,3,"111111123",3,null,null,null,null,1,1,null,1,null,3,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,1,2,4,"111111124",4,null,null,null,null,null,2,null,1,null,4,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,2,5,"111111125",5,null,null,null,null,1,2,null,2,null,5,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,2,6,"111111126",6,null,null,null,null,2,2,null,2,null,6,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,2,8,"111111128",8,null,null,null,null,null,4,null,2,null,8,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,2,10,"1111111210",10,null,null,null,null,2,4,null,4,null,10,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,2,12,"1111111212",12,null,null,null,null,null,6,null,3,null,12,null,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,2,15,"1111111215",15,null,null,null,null,3,6,null,6,null,15,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,1,2,16,"1111111216",16,null,null,null,null,null,8,null,4,null,16,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,1,1,"111111211",1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,1,2,1,2,"111111212",2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,2,1,3,"111111213",3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,2,1,4,"111111214",4,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,1,5,"111111215",5,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,1,6,"111111216",6,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,1,8,"111111218",8,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,1,10,"1111112110",10,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,1,12,"1111112112",12,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,1,15,"1111112115",15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,1,16,"1111112116",16,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,2,1,"111111221",1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,1,2,2,2,"111111222",2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,2,2,3,"111111223",3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,2,2,4,"111111224",4,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,2,5,"111111225",5,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,2,6,"111111226",6,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,2,8,"111111228",8,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,2,10,"1111112210",10,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,2,12,"1111112212",12,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,2,15,"1111112215",15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,2,2,16,"1111112216",16,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,1,1,"111111311",1,null,null,null,null,1,null,null,null,null,2,2,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,1,3,1,2,"111111312",2,null,null,null,null,null,1,null,null,null,2,2,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,3,1,3,"111111313",3,null,null,null,null,1,1,null,1,null,3,3,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,3,1,4,"111111314",4,null,null,null,null,null,2,null,1,null,4,4,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,1,5,"111111315",5,null,null,null,null,1,2,null,2,null,5,5,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,1,6,"111111316",6,null,null,null,null,2,2,null,2,null,6,6,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,1,8,"111111318",8,null,null,null,null,null,4,null,2,null,8,8,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,1,10,"1111113110",10,null,null,null,null,2,4,null,4,null,10,10,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,1,12,"1111113112",12,null,null,null,null,null,6,null,3,null,12,12,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,1,15,"1111113115",15,null,null,null,null,3,6,null,6,null,15,15,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,1,16,"1111113116",16,null,null,null,null,null,8,null,4,null,16,16,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,2,1,"111111321",1,null,null,null,null,1,null,null,null,null,2,2,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,1,3,2,2,"111111322",2,null,null,null,null,null,1,null,null,null,2,2,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,3,2,3,"111111323",3,null,null,null,null,1,1,null,1,null,3,3,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,1,3,2,4,"111111324",4,null,null,null,null,null,2,null,1,null,4,4,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,2,5,"111111325",5,null,null,null,null,1,2,null,2,null,5,5,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,2,6,"111111326",6,null,null,null,null,2,2,null,2,null,6,6,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,2,8,"111111328",8,null,null,null,null,null,4,null,2,null,8,8,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,2,10,"1111113210",10,null,null,null,null,2,4,null,4,null,10,10,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,2,12,"1111113212",12,null,null,null,null,null,6,null,3,null,12,12,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,2,15,"1111113215",15,null,null,null,null,3,6,null,6,null,15,15,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,1,3,2,16,{"$f":"A68&B68&C68&D68&E68&F68&G68&H68&I68","v":"1111113216"},16,null,null,null,null,null,8,null,4,null,16,16,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,1,1,"111112111",null,1,null,null,null,null,null,1,null,null,2,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,2,1,1,2,"111112112",null,2,null,null,null,null,null,2,1,null,4,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,1,1,3,"111112113",null,3,null,null,null,null,null,3,2,null,6,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,1,1,4,"111112114",null,4,null,null,null,null,null,4,3,null,8,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,1,5,"111112115",null,5,null,null,null,null,null,5,4,null,10,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,1,6,"111112116",null,6,null,null,null,null,null,6,4,null,12,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,1,8,"111112118",null,8,null,null,null,null,null,8,6,null,16,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,1,10,"1111121110",null,10,null,null,null,null,null,10,8,null,20,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,1,12,"1111121112",null,12,null,null,null,null,null,12,9,null,24,null,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,1,15,"1111121115",null,15,null,null,null,null,null,15,12,null,30,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,1,16,"1111121116",null,16,null,null,null,null,null,16,12,null,32,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,2,1,"111112121",null,1,null,null,null,null,null,1,null,null,2,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,2,1,2,2,"111112122",null,2,null,null,null,null,null,2,1,null,4,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,1,2,3,"111112123",null,3,null,null,null,null,null,3,2,null,6,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,1,2,4,"111112124",null,4,null,null,null,null,null,4,3,null,8,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,2,5,"111112125",null,5,null,null,null,null,null,5,4,null,10,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,2,6,"111112126",null,6,null,null,null,null,null,6,4,null,12,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,2,8,"111112128",null,8,null,null,null,null,null,8,6,null,16,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,2,10,"1111121210",null,10,null,null,null,null,null,10,8,null,20,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,2,12,"1111121212",null,12,null,null,null,null,null,12,9,null,24,null,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,2,15,"1111121215",null,15,null,null,null,null,null,15,12,null,30,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,1,2,16,"1111121216",null,16,null,null,null,null,null,16,12,null,32,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,1,1,"111112211",null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,2,2,1,2,"111112212",null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,2,1,3,"111112213",null,3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,2,1,4,"111112214",null,4,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,1,5,"111112215",null,5,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,1,6,"111112216",null,6,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,1,8,"111112218",null,8,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,1,10,"1111122110",null,10,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,1,12,"1111122112",null,12,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,1,15,"1111122115",null,15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,1,16,"1111122116",null,16,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,2,1,"111112221",null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,2,2,2,2,"111112222",null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,2,2,3,"111112223",null,3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,2,2,4,"111112224",null,4,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,2,5,"111112225",null,5,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,2,6,"111112226",null,6,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,2,8,"111112228",null,8,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,2,10,"1111122210",null,10,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,2,12,"1111122212",null,12,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,2,15,"1111122215",null,15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,2,2,16,"1111122216",null,16,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,1,1,"111112311",null,1,null,null,null,null,null,1,null,null,2,2,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,2,3,1,2,"111112312",null,2,null,null,null,null,null,2,1,null,4,4,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,3,1,3,"111112313",null,3,null,null,null,null,null,3,2,null,6,6,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,3,1,4,"111112314",null,4,null,null,null,null,null,4,3,null,8,8,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,1,5,"111112315",null,5,null,null,null,null,null,5,4,null,10,10,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,1,6,"111112316",null,6,null,null,null,null,null,6,4,null,12,12,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,1,8,"111112318",null,8,null,null,null,null,null,8,6,null,16,16,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,1,10,"1111123110",null,10,null,null,null,null,null,10,8,null,20,20,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,1,12,"1111123112",null,12,null,null,null,null,null,12,9,null,24,14,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,1,15,"1111123115",null,15,null,null,null,null,null,15,12,null,30,30,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,1,16,"1111123116",null,16,null,null,null,null,null,16,12,null,32,32,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,2,1,"111112321",null,1,null,null,null,null,null,1,null,null,2,2,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,2,3,2,2,"111112322",null,2,null,null,null,null,null,2,1,null,4,4,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,3,2,3,"111112323",null,3,null,null,null,null,null,3,2,null,6,6,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,2,3,2,4,"111112324",null,4,null,null,null,null,null,4,3,null,8,8,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,2,5,"111112325",null,5,null,null,null,null,null,5,4,null,10,10,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,2,6,"111112326",null,6,null,null,null,null,null,6,4,null,12,12,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,2,8,"111112328",null,8,null,null,null,null,null,8,6,null,16,16,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,2,10,"1111123210",null,10,null,null,null,null,null,10,8,null,20,20,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,2,12,{"$f":"A132&B132&C132&D132&E132&F132&G132&H132&I132","v":"1111123212"},null,12,null,null,null,null,null,12,9,null,24,14,null,null,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,2,15,"1111123215",null,15,null,null,null,null,null,15,12,null,30,30,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,2,3,2,16,"1111123216",null,16,null,null,null,null,null,16,12,null,32,32,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,1,1,"111113111",1,null,null,null,null,null,null,1,null,null,2,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,3,1,1,2,"111113112",2,null,null,null,null,null,null,2,null,1,3,null,null,null,null,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,3,1,1,3,"111113113",3,null,null,null,null,null,null,3,null,2,4,null,null,null,null,null,null,null,null,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,3,1,1,4,"111113114",4,null,null,null,null,null,null,4,null,3,5,null,null,null,null,null,null,null,null,null,3,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,1,5,"111113115",5,null,null,null,null,null,null,5,null,4,6,null,null,null,null,null,null,null,null,null,4,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,1,6,"111113116",6,null,null,null,null,null,null,6,null,4,7,null,null,null,null,null,null,null,null,null,4,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,1,8,"111113118",8,null,null,null,null,null,null,8,null,6,9,null,null,null,null,null,null,null,null,null,6,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,1,10,"1111131110",10,null,null,null,null,null,null,10,null,8,12,null,null,null,null,null,null,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,1,12,"1111131112",12,null,null,null,null,null,null,12,null,9,15,null,null,null,null,null,null,null,null,null,9,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,1,15,"1111131115",15,null,null,null,null,null,null,15,null,12,18,null,null,null,null,null,null,null,null,null,12,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,1,16,"1111131116",16,null,null,null,null,null,null,16,null,12,20,null,null,null,null,null,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,2,1,"111113121",1,null,null,null,null,null,null,1,null,null,2,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,3,1,2,2,"111113122",2,null,null,null,null,null,null,2,null,1,3,null,null,null,null,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,3,1,2,3,"111113123",3,null,null,null,null,null,null,3,null,2,4,null,null,null,null,null,null,null,null,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,3,1,2,4,"111113124",4,null,null,null,null,null,null,4,null,3,5,null,null,null,null,null,null,null,null,null,3,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,2,5,"111113125",5,null,null,null,null,null,null,5,null,4,6,null,null,null,null,null,null,null,null,null,4,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,2,6,"111113126",6,null,null,null,null,null,null,6,null,4,7,null,null,null,null,null,null,null,null,null,4,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,2,8,"111113128",8,null,null,null,null,null,null,8,null,6,9,null,null,null,null,null,null,null,null,null,6,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,2,10,"1111131210",10,null,null,null,null,null,null,10,null,8,12,null,null,null,null,null,null,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,2,12,"1111131212",12,null,null,null,null,null,null,12,null,9,15,null,null,null,null,null,null,null,null,null,9,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,2,15,"1111131215",15,null,null,null,null,null,null,15,null,12,18,null,null,null,null,null,null,null,null,null,12,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,1,2,16,"1111131216",16,null,null,null,null,null,null,16,null,12,20,null,null,null,null,null,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,1,1,"111113211",1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,3,2,1,2,"111113212",2,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,3,2,1,3,"111113213",3,null,null,1,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,3,2,1,4,"111113214",4,null,null,1,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,1,5,"111113215",5,null,null,1,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,1,6,"111113216",6,null,null,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,1,8,"111113218",8,null,null,2,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,1,10,"1111132110",10,null,null,2,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,1,12,"1111132112",12,null,null,3,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,1,15,"1111132115",15,null,null,3,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,1,16,"1111132116",16,null,null,4,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,2,1,"111113221",1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,1,3,2,2,2,"111113222",2,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,3,2,2,3,"111113223",3,null,null,1,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,1,3,2,2,4,"111113224",4,null,null,1,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,2,5,"111113225",5,null,null,1,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,2,6,"111113226",6,null,null,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,2,8,"111113228",8,null,null,2,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,2,10,"1111132210",10,null,null,2,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,2,12,"1111132212",12,null,null,3,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,2,15,"1111132215",15,null,null,3,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,2,2,16,"1111132216",16,null,null,4,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,1,3,3,1,1,"111113311",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,2,"111113312",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,3,"111113313",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,4,"111113314",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,5,"111113315",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,6,"111113316",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,8,"111113318",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,10,"1111133110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,12,"1111133112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,15,"1111133115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,1,16,"1111133116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,1,"111113321",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,2,"111113322",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,3,"111113323",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,4,"111113324",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,5,"111113325",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,6,"111113326",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,8,{"$f":"A196&B196&C196&D196&E196&F196&G196&H196&I196","v":"111113328"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,10,"1111133210",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,12,"1111133212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,15,"1111133215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,1,3,3,2,16,"1111133216",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[1,1,1,1,2,1,1,1,1,"111121111",1,null,null,null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,2,1,1,1,2,"111121112",2,null,null,null,null,null,1,null,null,null,null,null,null,2,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,1,1,1,3,"111121113",3,null,null,null,null,1,1,null,1,null,null,null,null,3,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,1,1,1,4,"111121114",4,null,null,null,null,null,2,null,1,null,null,null,null,4,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,1,5,"111121115",5,null,null,null,null,1,2,null,2,null,null,null,null,5,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,1,6,"111121116",6,null,null,null,null,2,2,null,2,null,null,null,null,6,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,1,8,"111121118",8,null,null,null,null,null,4,null,2,null,null,null,null,8,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,1,10,"1111211110",10,null,null,null,null,2,4,null,4,null,null,null,null,10,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,1,12,"1111211112",12,null,null,null,null,null,6,null,3,null,null,null,null,12,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,1,15,"1111211115",15,null,null,null,null,3,6,null,6,null,null,null,null,15,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,1,16,"1111211116",16,null,null,null,null,null,8,null,4,null,null,null,null,16,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,2,1,"111121121",1,null,null,null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,2,1,1,2,2,"111121122",2,null,null,null,null,null,1,null,null,null,null,null,null,2,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,1,1,2,3,"111121123",3,null,null,null,null,1,1,null,1,null,null,null,null,3,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,1,1,2,4,"111121124",4,null,null,null,null,null,2,null,1,null,null,null,null,4,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,2,5,"111121125",5,null,null,null,null,1,2,null,2,null,null,null,null,5,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,2,6,"111121126",6,null,null,null,null,2,2,null,2,null,null,null,null,6,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,2,8,"111121128",8,null,null,null,null,null,4,null,2,null,null,null,null,8,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,2,10,"1111211210",10,null,null,null,null,2,4,null,4,null,null,null,null,10,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,2,12,"1111211212",12,null,null,null,null,null,6,null,3,null,null,null,null,12,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,2,15,"1111211215",15,null,null,null,null,3,6,null,6,null,null,null,null,15,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,1,2,16,"1111211216",16,null,null,null,null,null,8,null,4,null,null,null,null,16,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,1,1,"111121311",1,null,null,null,null,1,null,null,null,null,null,2,null,2,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,2,1,3,1,2,"111121312",2,null,null,null,null,null,1,null,null,null,null,2,null,2,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,1,3,1,3,"111121313",3,null,null,null,null,1,1,null,1,null,null,3,null,3,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,1,3,1,4,"111121314",4,null,null,null,null,null,2,null,1,null,null,4,null,4,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,1,5,"111121315",5,null,null,null,null,1,2,null,2,null,null,5,null,5,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,1,6,"111121316",6,null,null,null,null,2,2,null,2,null,null,6,null,6,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,1,8,"111121318",8,null,null,null,null,null,4,null,2,null,null,8,null,8,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,1,10,"1111213110",10,null,null,null,null,2,4,null,4,null,null,10,null,10,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,1,12,"1111213112",12,null,null,null,null,null,6,null,3,null,null,12,null,12,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,1,15,"1111213115",15,null,null,null,null,3,6,null,6,null,null,15,null,15,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,1,16,"1111213116",16,null,null,null,null,null,8,null,4,null,null,16,null,16,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,2,1,"111121321",1,null,null,null,null,1,null,null,null,null,null,2,null,2,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,2,1,3,2,2,"111121322",2,null,null,null,null,null,1,null,null,null,null,2,null,2,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,1,3,2,3,"111121323",3,null,null,null,null,1,1,null,1,null,null,3,null,3,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,1,3,2,4,"111121324",4,null,null,null,null,null,2,null,1,null,null,4,null,4,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,2,5,"111121325",5,null,null,null,null,1,2,null,2,null,null,5,null,5,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,2,6,"111121326",6,null,null,null,null,2,2,null,2,null,null,6,null,6,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,2,8,"111121328",8,null,null,null,null,null,4,null,2,null,null,8,null,8,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,2,10,"1111213210",10,null,null,null,null,2,4,null,4,null,null,10,null,10,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,2,12,"1111213212",12,null,null,null,null,null,6,null,3,null,null,12,null,12,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,2,15,"1111213215",15,null,null,null,null,3,6,null,6,null,null,15,null,15,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,1,3,2,16,"1111213216",16,null,null,null,null,null,8,null,4,null,null,16,null,16,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,1,1,1,2,2,1,1,1,"111122111",null,1,null,null,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,2,2,1,1,2,"111122112",null,2,null,null,null,null,null,2,1,null,null,null,null,4,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,2,1,1,3,"111122113",null,3,null,null,null,null,null,3,2,null,null,null,null,6,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,2,1,1,4,"111122114",null,4,null,null,null,null,null,4,3,null,null,null,null,8,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,1,1,1,2,2,1,1,5,"111122115",null,5,null,null,null,null,null,5,4,null,null,null,null,10,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,2,1,1,6,"111122116",null,6,null,null,null,null,null,6,4,null,null,null,null,12,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,2,2,1,2,2,"111122122",null,2,null,null,null,null,null,2,1,null,null,null,null,4,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,1,1,1,2,3,1,2,1,"111123121",1,null,null,null,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,1,1,1,2,3,1,2,12,"1111231212",12,null,null,null,null,null,null,12,9,null,null,null,null,12,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[1,1,1,1,3,1,1,1,6,"111131116",6,null,null,null,null,2,2,null,2,null,null,null,null,null,6,null,null,null,null,4,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,1,1,1,3,2,1,2,4,"111132124",null,4,null,null,null,null,null,4,3,null,null,null,null,null,null,8,null,null,null,3,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,2,1,1,1,1,2,1,15,"1211112115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[1,2,1,1,1,1,3,1,4,"121111314",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,2,null,1,4,4,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,1]
[1,2,1,1,1,2,1,2,5,"121112125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,5,4,10,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[1,2,1,1,1,2,3,1,3,"121112313",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,3,2,6,6,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[1,2,1,1,2,1,1,1,16,"1211211116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,null,null,8,null,4,null,null,null,8,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,2,1,1,2,1,3,1,2,"121121312",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,1,null,null,null,2,null,2,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[1,2,1,1,2,2,3,1,1,"121122311",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,2,null,2,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,2,1,1,2,2,3,1,6,{"$f":"A580&B580&C580&D580&E580&F580&G580&H580&I580","v":"121122316"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,6,4,null,12,null,12,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[1,2,1,1,3,1,1,2,16,"1211311216",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,null,null,8,null,4,null,null,null,null,16,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,1]
[1,3,1,1,1,1,1,1,1,"131111111",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[1,3,1,1,1,4,1,2,15,"1311141215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,1]
[2,1,1,1,1,1,1,2,4,"211111124",4,null,null,null,null,null,2,null,1,null,4,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,1]
[2,1,1,1,1,1,3,1,2,"211111312",2,null,null,null,null,null,1,null,null,null,2,2,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,1]
[2,1,1,1,1,2,1,2,10,"2111121210",null,10,null,null,null,null,null,10,8,null,20,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,1,null,null,null,null,null,1]
[2,1,1,1,1,2,2,2,10,"2111122210",null,10,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,1,null,null,null,null,null,1]
[2,1,1,1,1,2,3,2,2,"211112322",null,2,null,null,null,null,null,2,1,null,4,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,1]
[2,1,1,1,1,3,2,2,1,"211113221",1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,1]
[2,1,1,1,1,3,3,2,12,"2111133212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[2,1,1,1,2,1,1,1,16,"2111211116",16,null,null,null,null,null,8,null,4,null,null,null,null,16,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,null,1,null,1]
[2,1,1,1,2,1,3,1,12,"2111213112",12,null,null,null,null,null,6,null,3,null,null,12,null,6,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1,null,1]
[2,1,1,1,2,2,3,1,15,"2111223115",null,15,null,null,null,null,null,15,12,null,null,30,null,30,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1,null,1]
[2,1,1,1,2,3,1,1,12,"2111231112",12,null,null,null,null,null,null,12,9,null,null,null,null,15,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1,null,1]
[2,1,1,1,2,3,3,1,15,"2111233115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[2,1,1,1,3,2,1,1,10,"2111321110",null,10,null,null,null,null,null,10,8,null,null,null,null,null,null,20,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,1,null,null,null,null,null,1]
[2,1,1,2,1,1,1,1,5,"211211115",5,null,null,null,null,1,2,null,2,null,5,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[2,1,1,2,1,1,2,1,2,"211211212",2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,1,2,1,1,3,1,1,"211211311",1,null,null,null,null,1,null,null,null,null,2,2,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,1,2,1,2,2,1,6,"211212216",null,6,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[2,1,1,2,1,2,2,2,16,"2112122216",null,16,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,null,1]
[2,1,1,2,1,3,1,2,10,"2112131210",10,null,null,null,null,null,null,10,null,8,12,null,null,null,null,null,null,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[2,1,1,2,1,3,2,2,15,"2112132215",15,null,null,3,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[2,1,1,2,1,3,3,2,12,"2112133212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[2,1,1,2,2,1,1,2,8,"211221128",8,null,null,null,null,null,4,null,2,null,null,null,null,8,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,null,1]
[2,1,1,2,2,1,3,2,3,"211221323",3,null,null,null,null,1,1,null,1,null,null,3,null,3,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,1,2,2,2,3,1,12,"2112223112",null,12,null,null,null,null,null,12,9,null,null,14,null,24,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[2,1,1,2,2,3,1,2,2,"211223122",2,null,null,null,null,null,null,2,1,null,null,null,null,2,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,1,2,2,3,3,2,1,"211223321",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[2,1,1,2,3,2,1,2,3,"211232123",null,3,null,null,null,null,null,3,2,null,null,null,null,null,null,6,null,null,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,2,1,1,1,1,1,16,"2121111116",16,null,null,null,null,null,8,null,4,null,16,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,1,5,null,null,1,null,null,null,null,null,1]
[2,1,2,1,1,2,2,1,5,"212112215",null,5,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,1,null,null,null,null,1]
[2,1,2,1,1,3,1,1,15,"2121131115",15,null,null,null,null,null,null,15,null,12,18,null,null,null,null,null,null,null,null,null,12,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,1,null,null,null,null,null,1]
[2,1,2,1,1,3,3,1,12,"2121133112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[2,1,2,1,2,1,1,1,16,"2121211116",16,null,null,null,null,null,8,null,4,null,null,null,null,16,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,1,5,null,null,1,null,null,null,null,null,1]
[2,1,2,1,2,2,3,1,3,"212122313",null,3,null,null,null,null,null,3,2,null,null,6,null,6,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,1,null,null,null,null,1]
[2,1,2,1,3,1,1,1,6,"212131116",6,null,null,null,null,2,2,null,2,null,null,null,null,null,6,null,null,null,null,4,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,1,null,null,null,null,1]
[2,1,3,1,1,1,1,2,2,"213111122",2,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,3,1,1,1,3,1,1,"213111311",1,null,null,null,null,1,null,null,null,null,2,2,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,3,1,1,2,1,2,6,"213112126",null,6,null,null,null,null,null,6,4,null,12,null,null,null,null,null,null,null,null,2,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,3,1,1,2,2,1,16,"2131122116",null,16,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[2,1,3,1,1,3,1,1,2,"213113112",2,null,null,null,null,null,null,2,null,1,3,null,null,null,null,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,3,1,1,3,2,1,15,"2131132115",15,null,null,3,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[2,1,3,1,1,3,2,2,2,"213113222",2,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,3,1,2,1,1,1,12,"2131211112",12,null,null,null,null,null,6,null,3,null,null,null,null,12,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[2,1,3,1,2,1,3,1,3,"213121313",3,null,null,null,null,1,1,null,1,null,null,3,null,3,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,3,1,2,2,1,2,3,"213122123",null,3,null,null,null,null,null,3,2,null,null,null,null,6,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,3,1,2,3,1,1,8,"213123118",8,null,null,null,null,null,null,8,6,null,null,null,null,8,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,null,1]
[2,1,3,1,2,3,3,1,12,"2131233112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[2,1,3,1,3,1,1,1,1,"213131111",1,null,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,1,3,1,3,2,1,2,16,"2131321216",null,16,null,null,null,null,null,16,12,null,null,null,null,null,null,32,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[2,2,1,1,1,1,2,1,15,"2211112115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1,null,1]
[2,2,1,1,1,1,2,2,15,"2211112215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1,null,1]
[2,2,1,1,1,2,2,1,5,"221112215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,1,null,null,null,null,1]
[2,2,1,1,1,2,2,2,12,"2211122212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1,null,1]
[2,2,1,1,1,2,3,2,10,"2211123210",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,null,10,8,20,20,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,1,null,null,null,null,null,1]
[2,2,1,1,2,1,1,2,16,"2211211216",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,null,null,8,null,4,null,null,null,8,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,null,1,null,1]
[2,2,1,1,2,2,1,2,8,"221122128",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,8,6,null,null,null,16,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,1,null,null,null,null,null,1]
[2,2,1,1,2,2,3,2,6,"221122326",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,6,4,null,12,null,12,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,1,null,null,null,null,1]
[2,2,1,1,3,1,1,2,1,"221131121",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,1]
[2,2,1,2,1,1,1,2,5,"221211125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,1,2,null,2,5,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,1]
[2,2,1,2,1,1,2,2,8,"221211228",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,null,1]
[2,2,1,2,1,1,3,1,15,"2212113115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,3,6,null,6,15,15,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[2,2,1,2,1,2,2,2,2,"221212222",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,2,1,2,1,2,3,1,12,"2212123112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,12,9,24,24,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[2,2,1,2,2,1,1,1,10,"2212211110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,2,4,null,4,null,null,null,6,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[2,2,1,2,2,1,3,1,10,"2212213110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,2,4,null,4,null,10,null,6,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[2,2,1,2,2,2,3,1,8,"221222318",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,8,6,null,16,null,16,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,null,1]
[2,2,1,2,2,2,3,2,15,"2212223215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,15,12,null,30,null,30,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,1]
[2,2,1,2,3,2,1,1,1,{"$f":"A2500&B2500&C2500&D2500&E2500&F2500&G2500&H2500&I2500","v":"221232111"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,2,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,2,2,1,1,1,3,1,5,"222111315",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,1,2,null,2,5,5,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,1,null,null,null,null,1]
[2,2,2,1,1,2,2,1,4,"222112214",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,1,null,null,null,null,1]
[2,2,2,1,1,2,3,1,15,"2221123115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,15,12,30,30,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,1,null,null,null,null,null,1]
[2,2,2,1,2,2,3,1,6,"222122316",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,6,4,null,12,null,12,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,1,null,null,null,null,1]
[2,2,2,1,3,2,1,1,12,"2221321112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,12,9,null,null,null,null,null,24,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,1,4,null,null,1,null,null,null,null,null,1]
[2,2,3,1,1,1,1,2,10,"2231111210",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,2,4,null,4,10,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[2,2,3,1,1,1,3,2,8,"223111328",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,4,null,3,8,8,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,null,1]
[2,2,3,1,1,2,1,2,8,"223112128",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,8,7,16,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,null,1]
[2,2,3,1,1,2,2,1,8,"223112218",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,null,1]
[2,2,3,1,1,2,3,2,1,"223112321",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,2,2,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,2,3,1,2,1,3,2,5,"223121325",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,1,2,null,2,null,5,null,5,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,2,3,1,2,2,1,1,10,"2231221110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,null,10,8,null,null,null,20,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[2,2,3,1,2,2,3,1,15,"2231223115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,15,12,null,30,null,30,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,1,3,null,null,null,null,null,null,null,null,1]
[2,2,3,1,3,2,1,1,3,"223132113",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,3,2,null,null,null,null,null,6,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,3,1,1,1,1,1,1,12,"2311111112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,3,9,null,null,3,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,1]
[2,3,1,1,1,4,1,1,10,"2311141110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,2,8,null,5,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,1,null,null,null,null,null,1]
[2,3,1,2,1,4,1,1,4,"231214114",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,2,2,null,2,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[2,3,2,1,1,1,1,1,8,{"$f":"A3012&B3012&C3012&D3012&E3012&F3012&G3012&H3012&I3012","v":"232111118"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,2,6,1,null,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,1]
[2,3,2,1,1,4,1,1,4,"232114114",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,2,2,null,2,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,1,null,null,null,null,1]
[2,3,3,1,1,4,1,1,6,"233114116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,2,4,null,3,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,1]
[3,1,1,1,1,1,1,1,15,"3111111115",15,null,null,null,null,3,6,null,6,null,15,null,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,5,null,null,null,null,null,null,null,null,1,null,1]
[3,1,1,1,1,1,3,1,5,"311111315",5,null,null,null,null,1,2,null,2,null,5,5,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[3,1,1,1,1,1,3,2,15,"3111113215",15,null,null,null,null,3,6,null,6,null,15,15,null,null,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,5,null,null,null,null,null,null,null,null,1,null,1]
[3,1,1,1,1,2,2,1,16,"3111122116",null,16,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,6,null,null,null,null,null,null,null,null,1,null,1]
[3,1,1,1,1,3,1,1,3,"311113113",3,null,null,null,null,null,null,3,null,2,4,null,null,null,null,null,null,null,null,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,1,null,null,1]
[3,1,1,1,1,3,2,1,6,"311113216",6,null,null,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,2,null,null,1,null,null,null,null,1]
[3,1,1,1,1,3,2,2,10,"3111132210",10,null,null,2,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,3,null,null,1,null,null,null,null,null,1]
[3,1,1,1,2,1,1,2,8,"311121128",8,null,null,null,null,null,4,null,2,null,null,null,null,8,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,3,null,null,1,null,null,null,null,null,1]
[3,1,1,1,2,1,3,1,1,"311121311",1,null,null,null,null,1,null,null,null,null,null,2,null,2,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,1,null,null,1,null,null,null,1]
[3,1,1,1,2,2,1,2,6,"311122126",null,6,null,null,null,null,null,6,4,null,null,null,null,12,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,2,null,null,1,null,null,null,null,1]
[3,1,1,1,2,2,3,2,8,"311122328",null,8,null,null,null,null,null,8,6,null,null,16,null,16,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,3,null,null,1,null,null,null,null,null,1]
[3,1,1,1,2,3,3,2,5,"311123325",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[3,1,1,1,3,1,1,2,4,"311131124",4,null,null,null,null,null,2,null,1,null,null,null,null,null,4,null,null,null,null,3,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,1]
[3,1,1,1,3,2,1,2,10,"3111321210",null,10,null,null,null,null,null,10,8,null,null,null,null,null,null,20,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,3,null,null,1,null,null,null,null,null,1]
[3,1,1,2,1,1,2,2,3,"311211223",3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[3,1,1,2,1,1,3,2,3,"311211323",3,null,null,null,null,1,1,null,1,null,3,3,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,1,null,null,1]
[3,1,1,2,1,2,1,1,10,"3112121110",null,10,null,null,null,null,null,10,8,null,20,null,null,null,null,null,null,null,null,2,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,3,null,null,null,null,null,null,null,null,1]
[3,1,1,2,1,2,2,1,8,"311212218",null,8,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[3,1,1,2,1,3,1,2,4,"311213124",4,null,null,null,null,null,null,4,null,3,5,null,null,null,null,null,null,null,null,null,3,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[3,1,1,2,1,3,2,1,6,"311213216",6,null,null,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,2,null,null,null,null,null,null,null,1]
[3,1,1,2,1,3,2,2,16,"3112132216",16,null,null,4,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,6,null,null,null,null,null,null,null,null,1]
[3,1,1,2,2,1,3,1,5,"311221315",5,null,null,null,null,1,2,null,2,null,null,5,null,5,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[3,1,1,2,2,2,1,1,4,"311222114",null,4,null,null,null,null,null,4,3,null,null,null,null,8,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[3,1,1,2,2,2,3,1,5,"311222315",null,5,null,null,null,null,null,5,4,null,null,10,null,10,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[3,1,1,2,2,3,3,1,3,"311223313",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[3,1,1,2,2,3,3,2,8,"311223328",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[3,1,1,2,3,1,1,2,10,"3112311210",10,null,null,null,null,2,4,null,4,null,null,null,null,null,10,null,null,null,null,8,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,3,null,null,null,null,null,null,null,null,1]
[3,1,1,2,3,2,1,2,8,"311232128",null,8,null,null,null,null,null,8,6,null,null,null,null,null,null,16,null,null,null,6,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[3,2,1,1,1,1,3,1,1,"321111311",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,2,2,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,1,null,null,1,null,null,null,1]
[3,2,1,1,1,1,3,2,6,"321111326",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,2,2,null,2,6,6,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,2,null,null,1,null,null,null,null,1]
[3,2,1,1,1,2,2,2,3,"321112223",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,1,null,null,1]
[3,2,1,1,1,2,3,2,5,"321112325",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,5,4,10,10,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[3,2,1,1,2,1,1,2,4,"321121124",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,2,null,1,null,null,null,4,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,1]
[3,2,1,1,2,1,3,1,12,"3211213112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,6,null,3,null,12,null,6,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,4,null,null,1,null,null,null,null,null,1]
[3,2,1,1,2,2,3,2,3,"321122323",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,3,2,null,6,null,6,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,1,null,null,1]
[3,2,1,1,3,1,1,1,4,"321131114",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,2,null,1,null,null,null,null,4,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,1]
[3,2,1,1,3,2,1,1,10,"3211321110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,null,10,8,null,null,null,null,null,20,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,3,null,null,1,null,null,null,null,null,1]
[3,2,1,2,1,1,1,1,8,"321211118",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,4,null,2,8,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,3,null,null,null,null,null,null,null,null,1]
[3,2,1,2,1,1,3,1,5,"321211315",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,1,2,null,2,5,5,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[3,2,1,2,1,2,1,1,6,"321212116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,6,5,12,null,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,2,null,null,null,null,null,null,null,1]
[3,2,1,2,1,2,2,2,16,"3212122216",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,2,null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,6,null,null,null,null,null,null,null,null,1]
[3,2,1,2,2,1,1,1,5,"321221115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,1,2,null,2,null,null,null,5,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[3,2,1,2,2,1,3,1,4,"321221314",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,2,null,1,null,4,null,4,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[3,2,1,2,2,1,3,2,6,"321221326",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,2,2,null,2,null,6,null,6,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,2,null,null,null,null,null,null,null,1]
[3,2,1,2,2,2,1,2,12,"3212221212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,12,9,null,null,null,24,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,4,null,null,null,null,null,null,null,null,1]
[3,2,1,2,3,1,1,2,1,"321231121",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[3,3,1,1,1,1,1,1,2,"331111112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1,1,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,1,null,null,1]
[3,3,1,1,1,4,1,1,8,"331114118",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,2,6,null,4,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,1,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,3,null,null,1,null,null,null,null,null,1]
[3,3,1,2,1,4,1,1,1,"331214111",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,1,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,1,null,null,null,1]
[3,3,1,2,1,4,1,2,6,"331214126",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,2,4,null,3,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,2,null,null,null,null,null,null,null,1]
[4,1,1,1,1,1,3,1,10,"4111113110",10,null,null,null,null,2,4,null,4,null,10,10,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},3,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,4,null,null,null,null,null,null,null,null,1]
[4,1,1,1,1,2,1,1,5,"411112115",null,5,null,null,null,null,null,5,4,null,10,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},3,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,1,1,1,2,3,1,10,"4111123110",null,10,null,null,null,null,null,10,8,null,20,20,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},3,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,4,null,null,null,null,null,null,null,null,1]
[4,1,1,1,2,1,1,1,4,"411121114",4,null,null,null,null,null,2,null,1,null,null,null,null,4,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},3,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,1,1,2,2,1,1,3,"411122113",null,3,null,null,null,null,null,3,2,null,null,null,null,6,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},3,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,1,1,2,3,1,1,12,"4111231112",12,null,null,null,null,null,null,12,9,null,null,null,null,12,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},3,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,4,null,null,null,null,null,null,null,null,1]
[4,1,2,1,1,1,1,1,2,"412111112",2,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,1]
[4,1,2,1,1,1,3,1,4,"412111314",4,null,null,null,null,null,2,null,1,null,4,4,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,1]
[4,1,2,1,1,3,1,1,1,"412113111",1,null,null,null,null,null,null,1,null,null,2,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,1]
[4,1,2,1,1,3,2,1,16,"4121132116",16,null,null,4,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,4,null,null,1,null,null,null,null,null,1,null,1]
[4,1,2,1,2,1,3,1,5,"412121315",5,null,null,null,null,1,2,null,2,null,null,5,null,5,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,2,1,2,2,1,1,5,"412122115",null,5,null,null,null,null,null,5,4,null,null,null,null,10,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,2,1,3,1,1,1,16,"4121311116",16,null,null,null,null,null,8,null,4,null,null,null,null,null,16,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,4,null,null,1,null,null,null,null,null,1,null,1]
[4,1,3,1,1,1,1,1,4,"413111114",4,null,null,null,null,null,2,null,1,null,4,null,null,null,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,1,1,2,1,3,"413111213",3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,1,1,3,1,6,"413111316",6,null,null,null,null,2,2,null,2,null,6,6,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,1,2,null,null,1,null,null,null,null,1]
[4,1,3,1,1,2,2,1,2,"413112212",null,2,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,1,2,2,2,10,"4131122210",null,10,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,3,null,null,1,null,null,null,null,null,1]
[4,1,3,1,1,2,3,2,8,"413112328",null,8,null,null,null,null,null,8,6,null,16,16,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,1,2,null,null,1,null,null,null,null,null,1]
[4,1,3,1,1,3,2,2,16,"4131132216",16,null,null,4,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,null,null,null,null,null,null,1,null,1]
[4,1,3,1,2,1,1,1,2,"413121112",2,null,null,null,null,null,1,null,null,null,null,null,null,2,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,2,1,1,2,5,"413121125",5,null,null,null,null,1,2,null,2,null,null,null,null,5,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,2,2,1,2,4,"413122124",null,4,null,null,null,null,null,4,3,null,null,null,null,8,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,2,2,3,2,4,"413122324",null,4,null,null,null,null,null,4,3,null,null,8,null,8,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,2,3,1,2,3,"413123123",3,null,null,null,null,null,null,3,2,null,null,null,null,3,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,3,1,1,2,5,"413131125",5,null,null,null,null,1,2,null,2,null,null,null,null,null,5,null,null,null,null,4,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,1,3,2,1,2,2,"413132122",null,2,null,null,null,null,null,2,1,null,null,null,null,null,null,4,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,1,3,2,1,1,1,1,5,{"$f":"A5188&B5188&C5188&D5188&E5188&F5188&G5188&H5188&I5188","v":"413211115"},5,null,null,null,null,1,2,null,2,null,5,null,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,3,2,1,1,2,1,8,"413211218",8,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,1,2,null,null,null,null,null,null,null,null,1]
[4,1,3,2,1,2,1,1,16,"4132121116",null,16,null,null,null,null,null,16,12,null,32,null,null,null,null,null,null,null,null,12,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,null,null,null,null,null,null,1]
[4,1,3,2,1,2,2,1,6,"413212216",null,6,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,1,2,null,null,null,null,null,null,null,1]
[4,1,3,2,1,2,3,1,5,"413212315",null,5,null,null,null,null,null,5,4,null,10,10,null,null,null,null,null,null,null,4,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,3,2,1,3,2,1,1,"413213211",1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,3,2,1,3,3,1,4,"413213314",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[4,1,3,2,2,1,1,1,3,"413221113",3,null,null,null,null,1,1,null,1,null,null,null,null,3,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,3,2,2,2,1,1,2,"413222112",null,2,null,null,null,null,null,2,1,null,null,null,null,4,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,3,2,2,2,3,1,2,"413222312",null,2,null,null,null,null,null,2,1,null,null,4,null,4,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,3,2,2,2,3,2,2,"413222322",null,2,null,null,null,null,null,2,1,null,null,4,null,4,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,1,3,2,2,3,3,1,1,"413223311",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[4,1,3,2,3,1,1,2,16,"4132311216",16,null,null,null,null,null,8,null,4,null,null,null,null,null,16,null,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,null,null,null,null,null,null,1]
[4,1,3,2,3,2,1,2,3,"413232123",null,3,null,null,null,null,null,3,2,null,null,null,null,null,null,6,null,null,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,2,1,1,1,1,2,1,5,"421111215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,2,null,null,null,null,1]
[4,2,1,1,1,2,2,1,12,"4211122112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,4,null,null,null,null,null,null,null,null,1,null,2]
[4,2,1,1,2,1,3,1,12,"4211213112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,6,null,3,null,12,null,6,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,4,null,null,null,null,null,null,null,null,1,null,2]
[4,2,1,1,2,2,3,1,3,"421122313",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,3,2,null,6,null,6,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,2,null,null,null,null,1]
[4,2,2,1,1,1,1,1,15,"4221111115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,3,6,null,6,15,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,3,null,null,1,null,null,null,null,null,1,null,1]
[4,2,2,1,1,2,1,1,2,"422112112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,2,1,4,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,1]
[4,2,2,1,1,2,1,1,15,"4221121115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,15,12,30,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1,3,null,null,1,null,null,null,null,null,1,null,1]
[4,2,2,1,2,1,3,1,1,"422121311",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,2,null,2,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,1]
[4,2,2,1,2,2,3,1,5,"422122315",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,5,4,null,10,null,10,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,2,3,1,1,1,1,1,16,"4231111116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,null,null,8,null,4,16,null,null,null,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,null,null,null,null,null,null,1,null,1]
[4,2,3,1,1,1,2,1,15,"4231112115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,null,null,null,null,null,null,1,null,1]
[4,2,3,1,1,1,3,2,6,"423111326",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,2,2,null,2,6,6,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,1,2,null,null,1,null,null,null,null,1]
[4,2,3,1,1,2,2,1,12,"4231122112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,3,null,null,null,null,null,null,null,null,1,null,1]
[4,2,3,1,1,2,3,2,1,"423112321",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,2,2,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,2,3,1,2,1,1,1,3,{"$f":"A5956&B5956&C5956&D5956&E5956&F5956&G5956&H5956&I5956","v":"423121113"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,1,1,null,1,null,null,null,3,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,2,3,1,2,2,1,1,8,"423122118",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,8,6,null,null,null,16,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,1,2,null,null,1,null,null,null,null,null,1]
[4,2,3,1,2,2,3,2,2,"423122322",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,2,1,null,4,null,4,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,2,3,1,3,1,1,1,1,"423131111",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,1,null,null,null,null,1]
[4,2,3,1,3,1,1,2,12,"4231311212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,6,null,3,null,null,null,null,12,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,3,null,null,null,null,null,null,null,null,1,null,1]
[4,2,3,2,1,1,1,2,16,"4232111216",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,null,null,8,null,4,16,null,null,null,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,null,null,null,null,null,null,1]
[4,2,3,2,1,1,2,2,15,"4232112215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,null,null,null,null,null,null,1]
[4,2,3,2,1,2,1,1,3,"423212113",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,3,2,6,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,2,3,2,1,2,2,2,12,"4232122212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,3,null,null,null,null,null,null,null,null,1]
[4,2,3,2,1,2,3,2,5,"423212325",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,5,4,10,10,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,2,3,2,2,1,1,2,3,"423221123",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,1,1,null,1,null,null,null,3,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,2,3,2,2,1,3,2,2,"423221322",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,1,null,null,null,2,null,2,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,2,3,2,2,2,3,2,15,"4232223215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,15,12,null,30,null,30,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,null,null,null,null,null,null,1]
[4,2,3,2,3,1,1,2,1,"423231121",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,2,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},2,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,3,1,1,1,4,1,1,1,"431114111",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,1,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},3,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,2,null,null,null,null,null,null,null,1]
[4,3,2,1,1,1,1,1,16,"4321111116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,4,12,2,null,4,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},3,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,1,null,1,5,null,null,null,null,null,null,null,null,1]
[4,3,3,1,1,1,1,1,15,"4331111115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,3,12,null,null,3,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,1,3,null,null,1,null,null,null,null,null,1]
[4,3,3,1,1,4,1,1,8,"433114118",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,2,6,null,4,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,1,1,null,null,1,null,null,null,null,null,1]
[4,3,3,2,1,4,1,1,12,{"$f":"A6468&B6468&C6468&D6468&E6468&F6468&G6468&H6468&I6468","v":"4332141112"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,2,8,2,6,4,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,1,null,null,null,3,null,null,null,null,null,null,null,null,1]
[5,1,0,1,1,1,1,1,2,"510111112",2,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,1,0,1,1,1,2,1,3,"510111213",3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,1,0,1,1,1,3,1,2,"510111312",2,null,null,null,null,null,1,null,null,null,2,2,null,null,null,null,null,null,null,1,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,1,0,1,1,2,2,1,3,"510112213",null,3,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,1,0,1,1,2,3,1,1,"510112311",null,1,null,null,null,null,null,1,null,null,2,2,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,null,null,null,1]
[5,1,0,1,1,3,1,2,12,"5101131212",12,null,null,null,null,null,null,12,null,9,15,null,null,null,null,null,null,null,null,null,9,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,1,0,1,1,3,3,1,5,"510113315",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[5,1,0,1,1,3,3,2,15,"5101133215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[5,1,0,1,2,1,1,2,4,"510121124",4,null,null,null,null,null,2,null,1,null,null,null,null,4,null,null,null,null,null,3,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,1,0,1,2,2,1,2,12,"5101221212",null,12,null,null,null,null,null,12,9,null,null,null,null,24,null,null,null,null,null,9,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,1,0,1,2,2,3,1,15,"5101223115",null,15,null,null,null,null,null,15,12,null,null,30,null,30,null,null,null,null,null,12,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,1,0,1,2,3,1,2,10,"5101231210",10,null,null,null,null,null,null,10,8,null,null,null,null,10,null,null,null,null,null,8,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,1,null,null,null,null,null,null,null,null,1]
[5,1,0,1,2,3,3,2,2,"510123322",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0}]
[5,1,0,1,3,2,1,1,16,"5101321116",null,16,null,null,null,null,null,16,12,null,null,null,null,null,null,32,null,null,null,12,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,1,1,1,2,1,"520111121",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,null,null,null,1]
[5,2,0,1,1,1,3,1,6,"520111316",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,2,2,null,2,6,6,null,null,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,2,0,1,1,1,3,1,16,"5201113116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,null,null,8,null,4,16,16,null,null,null,null,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,1,2,2,1,15,"5201122115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,1,2,3,1,1,"520112311",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,2,2,null,null,null,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,null,null,null,1]
[5,2,0,1,2,1,1,1,12,"5201211112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,6,null,3,null,null,null,6,null,null,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,2,1,3,2,8,"520121328",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,4,null,2,null,8,null,8,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[5,2,0,1,2,2,3,1,10,"5201223110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,null,10,8,null,null,null,20,null,null,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,1,null,null,null,null,null,null,null,null,1]
[5,2,0,1,3,1,1,2,2,"520131122",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,1,null,null,null,null,null,null,2,null,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,2,0,1,3,2,1,1,5,"520132115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,5,4,null,null,null,null,null,10,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,1,6,"520132116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,6,5,null,null,null,null,null,12,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,1,8,"520132118",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,8,7,null,null,null,null,null,16,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,1,10,"5201321110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,null,10,8,null,null,null,null,null,20,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,1,null,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,1,12,"5201321112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,12,9,null,null,null,null,null,24,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,1,15,"5201321115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,15,12,null,null,null,null,null,30,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,1,16,{"$f":"A7108&B7108&C7108&D7108&E7108&F7108&G7108&H7108&I7108","v":"5201321116"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,null,null,16,12,null,null,null,null,null,32,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,2,1,"520132121",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,null,null,2,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,null,null,null,1]
[5,2,0,1,3,2,1,2,2,"520132122",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,2,1,null,null,null,null,null,4,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,2,0,1,3,2,1,2,3,"520132123",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,3,2,null,null,null,null,null,6,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,2,0,1,3,2,1,2,4,"520132124",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,4,3,null,null,null,null,null,8,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,2,5,"520132125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,5,4,null,null,null,null,null,10,null,null,null,null,null,1,1,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,2,6,"520132126",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,6,5,null,null,null,null,null,12,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,2,8,"520132128",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,null,null,8,7,null,null,null,null,null,16,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,2,10,"5201321210",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,null,null,10,8,null,null,null,null,null,20,null,null,null,null,null,1,2,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,1,null,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,2,12,"5201321212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,null,null,12,9,null,null,null,null,null,24,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,2,15,"5201321215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,15,12,null,null,null,null,null,30,null,null,null,null,null,1,3,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,2,0,1,3,2,1,2,16,"5201321216",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,null,null,16,12,null,null,null,null,null,32,null,null,null,null,null,1,4,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,1,1,"530111111",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,null,null,null,1]
[5,3,0,1,1,1,1,1,2,"530111112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1,1,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,3,0,1,1,1,1,1,3,"530111113",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,1,2,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,3,0,1,1,1,1,1,4,"530111114",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,1,3,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,1,5,"530111115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,1,4,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,1,6,"530111116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,2,4,1,null,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,1,8,"530111118",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,2,6,1,null,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,1,10,"5301111110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,2,8,1,null,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,1,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,1,12,"5301111112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,3,9,null,null,3,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,1,15,"5301111115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,3,12,null,null,3,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,1,16,"5301111116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,4,12,null,null,4,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,2,1,"530111121",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,null,null,null,1]
[5,3,0,1,1,1,1,2,2,"530111122",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,1,1,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,3,0,1,1,1,1,2,3,"530111123",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,1,2,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,3,0,1,1,1,1,2,4,"530111124",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,1,3,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,2,5,"530111125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,1,4,null,null,1,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,2,6,"530111126",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,2,4,1,null,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,2,8,"530111128",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,2,6,1,null,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,2,10,"5301111210",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,2,8,1,null,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,1,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,2,12,"5301111212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,3,9,null,null,3,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,2,15,"5301111215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,3,12,null,null,3,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,1,1,2,16,"5301111216",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,4,12,null,null,4,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,1,1,"530114111",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,1,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,null,null,null,1]
[5,3,0,1,1,4,1,1,2,"530114112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,2,1,null,1,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,3,0,1,1,4,1,1,3,"530114113",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,3,0,1,1,4,1,1,4,"530114114",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,2,2,null,2,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,1,5,"530114115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,1,6,"530114116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,2,4,null,3,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,1,8,"530114118",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,2,6,null,4,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,1,10,"5301141110",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,2,8,null,5,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,1,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,1,12,"5301141112",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,2,8,2,6,4,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,1,15,"5301141115",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,1,16,"5301141116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,4,12,null,8,4,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,2,1,"530114121",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,null,1,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,null,null,null,null,null,null,1,null,null,null,1]
[5,3,0,1,1,4,1,2,2,"530114122",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,2,1,null,1,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,3,0,1,1,4,1,2,3,"530114123",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,1]
[5,3,0,1,1,4,1,2,4,"530114124",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,2,2,null,2,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,2,5,"530114125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,2,6,"530114126",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,2,4,null,3,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,2,8,"530114128",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,2,6,null,4,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1,1,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,2,10,"5301141210",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,2,8,null,5,2,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1,1,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,2,12,"5301141212",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,2,8,2,6,4,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,2,15,"5301141215",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]
[5,3,0,1,1,4,1,2,16,"5301141216",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,4,12,null,8,4,{"$f":"IF(Zwischenwerte!$AB$14=Zwischenwerte!$AB$26,1,0)","v":0},1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,1,2,null,null,null,null,null,null,null,null,1]

{"sheet":"Klimazonen","index":3,"n_rows":436,"n_cols":161,"rows_kept":436,"cut":false,"hidden":true,"merged":[[400,35,400,37],[400,38,400,40],[401,2,401,4],[401,5,401,7],[401,8,401,10],[401,11,401,13],[401,14,401,16],[401,17,401,19],[401,20,401,22],[401,23,401,25],[401,26,401,28],[401,29,401,31],[401,32,401,34],[401,35,401,37],[401,38,401,40],[400,26,400,28],[400,29,400,31],[400,32,400,34],[400,23,400,25],[340,0,355,0],[340,2,340,4],[340,5,340,7],[340,11,340,13],[340,14,340,16],[340,17,340,19],[340,20,340,22],[400,0,415,0],[400,2,400,4],[400,5,400,7],[400,8,400,10],[400,11,400,13],[400,14,400,16],[400,17,400,19],[400,20,400,22],[360,0,375,0],[360,2,360,4],[360,5,360,7],[360,8,360,10],[360,11,360,13],[360,14,360,16],[360,17,360,19],[360,20,360,22],[381,14,381,16],[60,95,60,97],[61,95,61,97],[60,98,60,100],[61,98,61,100],[60,104,60,106],[61,104,61,106],[61,65,61,67],[61,68,61,70],[61,71,61,73],[61,74,61,76],[60,86,60,88],[61,86,61,88],[60,83,60,85],[61,83,61,85],[60,65,60,67],[60,68,60,70],[60,71,60,73],[60,74,60,76],[60,2,60,4],[61,2,61,4],[60,17,60,19],[61,17,61,19],[60,20,60,22],[60,23,60,25],[60,26,60,28],[60,29,60,31],[61,20,61,22],[61,23,61,25],[61,26,61,28],[61,29,61,31],[60,5,60,7],[61,5,61,7],[320,0,335,0],[320,2,320,4],[320,5,320,7],[320,11,320,13],[320,14,320,16],[320,17,320,19],[320,32,320,34],[320,8,320,10],[320,35,320,37],[321,2,321,4],[321,5,321,7],[321,11,321,13],[321,14,321,16],[321,17,321,19],[321,32,321,34],[321,8,321,10],[321,35,321,37],[280,14,280,16],[300,0,315,0],[300,2,300,4],[300,5,300,7],[300,8,300,10],[300,11,300,13],[300,14,300,16],[300,17,300,19],[301,2,301,4],[301,5,301,7],[301,8,301,10],[301,11,301,13],[301,14,301,16],[301,17,301,19],[281,2,281,4],[281,5,281,7],[281,8,281,10],[281,11,281,13],[281,14,281,16],[281,23,281,25],[260,0,275,0],[260,2,260,4],[260,5,260,7],[260,8,260,10],[260,11,260,13],[260,14,260,16],[260,17,260,19],[261,2,261,4],[261,5,261,7],[261,8,261,10],[261,11,261,13],[261,14,261,16],[261,17,261,19],[280,23,280,25],[280,17,280,19],[281,17,281,19],[280,20,280,22],[281,20,281,22],[280,0,295,0],[280,2,280,4],[280,5,280,7],[280,8,280,10],[280,11,280,13],[81,116,81,118],[81,119,81,121],[81,122,81,124],[81,125,81,127],[80,116,80,118],[80,119,80,121],[80,122,80,124],[80,125,80,127],[80,83,80,85],[81,83,81,85],[80,86,80,88],[80,89,80,91],[80,98,80,100],[80,104,80,106],[80,107,80,109],[80,110,80,112],[80,113,80,115],[81,95,81,97],[80,101,80,103],[80,95,80,97],[81,101,81,103],[81,86,81,88],[81,89,81,91],[81,98,81,100],[81,104,81,106],[81,107,81,109],[81,110,81,112],[81,113,81,115],[80,77,80,79],[81,5,81,7],[81,8,81,10],[81,11,81,13],[81,14,81,16],[81,17,81,19],[81,20,81,22],[81,23,81,25],[81,29,81,31],[81,32,81,34],[81,35,81,37],[81,38,81,40],[81,41,81,43],[81,44,81,46],[81,47,81,49],[81,53,81,55],[81,56,81,58],[81,62,81,64],[81,65,81,67],[81,68,81,70],[81,71,81,73],[81,77,81,79],[80,5,80,7],[80,8,80,10],[80,11,80,13],[80,14,80,16],[80,17,80,19],[80,20,80,22],[80,23,80,25],[80,29,80,31],[80,32,80,34],[80,35,80,37],[80,38,80,40],[80,41,80,43],[80,44,80,46],[80,47,80,49],[80,53,80,55],[80,56,80,58],[80,62,80,64],[80,65,80,67],[80,68,80,70],[80,71,80,73],[241,2,241,4],[241,5,241,7],[241,8,241,10],[241,11,241,13],[241,14,241,16],[241,17,241,19],[240,0,255,0],[240,2,240,4],[240,5,240,7],[240,8,240,10],[240,11,240,13],[240,14,240,16],[240,17,240,19],[221,26,221,28],[220,0,235,0],[220,2,220,4],[220,5,220,7],[220,8,220,10],[220,11,220,13],[220,14,220,16],[220,17,220,19],[220,20,220,22],[220,23,220,25],[220,26,220,28],[221,2,221,4],[221,5,221,7],[221,8,221,10],[221,11,221,13],[221,14,221,16],[221,17,221,19],[221,20,221,22],[221,23,221,25],[41,11,41,13],[0,0,15,0],[0,2,0,4],[1,2,1,4],[21,8,21,10],[21,80,21,82],[21,2,21,4],[21,44,21,46],[21,23,21,25],[21,41,21,43],[20,41,20,43],[20,62,20,64],[21,65,21,67],[21,62,21,64],[20,80,20,82],[20,2,20,4],[20,44,20,46],[20,23,20,25],[20,65,20,67],[20,8,20,10],[20,0,35,0],[0,6,0,7],[1,6,1,7],[20,50,20,52],[40,29,40,31],[40,32,40,34],[40,35,40,37],[21,50,21,52],[21,131,21,133],[21,140,21,142],[21,155,21,157],[20,101,20,103],[20,107,20,109],[20,35,20,37],[21,35,21,37],[20,53,20,55],[21,53,21,55],[20,47,20,49],[21,47,21,49],[20,128,20,130],[21,128,21,130],[20,125,20,127],[21,125,21,127],[20,119,20,121],[21,119,21,121],[20,122,20,124],[21,122,21,124],[20,98,20,100],[41,14,41,16],[41,17,41,19],[41,20,41,22],[41,23,41,25],[41,26,41,28],[40,14,40,16],[40,17,40,19],[40,20,40,22],[40,23,40,25],[40,26,40,28],[60,107,60,109],[60,14,60,16],[60,11,60,13],[60,8,60,10],[60,77,60,79],[61,107,61,109],[61,14,61,16],[61,11,61,13],[61,8,61,10],[61,77,61,79],[60,35,60,37],[61,35,61,37],[60,53,60,55],[61,53,61,55],[60,62,60,64],[61,62,61,64],[60,101,60,103],[61,101,61,103],[60,89,60,91],[61,89,61,91],[60,92,60,94],[61,92,61,94],[60,41,60,43],[60,44,60,46],[40,0,55,0],[40,2,40,4],[40,5,40,7],[40,8,40,10],[40,11,40,13],[41,2,41,4],[41,5,41,7],[41,8,41,10],[81,92,81,94],[80,0,95,0],[80,50,80,52],[80,26,80,28],[80,74,80,76],[80,80,80,82],[80,92,80,94],[80,59,80,61],[80,2,80,4],[81,50,81,52],[81,74,81,76],[81,80,81,82],[41,29,41,31],[41,32,41,34],[41,35,41,37],[60,0,75,0],[101,26,101,28],[81,59,81,61],[81,2,81,4],[100,0,115,0],[100,2,100,4],[100,5,100,7],[100,8,100,10],[100,14,100,16],[100,23,100,25],[100,20,100,22],[100,11,100,13],[100,17,100,19],[100,26,100,28],[101,2,101,4],[101,5,101,7],[101,8,101,10],[101,14,101,16],[81,26,81,28],[100,29,100,31],[100,32,100,34],[101,23,101,25],[101,20,101,22],[101,11,101,13],[101,17,101,19],[140,0,155,0],[140,11,140,13],[140,14,140,16],[140,17,140,19],[140,20,140,22],[141,11,141,13],[141,14,141,16],[141,17,141,19],[141,20,141,22],[141,5,141,7],[141,8,141,10],[140,2,140,4],[140,5,140,7],[140,8,140,10],[141,2,141,4],[181,20,181,22],[180,8,180,10],[180,11,180,13],[180,14,180,16],[180,17,180,19],[180,20,180,22],[160,0,175,0],[160,11,160,13],[160,2,160,4],[160,5,160,7],[160,8,160,10],[161,11,161,13],[161,2,161,4],[161,5,161,7],[161,8,161,10],[200,0,215,0],[200,5,200,7],[200,2,200,4],[201,5,201,7],[201,2,201,4],[181,8,181,10],[181,11,181,13],[181,14,181,16],[181,17,181,19],[180,0,195,0],[180,2,180,4],[180,5,180,7],[181,2,181,4],[181,5,181,7],[120,0,135,0],[120,2,120,4],[120,5,120,7],[120,8,120,10],[120,11,120,13],[120,14,120,16],[120,17,120,19],[120,20,120,22],[120,23,120,25],[121,2,121,4],[121,5,121,7],[121,8,121,10],[121,11,121,13],[121,14,121,16],[121,17,121,19],[121,20,121,22],[121,23,121,25],[220,41,220,43],[220,44,220,46],[220,47,220,49],[220,50,220,52],[180,23,180,25],[180,26,180,28],[181,23,181,25],[181,26,181,28],[181,29,181,31],[180,29,180,31],[101,29,101,31],[101,32,101,34],[220,53,220,55],[220,56,220,58],[220,59,220,61],[220,62,220,64],[220,65,220,67],[221,29,221,31],[221,32,221,34],[221,35,221,37],[221,38,221,40],[221,41,221,43],[221,44,221,46],[221,47,221,49],[221,50,221,52],[221,53,221,55],[221,56,221,58],[221,59,221,61],[221,62,221,64],[221,65,221,67],[220,29,220,31],[220,32,220,34],[220,35,220,37],[220,38,220,40],[420,0,435,0],[420,2,420,4],[420,5,420,7],[420,8,420,10],[420,11,420,13],[420,14,420,16],[420,17,420,19],[420,20,420,22],[420,23,420,25],[420,26,420,28],[420,29,420,31],[420,32,420,34],[420,35,420,37],[421,2,421,4],[421,5,421,7],[421,8,421,10],[421,11,421,13],[421,14,421,16],[421,17,421,19],[421,20,421,22],[421,23,421,25],[421,26,421,28],[421,29,421,31],[421,32,421,34],[421,35,421,37],[60,47,60,49],[60,50,60,52],[61,41,61,43],[61,44,61,46],[61,47,61,49],[61,50,61,52],[60,56,60,58],[61,56,61,58],[60,59,60,61],[61,59,61,61],[60,110,60,112],[61,110,61,112],[20,11,20,13],[21,11,21,13],[20,32,20,34],[21,32,21,34],[20,68,20,70],[21,68,21,70],[20,71,20,73],[21,71,21,73],[20,83,20,85],[21,83,21,85],[20,38,20,40],[21,38,21,40],[20,14,20,16],[21,14,21,16],[20,17,20,19],[21,17,21,19],[60,32,60,34],[61,32,61,34],[60,38,60,40],[61,38,61,40],[60,80,60,82],[61,80,61,82],[21,98,21,100],[20,110,20,112],[21,110,21,112],[20,116,20,118],[21,116,21,118],[21,101,21,103],[21,107,21,109],[20,74,20,76],[21,74,21,76],[21,113,21,115],[20,113,20,115],[21,92,21,94],[20,89,20,91],[21,89,21,91],[20,92,20,94],[20,146,20,148],[21,146,21,148],[20,149,20,151],[21,149,21,151],[20,152,20,154],[21,152,21,154],[20,158,20,160],[21,158,21,160],[20,134,20,136],[21,134,21,136],[20,137,20,139],[21,137,21,139],[20,143,20,145],[21,143,21,145],[20,131,20,133],[20,140,20,142],[20,155,20,157],[341,8,341,10],[20,5,20,7],[21,5,21,7],[20,104,20,106],[21,104,21,106],[20,20,20,22],[21,20,21,22],[20,26,20,28],[21,26,21,28],[20,95,20,97],[21,95,21,97],[20,59,20,61],[21,59,21,61],[20,86,20,88],[21,86,21,88],[20,77,20,79],[21,77,21,79],[20,29,20,31],[21,29,21,31],[20,56,20,58],[21,56,21,58],[340,35,340,37],[340,38,340,40],[341,2,341,4],[341,5,341,7],[341,11,341,13],[341,14,341,16],[341,17,341,19],[341,20,341,22],[341,35,341,37],[341,38,341,40],[340,23,340,25],[340,26,340,28],[340,29,340,31],[341,23,341,25],[340,8,340,10],[341,26,341,28],[341,29,341,31],[340,32,340,34],[341,32,341,34],[360,23,360,25],[360,26,360,28],[360,29,360,31],[360,32,360,34],[360,35,360,37],[360,38,360,40],[361,2,361,4],[361,5,361,7],[361,8,361,10],[361,11,361,13],[361,14,361,16],[361,17,361,19],[361,20,361,22],[361,23,361,25],[361,26,361,28],[361,29,361,31],[361,32,361,34],[361,35,361,37],[361,38,361,40],[361,41,361,43],[361,44,361,46],[360,41,360,43],[360,44,360,46],[380,0,395,0],[380,2,380,4],[380,5,380,7],[380,8,380,10],[380,11,380,13],[380,14,380,16],[380,26,380,28],[380,20,380,22],[380,23,380,25],[380,17,380,19],[380,29,380,31],[380,32,380,34],[380,35,380,37],[380,38,380,40],[380,41,380,43],[380,44,380,46],[381,2,381,4],[381,5,381,7],[381,8,381,10],[381,11,381,13],[381,44,381,46],[381,26,381,28],[381,20,381,22],[381,23,381,25],[381,17,381,19],[381,29,381,31],[381,32,381,34],[381,35,381,37],[381,38,381,40],[381,41,381,43]]}
[{"$f":"Zwischenwerte!A14","v":"Germany"},"Zeile",{"$f":"Zwischenwerte!B14","v":"Aachen"}]
[null,"Breitengrad",50.77]
[null,null,"Global","Diffus","Außentemp",null,null,"Hinweis Datenimport Meteonorm"]
[null,"Jan",0.72,0.44,2.8]
[null,"Feb",1.36,0.9,4,null,null,"- Breitengrad aus Übersicht im oberen Bereich übernehmen"]
[null,"Mar",2.38,1.55,6.7,null,null,"- Format >> Userdefined: Monat - Globalstrahlung hor. - Diffusstrahlung hor. - Lufttemperatur - Windgeschw."]
[null,"Apr",3.84,1.75,9.6,null,null,"- Format >> Userdefined: Einheit: Monatswerte - kWh/m²d"]
[null,"Mai",4.99,2.79,13.8,null,null,"- Auswertung: Daten aus Tabelle kopieren (Strg+C) und als \"Inhalte einfügen\" als Text einfügen"]
[null,"Jun",5.07,2.56,16.8]
[null,"Jul",5.12,2.4700000000000002,17.8]
[null,"Aug",4.45,2.25,18.7]
[null,"Sep",2.91,1.71,15.1]
[null,"Okt",1.76,1.1100000000000001,10.9]
[null,"Nov",0.87,0.55000000000000004,6.2]
[null,"Dez",0.47,0.35,3.4]
[null,"Jahr",2.83,1.54,10.5]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A17","v":"Germany"},"Stadt","Aachen",null,null,"Augsburg",null,null,"Berlin",null,null,"Bochum",null,null,"Bonn",null,null,"Bielefeld",null,null,"Braunschweig",null,null,"Bremen",null,null,"Chemnitz",null,null,"Cottbus",null,null,"Dortmund",null,null,"Dresden",null,null,"Duisburg",null,null,"Düsseldorf",null,null,"Erfurt",null,null,"Essen",null,null,"Frankfurt/Main",null,null,"Freiburg",null,null,"Gelsenkirchen",null,null,"Halle/Saale",null,null,"Hamburg",null,null,"Hannover",null,null,"Karlsruhe",null,null,"Kassel",null,null,"Kiel",null,null,"Koblenz",null,null,"Köln",null,null,"Leipzig",null,null,"Leverkusen",null,null,"Ludwigshafen",null,null,"Lübeck",null,null,"Magdeburg",null,null,"Mainz",null,null,"Mannheim",null,null,"Mönchengladbach",null,null,"München",null,null,"Münster",null,null,"Nürnberg",null,null,"Oberhausen",null,null,"Oldenburg",null,null,"Osnabrück",null,null,"Paderborn",null,null,"Potsdam",null,null,"Rostock",null,null,"Saarbrücken",null,null,"Schwerin",null,null,"Stuttgart",null,null,"Ulm",null,null,"Wiesbaden",null,null,"Wolfsburg",null,null,"Wuppertal",null,null,"Würzburg",null,null,"Zwickau"]
[null,"Breitengrad",50.77,null,null,48.35,null,null,52.53,null,null,51.47,null,null,50.73,null,null,52.03,null,null,52.25,null,null,53.08,null,null,50.83,null,null,51.72,null,null,51.53,null,null,51.05,null,null,51.43,null,null,51.22,null,null,50.97,null,null,51.47,null,null,50.1,null,null,47.9,null,null,51.5,null,null,51.47,null,null,53.55,null,null,52.23,null,null,49,null,null,51.3,null,null,54.33,null,null,50.35,null,null,50.93,null,null,51.33,null,null,51.03,null,null,49.48,null,null,53.87,null,null,52.13,null,null,50,null,null,49.5,null,null,51.2,null,null,48.13,null,null,51.97,null,null,49.45,null,null,51.47,null,null,55.13,null,null,52.28,null,null,51.72,null,null,52.4,null,null,54.07,null,null,49.25,null,null,53.63,null,null,48.78,null,null,48.4,null,null,50.08,null,null,52.45,null,null,51.25,null,null,49.8,null,null,50.72]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.72,0.44,2.8,1.01,0.52,-1.3,0.6,0.41,0.1,0.63,0.43,2.8,0.72,0.45,2.2000000000000002,0.64,0.39,0.9,0.65,0.39,0.3,0.6,0.35,2,0.74,0.44,-0.8,0.71,0.42,-1.2,0.63,0.42,2.8,0.72,0.43,0.3,0.63,0.46,2,0.66,0.43,2.9,0.7,0.43,0.7,0.63,0.45,2,0.69,0.5,1,0.84,0.56999999999999995,1.6,0.62,0.42,2,0.75,0.49,-0.2,0.53,0.35,3,0.64,0.39,1.8,0.81,0.5,2.5,0.65,0.42,1,0.51,0.34,1.7,0.69,0.48,1.2,0.7,0.42,2.8,0.72,0.43,1.8,0.69,0.43,2.2000000000000002,0.75,0.54,1.4,0.52,0.34,1.7,0.66,0.41,-0.1,0.7,0.5,1.2,0.74,0.47,1.4,0.67,0.43,2,1.04,0.6,-1.3,0.63,0.42,2.5,0.77,0.54,-0.8,0.63,0.46,2.8,0.6,0.38,2.2000000000000002,0.62,0.43,2.2000000000000002,0.65,0.43,0.5,0.6,0.42,-0.6,0.48,0.36,0.6,0.72,0.52,1.2,0.52,0.38,0.7,0.91,0.48,1.3,0.92,0.54,-0.9,0.69,0.5,0.9,0.64,0.38,0.3,0.66,0.43,1.7,0.81,0.48,-0.4,0.71,0.44,-1.6]
[null,"Feb",1.36,0.9,4,1.8,0.99,-0.7,1.23,0.76,1.4,1.32,0.92,4,1.39,0.91,2.8,1.32,0.84,1.3,1.3,0.87,0.7,1.22,0.84,2.9,1.38,0.73,0.3,1.37,0.87,-0.1,1.32,0.92,4,1.37,0.88,1.9,1.32,0.8,2.5,1.33,0.93,4.0999999999999996,1.44,0.79,2.2000000000000002,1.32,0.9,2.5,1.41,0.97,2.6,1.58,1.02,3.2,1.32,0.92,2.5,1.37,0.94,0.2,1.1599999999999999,0.82,3.5,1.3,0.89,3,1.56,1,3.7,1.41,0.9,2.4,1.1000000000000001,0.63,2.2999999999999998,1.39,0.86,2.2000000000000002,1.37,0.93,4.2,1.38,0.91,2.5,1.36,0.92,2.8,1.49,0.95,2.8,1.1399999999999999,0.72,2.5,1.35,0.74,0.2,1.4,0.89,2.8,1.49,0.94,2.8,1.32,0.9,2.6,1.83,0.92,0.9,1.29,0.87,3.6,1.56,1,0.9,1.32,0.89,3.9,1.22,0.8,3.1,1.27,0.82,3.3,1.37,0.79,1,1.22,0.79,0.4,1.1100000000000001,0.67,1.5,1.51,1.01,2.8,1.1499999999999999,0.8,1.7,1.66,1.03,2.8,1.66,0.95,0,1.39,0.91,1.9,1.29,0.86,0.7,1.31,0.9,2.2999999999999998,1.56,0.95,1.3,1.45,0.94,-0.7]
[null,"Mar",2.38,1.55,6.7,2.84,1.58,4.0999999999999996,2.35,1.35,3.8,2.04,1.2,6.7,2.25,1.55,6,2.17,1.24,4.3,2.23,1.47,3.7,2.11,1.22,4.9000000000000004,2.38,1.33,3.8,2.4300000000000002,1.41,3.4,2.06,1.27,6.8,2.33,1.46,4.9000000000000004,2.08,1.38,5.2,2.14,1.33,6.7,2.33,1.56,4.8,2.04,1.22,5.2,2.39,1.32,5.8,2.62,1.43,6.9,2.04,1.2,5.2,2.35,1.49,3.8,2.11,1.38,4.5,2.2200000000000002,1.42,5.2,2.5299999999999998,1.56,7.2,2.2599999999999998,1.35,5.4,2.09,1.24,4,2.33,1.41,5.5,2.2400000000000002,1.34,6.8,2.36,1.52,5.0999999999999996,2.21,1.43,5.9,2.4500000000000002,1.51,6.1,2.13,1.34,4.2,2.3199999999999998,1.36,3.7,2.4,1.37,6,2.4500000000000002,1.38,6.1,2.23,1.42,5.3,2.88,1.56,4.5,2.17,1.37,6,2.4300000000000002,1.37,4.4000000000000004,2.06,1.34,6.6,2.12,1.42,5.0999999999999996,2.1800000000000002,1.34,5.6,2.16,1.49,4.4000000000000004,2.35,1.34,3.9,2.2799999999999998,1.22,3.3,2.4900000000000002,1.38,6.1,2.2000000000000002,1.41,3.6,2.59,1.45,6.3,2.69,1.57,4.3,2.4,1.41,5.4,2.2200000000000002,1.41,3.7,2.14,1.3,5,2.59,1.42,4.7,2.36,1.33,2.9]
[null,"Apr",3.84,1.75,9.6,4.0199999999999996,2.23,7.7,3.7,2.0099999999999998,8.9,3.55,2.0699999999999998,10.199999999999999,3.58,2.25,8.3000000000000007,3.55,2.2400000000000002,7.8,3.58,2.19,7.8,3.55,2.11,8.9,3.61,2.31,8,3.88,2.2000000000000002,7.9,3.56,2.12,10.3,3.51,1.87,10,3.58,1.88,8.6,3.61,2.23,9.8000000000000007,3.61,2.08,8.6,3.55,2,8.6,3.85,1.85,9.1,3.84,2.16,10.1,3.55,2.1,8.6,3.7,2.2200000000000002,8,3.54,1.97,7.7,3.57,1.86,9.3000000000000007,3.92,2.4700000000000002,11.7,3.64,2.09,9,3.55,2.1,7.9,3.74,1.98,9,3.6,2.09,9.9,3.59,2.13,10.1,3.6,2.2400000000000002,8.4,3.84,2.0299999999999998,9.9,3.55,2.09,8.1,3.7,2.16,8.1,3.84,1.92,9.3000000000000007,3.84,2.12,9.9,3.72,2.02,8.4,4.01,2.34,8.6,3.58,2.42,9.5,3.7,2.2599999999999998,8.6,3.57,2.2200000000000002,9.6999999999999993,3.56,2.02,9,3.55,1.83,9.3000000000000007,3.56,2.09,8,3.67,2.1,8.1999999999999993,3.82,1.94,8.1,3.77,2.0499999999999998,9.3000000000000007,3.67,1.96,8.3000000000000007,3.87,2.0099999999999998,10.4,4.05,2.02,8,3.84,1.96,9.4,3.57,2.2799999999999998,7.8,3.58,2.11,8.3000000000000007,3.93,2.0699999999999998,8.6,3.67,2.09,7.1]
[null,"Mai",4.99,2.79,13.8,5.09,2.72,12.6,4.9400000000000004,2.2999999999999998,13.8,4.54,2.5499999999999998,14.5,4.58,2.2000000000000002,12.8,4.6900000000000004,2.06,12.4,4.8499999999999996,2.71,12.4,4.75,2.66,12.9,4.76,2.75,13,5.13,2.5299999999999998,13.1,4.5599999999999996,2.72,14.6,4.7300000000000004,2.2599999999999998,15,4.58,2.5299999999999998,13,4.63,2.76,14,4.6399999999999997,2.57,13.5,4.54,2.71,13,4.9000000000000004,2.74,13.6,4.82,2.5099999999999998,15,4.54,2.65,13,4.8,2.6,12.9,4.75,2.73,11.6,4.79,2.75,13.7,4.93,2.4900000000000002,16.100000000000001,4.74,2.5,13.6,4.88,2.61,12,4.7699999999999996,2.52,13.5,4.63,2.39,14.2,4.7300000000000004,2.84,14.8,4.62,2.65,12.8,4.99,2.77,14.5,4.8,2.81,12.2,4.84,2.58,13,4.92,2.71,13.8,4.99,2.69,14.5,4.76,2.48,12.8,5.09,2.82,14,4.7300000000000004,2.85,13.6,4.99,2.69,13.9,4.5599999999999996,2.5,13.9,4.76,2.66,12.9,4.78,2.52,13.5,4.63,2.4900000000000002,12.7,4.9000000000000004,2.4300000000000002,13.4,5.26,2.67,12.5,4.8499999999999996,2.23,13.9,4.93,2.67,12.7,4.9000000000000004,2.5499999999999998,15.1,4.96,2.09,12.7,4.92,2.63,13.8,4.8499999999999996,2.4,12.5,4.6100000000000003,2.72,12.7,5.09,2.71,13.6,4.7,2.4300000000000002,11.9]
[null,"Jun",5.07,2.56,16.8,5.41,2.91,15.2,5.31,2.75,16.600000000000001,4.4400000000000004,2.72,17.399999999999999,4.7300000000000004,2.83,16.100000000000001,4.74,2.81,15.8,5.16,3.03,15.9,4.7,2.84,15.7,4.97,2.4700000000000002,16.399999999999999,5.3,3,16.5,4.47,2.4900000000000002,17.5,4.9400000000000004,2.8,17.8,4.51,2.88,16,4.5999999999999996,2.95,16.899999999999999,4.91,2.77,16.100000000000001,4.4400000000000004,2.7,15.9,5.12,2.73,16.8,5.33,2.86,18.5,4.4400000000000004,2.5299999999999998,15.9,5.45,3.09,16.399999999999999,5.09,2.87,14.3,5.04,2.65,16.5,5.17,2.87,19.7,4.78,2.85,16.5,5.0199999999999996,2.73,15,4.96,2.95,16.600000000000001,4.74,2.67,17.100000000000001,5.39,2.66,17.5,4.6900000000000004,2.93,16,5.09,2.86,17.899999999999999,5.0999999999999996,2.76,15,5.29,3.07,16.2,5.1100000000000003,2.9,17.100000000000001,5.09,3.05,17.899999999999999,4.8,3.17,15.8,5.41,2.6,17.2,4.7300000000000004,2.72,16.3,5.04,2.7,17.2,4.4800000000000004,2.86,16.7,4.7300000000000004,2.9,15.7,4.75,2.84,16.2,4.7300000000000004,2.86,15.6,5.3,2.96,16.8,5.47,2.8,15.5,5.21,2.17,17.3,5.18,3.09,15.6,5.09,2.39,18.600000000000001,5.26,2.74,15.5,5.1100000000000003,2.85,17,5.16,2.77,15.9,4.54,3.16,15.6,5.44,2.88,16.899999999999999,4.95,2.93,15.2]
[null,"Jul",5.12,2.4700000000000002,17.8,5.39,2.67,17.899999999999999,5.09,2.6,18.399999999999999,4.63,2.69,18.5,4.75,2.75,17.8,4.78,2.4900000000000002,16.899999999999999,4.82,2.71,17.100000000000001,4.68,2.37,17.3,4.92,2.71,17.899999999999999,5.0599999999999996,2.74,17.899999999999999,4.6399999999999997,2.82,18.600000000000001,4.92,2.65,19.2,4.6500000000000004,2.78,17.5,4.71,2.64,18.100000000000001,4.96,2.61,17.399999999999999,4.63,2.64,17.5,5.13,2.93,17.899999999999999,5.4,2.72,19.2,4.63,2.73,17.5,5.33,2.64,18,4.7,2.4300000000000002,16.5,4.8099999999999996,2.68,18,5.23,2.73,20.9,4.8600000000000003,2.34,17.7,5.01,2.81,17.100000000000001,4.9800000000000004,2.81,18.3,4.78,2.83,18.2,5.28,2.79,19.2,4.75,2.5499999999999998,17.7,5.14,2.54,18.899999999999999,4.76,2.75,17,5.04,2.93,17.8,5.14,2.61,18.2,5.14,2.76,18.899999999999999,4.8600000000000003,2.84,17.399999999999999,5.39,2.65,17.8,4.79,2.75,17.7,5.1100000000000003,3,17.899999999999999,4.6399999999999997,2.5099999999999998,17.899999999999999,4.6900000000000004,2.81,17.399999999999999,4.8499999999999996,2.84,17.600000000000001,4.7300000000000004,2.73,17.2,5.09,2.82,18.100000000000001,5.23,2.4700000000000002,17.399999999999999,5.37,2.54,18.3,4.87,2.46,17.5,5.28,2.81,19.5,5.35,2.41,17.8,5.13,2.57,18.7,4.82,2.76,17.2,4.67,2.63,17.2,5.28,2.61,17.7,4.99,2.54,16.8]
[null,"Aug",4.45,2.25,18.7,4.66,2.21,17.399999999999999,4.3899999999999997,2.41,18.5,3.92,2.29,19.399999999999999,4.0999999999999996,1.99,17.8,4.1399999999999997,2.39,16.600000000000001,4.18,2.09,16.899999999999999,4.0599999999999996,2.27,18.100000000000001,4.3099999999999996,2.42,17.600000000000001,4.6100000000000003,2.2599999999999998,17.600000000000001,3.94,2.25,19.5,4.25,2.38,19.399999999999999,3.96,2.4,17.2,4.03,2.34,18.7,4.37,2.21,18.100000000000001,3.92,2.12,17.2,4.42,2.34,18.7,4.75,2.36,19.600000000000001,3.91,2.2400000000000002,17.2,4.47,2.19,17.600000000000001,4.08,2.0699999999999998,17.399999999999999,4.16,2.36,18.8,4.58,2.5099999999999998,20.3,4.1500000000000004,2.42,18.399999999999999,4.25,2.25,17.899999999999999,4.3,2.17,17.8,4.12,2.04,19,4.45,2.21,18.8,4.09,2.41,17.7,4.47,2.33,19.100000000000001,4.0999999999999996,2.27,17.600000000000001,4.3600000000000003,2.2200000000000002,17.399999999999999,4.46,2.19,18.899999999999999,4.46,2.27,19.100000000000001,4.2,2.4,17.2,4.6500000000000004,2.25,18.5,4.1500000000000004,2.39,18.399999999999999,4.47,2.33,18.5,3.94,2.44,18.399999999999999,4.07,2.39,18.100000000000001,4.2,2.35,18.399999999999999,4.1100000000000003,2.52,17,4.34,2,17.600000000000001,4.4400000000000004,2.2799999999999998,18,4.58,2.5099999999999998,19,4.2300000000000004,2.11,18.100000000000001,4.63,2.46,19.5,4.6500000000000004,2.35,17.3,4.45,2.19,18.2,4.17,2.38,17,4.01,2.31,17,4.5599999999999996,2.4500000000000002,18.600000000000001,4.38,2.42,16.3]
[null,"Sep",2.91,1.71,15.1,3.47,1.9,14.1,3,1.63,14.4,2.59,1.35,15.9,2.76,1.69,15,2.68,1.55,13.9,2.86,1.63,13.7,2.73,1.63,14.6,2.92,1.49,14.1,3.03,1.57,13.9,2.6,1.77,16.100000000000001,2.93,1.79,15,2.63,1.59,14.5,2.66,1.53,15.3,2.86,1.57,13.9,2.6,1.5,14.5,2.99,1.49,14.6,3.36,1.91,15,2.59,1.45,14.5,2.95,1.69,14.1,2.74,1.63,14.4,2.81,1.57,15,3.19,1.56,16.3,2.8,1.8,14.5,2.66,1.59,14.5,2.89,1.47,14.6,2.75,1.79,15.5,2.95,1.56,15.1,2.71,1.57,14.9,3.15,1.63,14.9,2.77,1.5,14.2,2.89,1.62,14,3,1.47,14.7,3.14,1.79,14.9,2.76,1.49,14.4,3.51,2.02,13.8,2.76,1.61,14.9,3.05,1.78,13.9,2.61,1.59,15.2,2.74,1.41,14.7,2.81,1.49,14.8,2.6,1.49,13.9,3,1.65,13.9,2.88,1.43,14.3,3.12,1.86,14.6,2.81,1.45,14.3,3.22,1.78,15.4,3.29,1.61,14.2,3,1.48,14.9,2.85,1.42,13.7,2.6,1.41,14.2,3.31,1.75,14.1,2.89,1.52,13]
[null,"Okt",1.76,1.1100000000000001,10.9,2.09,1.0900000000000001,9.4,1.68,1.06,9.4,1.63,1.08,11.1,1.73,1.1000000000000001,10.6,1.64,1.07,9.9,1.63,0.9,9.5,1.63,0.92,9.8000000000000007,1.83,1.08,9.6999999999999993,1.78,1.07,9.3000000000000007,1.63,0.93,11.2,1.83,1.01,10,1.65,1.1200000000000001,10.6,1.67,1.01,10.9,1.76,1.0900000000000001,9.1999999999999993,1.63,0.97,10.7,1.67,1.06,9.8000000000000007,1.92,1.1100000000000001,10.8,1.63,1.0900000000000001,10.7,1.75,1.07,9.6999999999999993,1.52,0.93,9.9,1.63,0.98,10,1.81,1.27,11.6,1.59,0.94,9.5,1.46,0.83,9.8000000000000007,1.67,0.96,10,1.71,1.1499999999999999,11,1.77,1.03,10.3,1.69,0.94,10.6,1.75,1.17,10.4,1.52,0.91,9.5,1.69,0.9,9.5,1.64,0.9,9.9,1.75,1.1499999999999999,10.4,1.69,1.05,10.6,2.13,1.17,9.4,1.69,0.91,10.4,1.85,1.01,9,1.64,1.01,10.8,1.62,1.02,9.9,1.7,0.99,10.199999999999999,1.61,1.02,9.9,1.68,0.98,9.5,1.56,0.9,9.3000000000000007,1.75,0.97,10.199999999999999,1.55,0.93,9.3000000000000007,1.87,1.17,10.7,1.96,1.0900000000000001,9.5,1.63,0.91,10.199999999999999,1.62,1.08,9.5,1.65,0.93,10.5,1.87,1.1499999999999999,9.3000000000000007,1.75,0.92,8.4]
[null,"Nov",0.87,0.55000000000000004,6.2,1.0900000000000001,0.74,3.2,0.71,0.48,4.2,0.79,0.57999999999999996,6.5,0.89,0.52,6.1,0.75,0.51,5.3,0.75,0.56000000000000005,4.9000000000000004,0.74,0.48,5.4,0.81,0.54,4.3,0.85,0.59,4.0999999999999996,0.79,0.56999999999999995,6.5,0.82,0.59,4.5,0.8,0.54,5.8,0.81,0.53,6.4,0.77,0.51,4.4000000000000004,0.79,0.44,5.8,0.82,0.56000000000000005,5,1.03,0.63,5.2,0.79,0.59,5.8,0.81,0.52,4.5999999999999996,0.69,0.44,5.5,0.74,0.53,5.5,0.98,0.65,6.1,0.8,0.5,5.2,0.66,0.48,5.4,0.84,0.54,5.2,0.86,0.57999999999999996,6.4,0.79,0.49,5.2,0.85,0.53,6,0.91,0.57999999999999996,5.3,0.67,0.45,5,0.78,0.53,4.5,0.82,0.63,5.0999999999999996,0.91,0.59,5.3,0.82,0.5,5.8,1.1200000000000001,0.69,3.3,0.78,0.54,6,0.89,0.56000000000000005,3.4,0.8,0.56000000000000005,6.3,0.74,0.46,5.6,0.77,0.5,5.8,0.75,0.54,4.9000000000000004,0.7,0.48,4.4000000000000004,0.68,0.44,4.4000000000000004,0.91,0.53,5.0999999999999996,0.7,0.44,4.5,1.06,0.7,5.0999999999999996,1.06,0.68,3.6,0.81,0.6,4.9000000000000004,0.74,0.51,4.9000000000000004,0.78,0.55000000000000004,5.5,0.89,0.63,3.8,0.79,0.51,3.2]
[null,"Dez",0.47,0.35,3.4,0.77,0.47,1,0.44,0.32,0.9,0.46,0.28000000000000003,3.5,0.53,0.38,3.8,0.44,0.33,2.4,0.46,0.35,1.9,0.41,0.27,2.6,0.55000000000000004,0.37,0.9,0.54,0.41,0.4,0.46,0.33,3.5,0.55000000000000004,0.35,0.9,0.46,0.33,3.1,0.48,0.34,3.5,0.53,0.38,1.1000000000000001,0.46,0.33,3,0.52,0.38,2.2000000000000002,0.7,0.53,2.6,0.46,0.3,3,0.53,0.37,1.5,0.41,0.32,3.1,0.45,0.32,2.5,0.62,0.4,3.1,0.48,0.31,2,0.37,0.26,2.5,0.52,0.39,2.4,0.51,0.34,3.7,0.54,0.37,2,0.5,0.36,3.7,0.55000000000000004,0.38,2.6,0.38,0.28000000000000003,2.2000000000000002,0.48,0.35,1.3,0.53,0.39,2.4,0.55000000000000004,0.38,2.5,0.46,0.35,3.1,0.8,0.44,0.3,0.44,0.3,3,0.6,0.39,0.4,0.46,0.32,3.3,0.41,0.27,2.7,0.43,0.31,2.9,0.46,0.31,2.1,0.43,0.32,1,0.36,0.28000000000000003,1.5,0.57999999999999996,0.38,2.4,0.39,0.28999999999999998,1.6,0.7,0.52,2.2000000000000002,0.7,0.46,1,0.52,0.38,1.9,0.45,0.3,1.9,0.48,0.32,2.8,0.6,0.41,0.9,0.53,0.39,0.1]
[null,"Jahr",2.83,1.54,10.5,3.14,1.67,8.4,2.79,1.51,9.1999999999999993,2.5499999999999998,1.52,10.9,2.67,1.55,9.9,2.63,1.5,9,2.71,1.58,8.6999999999999993,2.6,1.5,9.6,2.77,1.56,8.8000000000000007,2.89,1.59,8.6,2.5499999999999998,1.55,11,2.74,1.54,9.9,2.57,1.56,9.6999999999999993,2.61,1.59,10.6,2.74,1.55,9.1999999999999993,2.5499999999999998,1.5,9.6999999999999993,2.83,1.58,9.8000000000000007,3.02,1.65,10.6,2.54,1.52,9.6999999999999993,2.85,1.61,8.9,2.61,1.5,9.3000000000000007,2.68,1.54,9.9,2.94,1.67,11.6,2.68,1.54,9.6,2.63,1.49,9.1999999999999993,2.76,1.55,9.6999999999999993,2.67,1.55,10.7,2.83,1.58,10.199999999999999,2.65,1.58,9.9,2.88,1.61,10.3,2.62,1.52,9.1,2.78,1.58,8.8000000000000007,2.83,1.54,10,2.88,1.64,10.3,2.69,1.59,9.6,3.16,1.68,8.9,2.65,1.6,10.199999999999999,2.87,1.64,8.9,2.56,1.56,10.5,2.6,1.55,9.6999999999999993,2.66,1.53,10,2.61,1.57,8.9,2.77,1.53,8.9,2.8,1.46,8.9,2.91,1.51,10,2.68,1.5,9,2.98,1.61,10.6,3.05,1.54,8.6,2.82,1.53,9.8000000000000007,2.7,1.55,8.8000000000000007,2.59,1.57,9.4,2.99,1.63,9.1,2.76,1.54,7.7]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A18","v":"France"},"Stadt","Bordeaux",null,null,"Brest",null,null,"Le Havre",null,null,"Lille",null,null,"Lyon",null,null,"Marseille",null,null,"Metz",null,null,"Montpellier",null,null,"Nantes",null,null,"Paris",null,null,"Toulouse",null,null,"Strasbourg"]
[null,"Breitengrad",44.8,null,null,48.4,null,null,49.5,null,null,50.65,null,null,45.7,null,null,43.3,null,null,49.12,null,null,43.6,null,null,47.23,null,null,50.83,null,null,43.6,null,null,48.56]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",1.32,0.79,7,0.87,0.53,8.6999999999999993,0.88,0.53,6.6,0.7,0.46,3.7,1.03,0.6,3.8,1.74,0.86,8.6999999999999993,0.76,0.48,2.2000000000000002,1.68,0.7,7.2,1.01,0.69,6.1,0.74,0.51,4.5,1.37,0.73,6.4,0.81,0.56000000000000005,1.9]
[null,"Feb",1.99,1.2,7.4,1.54,1.05,8.5,1.6,1.03,6.8,1.34,0.83,5,1.76,1.1499999999999999,5,2.83,1,8.6999999999999993,1.51,0.99,3.6,2.52,1.1000000000000001,7.9,1.77,0.97,6.6,1.35,1.02,5.6,2.17,1.23,6.9,1.58,1.1000000000000001,3.5]
[null,"Mar",3.26,1.72,10.6,2.57,1.52,8.9,2.65,1.51,8,2.2799999999999998,1.47,7.4,2.98,1.63,9.3000000000000007,4.3099999999999996,1.48,11.2,2.5099999999999998,1.58,6.9,3.82,1.64,11.2,2.93,1.48,9.1999999999999993,2.3199999999999998,1.52,8.6999999999999993,3.33,1.69,10.1,2.61,1.46,7.1]
[null,"Apr",4.3,2.29,12.4,3.87,2.17,9.4,4.0199999999999996,2.2400000000000002,9.3000000000000007,3.77,2.4,10,4.25,2.31,11.7,5.12,2.23,13.3,3.87,2.13,9.8000000000000007,4.9400000000000004,2.11,13.5,4.18,2.37,10.8,3.54,1.98,10.9,4.5999999999999996,2.27,12.1,3.98,2.2599999999999998,10.7]
[null,"Mai",5.3,2.54,16.5,5.04,2.6,11.9,5,2.74,12.3,4.75,2.58,13.7,5.08,2.82,16.8,6.42,2.6,17.7,4.9000000000000004,2.4300000000000002,14.6,5.93,2.82,17.8,5.3,2.5099999999999998,14.6,4.4800000000000004,2.5,15,5.37,2.52,16.2,4.99,2.4300000000000002,15.6]
[null,"Jun",5.88,2.79,20,5.3,2.98,14.4,5.41,3.22,15.4,5.12,3.07,16.7,5.78,2.59,20.8,7.26,2.42,22,5.33,3.15,18,6.89,2.5,22.1,5.86,2.93,17.899999999999999,4.8899999999999997,2.81,18.5,6.03,3,20.6,5.4,2.76,19]
[null,"Jul",5.93,2.79,20.8,5.09,2.9,16,5.31,2.6,16.899999999999999,4.95,2.66,17.899999999999999,6.02,2.74,21.9,7.13,2.17,24.1,5.39,2.66,19.100000000000001,6.94,2.4700000000000002,24,5.74,2.82,19.100000000000001,4.97,2.96,19.600000000000001,6.18,2.69,21.9,5.38,2.97,19.7]
[null,"Aug",5.21,2.5,21.7,4.5599999999999996,2.4300000000000002,17,4.58,2.36,18.3,4.41,2.44,18.8,5.0999999999999996,2.11,22.3,6.08,2.0499999999999998,24.4,4.62,2.2200000000000002,19.7,5.9,2.15,23.9,5.14,2.39,19.899999999999999,4.43,2.36,20.6,5.36,2.34,22.4,4.68,2.4700000000000002,20.100000000000001]
[null,"Sep",4.0599999999999996,1.8,18.3,3.44,1.79,15.9,3.31,1.85,16.399999999999999,2.98,1.62,15.6,3.82,1.63,17.600000000000001,4.6399999999999997,1.72,20.5,3.24,1.67,15.2,4.46,1.77,19.7,3.91,1.65,17,3.13,1.72,16.5,4.1900000000000004,1.86,18.7,3.31,1.71,15.6]
[null,"Okt",2.59,1.31,14.8,1.97,1.1399999999999999,13.7,1.95,1.2,13.4,1.75,1,11.6,2.21,1.29,13.6,3.01,1.33,17.2,1.82,1.1200000000000001,10.9,2.81,1.26,16.2,2.21,1.27,13.4,1.9,1.1399999999999999,12.5,2.71,1.25,14.9,1.8,1.1499999999999999,11.1]
[null,"Nov",1.51,0.93,9.1,1.1599999999999999,0.72,10.7,1.1200000000000001,0.62,9.3000000000000007,0.86,0.52,6.9,1.23,0.73,7.3,1.95,0.84,11.4,0.94,0.64,5.9,1.89,0.96,10.3,1.32,0.72,8.6,1.08,0.72,7.5,1.61,0.92,8.6,0.96,0.69,5.6]
[null,"Dez",1.1000000000000001,0.62,7,0.72,0.47,9.1,0.72,0.48,6.9,0.52,0.37,4.2,0.85,0.52,4.4000000000000004,1.5,0.75,8.8000000000000007,0.6,0.41,3.1,1.44,0.71,7.4,0.84,0.61,6.2,0.57999999999999996,0.45,5,1.18,0.7,6.3,0.65,0.42,2.8]
[null,"Jahr",3.54,1.78,13.8,3.01,1.69,12,3.05,1.7,11.6,2.79,1.62,11,3.34,1.68,12.9,4.33,1.62,15.7,2.96,1.63,10.8,4.0999999999999996,1.69,15.1,3.35,1.7,12.5,2.78,1.64,12.1,3.67,1.77,13.8,3.01,1.67,11.1]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A19","v":"Switzerland"},"Stadt","Altdorf",null,null,"Appenzell",null,null,"Ausserbin",null,null,"Basel",null,null,"Bern",null,null,"Buchs-Suhr",null,null,"Chur-Ems",null,null,"Davos",null,null,"Engelberg",null,null,"Fahy",null,null,"Fribourg",null,null,"Geneve",null,null,"Glarus",null,null,"Hinterrhein",null,null,"Interlaken",null,null,"La Chaux-de-Fonts",null,null,"La Dole",null,null,"Lausanne",null,null,"Locarno",null,null,"Lugano",null,null,"Luzern",null,null,"Moleson",null,null,"Montana",null,null,"Neuchatel",null,null,"Payerne",null,null,"Saint-Aubin",null,null,"Schaffhausen",null,null,"Schwyz",null,null,"Sion",null,null,"Solothurn",null,null,"St. Gallen",null,null,"Taenikon",null,null,"Wädenswil",null,null,"Winterthur",null,null,"Zermatt",null,null,"Zürich",null,null,"Zug"]
[null,"Breitengrad",46.870199999999997,null,null,47.33,null,null,46.38,null,null,47.58,null,null,46.95,null,null,47.384500000000003,null,null,46.8705,null,null,46.813099999999999,null,null,46.821599999999997,null,null,47.4236,null,null,46.804000000000002,null,null,46.22,null,null,47.04,null,null,46.52,null,null,46.67,null,null,47.09,null,null,46.43,null,null,46.53,null,null,46.17,null,null,null,null,null,47.05,null,null,46.55,null,null,46.31,null,null,47,null,null,46.81,null,null,46.38,null,null,47.698999999999998,null,null,47.021000000000001,null,null,46.22,null,null,47.21,null,null,47.426000000000002,null,null,47.48,null,null,47.22,null,null,47.5,null,null,46.03,null,null,47.38,null,null,47.167999999999999]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",1.01,0.57999999999999996,0.3,1.02,0.53,0.2,1.5,0.64,-1.4,0.98,0.53,1.5,1.05,0.65,0.4,0.79,0.51,-0.3,1.37,0.6,-0.5,1.78,0.65,-5.3,1.27,0.61,-2.7,0.98,0.55000000000000004,-0.1,0.98,0.56000000000000005,0.5,0.96,0.57999999999999996,1.8,1.17,0.57999999999999996,1.2,1.68,0.65,-6.6,1.18,0.59,-1,1.32,0.56999999999999995,-2,1.44,0.62,-3.1,1.03,0.56999999999999995,0.8,1.44,0.76,2.6,1.27,0.78,2.6,0.89,0.55000000000000004,0.8,1.51,0.67,-4,1.66,0.74,-2.5,0.82,0.54,0.5,0.98,0.63,-0.8,0.9,0.63,2.1,0.84,0.53,0.5,0.99,0.57999999999999996,2.8,1.48,0.59,-0.6,0.93,0.62,0.2,1,0.54,0.2,0.94,0.54,-1.1000000000000001,0.94,0.56000000000000005,-0.4,0.92,0.55000000000000004,0.5,1.68,0.63,-4.8,0.91,0.61,0.5,0.93,0.56000000000000005,2]
[null,"Feb",1.9,1.03,1.7,1.7,1.07,1.3,2.5099999999999998,0.97,-1.3,1.68,1.0900000000000001,3,1.8,1,1.8,1.51,0.88,1.2,2.23,1,1.3,2.71,0.77,-4.7,2.2400000000000002,0.92,-1.6,1.7,1.03,1.1000000000000001,1.75,1.1100000000000001,1.9,1.8,1.1399999999999999,3,1.99,1.08,2.4,2.91,0.79,-5.8,2.02,1.1299999999999999,0.6,2.06,0.87,-1,2.11,0.93,-3.2,1.83,1.0900000000000001,2.1,2.11,1.18,4.0999999999999996,1.87,1.1100000000000001,4,1.56,0.94,1.9,2.38,0.88,-4.0999999999999996,2.59,0.91,-2.1,1.58,0.99,2,1.7,0.98,0.8,1.68,1.17,3.1,1.61,1.06,1.9,1.78,1.07,3.6,2.38,1.01,1.6,1.68,1.08,1.3,1.68,1.08,1.3,1.68,0.98,0.2,1.7,1.1200000000000001,1,1.65,1.0900000000000001,1.8,2.83,0.88,-4,1.63,0.98,1.8,1.66,1.08,2.7]
[null,"Mar",3.1,1.69,4.7,2.73,1.66,4.5999999999999996,3.79,1.47,2.1,2.8,1.45,6.8,2.93,1.25,6.1,2.52,1.47,4.5,3.41,1.47,4.8,4.08,1.25,-2.2000000000000002,3.29,1.61,0.9,2.59,1.7,3.9,3,1.78,6,3.24,1.58,6.9,3.17,1.56,6.6,4.3,1.07,-3.1,3.14,1.7,3.8,3.05,1.55,1,3.12,1.64,-1.9,3.14,1.56,6.3,3.31,1.63,7.4,2.86,1.87,7.1,2.69,1.47,6,3.38,1.32,-3.3,3.77,1.53,-0.1,2.78,1.49,4.8,2.88,1.39,4,2.96,1.75,6.2,2.71,1.42,6.1,2.94,1.52,7.4,3.63,1.51,5.3,2.85,1.41,5.4,2.75,1.5,5,2.74,1.56,3.5,2.83,1.5,4.2,2.76,1.55,5.9,4.2699999999999996,1.39,-1.5,2.71,1.46,6,2.79,1.64,6.1]
[null,"Apr",4.18,2.2799999999999998,8.5,3.79,2.2200000000000002,7.6,4.72,2.0499999999999998,4.4000000000000004,3.74,1.9,9.8000000000000007,3.91,2.44,8.9,3.48,2.19,8.4,4.57,2.21,8.3000000000000007,5.08,2.0299999999999998,1.3,4.3,1.66,4.5,3.5,1.86,7,3.99,2.17,8.8000000000000007,4.1500000000000004,2.16,9.6999999999999993,4.09,2.11,9.9,5.26,2.0299999999999998,0.5,4.13,2.25,7.6,3.86,2.2400000000000002,4.3,3.86,1.93,0.8,4.2300000000000004,2.2999999999999998,9.1999999999999993,3.96,2.39,11,3.36,2.04,10.7,3.65,2.04,9.1999999999999993,4.42,2.17,-1,4.8499999999999996,1.82,3.2,3.84,2.1800000000000002,8.5,3.94,2.4700000000000002,7.7,3.97,2.12,8.6,3.89,2.2799999999999998,9.3000000000000007,4,2.2799999999999998,10.4,4.95,2.27,9.4,3.89,2.09,8.5,3.83,2.06,8,3.82,1.92,7.1,3.91,2.0299999999999998,8.1,3.9,2.02,9,5.38,1.87,2,3.84,2.09,9.1,3.9,2.38,8.8000000000000007]
[null,"Mai",5.29,2.68,12.8,4.66,2.77,12.8,5.43,2.67,9.6999999999999993,4.8899999999999997,2.57,14.8,4.83,2.54,14.2,4.42,2.8,12.8,5.34,2.61,12.7,5.91,2.33,5.9,5.16,2.5299999999999998,9.1,4.37,2.74,11.1,4.92,2.35,14,5.28,2.74,14.8,4.9400000000000004,2.76,14.9,5.42,2.4500000000000002,5.0999999999999996,5.0199999999999996,2.37,11.8,4.3899999999999997,2.2999999999999998,8.5,4.3,2.29,5,5.2,2.71,14.3,4.78,3,14.5,4.2,2.66,14.5,4.45,2.58,14.2,4.78,2.62,2.9,5.69,2.61,7.7,4.8,2.54,12.6,4.92,2.58,11.9,4.8899999999999997,2.91,13.5,4.92,2.5099999999999998,14.4,4.9400000000000004,2.31,15.2,5.76,2.56,13.7,4.91,2.38,13.7,4.72,2.5499999999999998,13.2,4.7,2.5,11.5,4.87,2.57,12.4,4.84,2.2999999999999998,13.9,6.06,2.4900000000000002,6.7,4.82,2.86,14.1,4.78,2.3199999999999998,13.6]
[null,"Jun",5.31,2.4900000000000002,15.6,4.97,2.87,16.100000000000001,5.73,2.11,13.4,5.44,2.95,18.399999999999999,5.34,2.8,17.899999999999999,4.9000000000000004,2.54,16.100000000000001,5.65,2.5499999999999998,15.6,5.94,2.31,9,4.97,2.75,12.1,5.0199999999999996,3.01,14.3,5.58,2.79,17.7,5.85,2.5299999999999998,18.7,5.13,2.73,18,5.73,2.46,8.9,5.23,3.03,14.9,4.99,2.4900000000000002,11.7,4.68,2.4300000000000002,8.6,5.81,2.82,18,5.66,2.95,18.100000000000001,5.0199999999999996,2.41,18.399999999999999,4.76,2.7,17.600000000000001,4.78,2.42,6.4,6.22,2.4300000000000002,11.2,5.33,2.74,16,5.52,3.03,15.3,5.58,2.75,17.100000000000001,5.4,2.56,17.899999999999999,5.15,3,18.2,6.39,2.54,17,5.47,2.8,17.399999999999999,5.07,2.59,16.5,5.16,2.92,14.9,5.21,2.88,15.7,5.29,2.93,17.399999999999999,6.51,2.74,10,5.28,2.68,17.600000000000001,5.13,2.75,17]
[null,"Jul",5.28,2.64,17.5,5.17,2.68,16.7,5.83,2.5099999999999998,14.2,5.4,2.88,19.100000000000001,5.57,2.52,18.600000000000001,5.35,2.38,18.2,5.71,2.6,17.7,5.96,2.6,11.3,4.99,2.6,14.3,5.5,2.57,16.7,5.56,2.52,18.5,5.81,2.5299999999999998,19.7,5.21,2.2599999999999998,18.399999999999999,5.75,2.52,11.5,5.4,2.78,17.100000000000001,5.62,2.6,14.3,5.33,2.57,11.4,5.94,2.8,18.8,6.05,2.46,20.8,5.38,2.63,21.1,5,2.71,18.3,5.4,2.62,9.1999999999999993,6.3,2.38,13.9,5.83,2.5499999999999998,18.600000000000001,5.98,2.29,17.7,5.54,2.73,18.3,5.5,2.35,18.5,5.24,2.62,19,6.36,2.12,19.100000000000001,5.52,2.59,18.2,5.23,2.62,17.100000000000001,5.57,2.71,17,5.59,2.59,18,5.45,2.67,18,6.37,2.08,12.5,5.54,2.93,18.2,5.31,2.46,17.899999999999999]
[null,"Aug",4.46,2.14,16.7,4.45,2.4500000000000002,17.3,5.07,2.0499999999999998,14.7,4.75,2.4900000000000002,19.5,4.82,2.2200000000000002,18.899999999999999,4.42,2.5299999999999998,17.2,4.82,2.42,16.899999999999999,5.16,2.09,10.8,4.38,2.08,13.6,4.68,2.1800000000000002,16.2,4.79,2.34,18.8,4.99,2.48,19.7,4.33,2.25,18.8,4.8899999999999997,2.1800000000000002,10.9,4.63,2.2400000000000002,16.100000000000001,4.75,2.0299999999999998,13.7,4.6100000000000003,2.13,11.1,5.08,2.2000000000000002,19,5.26,2.12,19.899999999999999,4.99,2.2200000000000002,20.3,4.37,1.95,18.600000000000001,4.8,2.0699999999999998,8.8000000000000007,5.4,2.37,13.1,4.92,2.17,17.899999999999999,5.0599999999999996,2.25,17,4.7699999999999996,2.38,18.899999999999999,4.72,2.2599999999999998,18.899999999999999,4.47,2.5,19.399999999999999,5.38,2.2400000000000002,18,4.75,2.37,18.399999999999999,4.5,2.0699999999999998,17.7,4.7300000000000004,2.39,16.2,4.75,2.37,17,4.67,2.12,18.5,5.57,2.19,11.7,4.68,2.2000000000000002,18.600000000000001,4.57,2.4500000000000002,18.600000000000001]
[null,"Sep",3.51,1.75,14,3.12,1.65,12.9,3.79,1.95,10.7,3.26,1.84,14.8,3.45,1.75,14.3,3.12,1.88,14,3.67,1.72,14.2,3.78,1.73,8.3000000000000007,3.29,1.77,11,3.38,1.82,13.4,3.41,1.79,14.3,3.58,1.88,15.4,3.48,1.88,14.6,3.63,1.79,8.3000000000000007,3.48,1.81,13.3,3.55,1.77,11.3,3.62,1.65,8.9,3.67,1.65,14.5,3.84,1.88,16.8,3.67,1.72,17.2,3.1,1.84,14.3,3.74,1.67,7.1,4.0999999999999996,1.82,10.8,3.58,1.77,14.8,3.65,1.71,13.8,3.38,1.76,14.9,3.31,1.84,14.3,3.37,1.88,15.5,4.01,1.93,14.8,3.34,1.72,13.9,3.15,1.81,13.3,3.34,1.84,13.2,3.38,1.77,14.2,3.32,1.54,14,4.33,1.68,9,3.37,1.93,14.1,3.28,1.61,14.7]
[null,"Okt",2.13,1.19,9.6999999999999993,1.89,1.07,9.4,2.52,1.1299999999999999,7.3,1.94,0.94,10.8,2.0099999999999998,1.08,10,1.75,1.2,9.3000000000000007,2.4900000000000002,1.32,9.6999999999999993,2.71,1.1599999999999999,4.5,2.2799999999999998,1.1399999999999999,7,2.04,1.06,9.1,2.0099999999999998,1.1200000000000001,10,2.12,1.01,11.1,2.17,1.1599999999999999,10.8,2.46,1.24,4.0999999999999996,2.2599999999999998,1.29,8.6999999999999993,2.2799999999999998,1.1299999999999999,7.4,2.4500000000000002,1.24,5.6,2.2000000000000002,1.18,10.3,2.2799999999999998,1.21,12,2.14,1.1599999999999999,12.5,1.85,1.07,10.3,2.66,1.23,4.5999999999999996,2.76,1.23,6.9,1.99,1.17,10,2.04,1.21,9,1.97,1.1299999999999999,10.9,1.83,1.05,10,2.02,1.23,11.9,2.66,1.34,9.6999999999999993,1.88,1.1399999999999999,9.6999999999999993,1.89,1.02,9.6,1.92,1.1000000000000001,8.5,1.99,1.19,9.5,1.89,1.1000000000000001,10,2.91,1.23,4.8,1.91,0.94,9.9,1.91,1.1599999999999999,10.8]
[null,"Nov",1.28,0.84,4.5999999999999996,1.0900000000000001,0.69,3.7,1.51,0.78,1.5,1.05,0.7,5.0999999999999996,1.1499999999999999,0.71,4,0.84,0.61,4,1.46,0.76,3.9,1.73,0.75,-1.1000000000000001,1.47,0.64,1.5,1.1499999999999999,0.69,4.0999999999999996,1.1000000000000001,0.73,4,1.08,0.68,5.2,1.27,0.79,5,1.63,0.79,-1.7,1.34,0.86,3.2,1.39,0.78,1.8,1.56,0.72,0.2,1.23,0.76,4.3,1.51,0.78,6.7,1.39,0.88,7.3,1.01,0.64,4.5,1.68,0.72,-0.2,1.75,0.73,1.5,0.94,0.61,4.5999999999999996,1.03,0.7,3.7,1.05,0.72,5.2,0.96,0.71,4.2,1.1599999999999999,0.71,6.5,1.59,0.81,3.7,1.01,0.67,3.8,1.07,0.72,3.8,0.98,0.71,3.3,1.01,0.61,4.3,1.01,0.64,4.2,1.84,0.79,-0.8,0.97,0.7,4.2,1.04,0.64,5.2]
[null,"Dez",0.87,0.57999999999999996,1,0.8,0.49,0.9,1.17,0.59,-0.9,0.72,0.49,2.4,0.81,0.53,1.2,0.6,0.46,0.7,1.06,0.61,-0.1,1.29,0.54,-4.4000000000000004,0.94,0.56999999999999995,-2,0.84,0.51,0.8,0.77,0.53,1.3,0.77,0.56000000000000005,2.6,0.91,0.51,2,1.32,0.56999999999999995,-5.6,0.91,0.55000000000000004,-0.2,1.08,0.6,-1.2,1.27,0.56999999999999995,-2,0.86,0.56000000000000005,1.6,1.2,0.67,3.7,1.08,0.65,3.8,0.7,0.44,1.8,1.34,0.59,-2.7,1.32,0.56000000000000005,-1.3,0.67,0.47,1.4,0.77,0.52,0.3,0.72,0.54,3,0.67,0.46,1.5,0.8,0.5,3.7,1.18,0.54,-0.1,0.7,0.51,1.2,0.78,0.43,1,0.72,0.49,0,0.74,0.53,0.7,0.71,0.49,1.4,1.4,0.62,-3.8,0.7,0.43,1.5,0.72,0.51,2.8]
[null,"Jahr",3.19,1.66,8.9,2.95,1.68,8.6,3.63,1.58,6.2,3.05,1.66,10.5,3.14,1.63,9.6999999999999993,2.81,1.62,8.8000000000000007,3.48,1.66,8.6999999999999993,3.84,1.52,2.8,3.21,1.58,5.6,2.98,1.65,8.1,3.16,1.65,9.6999999999999993,3.3,1.66,10.7,3.16,1.64,10.199999999999999,3.75,1.55,2.2000000000000002,3.23,1.72,8,3.2,1.58,5.8,3.2,1.56,3.5,3.35,1.69,9.9,3.45,1.75,11.5,3.1,1.68,11.6,2.84,1.58,9.8000000000000007,3.41,1.58,2,3.87,1.6,5.2,3.09,1.6,9.3000000000000007,3.21,1.65,8.4,3.12,1.72,10.199999999999999,3.03,1.59,9.8000000000000007,3.07,1.69,11.1,3.81,1.62,9.3000000000000007,3.08,1.62,9.3000000000000007,2.97,1.58,8.9,3.02,1.64,7.9,3.08,1.65,8.6999999999999993,3.03,1.59,9.6,4.0999999999999996,1.55,3.5,3.03,1.65,9.6,3,1.63,10]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A20","v":"USA"},"Stadt","Albany",null,null,"Anchorage",null,null,"Atlanta",null,null,"Baltimore",null,null,"Beaumont",null,null,"Boston",null,null,"Buffalo",null,null,"Chattanooga",null,null,"Chicago",null,null,"Cincinnati",null,null,"Cleveland",null,null,"Colorado",null,null,"Dallas",null,null,"Denver",null,null,"Detroit",null,null,"El Paso",null,null,"Glendale",null,null,"Greensboro",null,null,"Hampton",null,null,"Houston",null,null,"Indianapolis",null,null,"Irvine",null,null,"Kansas City",null,null,"Knoxville",null,null,"Las Vegas",null,null,"Lincoln",null,null,"Los Angeles",null,null,"Luisville",null,null,"Memphis",null,null,"Miami",null,null,"Minneapolis",null,null,"Montgomery",null,null,"New Orleans",null,null,"New York",null,null,"Oklahoma",null,null,"Orlando",null,null,"Philadelphia",null,null,"Phoenix",null,null,"Sacramento",null,null,"Salt Lake City",null,null,"Seattle",null,null,"Washington"]
[null,"Breitengrad",42.67,null,null,61.16,null,null,33.799999999999997,null,null,39.299999999999997,null,null,30.08,null,null,42.33,null,null,42.88,null,null,35.03,null,null,41.83,null,null,39.200000000000003,null,null,41.5,null,null,41.5,null,null,32.83,null,null,39.75,null,null,42.33,null,null,31.8,null,null,34.15,null,null,36.07,null,null,37.03,null,null,29.8,null,null,39.75,null,null,33.68,null,null,39,null,null,35.79,null,null,36.17,null,null,40.799999999999997,null,null,34,null,null,38.25,null,null,35.119999999999997,null,null,25.87,null,null,44.95,null,null,32.380000000000003,null,null,30.01,null,null,40.75,null,null,35.47,null,null,28.5,null,null,40,null,null,33.5,null,null,38.5,null,null,40.75,null,null,47.58,null,null,38.869999999999997]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",1.75,0.93,-5.2,0.31,0.19,-7.3,2.56,1.07,6.5,2.04,0.85,1.1000000000000001,2.7,1.45,12,1.88,0.86,-0.5,1.59,0.77,-4.0999999999999996,2.38,1.1499999999999999,5.2,1.82,0.75,-3.5,1.94,0.89,-0.2,1.61,0.89,-1.9,2.52,0.91,-0.4,2.88,1.27,8.6999999999999993,2.4,0.86,0.5,1.64,0.84,-3.5,3.7,0.98,8.9,3.02,1.02,13.2,2.4,1.1000000000000001,4,2.2200000000000002,0.98,4.5999999999999996,2.65,1.56,12.5,1.94,0.89,-1.9,2.92,1.03,14,2.2400000000000002,0.99,-1.1000000000000001,2.2000000000000002,1.1000000000000001,3.9,2.99,0.83,9.5,2.35,0.85,-4.3,2.93,1.1499999999999999,14.3,2.0099999999999998,0.93,1.8,2.44,1.1200000000000001,5.7,3.52,1.45,19.5,1.77,0.68,-8.8000000000000007,2.64,1.1200000000000001,9.6999999999999993,2.71,1.25,14.2,1.8,0.82,0.1,2.66,1.1299999999999999,3.4,3.34,1.29,15.4,1.94,0.94,0.3,3.28,0.92,13.5,1.91,1.1100000000000001,8.1999999999999993,2.02,0.8,0.1,0.84,0.59,7.3,2.17,0.97,1.9]
[null,"Feb",2.59,1.17,-2.2999999999999998,0.96,0.54,-4.2,3.4,1.67,8.5,2.88,1.29,3.2,3.5,1.39,13.5,2.69,1.1499999999999999,1.3,2.34,1.27,-2.2000000000000002,3.1,1.35,7.3,2.62,1.26,0,2.67,1.4,2.5,2.4,1.3,0.5,3.38,1.23,0.4,3.65,1.49,11,3.3,1.1299999999999999,1.3,2.46,1.35,-1,4.9000000000000004,0.93,10.8,3.92,1.33,13.1,3.22,1.5,5.9,3.01,1.6,6.2,3.42,1.84,14.1,2.78,1.1599999999999999,1.4,3.78,1.34,14.1,3,1.19,2.6,2.95,1.39,6.2,4,1.08,11,3.14,1.1499999999999999,-0.7,3.79,1.41,14.4,2.83,1.35,4.5999999999999996,3.24,1.33,8.3000000000000007,4.22,1.78,21.1,2.71,1.01,-4.8,3.48,1.59,12,3.55,1.8,15.4,2.6,1.33,2.2999999999999998,3.5,1.31,6.4,4.2300000000000004,1.68,17.2,2.73,1.37,2.6,4.3600000000000003,1.1200000000000001,14.8,2.97,1.26,10.199999999999999,3.15,1.19,1,1.65,1.1299999999999999,7.4,3.03,1.39,4.0999999999999996]
[null,"Mar",3.57,1.81,1.6,2.2799999999999998,1.0900000000000001,-2.7,4.5599999999999996,1.91,12.1,3.89,1.82,6.9,4.32,2.2799999999999998,16.399999999999999,3.72,1.78,3.4,3.39,1.75,0.8,4.08,1.93,11,3.49,1.7,3.5,3.61,1.83,6,3.34,1.77,3.2,4.49,1.76,3.8,4.7,1.86,14,4.43,1.73,4.9000000000000004,3.46,1.83,2.4,6.34,1.1299999999999999,14.8,5.03,1.67,15,4.32,1.83,9.5,4.07,1.86,9.4,4.2300000000000004,2.23,16.8,3.6,1.82,5,4.92,1.78,15.5,3.94,1.82,6.4,3.95,2.13,9.9,5.4,1.46,15.7,4.2,1.65,3.7,4.92,1.7,15.7,3.79,1.95,8,4.24,2.14,11.6,5.13,2.34,22.6,3.74,1.62,-0.3,4.51,1.96,15.5,4.4400000000000004,2.27,17.8,3.67,1.9,5.4,4.46,1.74,9.6999999999999993,5.34,2.0299999999999998,19.399999999999999,3.79,1.78,5.9,5.61,1.6,18.7,4.3099999999999996,1.75,12.8,4.5599999999999996,1.44,6.5,2.91,1.74,8.4,4.04,2.1,7.6]
[null,"Apr",4.5599999999999996,2.4300000000000002,8.5,3.65,1.87,2.7,5.66,2.2999999999999998,16.5,4.9000000000000004,2.4,12.7,5.14,2.42,20.3,4.71,2.2599999999999998,8.1999999999999993,4.54,2.0499999999999998,7.2,5.26,2.44,15.8,4.58,2.35,10.199999999999999,4.75,2.2799999999999998,12.3,4.6100000000000003,2.14,9.4,5.64,2.29,8.1,5.59,2.17,19.2,5.55,2.1,8.9,4.5999999999999996,2.4900000000000002,9.1,7.63,1.22,19.3,6.29,2.0499999999999998,16.3,5.4,2.4300000000000002,14.6,5.13,2.4,14.4,5.0199999999999996,2.4900000000000002,20.7,4.75,2.37,11.9,6.18,2.14,16.5,5.0999999999999996,2.15,13.3,5.16,2.1,14.8,6.91,1.52,19,5.16,2.08,11.1,6.17,2.21,16.5,4.9400000000000004,2.4700000000000002,14.2,5.4,2.2799999999999998,17.3,6,2.59,24,4.7,2.12,8.5,5.64,2.2200000000000002,19.399999999999999,5.52,2.58,21.3,4.66,2.14,11.1,5.47,2.0299999999999998,15.5,6.33,2.14,21.6,4.8,2.46,11.8,7.22,1.48,22.3,5.9,2.0299999999999998,14.6,5.76,1.9,10.199999999999999,4.07,2.25,10.3,5.09,2.38,13.4]
[null,"Mai",5.37,2.54,14.4,4.5599999999999996,2.4500000000000002,8.6999999999999993,6.42,2.57,21.1,5.63,2.66,17.7,5.84,2.73,24.4,5.62,2.4300000000000002,13,5.5,2.58,13.6,5.81,2.76,20.5,5.7,2.4300000000000002,15.6,5.73,2.9,17.399999999999999,5.6,2.78,15.3,6.2,2.4,13.9,6.22,2.62,24.2,6.19,2.23,14.6,5.68,2.8,15,8.26,1.58,25.6,6.6,2.61,18.899999999999999,5.95,2.67,19,5.76,2.44,19,5.62,2.68,24.8,5.95,2.5299999999999998,17.100000000000001,6.54,2.5,18.899999999999999,5.9,2.67,18.600000000000001,5.85,2.69,19.600000000000001,7.82,1.77,25.8,6.18,2.74,16.8,6.53,2.68,18.7,5.81,2.75,19.5,6.12,2.74,22.2,5.95,2.7,26.2,5.71,2.57,14.3,6.22,2.7,24.2,6.05,2.73,25.3,5.59,2.76,16.100000000000001,6.17,2.4300000000000002,20.8,6.77,2.48,24.9,5.55,2.34,16.8,8.02,1.59,28.8,7.2,2.17,18.8,7.06,2.23,16,5.29,2.8,13,5.9,2.71,18.2]
[null,"Jun",5.88,3.01,20,4.92,2.9,13.3,6.48,2.56,24.3,6.15,2.88,22.7,6.27,2.82,27,6.12,2.74,18.8,6.12,2.99,19.399999999999999,6.14,2.9,24,6.28,2.7,21.4,6.29,2.82,21.9,6.15,2.87,21.2,6.94,2.25,18.3,6.91,2.78,27.6,6.84,2.5,19.5,6.25,2.86,21.1,8.42,1.58,28.8,6.59,2.87,20.3,6.24,3.05,23.2,6.15,3.12,23.6,6.02,2.89,27.4,6.53,2.6,21.8,6.76,2.76,20.2,6.45,2.91,22.9,6.22,2.87,23.2,8.35,1.72,30.6,6.94,2.23,22.4,6.64,2.63,19.8,6.31,2.97,23.6,6.62,2.77,25.8,5.59,2.84,27.6,6.24,2.79,19.899999999999999,6.43,3.07,26.7,6.12,2.68,27.3,5.94,2.61,21.9,6.77,2.79,24.5,6.24,2.92,26.4,6.11,2.88,22.2,8.16,1.91,33.1,7.85,2.16,21.9,7.68,2.09,21.2,5.94,2.56,16,6.36,3.06,23.1]
[null,"Jul",5.91,2.58,21.8,4.63,2.5299999999999998,15.4,6.19,2.64,26.2,6.03,2.56,24.9,6.05,3.02,27.9,6.04,2.88,22.1,6.03,2.7,21.7,5.86,2.68,26.1,6.12,2.72,24.2,6.1,2.91,24,6.11,2.72,23.3,6.65,2.48,22.1,7.01,2.4300000000000002,30.4,6.7,2.4700000000000002,24.1,6.14,2.63,23.2,7.7,1.99,29,7.64,2.04,23.4,6.05,2.62,24.9,5.86,2.95,25.7,5.93,3,28.5,6.38,2.57,23.9,7.36,2.2999999999999998,22.4,6.56,2.33,26.1,5.91,2.91,25.1,7.85,1.96,33.799999999999997,6.88,2.42,25.6,7.45,2.15,21.6,6.12,2.75,25.8,6.5,2.5499999999999998,27.8,5.83,2.56,28.5,6.34,2.57,23,6.05,2.97,28.5,5.74,2.85,28.8,5.94,2.79,24.5,6.74,2.5099999999999998,27.9,6.14,2.84,27.4,5.94,2.88,24.7,7.39,2.33,35.299999999999997,7.94,1.82,24,7.82,1.87,26.8,6.13,2.68,19,6.1,2.85,25.4]
[null,"Aug",5.09,2.64,21.5,3.53,1.94,14.3,5.8,2.61,25.8,5.33,2.65,24.4,5.71,2.89,27.7,5.35,2.5,22.2,5.16,2.34,21.2,5.5,2.74,25.5,5.36,2.5499999999999998,23.2,5.47,2.5499999999999998,23.2,5.27,2.34,22.5,6.03,1.94,20,6.34,2.41,30.2,5.97,2.04,22,5.3,2.4900000000000002,22.3,7.18,1.89,27.8,6.98,1.98,24.2,5.52,2.76,24.3,5.4,2.76,25.2,5.62,2.54,28.3,5.78,2.31,23.3,6.8,1.93,23,5.77,2.4,25.3,5.48,2.37,24.7,7.2,1.68,32.799999999999997,5.98,2.0299999999999998,23.9,6.83,2.06,22.3,5.59,2.54,25.2,5.97,2.48,27.4,5.59,2.92,28.5,5.4,2.34,21.4,5.71,2.8,28,5.45,2.77,29.2,5.23,2.54,24.4,6.24,2.16,27.5,5.75,2.52,27.1,5.4,2.4300000000000002,24.4,6.89,2.09,34.299999999999997,7.03,1.77,23.6,6.77,1.81,25.3,5.23,2.39,19.399999999999999,5.5,2.65,24.9]
[null,"Sep",4.0199999999999996,1.94,17.3,2.23,1.1399999999999999,9.9,4.8499999999999996,2.14,22.6,4.4000000000000004,2.0099999999999998,20.7,4.9800000000000004,2.2599999999999998,25.9,4.25,1.88,19,3.92,1.79,17.7,4.54,2.21,22.4,4.2,1.86,19.600000000000001,4.4400000000000004,2.06,19.399999999999999,4.1100000000000003,2.0099999999999998,19.100000000000001,5.14,1.72,16.3,5.21,2.0499999999999998,26.5,4.99,1.81,17.7,4.13,2.04,18.899999999999999,6.1,1.45,25.6,5.58,1.78,22.5,4.6100000000000003,1.94,20.8,4.4800000000000004,2.2000000000000002,22.3,4.8600000000000003,2.4900000000000002,26.2,4.66,1.8,19.7,5.47,1.53,22,4.62,1.92,20.8,4.55,2.21,21.7,6.14,1.34,28,4.63,1.85,19.5,5.47,1.76,21.5,4.53,1.98,21.5,4.82,2.27,24.2,4.8899999999999997,2.46,27.8,4.08,1.9,17.399999999999999,4.92,2.2599999999999998,25.6,4.9000000000000004,2.2999999999999998,27.8,4.22,1.87,20.7,4.72,1.95,23.2,5.13,2.2599999999999998,26.4,4.3499999999999996,1.91,20.399999999999999,5.97,1.7,31.5,5.7,1.51,21.7,5.47,1.58,18.8,3.74,1.53,16.899999999999999,4.6100000000000003,1.87,21.2]
[null,"Okt",2.79,1.37,10,1.1000000000000001,0.71,2.2999999999999998,4.0999999999999996,1.57,17.100000000000001,3.31,1.47,13.7,4.29,1.74,21.2,3,1.44,12.7,2.64,1.37,10.7,3.79,1.58,16.399999999999999,3,1.54,12.7,3.26,1.35,12.9,2.84,1.55,12.8,4.01,1.19,10,4.2,1.58,20.5,3.8,1.34,10.9,2.83,1.28,11.8,5.26,1.1399999999999999,19.2,4.2699999999999996,1.54,19,3.74,1.53,15.1,3.47,1.65,16.3,4.21,1.86,21.7,3.43,1.54,13,4.26,1.4,19.3,3.55,1.26,14.1,3.72,1.28,15.5,4.72,0.99,20.8,3.5,1.34,12.2,4.2300000000000004,1.55,19.100000000000001,3.43,1.49,15.1,3.96,1.46,18,4.34,2.17,26.1,2.78,1.21,10,4.1500000000000004,1.52,20.2,4.32,1.81,23.6,3.12,1.46,13.9,3.96,1.54,16.5,4.51,1.84,23.5,3.21,1.48,13.5,4.82,1.25,24.3,4.0199999999999996,1.21,17.100000000000001,3.89,1.18,11.9,2.33,1.1499999999999999,12.6,3.46,1.57,14.4]
[null,"Nov",1.69,0.87,4.7,0.43,0.27,-3.4,3.08,1.19,11.8,2.2200000000000002,1.05,8.6,3.09,1.29,16.399999999999999,1.9,0.98,7.6,1.58,0.97,5.2,2.62,1.3,10.7,1.82,0.92,5.9,2.02,1.02,7.3,1.68,1.01,7.1,2.78,0.91,3.3,3.12,1.27,14.1,2.64,0.86,4.2,1.71,0.95,5.8,3.98,0.97,12.5,3.24,1.1299999999999999,15.3,2.64,1.23,10.199999999999999,2.5099999999999998,1.01,11.1,3.06,1.43,16.899999999999999,1.99,1.0900000000000001,6.7,3.21,1.08,16.2,2.36,1.08,7.3,2.46,1.23,9.6999999999999993,3.37,0.89,13.1,2.27,0.91,4.5,3.2,1.1000000000000001,16.5,2.2000000000000002,1.1599999999999999,9.1999999999999993,2.66,1.21,12,3.64,1.67,23.4,1.7,0.88,2.2999999999999998,3.03,1.31,15.1,3.12,1.37,18.899999999999999,1.85,1.08,8.8000000000000007,2.85,1.21,10,3.86,1.3,20,2.13,1.0900000000000001,8.5,3.57,1.03,17.5,2.39,1.1499999999999999,11.5,2.35,0.93,4.4000000000000004,1.08,0.7,8.6,2.2999999999999998,1.22,9.1999999999999993]
[null,"Dez",1.38,0.68,-0.9,0.17,0.11,-6.2,2.41,1.1200000000000001,6.6,1.77,0.94,3.4,2.5299999999999998,1.3,12.1,1.51,0.78,3.3,1.27,0.71,-0.4,2.11,1.03,5.7,1.46,0.8,-0.8,1.57,0.83,1.7,1.3,0.7,1,2.2799999999999998,0.84,-0.5,2.62,1.1200000000000001,9.1999999999999993,2.16,0.79,0.5,1.3,0.7,-0.3,3.41,0.89,7.4,2.77,0.97,13,2.14,1,5,2.0099999999999998,0.83,6.5,2.5099999999999998,1.1499999999999999,12.4,1.54,0.9,0.3,2.71,1.07,13.8,1.9,0.86,0.9,1.94,1.07,4.5999999999999996,2.73,0.78,8.6999999999999993,1.9,0.72,-2,2.7,0.93,14.2,1.72,0.82,3.2,2.1800000000000002,1.03,6.5,3.28,1.32,20.8,1.36,0.62,-5,2.5,1.24,10.5,2.59,1.24,14.9,1.47,0.88,3.6,2.42,0.99,4.5999999999999996,3.31,1.21,16.3,1.67,0.82,3.3,2.94,0.91,12.6,1.72,0.92,8.5,1.8,0.79,-0.2,0.69,0.49,6.9,1.82,0.96,4.0999999999999996]
[null,"Jahr",3.72,1.83,9.3000000000000007,2.4,1.32,3.6,4.63,1.94,16.600000000000001,4.05,1.89,13.3,4.54,2.14,20.399999999999999,3.9,1.81,10.9,3.67,1.78,9.1999999999999993,4.26,2.0099999999999998,15.9,3.87,1.8,11,3.99,1.91,12.4,3.75,1.84,11.1,4.67,1.66,9.6,4.87,1.92,19.600000000000001,4.58,1.66,10.8,3.79,1.86,10.4,6.07,1.32,19.100000000000001,5.16,1.75,17.899999999999999,4.3499999999999996,1.97,14.7,4.17,1.99,15.4,4.43,2.1800000000000002,20.9,4.1100000000000003,1.8,11.9,5.08,1.74,18,4.28,1.8,13.1,4.2,1.95,14.9,5.62,1.34,20.7,4.43,1.67,11.1,5.07,1.78,17.899999999999999,4.1100000000000003,1.93,14.3,4.51,1.95,17.2,4.83,2.2400000000000002,24.7,3.88,1.7,8.1999999999999993,4.6100000000000003,2.0699999999999998,19.600000000000001,4.54,2.14,22,3.84,1.85,12.7,4.66,1.82,15.8,5.08,2.04,22.1,3.97,1.87,12.9,5.69,1.5,23.9,4.91,1.57,16.100000000000001,4.8600000000000003,1.49,11.8,3.33,1.67,12.2,4.2,1.98,14]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A21","v":"Great Britain"},"Stadt","Aberdeen",null,null,"Ashfield",null,null,"Barnsley",null,null,"Enfield",null,null,"Lancaster ",null,null,"Leeds",null,null,"Liverpool",null,null,"London",null,null,"Manchester",null,null,"Ogwr",null,null,"Plymouth"]
[null,"Breitengrad",57.15,null,null,53.13,null,null,53.57,null,null,51.6,null,null,54.67,null,null,53.8,null,null,53.42,null,null,51.5,null,null,53.5,null,null,51.5,null,null,50.38]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.43,0.28999999999999998,5.8,0.6,0.37,4.3,0.6,0.35,4.5,0.63,0.44,4.7,0.45,0.28999999999999998,4.4000000000000004,0.57999999999999996,0.35,4.4000000000000004,0.57999999999999996,0.36,5.4,0.64,0.45,6.4,0.57999999999999996,0.35,5.0999999999999996,0.71,0.43,5.5,0.73,0.45,6.6]
[null,"Feb",1.03,0.68,5.3,1.1499999999999999,0.69,4.9000000000000004,1.1399999999999999,0.64,5,1.19,0.7,4.8,1.1000000000000001,0.61,4.4000000000000004,1.05,0.66,4.8,1.2,0.8,5.8,1.17,0.76,6.8,1.17,0.78,5.4,1.24,0.82,5.8,1.36,0.91,6.7]
[null,"Mar",2.09,1.0900000000000001,5.7,1.98,1.26,6.3,2.13,1.24,6.4,2.1800000000000002,1.45,6.3,2.02,1.17,5.6,2.0699999999999998,1.33,6.1,2.17,1.39,7.2,2.19,1.3,8.5,2.16,1.35,7,2.3199999999999998,1.39,7.2,2.46,1.65,8]
[null,"Apr",3.26,2.1,6.8,3.36,1.85,8.1999999999999993,3.29,2.0699999999999998,8.3000000000000007,3.41,1.94,8.4,3.01,1.84,7.3,3.21,1.86,8,3.61,2.23,8.9,3.37,2.06,10.4,3.55,2.0299999999999998,8.8000000000000007,3.44,2.0699999999999998,8.8000000000000007,4,2.21,9.4]
[null,"Mai",4.34,2.62,8.9,4.3,2.54,11.3,4.4400000000000004,2.31,11.3,4.3899999999999997,2.67,11.6,4.0999999999999996,2.63,10.4,4.47,2.33,11,4.83,2.91,12.1,4.3899999999999997,2.73,13.7,4.74,2.73,12,4.71,2.72,11.9,5.01,2.64,12.3]
[null,"Jun",4.7,3.15,11.5,4.46,2.77,14.3,4.72,2.73,14.1,4.79,2.91,14.7,4.42,2.86,12.7,4.8600000000000003,2.85,13.8,5.01,2.81,14.7,4.8099999999999996,2.42,16.899999999999999,5,2.85,14.5,5.0199999999999996,2.71,14.5,5.22,2.78,14.7]
[null,"Jul",4.25,2.7,13.6,4.4400000000000004,2.5299999999999998,16.100000000000001,4.68,2.69,15.8,4.54,2.5299999999999998,16.3,4,2.66,14.5,4.66,2.5299999999999998,15.6,4.7699999999999996,2.96,16.3,4.5599999999999996,2.46,18.399999999999999,4.78,2.74,16.2,4.6399999999999997,2.59,16.3,5.01,2.88,16.399999999999999]
[null,"Aug",3.58,2.12,14.3,3.85,2.36,16.600000000000001,3.86,2.33,16.3,3.91,2.13,16.5,3.52,2.44,14.7,3.77,2.11,16,3.9,2.3199999999999998,16.8,3.95,2.2799999999999998,19.100000000000001,3.91,1.92,16.600000000000001,3.98,2.12,16.8,4.3499999999999996,2.38,17]
[null,"Sep",2.38,1.45,13,2.62,1.45,13.9,2.64,1.53,13.8,2.81,1.86,14.3,2.2999999999999998,1.36,12.7,2.57,1.52,13.5,2.74,1.57,14.6,2.86,1.87,16.2,2.7,1.62,14.3,2.97,1.63,14.8,3.17,1.73,15.2]
[null,"Okt",1.3,0.83,10.199999999999999,1.45,0.94,10.3,1.5,0.81,10.3,1.62,1.08,10.7,1.24,0.78,9.4,1.49,0.96,10.1,1.52,0.98,11.2,1.65,1.02,12.7,1.5,0.87,10.8,1.72,1.06,11.5,1.81,1.04,12.2]
[null,"Nov",0.57999999999999996,0.35,7.4,0.78,0.49,6.8,0.77,0.42,6.8,0.84,0.54,7,0.64,0.39,6.5,0.79,0.48,6.6,0.73,0.49,8.1,0.83,0.57999999999999996,9,0.74,0.52,7.5,0.9,0.55000000000000004,8.3000000000000007,0.96,0.54,9.1]
[null,"Dez",0.28999999999999998,0.22,5.8,0.44,0.31,4.4000000000000004,0.46,0.31,4.5,0.48,0.37,4.8,0.37,0.24,4.5,0.47,0.33,4.2,0.42,0.3,5.5,0.49,0.34,6.7,0.43,0.32,5.0999999999999996,0.55000000000000004,0.35,5.9,0.57999999999999996,0.42,6.9]
[null,"Jahr",2.35,1.47,9,2.4500000000000002,1.47,9.8000000000000007,2.52,1.46,9.8000000000000007,2.57,1.56,10,2.2599999999999998,1.44,8.9,2.5,1.45,9.5,2.62,1.6,10.6,2.58,1.53,12.1,2.6,1.51,10.3,2.68,1.54,10.6,2.89,1.64,11.2]
[]
[]
[]
[]
[{"$f":"Translation!A24","v":"Czech Republic"},"Stadt","Brno",null,null,"Hradec Králové",null,null,"Liberec",null,null,"Olomouc",null,null,"Ostrava",null,null,"Plzen",null,null,"Praha",null,null,"Ústí nad Labem"]
[null,"Breitengrad",49.22,null,null,50.22,null,null,50.8,null,null,49.63,null,null,49.83,null,null,49.75,null,null,50.1,null,null,50.68]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.81,0.47,-1.9,0.74,0.46,-0.9,0.7,0.44,-1.8,0.79,0.46,-1.8,0.79,0.45,-1.8,0.72,0.51,-2,0.69,0.48,-0.8,0.74,0.43,-1.6]
[null,"Feb",1.66,0.9,0.3,1.41,0.94,1.1000000000000001,1.31,0.79,-0.3,1.51,0.94,0.2,1.49,1.01,0,1.4,0.82,-0.2,1.35,0.81,1.5,1.34,0.79,0.6]
[null,"Mar",2.66,1.51,4,2.54,1.56,4.2,2.39,1.27,2.6,2.4500000000000002,1.53,3.7,2.4,1.42,3.2,2.36,1.51,3,2.29,1.32,4.3,2.41,1.28,3.6]
[null,"Apr",4.07,2.23,9.6999999999999993,3.93,1.94,9.1,3.79,1.81,7.7,3.81,1.77,9.1999999999999993,3.67,2,8.9,3.82,2.2000000000000002,7.7,3.66,2.29,9.1,3.7,2.12,8.9]
[null,"Mai",5.34,2.84,15.1,5.21,2.48,14.7,4.84,2.68,13,4.9800000000000004,2.6,14.7,4.92,2.65,14.4,4.82,2.4,13.2,4.84,2.52,14.5,4.8099999999999996,2.34,13.9]
[null,"Jun",5.52,2.66,17.8,5.54,2.89,17.2,5.05,2.4,15.5,5.12,2.77,17.2,4.99,2.79,16.899999999999999,4.96,2.85,16,4.8899999999999997,2.5299999999999998,17.100000000000001,4.92,2.87,16.5]
[null,"Jul",5.4,2.66,19,5.23,2.88,18.3,4.8899999999999997,2.71,16.7,5.07,2.78,18.5,5.0199999999999996,2.81,18.399999999999999,4.83,2.89,17,4.8600000000000003,2.44,18.3,4.82,2.75,17.7]
[null,"Aug",4.76,2.23,19.600000000000001,4.6100000000000003,2.39,18.899999999999999,4.43,2.41,17.3,4.51,2.44,18.899999999999999,4.4400000000000004,2.34,18.5,4.42,2.1800000000000002,17.8,4.3899999999999997,2.14,19,4.3899999999999997,2.42,18.600000000000001]
[null,"Sep",3.13,1.93,14.3,3.19,1.56,13.9,2.89,1.83,12.7,2.92,1.75,13.7,2.83,1.71,13.6,2.91,1.72,12.8,2.86,1.8,14,2.9,1.69,13.7]
[null,"Okt",1.91,1.28,9.4,1.85,1.06,9.5,1.75,1.0900000000000001,8.6,1.86,1.01,9.3000000000000007,1.85,1.1100000000000001,9.4,1.81,1.03,8.1999999999999993,1.77,1.23,9.4,1.79,1.08,8.9]
[null,"Nov",0.9,0.61,4.0999999999999996,0.79,0.53,4.0999999999999996,0.79,0.52,3.4,0.86,0.55000000000000004,4.2,0.84,0.61,4.3,0.84,0.55000000000000004,2.7,0.78,0.56000000000000005,3.8,0.8,0.53,3.3]
[null,"Dez",0.63,0.43,-1.3,0.55000000000000004,0.42,-0.4,0.51,0.39,-1.1000000000000001,0.56000000000000005,0.41,-1.2,0.55000000000000004,0.38,-1,0.52,0.37,-1.3,0.49,0.39,-0.2,0.51,0.39,-0.9]
[null,"Jahr",3.06,1.65,9.1999999999999993,2.97,1.6,9.1,2.78,1.53,7.9,2.87,1.59,8.9,2.82,1.61,8.6999999999999993,2.78,1.59,7.9,2.74,1.54,9.1999999999999993,2.76,1.56,8.6]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A23","v":"Poland"},"Stadt","Bialystok ",null,null,"Bydgoszcz ",null,null,"Dabrowa Górnicza ",null,null,"Warschau",null,null,"Wloclawek",null,null,"Zabrze",null,null,"Zielona Góra"]
[null,"Breitengrad",53.15,null,null,53.27,null,null,53.27,null,null,52.25,null,null,52.65,null,null,50.3,null,null,51.95]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.73,0.39,-3.1,0.64,0.41,-1.5,0.64,0.41,-1.5,0.57999999999999996,0.42,-2,0.61,0.38,-1.5,0.74,0.45,-1.8,0.7,0.41,-0.8]
[null,"Feb",1.44,0.75,-1.7,1.29,0.82,0,1.29,0.82,0,1.17,0.76,-0.5,1.27,0.85,0,1.44,0.96,-0.2,1.36,0.75,1]
[null,"Mar",2.44,1.36,1.1000000000000001,2.36,1.31,2.5,2.36,1.31,2.5,2.29,1.46,2.2999999999999998,2.29,1.32,2.6,2.38,1.45,2.8,2.4300000000000002,1.37,3.5]
[null,"Apr",3.96,1.94,7.9,4,2.14,8.4,4,2.14,8.4,3.48,2,8.6999999999999993,3.75,2.04,8.6,3.72,2.09,8.6999999999999993,4.0199999999999996,1.93,9.1]
[null,"Mai",5.26,2.57,13.2,4.96,2.48,13.7,4.96,2.48,13.7,4.97,2.69,14.5,4.95,2.5,14,4.88,2.36,14.4,5.15,2.52,14.3]
[null,"Jun",5.26,2.99,16,5.16,2.85,16.3,5.16,2.85,16.3,5.28,2.65,16.899999999999999,5.13,2.74,16.600000000000001,5.0199999999999996,2.6,16.8,5.35,2.74,16.899999999999999]
[null,"Jul",5.2,2.72,18.3,4.8499999999999996,2.67,18.2,4.8499999999999996,2.67,18.2,5.13,2.5499999999999998,18.899999999999999,4.8899999999999997,2.83,18.600000000000001,4.9800000000000004,2.95,18.2,5.04,2.41,18.399999999999999]
[null,"Aug",4.45,2.33,17.3,4.28,2.2599999999999998,18.3,4.28,2.2599999999999998,18.3,4.42,2.29,18.600000000000001,4.4000000000000004,2.1800000000000002,18.600000000000001,4.41,2.52,18.2,4.67,2.35,19]
[null,"Sep",2.92,1.6,12,2.82,1.67,13.5,2.82,1.67,13.5,2.83,1.58,13.4,2.79,1.75,13.6,2.84,1.81,13.2,3.04,1.59,14.1]
[null,"Okt",1.75,1.02,7.5,1.68,0.96,8.6,1.68,0.96,8.6,1.62,0.94,8.6,1.67,0.96,8.8000000000000007,1.8,1,9,1.75,0.96,9.4]
[null,"Nov",0.85,0.52,2.4,0.87,0.53,3.4,0.87,0.53,3.4,0.68,0.51,3.3,0.8,0.55000000000000004,3.5,0.82,0.55000000000000004,3.8,0.88,0.56000000000000005,3.7]
[null,"Dez",0.51,0.34,-2.6,0.5,0.34,-0.7,0.5,0.34,-0.7,0.41,0.3,-1.4,0.46,0.3,-0.9,0.52,0.35,-1.3,0.54,0.35,-0.1]
[null,"Jahr",2.9,1.55,7.4,2.79,1.54,8.4,2.79,1.54,8.4,2.74,1.52,8.4,2.75,1.54,8.5,2.8,1.59,8.5,2.91,1.5,9]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A24","v":"Austria"},"Stadt","Innsbruck",null,null,"Linz",null,null,"Salzburg",null,null,"Wien"]
[null,"Breitengrad",47.28,null,null,48.3,null,null,47.8,null,null,48.22]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",1.22,0.57999999999999996,-1.4,0.92,0.53,-0.8,0.92,0.53,-0.8,0.85,0.51,0.8]
[null,"Feb",1.99,1.1000000000000001,0.6,1.64,0.87,1.3,1.64,0.87,1.3,1.58,1.05,2.9]
[null,"Mar",3.17,1.67,5.4,2.62,1.71,5.4,2.62,1.71,5.4,2.7,1.7,6.4]
[null,"Apr",4.03,2.41,9.1,3.9,1.96,10.3,3.9,1.96,10.3,4.03,1.93,11.7]
[null,"Mai",4.82,2.16,14.7,4.8600000000000003,2.5499999999999998,15.9,4.8600000000000003,2.5499999999999998,15.9,5.28,2.8,17.2]
[null,"Jun",4.92,2.96,17.399999999999999,4.9400000000000004,2.95,18.399999999999999,4.9400000000000004,2.95,18.399999999999999,5.58,3.04,19.899999999999999]
[null,"Jul",4.92,2.25,17.899999999999999,5.37,2.85,19.2,5.37,2.85,19.2,5.44,2.7,21.1]
[null,"Aug",4.32,2.3199999999999998,18.2,4.5,2.38,19.7,4.5,2.38,19.7,4.74,2.2000000000000002,21.6]
[null,"Sep",3.31,1.74,13.8,3.15,1.79,14.8,3.15,1.79,14.8,3.29,1.92,16.3]
[null,"Okt",2.38,1.08,9.6999999999999993,2.0499999999999998,1.07,10.1,2.0499999999999998,1.07,10.1,2.0299999999999998,1.1000000000000001,11.6]
[null,"Nov",1.39,0.71,3.4,0.98,0.64,4.7,0.98,0.64,4.7,0.97,0.63,6.4]
[null,"Dez",0.96,0.48,-0.6,0.71,0.46,0.3,0.71,0.46,0.3,0.66,0.44,1.4]
[null,"Jahr",3.12,1.62,9,2.97,1.65,9.9,2.97,1.65,9.9,3.09,1.67,11.4]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A25","v":"Sweden"},"Stadt","Boras",null,null,"Göteborg",null,null,"Helsingborg",null,null,"Joenkoeping ",null,null,"Linkoeping",null,null,"Malmoe",null,null,"Oerebro",null,null,"Stockholm",null,null,"Uppsala",null,null,"Vaesteras"]
[null,"Breitengrad",57.7,null,null,57.75,null,null,56.08,null,null,57.75,null,null,58.42,null,null,55.85,null,null,59.3,null,null,59.35,null,null,59.88,null,null,59.6]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.37,0.24,-1.1000000000000001,0.37,0.24,0,0.46,0.33,1.9,0.37,0.27,-2,0.39,0.24,-1.4,0.46,0.3,0.8,0.37,0.25,-1.9,0.31,0.22,-1.6,0.31,0.21,-2.6,0.34,0.23,-2.5]
[null,"Feb",0.91,0.57999999999999996,-0.9,0.9,0.61,0.1,1.04,0.7,2,0.92,0.59,-1.8,0.97,0.64,-1.6,1.01,0.69,1.1000000000000001,0.97,0.59,-1.5,0.94,0.52,-1.7,0.93,0.56000000000000005,-2.8,0.97,0.59,-2.5]
[null,"Mar",1.9,1.1599999999999999,0.8,1.87,1.1000000000000001,1.5,2.1,1.24,2.7,1.87,1.1000000000000001,0,2.15,1.1399999999999999,0.8,2.11,1.36,2.4,2.13,1.06,1,2.1800000000000002,1.06,0.9,2.14,0.96,-0.3,2.15,0.97,0.8]
[null,"Apr",3.5,1.84,5.7,3.49,1.97,6.3,3.78,2.08,6.6,3.58,1.85,5,3.59,1.8,5.7,3.79,1.97,6.7,3.58,1.94,6,3.67,1.73,6,3.64,1.69,5,3.64,1.68,6.3]
[null,"Mai",4.93,2.38,10.3,4.93,2.31,10.7,5.13,2.41,10.9,4.68,2.42,9.8000000000000007,5.24,2.33,10.8,5.21,2.56,11.2,5.1100000000000003,2.29,11.3,5.28,2.38,11,5.17,2.3199999999999998,9.9,5.14,2.19,11.5]
[null,"Jun",5.33,2.9,13.6,5.36,2.82,14.1,5.37,2.65,13.9,5,2.76,13.6,5.45,2.5099999999999998,14.8,5.37,2.77,14.5,5.4,2.66,15.1,5.81,2.62,15.6,5.7,2.7,14.3,5.61,2.89,15.9]
[null,"Jul",5.23,2.38,16,5.31,2.5,16.5,5.23,2.84,16.399999999999999,4.88,2.4900000000000002,15.7,5.24,2.87,17.100000000000001,5.24,2.61,16.899999999999999,5.22,2.58,17.600000000000001,5.33,2.72,18.600000000000001,5.23,2.76,17.2,5.22,2.77,18.600000000000001]
[null,"Aug",4.03,2.29,16.2,4.0199999999999996,2.16,16.8,4.26,2.19,17.399999999999999,3.94,1.91,15.7,4.28,1.97,16.7,4.25,2.2000000000000002,17.5,4.1500000000000004,2.08,16.8,4.2,2.29,18,4.16,2.08,16.399999999999999,4.1399999999999997,2.08,17.7]
[null,"Sep",2.56,1.47,11.9,2.57,1.44,12.9,2.66,1.67,13.9,2.4500000000000002,1.37,11.2,2.63,1.32,12.2,2.68,1.53,13.9,2.61,1.21,12,2.62,1.4,13.1,2.57,1.34,11.6,2.59,1.4,12.9]
[null,"Okt",1.22,0.69,7.1,1.22,0.78,8.1,1.39,0.97,9.4,1.24,0.77,6.3,1.23,0.73,6.9,1.39,0.84,9.4,1.18,0.67,6.5,1.18,0.69,7.3,1.1599999999999999,0.73,6.1,1.19,0.67,6.9]
[null,"Nov",0.53,0.34,2.8,0.53,0.33,3.9,0.6,0.43,5.3,0.54,0.34,2,0.44,0.31,2.7,0.61,0.38,5.2,0.47,0.32,2.1,0.41,0.28000000000000003,3,0.42,0.28999999999999998,1.8,0.45,0.31,2.2000000000000002]
[null,"Dez",0.25,0.17,-0.4,0.25,0.19,0.5,0.32,0.22,2.5,0.26,0.19,-1.5,0.22,0.17,-0.7,0.33,0.25,1.9,0.23,0.16,-1.4,0.19,0.15,-0.6,0.2,0.12,-1.8,0.22,0.15,-1.5]
[null,"Jahr",2.56,1.37,6.8,2.57,1.37,7.6,2.7,1.48,8.6,2.48,1.34,6.2,2.65,1.34,7,2.71,1.46,8.5,2.62,1.32,7,2.68,1.34,7.5,2.64,1.32,6.2,2.64,1.33,7.2]
[]
[]
[]
[]
[{"$f":"Zwischenwerte!A26","v":"Ireland"},"Stadt","Cork",null,null,"Dublin"]
[null,"Breitengrad",51.9,null,null,53.33]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.62,0.41,6.4,0.65,0.42,6.9]
[null,"Feb",1.26,0.9,6.6,1.18,0.75,6.5]
[null,"Mar",2.31,1.38,7.6,2.2400000000000002,1.1299999999999999,7]
[null,"Apr",3.86,2.11,8.6999999999999993,3.56,2,7.8]
[null,"Mai",4.78,2.59,11.2,4.63,2.58,10.199999999999999]
[null,"Jun",4.9800000000000004,2.57,13.4,4.78,2.56,12.8]
[null,"Jul",4.62,2.82,15.1,4.51,2.67,14.7]
[null,"Aug",4.01,2.11,15.4,3.84,2.2799999999999998,15.3]
[null,"Sep",2.85,1.75,14,2.72,1.67,14]
[null,"Okt",1.59,1.05,11.1,1.59,0.98,11]
[null,"Nov",0.86,0.52,8.4,0.82,0.46,8.4]
[null,"Dez",0.47,0.37,6.8,0.46,0.3,6.9]
[null,"Jahr",2.68,1.55,10.4,2.58,1.49,10.1]
[]
[]
[]
[]
[{"$f":"Translation!A29","v":"Italy"},"Stadt","Allessandria",null,null,"Ancona",null,null,"Bari",null,null,"Bergamo",null,null,"Bologna",null,null,"Bolzano",null,null,"Cagliari",null,null,"Catania",null,null,"Catanzaro",null,null,"Cosenza",null,null,"Ferrara",null,null,"Firenze",null,null,"Genova",null,null,"La Spezia",null,null,"Milano",null,null,"Napoli",null,null,"Palermo",null,null,"Parma",null,null,"Rimini",null,null,"Roma",null,null,"Taranto",null,null,"Venezia"]
[null,"Breitengrad",44.92,null,null,43.6,null,null,41.12,null,null,45.7,null,null,44.5,null,null,46.5,null,null,39.200000000000003,null,null,37.5,null,null,38.9,null,null,39.28,null,null,44.83,null,null,43.8,null,null,44.4,null,null,44.13,null,null,45.45,null,null,40.799999999999997,null,null,38.1,null,null,44.8,null,null,44.05,null,null,41.9,null,null,40.47,null,null,45.5]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",1.33,0.67,3.6,1.36,0.69,5.5,1.87,0.78,9.5,1.26,0.73,3,1.2,0.76,3.1,1.27,0.6,1.2,2.16,1,9.8000000000000007,2.2400000000000002,1.1200000000000001,10,2.0699999999999998,0.96,10.3,2.0499999999999998,0.86,8.9,1.18,0.75,3.4,1.39,0.7,5.7,1.38,0.79,10,1.41,0.69,6.5,1.08,0.69,3.4,1.68,0.93,10.5,2.19,1.0900000000000001,13.5,1.2,0.74,2.8,1.2,0.8,3.9,1.85,0.89,9.8000000000000007,1.82,0.94,11,1.18,0.65,4.7]
[null,"Feb",2.1,1.22,5.5,1.92,1.24,6.2,2.68,1.36,8.8000000000000007,2.0299999999999998,1.08,4.5999999999999996,1.71,1.1000000000000001,5.0999999999999996,2.09,0.94,4.5999999999999996,2.98,1.28,9.9,3.17,1.2,10.1,2.72,1.36,10.199999999999999,2.74,1.21,8.9,1.76,1.1399999999999999,5.2,2.2000000000000002,1.27,6.7,2.14,1.1200000000000001,10.5,2.2400000000000002,1.22,7.6,1.85,1.05,5.5,2.5099999999999998,1.25,10.1,3.04,1.28,12.8,1.96,1.1599999999999999,4.8,2.1,1.26,5.0999999999999996,2.62,1.23,9.9,2.64,1.19,10.8,1.97,1.1399999999999999,5.2]
[null,"Mar",3.31,1.81,9.8000000000000007,3.34,1.53,9.6,3.91,1.72,10.7,3.17,1.63,9,2.84,1.97,9.6,3.19,1.7,10.1,4.37,1.67,12.3,4.3899999999999997,1.77,12.1,3.92,1.87,12.1,3.94,1.55,10.9,2.93,1.71,9.6,3.33,1.67,10.3,3.23,1.87,12.1,3.38,1.82,10.8,3.07,1.61,10.1,3.72,1.76,11.9,4.33,1.85,13.8,3.25,1.81,9.5,3.42,1.83,8.9,3.94,1.74,12.2,3.9,1.84,12.3,3.14,1.77,8.8000000000000007]
[null,"Apr",4.3899999999999997,2.4300000000000002,12.8,4.99,2.25,12.6,5.37,2.35,12.9,4.1100000000000003,2.02,12.2,3.97,2.2400000000000002,13.1,4.41,2.14,13.2,5.35,2.2799999999999998,14.4,5.67,2.4500000000000002,14.5,5.35,2.4500000000000002,14.5,5.38,2.39,13.3,4.08,2.2400000000000002,13.2,4.58,2.4300000000000002,13.1,4.24,2.2799999999999998,13.6,4.67,2.12,13.1,4.45,2.36,13.2,5.03,2.37,13.7,5.62,2.38,15.4,4.25,2.17,13,4.3499999999999996,2.13,12.4,5.0999999999999996,2.4900000000000002,14,5.13,2.4,14.6,4.4400000000000004,2.2999999999999998,12.2]
[null,"Mai",5.32,2.5299999999999998,18.3,5.8,2.57,18.100000000000001,6.32,2.46,17.899999999999999,4.8899999999999997,2.78,18,4.95,2.62,19,4.51,2.84,18.399999999999999,6.62,2.5499999999999998,18.899999999999999,6.64,2.57,19,6.32,2.7,19.5,6.34,2.2799999999999998,18.5,5.15,2.91,19.2,5.67,2.65,18.7,5.15,2.6,18.100000000000001,5.67,2.65,18.3,5.15,2.67,19.2,6.03,2.5499999999999998,18.7,6.7,2.38,19.3,5.39,2.75,19,5.66,2.4700000000000002,17.8,6.2,2.58,19.2,6.2,2.58,20.2,5.66,2.86,17.7]
[null,"Jun",6.14,2.76,22.5,6.37,2.9,22.4,6.99,2.58,22.4,5.72,2.73,22.2,5.72,2.77,23.3,5.88,2.4500000000000002,22.1,7.46,2.5299999999999998,23.4,7.26,2.42,23.6,7.06,2.61,24,7.08,2.36,23.2,5.85,3.03,23.4,6.34,2.5299999999999998,23,6.05,2.91,21.9,6.53,2.56,22.3,5.85,2.73,23.4,6.88,2.57,23,7.45,2.36,23.4,6.07,2.67,23.2,6.09,2.8,22.4,6.76,2.89,23.7,6.96,2.62,25,6.22,2.91,21.5]
[null,"Jul",6.53,2.54,23.9,6.78,2.64,24.2,7.02,2.5,24.8,5.93,2.8,23.3,5.82,2.95,24.9,5.85,2.65,23,7.46,2.19,25.6,7.32,2.2000000000000002,26.1,6.99,2.4500000000000002,26.2,7.07,2.17,25.5,6,3.06,25,6.52,2.66,24.7,6.64,2.5299999999999998,23.9,6.98,2.5499999999999998,24.1,6.05,2.84,24.7,6.87,2.59,25,7.39,2.33,26,6.23,2.72,24.6,6.17,2.72,24,6.98,2.4500000000000002,25.9,7.01,2.29,27.7,6.41,2.76,23.2]
[null,"Aug",5.53,2.25,24,5.79,2.42,24.4,6.12,2.4900000000000002,25,5.19,2.56,23.5,5.05,2.4700000000000002,24.9,5.1100000000000003,2.41,23,6.58,2.15,26.3,6.47,2.2000000000000002,26.5,6.25,2.2400000000000002,26.5,6.3,2.0699999999999998,25.7,5.18,2.5099999999999998,25.1,5.61,2.2999999999999998,25,5.61,2.4300000000000002,24.9,5.87,1.97,24.6,5.23,2.33,24.7,6.08,2.23,25.7,6.53,2.14,26.8,5.36,2.39,24.7,5.39,2.41,24.1,6.13,2.37,26.5,6.12,2.46,27.7,5.47,2.52,23.7]
[null,"Sep",3.93,1.91,19.3,4.3499999999999996,1.83,19.7,4.76,1.85,21.2,3.66,1.91,18.5,3.72,2.09,19.600000000000001,3.81,1.69,18.2,5.18,1.74,22.4,5.18,1.9,23.1,5.07,1.8,22.2,5.0999999999999996,1.67,21.1,3.79,2.0699999999999998,19.8,4.18,1.73,20,3.9,1.92,21.8,4.21,1.79,20.2,3.74,1.75,19.8,4.63,1.96,21.8,5.07,1.69,24.2,3.89,2.04,19.5,3.85,2.17,19.2,4.74,1.85,22.5,4.74,2.02,23.3,4.08,1.8,19.3]
[null,"Okt",2.4500000000000002,1.33,14.4,2.57,1.35,15.9,3.31,1.41,17.7,2.2200000000000002,1.34,13.9,2.31,1.25,14.9,2.4700000000000002,1.34,13.2,3.63,1.42,19.399999999999999,3.77,1.53,19.600000000000001,3.51,1.63,19,3.51,1.34,17.899999999999999,2.36,1.39,15.1,2.69,1.41,16,2.54,1.29,18.2,2.69,1.48,16,2.2799999999999998,1.5,14.8,3.4,1.52,18.7,3.73,1.52,21.5,2.33,1.25,14.3,2.34,1.45,15.3,3.25,1.44,18.7,3.24,1.36,19.7,2.62,1.34,15.1]
[null,"Nov",1.47,0.82,8.4,1.4,0.82,10.8,2.13,1,13.7,1.33,0.84,7.8,1.25,0.68,8.6999999999999993,1.49,0.81,6.4,2.4500000000000002,1.1299999999999999,14.2,2.5499999999999998,1.21,15.2,2.33,1,14.9,2.34,0.96,13.7,1.2,0.8,9.1,1.54,0.93,10.6,1.58,0.93,13.4,1.61,0.78,10.9,1.22,0.76,8.4,1.95,1.08,14.7,2.52,1.1499999999999999,17.899999999999999,1.21,0.76,8.1,1.27,0.84,10,2.09,0.88,14,2.0699999999999998,1.06,15.3,1.34,0.72,9.6999999999999993]
[null,"Dez",1.1200000000000001,0.65,4.4000000000000004,1.2,0.66,6.9,1.6,0.81,10.6,1.01,0.63,3.7,0.96,0.62,3.8,1.03,0.56000000000000005,1.6,1.97,0.87,10.9,2,0.9,11.5,1.85,0.87,11.3,1.83,0.91,9.9,0.97,0.62,4.2,1.2,0.69,6.5,1.19,0.68,10.8,1.23,0.67,7.4,0.89,0.59,4.0999999999999996,1.59,0.81,11.4,1.97,0.94,14.8,1,0.6,3.7,1.1399999999999999,0.69,5.3,1.59,0.79,10.5,1.58,0.85,11.9,0.98,0.64,5.5]
[null,"Jahr",3.64,1.75,13.9,3.82,1.74,14.7,4.34,1.78,16.3,3.38,1.76,13.3,3.29,1.8,14.2,3.43,1.68,12.9,4.6900000000000004,1.74,17.3,4.72,1.79,17.600000000000001,4.45,1.83,17.600000000000001,4.47,1.65,16.5,3.37,1.86,14.4,3.77,1.75,15,3.64,1.78,16.600000000000001,3.87,1.69,15.2,3.41,1.74,14.3,4.2,1.8,17.100000000000001,4.71,1.76,19.100000000000001,3.51,1.76,13.9,3.58,1.8,14,4.2699999999999996,1.8,17.2,4.28,1.8,18.3,3.63,1.79,13.9]
[]
[]
[]
[]
[{"$f":"Translation!A30","v":"Hungary"},"Stadt","Budapest",null,null,"Debrecen",null,null,"Miskolc",null,null,"Nyiregyhaza",null,null,"Pécs",null,null,"Szeged"]
[null,"Breitengrad",47.5,null,null,47.5,null,null,48.1,null,null,48,null,null,46.08,null,null,46.2]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.96,0.56000000000000005,-0.7,1.17,0.71,-1.4,1.87,0.78,9.5,0.55000000000000004,0.45,-1.9,1.1499999999999999,0.71,-0.4,1.19,0.63,-0.7]
[null,"Feb",1.68,0.9,1.4,2.11,0.99,0.1,2.68,1.36,8.8000000000000007,1.47,0.93,0,1.97,1.1200000000000001,2,2.1,1.01,0.8]
[null,"Mar",2.82,1.72,5.6,3.26,1.6,4.9000000000000004,3.91,1.72,10.7,3.31,1.5,4.5999999999999996,3,1.78,6.1,3.19,1.82,5.5]
[null,"Apr",4.25,2.0499999999999998,11.6,4.54,1.96,11.5,5.37,2.35,12.9,4.75,2.13,11.2,4.5,2.31,11.3,4.55,2.12,11.3]
[null,"Mai",5.29,2.74,17.3,5.42,2.61,17.3,6.32,2.46,17.899999999999999,6.14,2.33,16.8,5.37,2.63,17.2,5.58,2.71,17.3]
[null,"Jun",5.8,3.07,20.3,5.69,2.66,19.899999999999999,6.99,2.58,22.4,6.02,2.79,19.399999999999999,5.73,2.91,20.3,6.1,2.88,20.3]
[null,"Jul",5.9,2.52,21.4,5.78,2.82,21.2,7.02,2.5,24.8,6.29,2.4300000000000002,20.7,5.86,2.8,21.3,6.08,2.69,21.5]
[null,"Aug",4.99,2.29,21.7,5.35,2.16,21.1,6.12,2.4900000000000002,25,5.33,2.44,20.5,5.21,2.35,21.6,5.28,2.5499999999999998,21.5]
[null,"Sep",3.65,1.98,16,4.01,1.55,15.6,4.76,1.85,21.2,4.3,1.76,15,3.84,1.96,16.2,3.87,1.92,16]
[null,"Okt",2.29,1.1399999999999999,11.1,2.57,1.2,10.8,3.31,1.41,17.7,2.74,1.1299999999999999,10.4,2.35,1.24,11.8,2.58,1.2,11.4]
[null,"Nov",1.1499999999999999,0.65,5.6,1.49,0.81,5.4,2.13,1,13.7,1.3,0.72,5,1.38,0.74,6,1.42,0.8,5.8]
[null,"Dez",0.74,0.53,-0.2,0.81,0.61,-0.6,1.6,0.81,10.6,0.75,0.5,-1.1000000000000001,0.84,0.57999999999999996,0.2,0.98,0.66,0.1]
[null,"Jahr",3.29,1.68,10.9,3.52,1.65,10.5,4.34,1.78,16.3,3.58,1.6,10.1,3.43,1.76,11.1,3.58,1.75,10.9]
[]
[]
[]
[]
[{"$f":"Translation!A31","v":"Belgium"},"Stadt","Antwerpen",null,null,"Brugge",null,null,"Bruxelles",null,null,"Charleroi",null,null,"Gent",null,null,"Liége"]
[null,"Breitengrad",51.2,null,null,51.2,null,null,50.8,null,null,50.4,null,null,51.03,null,null,50.63]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.67741935483870963,0.45161290322580644,3.8,0.77419354838709675,0.4838709677419355,4.0999999999999996,0.64516129032258063,0.45161290322580644,3.6,0.67741935483870963,0.45161290322580644,3,0.64516129032258063,0.4838709677419355,4.0999999999999996,0.70967741935483875,0.45161290322580644,3]
[null,"Feb",1.2857142857142858,0.8928571428571429,5.0999999999999996,1.3928571428571428,0.8571428571428571,5.0999999999999996,1.2857142857142858,0.8571428571428571,4.7,1.3214285714285714,0.8214285714285714,4,1.2857142857142858,0.8214285714285714,5.4,1.3571428571428572,0.9285714285714286,3.9]
[null,"Mar",2.2580645161290325,1.3870967741935485,7.4,2.3870967741935485,1.4193548387096775,7,2.193548387096774,1.4838709677419355,7.2,2.225806451612903,1.3548387096774193,6.7,2.193548387096774,1.4193548387096775,7.5,2.3870967741935485,1.4516129032258065,6.8]
[null,"Apr",3.6333333333333333,2.2666666666666666,10.1,4,2.1,9.4,3.4666666666666668,2.2000000000000002,9.9,3.5333333333333332,2.2999999999999998,9.3000000000000007,3.5333333333333332,2.2666666666666666,10.1,3.8333333333333335,1.7333333333333334,9.6]
[null,"Mai",4.67741935483871,2.4838709677419355,14.2,5,2.5483870967741935,12.9,4.580645161290323,2.806451612903226,13.8,4.612903225806452,2.129032258064516,13.4,4.5161290322580649,2.2903225806451615,13.8,5,2.903225806451613,13.7]
[null,"Jun",4.9666666666666668,3.1,17,5.5,2.7,16,4.833333333333333,2.4666666666666668,16.7,4.833333333333333,2.9333333333333331,16.3,4.8666666666666663,2.8333333333333335,16.7,5.0666666666666664,2.6666666666666665,16.7]
[null,"Jul",4.806451612903226,2.806451612903226,18.3,5.32258064516129,2.935483870967742,17.3,4.645161290322581,2.6451612903225805,17.899999999999999,4.67741935483871,3.129032258064516,17.5,4.709677419354839,2.6129032258064515,18,5.129032258064516,2.903225806451613,17.7]
[null,"Aug",4.258064516129032,2.4193548387096775,19.100000000000001,4.67741935483871,2.3225806451612905,18.3,4.161290322580645,2.4516129032258065,18.7,4.193548387096774,2.3870967741935485,18.3,4.225806451612903,2.3870967741935485,18.8,4.4516129032258061,2.4193548387096775,18.600000000000001]
[null,"Sep",2.9,1.7333333333333334,15.7,3.0666666666666669,1.5,15.7,2.8666666666666667,1.7,15.3,2.9,1.5666666666666667,14.9,2.9,1.5666666666666667,15.8,2.9333333333333331,1.5666666666666667,15.1]
[null,"Okt",1.7419354838709677,1.032258064516129,11.5,1.7741935483870968,1.096774193548387,11.8,1.7096774193548387,1.064516129032258,11.3,1.7419354838709677,1.096774193548387,10.8,1.7096774193548387,1.1290322580645162,11.9,1.7741935483870968,1.032258064516129,11]
[null,"Nov",0.83333333333333337,0.53333333333333333,7.1,0.8666666666666667,0.56666666666666665,7.7,0.83333333333333337,0.56666666666666665,6.8,0.8666666666666667,0.6333333333333333,6.2,0.83333333333333337,0.56666666666666665,7.5,0.8666666666666667,0.6333333333333333,6.3]
[null,"Dez",0.4838709677419355,0.35483870967741937,4.2,0.5161290322580645,0.38709677419354838,4.8,0.4838709677419355,0.38709677419354838,3.9,0.4838709677419355,0.35483870967741937,3.4,0.5161290322580645,0.38709677419354838,4.5999999999999996,0.4838709677419355,0.38709677419354838,3.4]
[null,"Jahr",2.7095890410958905,1.6246575342465754,11.1,2.9342465753424656,1.5835616438356164,10.8,2.6383561643835618,1.5917808219178082,10.8,2.6684931506849314,1.5972602739726027,10.3,2.6602739726027398,1.5671232876712329,11.2,2.8356164383561642,1.5972602739726027,10.5]
[]
[]
[]
[]
[{"$f":"Translation!A32","v":"Netherlands"},"Stadt","Amsterdam",null,null,"Eindhoven",null,null,"Enschede",null,null,"Groningen",null,null,"Maastricht",null,null,"Rotterdam",null,null,"Utrecht",null,null,"Zaanstad"]
[null,"Breitengrad",52.35,null,null,51.43,null,null,52.2,null,null,53.2,null,null,50.85,null,null,51.92]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.61290322580645162,0.38709677419354838,4.5999999999999996,0.67741935483870963,0.41935483870967744,3,0.61290322580645162,0.38709677419354838,2.4,0.58064516129032262,0.38709677419354838,3.7,0.70967741935483875,0.41935483870967744,3.1,0.61290322580645162,0.45161290322580644,4.8,0.61290322580645162,0.38709677419354838,4.3,0.61290322580645162,0.38709677419354838,4.5999999999999996]
[null,"Feb",1.2857142857142858,0.8571428571428571,5.2,1.3214285714285714,0.8928571428571429,4.2,1.2857142857142858,0.8571428571428571,3.4,1.25,0.7142857142857143,4.0999999999999996,1.3571428571428572,0.8571428571428571,4.2,1.25,0.75,5.5,1.2857142857142858,0.8928571428571429,5.0999999999999996,1.2857142857142858,0.75,5.2]
[null,"Mar",2.193548387096774,1.4193548387096775,6.5,2.2580645161290325,1.4516129032258065,6.7,2.193548387096774,1.2580645161290323,5.8,2.129032258064516,1.3548387096774193,5.4,2.3870967741935485,1.2903225806451613,6.9,2.193548387096774,1.5161290322580645,6.6,2.193548387096774,1.4838709677419355,6.5,2.2580645161290325,1.3870967741935485,6.4]
[null,"Apr",3.6,2.1333333333333333,9,3.7333333333333334,2.0666666666666669,9.6999999999999993,3.6666666666666665,1.8333333333333333,9.1,3.6333333333333333,2.2000000000000002,8.3000000000000007,3.9,2.2000000000000002,9.6999999999999993,3.6,2.1666666666666665,9,3.5666666666666669,2.1333333333333333,9,3.7,2.2000000000000002,8.9]
[null,"Mai",4.67741935483871,2.6129032258064515,12.5,4.774193548387097,2.5483870967741935,13.7,4.774193548387097,2.4516129032258065,13,4.806451612903226,2.4193548387096775,11.7,5.064516129032258,2.4838709677419355,13.9,4.612903225806452,2.3548387096774195,12.4,4.67741935483871,3.032258064516129,12.6,4.838709677419355,2.5806451612903225,12.4]
[null,"Jun",4.9000000000000004,2.9,15.1,4.9333333333333336,2.7,16.5,4.833333333333333,2.7333333333333334,15.7,4.8,2.5333333333333332,14.5,5.1333333333333337,3.1,16.8,4.8,2.8,15.2,4.9000000000000004,2.9666666666666668,15.3,5.0333333333333332,2.8333333333333335,15.1]
[null,"Jul",4.645161290322581,2.5161290322580645,16.8,4.774193548387097,2.4516129032258065,17.7,4.741935483870968,2.4838709677419355,17.2,4.741935483870968,2.774193548387097,16.399999999999999,5.193548387096774,2.6451612903225805,17.899999999999999,4.5483870967741939,2.838709677419355,17,4.67741935483871,2.838709677419355,17,4.806451612903226,2.7419354838709675,16.8]
[null,"Aug",4.096774193548387,2.4516129032258065,18,4.161290322580645,2.4516129032258065,18.3,4.161290322580645,2.5483870967741935,17.8,4.096774193548387,2.2903225806451615,17.600000000000001,4.5161290322580649,2.3548387096774195,18.600000000000001,4,2.064516129032258,18.100000000000001,4.161290322580645,2.225806451612903,17.899999999999999,4.193548387096774,2.2580645161290325,17.899999999999999]
[null,"Sep",2.8,1.4666666666666666,15.5,2.8333333333333335,1.7666666666666666,14.9,2.7666666666666666,1.7666666666666666,14.2,2.7666666666666666,1.4666666666666666,14.6,2.9333333333333331,1.7,15.1,2.7666666666666666,1.7333333333333334,15.6,2.8,1.6,15.2,2.8,1.7,15.5]
[null,"Okt",1.6129032258064515,1.032258064516129,11.8,1.6774193548387097,1.096774193548387,10.8,1.6774193548387097,0.967741935483871,10.199999999999999,1.5806451612903225,0.967741935483871,10.7,1.7419354838709677,1.064516129032258,11.1,1.6129032258064515,0.93548387096774188,12,1.6451612903225807,0.87096774193548387,11.4,1.6129032258064515,0.90322580645161288,11.8]
[null,"Nov",0.76666666666666672,0.5,7.8,0.83333333333333337,0.6,6.3,0.8,0.53333333333333333,6,0.73333333333333328,0.5,6.7,0.8666666666666667,0.6,6.4,0.76666666666666672,0.53333333333333333,7.9,0.8,0.53333333333333333,7.4,0.76666666666666672,0.5,7.8]
[null,"Dez",0.45161290322580644,0.32258064516129031,5.2,0.4838709677419355,0.32258064516129031,3.5,0.45161290322580644,0.32258064516129031,2.9,0.41935483870967744,0.32258064516129031,4,0.45161290322580644,0.35483870967741937,3.5,0.45161290322580644,0.32258064516129031,5.3,0.4838709677419355,0.35483870967741937,4.8,0.45161290322580644,0.32258064516129031,5.0999999999999996]
[null,"Jahr",2.6383561643835618,1.5561643835616439,10.7,2.7013698630136984,1.5726027397260274,10.4,2.6630136986301371,1.515068493150685,9.8000000000000007,2.6328767123287671,1.4931506849315068,9.8000000000000007,2.8547945205479452,1.5890410958904109,10.6,2.6054794520547944,1.5424657534246575,10.8,2.6520547945205482,1.6164383561643836,10.5,2.6958904109589041,1.547945205479452,10.6]
[]
[]
[]
[]
[{"$f":"Translation!A33","v":"Slovakia"},"Stadt","Bratislava",null,null,"Kosice",null,null,"Nitra",null,null,"Poprad"]
[null,"Breitengrad",48.17,null,null,48.73,null,null,48.28,null,null,49.07]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.83870967741935487,0.5161290322580645,-0.6,0.74193548387096775,0.54838709677419351,-2.6,0.87096774193548387,0.5161290322580645,-1.3,1.096774193548387,0.58064516129032262,-4.5999999999999996]
[null,"Feb",1.6428571428571428,0.9642857142857143,1.7,1.5,0.9642857142857143,-0.7,1.6428571428571428,1,0.8,1.9642857142857142,0.8571428571428571,-2.4]
[null,"Mar",2.7419354838709675,1.5483870967741935,5.5,2.774193548387097,1.6129032258064515,3.8,2.7419354838709675,1.5806451612903225,4.9000000000000004,3.032258064516129,1.6129032258064515,0.9]
[null,"Apr",4.166666666666667,2.0333333333333332,11,4.0666666666666664,2.1666666666666665,10.199999999999999,4.2333333333333334,2.0333333333333332,10.9,4.0333333333333332,1.9333333333333333,6.6]
[null,"Mai",5.4838709677419351,2.4838709677419355,16.600000000000001,5.354838709677419,2.5161290322580645,15.6,5.4838709677419351,2.5483870967741935,16.3,4.903225806451613,2.3870967741935485,12.4]
[null,"Jun",5.833333333333333,2.7333333333333334,19.5,5.6,2.7333333333333334,18.399999999999999,5.833333333333333,2.8,19,5.0666666666666664,2.8333333333333335,15.1]
[null,"Jul",5.709677419354839,2.5161290322580645,20.7,5.5161290322580649,2.6451612903225805,19.8,5.709677419354839,2.806451612903226,20.3,5,2.967741935483871,16.2]
[null,"Aug",4.903225806451613,2.2580645161290325,21.1,4.709677419354839,2.032258064516129,19.7,4.903225806451613,2.2903225806451615,20.7,4.4838709677419351,2.161290322580645,16.2]
[null,"Sep",3.4,1.8333333333333333,15.6,3.3333333333333335,1.7333333333333334,14.3,3.4,1.7666666666666666,15.5,3.4,1.6333333333333333,11.2]
[null,"Okt",2.161290322580645,1.096774193548387,10.8,2.064516129032258,1.032258064516129,9.4,2.129032258064516,1.064516129032258,10.5,2.161290322580645,1.032258064516129,7.1]
[null,"Nov",0.96666666666666667,0.56666666666666665,5.5,0.93333333333333335,0.6333333333333333,4.2,1,0.6,5.2,1.2,0.6333333333333333,2]
[null,"Dez",0.64516129032258063,0.41935483870967744,0.1,0.58064516129032262,0.45161290322580644,-1.9,0.67741935483870963,0.45161290322580644,-0.5,0.83870967741935487,0.5161290322580645,-3.8]
[null,"Jahr",3.2109589041095892,1.5835616438356164,10.6,3.0931506849315067,1.5890410958904109,9.1999999999999993,3.2164383561643834,1.6301369863013699,10.199999999999999,3.1013698630136988,1.5945205479452054,6.4]
[]
[]
[]
["Platzhalter für Auswahl Klimazone leer (falls im Ausdruck nichts stehen soll)"]
[{"$f":"Translation!A34","v":"Finland"},"Stadt","Espoo",null,null,"Helsinki",null,null,"Jyväskylä",null,null,"Oulu",null,null,"Tampere",null,null,"Turku",null,null,"Lahti",null,null,"Lappeenranta",null,null,"Rovaniemi",null,null,"Vaasa",null,null,"Vantaa"]
[null,"Breitengrad",60.17,null,null,60.22,null,null,62.24,null,null,65.17,null,null,61.53,null,null,60.45,null,null,60.96,null,null,61.05,null,null,66.569999999999993,null,null,63.05,null,null,60.3]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.24,0.18,-3.4,0.25,0.18,-3.3,0.2,0.15,-7.4,0.12,0.08,-8.1999999999999993,0.24,0.18,-5.6,0.24,0.16,-3.7,0.26,0.18,-5.6,0.23,0.17,-6.4,7.0000000000000007E-2,0.04,-10.4,0.2,0.14000000000000001,-5.2,0.26,0.19,-4.2]
[null,"Feb",0.87,0.55000000000000004,-4.5999999999999996,0.88,0.55000000000000004,-4.5,0.75,0.45,-8,0.67,0.36,-8.6,0.85,0.47,-6.6,0.86,0.5,-4.9000000000000004,0.87,0.51,-6.6,0.83,0.5,-8.1,0.51,0.28999999999999998,-10.3,0.77,0.46,-6.4,0.85,0.5,-5.0999999999999996]
[null,"Mar",2.04,1.1399999999999999,-2.2000000000000002,2.0499999999999998,1.02,-2.2000000000000002,2.0299999999999998,0.93,-4.2,1.86,0.83,-5,2.0499999999999998,1.08,-3.1,2.16,1.1399999999999999,-2,2.0499999999999998,0.95,-3.3,2.02,1.1200000000000001,-3.4,1.79,0.81,-6.2,1.98,0.98,-3.4,2.04,1.1200000000000001,-2.2999999999999998]
[null,"Apr",3.59,1.79,3.2,3.59,1.96,3.1,3.56,1.63,2.5,3.74,1.47,1.4,3.51,1.74,3.6,3.55,1.79,4.3,3.51,1.72,3.8,3.5,1.83,4.3,3.54,1.48,-0.3,3.61,1.58,3.8,3.54,1.72,4.0999999999999996]
[null,"Mai",5.34,2.1800000000000002,8.6,5.33,2.2799999999999998,8.4,4.8499999999999996,2.16,8.4,4.9000000000000004,2.08,7.1,4.83,2.37,9,5.18,2.29,9.4,5.03,2.29,9.4,5.22,2.14,10,4.57,1.99,5.5,4.99,2.35,8.9,5.31,2.1,9.6999999999999993]
[null,"Jun",6.14,2.72,13.8,6.1,2.7,13.7,5.0599999999999996,2.4,14,5.66,2.54,13.8,5.47,2.63,14.2,6.11,2.59,14.2,5.72,2.31,14.5,5.92,2.63,15.1,5.12,2.5,12.7,5.46,2.46,14.1,5.89,2.75,14.6]
[null,"Jul",5.53,2.42,17.7,5.52,2.6,17.600000000000001,4.99,2.4900000000000002,17.100000000000001,5.01,2.62,17.2,4.9800000000000004,2.39,17.3,5.42,2.6,17.600000000000001,5.17,2.3199999999999998,17.5,5.4,2.63,18.600000000000001,4.62,2.21,16.100000000000001,5.0599999999999996,2.41,17.2,5.44,2.4700000000000002,18]
[null,"Aug",4.13,1.94,16.8,4.09,2.0099999999999998,16.8,3.9,2.09,15,3.51,1.77,14.8,3.87,1.97,15.5,4.0999999999999996,1.86,16.3,4.0199999999999996,2.17,15.4,4.0199999999999996,2.06,16,3.26,1.77,12.9,3.78,1.96,15.3,4.12,2.09,16.600000000000001]
[null,"Sep",2.36,1.43,12,2.35,1.44,12.1,2.27,1.21,9.4,1.97,1.05,9.6,2.2799999999999998,1.05,10.199999999999999,2.35,1.42,11.3,2.34,1.29,9.8000000000000007,2.2999999999999998,1.27,10.9,1.8,0.96,7.5,2.25,1.22,10.8,2.4300000000000002,1.3,11.5]
[null,"Okt",1.05,0.68,6.6,1.05,0.6,6.7,0.78,0.57999999999999996,3.7,0.75,0.5,3.7,0.99,0.63,4.5999999999999996,1.07,0.74,5.7,1.06,0.6,4.5,0.98,0.66,4.9000000000000004,0.6,0.39,1.2,0.91,0.6,5.2,1.03,0.63,5.8]
[null,"Nov",0.3,0.22,2.2000000000000002,0.3,0.24,2.2999999999999998,0.24,0.19,-0.7,0.19,0.13,-1.5,0.35,0.22,0,0.36,0.27,1.2,0.37,0.24,0.1,0.28999999999999998,0.23,-0.9,0.12,0.09,-4.8,0.27,0.18,0,0.33,0.25,1.3]
[null,"Dez",0.14000000000000001,0.1,-1.9,0.14000000000000001,0.11,-1.7,0.08,0.06,-6.2,0.05,0.03,-7.2,0.13,0.09,-4.5999999999999996,0.17,0.12,-2.7,0.15,0.1,-4.5999999999999996,0.12,0.09,-3.9,0,0,-9.5,0.09,7.0000000000000007E-2,-3.1,0.14000000000000001,0.12,-2.9]
[null,"Jahr",2.65,1.28,5.7,2.64,1.31,5.8,2.39,1.2,3.6,2.37,1.1299999999999999,3.1,2.46,1.24,4.5,2.63,1.29,5.6,2.5499999999999998,1.23,4.5999999999999996,2.57,1.28,4.8,2.17,1.05,1.2,2.4500000000000002,1.2,4.8,2.61,1.27,5.6]
[]
[]
[]
[]
[{"$f":"Translation!A35","v":"Bosnia-Herzegovina"},"Stadt","Banja Luka",null,null,"Doboj",null,null,"Grude",null,null,"Livno",null,null,"Mostar",null,null,"Prijedor",null,null,"Sarajevo",null,null,"Slavonski Brod",null,null,"Tuzla",null,null,"Zenica"]
[null,"Breitengrad",44.7,null,null,44.73,null,null,43.37,null,null,43.83,null,null,43.35,null,null,44.98,null,null,43.87,null,null,45.16,null,null,44.55,null,null,44.22]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",1.32,0.65,-0.1,1.32,0.66,0.2,1.65,0.73,6.8,1.42,0.77,-1.5,1.42,0.69,-0.2,1.3,0.66,0.6,1.41,0.77,-1.3,1.28,0.65,-0.2,1.31,0.76,0.6,1.34,0.77,-0.4]
[null,"Feb",1.94,1.1399999999999999,2.2999999999999998,1.96,1.1499999999999999,2.4,2.56,1.1000000000000001,6.9,2.2999999999999998,1.17,-0.8,2.2799999999999998,1.19,0.4,1.93,1.07,2.7,2.17,1.22,-0.7,1.97,1.06,2.2999999999999998,2.08,1.17,2.2999999999999998,2.14,1.1499999999999999,0.2]
[null,"Mar",3.19,1.72,6.9,3.19,1.83,7.2,3.78,1.62,10.199999999999999,3.49,1.55,4.0999999999999996,3.38,1.58,5.3,3.17,1.64,7.1,3.31,1.63,3.6,3.15,1.76,7,3.22,1.54,6.7,3.26,1.75,5.2]
[null,"Apr",4.3,2.15,11.8,4.3499999999999996,2.2400000000000002,12.2,4.99,2.3199999999999998,13.6,4.74,2.13,8.8000000000000007,4.51,2.09,10,4.28,2.21,11.7,4.3499999999999996,2.27,8.4,4.3600000000000003,2.08,12,4.46,2.31,11.6,4.3099999999999996,2.14,9.9]
[null,"Mai",5.5,2.41,17.600000000000001,5.48,2.5499999999999998,18,6.15,2.5,19.3,5.7,2.57,14.2,5.42,2.31,15.4,5.49,2.66,17.399999999999999,5.28,2.68,14,5.46,2.57,17.7,5.3,2.66,17.2,5.23,2.36,15.3]
[null,"Jun",5.59,2.9,21,5.63,3.13,21.4,6.7,2.85,23.5,6.18,2.6,17.8,5.83,2.5499999999999998,19,5.59,2.5499999999999998,20.9,5.53,2.58,17.5,5.67,2.82,21.2,5.71,2.5499999999999998,20.6,5.56,2.91,18.899999999999999]
[null,"Jul",6.14,2.59,22,6.12,2.58,22.3,6.79,2.4500000000000002,25.5,6.37,2.12,19.100000000000001,6.11,2.58,20.2,6.13,2.68,21.9,5.89,2.65,18.8,6.06,2.69,22.2,5.96,2.65,21.6,5.89,2.6,20.100000000000001]
[null,"Aug",5.1100000000000003,2.2799999999999998,21.9,5.1100000000000003,2.2200000000000002,22.4,5.86,2.15,25.3,5.46,2.4,18.8,5.24,2.2999999999999998,19.899999999999999,5.0999999999999996,2.3199999999999998,21.9,5.0199999999999996,2.27,18.7,5.13,2.4,22.1,5.08,2.16,21.6,5,2.23,19.8]
[null,"Sep",3.86,2.0299999999999998,16.2,3.85,1.92,16.600000000000001,4.55,1.7,20.100000000000001,4.13,1.76,13.5,3.91,1.82,14.6,3.85,1.73,16.3,3.68,2.0499999999999998,13.4,3.83,2.02,16.3,3.72,1.76,16.2,3.65,1.55,14.5]
[null,"Okt",2.52,1.32,12.1,2.5099999999999998,1.1599999999999999,12.4,3.28,1.17,16.399999999999999,2.9,1.29,9.6,2.79,1.24,10.7,2.5,1.32,12.2,2.64,1.19,9.6,2.4900000000000002,1.23,12.1,2.57,1.26,12.1,2.58,1.0900000000000001,10.6]
[null,"Nov",1.37,0.88,6.4,1.38,0.78,6.7,1.97,0.89,11.9,1.72,0.84,4.5999999999999996,1.68,0.85,5.7,1.35,0.81,6.8,1.54,0.82,4.7,1.36,0.83,6.4,1.49,0.83,6.7,1.52,0.64,5.6]
[null,"Dez",1.08,0.68,0.9,1.0900000000000001,0.69,1,1.56,0.66,7.9,1.29,0.68,-0.6,1.24,0.64,0.6,1.06,0.64,1.4,1.17,0.74,-0.7,1.06,0.64,0.8,1.1000000000000001,0.67,1.2,1.1000000000000001,0.64,0.4]
[null,"Jahr",3.49,1.73,11.6,3.5,1.75,11.9,4.1500000000000004,1.68,15.6,3.81,1.66,9,3.65,1.66,10.1,3.48,1.7,11.7,3.5,1.74,8.8000000000000007,3.48,1.73,11.7,3.5,1.69,11.5,3.46,1.66,10]
[]
[]
[]
[]
[{"$f":"Translation!A36","v":"Denmark"},"Stadt","Alborg",null,null,"Arhus",null,null,"Esbjerg",null,null,"Helsingør",null,null,"Herning",null,null,"Hjørring",null,null,"Holbæk",null,null,"København",null,null,"Kolding",null,null,"Nykøbing",null,null,"Odense",null,null,"Rønne",null,null,"Slagelse",null,null,"Sønderburg",null,null,"Svendborg"]
[null,"Breitengrad",57.05,null,null,56.17,null,null,55.47,null,null,56.03,null,null,56.14,null,null,57.45,null,null,55.71,null,null,55.72,null,null,55.496000000000002,null,null,54.765000000000001,null,null,55.4,null,null,55.1,null,null,55.404000000000003,null,null,54.91,null,null,55.067]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",0.42,0.28999999999999998,0.8,0.51,0.3,0.9,0.5,0.35,1.7,0.47,0.33,0,0.48,0.3,1.3,0.39,0.28000000000000003,0.1,0.5,0.32,0.7,0.49,0.33,0.6,0.51,0.35,1.2,0.49,0.32,1.2,0.52,0.35,1.8,0.49,0.32,1.5,0.53,0.33,1.1000000000000001,0.5,0.38,2,0.5,0.31,1.8]
[null,"Feb",1.05,0.57999999999999996,1.1000000000000001,1.1200000000000001,0.66,1.2,1.1499999999999999,0.65,1.9,1.06,0.63,0.7,1.1399999999999999,0.72,1.6,0.99,0.57999999999999996,0.6,1.1100000000000001,0.64,1.1000000000000001,1.0900000000000001,0.66,1,1.1399999999999999,0.65,1.6,1.1100000000000001,0.7,1.6,1.1399999999999999,0.67,2.2999999999999998,1.1399999999999999,0.64,1.4,1.1399999999999999,0.66,1.4,1.08,0.74,2.4,1.1200000000000001,0.65,2.2000000000000002]
[null,"Mar",2,1.23,2.6,2.15,1.18,2.5,2.2000000000000002,1.1499999999999999,3.4,2.11,1.2,2.6,2.14,1.26,3,1.95,1.02,2.6,2.11,1.31,2.5,2.16,1.34,2.4,2.17,1.21,3.4,2.23,1.39,3.1,2.16,1.27,3.8,2.23,1.25,2.5,2.14,1.36,2.8,2.08,1.17,4.2,2.15,1.39,3.7]
[null,"Apr",3.7,1.88,6.8,3.88,1.92,6.8,3.86,1.93,7.7,3.78,1.93,7.4,3.87,1.74,7.1,3.53,1.96,7.1,3.82,1.7,6.9,3.8,2.0499999999999998,6.8,3.84,1.92,7.7,3.84,1.86,6.8,3.91,2.0499999999999998,8.1999999999999993,3.91,2.04,6.8,3.86,1.73,7.1,3.59,2.1,8.5,3.78,2.2400000000000002,7.8]
[null,"Mai",4.84,2.33,10.9,4.96,2.61,11.2,5.14,2.27,11.7,5.14,2.54,11.9,4.78,2.36,11.2,4.8499999999999996,2.2599999999999998,11.4,5.0999999999999996,2.27,11.3,5.13,2.46,11.3,5.0199999999999996,2.38,12,5.0999999999999996,2.35,11.5,4.95,2.4500000000000002,12.6,5.15,2.2599999999999998,11.2,5.07,2.42,11.6,4.92,2.44,13,4.97,2.42,12.3]
[null,"Jun",5.16,2.8,14,5.26,2.73,14.1,5.36,2.72,14.4,5.39,2.42,15,5.15,2.92,14,5.19,2.73,14.6,5.33,2.65,14.4,5.44,2.74,14.5,5.24,2.4700000000000002,14.7,5.37,2.67,14.9,5.21,2.74,15.5,5.39,2.98,14.9,5.31,2.94,14.6,5.05,2.9,15.7,5.16,2.72,15.1]
[null,"Jul",5.01,2.56,16.3,5.01,2.77,16.399999999999999,5.17,2.57,16.600000000000001,5.24,2.58,17.100000000000001,4.92,2.4700000000000002,16.2,5.15,2.61,16.8,5.27,2.87,16.8,5.24,2.29,16.8,5.05,2.5299999999999998,16.899999999999999,5.16,2.68,17.3,5.09,2.5499999999999998,17.7,5.25,2.72,17.600000000000001,5.24,2.71,17,5.08,2.92,18,5.05,2.81,17.399999999999999]
[null,"Aug",4.08,2.2599999999999998,16.899999999999999,4.25,2.4300000000000002,17,4.28,2.1800000000000002,17.600000000000001,4.28,2.35,17.600000000000001,4.1500000000000004,2.0299999999999998,17,4.0199999999999996,2.06,17.2,4.29,2.06,17.3,4.3099999999999996,2.34,17.399999999999999,4.2699999999999996,2.4300000000000002,17.899999999999999,4.34,2.0699999999999998,18,4.2699999999999996,2.2000000000000002,18.399999999999999,4.38,2.2200000000000002,18.600000000000001,4.29,2.2000000000000002,17.7,4.26,2.29,18.899999999999999,4.2300000000000004,2.31,18.3]
[null,"Sep",2.63,1.36,13.2,2.73,1.5,13.3,2.66,1.54,14.2,2.67,1.43,13.3,2.68,1.38,13.4,2.5499999999999998,1.3,13.2,2.68,1.4,13.7,2.7,1.44,13.6,2.67,1.58,14.1,2.81,1.64,14.6,2.72,1.5,14.6,2.74,1.38,14.9,2.7,1.34,14.1,2.62,1.61,15.2,2.69,1.27,14.8]
[null,"Okt",1.38,0.74,8.6999999999999993,1.41,0.83,8.9,1.4,0.91,9.6999999999999993,1.39,0.9,8.5,1.44,0.78,8.9,1.31,0.8,8.6,1.43,0.89,9.1999999999999993,1.42,0.92,9.1,1.42,0.92,9.4,1.51,0.8,10.1,1.46,0.84,9.9,1.52,0.94,10.3,1.45,0.86,9.5,1.42,0.89,10.4,1.43,0.91,10.199999999999999]
[null,"Nov",0.62,0.38,4.7,0.69,0.41,4.8,0.66,0.44,5.6,0.6,0.42,4.3,0.71,0.45,4.8,0.59,0.39,4.5,0.62,0.45,5,0.61,0.38,4.9000000000000004,0.66,0.44,5.0999999999999996,0.68,0.44,5.7,0.7,0.44,5.6,0.69,0.41,5.9,0.66,0.39,5.3,0.64,0.42,6,0.68,0.43,5.8]
[null,"Dez",0.3,0.22,1.5,0.35,0.23,1.6,0.35,0.25,2.6,0.32,0.25,0.9,0.35,0.25,1.8,0.28000000000000003,0.21,1,0.35,0.24,1.7,0.34,0.26,1.6,0.35,0.25,1.9,0.36,0.26,2.5,0.36,0.23,2.5,0.4,0.3,2.8,0.37,0.27,2.1,0.35,0.24,2.8,0.36,0.26,2.6]
[null,"Jahr",2.6,1.39,8.1,2.69,1.47,8.1999999999999993,2.73,1.42,8.9,2.7,1.42,8.3000000000000007,2.65,1.39,8.4,2.57,1.35,8.1,2.72,1.41,8.4,2.73,1.44,8.3000000000000007,2.7,1.43,8.8000000000000007,2.75,1.44,8.9,2.71,1.45,9.4,2.77,1.46,9,2.73,1.44,8.6999999999999993,2.63,1.51,9.8000000000000007,2.68,1.48,9.3000000000000007]
[]
[]
[]
[]
[{"$f":"Translation!A37","v":"Morocco"},"Stadt","Agadir",null,null,"Béni-Mellal",null,null,"Casablanca",null,null,"Fez",null,null,"Marrakech",null,null,"Meknès",null,null,"Oujda",null,null,"Rabat",null,null,"Safi",null,null,"Tanger"]
[null,"Breitengrad",30.5,null,null,32.369999999999997,null,null,33.590000000000003,null,null,34.08,null,null,31.63,null,null,33.880000000000003,null,null,34.68,null,null,34.03,null,null,32.200000000000003,null,null,35.74]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp","Global","Diffus","Außentemp"]
[null,"Jan",3.26,1.35,15.3,2.93,1.27,10.1,2.83,1.1200000000000001,14.6,2.5499999999999998,1.19,10.1,2.9,1.28,12.3,2.73,1.28,10.199999999999999,2.61,1.23,10,2.7,1.1499999999999999,13.6,2.77,1.35,14.9,2.66,1.01,12.7]
[null,"Feb",4.1399999999999997,1.51,16,3.77,1.43,11.9,3.67,1.41,14.9,3.36,1.44,11.2,3.68,1.65,14.3,3.49,1.43,11.2,3.54,1.32,10.5,3.58,1.28,13.7,3.71,1.68,15.1,3.55,1.4,13.1]
[null,"Mar",5.55,1.76,16.7,5.22,1.77,15.3,4.8899999999999997,1.98,16.100000000000001,4.9400000000000004,1.72,14.2,5.0599999999999996,2.11,17.3,4.93,1.73,14.3,4.9400000000000004,1.6,13,4.8099999999999996,1.98,15.2,5.0999999999999996,1.92,16.600000000000001,4.68,1.88,15.1]
[null,"Apr",6.7,2.14,16.5,6.55,2.04,17.2,6.02,2.1,16.5,6.4,2.08,15.4,6.23,2.12,18.399999999999999,6.25,2.2999999999999998,15.1,5.93,2.2999999999999998,14.6,6.1,2.2799999999999998,15.5,7,1.8,17.100000000000001,6.08,2.23,16.399999999999999]
[null,"Mai",7.35,2.34,18,7.02,2.4500000000000002,20.8,6.7,2.58,18.2,6.84,2.4900000000000002,18.8,6.74,2.31,21.3,6.68,2.54,18.399999999999999,7.16,2.02,17.899999999999999,6.77,2.4300000000000002,17.600000000000001,7.39,2.23,18.7,6.71,2.5,18.600000000000001]
[null,"Jun",6.8,2.88,19.5,7.87,2.21,26.1,7.01,2.82,21.1,8.23,1.8,24,7.4,2.39,25.9,7.62,2.37,23.3,7.73,2.09,23.1,7.13,2.72,20.6,8.1300000000000008,1.92,21.3,7.5,2.41,22.5]
[null,"Jul",6.9,2.92,21.6,7.76,2.12,28.3,7.01,2.62,22.4,8.32,1.41,26.1,7.23,2.58,27.9,7.72,2.06,25,7.68,2.11,25.4,7.1,2.79,22.1,8.19,1.58,23.2,7.57,2.27,23.9]
[null,"Aug",6.42,2.71,22.1,6.92,2.12,28.2,6.46,2.56,23.4,7.19,1.82,26.2,6.35,2.4900000000000002,27.9,6.77,2.13,25.2,7,1.82,25.7,6.45,2.44,22.7,7.13,2.0299999999999998,24,6.33,2.41,24.2]
[null,"Sep",5.8,2.2200000000000002,22.3,5.96,1.88,24.8,5.47,1.99,22.9,5.83,1.62,22.9,5.5,2.14,25,5.52,1.84,22.4,5.73,1.69,22,5.42,2.11,22,6.03,1.87,23.3,5.37,1.93,22.5]
[null,"Okt",4.55,1.72,20.9,4.3899999999999997,1.62,20.8,4.13,1.75,20.9,4.13,1.61,19.100000000000001,4.29,1.64,21.7,4.18,1.62,19,4.1900000000000004,1.56,18.5,4.0599999999999996,1.64,19.8,4.42,1.67,21.5,3.99,1.62,19.7]
[null,"Nov",3.33,1.53,18.600000000000001,3.18,1.23,14.5,3.05,1.32,17.3,2.7,1.26,13.8,3.07,1.33,16.2,2.91,1.1499999999999999,13.7,2.8,1.26,13.2,2.95,1.23,16,3,1.45,17.8,2.92,1,15.6]
[null,"Dez",3.03,1.18,15.7,2.67,1.03,11.2,2.4700000000000002,1.04,15.6,2.3199999999999998,1.02,10.9,2.68,1.23,13.1,2.35,1.02,11,2.3199999999999998,0.9,10.7,2.36,1.04,14.6,2.4500000000000002,1.1599999999999999,15.9,2.2799999999999998,0.94,13.4]
[null,"Jahr",5.32,2.02,18.600000000000001,5.35,1.77,19.100000000000001,4.97,1.94,18.7,5.23,1.62,17.7,5.09,1.94,20.100000000000001,5.0999999999999996,1.79,17.399999999999999,5.14,1.66,17.100000000000001,4.95,1.93,17.8,5.44,1.72,19.100000000000001,4.97,1.8,18.100000000000001]
[]
[]
[]
[]
[{"$f":"Translation!A38","v":"Europe"},"Stadt","Ploce, Hrvatska",null,null,"Tivat, Crna Gora"]
[null,"Breitengrad",43.0563,null,null,42.4]
[null,null,"Global","Diffus","Außentemp","Global","Diffus","Außentemp",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Global","Diffus","Außentemp"]
[null,"Jan",1.74,0.86,9.1,1.82,0.9,7.2]
[null,"Feb",2.66,1.06,9.1,2.4500000000000002,1.1200000000000001,7.6]
[null,"Mar",3.89,1.67,11.6,3.74,1.54,10.1]
[null,"Apr",5.27,2.2799999999999998,14.4,5.04,2.39,13.3]
[null,"Mai",6.37,2.46,19.8,6.39,2.5,18.7]
[null,"Jun",6.96,2.5,23.9,7.02,2.63,22.9]
[null,"Jul",6.97,2.4300000000000002,26,7.3,1.96,24.9]
[null,"Aug",6.04,2.21,26.1,6.51,2,24.8]
[null,"Sep",4.7699999999999996,1.75,21.7,4.92,1.72,20.100000000000001]
[null,"Okt",3.43,1.24,18.2,3.32,1.17,16.100000000000001]
[null,"Nov",2.08,0.85,14,2.2799999999999998,0.86,12.2]
[null,"Dez",1.68,0.62,10.199999999999999,1.55,0.73,8.5]
[null,"Jahr",4.32,1.66,17,4.3600000000000003,1.63,15.5,4.1500000000000004,1.68,15.6,3.81,1.66,9,3.65,1.66,10.1,3.48,1.7,11.7,3.5,1.74,8.8000000000000007,3.48,1.73,11.7,3.5,1.69,11.5,3.46,1.66,10]
[]
[]
[]
["Platzhalter für Auswahl Klimazone leer (falls im Ausdruck nichts stehen soll)"]
["---","Stadt","---"]
[null,"Breitengrad"]
[]
[null,"Jan"]
[null,"Feb"]
[null,"Mar"]
[null,"Apr"]
[null,"Mai"]
[null,"Jun"]
[null,"Jul"]
[null,"Aug"]
[null,"Sep"]
[null,"Okt"]
[null,"Nov"]
[null,"Dez"]
[null,"Jahr"]

{"sheet":"Translation","index":4,"n_rows":365,"n_cols":12,"rows_kept":365,"cut":false,"hidden":true,"merged":[]}
["(Großbritannien)","(Deutschland)","(Großbritannien)","(Frankreich)","(Italien)","(Niederlande)","(Tschechien)","(Slowakei)","(Polen)","(Ungarn)","(Finland)","(Dänemark)"]
["Great Britain","Deutsch","Great Britain","France","Italia","Nederland","Česká republika","Slowakei","Polska","Magyarország","Suomi","Dansk"]
[]
["Engineering tool","Planungstool","Engineering tool","Outil de planification","Strumento di pianificazione","Planningshulpmiddel","Projekční pomůcka","Projekčná pomôcka","Narzędzia projektowe","Tervező","Suunnittelutyökalu","Planlægningsværktøj"]
["Solar system","Solaranlage","Solar system","Installation solaire","Impianto solare","Solarsysteem","Solární zařízení","Solárny zariadenie","Instalacja solarna","Szolárrendszer","Aurinkokeräinjärjestelmä","Solfangersystem"]
["Next >>","Weiter >>","Next >>","suivant","Avanti","Verder >>","Dále","Ďalej","Dalej","Tovább","Seuraava","Videre >>"]
["<< Back","<< Zurück","<< Back","précédant","Indietro","<< Terug","Zpět","Späť","Powrót","Vissza","Takaisin","<< Tilbage"]
[]
["Project data","Projektdaten","Project data","Projet","Dati del progetto","Projectdata","Data projektu","Dáta projektu","Dane Projektowe","Projekt","Projekti","Projekt data"]
["Project","Bauvorhaben","Project","Projet","Progetto di costruzione","Project","Akce","Stavebný projekt","Inwestycja","Építmény","Projekti","Projekt"]
["Name","Name","Name","Nom","Nome","Naam","Jméno","Meno","Nazwisko","Név","Nimi","Navn"]
["Street","Straße","Street","Rue","Via","Straat","Ulice","Ulica","Ulica","Utca","Katuosoite","Gade"]
["Postcode/Town","PLZ/Ort","Postcode/Town","CP/commune","CAP/Località","Postcode/Plaats","PSČ","PSČ","Kod pocztowy/Miejscowość","Ir.szám/Helyiség","Postinumero/paikkakunta","Postnr./By"]
["Phone","Telefon","Phone","Téléphone","Telefono","Telefoon","Telefon","Telefón","Tel.","Telefon","Puhelin","Telefon"]
["Customer","Auftraggeber","Customer","Donneur d'ordre","Committente","Klant","Zákazník","Zákazník","Zleceniodawca","Megbízó","Asiakas","Kunde"]
["Climate zone","Klimazone","Climate zone","Zone climatique","Zona climatica","Klimaatzone","Klimatická zóna","Klimatická zóna","Strefa klimatyczna","Éghajlati övezet","Ilmastovyöhyke","Klimazone"]
["Country selection","Auswahl Land","Country selection","Choix du pays","Selezione Paese","Land selectie","Volba země","Voľba krajiny","Wybór kraju","Ország kiválasztása","Maa","Valg af Land"]
["City/region selection","Auswahl Stadt/Region","City/region selection","Choix ville/région","Selezione Città/Regione","Selectie van Stad/Regio","Volba města/regionu","Voľba mesta/ regiónu","Wybór miasta/regionu","Város/régió kiválasztása","Kaupungin/alueen valinta","Valg af by/region"]
["Germany","Deutschland","Germany","Allemagne","Germania","Duitsland","Německo","Nemecko","Niemcy","Németország","Saksa","Tyskland"]
["France","Frankreich","France","France","Francia","Frankrijk","Francie","Francúzsko","Francja","Franciaország","Ranska","Frankrig"]
["Switzerland","Schweiz","Switzerland","Suisse","Svizzera","Zwitserland","Švýcarsko","Švajčiarsko","Szwajcaria","Svájc","Sveitsi","Schweiz"]
["USA","USA","USA","USA","USA","USA","USA","USA","USA","USA","Yhdysvallat","USA"]
["Great Britain","England","Great Britain","Grande-Bretagne","Gran Bretagna","Groot-Brittannië","Velká Británie","Veľká Británia","Wielka Brytania","Nagy-Britannia","Iso-Britannia","England"]
["Czech Republic","Tschechien","Czech Republic","République tchèque","Repubblica ceca","Tsjechië","Česká republika","Česká republika","Czechy","Cseh Köztársaság","Tsekki","Tjekkiet"]
["Poland","Polen","Poland","Pologne","Polonia","Polen","Polsko","Poľsko","Polska","Lengyelország","Puola","Polen"]
["Austria","Österreich","Austria","Autriche","Austria","Oostenrijk","Rakousko","Rakúsko","Austria","Ausztria","Itävalta","Østrig"]
["Sweden","Schweden","Sweden","Suède","Svezia","Zweden","Švédsko","Švédsko","Szwecja","Svédország","Ruotsi","Sverige"]
["Ireland","Irland","Ireland","Irlande","Irlanda","Ierland","Irsko","Írsko","Irlandia","Írország","Irlanti","Irland"]
["Italy","Italien","Italy","Italie","Italia","Italië","Itálie","Taliansko","Włochy","Olaszország","Italia","Italien"]
["Hungary","Ungarn","Hungary","Hongrie","Ungheria","Hongarije","Maďarsko","Maďarsko","Węgry","Magyarország","Unkari","Ungarn"]
["Belgium","Belgien","Belgium","Belquique","Belgio","Belgie","Belgie","Belgicko","Belgia","Belgium","Belgia","Belgien"]
["Netherlands","Niederlande","Netherlands","Pays-Bas","Paesi Bassi","Nederland","Nizozemi","Holandsko","Holandia","Hollandia","Hollanti","Holland"]
["Slovakia","Slovakei","Slovakia","Slovaquie","Slovacca","Slowakije","Slovensko","Slovensko","Slowacja","Slovakia","Slovakia","Slovakiet"]
["Finland","Finnland","Finland","Finlande","Finlandia","Finland","Finsko","Finsko","Finlandia","Finnország","Suomi","Finland"]
["Bosnia-Herzegovina","Bosnien-Herzegovina","Bosnia-Herzegovina","Bosnie-Herzegovine","Bosnia ed Erzegovina","Bosnie-Herzegovina","Bosna a Hercegovina","Bosna a Hercegovina","Bosnia i Hercegowina","Bosznia-Hecegovina","Bosnia ja Hertsegovina","Bosnien-Herzegovina"]
["Denmark","Dänemark","Denmark","Danemark","Danimarca","Denemarken","Denmark","Dánsko","Dania","Denmark","Tanska","Danmark"]
["Morocco","Marokko","Morocco","Morocco","Marocco","Morocco","Morocco","Maroko","Morocco","Morocco","Morocco","Marokko"]
["Europe","Europa","Europe","Europe","Europa","Europa","Európa","Európa","Europa","Europa","Eurooppa","Europa"]
["| Import","| Import","| Import","| Import","| Import","| Import","| Import","| Import","| Import","| Import","| Tuo tiedot","| Importer"]
["| Export","| Export","| Export","| Export","| Export","| Export","| Export","| Export","| Export","| Export","| Vie tiedot","| Eksporter"]
[]
["System selection","Systemauswahl","System selection","Sélection du système","Seleziona il sistema","Systeemkeuze","Volba soustavy","Voľba systému","Wybór systemu","Rendszer kiválasztás","Järjestelmän valinta","Systemvalg"]
["Solar DHW heating","Solare Warmwasserbereitung","Solar DHW heating","Production ECS solaire","Produzione acqua calda solare","Solar warmwaterbereiding","Solární příprava teplé vody","Solárna príprava teplej vody","Przygotowanie ciepłej wody w instalacji solarnej","Szolár HMV előállítás","Käyttöveden lämmitys","Solar VV-opvarmning"]
["Number of occupants","Personenzahl","Number of occupants","Nombre de personnes","Numero di persone","Aantal bewoners","Počet osob","Počet osôb","Liczba osób","Személyek száma","Käyttöveden kuluttajat","Antal personer"]
["DHW demand","Warmwasserbedarf","DHW demand","Besoin en ECS","Fabbisogno acqua calda","Warmwatervraag","Potřeba teplé vody","Spotreba teplej vody","Zapotrzebowanie na ciepłą wodę","Melegvíz-szükséglet","Käyttöveden kulutus","Varmtvandsforbrug"]
["Very low demand (15 litres)","Sehr geringer Bedarf (15 Liter)","Very low demand (15 litres)","Besoin très faible (15 litres)","Necessità molto ridotta (15 litri)","Zeer laag verbgruik (15 liter)","Velmi malá spotřeba (15 litrů)","Veľmi malá spotreba (15 litrov)","Nieznaczne zapotrzebowanie (15 l)","Nagyon kevés szükséglet (15 liter)","Erittäin alhainen kulutus (15 litraa)","Meget lavt forbrug (15 liter)"]
["Low demand (30 litres)","Geringer Bedarf (30 Liter)","Low demand (30 litres)","Besoin faible (30 litres)","Necessità ridotta (30 litri)","Laag verbruik (30 liter)","Malá spotřeba (30 litrů)","Malá spotreba (30 litrov)","Niewielkie zapotrzebowanie (30 l)","Kevés szükséglet (30 liter)","Alhainen kulutus (30 litraa)","Lavt forbrug (30 liter)"]
["Standard demand (40 litres)","Normaler Bedarf (40 Liter)","Standard demand (40 litres)","Besoin normal (40 litres)","Necessità normale (40 litri)","Standaard verbruik (40 liter)","Normální spotřeba (40 litrů)","Normálna spotreba (40 litrov)","Normalne zapotrzebowanie (40 l)","Normál szükséglet (40 liter)","Normaali kulutus (40 litraa)","Standard forbrug (40 liter)"]
["High demand (60 litres)","Hoher Bedarf (60 Liter)","High demand (60 litres)","Besoin élevé (60 litres)","Necessità alta (60 litri)","Hoog verbruik (60 liter)","Vysoká spotřeba (60 litrů)","Vysoká spotreba (60 litrov)","Duże zapotrzebowanie (60 l)","Magas szükséglet (60 liter)","Korkea kulutus (60 litraa)","Højt forbrug (60 liter)"]
["Very high demand (80 litres)","Sehr hoher Bedarf (80 Liter)","Very high demand (80 litres)","Besoin très élevé (80 litres)","Necessità molto alta (80 litri)","Zeer hoog verbruik (80 liter)","Velmi vysoká spotřeba (80 litrů)","Veľmi vysoká spotreba (80 litrov)","Bardzo duże zapotrzebowanie (80 l)","Nagyon magas szükséglet (80 liter)","Erittäin korkea kulutus (80 litraa)","Meget højet forbrug (80 liter)"]
["Solar central heating backup","Solare Heizungsunterstützung","Solar central heating backup","Chauffage d'appoint","Supporto di riscaldamento","Solar verwarmingsondersteuning","Podpora vytápění","Solárna podpora vykurovania","Wspomaganie ogrzewania","Fűtésrásegítés","Aurinkolämmöllä tuettu lämmitys","Solar centralvarmebackup"]
["Heat demand building","Gebäudeheizlast","Heat demand building","Déperditions du bâtiment","Fabbisogno riscaldamento edificio","Verwarmingslast","Tepelná ztráta budovy","Tepelné straty budovy","Obciążenie grzewcze budynku","Épület fűtésterhelése","Rakennuksen lämpökuorma","Bygningens energibehov"]
["Cylinder type","Speicherart","Cylinder type","Type de ballon","Tipo accumulatore","Boilertype","Druh zásobníku","Druh zásobníka","Typ zasobnika","Tároló jellege","Varaajan tyyppi","Beholdertype"]
["Two cylinder system (SBB+SBP)","Zwei Speicher (SBB+SBP)","Two cylinder system (SBB+SBP)","Système à 2 ballons (tampon+ECS)","due accumulatori (SBB + SBP)","Twee vaten systeem (SBB+SBP)","Dva zásobníky (SBB+SBP)","Dva zásobníky (SBB+SBP)","Dwa zasobniki (SBB + SBP)","Két tárolós rendszer (SBB+SBP)","Kaksi varaajaa (SBB+SBP)","To-beholdersystem (SBB+SBP)"]
["Instantaneous water heater (SBS)","Durchlaufspeicher (SBS)","Instantaneous water heater (SBS)","Ballon à production ECS instantanée (SBS)","Scaldacqua istantaneo (SBS)","Doorstroomboiler (SBS)","Průtokový zásobník (SBS)","Prietokový zásobník (SBS)","Zasobnik przepływowy (SBS)","Átfolyós HMV tároló (SBS)","Läpivirtausvaraaja (SBS)","Gennemstrømningsvandvarmer (SBS)"]
["Combi cylinder (SBK)","Kombispeicher (SBK)","Combi cylinder (SBK)","Ballon combiné (SBK)","Accumulatore combinato (SBK)","Combi zonne-verwarmingsboiler (SBK)","Kombinovaný zásobník (SBK)","Kombinovaný zásobník (SBK)","Zasobnik kombinowany (SBK)","Kombi HMV tároló (SBK)","Kombivaraaja (SBK)","Kombibeholder (SBK)"]
["Solar swimming pool heating","Solare Schwimmbaderwärmung","Solar swimming pool heating","Chauffage de piscine","Riscaldamento piscina","Solar zwembadverwarming","Solární ohřev bazénu","Solárna ohrev bazéna","Podgrzew wody basenowej","Uszodafűtés","Uima-altaan lämmitys","Solar swimmingpool opvarmning"]
["Swimming pool type","Schwimmbadart","Swimming pool type","Type de piscine","Tipo di piscina","Zwembadtype","Druh bazénu","Bazén","Typ basenu","Medence jellege","Uima-altaan tyyppi","Swimmingpooltype"]
["Open air swimming pool with cover","Freibad mit Abdeckung","Open air swimming pool with cover","Piscine de plein air avec bâche","Piscina all'aperto con copertura","Openluchtzwembad met afdekking","Zastřešený venkovní bazén","Zastrešený vonkajší bazén","Basen otwarty z pokrywą","Szabadtéri fedett medence","Katettu ulkoilmauima-allas","Udendørs swimmingpool med afdækning"]
["Open air pool without cover","Freibad ohne Abdeckung","Open air pool without cover","Piscine de plein air sans bâche","Piscina all'aperto senza copertura","Openluchtzwembad zonder afdekking","Nezastřešený venkovní bazén","Nezastrešený vonkajší bazén","Basen otwarty bez pokrywy","Szabadtéri fedetlen medence","Kattamaton ulkoilmauima-allas","Udendørs swimmingpool uden afdækning"]
["Indoor pool with cover","Hallenbad mit Abdeckung","Indoor pool with cover","Piscine couverte, avec bâche","Piscina coperta con copertura","Binnenzwembad met afdekking","Zakrytý vnitřní bazén ","Krytý vnútorný bazén","Basen kryty z pokrywą","Beltéri fedett medence","Katettu sisäuima-allas","Indendørs swimmingpool med afdækning"]
["Indoor pool without cover","Hallenbad ohne Abdeckung","Indoor pool without cover","Piscine couverte, sans bâche","Piscina coperta senza copertura","Binnenzwembad zonder afdekking","Nezakrytý vnitřní bazén","Nekrytý vnútorný bazén","Basen kryty bez pokrywy","Beltéri fedetlen medence","Kattamaton sisäuima-allas","Indendørs swimmingpool uden afdækning"]
["Volume in m³","Volumen in m³","Volume in m³","Volume en m³","Volume in m³","Volume in m ³","Objem v m³","Objem v m³","Pojemność w m³","Térfogat m³-ben","Tilavuus [m³]","Volumen i m³"]
[]
["Collector details","Kollektordaten","Collector details","Données capteur","Dati collettore","Collectorgegevens","Údaje o kolektoru"," Údaje o kolektore","Dane kolektorów","Kollektoradatok","Keräintiedot","Kollektordata"]
["Collector type","Kollektortyp","Collector type","Modèle de capteur","Tipo di collettore","Collector type","Typ kolektoru","Typ kolektora","Typ kolektora","Kollektor típusa","Keräinmalli","Kollektortype"]
["Rooftop","Aufdach","Rooftop","Sur toiture","Sopra tetto","Op het dak","Na střechu","Na strechu","Montaż na dachu","Tetőre szerelt","Katolle,","Oven på tag"]
["Roof integration","Indach","Roof integration","Intégré en toiture","Sottotetto"," In het dak","Vestavný","Vstavaný","Montaż w dachu","Tetőbe szerelt","Kattointegraatio,","Tagintegreret"]
["Collector number","Kollektoranzahl","Collector number","Nombre de capteurs","Numero di collettori","Collector aantal","Počet kolektorů","Počet kolektorov","Liczba kolektorów","Kollektorok száma","Keräinten määrä","Kollektorantal"]
["Determine the optimum number","Optimale Anzahl berechnen","Determine the optimum number","Détermination du nombre optimal de capteurs","numero ottimale da calcolare","Optimale aantal berekenen","Vypočítat optimální počet","Vypočítať optimálny počet","Obliczenie optymalnej ilości","Az optimális darabszám meghatározása","Optimilukumäärä","Beregn det optimal antal"]
["Collector inclination","Kollektorneigung","Collector inclination","Inclinaison des capteurs","Pendenza collettore","Collector hoek","Sklon kolektorů","Sklon kolektorov","Nachylenie kolektora","Kollektor dőlése","Keräinkaltevuus","Kollektorhældning"]
["Collector orientation","Kollektorausrichtung","Collector orientation","Orientation des capteurs","Orientamento collettore","Collector orientatie","Orientace kolektorů","Orientácia kolektorov","Ustawienie kolektora","Kollektor iránya","Katon suunta","Kollektororientering"]
["South","Süd","South","Sud","Sud","Zuid","Jih","Juh","Południe","Dél","Etelä","Syd"]
["Southeast","Südost","Southeast","Sud-est","Sudest","Zuidoost","Jihovýchod","Juhovýchod","Południowy wschód","Dél-kelet","Kaakko","Sydøst"]
["Southwest","Südwest","Southwest","Sud-ouest","Sudovest","Zuidwest","Jihozápad","Juhozápad","Południowy zachód","Dél-nyugat","Lounas","Sydvest"]
["East","Ost","East","Est","Est","Oost","Východ","Východ","Wschód","Kelet","Itä","Øst"]
["West","West","West","Ouest","Ovest","West","Západ","Západ","Zachód","Nyugat","Länsi","Vest"]
["Arrangement","Kollektoranordnung","Arrangement","Disposition des capteurs","Disposizione dei collettori","Collectoropstelling","Uspořádání kolektorů","Usporiadanie kolektorov","Układ kolektorów","Kollektor elrendezése","Järjestely","Arrangering"]
["On end next to each other","Senkrecht nebeneinander","On end next to each other","Vertical côte á côte","Verticale adiacente","Vertikaal naast elkaar","Svisle vedle sebe","Zvisle vedľa seba","Pionowo obok siebie","Függőlegesen egymás mellett","S-mallit vierekkäin","Lodret side om side"]
["Across above each other","Waagerecht übereinander","Across above each other","Horizontal superposé","Orizzontale sovrapposti","Horizontaal boven elkaar","Vodorovně nad sebou","Vodorovne nad sebou","Poziomo jeden nad drugim","Vízszintesen egymás fölött","W-mallit päällekkäin","Vandret over hinanden"]
["Across next to each other","Waagerecht nebeneinander","Across next to each other","Horizontal côte á côte","Orizzontale adiacente","Horizontaal naast elkaar","Vodorovně vedle sebe","Vodorovne vedľa seba","Poziomo obok siebie","Vízszintesen egymás mellett","W-mallit vierekkäin","Vandret side om side"]
["On end above each other","Senkrecht übereinander","On end above each other","Vertical superposé","Verticale sovrapposti","Vertikaal boven elkaar","Svisle nad sebou","Zvisle nad sebou","Pionowo jeden nad drugim","Függőlegesen egymás fölött","S-mallit päällekkäin","Lodret over hinanden"]
["Shape of roof","Dachform","Shape of roof","Forme du toit","Forma del tetto","Dak vorm","Tvar střechy","Tvar strechy","Kształt dachu","Tetőforma","Katon tyyppi","Tagtype"]
["Tiled roof","Pfannendach","Tiled roof","Toit en tuiles","Tetto a coppi","Pannendak","Tašková střecha","Škridlová strecha","Dach kryty dachówką holenderską","Cseréptető","Tiilikatto","Tegltag"]
["Corrugated roof","Welldach","Corrugated roof","Toit en tôles ondulées","Tetto ondulato","Golfplatendak","Vlnitá střecha","Vlnitá strecha","Dach kryty blachą falistą","Hullámtető","Aaltopeltikatto","Eternittag"]
["Fixing type","Befestigungsart","Fixing type","Type de fixation","Tipo di fissaggio","Bevestigingswijze","Druh upevnění","Druh upevnenia","Sposób mocowania","Rögzítés módja","Asennustapa","Montagetype"]
["Standard fixings","Standardbefestigung","Standard fixings","Fixation standard","Fissaggio standard","Standaard bevestiging","Standardní upevnění","Štandardné upevnenie","Mocowanie standardowe","Normál rögzítés","Perusasennus","Standard montering"]
["Support stands 15°- 30°","Aufständerung 15°- 30°","Support stands 15°- 30°","Châssis d'inclinaison 15°- 30°","Supporto da 15°- 30°","Steun 15°- 30°","Podpěra 15°-30°","Oporný rám  15°-30°","Stelaż 15°-30°","Felállítási szög 15° – 30°","Kulmaan tuettu 15-30°","Elevation 15°-30°"]
["Quick assembly fixings","Schnellbefestigung","Quick assembly fixings","Fixation rapide","Fissaggio rapido","Snelbevestiging","Rychlé upevnění","Rýchle upevnenie","Szybkie mocowanie","Gyorszáras rögzítés","Pika-asennus","Kvikmontering"]
["Slate roof","Schiefer-Eindeckung","Slate roof","Toiture en ardoise","Coperture in Ardesia","Schiefer-dakbedekking","Břidlice","Bridlica","Pokrycie łupkowe","Pala borítás","Konesaumapeltikatto","Skifertag"]
["Shingle roof","Schindel-Eindeckung","Shingle roof","Toiture en bardeaux","Coperture Lamellare","Schindel-dakbedekking","Šindel","Šindeľová krytina","Pokrycie gontowe","Zsindely borítás","Pärekatto","Singlestag"]
["Plain tile roof","Biberschwanz-Eindeckung","Plain tile roof","Toitures en tuiles plates","Tegole a coda di castoro","Biberschwanz-dakbedekking","Bobrovka","Bobrovka","Dachówka kurpiówka","Hódfarkú cserép","Kalansuomukatto (saksalainen)","Bæverhaletegltag"]
["Click at desired collector arrangement","Gewünschte Kollektoranordnung im Bild anklicken.","Click at desired collector arrangement","Cliquer la disposition souhaitée","Scegliere la disposizione desiderata","Gewenste collectorrangschikking aanklikken","Zaklikněte uspořádání kolektorů","Zakliknite želané usporiadanie kolektorov","Kliknąć na odpowiednie usytuowanie kolektorów","Klikkeljen a kívánt kollektorelrendezésre","Klikkaa soveltuvaa keräinjärjestelyä","Klik på ønsket kollektorarrangement"]
[]
["Material composition","Materialliste","Material composition","Choix du matériel","Composizione materiali","Materiaal samenstelling","Soupis materiálu","Súpis materiálu","Wykaz materiałów","Anyagok összetétele","Osaluettelo","Materialeliste"]
["Position","Position","Position","Position","Posizione","Positie","Pozice","Pozícia","Położenie","Helyzet","Positio","Position"]
["Number","Anzahl","Number","Quantité","Numero","Aantal","Počet","Počet","Liczba","Darabszám","Lukumäärä","Mængde"]
["ID","Ident.-Nr.","ID","Code article","No. ident.","Identiteitsnr.","Objed.číslo","Objednávacie číslo","Nr kat.","Azonosító","ID","Varenr."]
["Description","Bezeichnung","Description","Désignation","Descrizione","Beschrijving","Označení","Označenie","Nazwa","Megnevezés","Kuvaus","Beskrivelse"]
["Price each","Einzelpreis","Price each","Prix unitaire","Prezzo unitario","Stuks prijs","Cena za jednotku","Cena za jednotku","Cena jedn.","Darabár","Kpl-hinta","Stykpris"]
["Total price","Gesamtpreis","Total price","Prix total","Prezzo complessivo","Totale prijs","Celková cena","Celková cena","Razem","Össz ár","Hinta yhteensä","Samlet pris"]
["Recommended retail price excl. VAT","Empfohlener Richtpreis ohne Mehrwertsteuer","Recommended retail price excl. VAT","Prix indicatif H.T.","Prezzo indicativo suggerito al netto di IVA","Advies verkoopprijs excl. BTW","Doporučená cena bez DPH","Doporučená cena bez DPH","Zalecana cena orientacyjna netto","Ajánlott ár ÁFA nélkül","Bruttohinta (alv. 0 %)","Vejl. udsalgspris ekskl. moms"]
["Add product","Artikel hinzufügen","Add product","Ajouter un article","Aggiunta di un articolo","Toevoegen van een product","Zaveďte výrobek","Pridať položku","Kliknij dwukrotnie","Cikk hozzáfűtése","Lisää tuote","Tilføj produkt"]
["Reset standard values","Standard wiederherstellen","Reset standard values","Restaurer les valeurs standards","Ripristina predefinito","Standaard terugzetten","Standard opravit","Späť na štandard","Powrót do standardowego","Alaphelyzet visszaállítása","Palauta oletusarvot","Gendan standardværdier"]
["Optional accessories","Optionales Zubehör","Optional accessories","Accessoires en option","Accessori opzionali","Optionele toebehoren","Možné příslušenství","Možné príslušenstvo","Opcjonalne wyposażenie dodatkowe","Opcionális tartozék","Vaihtoehtoiset lisävarusteet","Ekstra tilbehør"]
["SOKI with integral control unit","SOKI mit integrierter Regelung","SOKI with integral control unit","SOKI à régulation intégrée","SOKI con regolazione integrata","SOKI met geïntergreerde regeling","SOKI s vestavěnou regulací","SOKI s integrovanou reguláciou","SOKI ze zintegrowaną regulacją","Kompakt szolárrendszer integrált szabályozással","SOKI integroidulla ohjausyksiköllä","SOKI med ingreret styring"]
["SOKI installation at the SBB...Plus","SOKI Montage an SBB...Plus","SOKI installation at the SBB...Plus","Montage SOKI sur SBB...Plus","SOKI Montaggio su SBB...Plus","SOKI installatie op SBB… Plus","Montáž SOKI na SBB...plus","Montáž SOKI na SBB ... Plus","Montaż SOKI w SBB...Plus","Kompakt szolárrendszer szerelése SBB...Plus-ra","SOKI-asennus SBB..plussaan","SOKI montage på SBB…Plus"]
["Heat metering","Wärmemengenzählung","Heat metering","Compteur de chaleur","Contatore quantità di calore","Warmtehoeveelheidsmeting","Měřič tepla","Merač tepla","Licznik ciepła","Hőmennyiségmérés","Lämpömäärän mittaus","Energimåler"]
["Heating diverter valve","Heizungsumschaltventil","Heating diverter valve","Vanne d'inversion chauffage","Valvola di interscambio riscaldamento","Verwarmingsomschakelventiel","Přepínací ventil vytápění","Prepínací ventil vykurovania","Zawór przełączający ogrzewania","Fűtéskapcsoló szelep","Lämmönjakoventtiili","Varme-omskifterventil"]
["Threaded immersion heater BGC","Elektrische Nacherwärmung","Threaded immersion heater BGC","Corps de chauffe à visser BGC","Riscaldatore a vite BGC","Verwarmingselement BGC","Šroubovatelné topné těleso BGC","Skrutkovacie ohrievacie teleso BGC","Grzałka wkręcana BGC","BGC becsavarható fűtőtest","Lisäsähkövastus BGC","Elektrisk varmelegeme BGC"]
["Central thermostatic valve","Zentral-Thermostatarmatur","Central thermostatic valve","Mitigeur thermostatique ECS","Miscelatore termostatico centrale","Centraal thermostaatventiel","Centrální termostatická armatura","Centrálna termostatická batéria","Centralna armatura termostatyczna","Központi termosztát","Kolmitiesekoitusventtiili","Central-thermostatiskventil"]
["Heat transfer medium H-30 LS","Wärmeträger-Flüssigkeit H-30 LS","Heat transfer medium H-30 LS","Fluide caloporteur H-30 LS","Termovettore - liquido H-30 LS","Warmtedragervloeistof H-30 LS","Nemrznoucí kapalina H-30 LS","Nemrznúca kvapalina H-30 LS","Ciecz przenosząca ciepło H-30 LS","Hőhordozó folyadék H-30 LS","Lämmönsiirtoaine H-30 LS","Varmeoverførselsvæske"]
["Please enter product number and description.","Bitte Artikelnummer oder -bezeichnung eingeben.","Please enter product number and description.","Merci d'entrer le code article ou sa désignation.","Inserire il numero di articolo o descrizione.","Gelieve artikelnummer of beschrijving opgeven","Prosím zadejte objednací číslo nebo označení","Prosím zadajte objednávacie číslo alebo označenie","Podaj numer lub nazwę artykułu.","Kérjük, adja meg a cikk számát vagy megnevezését.","Anna tuotenumero tai kuvaus.","Indtast varenr. og beskrivelse"]
["Search...","Suchen...","Search...","Rechercher...","Ricerca in corso...","Zoeken…","Hledat...","Hľadať...","Znajdź...","Keresés...","Hae…","Søg…"]
["Add to material list","Zu Materialliste hinzufügen","Add to material list","Ajouter à la liste de matériel","Aggiungere all'elenco materiali","Toevoegen aan materiaallijst","Zavést do seznamu výrobků","Pridať do zoznamu výrobkov","Dodaj do listy materiałów","Hozzáfűzés az anyaglistához","Lisää osaluetteloon","Tilføj til materialeliste"]
["Remove from material list","Aus Materialliste entfernen","Remove from material list","Supprimer de la liste de matériel","Rimuovere dall'elenco materiali","Verwijderen uit materiaallijst","Odstranit ze seznamu výrobků","Odstrániť zo zoznamu výrobkov","Usuń z listy materiałów","Eltávolítás az anyaglistából","Poista osaluettelosta","Fjern fra materialeliste"]
["Close window","Fenster schließen","Close window","Fermer la fenêtre","Chiudi finestra","Venster sluiten","Zavřít okno","Zavrieť okno","Zamknij okno","Ablak bezárása","Sulje ikkuna","Luk vindue"]
["The DHW cylinder determined by reference to collector number is not sufficient for the specified DHW demand. This cylinder is recommended:","Der anhand der Kollektorzahl ermittelte Standard-Systemspeicher ist für den angegebenen Warmwasserbedarf nicht ausreichend. Für die gewählte Anlagenkonfiguration wird folgender Speichertyp empfohlen:","The DHW cylinder determined by reference to collector number is not sufficient for the specified DHW demand. This cylinder is recommended:","Le ballon ECS préconisé en fonction du nombre de capteur n'est pas suffisant pour couvrir les besoins ECS. Pour la configuration choisie, nous préconisons le ballon suivant :","In base alla scelta del numero dei collettori solari, con il sistema standard, il bollitore non è sufficiente alla richiesta dell'acqua calda.\nPer il sistema scelto viene consigliato il seguente tipo:","De boiler, welke gekozen is aan de hand van het aantal collectoren, is niet toereikend voor het gekozen warmwater gebruik. Voor de gekozen configuratie wordt de volgende boiler aanbevolen:","Standardní systémový zásobník zvolený na základě počtu kolektorů je pro zadanou potřebu teplé vody nedostatečný. Pro zvolenou konfiguraci zařízení doporučujeme následující typ zásobníku:","Štandardný zásobník zvolený na základe počtu kolektorov je pre udanú spotrebu teplej vody nedostatočný. Pre zvolenú konfiguráciu systému doporučujeme nasledujúci typ zásobníka:","Der anhand der Kollektorzahl ermittelte Standard-Systemspeicher ist für den angegebenen Warmwasserbedarf nicht ausreichend. Für die gewählte Anlagenkonfiguration wird folgender Speichertyp empfohlen:","A kollektorszámból adódó tárolókapacitás nem elég a megadott melegvízigényhez. A kiválasztott rendszerkonfigurációhoz a következő tároló(k) ajánlott:","Esivalittu käyttövesivaraaja ei sovellu optimaalisesti osaluettelon keräinmäärälle. Seuraavaa varaajaa suositellaan:","Varmtvandsbeholderen valgt på baggrund af kollektor antallet, er ikke tilstrækkelig til det specificerede varmtvandsforbrug. Det anbefales at benytte denne beholder:"]
["Do you want to replace DHW cylinder ?","Soll der vorhandene Speicher ersetzt werden ?","Do you want to replace DHW cylinder ?","Le ballon ECS existant doit-il être remplacé?","Sostituire l'accumulatore esistente?","Dient de huidige boiler verwijderd te worden?","Má být použit stávající zásobník","Má byť zásobník nahradený?","Czy istniejący zasobnik ma być wymieniony ?","Kicseréli a tárolót?","Korvataanko käyttövesivaraaja?","Vil du ændre varmtvandsbeholder ?"]
["Print material list","Materialliste drucken","Print material list","Imprimer la liste de matériel","Stampa lista del materiale","Materiaallijst afdrukken","Výpis materiálu - tisk","Výpis materiálu- tlač","Drukowanie listy materiałowej","Anyaglista nyomtatása","Tulosta osaluettelo","Udskriv materialeliste"]
["Printout with prices","Ausdruck mit Preisen","Printout with prices","Imprimer avec les prix","Richiedi tariffe","Afdrukken met prijzen","Získat sazby","Získať sadzby","Sprawdź cenę","Tarifák","Tulosta hintojen kanssa","Udskriv med priser"]
["Printout without prices","Ausdruck ohne Preise","Printout without prices","Imprimer sans les prix","Printout without prices","Afdrukken zonder prijzen","Printout without prices","Printout without prices","Printout without prices","Printout without prices","Tulosta ilman hintoja","Udskriv uden priser"]
["Export material-list","Excel-Blatt exportieren","Export material-list","Exporter le fichier Excel","Esportare","Excel blad exporteren","Exportovat do Excelu","Exportovať do excelu","zapisać w pamieci","Excell tábla exprtálása","Tallenna osaluettelo","Eksporter materialeliste"]
["Edit pricelist","Preisliste bearbeiten","Edit pricelist","Modifier le tarif","Modifica listino prezzi","Bewerking prijslijst","Zpracovávání ceníku","Spracovať cenník","Edytuj cennik","Árlista szerkesztés","Muokkaa hintaluetteloa","Rediger prisliste"]
["There were changes made to the selected solar system. The material list will be rebuilt (reset of  manual changes).","Es wurden Änderungen am gewählten Solar-System vorgenommen. Die Materialliste wird neu erstellt und manuelle Änderungen zurückgesetzt.","There were changes made to the selected solar system. The material list will be rebuilt (reset of  manual changes).","Des modifications ont été apportées au système sélectionné solaire. La liste de matériel va être réédité et les modifications manuelles réinitialisées.","Ci sono state le modifiche apportate al sistema selezionato solare. La lista dei materiali sarà ricostruito e resettare le modifiche manuali.","Er zijn veranderingen aangebracht in het geselecteerde systeem. De materiallijst wordt opnieuw samengesteld en handmatige wijzigingen teruggezet.","Tam byly změny vybraného sluneční soustavy. Materiály seznam bude přestavěn a reset ruční změny.","Tam boli zmeny vybraného slnečnej sústavy. Materiály zoznam bude prestavaný a reset ručné zmeny.","Nie było zmian do wybranego układu słonecznego. Lista materiałów zostanie przebudowana i kasowanie ręczne zmiany.","Voltak változások a kiválasztott Naprendszerben. Az anyagok lista átépítették és reset manuális változásokat.","Valittuun aurinkolämpöjärjestelmään tehtiin muutoksia. Osaluettelo laadittiin uusiksi.","Der er lavet ændringer til det valgte solfangersystem. Materialelisten vil blive omskrevet (brugerændringer vil blive nulstillet)."]
["All changes and items manually added will be resetted. Continue ?","Alle Änderungen und manuell hinzugefügten Artikel werden zurückgesetzt. Fortfahren ?","All changes and items manually added will be resetted. Continue ?","Tous les changements et les éléments ajoutés manuellement seront réinitialisés. Continuer?","Tutte le modifiche e le voci aggiunte manualmente verrà azzerata. Continua?","Alle wijzigingen en handmatig toegevoegde items worden teruggezet. Doorgaan?","Všechny změny a ručně přidané položky bude reset. Chcete pokračovat?","Všetky zmeny a ručne pridanej položky bude reset. Chcete pokračovať?","Wszystkie zmiany i ręcznie dodane elementy zostaną zresetowane. Kontynuować?","Minden változás, és manuálisan hozzáadott elemek visszaáll. Folytatás?","Kaikki aiemmat muutokset ja osat korvataan. Haluatko jatkaa?","Alle ændringer og tilføjede produkter vil blive fjernet. Fortsæt ?"]
[]
["Stiebel Eltron pricelist","Stiebel Eltron Preisliste","Stiebel Eltron pricelist","Tarif Stiebel Eltron","Listino prezzi Stiebel Eltron","Stiebel Eltron prijslijst","Stiebel Eltron Ceník","Stiebel Eltron Cenník","Cennik Stiebel Eltron","Stiebel Eltron árlista","Stiebel Eltron bruttohinnasto (alv. 0%)","Stiebel Eltron prisliste"]
["Edit","Bearbeiten","Edit","Modifier","Modifica","Bewerking","Zpracovávání","Spracovávanie","Edytuj","Szerkesztés","Muokkaa","Rediger"]
["Back to main window","Zurück zum Hauptfenster","Back to main window","Retour à la page principale","Indietro","Terug naar het hoofdvenster","zpět do hlavního okna","Späť do hlavného okna","Powrót do okna głównego","Vissza a főmenübe","Takaisin päävalikkoon","Tilbage til hovedskærmbillede"]
["Show values changed","Geänderte Werte anzeigen","Show values changed","Afficher les valeurs modifiées","mostra valori modificati","Veranderde waarden aangeven","Zobrazit změněné hodnoty","Zobraziť zmenené hodnoty","Pokazanie zmienionych wartości","Megváltoztatott értékeket megmutat","Näytä muokatut arvot","Vis ændrede værdier"]
["Add product to price list","Artikel zur Preisliste hinzufügen","Add product to price list","Ajouter un produit à la liste de prix","Aggiungi il Prodotto al listino","Product toevoegen aan prijslijst","Zavést výrobek do ceníku","Pridať položku do cenníku","Dodanie pozycji do cennika","Cikket az árlistához ad","Lisää tuote hintaluetteloon","Tilføj vare til prislisten"]
["Import pricelist","Preisliste importieren","Import pricelist","Importer tarif","Importazione listino prezzi","Prijslijst importeren","Import ceníku","Import cenník","wczytaj cennik","Import pricelist","Tuo hintaluettelo","Importer prisliste"]
[]
["Solar yield","Solarer Ertrag","Solar yield","Production solaire","Resa solare","Solar bijdrage","Solární zisk","Solármy zisk","Zysk solarny","Napenergia hozam","Lämmöntuotto","Solvarmeudbytte"]
["Occupants","Personen","Occupants","Personnes","Persone","Personen","Počet osob","Počet osôb","Osoby","Személyek","kuluttajaa","Antal personer"]
["l/day","l/Tag","l/day","l/jour","l/giorno","l/dag","l/den","l/deň","l/dzień","l/nap","litraa/päivä","L/dag"]
["Recommended cylinder","Speicherempfehlung","Recommended cylinder","Ballon recommandé","Suggerimento accumulatore","Geadviseerde boiler","Doporučení zásobníku","Odporúčanie zásobníka","Zalecenie dotyczące zasobnika","Ajánlott tároló","Suositeltu varaaja","Anbefalet beholder"]
["Heat demand","Wärmebedarf","Heat demand","Besoin en chaleur","Necessità di calore","Warmtevraag","Potřeba tepla","Spotreba tepla","Zapotrzebowanie ciepła","Hőigény","Lämmöntarve","Varmebehov"]
["Solar coverage DHW heating","Deckungsanteil Warmwasserbereitung","Solar coverage DHW heating","Couverture production ECS","Copertura produzione acqua calda","Dekkingsgraad warmwaterbereiding","Pokrytí přípravy teplé vody","Pokrytie prípravy  teplej vody","Pokrycie przy przygotowaniu ciepłej wody (ogrzewania wody)","Melegvízkészítés fedezete","Kattavuus, käyttövesi","Dækningsgrad VV-opvarmning"]
["Annual heat demand","Jahresheizwärmebedarf","Annual heat demand","Besoin annuel en chauffage","Fabbisogno calorifico annuale","Jaarlijks warmteverlies","Roční spotřeba tepla pro vytápění","Ročná spotreba tepla na vykurovanie","Roczne zapotrzebowanie ciepła grzewczego","Éves fűtési hőenergia-szükséglet","Vuotuinen lämmitysenergiantarve","Årligt varmeforbrug"]
["Heating water buffer cylinder","Heizungspufferspeicher","Heating water buffer cylinder","Ballon tampon","Accumulatore tampone del riscaldamento","Buffervat (verwarming)","Vyrovnávací zásobník topení","Akumulačná nádrž vykurovania","Zbiornik buforowy ogrzewania","Fűtési puffertároló","SOL-puskurivaraaja","Bufferbeholder centralvarme"]
["Solar yield heating backup","Solarer Ertrag Heizungsunterstützung","Solar yield heating backup","Apport solaire appoint chauffage","Reddito solare termico sostegno del riscaldamento ","Solar opbrengst verwarmingsondersteuning","Solární teplo, dodané do topení","Solárne teplo, dodané do vykurovacieho systému","Solarny zysk przy wspomaganiu ogrzewania","Szolár fűtésrásegítés hozam","Lämmitysenergiantuotto lämmitykseen","Solvarmeudbytte opvarmning"]
["Coverage DHW | Heating backup","Deckung Warmwasser | Heizung","Coverage DHW | Heating backup","Couverture chauffage | ECS","Copertura riscaldamento | Acqua calda sanitaria","Dekkingsdeel verwarming | warmwater","Pokrytí topení | teplé vody","Pokrytie podielu  teplej vody| vykurovanie","Pokrycie przy c.o. | c.w.u.","Melegvíz | fűtés fedezet","Kattavuus, käyttövesi ja lämmitys","Dækning af VV | Varme"]
["Swimming pool type | Volume","Schwimmbadart | Volumen","Swimming pool type | Volume","Type de piscine | Volume","Tipo di piscina | Volume","Zwembadtype | Volume","Druh bazénu | Objem","Druh bazénu | Objem","Typ basenu | Pojemność","Medence jellege | Térfogat","Uima-altaan tyyppi | Tilavuus","Swimmingpooltype | Volumen"]
["Duration of use | Cooling","Nutzungsdauer | Abkühlung","Duration of use | Cooling","Durée d'utilisation | Refroidissement","Durata uso | Raffreddamento","Gebruiksduur | Afkoeling","Doba využitelnosti | chlazení","Doba využitelnosti | Chladenie","Czas użytkowania | ochłodzenie","Használati időtartam | Kihűlés","Käyttöaika | Lämpöhukka","Brugstid | Køling"]
["Heat demand for reheating","Wärmebedarf Nachheizung","Heat demand for reheating","Besoin en chaleur chauffage complémentaire","Fabbisogno calorifico riscaldamento supplementare","Warmtevraag naverwarming","Spotřeba tepla – dohřívání","Spotreba tepla doplnkový ohrev","Zapotrzebowanie ciepła do ogrzewania dodatkowego","Hőigény | Utánfűtés","Päivittäinen lämmöntarve","Varmebehov til genopvarmning"]
["Solar yield swimming pool","Solarer Ertrag Schwimmbad","Solar yield swimming pool","Apport solaire piscine","Reddito solare termico sostegno della piscina","Solar bijdrage zwembad","Solární teplo, dodané do bazénu","Solárne teplo, dodané do bazénu","Solarny zysk przy basenie","Szolár medencefűtés hozam","Lämmöntuotto uima-altaaseen","Solvarmeudbytte swimmingpool"]
["Coverage heat loss swimming pool","Deckung Wärmeverluste Schwimmbad","Coverage heat loss swimming pool","Couverture déperditions piscine","Copertura perdita calore piscina","Dekkingsgraad warmteverlies zwembad","Pokrytí tepelných ztrát koupaliště","Pokrytie tepelných strát bazén","Pokrycie strat ciepła wody basenowej","Uszoda hőveszteségeinek fedezete","Uima-altaan lämpöhäviöiden kattavuus","Dækning af varmetab fra swimmingpool"]
["Show list of results","Ergebnistabelle anzeigen","Show list of results","Afficher le tableau des résultats","Visualizza Risultati","Resultaten tabel tonen","Zobrazit tabulku výsledků","Zobraziť tabuľku s výsledkami","Pokazanie tabeli wyników","Eredménylistát megmutat","Näytä yhteenvetoluettelo","Vis resultatliste"]
["Show graph","Diagramm anzeigen","Show graph","Afficher le diagramme","Visualizza grafico","Diagram tonen","Zobrazit diagram","Zobraziť diagram","Pokazanie wykresu","Grafikont megmutat","Näytä graafi","Vis graf"]
["Jan","Jan","Jan","Jan","Jan","Jan","Jan","Jan","Jan","Jan","Tam","Jan"]
["Feb","Feb","Feb","Fév","Feb","Feb","Feb","Feb","Feb","Feb","Hel","Feb"]
["Mar","Mrz","Mar","Mar","Mar","Mrt","Mar","Mar","Mar","Mar","Maa","Mar"]
["Apr","Apr","Apr","Avr","Apr","Apr","Apr","Apr","Apr","Apr","Huh","Apr"]
["May","Mai","May","Mai","May","Mei","May","May","May","May","Tou","Maj"]
["Jun","Jun","Jun","Jun","Jun","Jun","Jun","Jun","Jun","Jun","Kes","Jun"]
["Jul","Jul","Jul","Jul","Jul","Jul","Jul","Jul","Jul","Jul","Hei","Jul"]
["Aug","Aug","Aug","Aou","Aug","Aug","Aug","Aug","Aug","Aug","Elo","Aug"]
["Sep","Sep","Sep","Sep","Sep","Sep","Sep","Sep","Sep","Sep","Syy","Sep"]
["Oct","Okt","Oct","Oct","Oct","Okt","Oct","Oct","Oct","Oct","Lok","Okt"]
["Nov","Nov","Nov","Nov","Nov","Nov","Nov","Nov","Nov","Nov","Mar","Nov"]
["Dec","Dez","Dec","Déc","Dec","Dec","Dec","Dec","Dec","Dec","Jou","Dec"]
["DHW heating","Warmwasserbereitung","DHW heating","Production ECS","Produzione di acqua calda","Warmwaterbereiding","Příprava teplé vody","Teplá vody","Przygotowanie ciepłej wody","Melegvíz-előállítás",", käyttöveden lämmitys","Varmtvandsopvarmning"]
["Solar coverage","Solarer Deckungsanteil","Solar coverage","Taux de couverture solaire","Quota copertura solare","Solar dekkingsaandeel","Solární pokrytí","Podiel pokrytia solár. zariadením","Pokrycie zapotrzebowania przez instalację solarną","Szolárfedezet","Kattavuus","Solvarmedækningsgrad"]
["Extended settings","Erweiterte Einstellungen","Extended settings","Configuration étendue","Impostazioni avanzate","Gewijzigde instellingen","Rozšířené nastavení","Rozšírené nastavenie","Ustawienia zaawansowane","További beállítások","Lisäasetukset","Flere indstillinger"]
["Cold water temperature","Kaltwassertemperatur","Cold water temperature","Température eau froide","Temperatura acqua fredda","Koudwater temperatuur","Teplota studené vody","Teplota studenej vody","Temperatura zimnej wody","Hidegvíz hőmérséklete","Kylmän veden lämpötila","Koldtvandstemperatur"]
["Cylinder temperature","Speichertemperatur","Cylinder temperature","Température ballon","Temperatura accumulatore","Boiler temperatuur","Teplota v zásobníku","Teplota v zásobníku","Temperatura zasobnika","Tároló-hőmérséklet","Varaajan lämpötila","Buffertemperatur"]
["System losses DHW","Systemverluste WWB","System losses DHW","Déperditions du système ECS","Perdite di sistema WWB","Syteem verliezen WWB","Systémová ztráta přípravy TV","Systémová strata prípravy teplej vody","Straty w układzie c.w.u.","HMV készítés rendszerveszteségei","Käyttövesihäviöt","Systemtab VV"]
["Standard outside temperature","Normaußentemperatur","Standard outside temperature","Température extérieure de base","Temperatura esterna di norma","Norm buitentemperatuur","Normovaná venkovní teplota","Normovaná vonkajšia teplota","Normatywna temperatura zewnętrzna","Normál külső hőmérséklet","Mitoitusulkolämpötila","Standard udetemperatur"]
["Heating limit temperature","Heizgrenztemperatur","Heating limit temperature","Temp. limite de chauffage","Temperatura limite di riscaldamento","Verwarmingsgrens","Mezní teplota ohřevu","Hraničná teplota ohrevu","Temperatura graniczna ogrzewania","Fűtési határhőmérséklet","Lämmityksen lämpötilaraja","Varmegrænsetemperatur"]
["Accept","Übernehmen","Accept","Appliquer","Applica","Accepteren","Přijmout","Prevziať","Zastosuj","Beállítás","Hyväksy","Accepter"]
["Standard values","Standardwerte","Standard values","Valeurs standards","Valori predefiniti","Standaard waarden","Standardní hodnota","Štandardná hodnota","Wartości standardowe","Alapértékek","Oletusarvot","Standard værdier"]
[]
["Hydraulical scetch","Hydraulik | Elektrik","Hydraulical scetch","Hydraulique | Électrique","Idraulica |Elettrica","Hydraulisch | Electrisch","Hydraulika |Elektro","Príprava teplej vody","Hydraulika | Elektryka","Hidraulika | Villanyszerelés","Kytkentäkaavio","Installationstegning"]
["Scheme is not available yet.","Zeichnung bisher nicht verfügbar.","Scheme is not available yet.","Le schéma n'est pas encore disponible","Disegno non disponibile","Tekening is niet beschikbaar","Výkres není k dispozici","Výkres nie je k dispozícii","Rysunek na razie niedostępny","Rajz még nem elérhető","Kytkentäkaaviota ei ole tällä hetkellä saatavilla.","Installationstegning er ikke tilgængelig"]
["Second Heat source","Zweiter Wärmeerzeuger","Second Heat source","2ème générateur de chaleur","2. generatore di calore","2e Warmtebron","2.zdroj tepla","2.zdroj tepla","Druga wytwornica ciepła","2. hőfejlesztő","Toinen lämmönlähde","Anden varmekilde"]
["None","Keiner","None","sans","Nessuno","Geen","Žádný","Žiadny","Brak","Nincs","Ei mikään","Ingen"]
["Heat pump","Wärmepumpe","Heat pump","Pompe à chaleur","Pompa di calore","Warmtepomp","Tepelné čerpadlo","Tepelné čerpadlo","Pompa ciepła","Hőszivattyú","Lämpöpumppu","Varmepumpe"]
["Instantaneous water heater","Durchlauferhitzer","Instantaneous water heater","Chauffe-eau instantané","Scaldacqua istantaneo","Doorstromer","Průtokový ohřívač","Prietokový ohrievač","Ogrzewacz przepływowy","Átfolyós vízmelegítő","Läpivirtauslämmitin","Gennemstrømningsvandvarmer"]
["Oil/gas boiler","Öl-/Gaskessel","Oil/gas boiler","Chaudière fuel / gaz","Caldaia Olio combustibile | Gas","Olie-/Gasketel","Olej./plyn.kotel","Olejový/ Plynový kotol","Kocioł olejowy/gazowy","Olaj-/gázkazán","Öljy-/kaasukattila","Oli/gaskedel"]
["Solid fuel boiler","Feststoffkessel","Solid fuel boiler","Chaudière à combustible solide","Caldaia a propellente solido","Allesbrander","Kotel na tuhá paliva","Kotol na tuhé palivo","Kocioł paliwa stałego","Szilárd tüzelésű kazán","Kiinteän polttoaineen kattila","Fastbrændselskedel"]
["Show hydraulic scetch","Hydraulik anzeigen","Show hydraulic scetch","Afficher le schéma hydraulique","Visualizza schema idraulico","Hydraulisch plan tonen","Zobrazit hydraulické schéma","Zobraziť schému hydraulického zapojenia","Pokazanie hydrauliki","Hidraulikus vázlatot megmutat","Näytä LVI-kytkentäkaavio","Vis hydraulisk tegning"]
["Show electrical scetch","Elektrik anzeigen","Show electrical scetch","Afficher le schéma électrique","Visualizza schema elettrico","Elektrisch plan tonen","Zobrazit elektrické schéma","Zobraziť schému elektrického zapojenia","Pokazanie elektryki","Elektromos vázlatot megmutat","Näytä sähkökytkentäkaavio","Vis el tegning"]
["Show description","Positionsliste anzeigen","Show description","Afficher la nomenclature","Visualizza lista posizione","Positielijst tonen","Zobrazit výpis materiálu","Zobraziť súpis materiálu","Pokazanie listy pozycji","Kiírást megmutat","Näytä kuvaukset","Vis beskrivelse"]
["Show pipework installation","Rohrinstallation anzeigen","Show pipework installation","Afficher le réseau hydraulique","Installazione tubazione","Leidinginstallatie","Instalace trubek","Zobraziť inštaláciu trubiek","Instalacja rurowa","Csőtelepítés","Näytä putkiasennuskuva","Vis rørinstallation"]
["Heat pump","Wärmepumpe","Heat pump","Pompe à chaleur","Pompa di Calore","Warmtepomp","Tepelné čerpadlo","Tepelné čerpadlo","Pompa ciepła","Hőszivattyú","Lämpöpumppu","Varmepumpe"]
["Exhaust air module: LWM 250","Luftungsmodul LWM 250","Exhaust air module: LWM 250","Module de ventilation centralisé LWM 250","Modulo per Aria Esausta: LWM 250","Ventilatiemodule LWM 250","Ventilační modul LWM 250","Odvetrávací modul LWM 250","Moduł wentylacji LWM 250","Szellőztető modul LWM 250","Ilmastointimoduuli LWM 250","Udsugningsmodul: LWM 250"]
["Cooling module: WPAC","Kühlmodul WPAC","Cooling module: WPAC","Module de rafraîchissement WPAC","Modulo Raffrescamento:WPAC","Koelmodule WPAC","Chladicí modul WPAC","Chladiaci modul WPAC","Moduł chłodzący WPAC","Hűtőmodul WPAC","Jäähdytysmoduuli WPAC","Kølemodul: WPAC"]
["Control unit: WPMW","Regelgerät WPMW / WPMS","Control unit: WPMW","Régulation de pompe à chaleur WPMW","Termoregolatore: WPMW","WP manager WPMW","Regulace WPMW","Regulačná jednotka WPMW","Regulator WPMW","Szabályzó berendezés WPMW","Ohjausautomatiikka WPMW","Styresystem: WPMW / WPMS"]
["Swimming pool module: MSMW","Mischermodul MSMW / WPMS","Swimming pool module: MSMW","Régulation auxiliaire MSMW circuit mélangeur/piscine ","Modulo Piscina:MSM","Zwembadregeling MSMW","Směšovací modul MSMW","Modul miešača MSMW","Moduł mieszacza MSMW","Keverőmodul MSMW","Lisäautomatiikka MSMW","Swimmingpoolmodul: MSMW"]
["Remote control: FE 7","Fernbedienung FE 7","Remote control: FE 7","Commande à distance FE7","Controllo remoto:FE7","Thermostaat FE7","Dálkový ovladač FE 7","Diaľkové ovládanie FE 7","Zdalne sterowanie FE7","Távirányító FE 7","Kauko-ohjain FE 7","Fjenbetjening: FE 7"]
["Remote control cooling: FEK","Fernbedienung Kühlung FEK","Remote control cooling: FEK","Commande à distance pour rafraîchissement FEK","Controllo remoto raffrescamento:FEK","Thermostaat met koel-functie FEK","Dálkový ovladač chlazení FEK","Diaľkové ovládanie Chladenie FEK","Zdalne sterowanie chłodzenia FEK","Hűtés távirányító FEK","Jäähdytyksen kauko-ohjain FEK","Fjernbetjening køling: FEK"]
["Temperature sensor: Outside temperature","Außentemperaturfühler","Temperature sensor: Outside temperature","Sonde de température extérieure","Sensore di Temperatura: Temperatura Esterna","Buitentemperatuurvoeler","Snímač venkovní teploty","Snímač vonkajšej teploty","Czujnik temperatury zewnętrznej","Külső hőmérséklet-érzékelő","Ulkolämpötila-anturi","Temperatursensor: Udetemperatur"]
["Temperature sensor: Return temperature","Rücklauftemperaturfühler Wärmepumpe","Temperature sensor: Return temperature","Sonde de température retour PAC","Sensore di Temperatura: Temperatura di Ritorno","Retourtemperatuurvoeler WP","Snímač teploty vratného toku tepelného čerpadla","Snímač vratnej teploty Tepelné čerpadlo","Czujnik temperatury powrotu pompy ciepła","Hőszivattyú visszatérő ági hőmérséklet-érzékelője","Paluuvirtauksen/puskurivaraajan lämpötila-anturi","Temperatursensor: Returtemperatur"]
["Temperature sensor: Flow temperature, DHW \"off\"","Vorlauftemperaturfühler, Warmwasserbereitung \"Aus\"","Temperature sensor: Flow temperature, DHW \"off\"","Sonde de température départ PAC, ECS \"OFF\"","Sensore di Temperatura: Temperatura di Mandata, ACS\"off\"","Aanvoertemp. voeler, warmwaterbereiding \"uit\"","Snímač teploty přítoku, příprava teplé vody \"VYP\"","Snímač prívodnej teploty, príprava teplej vody „Vyp”","Czujnik temperatury zasilania, przygotowanie ciepłej wody „wył”","Előremenő ági hőmérséklet-érzékelő, melegvízkészítés „Ki”","Lämpöpumpun menovirtauksen lämpötila-anturi","Temperatursensor: Fremløbstemperatur, ingen VV"]
["Temperature sensor: Flow temperature, DHW \"on\"","Warmwassertemperaturfühler, Warmwasserbereitung \"Ein\"","Temperature sensor: Flow temperature, DHW \"on\"","Sonde de température départ PAC, ECS \"ON\"","Sensore di Temperatura: Temperatura di Mandata, ACS\"on\"","Warmwatertemp. voeler, warmwaterbereiding \"aan\"","Snímač teploty teplé vody, příprava teplé vody \"Zap\"","Snímač teploty teplej vody, príprava teplej vody „Zap”","Czujnik temperatury ciepłej wody, przygotowanie ciepłej wody „zał”","Melegvíz hőmérséklet-érzékelő, melegvízkészítés „Be”","Käyttövesivaraajan lämpötila-anturi","Temperatursensor: Fremløbstemperatur, med VV"]
["Temperature sensor: Mixer control","Heizkreistemperaturfühler für Mischerregelung","Temperature sensor: Mixer control","Sonde de température départ du circuit de chauffage mélangé","Sensore di temperatura: Miscelazione","Temperatuurvoeler verwarming voor mengregeling","Snímač teploty topného okruhu pro regulaci směšovače","Snímač teploty ohrievacieho okruhu pre reguláciu miešača","Czujnik temperatury obiegu grzewczego do regulacji mieszacza","Fűtőköri hőmérséklet-érzékelő keverőszabályozáshoz","Lämmityspiirin lämpötila-anturi sekoittimen säätöyksikköön","Temperatursensor: Blandeventil"]
["Temperature sensor: Heat source 2","Temperaturfühler zweiter Wärmeerzeuger","Temperature sensor: Heat source 2","Sonde de température 2ème générateur de chaleur","Sensore di temperatura: 2°Generatore di calore","Temperatuurvoeler van 2e verwarmingstoestel","Snímač teploty 2. tepelného zdroje","Snímač teploty 2. generátor tepla","Czujnik temperatury 2. wytwornicy ciepła","Hőmérséklet-érzékelő 2. Hőfejlesztő","Lämpötila-anturi, 2. lämmöntuottaja","Temperatursensor: 2. varmekilde"]
["Temperature sensor: Heat source ","Wärmequellentemperaturfühler","Temperature sensor: Heat source ","Sonde de température source primaire","Sensore di temperatura: Generatore di calore","Bronaanvoertemperatuurvoeler","Snímač teploty tepelného zdroje","Snímač teploty zdroja tepla","Czujnik temperatury dolnego źródła","Hőforrás hőmérséklet-érzékelője","Lämmönlähteen lämpötila-anturi","Temperatursensor: Varmekilde"]
["Temperature sensor: Swimming pool water heating","Schwimmbadtemperaturfühler","Temperature sensor: Swimming pool water heating","Sonde de température piscine","Sensore di Temperatura: Riscaldamento Piscina","Aanlegvoeler zwembad","Snímač teploty bazénu","Snímač teploty bazénu","Czujnik temperatury wody basenowej","Medence hőmérséklet-érzékelője","Uima-altaan lämpötila-anturi","Temperatursensor: Swimmingpooltemperatur"]
["Temperature sensor: solar panel","Kollektorfühler-Solaranlage","Temperature sensor: solar panel","Sonde de température capteur solaire (retour)","Sensore di Temperatura: Collettore solare","Collectorvoeler zonnepanelen","Snímač kolektoru solárního systému","Snímač kolektora-solárny kolektor","Czujnik kolektora instalacji solarnej","Szolárrendszer kollektorérzékelője","Aurinkokeräimen lämpötila-anturi","Temperatursensor: Solvarmepanel"]
["Temperature sensor: solar panel East","Kollektorfühler-Solaranlage Ost","Temperature sensor: solar panel East","Sonde de température capteur solaire est","Sensore di Temperatura: Collettore solare Est","Collectorvoeler zonnepanelen Oost","Snímač kolektoru solárního systému - východ","Snímač kolektora-solárny kolektor Východ","Czujnik kolektora instalacji solarnej wschód","Szolárrendszer kollektorérzékelője - kelet","Aurinkokeräimen lämpötila-anturi, itäsuunta","Temperatursensor: Solvarmepanel øst"]
["Temperature sensor: solar panel West","Kollektorfühler-Solaranlage West","Temperature sensor: solar panel West","Sonde de température capteur solaire ouest","Sensore di Temperatura: Collettore solare Ovest","Collectorvoeler zonnepanelen West","Snímač kolektoru solárního systému - západ","Snímač kolektora-solárny kolektor Západ","Czujnik kolektora instalacji zachód","Szolárrendszer kollektorérzékelője - nyugat","Aurinkokeräimen lämpötila-anturi, länsisuunta","Temperatursensor: Solvarmepanel vest"]
["Temperature sensor 1:  return flow temperature increase","Fühler 1 Rücklauftemperaturanhebung","Temperature sensor 1:  return flow temperature increase","Sonde 1, élévation de la  température de retour ","Sensore di Temperatura 1: Incremento Temperatura di ritorno","Voeler 1 retourtemperatuurstijging","Snímač 1 zvýšení teploty vratného toku","Snímač 1 Zvýšenie vratnej teploty","Czujnik 1 Podwyższenie temperatury powrotu","Visszatérő hőmérséklet-emelés, érzékelő 1","Anturi 1, paluuvirtauslämpötilan nosto","Temperatursensor 1: Returtemperaturstigning"]
["Temperature sensor 2:  return flow temperature increase","Fühler 2 Rücklauftemperaturanhebung","Temperature sensor 2:  return flow temperature increase","Sonde 2, élévation de la  température de retour ","Sensore di Temperatura 2: Incremento Temperatura di ritorno","Voeler 2 retourtemperatuurstijging","Snímač 2 zvýšení teploty vratného toku","Snímač 2 Zvýšenie vratnej teploty","Czujnik 2 Podwyższenie temperatury powrotu","Visszatérő hőmérséklet-emelés, érzékelő 2","Anturi 2, paluuvirtauslämpötilan nosto","Temperatursensor 2: Returtemperaturstigning"]
["Temperature sensor: solar buffer cylinder","Speicherfühler-Solaranlage Puffer","Temperature sensor: solar buffer cylinder","Sonde ballon tampon solaire","Sensore di Temperatura: Riscaldamento Piscina","Buffertemperatuurvoeler zonnepanelen","Snímač zásobníku - akumulace solárního zařízení","Snímač zásobníka-solárny kolektor Vyrovnávací zásobník","Czujnik zasobnika instalacji solarnej, bufor","Szolárrendszer puffertároló érzékelő","Aurinkolämpöjärjestelmän puskurivaraajan lämpötila-anturi","Temperatursensor: Solfangerbeholder"]
["Temperature sensor: additional solar buffer cylinder","Speicherfühler-Solaranlage weiterer Speicher","Temperature sensor: additional solar buffer cylinder","Sonde ballon tampon solaire supplémentaire","Sensore di Temperatura: Boiler solare addizionale","Buffertemperatuurvoeler zonnepanelen extra boiler","Snímač zásobníku solárního zařízení - další zásobník","Snímač zásobníka-Solárny kolektor Ďalší zásobník","Czujnik zasobnika instalacji solarnej, kolejny zasobnik","Szolárrendszeri tárolóérzékelő, egyéb tároló","Aurinkolämpöjärjestelmän lisäpuskurivaraajan lämpötila-anturi","Temperatursensor: Ekstra solfanger-bufferbeholder"]
["Temperature sensor: solar system hot water/ cooling","Speicherfühler-Solaranlage Warmwasser / Kühlbetrieb","Temperature sensor: solar system hot water/ cooling","Sonde ballon tampon solaire / rafraîchissement","Sensore di Temperatura:Solare ACS/Raffrescamento","Buffertemperatuurvoeler zonnepanelen warmwater/koelbedrijf","Snímač zásobníku solárního zařízení - teplá voda / režim chlazení","Snímač zásobníka-Solárny kolektor Teplá voda/Chladiaci režim","Czujnik zasobnika instalacji solarnej, ciepła woda / chłodzenie","Szolárrendszeri tárolóérzékelő, melegvíz / hűtőüzem","Aurinkolämpö-/jäähdytyksen lämpötila-anturi","Temperatursensor: Solfangersystem varmtvand / køling"]
["Circulation pump: Heat pump - heat source","Umwälzpumpe für die Wärmepumpe (Wärmequelle)","Circulation pump: Heat pump - heat source","Circulateur PAC (côté primaire)","Pompa Sorgente Pompa di calore","Circulatiepomp voor de WP (bronzijdig)","Oběhové čerpadlo pro tepelné čerpadlo (tepelný zdroj)","Obehové čerpadlo pre tepelné čerpadlo (zdroj tepla)","Pompa obiegowa do pompy ciepła (dolne źródło)","Hőszivattyú (hőforrás) keringető szivattyúja","Keruupiirin liuospumppu","Cirkulationspumpe: Varmepumpe - varmekilde"]
["Circulation pump: Heat pump - heating side","Umwälzpumpe für die Wärmepumpe (heizungsseitig)","Circulation pump: Heat pump - heating side","Circulateur PAC (côté secondaire)","Pompa di circolazione Accumulo Termico","Circulatiepomp voor de WP (CV-afgiftezijdig)","Oběhové čerpadlo pro tepelné čerpadlo (strana topení)","Obehové čerpadlo pre tepelné čerpadlo (na strane ohrevu)","Pompa obiegowa do pompy ciepła (po str. ogrzewania)","Hőszivattyú (fűtésoldali) keringető szivattyúja","Lämmityksen latauspumppu","Cirkulationspumpe: Varmepumpe - varmeside"]
["Circulation pump: DHW heating","Umwälzpumpe für die Warmwassererwärmung","Circulation pump: DHW heating","Circulateur Eau Chaude Sanitaire ","Circolatore: ACS ","Circulatiepomp warmwater","Oběhové čerpadlo pro ohřev teplé vody","Obehové čerpadlo pre prípravu teplej vody","Pompa obiegowa do podgrzewania ciepłej wody","Vízmelegítés keringető szivattyúja","Käyttöveden latauspumppu","Cirkulationspumpe: VV-opvarmning"]
["Circulation pump: Heating circuit 1","Umwälzpumpe für den Heizkreis 1","Circulation pump: Heating circuit 1","Circulateur circuit de chauffage 1","Circolatore: Circuito Riscaldamento 1","Circulatiepomp stooklijn1","Oběhové čerpadlo pro topný okruh 1","Obehové čerpadlo pre ohrievací okruh 1","Pompa obiegowa do obiegu grzewczego 1","Keringető szivattyú, fűtőkör 1","Lämmityspiirin 1 kiertopumppu","Cirkulationspumpe: Varmekreds 1"]
["Circulation pump: Heating circuit 2","Umwälzpumpe für den Heizkreis 2","Circulation pump: Heating circuit 2","Circulateur circuit de chauffage 2","Circolatore: Circuito Riscaldamento 2","Circulatiepomp stooklijn2","Oběhové čerpadlo pro topný okruh 2","Obehové čerpadlo pre ohrievací okruh 2","Pompa obiegowa do obiegu grzewczego 2","Keringető szivattyú, fűtőkör 2","Lämmityspiirin 2 kiertopumppu","Cirkulationspumpe: Varmekreds 2"]
["Circulation pump: Swimming pool","Umwälzpumpe für die Schwimmbadwassererwärmung","Circulation pump: Swimming pool","Circulateur chauffage piscine","Circolatore: Piscina","Circulatiepomp zwembadverwarming","Oběhové čerpadlo pro ohřev vody v bazénu","Obehové čerpadlo pre ohrievanie vody bazénu","Pompa obiegowa do podgrzewania wody basenowej","Keringető szivattyú, medence vízmelegítés","Uima-allasveden lämmityksen kiertopumppu","Cirkulationspumpe: Swimmingpool"]
["Circulation pump: Solar DHE heating","Umwälzpumpe für die Solaranlage Warmwasserbereitung","Circulation pump: Solar DHE heating","Circulateur ECS installation solaire","Pompa di circolazione: ACS solare","Circulatiepomp solar warmwaterondersteuning","Oběhové čerpadlo pro solární zařízení na ohřev vody","Obehové čerpadlo pre solárny kolektor Príprava teplej vody","Pompa obiegowa do przygotowania ciepłej wody w instalacji solarnej","Keringető szivattyú, szolárrendszer melegvízkészítés","Aurinkolämpöjärjestelmän kiertopumppu, käyttöveden lämmitys","Cirkulationspumpe: Solfanger VV-opvarmning"]
["Circulation pump: Solar heating system","Umwälzpumpe für die Solaranlage Heizungsunterstützung","Circulation pump: Solar heating system","Circulateur installation solaire appoint chauffage","Pompa di circolazione: Riscaldamento solare","Circulatiepomp solar verwarmingsondersteuning","Oběhové čerpadlo pro solární zařízení - podpora vytápění","Obehové čerpadlo pre solárny kolektor Podpora ohrevu","Pompa obiegowa do wspomagania ogrzewania w instalacji solarnej","Keringető szivattyú, szolárrendszer fűtésrásegítés","Aurinkolämpöjärjestelmän kiertopumppu, lämmitys","Cirkulationspumpe: Solfanger varmesystem"]
["Circulation pump: Solar Swimming pool","Umwälzpumpe für die Solaranlage Schwimmbadwasser","Circulation pump: Solar Swimming pool","Circulateur installation solaire pour piscine","Pompa di circolazione: Riscaldamento Piscina solare","Circulatiepomp solar zwembadondersteuning","Oběhové čerpadlo pro solární zařízení - voda v bazénu","Obehové čerpadlo pre solárny kolektor Voda bazénu","Pompa obiegowa do wody basenowej w instalacji solarnej","Keringető szivattyú, szolárrendszer medencefűtés","Aurinkolämpöjärjestelmän kiertopumppu, uima-allas","Cirkulationspumpe: Solfanger swimmingpool"]
["Circulation pump: Solar panel East","Umwälzpumpe für die Solaranlage Feld Ost","Circulation pump: Solar panel East","Circulateur installation solaire champs de panneaux est","Pompa di circolazione: Collettore solare Est","Circulatiepomp solarveld Oost","Oběhové čerpadlo pro solární zařízení - pole východ","Obehové čerpadlo pre solárny kolektor Pole Východ","Pompa obiegowa do instalacji solarnej, pole wschód","Keringető szivattyú, szolárrendszer keleti mező","Aurinkolämpöjärjestelmän kiertopumppu, itäpuoli","Cirkulationspumpe: Solfangerpaneler øst"]
["Circulation pump: Solar panel West","Umwälzpumpe für die Solaranlage Feld West","Circulation pump: Solar panel West","Circulateur installation solaire champs de panneaux ouest","Pompa di circolazione: Collettore solare Ovest","Circulatiepomp solarveld West","Oběhové čerpadlo pro solární zařízení - pole západ","Obehové čerpadlo pre solárny kolektor Pole Západ","Pompa obiegowa do instalacji solarnej, pole zachód","Keringető szivattyú, szolárrendszer nyugati mező","Aurinkolämpöjärjestelmän kiertopumppu, länsipuoli","Cirkulationspumpe: Solfangerpaneler vest"]
["Circulation pump: Solid fuel boiler","Umwälzpumpe für den Feststoffkessel","Circulation pump: Solid fuel boiler","Circulateur chaudière bois/coke","Pompa di circolazione: Bollitore a combustibile solido","Circulatiepomp houtkachel","Oběhové čerpadlo pro kotel na tuhá paliva","Obehové čerpadlo pre kotol na tuhé palivo","Pompa obiegowa do kotła paliwa stałego","Keringető szivattyú, szilárdtüzelésű kazán","Kiinteän polttoaineen kattilan kiertopumppu","Cirkulationspumpe: Fastbrændselsfyr"]
["Circulation pump: Cooling - hest source","Umwälzpumpe für die Kühlung (heizungsseitig)","Circulation pump: Cooling - hest source","Circulateur rafraîchissement (côté chauffage)","Circolatore:Raffrescamento - Sorgente di calore","Circulatiepomp koeling (afgiftezijdig)","Oběhové čerpadlo pro chlazení (strana topení)","Obehové čerpadlo pre chladenie (na strane ohrevu)","Pompa obiegowa do chłodzenia (po str. ogrzewania)","Keringető szivattyú, hűtés (fűtésoldali)","Jäähdytyksen (lämmityspuoli) kiertopumppu","Cirkulationspumpe: Køling - varmekilde"]
["Circulation pump: Heat pump - heat source","Umwälzpumpe für die Wärmepumpe (Wärmequelle)","Circulation pump: Heat pump - heat source","Circulateur PAC (côté primaire)","Circolatore:Pompa di calore - Sorgente di calore","Circulatiepomp voor de WP (bronzijdig)","Oběhové čerpadlo pro tepelné čerpadlo (tepelný zdroj)","Obehové čerpadlo pre tepelné čerpadlo (zdroj tepla)","Pompa obiegowa do pompy ciepła (dolne źródło)","Hőszivattyú (hőforrás) keringető szivattyúja","Lämpöpumpun (lämmönlähde) kiertopumppu","Cirkulationspumpe: Varmepumpe - varmekilde"]
["Compact installation: WPKI","Wärmepumpenkompaktinstallation ","Compact installation: WPKI","Kit compact hydraulique, type WPKI ","Installazione Compatta: WPKI","Compact installatie WPKI","Kompaktní instalace, typ WPKI","Kompaktná inštalácia, typ WPKI","Instalacja kompaktowa, typ WPKI","Kompakt szerelvény, WPKI típus","WPKI asennussarja","Tilslutningssæt: WPKI"]
["Safety valve","Sicherheitsventil","Safety valve","Soupape  de sécurité","Valvola di sicurezza","Veiligheidsventiel","Pojistný ventil","Poistný ventil","Zawór bezpieczeństwa","Biztonsági szelep","Varoventtiili","Sikkerhedsventil"]
["Expansion vessel","Ausdehnungsgefäß","Expansion vessel","Vase d'expansion","Vaso d`espansione","Expansievat","Expanzní nádoba","Expanzná nádoba","Naczynie wzbiorcze","Tágulási tartály","Paisunta-astia","Ekspansionsbeholder"]
["Buffer cylinder/ low loss header","Pufferspeicher / hydraulische Weiche","Buffer cylinder/ low loss header","Ballon tampon / bouteille de découplage","Accumulo Termico/Separatore Idraulico","Buffervat / openverdeler","Akumulační zásobník / termohydraulický rozdělovač","Vyrovnávací zásobník/hydraulická výhybka","Zbiornik buforowy / rozdzielacz hydrauliczny","Puffertároló / hidraulikus szelep","Puskurivaraaja / hydraulinen tasaaja","Bufferbeholder / hydraulisk separator"]
["Anti-vibration mount","Schwingungsdämpfer oder Verbindungsschlauch","Anti-vibration mount","Flexible anti-vibratoire ou tuyau de raccordement","Tubi flessibili anti vibrazione","Compensator / verbindingsslang","Tlumič vibrací nebo spojovací hadice","Tlmič vibrácií alebo spojovacia hadica","Amortyzator drgań lub wąż łączący","Gumipuffer vagy csatlakozótömlő","Joustava paineletku","Vibrationsdæmper eller slangetilslutning"]
["Non-return valve","Rückschlagventil","Non-return valve","Clapet anti-retour","Valvola di ritegno","Terugslagklep","Zpětný ventil","Spätný ventil","Zawór zwrotny","Visszacsapószelep","Takaiskuventtiili","Kontraventil"]
["Fill & drain valve","Füll- und Entleerungshahn","Fill & drain valve","Vanne de remplissage/vidange ","Valvola di carico/scarico impianto","Vul-en aftapkraan","Plnicí a vypouštěcí kohout","Plniaci a vypúšťací kohútik","Zawór napełniająco-spustowy","Töltő- és ürítőcsap","Täyttö- ja tyhjennyshana","Fylde- og aftapningsventil"]
["Oil fired boiler / Gas fired boiler","Ölkessel / Gaskessel","Oil fired boiler / Gas fired boiler","Chaudière fioul / gaz","Bruciatore a gasolio/gas","Gas of Olie gestookte CV ketel","Olejový kotel / plynový kotel","Olejový/plynový kotol","Kocioł olejowy / gazowy","Olajkazán / Gázkazán","Öljykattila/kaasukattila","Oliekedel / Gaskedel"]
["Electric central heating","Elektro-Zentralheizung","Electric central heating","Chauffage central électrique","Resistenze elettriche supplementari","Elektrische CV ketel","Elektrické ústřední topení","Elektrické ústredné vykurovanie","Centralne ogrzewanie elektryczne","Elektromos központi fűtés","Sähkökeskuslämmitys","Elektrisk centralvarme"]
["Mixing valve","Mischventil","Mixing valve","Vanne mélangeuse","Valvola miscelatrice","Mengventiel","Směšovací ventil","Zmiešavací ventil","Zawór mieszający","Keverőszelep","Sekoitusventtiili","Blandeventil"]
["Mixing valve actuator","Stellmotor für Mischventil","Mixing valve actuator","Moteur pour vanne mélangeuse","Attuatore Valvola Miscelatrice","Aandrijfmotor voor mengventiel","Servomotor pro směšovací ventil","Servomotor pre zmiešavací ventil","Siłownik do zaworu mieszającego","Szelepmotor keverőszelephez","Sekoitusventtiilin toimilaite","Aktuator til blandeventil"]
["Heating control unit","Heizungsregelgerät","Heating control unit","Régulation de chauffage","Termoregolatore ","Regelunit verwarming","Regulační zařízení topení","Regulačná jednotka ohrevu","Regulator ogrzewania","Fűtésszabályozó készülék","Lämmityksen säätölaite","Varmestyringsmodul"]
["Remote set value selector","Sollwertfernversteller","Remote set value selector","Commande à distance de la consigne","Centralina remota","Grenswaardeverstelling","Dálková regulace požadovaných hodnot","Diaľkový regulátor požadovanej hodnoty","Zdalny nastawnik wartości zadanej","Alapjel távirányító","Ohjearvon kaukoasetin","Sætpuntsvælger"]
["Temperature sensor: Outside temperature","Außentemperaturfühler separates Heizungsregelgerät","Temperature sensor: Outside temperature","Sonde température extérieure","Sensore di temperatura: Temperatura Esterna","Buitentemperatuurvoeler","Snímač venkovní teploty","Snímač vonkajšej teploty","Czujnik temperatury zewnętrznej","Külső hőmérséklet-érzékelő","Ulkolämpötila-anturi","Temperatursensor: Udetemperatur"]
["Temperature sensor: Flow temperature","Vorlauftemperaturfühler separates Heizungsregelgerät","Temperature sensor: Flow temperature","Sonde température départ","Sensore di temperatura: Temperatura di Mandata","Aanvoertemperatuurvoeler","Snímač přívodní teploty","Snímač prívodnej teploty","Czujnik temperatury zasilania","Előremenő ági hőmérséklet-érzékelő","Menovirtauksen lämpötila-anturi","Temperatursensor: Fremløbstemperatur"]
["Air vent valve","Entlüftung","Air vent valve","Purge ","Valvola sfogo aria","Ontluchting","Odvzdušnění","Odvzdušnenie","Odpowietrzanie","Szellőztetés","Ilmausventtiili","Udluftningsventil"]
["Solid fuel boiler","Feststoffkessel mit thermischer Ablaufsicherung","Solid fuel boiler","Chaudière bois / coke avec sécurité thermique","Bollitore a combustibile solido","Houtkachel met thermostatische begrenzing","Kotel na tuhá paliva s tepelnou pojistkou","Kotol na tuhé palivo s tepelnou odtokovou poistkou","Kocioł paliwa stałego z termicznym bezpiecznikiem odpływu","Szilárd tüzelésű kazán termikus biztonsági szeleppel","Kiinteän polttoaineen kattilan terminen poistoventtiili","Fastbrændselskedel med termisk udløbssikring"]
["Motorised valve / Solenoid valve","Motorventil / Magnetventil","Motorised valve / Solenoid valve","Electrovanne / vanne magnétique","Motore Valvola/solenoide","Mengventiel / Magneetventiel","Motorový ventil / magnetický ventil","Motorový/magnetický ventil","Zawór silnikowy / zawór elektromagnetyczny","Motoros szelep / Mágnesszelep","Moottori-/magneettiventtiili","Motorventil / magnetventil"]
["Diverter valve","Umsteuerventil","Diverter valve","Vanne d'inversion","Valvola deviatrice","Omschakelventiel","Přepínací ventil","Vratný ventil","Zawór sterujący","Irányváltó szelep","Suunnanvaihtoventtiili","Skifteventil"]
["Threaded immersion heater","Einschraubheizkörper","Threaded immersion heater","Corps de chauffe à visser","Resistenze elettriche supplementari attacco filettato","Inschroef verwarmingselement","Šroubovací topné těleso","Závitové vykurovacie teleso","Grzałka wkręcana","Becsavarható fűtőtest","Sähkövastus","Indskrueningsvarmelegeme"]
["Heat exchanger","Wärmeaustauscher","Heat exchanger","Echangeur","Scambiatore di calore","Warmtewisselaar","Výměník tepla","Tepelný výmenník","Wymiennik ciepła","Hőcserélő","Lämmönsiirrin","Varmeveksler"]
["Combi cylinder","Kombispeicher","Combi cylinder","Ballon combiné","Accumulo Combi","Combi boiler","Kombinovaný zásobník","Kombinovaný zásobník","Zasobnik kombinowany","Kombi melegvíztároló","Yhdistelmävaraaja","Kombibeholder"]
["DHW cylinder","Warmwasserspeicher","DHW cylinder","Ballon ECS","Accumulo ACS","Warmwaterboiler","Zásobník teplé vody","Zásobník teplej vody","Zasobnik ciepłej wody","Melegvíztároló","Käyttövesivaraaja","VV-beholder"]
["Central control thermostat","Zentralthermostat","Central control thermostat","Thermostat centralisé","Termostato centralizzato","Centraal thermostaat","Centrální termostat","Centrálny termostat","Centralny termostat","Központi termosztát","Keskustermostaatti","Centraltermostat"]
["Cold water - safety equipment assembly","Kaltwasser-Sicherheitsgruppe nach DIN 1988","Cold water - safety equipment assembly","groupe de sécurité eau froide","Gruppo di sicurezza carico acqua","Koudwater veiligheidsgroep","Bezpečnostní skupina pro studenou vodu podle DN 1988","Studená voda-poistné skupinové zariadenie podľa DIN 1988","Zespół ochronny do zimnej wody wg DIN 1988","DIN 1988 szabványnak megfelelő hidegvizes biztonsági szivattyú","Kylmän veden varolaiteryhmä, SFS 1988:n mukainen","Koldtvand - sikkerhedsgruppe"]
["Controller: Swimming pool water","Temperaturregler für Schwimmbadwasser","Controller: Swimming pool water","régulateur de température eau piscine","Termoregolatore per riscaldamento piscina","Temperatuurregelaar voor zwembad","Regulátor teploty pro vodu v bazénu","Regulátor teploty pre vodu bazéna","Regulator temperatury wody basenowej","Medencevíz hőfokszabályozó","Lämpötilansäädin uima-allasvedelle","Styring: Swimmingpoolvand"]
["Control thermostat","Elektronischer Temperaturregler","Control thermostat","thermostat électronique","Termostato","Elektronische temparatuurregelaar","Elektronický regulátor teploty","Elektronický regulátor teploty","Elektroniczny regulator temperatury","Elektronikus hőfokszabályozó","Elektroninen lämpötilansäädin","Elektronisk temperaturstyring"]
["Overflow valve","Überströmventil","Overflow valve","vanne de décharge / by-pass","Valvola di Compensazione","Overstortventiel","Přepouštěcí ventil","Prepúšťací ventil","Zawór przelewowy","Túlfolyószelep","Ylivirtausventtiili","Overstrømsventil"]
["cap valve","Absperrschieber - gegen unbeabsichtigtes Schließen sichern","cap valve","vanne d'arrêt - à protéger contre une fermeture involontaire","Valvola chiusura di servizio","Vergrendelbare afsluiter","Zajistěte uzavírací klapku proti manipulaci nepovolanými osobami","Posuvný uzáver - zaistenie proti neúmyselnému zatvoreniu","Zasuwa odcinająca – zabezpieczyć przed przypadkowym zamknięciem","Tolózár - véletlen zárás ellen biztosítani kell","Luistiventtiili – varmista tahatonta sulkemista vastaan","Afspærringsventil - sikret mod utilsigtet lukning"]
["Line regulating valve","Strangregulierventil","Line regulating valve","vanne limitatrice de débit","Regolatore di portata ","Strangventiel","Ventil regulace větve","Regulačný ventil vetvy","Zawór regulacyjny przewodu","Strangszabályozó szelep","Linjansäätöventtiili","Strengreguleringsventil"]
["Temperature differential controller","Temperatur-Differenzregelung / Solarregelung","Temperature differential controller","régulation différentielle de température / régulation solaire","Regolatore differenziale di temperatura ","Temperatuur verschilmeter / Regelunit solar","Regulace na základě rozdílu teplot / regulační zařízení Solar","Regulácia teplotného rozdielu/Regulačná jednotka Solárny kolektor","Regulator temperatury różnicowej / regulator Solar","Hőmérsékletkülönbség-szabályozás / Szolár szabályozó","Lämpötilaeron säädin / säätölaite aurinkolämpöjärjestelmään","Differenstemperatursstyring / Solfangerstyring"]
["Flow limiter","Strömungswächter","Flow limiter","contrôleur de débit","Misuratore di portata","Stromingsschakelaar","Kontrola průtoku","Obmedzovač prietoku","Przepływomierz","Áramlásőr","Virtausvahti","Flowbegrænser"]
["High limit thermostat - underfloor heating system ","Schutztemperaturregler-Fußbodenheizung","High limit thermostat - underfloor heating system ","Thermostat de sécurité pour plancher chauffant","Temostato di sicurezza riscaldamento a pavimento","Temperatuurbegrenzer vloerverwarming","Bezpečnostní regulátor teploty podlahového topení","Ochranný regulátor teploty-podlahové vykurovanie","Regulator temperatury ochronnej ogrzewania podłogowego","Biztonsági hőmérséklet-szabályozó - padlófűtés","Lattialämmitys lämpötilan turvasäätimen kera","Termostatafbryder - gulvarmebeskyttelse"]
["Zone valve","Zonenventil","Zone valve","vanne de zone","Valvola di Zona","Zone ventiel","Zónový ventil","Zónový ventil","Zawór strefowy","Zónaszelep","Alueventtiili","Zoneventil"]
["Inflow tube","Einströmrohr","Inflow tube","conduite d'admission","Tubo di immissione","Instroombuis","Vstupní potrubí","Vtoková rúra","Rura napływowa","Befolyócső","Tuloputki","Indløbsrør"]
["Filter / strainer","Schmutzfilter","Filter / strainer","filtre à tamis","Filtro/colino","Vuilvanger","Filtr na nečistoty","Filter nečistôt","Filtr zanieczyszczeń","Szennyszűrő","Likasuodatin","Snavssamler"]
["Fancoil ","Gebläsekonvektor","Fancoil ","ventilo-convecteur","Fancoil","Ventilator convector","Konvektor s ventilátorem","Konvektor s ventilátorom","Konwektor nadmuchowy","Klímakonvektor","Puhallinkonvektori","Blæsekonvektor"]
["Instantaneous water heater DHE","Durchlauferhitzer, vollelektronisch geregelter DHE","Instantaneous water heater DHE","chauffe-eau électrique instantané DHE","Boiler elettrico insantaneo ACS","Doorstromer DHE","Průtokový ohřívač DHE","Prietokový ohrievač DHE","Ogrzewacz przepływowy DHE","Átfolyós vízmelegítő DHE","Läpivirtauslämmitin DHE","Gennemstrømningsvandvarmer DHE"]
["Solar panel","Solarkollektor","Solar panel","Panneau solaire thermique  ","Collettrore solare","Solar collector","Solární kolektor","Solárny kolektor","Kolektor solarny","Napkollektor","Aurinkokeräin","Solfanger"]
["Electrical heating flang","Elektroheizflansch","Electrical heating flang","corps de chauffe électrique / bride électrique","Falangia Resistenza elettrica supplementare","Elektrisch verwarmingselement","Elektrická topná příruba","Elektrická vykurovacia príruba","Elektryczny kołnierz grzejny","Elektromos fűtőbetét","Sähkövastus","Elektrisk varmelegeme, flange"]
["Heat utilisation system","Wärmenutzungsanlage","Heat utilisation system","installation de chauffage/émetteurs de chaleur","Lato Utilizzi","Warmte installatie","Zařízení na využití tepla","Zariadenie využívajúce teplo","Instalacja wykorzystująca ciepło","Hőhasznosító berendezés","Lämmönkäyttölaitteisto","Varmeudnyttelsessystem"]
["Heat source system ","Wärmequellenanlage","Heat source system ","installation source de chaleur / circuit primaire ","Lato Sorgente","Bron installatie","Zařízení s tepelným zdrojem","Zariadenie zdroja tepla","System dolnego źródła","Hőforrás berendezés","Lämmönlähdelaitteisto","Varmekildesystem"]
["Solar panel","Solarkollektoren","Solar panel","panneaux solaires thermiques ","Collettrore solare","Solar collector","Solární kolektory","Solárne kolektory","Kolektory solarne","Napkollektorok","Aurinkokeräimet","Solfanger"]
["Cooling system","Kühlanlage","Cooling system","installation de rafraîchissement","Sistema di raffrescamento","Koel installatie","Chladicí zařízení","Chladiace zariadenie","Instalacja chłodnicza","Hűtőberendezés","Jäähdytyslaitteisto","Køling"]
["Radiator heating system ","Heizkörperheizung","Radiator heating system ","chauffage par radiateurs","Sitema riscaldamento a radiatori","Radiator verwarming","Ohřev topného tělesa","Ohrev vykurovacími telesami","Ogrzewanie grzejnikowe","Fűtőtestes fűtés","Patterilämmitys","Radiator"]
["Underfloor heating system","Flächenheizung","Underfloor heating system","chauffage au sol","Sistema riscaldamento a pavimento","Vloer / wandverwarming","Plošné topení","Povrchové vykurovanie","Ogrzewanie powierzchniowe","Falfűtés","Pintalämmitys","Gulvvarme"]
["DHW","Warmwasser","DHW","Eau Chaude Sanitaire","ACS","Warmwater","Teplá voda","Teplá voda","Ciepła woda","Melegvíz","Lämmin käyttövesi","Varmtvand"]
["Swimming pool water ","Schwimmbadwasser","Swimming pool water ","eau de piscine","Acqua Piscina","Zwembadwater","Voda v bazénu","Voda bazéna","Woda basenowa","Medencevíz","Uima-allasvesi","Swimmingpoolvand"]
[]
["Expansion vessel","Ausdehnungsgefäß","Expansion vessel","Vase d'expansion","Vaso di espansione","Expansievat","Expanzní nádrž","Expanzná nádrž","Naczynie wzbiorcze","Tágulási tartály","Paisuntasäiliö","Ekspansionsbeholder"]
["Components solar system","Anlagenkomponenten","Components solar system","Eléments du systèmes","Componenti del sistema","Systeemcomponenten","Součásti zařízení","Súčasti systému","Komponenty systemu","Rendszer elemek","Aurinkokeräinjärjestelmän komponentit","Anlægskomponenter"]
["Collector","Kollektor","Collector","Capteur","Collettore","Collector","Kolektor","Kolektor","Kolektor","Kollektor","Keräintiedot","Panel"]
["DHW cylinder","Warmwasserspeicher","DHW cylinder","Ballon ECS","Serbatoio tampone acqua calda","Warmwaterboiler","Zásobník teplé vody","Zásobník teplej vody","Zasobnik ciepłej wody","keringető szivattyúja","Käyttövesivaraaja","VV-beholder"]
["Buffer cylinder","Pufferspeicher","Buffer cylinder","Ballon de stockage","Serbatoio tampone","Buffervat","Akumulační nádrž","Akumulačná nádrž","Zbiornik buforowy","Puffertároló","Puskurivaraaja","Bufferbeholder"]
["Heat exchanger","Wärmetauscher","Heat exchanger","Échangeur de chaleur","Scambiatore di calore","Warmtewisselaar","Výměník","Výmenník tepla","Wymiennik ciepła","Hőcserélő","Lämmönvaihdin","Varmeveksler"]
["Flexible solar pipe","Solar-Flexrohr","Flexible solar pipe","Tube flexible solaire","Tubo flessibile solare","Flexibele solarbuis","Solár.flexibilní trubka"," Solárna flexibilná rúra","Giętka rura solarna","Szolár flexcső","Joustava aurinkokeräinputki","Fleksibelt solfangerrør"]
["Copper pipe 18 x 1.0","CU-Rohr 18 x 1,0","Copper pipe 18 x 1.0","Tube en cuivre 18 x 1,0","Tubo di rame 18 x 1,0","Totale pijplengte CU 18 x 1.0","Cu-trubky 18 x 1,0","Cu- rúra 18 x 1,0","Rury miedzianej 18 x 1,0","18 x 1,0 rézcső teljes hossza","Kupariputki 18 x 1.0","Kobber rør 18 x 1,0"]
["Copper pipe 22 x 1.0","CU-Rohr 22 x 1,0","Copper pipe 22 x 1.0","Tube en cuivre 22 x 1,0","Tubo di rame 22 x 1,0","Totale pijplengte CU 22 x 1.0","Cu-trubky 22 x 1,0","Cu- rúra 22 x 1,0","Rury miedzianej 22 x 1,0","22 x 1,0 rézcső teljes hossza","Kupariputki 22 x 1.0","Kobber rør 22 x 1,0"]
["Copper pipe 28 x 1.5","CU-Rohr 28 x 1,5","Copper pipe 28 x 1.5","Tube en cuivre 28 x 1,5","Tubo di rame 28 x 1,5","Totale pijplengte CU 28 x 1.5","Cu-trubky 28 x 1,5","Cu- rúra 28 x 1,5","Rury miedzianej 28 x 1,5","28 x 1,5 rézcső teljes hossza","Kupariputki 28 x 1.5","Kobber rør 28 x 1,5"]
["Copper pipe 35 x 1.5","CU-Rohr 35 x 1,5","Copper pipe 35 x 1.5","Tube en cuivre 35 x 1,5","Tubo di rame 35 x 1,5","Totale pijplengte CU 35 x 1.5","Cu-trubky 35 x 1,5","Cu- rúra 35 x 1,5","Rury miedzianej 35 x 1,5","35 x 1,5 rézcső teljes hossza","Kupariputki 35 x 1.5","Kobber rør 35 x 1,5"]
["Other installations","Sonstige Einbauten","Other installations","Autres bâtiments ","Volumi di altri componenti aggiunti","Volume van andere installaties","Objem jiných použitých prvků","Iné zariadenia","Pojemność pozostałych instalacji","Egyéb felépítmény térfogata","Muu tilavuus","Armaturer og fittings"]
["Get components from material list","Komponenten aus Materialliste","Get components from material list","Eléments de la liste de matériel","Componenti della lista del materiale","Componenten uit de materiaallijst","Součásti z výpisu materiálu","Komponenty zo súpisu materiálu","Komponenty z listy materiałowej","Elemek az anyaglistából","Hae komponentit osaluettelosta","Komponenter fra styklisten"]
["Expansion volume","Ausdehnungsvolumen","Expansion volume","Volume d'expansion","Volume espansione","Uitzettingsvolume","Objem rozpínání","Objem rozpínania","Objętość rozszerzenia","Tágulási térfogat","Laajenemistilavuus","Ekspansionsvolumen"]
["Litres","Liter","Litres","litre","litri","Liter","Litr","Liter","l","liter","litraa","Liter"]
["Pressure factor","Druckfaktor","Pressure factor","Facteur de pression","Fattore di pressione","Drukfactor","Tlakový faktor","Tlakový faktor","Współczynnik ciśnienia","Nyomástényező","Painekerroin","Trykfaktor"]
["Minimum size","Mindestgröße","Minimum size","Taille minimale","Dimensione minima","Minimale grootte","Min.velikost","Min. veľkosť","Wielkość minimalna","Minimális méret","Minimitilavuus","Minimum størrelse"]
["on site","bauseits","on site","à la charge du client","in loco","Montage","V rámci montáže","V rámci montáže","od strony konstrukcji","helyszíni","kohteessa","på stedet"]
["Recommendation","Empfehlung","Recommendation","Recommandation ","Suggerimento liquido termovettore","Aanbeveling","Doporučení teplonosné kapaliny","Odporúčanie","Zalecenie dotyczące cieczy przenoszącej ciepło","Ajánlott hőhordozó folyadék","Suositus","Anbefaling"]
["Heat transfer medium","Wärmeträgerflüssigkeit","Heat transfer medium","Fluide caloporteur","Termovettore - liquido","Warmtedragervloeistof","Nemrznoucí kapalina","Vyhrievacie médium","Ciecz przenosząca ciepło","Hőhordozó folyadék","Lämmönsiirtoaine","Varmeoverførselsvæske"]
["System volume","Anlagenvolumen","System volume","Volume de l'installation","Volumi impianto","Systeemvolume","Objem zařízení","Objem zariadenia","Pojemność instalacji","Rendszer térfogata","Järjestelmän tilavuus","Anlægsvolumen"]
["Liquid seal (min. 3 l)","Flüssigkeitsvorlage (min. 3l)","Liquid seal (min. 3 l)","Collecteur de fluide (min. 3 l)","Riserva liquido (Min. 3 l)","Vloeistofinhoud (min. 3 l)","Sběrač kapaliny (min. 3 l)","Zachytávač kvapaliny (min. 3 l)","Zbiornik na ciecz (min. 3 l)","Folyadéktartály (Min. 3 l)","Nestelukko (min. 3 l)","Liquid seal (min. 3 l)"]
["Total volume","Benötige Menge","Total volume","Volume total","Volume complessivo","Totaal volume","Celkový objem","Celkový objem","Pojemność całkowita","Össztérfogat","Kokonaistilavuus","Samlet volumen"]
["Applicable for up to 20 m height differential (collector - DEV), safety valve response pressure 6 bar","Gültig für max. 20 m Höhenunterschied (Kollektor - MAG), Ansprechdruck Sicherheitsventil 6 bar","Applicable for up to 20 m height differential (collector - DEV), safety valve response pressure 6 bar","Valable pour une différence de hauteur de 20 m max. (capteur - MAG), pression de tarage vanne de sécurité 6 bars","Valido per dislivello max. 20 m (collettore - MAG), Pressione di sollecitazione valvola di sicurezza 6 bar","Toepasbaar tot maximaal 20 m. hoogte verschil (collector - MAG), aanspreekdruk veiligheidsventiel 6 bar","Platné pro výškový rozdíl (kolektor-expanz.nádrž) max. 20 m, vybavovací tlak poj.ventilu 6 bar","Platné pre výškový rozdiel (kolektor-expanz.nádrž) max. 20 m, reakčný tlak poistného ventilu 6 bar","Dotyczy różnicy wysokości maks. 20 m (kolektor – MAG), ciśnienie zadziałania zaworu bezpieczeństwa 6 barów","Érvényes max. 20 m magasságkülönbségre (kollektor - MAG), biztonsági szelep nyitási nyomása 6 bar","Soveltuva 20 m korkeuseroihin (keräin - paisuntasäiliö), varoventtiilin paine 6 baria","Gælder for maks. 20 m højdeforskel (solfanger - ekspansionsbeholder), sikkerhedsventil til 6 bar"]
[]
["Printout","Ausdruck","Printout","Impression","Stampa","Afdruk ","Tisk","Tlač","Drukuj","Nyomtatás ","Tulostus","Udskrift"]
["Select printout","Druckauswahl","Select printout","Sélection d'impression","Stampa la selezione","Printen","Volba tlaku","Voľba tlače","Wybór  wydruku","Nyomtató kiválasztás","Valitse tuloste","Vælg udskrift"]
["Project","Projektdaten","Project","Projet","Dati del progetto","Projectdata","Data projektu","Dáta projektu","Dane projektu","Projekt adatok","Projektitiedot","Projekt data"]
["Description solar system","Anlagenbeschreibung","Description solar system","Description de l'installation","Descrizione dell'impianto","Systeembeschrijving","Popis soustavy","Popis systému","Opis systemu","Rendszer leírás","Aurinkojärjestelmän kokoonpano","Systembeskrivelse"]
["Type of utilisation","Nutzungsart","Type of utilisation","Type d'utilisation","Tipo utilizzo","Gebruikswijze","Druh využití","Spôsob využitia","Przeznaczenie","Hasznosítás jellege","Kohteen lämmitysjärjestelmä","Brug"]
["Material composition","Materialzusammenstellung","Material composition","Composition du matériel","Composizione materiali","Materiaal samenstelling","Specifikace materiálu","Špecifikácia materiálu","Wykaz materiałów","Anyagok összetétele","Osaluettelo","Materialeliste"]
["Hydraulic/wiring diagrams","Hydraulik-/Elektropläne","Hydraulic/wiring diagrams","Schémas hydrauliques/électriques","Schemi Idraulici/elettrici","Hydraulisch/bedradingsschema","Hydraulické/elektrické schéma","Hydraulické/ elektrické schémy","Schematy hydrauliczne/elektryczne","Hidraulikus/elektromos rajzok","LVI-/sähkökytkentäkaaviot","Hydraulisk- / elektrisktegning"]
["Pipework installation","Rohrinstallation","Pipework installation","Installation de la tuyauterie","Installazione tubazione","Leidinginstallatie","Instalace trubek","Inštalácia rúr","Instalacja rurowa","Csőtelepítés","Putkiasennuskuva","Rørinstallation"]
["Installation information","Hinweise zur Installation","Installation information","Remarques à propos de l'installation","Suggerimenti per l'installazione","Aanwijzingen voor installatie","Pokyny pro instalaci","Pokyny pre inštaláciu","Zasady instalacji","A telepítésre vonatkozó utasítások","Asennusinformaatio","Bemærkninger til installationen"]
["Select all","Alles auswählen","Select all","Sélectionner tout","Seleziona tutto","Alles selecteren","Vše zvolit","Vybrať všetko","Wybierz wszystko","Összes kiválasztása","Valitse kaikki","Vælg alle"]
["Print selection","Auswahl drucken","Print selection","Imprimer sélection","Stampa selezione","Selectie afdrukken","Volba tisku","Tlačiť","Drukuj wybór","Nyomtatás kiválasztása","Esikatselu","Udskriv afsnit"]
["Export printout","Ausdruck exportieren","Export printout","Exporter la sélection ","Export printout","Afdruk exporteren","Export printout","Export printout","Export printout","Export printout","Export printout","Eksporter udskrift"]
[]
["Design","Projektierung","Design","Etude","Progettazione","Ontwerp","Projektování","Projektovanie","Projekt","Kivetítés","Suunnittelu","Projektering"]
["Country","Land","Country","Pays","Campagna","Land","Stát","Štát","Kraj","Ország","Maa","Land"]
["City","Stadt","City","Ville","Città","Plaats","Město","Mesto","Miejscowość","Város","Kaupunki","By"]
["Volume","Volumen","Volume","Volume","Volume","Volume","Objem","Objem","Pojemność","Térfogat","Tilavuus","Volumen"]
["Total area","Gesamtfläche","Total area","Surface totale","Superficie complessiva","Totaal oppervlak","Celková plocha","Celková plocha","Powierzchnia całkowita","Összfelület","Kokonaispinta-ala","Samlet areal"]
["Location","Standort","Location","Site","Luogo","Plaats","Umístění","Umiestnenie","Lokalizacja","Helyszín","Sijainti","Placering"]
["Insolation, collector area","Einstrahlung Kollektorfläche","Insolation, collector area","Rayonnement surface de capteurs","Irradiazione superficie collettore","Instraling collectoroppervlak","Solární zisk kolektoru","Solárny zisk kolektora","Napromieniowanie powierzchni kolektorów","Kollektorfelület besugárzása","Auringonsäteily keräinpinta-alalle","Solindtråling, solfangere"]
["Calculation","Berechnung","Calculation","Calcul","Calcolo","Berekening","Výpočet","Výpočet","Obliczenia","Számítás","Laskelmat","Beregning"]
["Total volume","Gesamtvolumen","Total volume","Volume total","Volume complessivo","Totaal volume","Celkový objem","Celkový objem","Pojemność całkowita","Össztérfogat","Kokonaistilavuus","Samlet volumen"]
["Heat transfer medium expansion","Ausdehnung Wärmeträger","Heat transfer medium expansion","Expansion du fluide caloporteur","Espansione vettore termico","Uitzetting warmtedragervloeistof","Rozpínání teplonosné kapal.","Rozpínanie ohrievacieho média","Rozszerzenie nośnika ciepła","Hőhordozó közeg tágulása","Lämmönsiirtoaineen laajentuminen","Varmeoverførselsvæske ekspansion"]
["Volume evaporation","Volumen Verdampfung","Volume evaporation","Volume d'évaporation","Evaporazione volumi","Verdampingsvolume","Objem odpaření","Objem odparenia","Pojemność parowania","Elpárologtató térfogata","Haihtumistilavuus","Fordampningsvolumen"]
["Nominal volume, expansion vessel","Nennvolumen Ausdehnungsgefäß","Nominal volume, expansion vessel","Volume nominale vase d'expansion","Volume nominale vaso di espansione","Nominaal volume expansievat","Jmen.objem expanzní nádrže","Menovitý objem expanznej nádrže","Pojemność znamionowa naczynia wzbiorczego","Tágulási tartály névleges térfogata","Paisuntasäiliön perustilavuus","Nominel volumen, ekspansionsbeholder"]
["Pre-charge pressure, expansion vessel","Vordruck Ausdehnungsgefäß","Pre-charge pressure, expansion vessel","Vase d'expansion pression d'alimentation","Pressione di mandata vaso di espansione","Voordruk expansievat","Přetlak expanzní nádrže","Pretlak expanznej nádrže","Ciśnienie wstępne w naczyniu wzbiorczym","Tágulási tartály előnyomása","Paisuntasäiliön esipaine","Fortryk, ekspansionsbeholder"]
[]
[]
[]
[]
[]
["Legal note","Rechtliche Hinweise","Legal note","Clause de non-responsabilité","Avviso legale","Wettelijke instructie","Právní upozornění","Právne upozornenie","Pouczenie prawne","Jogi nyilatkozat","Oikeudellinen huomautus","Juridiske betingelser"]
["Stiebel Eltron shall not provide any guarantees that the information, values and data provided, or values, information and recommendations determined with the aid or on the basis of such information, values and data, are complete, accurate, correct or current in every respect.\nStiebel Eltron shall reserve the right to make changes to the data, values and information provided at any time and without prior notification.\nErrors excepted. Subject to changes.\nNone of the information, values and data provided or the values, information and recommendations determined with the aid or on the basis of such information, values and data constitutes any basis for a financial decision or for any other purpose, but rather is merely initial non-binding information as an initial guide.\nUnder no circumstances should the following design tool be considered a substitute for consultation with Stiebel Eltron or another authorised expert engineer.\nPlease contact Stiebel Eltron or another authorised expert engineer in relation to specific project design.\nStiebel Eltron shall accept no liability for losses of any kind that may arise from the use of information, values and data provided, or values, information and recommendations determined with the aid or on the basis of such information, values and data. This exclusion of liability shall not apply if the loss is due to intent or gross negligence on the part of Stiebel Eltron or in the event of a fatality, physical injury or damage to health.\n","Stiebel Eltron übernimmt keinerlei Gewährleistung oder Garantie dafür, dass die bereitgestellten Angaben, Werte und Informationen oder die mit Hilfe bzw. anhand dieser Informationen, Werte und Angaben ermittelten Werte und Angaben in jeder Hinsicht vollständig, genau, richtig und aktuell sind. \n\nStiebel Eltron behält sich das Recht vor, jederzeit und ohne vorherige Ankündigung Änderungen der bereitgestellten Angaben, Werte und Informationen vorzunehmen.\nIrrtum und Änderungen sind ausdrücklich vorbehalten.\nKeine der bereitgestellten Angaben, Werte und Informationen oder der mit Hilfe bzw. anhand dieser Angaben, Werte und Informationen ermittelten Werte und Angaben sind als Grundlage für eine finanzielle Entscheidung oder für einen sonstigen Zweck anzusehen, sondern dienen vielmehr nur als eine erste unverbindliche Information und als Hilfe zur ersten Orientierung.\n\nUnter keinen Umständen ersetzt die Planungshilfe die Beratung durch Stiebel Eltron oder einen autorisierten Fachplaner.\n\nBitte wenden Sie sich für die konkrete Planung des Projektes an Stiebel Eltron oder einen anderen autorisierten Fachplaner.\n\nDie Haftung von Stiebel Eltron für Schäden jeglicher Art, die sich möglicherweise aus der Nutzung oder Verwendung der bereitgestellten Informationen, Werte und Angaben oder der mit Hilfe bzw. anhand dieser Angaben, Werte und Informationen ermittelten Werte und Angaben, ergeben, ist ausgeschlossen. Dieser Haftungsausschluss gilt nicht, wenn der Schaden auf Vorsatz oder grobe Fahrlässigkeit von Stiebel Eltron zurückzuführen ist sowie bei einer Verletzung des Lebens, des Körpers oder der Gesundheit.\n","Stiebel Eltron shall not provide any guarantees that the information, values and data provided, or values, information and recommendations determined with the aid or on the basis of such information, values and data, are complete, accurate, correct or current in every respect.\nStiebel Eltron shall reserve the right to make changes to the data, values and information provided at any time and without prior notification.\nErrors excepted. Subject to changes.\nNone of the information, values and data provided or the values, information and recommendations determined with the aid or on the basis of such information, values and data constitutes any basis for a financial decision or for any other purpose, but rather is merely initial non-binding information as an initial guide.\nUnder no circumstances should the following design tool be considered a substitute for consultation with Stiebel Eltron or another authorised expert engineer.\nPlease contact Stiebel Eltron or another authorised expert engineer in relation to specific project design.\nStiebel Eltron shall accept no liability for losses of any kind that may arise from the use of information, values and data provided, or values, information and recommendations determined with the aid or on the basis of such information, values and data. This exclusion of liability shall not apply if the loss is due to intent or gross negligence on the part of Stiebel Eltron or in the event of a fatality, physical injury or damage to health.\n","STIEBEL ELTRON ne se porte pas garant de l'exactitude, intégralité, actualité et pertinence des informations, valeurs ou données mises à disposition, ni de toute valeur, information ou recommandation établie à l'aide de ces données, valeurs et informations fournies.\nSTIEBEL ELTRON se réserve le droit de modifier, à tout moment et sans avis préalable, les données, valeurs et informations mises à disposition.\nSous réserve de modification et d'erreurs.\nLes informations, valeurs et données, ou les valeurs, informations et recommandations établies à l'aide de ces informations, valeurs et données, ne doivent être utilisées pour aucune prise de décision financière ou autre. Elles sont fournies à titre indicatif uniquement en ne représentent qu'une source approximative d'information.\nL'assistant de planification et les informations fournies ci-après ne remplacent en aucun cas le conseil direct d'un expert STIEBEL ELTRON ou de tout autre spécialiste autorisé.\nPour la planification concrète de votre projet, veuillez contacter STIEBEL ELTRON ou tout autre spécialiste autorisé.\nSTIEBEL ELTRON décline toute responsabilité pour les dommages éventuels découlant de l'utilisation ou du traitement des informations, valeurs et données mises à disposition, ou des valeurs, informations et recommandations établies à l'aide de ces informations, valeurs et données. Cette exclusion de garantie n'est pas valable en cas de dommage intentionnel découlant d'une négligence grave de la part de Stiebel Eltron, ni en cas d'atteinte à la vie, au corps ou à la santé des utilisateurs.\n","Stiebel Eltron non fornisce alcuna assicurazione o garanzia che le informazioni, valori o indicazioni o che i valori, informazioni e suggerimenti ottenuti con l'ausilio di queste informazioni, valori e indicazioni siano completi, esatti, corretti e aggiornati in ogni riguardo.\nStiebel Eltron si riserva il diritto di eseguire senza preavviso modifiche ai dati, valori e informazioni messi a disposizione.\nSono espressamente riservati errori e modifiche.\nNessuna delle informazioni, valori e indicazioni o dei valori, informazioni e suggerimenti ottenuti con l'ausilio di queste informazioni, valori e indicazioni siano utilizzati come presupposti per una decisione economica o per scopo simile, piuttosto sono molto più utili come prima informazione non vincolante e di aiuto in per un primo orientamento.\nIn nessun caso il seguente strumento di ausilio per la progettazione può sostituire la consulenza tramite Stiebel Eltron o un altro progettista specializzato autorizzato.\nPer la pianificazione effettiva del vostro progetto, rivolgetevi a Stiebel Eltron oppure ad un altro progettista specializzato autorizzato.\nÈ esclusa la responsabilità di Stiebel Eltron per qualsiasi tipo di danno possibilmente provocato dall'utilizzo o uso delle informazioni, valori e indicazioni messi a disposizione o dei valori, informazioni e suggerimenti ottenuti con l'ausilio di queste informazioni.  Questa clausola di esonero della responsabilità non è valida, quando i danni possono essere ricondotti a volontà colpevole o colpa grave di Stiebel Eltron nonché con una violazione della vita, del corpo e della salute.\n","Stiebel Eltron geeft geen enkele garantie dat de aangeboden informatie, waarden en gegevens of de met behulp van of aan de hand van deze informatie, waarden en gegevens berekende waarden, informatie en aanbevelingen in elk opzicht volledig, nauwkeurig, juist en actueel zijn. \n\nStiebel Eltron behoudt zich het recht voor om op elk moment zonder voorafgaande kennisgeving wijzigingen aan te brengen in de aangeboden gegevens, waarden en informatie.\nVergissingen en wijzigingen worden door Stiebel Eltron uitdrukkelijk voorbehouden.\nDe aangeboden informatie, waarden en gegevens of de met behulp van of aan de hand van deze informatie, waarden en gegevens berekende waarden, informatie en aanbevelingen betreffen een eerste Stiebel Eltron niet-bindende informatie voorziening die niet kan worden gebruikt als basis voor een financiële beslissing of voor andere doeleinden dan een eerste oriëntatie. \n\nDeze planningshulp kan in geen geval dienen als vervanging voor het persoonlijke advies van Stiebel Eltron of een andere geautoriseerde systeemadviseur. \n\nVoor de concrete planning van uw project dient u zich te allen tijde te wenden tot Stiebel Eltron of een andere geautoriseerde systeemadviseur. \n\nStiebel Eltron aanvaardt op geen enkele wijze aansprakelijkheid voor schade en/of ander nadeel, direct dan wel indirect, die voortvloeit uit het gebruik of de toepassing van de aangeboden informatie, waarden en gegevens of de met behulp van of aan de hand van deze informatie, waarden en gegevens van berekende waarden, informatie en aanbevelingen. De hierboven omschreven uitsluitingen gelden niet in geval van grove nalatigheid, opzet of schade aan leven, lichaam of gezondheid.\n\n","Firma Stiebel Eltron nepřebírá v žádném případě ručení nebo záruku za to, že jsou poskytnuté informace, hodnoty a údaje nebo s pomocí, resp. podle těchto informací, hodnot a údajů určené hodnoty, informace a doporučení z každého hlediska úplné, přesné, správné a aktuální.\nFirma Stiebel Eltron si vyhrazuje právo provést kdykoliv a bez předchozího upozornění změny údajů, hodnot a informací.\nOmyly a změny jsou výslovně vyhrazeny.\nŽádné z poskytnutých informací, hodnot a údajů nebo s pomocí, resp. podle těchto informací, hodnot a údajů určené hodnoty, informace a doporučení nelze považovat za podklad pro finanční rozhodnutí nebo pro jiný účel, nýbrž slouží spíše jen jako první nezávazná informace a jako pomůcka k první orientaci.\nNásledující pomůcka k projektování nenahrazuje za žádných okolností poradu s firmou Stiebel Eltron nebo s jiným autorizovaným odborným projektantem.\nPro konkrétní návrh projektu se prosím obraťte na firmu Stiebel Eltron nebo na jiného autorizovaného odborného projektanta.\nRučení firmy Stiebel Eltron za škody jakéhokoliv druhu, které případně vyplynou z využití nebo použití informací, hodnot a údajů nebo hodnot, informací a doporučení, určených s pomocí, resp. podle těchto informací, hodnot a údajů, je vyloučené. Toto vyloučení záruky neplatí, jestliže souvisí škody se záměrem nebo hrubou nedbalostí firmy Stiebel Eltron a při ohrožení života, těla nebo zdraví.\n","Spoločnosť Stiebel Eltron nezaručuje úplnosť, presnosť, správnosť a aktuálnosť poskytnutých informácií, hodnôt a údajov, alebo hodnôt, informácií a odporúčaní, ktoré boli sprostredkované na základe týchto informácií, hodnôt a údajov.\nSpoločnosť Stiebel Eltron si vyhradzuje právo na zmenu poskytnutých údajov, hodnôt a informácií, kedykoľvek a bez predchádzajúceho upozornenie.\nChyby a zmeny sú vyhradené.\nŽiadne z poskytnutých informácií, hodnôt a údajov, alebo hodnôt, informácií a odporúčaní, ktoré boli sprostredkované pomocou, resp. na základe týchto informácií, hodnôt a údajov, nesmú byť použité ako základ pri finančných alebo iných rozhodnutiach. Predstavujú skôr prvotnú nezáväznú informáciu a pomôcku na prvé zorientovanie.\nV žiadnom prípade nasledujúca pomoc pri plánovaní nenahrádza poradenské služby spoločnosti Stiebel Eltron, alebo inej autorizovanej odbornej firmy na plánovanie.\nPre konkrétne naplánovanie projektu sa, prosím, obráťte na spoločnosť Stiebel Eltron, alebo inú autorizovanú odbornú firmu na plánovanie.\nZáruka spoločnosti Stiebel Eltron sa nevzťahuje na akékoľvek škody, ktoré vznikli v dôsledku použitia a aplikácie poskytnutých informácií, hodnôt a údajov, alebo hodnôt, informácií a odporúčaní, ktoré boli sprostredkované pomocou, resp. na základe týchto informácií, hodnôt a údajov. Toto vylúčenie záruky neplatí, ak škoda bola spôsobená úmyselne alebo z hrubej nedbanlivosti zo strany spoločnosti Stiebel Eltron, ako aj pri ohrození života, poranení alebo poškodení zdravia.\n","Stiebel Eltron nie udziela żadnej rękojmi czy gwarancji na to, że udostępnione informacje, wartości i dane lub ustalone za pomocą wzgl. na podstawie tych informacji, wartości i danych – wartości, informacje i zalecenia – pod każdym względem będą kompletne, dokładne, prawidłowe i aktualne.  \nStiebel Eltron zastrzega sobie prawo do dokonywania zmian udostępnionych danych, wartości i informacji w każdym momencie i bez wcześniejszej zapowiedzi. \nZastrzegamy sobie stanowczo prawo do pomyłki i zmian. \nŻadna z udostępnionych informacji, wartości i danych czy ustalonych za pomocą wzgl. na podstawie tych informacji, wartości, danych – wartości, informacji i zaleceń nie stanowi podstawy dla decyzji finansowych czy też innego celu, lecz służy raczej jedynie jako informacja niewiążąca i pomocnicza do wstępnej orientacji. \n\nW żadnym wypadku poniższa pomoc koncepcyjna nie zastąpi doradztwa ze strony Stiebel Eltron lub innego autoryzowanego specjalisty-projektanta. \nW celu zaprojektowania konkretnego projektu prosimy zwracać się do firmy Stiebel Eltron lub do innego autoryzowanego specjalisty-projektanta. \nWyłącza się odpowiedzialność cywilną Stiebel Eltron za szkody wszelkiego rodzaju, które mogą wynikać z użytkowania lub stosowania udostępnionych informacji, wartości i danych lub z ustalonych za pomocą względnie na podstawie tych informacji, wartości i danych – wartości, informacji i zaleceń. Niniejsze wyłączenie odpowiedzialności cywilnej nie będzie obowiązywać, jeśli za przyczynę szkody uznane zostanie umyślne lub poważne zaniedbanie ze strony Stiebel Eltron, a także w przypadku zagrożenia życia, uszkodzenia ciała lub zdrowia.  \n","A Stiebel Eltron nem vállal jótállást, vagy garanciát azért, hogy a rendelkezésre álló információk, értékek és adatok vagy az ezek felhasználásával számított adatok minden tekintetben teljes körű, pontos, korrekt és aktuális értékek.\nA Stiebel Eltron fenntartja magának a jogot, hogy bármikor, előzetes értesítés nélkül ezeket az adatokat, értékeket és információkat megváltoztathassa.\nA Stiebel Eltron a tévedés és a módosítás jogát is nyomatékosan fenntartja.\nA használt információk, értékek és adatok vagy az ezek felhasználásával számított adatok nem pénzügyi döntések vagy egyéb hasonló döntések alapjául szolgáló adatok, hanem csak lényegesen több mint egy kezdeti, nem kötelező erejű információt és támogatást biztosító, első tájékozódásként szolgáló anyag.\nEz az alábbi tervezési segédlet semmilyen körülmények között nem helyettesíti a Stiebel Eltron vagy más engedéllyel rendelkező tervezők tervezési tanácsadását.\nKérjük, forduljon a konkrét tervezés ügyében a Stiebel Eltronhoz vagy más engedélyezett tervezőhöz.\nA Stiebel Eltron bármilyen felelőssége a kárért, amely a program használatából származó, vagy használatára vonatkozó adatok, információk vagy értékek, illetve az ezekből számított adatok, információk vagy értékek miatt következett be, nem érvényesíthető. Ez a nyilatkozat nem vonatkozik arra az esetre, ha a kár a Stiebel Eltron szándékosságára vagy súlyos gondatlanságára vezethető vissza, valamint a sérülések és egészségkárosodások esetére sem.","Stiebel Eltron ei takaa, että julkaistut tiedot ja arvot tai niiden avulla aikaansaadut tiedot tai arvot ovat joka suhteessa tarkkoja, oikeellisia ja ajantasaisia.\nStiebel Eltron pidättää itsellään oikeuden muuttaa julkaistuja tietoja ja arvoja ilman ennakkoilmoitusta.\nValmistaja ei vastaa mahdollisista virheistä tai muutoksista.\nMitään julkaistuja arvoja tai niiden pohjalta aikaansaatuja arvoja, tietoja tai suosituksia ei tule käyttää perustana taloudellisille päätöksille tai muuhun vastaavaan tarkoitukseen. Tiedot on tarkoitettu vain  ensikäden ei-sitovaksi tietomateriaaliksi ja alkuvaiheen opastukseksi.\nTämä suunnitteluapu ei missään tapauksessa korvaa Stiebel Eltronin tai muun valtuutetun ammattisuunnittelijan tarjoamaa neuvontapalvelua.\nKehotamme asiakasta konkreettisissa suunnittelukysymyksissä kääntymään Stiebel Eltronin tai muun valtuutetun ammattisuunnittelijan puoleen.\nStiebel Eltron ei vastaa julkaistujen tietojen tai arvojen käytöstä tai näiden tietojen nojalla aikaansaaduista arvoista, tiedoista ja suosituksista mahdollisesti aiheutuneista vahingoista. Tämä vastuuvapauslauseke ei päde, mikäli vahinko johtuu Stiebel Eltronin tarkoituksellisesta teosta tai karkeasta huolimattomuudesta tai mikäli seurauksena on ollut hengen, ruumiin tai terveyden loukkaus.\n","Stiebel Eltron giver ingen garantier for, at de oplysninger, værdier og data,  information og anbefalinger der defineres ved hjælp af eller på grundlag af disse oplysninger, værdier og data, er fuldstændige, nøjagtige, korrekte eller anvendelige i enhver henseende.\nStiebel Eltron forbeholder sig ret til at foretage ændringer i data, værdier og oplysninger, til en hver tid og uden forudgående varsel. \nDer tages forbehold for fejl og ændringer.\nIngen af de oplysninger, værdier og data der forudsættes, eller værdier, oplysninger og anbefalinger der bestemmes ved hjælp af eller på grundlag af disse oplysninger, værdier og data, bør danne grundlag for økonomiske beslutninger eller til andre formål.  Dette må snarere betragtes som en indledende ikke-bindende information, der kan benyttes som en indledende vejledning. \nUnder ingen omstændigheder må følgende designværktøj betragtes som en erstatning for konsultation med Stiebel Eltron eller anden autoriseres ekspertteknikker.\nKontakt venligst Stiebel Eltron eller anden autoriseret ekspertteknikker, i forhold til det konkrete projektdesign.\nStiebel Eltron påtager sig intet ansvar for tab af nogen art, der måtte opstå som følge af brug af oplysninger, værdier og data der forudsættes eller værdier, oplysninger og anbefalinger bestemt ved hjælp af eller på grundlag af diss oplysninger, værdier og data.  Denne udelukkelse af ansvar gælder ikke, hvis tabet skyldes forsæt eller grov uagtsomhed fra Stiebel Eltrons side eller i tilfælde af en dødsulykke, fysisk skade eller skade på helbredet. "]
[]
[]
[]
[]
[]
[]
["Illustration","Darstellung","Illustration","Représentation","Descrizione","Illustratie","Zobrazení","Zobrazenie","Prezentacja","Ábrázolás","Kuva","Illustrering"]
["Specification","Technische Daten","Specification","Données techniques","Dati tecnici","Specificaties","Technické údaje","Technické údaje","Dane techniczne","Műszaki adatok","Tekniset tiedot","Tekniske specifikationer"]
["Version","Ausführung","Version","Exécution","Esecuzione","Versie","Provedení","Prevedenie","Wykonanie","Kivitel","Malli","Udgave"]
["Overall area [m²]","Gesamtfläche [m²]","Overall area [m²]","Surface totale [m²]","Superficie complessiva [m²]","Totaal oppervlak [m²]","Celková plocha [m²]","Celková plocha [m²]","Powierzchnia całkowita [m²]","Összfelület [m²]","Kokonaispinta-ala [m²]","Samlet areal"]
["Aperture area [m²]","Aperturfläche [m²]","Aperture area [m²]","Surface ouverture [m²]","Superficie apertura [m²]","Apertuur oppervlak [m²]","Aperturní plocha [m²]","Apertúrna plocha [m²]","Powierzchnia czynna [m²]","Apertúra felület [m²]","Absorboiva pinta-ala [m²]","Aperturareal"]
["Subsidides area [m²]","Geförderte Fläche [m²]","Subsidides area [m²]","Surface subventionnée [m²]","Superficie alimentata [m²]","Vereiste oppervlak [m²]","Požadovaná plocha [m²]","Požadovaná plocha [m²]","Powierzchnia wymagana [m²]","Támogatott felület [m²]","Pinta-ala tukiaisiin (Saksassa) [m²]","Absorberingsareal"]
["Height [mm]","Höhe [mm]","Height [mm]","Hauteur [mm]","Altezza [mm]","Hoogte [mm]","Výška [mm]","Výška [mm]","Wysokość [mm]","Magasság [mm]","Korkeus [mm]","Højde [mm]"]
["Width [mm]","Breite [mm]","Width [mm]","Largeur [mm]","Larghezza [mm]","Breedte [mm]","Šířka [mm]","Šírka [mm]","Szerokość [mm]","Szélesség [mm]","Leveys [mm]","Bredde [mm]"]
["Depth [mm]","Tiefe [mm]","Depth [mm]","Profondeur [mm]","Profondità [mm]","Diepte [mm]","Hloubka [mm]","Hĺbka [mm]","Głębokość [mm]","Mélység [mm]","Syvyys [mm]","Dybde [mm]"]
["Weight, dry [kg]","Gewicht, leer [kg]","Weight, dry [kg]","Poids, à vide [kg]","Peso, a vuoto[kg]","Gewicht, leeg [kg]","Hmotnost, prázdný [kg]","Hmotnosť, prázdny [kg]","Masa własna [kg]","Súly, üres [kg]","Paino tyhjänä [kg]","Vægt, tør [kg]"]
["Capacity [l]","Inhalt [l]","Capacity [l]","Capacité [l]","Contenuto [I]","Inhoud [l]","Objem [l]","Objem [l]","Pojemność [l]","Űrtartalom [l]","Vetoisuus [l]","Kapacitet [l]"]
["Permissible operating pressure [bar]","Zul. Betriebsdruck [bar]","Permissible operating pressure [bar]","Pression de service adm. [bar]","Pressione d'esercizio ammessa [bar]","Toelaatbare werkdruk [bar]","Přípustný provozní tlak [bar]","Prípustný prevádzkový tlak [bar]","Dop. ciśnienie robocze [bar]","Megeng. üzemi túlnyomás [bar]","Sallittu käyttöpaine [bar]","Tilladt driftstryk [bar]"]
["Conversion factor Eta-0","Konversionsfaktor Eta-0","Conversion factor Eta-0","Facteur de conversion h0","Fattore di conversione Eta-0","Conversiefactor Eta-0","Konverzní faktor Eta-0","Konverzný faktor Eta-0","Współczynnik konwersji Eta-0","Konverziós tényező Eta-0","Muuntokerroin EƬα-0","Konversionsfaktor Eta-0"]
["Heat loss coefficient a0","Wärmeverlustfaktor a0","Heat loss coefficient a0","Coefficient de transfert thermique a1","Coefficiente di perdita di calore a0","Warmteverliesfactor a0","Součinitel ztráty tepla a0","Súčiniteľ tepelných strát a0","Współczynnik strat ciepła a0","Hőveszteségi tényező a0","Lämpöhäviökerroin a0","Varmetabskoefficient a0"]
["Heat loss coefficient a1","Wärmeverlustfaktor a1","Heat loss coefficient a1","Coefficient de transfert thermique a2","Coefficiente di perdita di calore a1","Warmteverliesfactor a1","Součinitel ztráty tepla a1","Súčiniteľ tepelných strát a1","Współczynnik strat ciepła a1","Hőveszeségi tényező a1","Lämpöhäviökerroin a1","Varmetabskoefficient a1"]
["Connection","Anschluss","Connection","Raccords","Allacciamento","Aansluiting","Připojení","Pripojenie","Przyłącze","csatlakozó","Liitos","Tilslutning"]
["Application range","Einsatzbereich","Application range","Domaine d'utilisation","Campo di utilizzo"," Toepassingsgebied","Oblast použití","Oblasť použitia","Zakres zastosowania","Alkalmazási terület","Käyttömahdollisuudet","Anvendelsesområde"]
["G ¾\" male","G ¾ außen","G ¾\" male","G ¾¨ extérieur","G ¾¨ esterno","G ¾ \" buiten","G¾ vnější","G¾ vonkajší","G ¾“, zewn.","G ¾ külső","G ¾\" uros","G ¾\" udv."]
["Flat roof","Flachdach","Flat roof","Toit plat","Tetto piatto","Platdak","Plochá střecha","Plochá strecha","Dach płaski","Lapos tető","Tasakatto","Fladttag"]
["Wall mounting","Wandmontage","Wall mounting","Montage mural","Montaggio a parete","Wandmontage","Nástěnná montáž","Montáž na stenu","Montaż ścienny","Fali szerelés","Seinäkiinnitys","Vægmontering"]
["Roof integration","Indachmontage","Roof integration","capteur intégré en toiture","Montaggio sottotetto","Geintegreerd in het dak","Střešní montáž","Monáž do strechy","Montaż w dachu","Tetőbe szerelés","Kattointegraatio","Tagintegrering"]
["Vertical","Senkrecht","Vertical","Vertical","Verticale","Vertikaal","Svisle","Zvisle","Pionowo","Függőlegesen","Vertikaalinen","Vertikal"]
["Horizontal","Waagerecht","Horizontal","Horizontal","Orizzontale","Horizontaal","Vodorovně","Vodorovne","Poziomo","Vízszintesen","Horisontaalinen","Horisontal"]
[]
["Beispielprojekt","Beispielprojekt","Beispielprojekt","Exemple de projet","Beispielprojekt","Voorbeeldproject","Beispielprojekt","Beispielprojekt","Beispielprojekt","Beispielprojekt","Beispielprojekt","Beispielprojekt"]
["Stiebel Eltron GmbH & Co. KG","Stiebel Eltron GmbH & Co. KG","Stiebel Eltron GmbH & Co. KG","Stiebel Eltron SAS","Stiebel Eltron GmbH & Co. KG","Stiebel Eltron Nederland B.V.","Stiebel Eltron GmbH & Co. KG","Stiebel Eltron GmbH & Co. KG","Stiebel Eltron GmbH & Co. KG","Stiebel Eltron GmbH & Co. KG","Stiebel Eltron GmbH & Co. KG","Stiebel Eltron GmbH & Co. KG"]
["Dr.-Stiebel-Straße","Dr.-Stiebel-Straße","Dr.-Stiebel-Straße","7-9, rue des Selliers-BP 85107","Dr.-Stiebel-Straße","Daviottenweg 36","Dr.-Stiebel-Straße","Dr.-Stiebel-Straße","Dr.-Stiebel-Straße","Dr.-Stiebel-Straße","Dr.-Stiebel-Straße","Dr.-Stiebel-Straße"]
["37603 Holzminden","37603 Holzminden","37603 Holzminden","57073 Metz Cedex 3","37603 Holzminden","5222 BH 's-HERTOGENBOSCH","37603 Holzminden","37603 Holzminden","37603 Holzminden","37603 Holzminden","37603 Holzminden","37603 Holzminden"]
["05531 / 702 110","05531 / 702 110","05531 / 702 110","03 87 74 51 36","05531 / 702 110","073-6230000","05531 / 702 110","05531 / 702 110","05531 / 702 110","05531 / 702 110","05531 / 702 110","05531 / 702 110"]

{"sheet":"Preisliste","index":5,"n_rows":1971,"n_cols":34,"rows_kept":1971,"cut":false,"hidden":true,"merged":[[3,33,4,33],[3,17,4,17],[3,18,4,18],[3,29,4,29],[3,30,4,30],[3,26,4,26],[3,27,4,27],[3,28,4,28],[3,31,4,31],[3,19,4,19],[3,32,4,32],[3,21,4,21],[3,16,4,16],[3,22,4,22],[3,23,4,23],[3,24,4,24],[3,25,4,25],[3,20,4,20]]}
[]
[null,{"$f":"Translation!A128","v":"Stiebel Eltron pricelist"}]
[null,null,null,null,null,null,null,null,null,null,null,"Gewählte Sprache/Preisliste zum Rückgängig machen manueller Änderungen",null,null,"Dt. Preisliste?"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!AB14=Zwischenwerte!AB17,TRUE,FALSE)","v":false},null,"Ident","Preis-Deutsch","Preis-Intern.","Französisch","Dänisch","Niederländisch","Deutschland","Großbritannien","Frankreich","Italien","Niederlande","Tschechien","Slovakei","Polen","Ungarn","Finnland","Dänemark","Neutral, ohne Übersetzung"]
[null,{"$f":"Translation!$A$98","v":"ID"},{"$f":"Translation!$A$99","v":"Description"},{"$f":"Translation!$A$100","v":"Price each"},null,null,null,null,null,null,null,"Ident.-Nr.","Bezeichnung","Preis","Eintrag geändert ?",null,null,"Preis(Dtld.)","Preis(Dtld.)","Preis(Dtld.)","Preis(Dtld.)","Preis(Dtld.)"]
[null,230016,"Solar flat-plate collector SOL 27 premium S",809,{"$f":"IF(O6=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,230016,"Solar flat-plate collector SOL 27 premium S",809,{"$f":"IF(AND(B6=L6,C6=M6,D6=N6),FALSE,TRUE)","v":false},null,230016,849,809,"1.195,00",5073,849,"Solar-Flachkollektor SOL 27 premium S","Solar flat-plate collector SOL 27 premium S","Capteur solaire plan SOL 27 premium S","Pannello solare piatto SOL 27 premium S","Opbouw-collector SOL 27 premium S","solární plochý kolektor SOL 27 premium S","Plochý solárny kolektor SOL 27 premium S","Plaski kolektor słoneczny  SOL 27 premium S","Solar síkkolektor SOL 27 premium S","Aurinko - tasokeräin SOL 27 premium S","Solfangerpanel, fritliggende\n SOL 27 premium S\n","SOL 27 premium S"]
[null,230017,"Solar flat-plate collector SOL 27 premium W",849,{"$f":"IF(O7=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,230017,"Solar flat-plate collector SOL 27 premium W",849,{"$f":"IF(AND(B7=L7,C7=M7,D7=N7),FALSE,TRUE)","v":false},null,230017,849,849,"1.195,00",5677,849,"Solar-Flachkollektor SOL 27 premium W","Solar flat-plate collector SOL 27 premium W","Capteur solaire plan SOL 27 premium W","Pannello solare piatto SOL 27 premium W","Opbouw-collector SOL 27 premium W","solární plochý kolektor SOL 27 premium W","Plochý solárny kolektor SOL 27 premium W","Plaski kolektor słoneczny  SOL 27 premium W","Solar síkkolektor SOL 27 premium W","Aurinko - tasokeräin SOL 27 premium W","Solfangerpanel, fritliggende\n SOL 27 premium W\n","SOL 27 premium W"]
[null,230185,"Push-fit connection SOL SV-A",49,"",null,null,null,null,null,null,230185,"Push-fit connection SOL SV-A",49,{"$f":"IF(AND(B8=L8,C8=M8,D8=N8),FALSE,TRUE)","v":false},null,230185,40.5,49,85,236,41,"Steckverbindung Kollektor SOL SV-A","Push-fit connection SOL SV-A","Raccord enfichable SOL SV-A ","collegamento di raccordo tra collettori SOL SV-A","Bevestigingssysteem SOL SV-A","násuvné propojení kolektoru SOL SV-A","Násuvné prepojenie kolektorov SOL SV-A","Mocowanie zatrzaskowe kolektora  SOL SV-A","Kollektor gyorscsatlakozás SOL SV-A","Pika-yhdistäjä SOL SV-A","Sammenkoblingstilbehør SOL SV-A\n","SOL SV-A"]
[null,231322,"Push-fit connection SOL SV-A50",55,"",null,null,null,null,null,null,231322,"Push-fit connection SOL SV-A50",55,false,null,231322,48.5,55,80,382,49,"Steckverbindung Kollektor SOL SV-A50","Push-fit connection SOL SV-A50","Raccord enfichable SOL SV-A 50","collegamento di raccordo tra collettori SOL SV-A50","Aansluit toebehoren SOL SV-A50","násuvné propojení kolektoru SOL SV-A50","Násuvné prepojenie kolektorov SOL SV-A50","Mocowanie zatrzaskowe kolektora  SOL SV-A50","Kollektor gyorscsatlakozás SOL SV-A50","Pika-yhdistäjä SOL SV-A50","Sammenkoblingstilbehør SOL SV-A50","SOL SV-A50"]
[null,230186,"Push-fit connection SOL SV-D",299,"",null,null,null,null,null,null,230186,"Push-fit connection SOL SV-D",299,false,null,230186,147,299,245,887,147,"Steckverbindung Kollektorgruppe SOL SV-D","Push-fit connection SOL SV-D","Raccord enfichable SOL SV-D ","collegamneto di raccordo per gruppi collettori SOL SV-D","Bevestigingssysteem SOL SV-D","násuvné propojení skupina kolektorů SOL SV-D","Násuvné prepojenie pre skupinu kolektorov SOL SV-D","Mocowanie zatrzaskowe grupa kolektora SOL SV-D","Kollektorcsoport gyorscsatlalkozás SOL SV-D","Pika-yhdistäjä  SOL SV-D","Sammenkoblingstilbehør SOL SV-D\n","SOL SV-D"]
[null,230913,"Push-fit connection SOL SV-F",162,"",null,null,null,null,null,null,230913,"Push-fit connection SOL SV-F",162,false,null,230913,122,162,190,991,122,"Steckverbindung Flachdach/Wand SOL SV-F","Push-fit connection SOL SV-F","Raccord enfichable SOL SV-F ","collegamento di raccordo per tetto piano / muro SOL SV-F","Steekverbindinng SOL SV-F","násuvné propojení plochá střecha/stěna SOL SV-F","Násuvné prepojenie kolektorov pre rovnú strechu/ stenu SOL SV-F","Mocowanie zatrzaskowe  dach płaski/ściana SOL SV-F","Lapostető/fal gyorscsatlakozás SOL SV-F","Pika-yhdistäjä SOL SV-F","Sammenkoblingstilbehør SOL SV-F\n","SOL SV-F"]
[null,228927,"Solar flat-plate collector SOL 27 Basic S",702,"",null,null,null,null,null,null,228927,"Solar flat-plate collector SOL 27 Basic S",702,false,null,228927,692,702,945,5342,692,"Solar-Flachkollektor SOL 27 Basic S","Solar flat-plate collector SOL 27 Basic S","Capteur solaire plan SOL 27 utile S","Pannello solare piatto SOL 27 Basic S","Opbouw-collector SOL 27 basic","solární plochý kolektor SOL 27 Basic S","Plochý solárny kolektor SOL 27 Basic S","Plaski kolektor słoneczny  SOL 27 Basic S","Solar síkkolektor SOL 27 Basic S","Aurinko - tasokeräin SOL 27 Basic S","Solfangerpanel, fritliggende\n SOL 27 basic S\n","SOL 27 Basic S"]
[null,230912,"Solar flat-plate collector SOL 27 Basic W",729,"",null,null,null,null,null,null,230912,"Solar flat-plate collector SOL 27 Basic W",729,false,null,230912,692,729,990,4708,692,"Solar-Flachkollektor SOL 27 Basic W","Solar flat-plate collector SOL 27 Basic W","Capteur solaire plan SOL 27 utile W","Pannello solare piatto SOL 27 Basic W","Opbouw-collector SOL 27 basic W","solární plochý kolektor SOL 27 Basic W","Plochý solárny kolektor SOL 27 Basic W","Plaski kolektor słoneczny  SOL 27 Basic W","Solar síkkolektor SOL 27 Basic W","Aurinko - tasokeräin SOL 27 Basic W","Solfangerpanel, fritliggende\n SOL 27 basic W\n","SOL 27 Basic W"]
[null,229322,"Collector sensor pocket KTH basic",36,"",null,null,null,null,null,null,229322,"Collector sensor pocket KTH basic",36,false,null,229322,19.3,36,55,147,19,"Kollektortauchhülse KTH basic","Collector sensor pocket KTH basic","Doigt de gant KTH-B","guaina sonda collettore KTH basic","Collectordompelbuis KTH basic","kolektorová jímka KTH basic","Ponorná rúrka kolektora KTH basic","Tuleja zanużeniowa kolektora  KTH basic","Kollektor merülőhüvely KTH basic","Keräimen anturitasku KTH basic","Følerlomme til SOL 27 basic KTH basic\n","KTH basic"]
[null,73469,"Corrugated stainless steel hose",73,"",null,null,null,null,null,null,73469,"Corrugated stainless steel hose",73,false,null,73469,98,73,105,450,98,"Edelstahl-Wellschlauch","Corrugated stainless steel hose","Tuyau souple SOL SL pour passage de toiture ","tubo flessibile in acciaio ondulato","RVS geribbelde slang","ocelová vlnová hadice","Nerezová vlnitá hadica","Wąż z nierdzewnej  blachy falistej","Rozsdamentes acél flexicső","RST haitariletku","Flexslange, rustfrit stål Flexslange, rustfrit stål","Edelstahl-Wellschlauch"]
[null,231980,"Quick-connector SOL SBP-S",260,"",null,null,null,null,null,null,231980,"Quick-connector SOL SBP-S",260,false,null,231980,231,260,365,1825,231,"Schnell-Befestigung SOL SBP-S","Quick-connector SOL SBP-S","Fixation rapide SOL SBP-S pour montage vertical ","fissaggio rapido SOL SBP-S","Bevestigingssysteem SOL SBP-S","rychloupevňovací sada SOL SBP-S","Montážny rám pre rýchlo- upevňovaciu sadu SOL SBP-S","szybkozłączki SOL SBP-S","Gyorsrögzítés SOL SBP-S","Pikakiinnike tiilikate SOL SBP-S","Quick-kobling SOL SBP-S","SOL SBP-S"]
[null,231981,"Quick-connector SOL SBP-W",261,"",null,null,null,null,null,null,231981,"Quick-connector SOL SBP-W",261,false,null,231981,231,261,385,1825,231,"Schnell-Befestigung SOL SBP-W","Quick-connector SOL SBP-W","Fixation rapide SOL SBP-W pour montage horizontal ","fissaggio rapido SOL SBP-W","Bevestigingssysteem SOL SBP-W","rychloupevňovací sada SOL SBP-W","Montážny rám pre rýchlo- upevňovaciu sadu SOL SBP-W","szybkozłączki SOL SBP-W","Gyorsrögzítés SOL SBP-W","Pikakiinnike tiilikate SOL SBP-W","Quick-kobling SOL SBP-W","SOL SBP-W"]
[null,231982,"Quick-connector SOL SBP-WE",263,"",null,null,null,null,null,null,231982,"Quick-connector SOL SBP-WE",263,false,null,231982,231,263,370,1848,231,"Schnell-Befestigung SOL SBP-WE","Quick-connector SOL SBP-WE","Fixation rapide SOL SBP-WE pour montage en superposition","fissaggio rapido SOL SBP-WE","Bevestigingssysteem SOL SBP-WE","rychloupevňovací sada SOL SBP-WE","Rýchlo- upevňovaciu sada SOL SBP-WE","szybkozłączki SOL SBP-WE","Gyorsrögzítés SOL SBP-WE","Pikakiinnike tiilikate SOL SBP-WE","Quick-kobling SOL SBP-WE","SOL SBP-WE"]
[null,230175,"Fixing Kit - tiled roof SOL BP",80,"",null,null,null,null,null,null,230175,"Fixing Kit - tiled roof SOL BP",80,false,null,230175,85,80,120,511,85,"Befestigung Pfannendach SOL BP","Fixing Kit - tiled roof SOL BP","Kit de fixation SOL BP pour toiture tuiles","fissagio per tetti a tegola SOL BP","Bevestigingssysteem SOL BP","upevnění na taškovou střechu SOL BP","Upevňovacia sada pre škridľovú strechu SOL BP","Mocowania dachówek SOL BP","Cseréptető rögzítés SOL BP","Kiinnityssarja - Tiilikatto SOL BP","Montagesystem tagsten SOL BP\n","SOL BP"]
[null,231998,"Fixing Kit - corrugated roof SOL BW",144,"",null,null,null,null,null,null,231998,"Fixing Kit - corrugated roof SOL BW",144,false,null,231998,131,144,170,879,131,"Befestigung Welldach SOL BW","Fixing Kit - corrugated roof SOL BW","Kit de fixation SOL BW pour tôles ondulées ","fissaggio per tetto ondulato SOL BW","Bevestigingssysteem SOL BW","upevnění na vlnitou střechu SOL BW","Upevňovacia sada na  vlnitú strechu SOL BW","Mocowanie na dachu z pokryciem falistym  SOL BW","Hullámtető rögzítés SOL BW","Kiinnityssarja - Peltikatto SOL BW","Montagesystem eternittag SOL BW","SOL BW"]
[null,230189,"Fixing kit - shingle roof SOL BS",119,"",null,null,null,null,null,null,230189,"Fixing kit - shingle roof SOL BS",119,false,null,230189,92,119,160,543,92,"Befestigungssatz Schindeldach SOL BS","Fixing kit - shingle roof SOL BS","Kit de fixation SOL BS pour toit ardoise ou bardeaux","fissaggio per tetto a lastre SOL BS","Bevestigingssysteem SOL BS","upevňovací sada na šindelovou střechu SOL BS","Upevňovacia sada pre bridlicovú/ šindľovú strechu SOL BS","Zestaw mocowania na dachu pokrytym gotem SOL BS","Rögzítőelem zsindelytetőhöz SOL BS","Kiinnityssarja SOL BS","Montagesystem skiffer SOL BS\n","SOL BS"]
[null,230190,"Fixing kit - plain tile roof SOL BB",190,"",null,null,null,null,null,null,230190,"Fixing kit - plain tile roof SOL BB",190,false,null,230190,159,190,305,1050,159,"Befestigung Biberschwanzpfanne SOL BB","Fixing kit - plain tile roof SOL BB","Kit de fixation SOL BB pour tuiles plates (acier galvanisé)","fissaggio per tetto a lastre SOL BB","Bevestigingssysteem SOL BB","upevnění na střechu z bobrovek SOL BB","Upevňovacia sada pre strešné tašky bobrovky SOL BB","Mocowanie na dachu z dachówką płaską (n.p.karpiówka) SOL BB","Rögzítőelem hódfarkú cseréptetőhöz SOL BB","Kiinnityssarja - SOL BB","Montagesystem bæverhaletag SOL BB\n","SOL BB"]
[null,230191,"Fixing kit - plain tile roof SOL BB-Cu",279,"",null,null,null,null,null,null,230191,"Fixing kit - plain tile roof SOL BB-Cu",279,false,null,230191,227,279,395,1356,227,"Befestigung Biberschwanzpfanne SOL BB-Cu","Fixing kit - plain tile roof SOL BB-Cu","Kit de fixation SOL BB-Cu pour tuiles plates (cuivre)","fissaggio per tetto a lastre SOL BB-Cu","Bevestigingssysteem SOL BB-Cu","upevnění na střechu z bobrovek SOL BB-Cu","Upevňovacia sada pre strešné tašky bobrovky SOL BB- Cu","Mocowanie na dachu z dachówką płaską (n.p.karpiówka) SOL BB-Cu","Rögzítőelem hódfarkú cseréptetőhöz SOL BB-Cu","Kiinnityssarja - SOL BB-Cu","Montagesystem bæverhale (kobber) SOL BB-Cu\n","SOL BB-Cu"]
[null,230177,"Mounting kit flat roof SOL BF-S",170,"",null,null,null,null,null,null,230177,"Mounting kit flat roof SOL BF-S",170,false,null,230177,187,170,160,1110,187,"Befestigungssatz Flachdach SOL BF-S","Mounting kit flat roof SOL BF-S","Kit de fixation SOL BF-S pour toit plat","fissaggio per tetto piano SOL BF-S","Bevestigingssysteem SOL BF-S","upevňovací sada na plochou střechu SOL BF-S","Upevňovacia sada pre rovnú strechu/ stenu SOL BF- S","Zestaw mocowania na dachu płaskim SOL BF-S","Rögzítőelem lapostetőhöz SOL BF-S","Asennussarja tasakatto SOL BF-S","Montagesystem fladtag/væg SOL BF-S\n","SOL BF-S"]
[null,230178,"Mounting kit flat roof SOL BF-W",170,"",null,null,null,null,null,null,230178,"Mounting kit flat roof SOL BF-W",170,false,null,230178,187,170,155,1244,187,"Befestigungssatz Flachdach SOL BF-W","Mounting kit flat roof SOL BF-W","Kit de fixation SOL BF-W pour toit plat","fissaggio per tetto piano SOL BF-W","Bevestigingssysteem SOL BF-W","upevňovací sada na plochou střechu SOL BF-W","Upevňovacia sada pre rovnú strechu/ stenu SOL BF- W","Zestaw mocowania na dachu płaskim SOL BF-W","Rögzítőelem lapostetőhöz SOL BF-W","Asennussarja tasakatto SOL BF-W","Montagesystem fladtag/væg SOL BF-W\n","SOL BF-W"]
[null,230169,"Mounting frame SOL R1",90,"",null,null,null,null,null,null,230169,"Mounting frame SOL R1",90,false,null,230169,98,90,110,589,98,"Montagerahmen SOL R1","Mounting frame SOL R1","Cadre de montage SOL R1 pour 1 capteur","telaio di montaggio SOL R1","Bevestigingssysteem SOL R1","montážní rámy SOL R1","Montážny rám SOL R1","Rama montażowa SOL R1","Szerelőkeret SOL R1","Profiilikisko SOL R1","Montageramme 1 panel SOL R1\n","SOL R1"]
[null,230920,"Mounting frame SOL R1 W",114,"",null,null,null,null,null,null,230920,"Mounting frame SOL R1 W",114,false,null,230920,171,114,160,745,171,"Montagerahmen SOL R1 W","Mounting frame SOL R1 W","Cadre de montage SOL R1 W pour 1 capteur","telaio di montaggio SOL R1 W","Bevestigingssysteem SOL R1 W","montážní rámy SOL R1 W","Montážny rám SOL R1 W","Rama montażowa SOL R1 W","Szerelőkeret SOL R1 W","Profiilikisko SOL R1 W","Montageramme 1 panel SOL R1 W\n","SOL R1 W"]
[null,230170,"Mounting frame SOL R2",160,"",null,null,null,null,null,null,230170,"Mounting frame SOL R2",160,false,null,230170,174,160,170,1170,174,"Montagerahmen SOL R2","Mounting frame SOL R2","Cadre de montage SOL R2 pour 2 capteurs","telaio di montaggio SOL R2","Bevestigingssysteem SOL R2","montážní rámy SOL R2","Montážny rám SOL R2","Rama montażowa SOL R2","Szerelőkeret SOL R2","Profiilikisko SOL R2","Montageramme 2 paneler SOL R2\n","SOL R2"]
[null,230171,"Frame connection set SOL RV",67,"",null,null,null,null,null,null,230171,"Frame connection set SOL RV",67,false,null,230171,39.5,67,65,426,40,"Rahmen-Verbindungssatz SOL RV","Frame connection set SOL RV","Kit d'assemblage SOL RV ","telaio di collegamento SOL RV","Bevestigingssysteem SOL RV","sada na propojení rámů SOL RV","Spojovník montážnych rámov SOL RV","Zestaw mocowania ramy SOL RV","Keret összekötőelem SOL RV","Rungon kiinnikesarja SOL RV","Rammeforbindelsessæt SOL RV\n","SOL RV"]
[null,230172,"Frame connection set SOL RV-W",166,"",null,null,null,null,null,null,230172,"Frame connection set SOL RV-W",166,false,null,230172,176,166,100,1050,176,"Rahmen-Verbindungssatz SOL RV-W","Frame connection set SOL RV-W","Kit d’assemblage  SOL RV-W","telaio di collegamento SOL RV-W","Bevestigingssysteem SOL RV-W","sada na propojení rámů SOL RV-W","Spojovník montážnych rámov SOL RV- W","Zestaw mocowania ramy SOL RV-W","Keret összekötőelem SOL RV-W","Rungon kiinnikesarja SOL RV-W","Rammeforbindelsessæt SOL RV-W\n","SOL RV-W"]
[null,230173,"Frame support SOL RA",67,"",null,null,null,null,null,null,230173,"Frame support SOL RA",67,false,null,230173,71,67,75,439,71,"Rahmenaufständerung SOL RA","Frame support SOL RA","Support d’inclinaison SOL RA","telaio per inclinazione SOL RA","Bevestigingssysteem SOL RA","podpěra rámu SOL RA","Podpera rámu SOL RA","Ramowa konstrukcja wsporcza SOL RA","Keret felállítása SOL RA","Runkotuki SOL RA","Rammeevelationsenhed SOL RA\n","SOL RA"]
[null,230931,"Cover strip SOL AL-S",115,"",null,null,null,null,null,null,230931,"Cover strip SOL AL-S",115,false,null,230931,66,115,170,550,66,"Abdeckleiste SOL AL-S","Cover strip SOL AL-S","Cache SOL AL-S pour interstice entre capteurs","Valvola deviatrice SOL AL-S","Bevestigingssysteem SOL AL-S","krycí lišta SOL AL-S","Krycia lišta SOL AL-S","Cover strip SOL AL-S","Takaróprofil SOL AL-S","Peitelista SOL AL-S","Afdækningslister SOL 27 premium S SOL AL-S\n","SOL AL-S"]
[null,230932,"Cover strip SOL AL-W",80,"",null,null,null,null,null,null,230932,"Cover strip SOL AL-W",80,false,null,230932,50.5,80,125,381,51,"Abdeckleiste SOL AL-W","Cover strip SOL AL-W","Cache SOL AL-W pour interstice entre capteurs","Valvola deviatrice SOL AL-W","Bevestigingssysteem SOL AL-W","krycí lišta SOL AL-W","Krycia lišta SOL AL-W","Cover strip SOL AL-W","Takaróprofil SOL AL-W","Peitelista SOL AL-W","Afdækningslister SOL 27 premium W SOL AL-W\n","SOL AL-W"]
[null,230020,"Solar flat-plate collector SOL 23 premium",1138,"",null,null,null,null,null,null,230020,"Solar flat-plate collector SOL 23 premium",1138,false,null,230020,834,1138,"1.550,00",6116,834,"Solar-Flachkollektor SOL 23 premium","Solar flat-plate collector SOL 23 premium","Capteur solaire plan intégrable en toiture SOL 23 premium","Pannello solare piatto SOL 23 premium","Inbouw collector SOL 23 premium","solární plochý kolektor SOL 23 premium","Plochý solárny kolektor SOL 23 premium","Płaski kolektor słoneczny  SOL 23 premium","Solar síkkolektor SOL 23 premium","Aurinko - tasokeräin SOL 23 premium","Solfangerpanel, integreret\n SOL 23 premium\n","SOL 23 premium"]
[null,230187,"Push-fit connection SOL SV-I",59,"",null,null,null,null,null,null,230187,"Push-fit connection SOL SV-I",59,false,null,230187,57,59,115,429,57,"Steckverbindung Kollektor SOL SV-I","Push-fit connection SOL SV-I","Raccord enfichable SOL SV-I pour capteur en intégration ","collegamento di raccordo tra collettori SOL SV-I","Bevestigingssysteem SOL SV-I","násuvné propojení kolektoru SOL SV-I","Násuvné prepojenie kolektorov SOL SV-I","Mocowanie zatrzaskowe kolektora  SOL SV-I","Kollektor gyorscsatlakozás SOL SV-I","Pika-yhdistäjä SOL SV-I","Sammenkoblingstilbehør SOL SV-I\n","SOL SV-I"]
[null,230188,"Push-fit connection SOL SV-R",193,"",null,null,null,null,null,null,230188,"Push-fit connection SOL SV-R",193,false,null,230188,92,193,260,901,92,"Steckverbindung Kollektorgruppe SOL SV-R","Push-fit connection SOL SV-R","Raccord enfichable SOL SV-R pour passage de toit","collegamneto di raccordo per gruppi collettori SOL SV-R","Bevestigingssysteem SOL SV-R","násuvné propojení skupina kolektorů SOL SV-R","Násuvné prepojenie pre skupinu kolektorov SOL SV-R","Mocowanie zatrzaskowe grupa kolektora SOL SV-R","Kollektorcsoport gyorscsatlalkozás SOL SV-R","Pika-yhdistäjä SOL SV-R","Sammenkoblingstilbehør SOL SV-R\n","SOL SV-R"]
[null,230184,"Side cover set SOL AS",370,"",null,null,null,null,null,null,230184,"Side cover set SOL AS",370,false,null,230184,267,370,480,1907,267,"Seitenabdeckungs-Set SOL AS","Side cover set SOL AS","Kit d'étanchéité latérale SOL AS pour capteur en intégration","Set coperture laterali SOL AS","Bevestigingssysteem SOL AS","sada bočních krytů SOL AS","Sada bočných krytov SOL AS","Zestaw pokrycia bocznego SOL AS","Kollektormező lezáró szett SOL AS","Sivusuojasarja SOL AS","Montagebeslag, SOL 23 premium SOL AS\n","SOL AS"]
[null,230183,"Side flashing SOL AZ",103,"",null,null,null,null,null,null,230183,"Side flashing SOL AZ",103,false,null,230183,81,103,155,613,81,"Abdeckung Erweiterung übereinander SOL AZ","Side flashing SOL AZ","Cache SOL AZ pour capteurs en intégration","copertura di lamiera per posa collettori sovrapposti SOL AZ","Bevestigingssysteem SOL AZ","rozšíření krytů nad sebou SOL AZ","Rozšírenie krytov pre montáž nad  SOL AZ ","Pokrycie rozszerzenia jeden na drugim SOL AZ","Szerelőkeret egymás fölé szerelt kollektorokhoz SOL AZ","Sivu SOL AZ","Montagebeslag, SOL 23 premium SOL AZ\n","SOL AZ"]
[null,234785,"Solar control unit SOM 7 E Plus",224,"",null,null,null,null,null,null,234785,"Solar control unit SOM 7 E Plus",224,false,null,234785,299,224,300,1594,299,"Solar-Regelung SOM 7 E Plus","Solar control unit SOM 7 E Plus","Régulation solaire SOM 7 E Plus","Regolazione solare SOM 7 E Plus","Solar regeling SOM 7 E Plus","solární regulace SOM 7 E Plus","Regulácia solárneho systému SOM 7 E Plus","Sterownik kolektora słonecznego SOM 7 E Plus","Solar vezérlő SOM 7 E Plus","Aurinkopiirin säätöyksikkö SOM 7 E Plus","Solfangerstyring SOM 7 E plus\n","SOM 7 E Plus"]
[null,230933,"Solar control unit SOM 8 plus",618,"",null,null,null,null,null,null,230933,"Solar control unit SOM 8 plus",618,false,null,230933,675,618,820,4038,675,"Solar-Regelung SOM 8 plus","Solar control unit SOM 8 plus","Régulation solaire SOM 8 Plus","Regolazione solare SOM 8 plus","Solar regeling SOM 8 plus","solární regulace SOM 8 Plus","Regulácia solárneho systému SOM 8 Plus","Sterownik kolektora słonecznego SOM 8 plus","Solar vezérlő SOM 8 plus","Aurinkopiirin säätöyksikkö SOM 8 Plus","Solfangerstyring SOM 8 plus\n","SOM 8 plus"]
[null,165818,"Temperature sensor PT 1000",19,"",null,null,null,null,null,null,165818,"Temperature sensor PT 1000",19,false,null,165818,30.6,19,40,125,31,"Temperaturfühler PT 1000","Temperature sensor PT 1000","Sonde de température PT 1000","Lamiera di copertura PT 1000","Temperatuurvoeler PT 1000","čidlo teploty PT 1000","Čidlo teploty PT 1000","Temperature Sensor PT 1000","Hőmérséklet érzékelő PT 1000","Lämpötila-anturi PT 1000","Temperaturføler PT 1000\n","PT 1000"]
[null,187872,"Sensor pack HKM",117,"",null,null,null,null,null,null,187872,"Sensor pack HKM",117,false,null,187872,167,117,165,790,167,"Fühlerpaket Heizkreismischer HKM","Sensor pack HKM","Kit de sondes HKM pour régulation solaire SOM 8","Set di sonde per gruppo risc. Miscelato HKM","HKM sensorpakket","sada čidla směšovacího okruhu HKM","Sada čidiel pre vykurovací okruh HKM","Sensor Pack Mixing valve HKM","Érzékelőszett kevertkörhöz HKM","Anturipaketti sekoitinventtiilille HKM","Følersæt Sensor pack HKM\n","HKM"]
[null,227729,"Heat meter SOM WMZ SOL",415,"",null,null,null,null,null,null,227729,"Heat meter SOM WMZ SOL",415,false,null,227729,445,415,575,3084,445,"Wärmemengenzähler SOM WMZ SOL","Heat meter SOM WMZ SOL","Calorimètre multi-fonctionnel SOM WMZ SOL","Contatore di energia SOM WMZ SOL","Warmteteller SOM WMZ SOL","měřič množství tepla SOM WMZ SOL","Merač tepla SOM WMZ SOL","Heat meter SOM WMZ SOL","Hőmennyiségmérő SOM WMZ SOL","Lämpömäärämittari SOM WMZ SOL","Energimåler SOM  WMZ SOL\n","SOM WMZ SOL"]
[null,170497,"Flowmeter V 40",226,"",null,null,null,null,null,null,170497,"Flowmeter V 40",226,false,null,170497,267,226,315,1520,267,"Volumenstrommesser V 40","Flowmeter V 40","Débitmètre V40 pour SOM 8 plus ou SOM WMZ SOL","Flowmeter V 40","Volumemeter V 40","měřič objemového průtoku V 40","Prietokomer V 40","Flowmeter V 40","Térfogatárammérő V 40","Tilavuusvirtamittari V 40","Flowmåler V 40\n","V 40"]
[null,234783,"Solar compact installation SOKI E trend",289,"",null,null,null,null,null,null,234783,"Solar compact installation SOKI E trend",289,false,null,234783,499,289,515,1743,799,"Solar-Kompaktinstallation SOKI E trend","Solar compact installation SOKI E trend","Kit hydraulique solaire SOKI utile","Installazione compatta solare SOKI E trend","Solar Compactinstallatie SOKI E trend","solární kompaktní instalace SOKI E trend","Čerpadlová skupina SOKI E trend","Kompaktowa instalacja kolektora słonecznego SOKI E trend","Solar egység SOKI E trend","Aurinko latausryhmä SOKI E trend","Kompaktpumpeinstallationssæt SOKI E trend\n","SOKI E trend"]
[null,234784,"Solar compact installation SOKI 7 E trend",540,"",null,null,null,null,null,null,234784,"Solar compact installation SOKI 7 E trend",540,false,null,234784,799,540,850,3338,499,"Solar-Kompaktinstallation SOKI 7 E trend","Solar compact installation SOKI 7 E trend","Kit hydraulique solaire SOKI 7 E trend","Installazione compatta solare SOKI 7 E trend","Solar Compactinstallatie SOKI 7 E trend","solární kompaktní instalace SOKI 7 E trend","Čerpadlová skupina SOKI 7 E trend","Kompaktowa instalacja kolektora słonecznego SOKI 7 E trend","Solar egység SOKI 7 E trend","Aurinko latausryhmä SOKI 7 E trend","Kompaktpumpeinstallationssæt SOKI 7 E trend\n","SOKI 7 E trend"]
[null,231014,"Solar compact installation SOKI E premium",859,"",null,null,null,null,null,null,231014,"Solar compact installation SOKI E premium",859,false,null,231014,1089,859,"sur demande",5304,1089,"Solar-Kompaktinstallation SOKI E premium","Solar compact installation SOKI E premium","Kit hydraulique solaire SOKI E premium","Installazione compatta solare SOKI E premium","Solar Compactinstallatie SOKI E premium","solární kompaktní instalace SOKI E premium","Čerpadlová skupina SOKI E premium","Kompaktowa instalacja kolektora słonecznego SOKI E premium","Solar egység SOKI E premium","Aurinko latausryhmä SOKI E premium","Kompaktpumpeinstallationssæt SOKI E premium\n","SOKI E premium"]
[null,231987,"Cylinder connection set SOKI SAS",142,"",null,null,null,null,null,null,231987,"Cylinder connection set SOKI SAS",142,false,null,231987,109,142,190,593,109,"Speicheranschlussset SOL SAS","Cylinder connection set SOKI SAS","Kit de montage SOKI SAS","Set di collegamento accumulatore SOKI SAS","Boileraansluitset SOKI SAS","sada k připojení zásobníku SOKI SAS","Pripájacia sada zásobníka SOKI SAS","Cylinder Connection-Set SOKI SAS","Tároló csatlakozási szett SOKI SAS","Varaajaliitäntäsarja SOKI SAS","Beholdertilslutningssæt SOKI SAS","SOKI SAS"]
[null,74098,"Warm water cylinder KS 150 SOL",1208,"",null,null,null,null,null,null,74098,"Warm water cylinder KS 150 SOL",1208,false,null,74098,1036,1208,"1.690,00",7532,1036,"Solar-Warmwasserspeicher KS 150 SOL","Warm water cylinder KS 150 SOL","Chauffe-eau solaire 150 litres KS 150 SOL","Bollitore solare KS 150 SOL","Zonneboiler KS 150 SOL","solární zásobník vody KS 150 SOL","Solárny zásobníkový ohrievač vody  KS 150 SOL","Zasobnik ciepłej wody solara słonecznego KS 150 SOL","Solar melegvíztároló KS 150 SOL","Käyttövesi-aurinkovaraaja KS 150 SOL","Varmtvandsbeholder, solar KS 150 SOL\n","KS 150 SOL"]
[null,187873,"Warm water cylinder SBB 300 plus",1692,"",null,null,null,null,null,null,187873,"Warm water cylinder SBB 300 plus",1692,false,null,187873,1295,1692,"2.240,00",10102,1295,"Solar-Warmwasserspeicher SBB 300 plus","Warm water cylinder SBB 300 plus","Chauffe-eau solaire 300 litres SBB 300 plus","Bollitore solare SBB 300 plus","Zonneboiler SBB 300 plus","solární zásobník vody SBB 300 plus","Solárny zásobníkový ohrievač vody  SBB 300 plus","Zasobnik ciepłej wody solara słonecznego SBB 300 plus","Solar melegvíztároló SBB 300 plus","Käyttövesi-aurinkovaraaja SBB 300 plus","Varmtvandsbeholder, solar SBB 300 plus\n","SBB 300 plus"]
[null,187874,"Warm water cylinder SBB 400 plus",1838,"",null,null,null,null,null,null,187874,"Warm water cylinder SBB 400 plus",1838,false,null,187874,1622,1838,"2.475,00",11473,1622,"Solar-Warmwasserspeicher SBB 400 plus","Warm water cylinder SBB 400 plus","Chauffe-eau solaire 400 litres SBB 400 plus","Bollitore solare SBB 400 plus","Zonneboiler SBB 400 plus","solární zásobník vody SBB 400 plus","Solárny zásobníkový ohrievač vody  SBB 400 plus","Zasobnik ciepłej wody solara słonecznego SBB 400 plus","Solar melegvíztároló SBB 400 plus","Käyttövesi-aurinkovaraaja SBB 400 plus","Varmtvandsbeholder, solar SBB 400 plus\n","SBB 400 plus"]
[null,187875,"Warm water cylinder SBB 600 plus",2700,"",null,null,null,null,null,null,187875,"Warm water cylinder SBB 600 plus",2700,false,null,187875,2123,2700,"3.145,00",17671,2123,"Solar-Warmwasserspeicher SBB 600 plus","Warm water cylinder SBB 600 plus","Chauffe-eau solaire 600 litres SBB 600 plus","Bollitore solare SBB 600 plus","Zonneboiler SBB 600 plus","solární zásobník vody SBB 600 plus","Solárny zásobníkový ohrievač vody  SBB 600 plus","Zasobnik ciepłej wody solara słonecznego SBB 600 plus","Solar melegvíztároló SBB 600 plus","Käyttövesi-aurinkovaraaja SBB 600 plus","Varmtvandsbeholder, solar SBB 600 plus\n","SBB 600 plus"]
[null,233490,"Warm water cylinder SBB 300 Trend",1291,"",null,null,null,null,null,null,233490,"Warm water cylinder SBB 300 Trend",1291,false,null,233490,1127,1291,"1.840,00",8844,1127,"Solar-Warmwasserspeicher SBB 300 Trend","Warm water cylinder SBB 300 Trend","Chauffe-eau solaire 300 litres SBB 300 Utile","Bollitore solare SBB 300 Trend","Zonneboiler SBB 300 trend","solární zásobník vody SBB 300 Trend","Solárny zásobníkový ohrievač vody  SBB 300 Trend","Zasobnik ciepłej wody solara słonecznego SBB 300 Trend","Solar melegvíztároló SBB 300 Trend","Käyttövesi-aurinkovaraaja SBB 300 Trend","Varmtvandsbeholder, solar SBB 300 Trend\n","SBB 300 Trend"]
[null,233491,"Warm water cylinder SBB 400 Trend",1508,"",null,null,null,null,null,null,233491,"Warm water cylinder SBB 400 Trend",1508,false,null,233491,1341,1508,"2.060,00",10331,1341,"Solar-Warmwasserspeicher SBB 400 Trend","Warm water cylinder SBB 400 Trend","Chauffe-eau solaire 400 litres SBB 400 Utile","Bollitore solare SBB 400 Trend","Zonneboiler SBB 400 trend","solární zásobník vody SBB 400 Trend","Solárny zásobníkový ohrievač vody  SBB 400 Trend","Zasobnik ciepłej wody solara słonecznego SBB 400 Trend","Solar melegvíztároló SBB 400 Trend","Käyttövesi-aurinkovaraaja SBB 400 Trend","Varmtvandsbeholder, solar SBB 400 Trend\n","SBB 400 Trend"]
[null,233492,"Warm water cylinder SBB 500 Trend",1629,"",null,null,null,null,null,null,233492,"Warm water cylinder SBB 500 Trend",1629,false,null,233492,1592,1629,"2.295,00",11159,1592,"Solar-Warmwasserspeicher SBB 500 Trend","Warm water cylinder SBB 500 Trend","Chauffe-eau solaire 500 litres SBB 500 Utile","Bollitore solare SBB 500 Trend","Zonneboiler SBB 500 trend","solární zásobník vody SBB 500 Trend","Solárny zásobníkový ohrievač vody  SBB 500 Trend","Zasobnik ciepłej wody solara słonecznego SBB 500 Trend","Solar melegvíztároló SBB 500 Trend","Käyttövesi-aurinkovaraaja SBB 500 Trend","Varmtvandsbeholder, solar SBB 600 Trend\n","SBB 500 Trend"]
[null,221362,"Warm water cylinder SBB 401 WP SOL",2135,"",null,null,null,null,null,null,221362,"Warm water cylinder SBB 401 WP SOL",2135,false,null,221362,2336,2135,"2.695,00",10728,2336,"Warmwasserspeicher SBB 401 WP SOL","Warm water cylinder SBB 401 WP SOL","Ballon ECS solaire  400 litres SBB 401 WP SOL","Accumulatore solare SBB 401 WP SOL","Warmwaterboiler SBB 401 WP SOL","zásobník teplé vody SBB 401 WP SOL","Zásobníkový ohrievač vody SBB 401 WP SOL","Zasobnik ciepłej wody   SBB 401 WP SOL","Melegvíztároló SBB 401 WP SOL","Käyttövesivaraaja SBB 401 WP SOL","Varmtvandsbeholder m. sol SBB 401 WP SOL\n","SBB 401 WP SOL"]
[null,227534,"Warm water cylinder SBB 501 WP SOL",2435,"",null,null,null,null,null,null,227534,"Warm water cylinder SBB 501 WP SOL",2435,false,null,227534,2569,2435,"3.080,00",12903,2569,"Warmwasserspeicher SBB 501 WP SOL","Warm water cylinder SBB 501 WP SOL","Ballon ECS solaire 500 litres SBB 501 WP SOL","Accumulatore solare SBB 501 WP SOL","Warmwaterboiler SBB 501 WP SOL","zásobník teplé vody SBB 501 WP SOL","Zásobníkový ohrievač vody SBB 501 WP SOL","Zasobnik ciepłej wody   SBB 501 WP SOL","Melegvíztároló SBB 501 WP SOL","Käyttövesivaraaja SBB 501 WP SOL","Varmtvandsbeholder m. sol SBB 501 WP SOL\n","SBB 501 WP SOL"]
[null,232628,"Wellrohrverbinder Wärmeübertrager WRV 32",107,"",null,null,null,null,null,null,232628,"Wellrohrverbinder Wärmeübertrager WRV 32",107,false,null,232628,103,107,155,733,103,"Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","WRV 32 - Elément pour raccordement échangeurs sup. et inf. ","Wellrohrverbinder Wärmeübertrager WRV 32","Doorverbinding warmtewisselaar WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","WRV 32"]
[null,229294,"Warm water cylinder SBB 751 SOL",2384,"",null,null,null,null,null,null,229294,"Warm water cylinder SBB 751 SOL",2384,false,null,229294,2572,2384,"3.050,00",13693,2572,"Warmwasserspeicher SBB 751 SOL","Warm water cylinder SBB 751 SOL","Ballon ECS solaire 750 litres SBB 751 SOL ","Accumulatore solare SBB 751 SOL","Warmwaterboiler SBB 751 SOL","zásobník teplé vody SBB 751 SOL","Zásobníkový ohrievač vody SBB 751 SOL","Zasobnik ciepłej wody SBB 751 SOL","Melegvíztároló SBB 751 SOL","Käyttövesivaraaja SBB 751 SOL","Varmtvandsbeholder m. sol SBB 751 SOL\n","SBB 751 SOL"]
[null,229295,"Warm water cylinder SBB 1001 SOL",2868,"",null,null,null,null,null,null,229295,"Warm water cylinder SBB 1001 SOL",2868,false,null,229295,3111,2868,"3.370,00",20391,3111,"Warmwasserspeicher SBB 1001 SOL","Warm water cylinder SBB 1001 SOL","Ballon ECS solaire 1000 litres SBB 1001 SOL ","Accumulatore solare SBB 1001 SOL","Warmwaterboiler SBB 1001 SOL","zásobník teplé vody SBB 1001 SOL","Zásobníkový ohrievač vody SBB 1001 SOL","Zasobnik ciepłej wody SBB 1001 SOL","Melegvíztároló SBB 1001 SOL","Käyttövesivaraaja SBB 1001 SOL","Varmtvandsbeholder m. sol SBB 1001 SOL\n","SBB 1001 SOL"]
[null,231923,"Thermal insulation WDH 751 SBB",595,"",null,null,null,null,null,null,231923,"Thermal insulation WDH 751 SBB",595,false,null,231923,600,595,740,3837,600,"Wärmedämmung WDH 751 SBB","Thermal insulation WDH 751 SBB","Isolation renforcée WDH 751 SBB pour SBB 751 (SOL). ","Isolazione WDH 751 SBB","Isolatie WDH 751 SBB","tepelná izolace WDH 751 SBB","Tepelná izolácia WDH 751 SBB","Ocieplenie WDH 751 SBB","Hőszigetelés WDH 751 SBB","Lämmöneristys WDH 751  SBB","Isolering til varmtvandsbeholder WDH 751 SBB","WDH 751 SBB"]
[null,231924,"Thermal insulation WDH 1001 SBB",661,"",null,null,null,null,null,null,231924,"Thermal insulation WDH 1001 SBB",661,false,null,231924,681,661,815,4232,681,"Wärmedämmung WDH 1001 SBB","Thermal insulation WDH 1001 SBB","Isolation renforcée WDH 1001 SBB pour SBB 1001 (SOL)","Isolazione WDH 1001 SBB","Isolatie WDH 1001 SBB","tepelná izolace WDH 1001 SBB","Tepelná izolácia WDH 1001 SBB","Ocieplenie WDH 1001 SBB","Hőszigetelés WDH 1001 SBB","Lämmöneristys WDH 1001  SBB","Isolering til varmtvandsbeholder WDH 1001 SBB","WDH 1001 SBB"]
[null,231910,"Warm water cylinder SBB 600 WP SOL",2991,"",null,null,null,null,null,null,231910,"Warm water cylinder SBB 600 WP SOL",2991,false,null,231910,3319,2991,"3.805,00",20949,3319,"Warmwasserspeicher SBB 600 WP SOL","Warm water cylinder SBB 600 WP SOL","Ballon ECS solaire 575 litres SBB 600 WP SOL ","Accumulatore solare SBB 600 WP SOL","Warmwaterboiler SBB 600 WP SOL","zásobník teplé vody SBB 600 WP SOL","Zásobníkový ohrievač vody SBB 600 WP SOL","Zasobnik ciepłej wody SBB 600 WP SOL","Melegvíztároló SBB 600 WP SOL","Käyttövesivaraaja SBB 600 WP SOL","Varmtvandsbeholder SBB 600 WP SOL","SBB 600 WP SOL"]
[null,231911,"Warm water cylinder SBB 800 WP SOL",3327,"",null,null,null,null,null,null,231911,"Warm water cylinder SBB 800 WP SOL",3327,false,null,231911,3690,3327,"4.120,00",23304,3690,"Warmwasserspeicher SBB 800 WP SOL","Warm water cylinder SBB 800 WP SOL","Ballon ECS solaire 770 litres SBB 800 WP SOL ","Accumulatore solare SBB 800 WP SOL","Warmwaterboiler SBB 800 WP SOL","zásobník teplé vody SBB 800 WP SOL","Zásobníkový ohrievač vody SBB 800 WP SOL","Zasobnik ciepłej wody SBB 800 WP SOL","Melegvíztároló SBB 800 WP SOL","Käyttövesivaraaja SBB 800 WP SOL","Varmtvandsbeholder SBB 800 WP SOL","SBB 800 WP SOL"]
[null,231912,"Warm water cylinder SBB 1000 WP SOL",3690,"",null,null,null,null,null,null,231912,"Warm water cylinder SBB 1000 WP SOL",3690,false,null,231912,4024,3690,"4.420,00",25844,4024,"Warmwasserspeicher SBB 1000 WP SOL","Warm water cylinder SBB 1000 WP SOL","Ballon ECS solaire 835 litres SBB 1000 WP SOL ","Accumulatore solare SBB 1000 WP SOL","Warmwaterboiler SBB 1000 WP SOL","zásobník teplé vody SBB 1000 WP SOL","Zásobníkový ohrievač vody SBB 1000 WP SOL","Zasobnik ciepłej wody SBB 1000 WP SOL","Melegvíztároló SBB 1000 WP SOL","Käyttövesivaraaja SBB 1000 WP SOL","Varmtvandsbeholder SBB 1000 WP SOL","SBB 1000 WP SOL"]
[null,231957,"Thermal insulation WDH 600 SBB",576,{"$f":"IF(O66=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,231957,"Thermal insulation WDH 600 SBB",576,false,null,231957,584,576,740,3837,584,"Wärmedämmung WDH 600 SBB","Thermal insulation WDH 600 SBB","Isolation WDH 600 SBB pour SBB 600 WP SOL","Isolazione WDH 600 SBB","Isolatie WDH 600 SBB","tepelná izolace WDH 600 SBB","Tepelná izolácia WDH 600 SBB","Ocieplenie WDH 600 SBB","Hőszigetelés WDH 600 SBB","Lämmöneristys WDH 600  SBB","Isolering til varmtvandsbeholder WDH 600 SBB","WDH 600 SBB"]
[null,231958,"Thermal insulation WDH 800 SBB",610,"",null,null,null,null,null,null,231958,"Thermal insulation WDH 800 SBB",610,{"$f":"IF(AND(B67=L67,C67=M67,D67=N67),FALSE,TRUE)","v":false},null,231958,611,610,785,4068,611,"Wärmedämmung WDH 800 SBB","Thermal insulation WDH 800 SBB","Isolation WDH 800 SBB pour SBB 800 WP SOL","Isolazione WDH 800 SBB","Isolatie WDH 800 SBB","tepelná izolace WDH 800 SBB","Tepelná izolácia WDH 800 SBB","Ocieplenie WDH 800 SBB","Hőszigetelés WDH 800 SBB","Lämmöneristys WDH 800  SBB","Isolering til varmtvandsbeholder WDH 800 SBB","WDH 800 SBB"]
[null,231959,"Thermal insulation WDH 1000 SBB",674,"",null,null,null,null,null,null,231959,"Thermal insulation WDH 1000 SBB",674,false,null,231959,678,674,870,4492,678,"Wärmedämmung WDH 1000 SBB","Thermal insulation WDH 1000 SBB","Isolation WDH 1000 SBB pour SBB 1000 WP SOL","Isolazione WDH 1000 SBB","Isolatie WDH 1000 SBB","tepelná izolace WDH 1000 SBB","Tepelná izolácia WDH 1000 SBB","Ocieplenie WDH 1000 SBB","Hőszigetelés WDH 1000 SBB","Lämmöneristys WDH 1000  SBB","Isolering til varmtvandsbeholder WDH 1000 SBB","WDH 1000 SBB"]
[null,229984,"Instantaneous cylinder SBS 601 W SOL",2628,"",null,null,null,null,null,null,229984,"Instantaneous cylinder SBS 601 W SOL",2628,false,null,229984,2879,2628,"3.465,00",17210,2879,"Durchlaufspeicher SBS 601 W SOL","Instantaneous cylinder SBS 601 W SOL","Ballon solaire combiné SBS 601 W SOL ","Accumulatore istantaneo SBS 601 W SOL","Doorstroomboiler SBS 601 W SOL","průtokový zásobník SBS 601 W SOL","Prietokový zásobníkový ohrievač vody SBS 601 W SOL","Zasobnik przepływowy SBS 601 W SOL","Átfolyó jellegű HMV tároló SBS 601 W SOL","Läpivirtausvaraaja SBS 601 W SOL","Gennemstrømningsbeholder m. sol SBS 601 W SOL\n","SBS 601 W SOL"]
[null,229985,"Instantaneous cylinder SBS 801 W SOL",2876,"",null,null,null,null,null,null,229985,"Instantaneous cylinder SBS 801 W SOL",2876,false,null,229985,3150,2876,"3.630,00",18834,3150,"Durchlaufspeicher SBS 801 W SOL","Instantaneous cylinder SBS 801 W SOL","Ballon solaire combiné SBS 801 W SOL","Accumulatore istantaneo SBS 801 W SOL","Doorstroomboiler SBS 801 W SOL","průtokový zásobník SBS 801 W SOL","Prietokový zásobníkový ohrievač vody SBS 801 W SOL","Zasobnik przepływowy SBS 801 W SOL","Átfolyó jellegű HMV tároló SBS 801 W SOL","Läpivirtausvaraaja SBS 801 W SOL","Gennemstrømningsbeholder m. sol SBS 801 W SOL\n","SBS 801 W SOL"]
[null,229986,"Instantaneous cylinder SBS 1001 W SOL",3343,"",null,null,null,null,null,null,229986,"Instantaneous cylinder SBS 1001 W SOL",3343,false,null,229986,3661,3343,"4.060,00",21896,3661,"Durchlaufspeicher SBS 1001 W SOL","Instantaneous cylinder SBS 1001 W SOL","Ballon solaire combiné SBS 1001 W SOL","Accumulatore istantaneo SBS 1001 W SOL","Doorstroomboiler SBS 1001 W SOL","průtokový zásobník SBS 1001 W SOL","Prietokový zásobníkový ohrievač vody SBS 1001 W SOL","Zasobnik przepływowy SBS 1001 W SOL","Átfolyó jellegű HMV tároló SBS 1001 W SOL","Läpivirtausvaraaja SBS 1001 W SOL","Gennemstrømningsbeholder m. sol SBS 1001 W SOL\n","SBS 1001 W SOL"]
[null,229987,"Instantaneous cylinder SBS 1501 W SOL",3897,"",null,null,null,null,null,null,229987,"Instantaneous cylinder SBS 1501 W SOL",3897,false,null,229987,4267,3897,"4.875,00",25524,4267,"Durchlaufspeicher SBS 1501 W SOL","Instantaneous cylinder SBS 1501 W SOL","Ballon solaire combiné SBS 1501 W SOL","Accumulatore istantaneo SBS 1501 W SOL","Doorstroomboiler SBS 1501 W SOL","průtokový zásobník SBS 1501 W SOL","Prietokový zásobníkový ohrievač vody SBS 1501 W SOL","Zasobnik przepływowy SBS 1501 W SOL","Átfolyó jellegű HMV tároló SBS 1501 W SOL","Läpivirtausvaraaja SBS 1501 W SOL","Gennemstrømningsbeholder m. sol SBS 1501 W SOL\n","SBS 1501 W SOL"]
[null,231925,"Thermal insulation WDH 601 SBS",582,"",null,null,null,null,null,null,231925,"Thermal insulation WDH 601 SBS",582,false,null,231925,554,582,750,3881,554,"Wärmedämmung WDH 601 SBS","Thermal insulation WDH 601 SBS","Isolation renforcée WDH 601 SBS pour SBS 601 W (SOL)","Isolazione WDH 601 SBS","Isolatie WDH 601 SBS","tepelná izolace WDH 601 SBS","Tepelná izolácia WDH 601 SBS","Ocieplenie WDH 601 SBS","Hőszigetelés WDH 601 SBS","Lämmöneriste WDH 601 SBS","Isolering til gennemstrømningsbeholder WDH 601 SBS","WDH 601 SBS"]
[null,231926,"Thermal insulation WDH 801 SBS",610,"",null,null,null,null,null,null,231926,"Thermal insulation WDH 801 SBS",610,false,null,231926,610,610,785,4068,610,"Wärmedämmung WDH 801 SBS","Thermal insulation WDH 801 SBS","Isolation renforcée WDH 801 SBS pour SBS 801 W (SOL)","Isolazione WDH 801 SBS","Isolatie WDH 801 SBS","tepelná izolace WDH 801 SBS","Tepelná izolácia WDH 801 SBS","Ocieplenie WDH 801 SBS","Hőszigetelés WDH 801 SBS","Lämmöneriste WDH 801 SBS","Isolering til gennemstrømningsbeholder WDH 801 SBS","WDH 801 SBS"]
[null,231927,"Thermal insulation WDH 1001 SBS",674,"",null,null,null,null,null,null,231927,"Thermal insulation WDH 1001 SBS",674,false,null,231927,680,674,870,4492,680,"Wärmedämmung WDH 1001 SBS","Thermal insulation WDH 1001 SBS","Isolation renforcée WDH 1001 SBS pour SBS 1001 W (SOL)","Isolazione WDH 1001 SBS","Isolatie WDH 1001 SBS","tepelná izolace WDH 1001 SBS","Tepelná izolácia WDH 1001 SBS","Ocieplenie WDH 1001 SBS","Hőszigetelés WDH 1001 SBS","Lämmöneriste WDH 1001 SBS","Isolering til gennemstrømningsbeholder WDH 1001 SBS","WDH 1001 SBS"]
[null,231928,"Thermal insulation WDH 1501 SBS",769,"",null,null,null,null,null,null,231928,"Thermal insulation WDH 1501 SBS",769,false,null,231928,782,769,995,5133,782,"Wärmedämmung WDH 1501 SBS","Thermal insulation WDH 1501 SBS","Isolation renforcée WDH 1501 SBS pour SBS 1501 W (SOL)","Isolazione WDH 1501 SBS","Isolatie WDH 1501 SBS","tepelná izolace WDH 1501 SBS","Tepelná izolácia WDH 1501 SBS","Ocieplenie WDH 1501 SBS","Hőszigetelés WDH 1501 SBS","Lämmöneriste WDH 1501 SBS","Isolering til gennemstrømningsbeholder WDH 1501 SBS","WDH 1501 SBS"]
[null,230312,"DHW Circulation set ZW 1 1/4",94,"",null,null,null,null,null,null,230312,"DHW Circulation set ZW 1 1/4",94,false,null,230312,124,94,140,616,124,"Zirkulationsset Durchlaufspeicher ZW 1 1/4","DHW Circulation set ZW 1 1/4","Set de circulation ZW 1 1/4 pour ballons combinés SBS","Set di circolazione accumulatore combinato ZW 1 1/4","Circulatieset ZW 1 1/4","cirkulační sada k průtokovému zásobníku ZW 1 1/4","Cirkulačná sada pre prietokový zásobník ZW 1 1/4","DHW Circulation set ZW 1 1/4","Cirkulációs szett átfolyó jellegű HMV tárolóhoz ZW 1 1/4","Käyttöveden kiertokytkentä ZW 1 1/4","Brugsvandscirkulationskit til SBS ZW 1 1/4\n","ZW 1 1/4"]
[null,74067,"Combi cylinder SBK 600/150",3206,"",null,null,null,null,null,null,74067,"Combi cylinder SBK 600/150",3206,false,null,74067,2907,3206,"sur demande",20420,"op aanvraag","Kombispeicher SBK 600/150","Combi cylinder SBK 600/150","Ballon combiné SBK 600/150","Accumulatore comninato SBK 600/150","Combiboiler SBK 600/150","kombinovaný zásobník SBK 600/150","Kombinovaný zásobníkový ohrievač vody SBK 600/150","Zasobnik dwuwężownicowy  SBK 600/150","Kombitároló SBK 600/150","Yhdistelmävaraaja SBK 600/150","Kombibeholder, solar SBK 600/150\n","SBK 600/150"]
[null,185460,"Buffer cylinder SBP 700 E SOL",1652,"",null,null,null,null,null,null,185460,"Buffer cylinder SBP 700 E SOL",1652,false,null,185460,1799,1652,"2.100,00",10408,1799,"Pufferspeicher SBP 700 E SOL","Buffer cylinder SBP 700 E SOL","Ballon tampon solaire 700 litres SBP 700 E SOL","Accumulatore SBP 700 E SOL","Buffervat SBP 700 E SOL","akumulační zásobník SBP 700 E SOL","Akumulačný zásobník SBP 700 E SOL","Bufor SBP 700 E SOL","Puffertároló SBP 700 E SOL","Puskurivaraaja SBP 700 E SOL","Bufferbeholder m. sol SBP 700 E SOL\n","SBP 700 E SOL"]
[null,227566,"Buffer cylinder SBP 1000 E SOL",2181,"",null,null,null,null,null,null,227566,"Buffer cylinder SBP 1000 E SOL",2181,false,null,227566,1849,2181,"2.365,00",13142,1849,"Pufferspeicher SBP 1000 E SOL","Buffer cylinder SBP 1000 E SOL","Ballon tampon solaire 1000 litres  SBP 1000 E SOL","Accumulatore SBP 1000 E SOL","Buffervat SBP 1000 E SOL","akumulační zásobník SBP 1000 E SOL","Akumulačný zásobník SBP 1000 E SOL","Bufor SBP 1000 E SOL","Puffertároló SBP 1000 E SOL","Puskurivaraaja SBP 1000 E SOL","Bufferbeholder m. sol SBP 1000  E SOL\n","SBP 1000 E SOL"]
[null,227567,"Buffer cylinder SBP 1500 E SOL",2564,"",null,null,null,null,null,null,227567,"Buffer cylinder SBP 1500 E SOL",2564,false,null,227567,2115,2564,"2.750,00",14729,2115,"Pufferspeicher SBP 1500 E SOL","Buffer cylinder SBP 1500 E SOL","Ballon tampon solaire 1500 litres SBP 1500 E SOL","Accumulatore SBP 1500 E SOL","Buffervat SBP 1500 E SOL","akumulační zásobník SBP 1500 E SOL","Akumulačný zásobník SBP 1500 E SOL","Bufor SBP 1500 E SOL","Puffertároló SBP 1500 E SOL","Puskurivaraaja SBP 1500 E SOL","Bufferbeholder m. sol SBP 1500  E SOL\n","SBP 1500 E SOL"]
[null,231929,"Thermal insulation WDH 1000 SBP",661,"",null,null,null,null,null,null,231929,"Thermal insulation WDH 1000 SBP",661,false,null,231929,689,661,800,4232,689,"Wärmedämmung WDH 1000 SBP","Thermal insulation WDH 1000 SBP","Isolation renforcée WDH 1000 SBP pour SBP 1000 E (SOL)","Isolazione WDH 1000 SBP","Isolatie WDH 1000 SBP","tepelná izolace WDH 1000 SBP","Tepelná izolácia WDH 1000 SBP","Ocieplenie WDH 1000 SBP","Hőszigetelés WDH 1000 SBP","Lämmöneriste WDH 1000 SBP","Isolering til bufferbeholder WDH 1000 SBP","WDH 1000 SBP"]
[null,231930,"Thermal insulation WDH 1500 SBP",761,"",null,null,null,null,null,null,231930,"Thermal insulation WDH 1500 SBP",761,false,null,231930,785,761,940,4865,785,"Wärmedämmung WDH 1500 SBP","Thermal insulation WDH 1500 SBP","Isolation renforcée WDH 1500 SBP pour SBP 1500 E (SOL)","Isolazione WDH 1500 SBP","Isolatie WDH 1500 SBP","tepelná izolace WDH 1500 SBP","Tepelná izolácia WDH 1500 SBP","Ocieplenie WDH 1500 SBP","Hőszigetelés WDH 1500 SBP","Lämmöneriste WDH 1500 SBP","Isolering til bufferbeholder WDH 1500 SBP","WDH 1500 SBP"]
[null,73221,"Heat transfer liquid H30-L, 10 l",41,"",null,null,null,null,null,null,73221,"Heat transfer liquid H30-L, 10 l",41,false,null,73221,42,41,"sur demande",245,42,"Wärmeträger-Flüssigkeit H30-L, 10 l","Heat transfer liquid H30-L, 10 l","Fluide caloporteur H30-L, 10 litres","Acqua glicolata H30-L, 10 l","Warmtedragervloeistof H-30 L, 10 liter","teplonosná kapalina H30-L, 10l","Teplonosná nemrznúca kvapalina H30-L, 10 l","Medium  H30-L, 10 l","Folyékony hőközvetítő közeg H30-L, 10 l","Lämmönsiirtoneste H30-L, 10L","Termisk væske H-30  L, 10 litres\n","H30-L, 10 l"]
[null,73222,"Heat transfer liquid H30-L, 20 l",79,"",null,null,null,null,null,null,73222,"Heat transfer liquid H30-L, 20 l",79,false,null,73222,81,79,"sur demande",470,81,"Wärmeträger-Flüssigkeit H30-L, 20 l","Heat transfer liquid H30-L, 20 l","Fluide caloporteur H30-L, 20 litres","Acqua glicolata H30-L, 20 l","Warmtedragervloeistof H-30 L, 20 liter","teplonosná kapalina H30-L, 20l","Teplonosná nemrznúca kvapalina H30-L, 20 l","Medium H30-L, 20 l","Folyékony hőközvetítő közeg H30-L, 20 l","Lämmönsiirtoneste H30-L, 20L","Termisk væske H-30  L, 20 litres\n","H30-L, 20 l"]
[null,74099,"Heat transfer liquid H30-LS, 10 l",51,"",null,null,null,null,null,null,74099,"Heat transfer liquid H30-LS, 10 l",51,false,null,74099,52,51,80,295,52,"Wärmeträger-Flüssigkeit H30-LS, 10 l","Heat transfer liquid H30-LS, 10 l","Fluide caloporteur H30-LS, 10 litres","Acqua glicolata H30-LS, 10 l","Warmtedragervloeistof H-30 LS, 10 liter","teplonosná kapalina H30-LS, 10l","Teplonosná nemrznúca kvapalina H30-LS, 10 l","Medium H30-LS, 10 l","Folyékony hőközvetítő közeg H30-LS, 10 l","Lämmönsiirtoneste H30-L, 10L","Termisk væske H-30 LS, 10 litres\n","H30-LS, 10 l"]
[null,74100,"Heat transfer liquid H30-LS, 20 l",99,"",null,null,null,null,null,null,74100,"Heat transfer liquid H30-LS, 20 l",99,false,null,74100,88,99,140,590,88,"Wärmeträger-Flüssigkeit H30-LS, 20 l","Heat transfer liquid H30-LS, 20 l","Fluide caloporteur H30-LS, 20 litres","Acqua glicolata H30-LS, 20 l","Warmtedragervloeistof H-30 LS, 20 liter","teplonosná kapalina H30-LS, 20l","Teplonosná nemrznúca kvapalina H30-LS, 20 l","Medium H30-LS, 20 l","Folyékony hőközvetítő közeg H30-LS, 20 l","Lämmönsiirtoneste H30-L, 20L","Termisk væske H-30 LS, 20 litres\n","H30-LS, 20 l"]
[null,154700,"Antifreeze tester H-30 L",39,"",null,null,null,null,null,null,154700,"Antifreeze tester H-30 L",39,false,null,154700,37.5,39,"sur demande",213,38,"Frostschutz-Prüfer H-30 L","Antifreeze tester H-30 L","Testeur d'antigel H-30 L","Controllo protezione antigelo H-30 L","H-30 L Vorstbeschermingstester","zkoušečka nemrznoucí směsi H-30 L","Zariadenie na kontrolu ochrany proti mrazu H-30 L","Anti Freeze Tester H-30 L","Fagyvédelem ellenőrző H-30 L","Jäätymisenestokoestin H-30 L","Antifrosttester til H-30 L Antifrosttester H-30  L\n","H-30 L"]
[null,231015,"Absorption-air seperator SOL LA",154,"",null,null,null,null,null,null,231015,"Absorption-air seperator SOL LA",154,false,null,231015,131,154,235,1073,131,"Absorptions-Luftabscheider SOL LA","Absorption-air seperator SOL LA","Dégazeur en laiton pour installations solaires SOL LA","Separatore d'aria SOL LA","Luchtafscheider SOL LA","absorpční odvzdušňovač SOL LA","Absorpčný odlučovač vzduchu SOL LA","Absorption-Air Seperator SOL LA","Abszorpciós levegőleválasztó SOL LA","Absorptio-ilmanerotin SOL LA","Absorptions luftudskiller SOL LA","SOL LA"]
[null,231898,"Quick-action air vent valve SOL SE",84,"",null,null,null,null,null,null,231898,"Quick-action air vent valve SOL SE",84,false,null,231898,56,84,125,397,56,"Automatischer Schnellentlüfter SOL SE","Quick-action air vent valve SOL SE","Purgeur automatique SOL SE","Quick-action air vent valve SOL SE","Snelontluchter SOL SE","Quick-action air vent valve SOL SE","Quick-action air vent valve SOL SE","Quick-action air vent valve SOL SE","Quick-action air vent valve SOL SE","Quick-action air vent valve SOL SE","Automatisk quick-udlufter SOL SE","SOL SE"]
[null,231979,"Pre-cooling vessel VAG 12",67,"",null,null,null,null,null,null,231979,"Pre-cooling vessel VAG 12",67,false,null,231979,93,67,105,460,93,"Vorschaltgefäß 12 l","Pre-cooling vessel VAG 12","Vase tampon solaire VAG 12 pour vase d'expansion solaire ","Vorschaltgefäß 12 l","Voorschakelvat VAG 12","Vorschaltgefäß 12 l","Vorschaltgefäß 12 l","Vorschaltgefäß 12 l","Vorschaltgefäß 12 l","Vorschaltgefäß 12 l","Pre-kølebeholder VAG 12","Vorschaltgefäß 12 l"]
[null,74029,"Solar expansion vessel 12 l",63,"",null,null,null,null,null,null,74029,"Solar expansion vessel 12 l",63,false,null,74029,98,63,95,366,98,"Solar-Ausdehnungsgefäß 12 l","Solar expansion vessel 12 l","Vase d'expansion solaire 12 litres, AG 12","Vaso espansione solare 12 l","Membraan-drukexpansievat AG 12","solární expanzní nádoba 12 l","Expanzná nádoba pre solárny systém 12 l","Naczynie zbiorcze solara 12 l","Solar tágulási tartály 12 l","Paisunta-astia / aurinko 12 L","Ekspansionsbeholder 12 liter, solar AG 12\n","12 l"]
[null,74030,"Solar expansion vessel 18 l",69,"",null,null,null,null,null,null,74030,"Solar expansion vessel 18 l",69,false,null,74030,104,69,100,437,104,"Solar-Ausdehnungsgefäß 18 l","Solar expansion vessel 18 l","Vase d'expansion solaire 18 litres, AG 18","Vaso espansione solare 18 l","Membraan-drukexpansievat AG 18","solární expanzní nádoba 18 l","Expanzná nádoba pre solárny systém 18 l","Naczynie zbiorcze solara 18 l","Solar tágulási tartály 18 l","Paisunta-astia / aurinko 18 L","Ekspansionsbeholder 18 liter, solar AG 18\n","18 l"]
[null,74031,"Solar expansion vessel 25 l",80,"",null,null,null,null,null,null,74031,"Solar expansion vessel 25 l",80,false,null,74031,113,80,115,505,113,"Solar-Ausdehnungsgefäß 25 l","Solar expansion vessel 25 l","Vase d'expansion solaire 25 litres, AG 25","Vaso espansione solare 25 l","Membraan-drukexpansievat AG 25","solární expanzní nádoba 25 l","Expanzná nádoba pre solárny systém 25 l","Naczynie zbiorcze solara 25 l","Solar tágulási tartály 25 l","Paisunta-astia / aurinko 25 L","Ekspansionsbeholder 25 liter, solar AG 25\n","25 l"]
[null,187868,"Solar expansion vessel 50 l",171,"",null,null,null,null,null,null,187868,"Solar expansion vessel 50 l",171,false,null,187868,185,171,230,1021,185,"Solar-Ausdehnungsgefäß 50 l","Solar expansion vessel 50 l","Vase d'expansion solaire 50 litres, AG 50","Vaso espansione solare 50 l","Membraan-drukexpansievat AG 50","solární expanzní nádoba 50 l","Expanzná nádoba pre solárny systém 50 l","Naczynie zbiorcze solara 50 l","Solar tágulási tartály 50 l","Paisunta-astia / aurinko 50 L","Ekspansionsbeholder 50 liter, solar AG 50\n","50 l"]
[null,231899,"Solar expansion vessel 80 l",236,"",null,null,null,null,null,null,231899,"Solar expansion vessel 80 l",236,false,null,231899,245,236,360,1617,245,"Solar-Ausdehnungsgefäß 80 l","Solar expansion vessel 80 l","Vase d'expansion solaire 80 litres, AG 80","Vaso espansione solare 80 l","Membraan-drukexpansievat AG 80","solární expanzní nádoba 80 l","Expanzná nádoba pre solárny systém 80 l","Naczynie zbiorcze solara 80 l","Solar tágulási tartály 80 l","Paisunta-astia / aurinko 80 L","Ekspansionsbeholder 80 liter, solar AG 80\n","80 l"]
[null,231905,"DEV connection set AGWH",46,"",null,null,null,null,null,null,231905,"DEV connection set AGWH",46,false,null,231905,43,46,70,315,43,"Wandhalterung Solar-Ausdehnungsgefäß AGWH","DEV connection set AGWH","Support mural AG WH pour vase d’expansion","DEV connection set AGWH","MAG aansluitset AGWH","DEV connection set AGWH","DEV connection set AGWH","DEV connection set AGWH","DEV connection set AGWH","DEV connection set AGWH","Vægmonteringskit ekspansionsbeholder AGWH","AGWH"]
[null,70633,"Heat exchanger WT 10",778,"",null,null,null,null,null,null,70633,"Heat exchanger WT 10",778,false,null,70633,944,778,820,"på forespørgsel",944,"Wärmetauscher WT 10","Heat exchanger WT 10","Echangeur de chaleur WT 10","Scambiatore WT 10","Warmtewisselaar WT 10","tepelný výměník WT 10","Doskový výmenník tepla WT 10","Wymiennik ciepła  WT 10","Hőcserélő WT 10","Levylämmönvaihdin WT 10","Varmeveksler 10 kW WT 10\n","WT 10"]
[null,70634,"Heat exchanger WT 20",809,"",null,null,null,null,null,null,70634,"Heat exchanger WT 20",809,false,null,70634,1290,809,880,"på forespørgsel",1290,"Wärmetauscher WT 20","Heat exchanger WT 20","Echangeur de chaleur WT 20","Scambiatore WT 20","Warmtewisselaar WT 20","tepelný výměník WT 20","Doskový výmenník tepla WT 20","Wymiennik ciepła  WT 20","Hőcserélő WT 20","Levylämmönvaihdin WT 20","Varmeveksler 20 kW WT 20\n","WT 20"]
[null,71091,"Heat exchanger WT 30",1291,"",null,null,null,null,null,null,71091,"Heat exchanger WT 30",1291,false,null,71091,1609,1291,"1.400,00","på forespørgsel",1609,"Wärmetauscher WT 30","Heat exchanger WT 30","Echangeur de chaleur WT 30","Scambiatore WT 30","Warmtewisselaar WT 30","tepelný výměník WT 30","Doskový výmenník tepla WT 30","Wymiennik ciepła  WT 30","Hőcserélő WT 30","Levylämmönvaihdin WT 30","Varmeveksler 30 kW WT 30\n","WT 30"]
[null,229338,"Heat exchanger WT 40",1787,"",null,null,null,null,null,null,229338,"Heat exchanger WT 40",1787,false,null,229338,1948,1787,"1.495,00",12710,1948,"Wärmetauscher WT 40","Heat exchanger WT 40","Echangeur de chaleur WT 40","Scambiatore WT 40","Warmtewisselaar WT 40","tepelný výměník WT 40","Doskový výmenník tepla WT 40","Wymiennik ciepła  WT 40","Hőcserélő WT 40","Levylämmönvaihdin WT 40","Varmeveksler 40 kW WT 40\n","WT 40"]
[null,75115,"Threaded immersion heater BGC/45",238,"",null,null,null,null,null,null,75115,"Threaded immersion heater BGC/45",238,false,null,75115,399,238,335,1565,399,"Einschraubheizkörper BGC","Threaded immersion heater BGC/45","Corps de chauffe à visser BGC","Resistenza elettrica BGC","Verwarmingselement BGC/45","šroubovací topné těleso BGC","Skrutkovacie teleso BGC","Electric threaded immersion heater BGC","Becsavarható fűtőelem BGC","Sähkövastus BGC","Elektrisk varmelegeme BGC/45\n","BGC"]
[null,74233,"Pipe assembly WPRB",78,"",null,null,null,null,null,null,74233,"Pipe assembly WPRB",78,false,null,74233,107,78,115,467,107,"Rohrbausatz für elektr. Nacherwärmung WPRB","Pipe assembly WPRB","Tube d'adaptation pour BGC, WPRB","Tubo di raccordo per resistenza elettrica WPRB","Buiskit WPRB buiskit","konstrukční sada pro el.dohřev WPRB","Nadstavec pre el. Doohrev WPRB","Pipe assembly WPRB WPRB","Csőkészlet elektromos utófűtőhöz WPRB","Putkiasennussarja WPRB","Rørsæt til BGC elpatron WPRB rørsæt","WPRB"]
[null,229322,"Collector sensor pocket KTH basic",36,"",null,null,null,null,null,null,229322,"Collector sensor pocket KTH basic",36,false,null,229322,19.3,36,55,147,19,"Kollektortauchhülse KTH basic","Collector sensor pocket KTH basic","Doigt de gant KTH-B","guaina sonda collettore KTH basic","Collectordompelbuis KTH basic","kolektorová jímka KTH basic","Ponorná rúrka kolektora KTH basic","Tuleja zanużeniowa kolektora  KTH basic","Kollektor merülőhüvely KTH basic","Keräimen anturitasku KTH basic","Følerlomme til SOL 27 basic KTH basic\n","KTH basic"]
[null,73469,"Corrugated stainless steel hose",73,"",null,null,null,null,null,null,73469,"Corrugated stainless steel hose",73,false,null,73469,98,73,105,450,98,"Edelstahl-Wellschlauch","Corrugated stainless steel hose","Tuyau souple SOL SL pour passage de toiture ","tubo flessibile in acciaio ondulato","RVS geribbelde slang","ocelová vlnová hadice","Nerezová vlnitá hadica","Wąż z nierdzewnej  blachy falistej","Rozsdamentes acél flexicső","RST haitariletku","Flexslange, rustfrit stål Flexslange, rustfrit stål","Edelstahl-Wellschlauch"]
[null,231900,"Three-way diverter valve SUV",130,"",null,null,null,null,null,null,231900,"Three-way diverter valve SUV",130,false,null,231900,136,130,185,820,136,"3-Wege-Umschaltventil mit Stellantrieb SUV","Three-way diverter valve SUV","Vanne d’inversion à 3 voies, SUV","Valvola a 3 vie SUV","3-Weg klep SUV","3-cestný přepínací ventil SUV","Trojcestný zmiešavací ventil SUV","zawór 3-drogowy SUV","3 járatú váltószelep SUV","Vaihtoventtiili, 3-tie SUV","3-vejsventil SUV","3-Wege-Umschaltventil SUV"]
[null,74244,"Regulating valve with flowmeter",69,"",null,null,null,null,null,null,74244,"Regulating valve with flowmeter",69,false,null,74244,109,69,100,463,109,"Strang-Regulierventil mit Durchflussmesser","Regulating valve with flowmeter","Contrôleur de débit avec débitmètre incorporé, DFM","misuratore di volume","Debietmeter DFM","větvový regulační ventil s průtokoměrem","Trojcestný prepínací ventil (zo strany stavby)","Zawór regulacyjny narurowy z przepływomierzem","Strangszabályozó szelep átfolyásmérővel","Säätöventtiili virtausmittarilla","Reguleringsventil med flowmeter DFM\n","Strang-Regulierventil mit Durchflussmesser"]
[null,73864,"Central-Thermostat ZTA 3/4",103,"",null,null,null,null,null,null,73864,"Central-Thermostat ZTA 3/4",103,false,null,73864,101,103,150,"på forespørgsel",101,"Zentral-Thermostat ZTA 3/4","Central-Thermostat ZTA 3/4","Mitigeur thermostatique ZTA 3/4","Termostato principale ZTA 3/4","Thermostaat armatuur ZTA 3/4","centrální termostat ZTA 3/4","Centrálny termostat ZTA 3/4","Central-Thermostat ZTA 3/4","Központi termosztát ZTA 3/4","Keskustermostaatti ZTA 3/4","Tilbehør DHE ZTA 3/4\n","ZTA 3/4"]
[null,232944,"Flexible solar pipe SFR 10, DN 20 10m",413,"",null,null,null,null,null,null,232944,"Flexible solar pipe SFR 10, DN 20 10m",413,false,null,232944,483,413,595,2771,483,"Solar-Flexrohr DN 20, 10m","Flexible solar pipe SFR 10, DN 20 10m","Tuyaux flexibles solaires SFR 10, DN 20 10m","Tubo flessibile Solare SFR 10, DN 20 10m","Flexibele Solarbuis DN 20, 10m","solární flexibilní potrubí SFR 10, DN 20 - 10m","Ohybná hadica pre solárny systém DN 20, 10m","Flexible solar pipe SFR 10, DN 20 10m","Solar flexicső SFR 10, DN 20 10m","Joustava lämmönsiirtoputkisto SFR 10, DN 20 10m","Solfanger flexrør SFR 10, DN 20 10m","SFR 10, DN 20 10m"]
[null,232945,"Flexible solar pipe SFR 15, DN 20 15m",585,"",null,null,null,null,null,null,232945,"Flexible solar pipe SFR 15, DN 20 15m",585,false,null,232945,695,585,825,3926,695,"Solar-Flexrohr DN 20, 15m","Flexible solar pipe SFR 15, DN 20 15m","Tuyaux flexiblex solaires SFR 15, DN 20 15m","Tubo flessibile Solare SFR 15, DN 20 15m","Flexibele Solarbuis DN 20, 15m","solární flexibilní potrubí SFR 15, DN 20 - 15m","Ohybná hadica pre solárny systém DN 20, 15m","Flexible solar pipe SFR 15, DN 20 15m","Solar flexicső SFR 15, DN 20 15m","Joustava lämmönsiirtoputkisto SFR 15, DN 20 15m","Solfanger flexrør SFR 15, DN 20 15m","SFR 15, DN 20 15m"]
[null,232946,"Flexible solar pipe SFR 20, DN 20 20m",757,"",null,null,null,null,null,null,232946,"Flexible solar pipe SFR 20, DN 20 20m",757,false,null,232946,904,757,"1.080,00",5081,904,"Solar-Flexrohr DN 20, 20m","Flexible solar pipe SFR 20, DN 20 20m","Tuyaux flexiblex solaires SFR 20, DN 20 20m","Tubo flessibile Solare SFR 20, DN 20 20m","Flexibele Solarbuis DN 20, 20m","solární flexibilní potrubí SFR 20, DN 20 - 20m","Ohybná hadica pre solárny systém DN 20, 20m","Flexible solar pipe SFR 20, DN 20 20m","Solar flexicső SFR 20, DN 20 20m","Joustava lämmönsiirtoputkisto SFR 20, DN 20 20m","Solfanger flexrør SFR 20, DN 20 20m","SFR 20, DN 20 20m"]
[null,232947,"Flexible solar pipe SFR 25, DN 20 25m",929,"",null,null,null,null,null,null,232947,"Flexible solar pipe SFR 25, DN 20 25m",929,false,null,232947,1113,929,"1.320,00",6236,1113,"Solar-Flexrohr DN 20, 25m","Flexible solar pipe SFR 25, DN 20 25m","Tuyaux flexiblex solaires SFR 25, DN 20 25m","Tubo flessibile Solare SFR 25, DN 20 25m","Flexibele Solarbuis DN 20, 25m","solární flexibilní potrubí SFR 25, DN 20 - 25m","Ohybná hadica pre solárny systém DN 20, 25m","Flexible solar pipe SFR 25, DN 20 25m","Solar flexicső SFR 25, DN 20 25m","Joustava lämmönsiirtoputkisto SFR 25, DN 20 25m","Solfanger flexrør SFR 25, DN 20 25m","SFR 25, DN 20 25m"]
[null,231906,"Collector handle set KGS",210,"",null,null,null,null,null,null,231906,"Collector handle set KGS",210,false,null,231906,126,210,310,1468,126,"Kollektorgriffset KGS zur Montagehilfe","Collector handle set KGS","Poignées pour transports de capteurs solaires, KGS","Collector handle set KGS","Collector-grepen KGS","Collector handle set KGS","Collector handle set KGS","Collector handle set KGS","Collector handle set KGS","Collector handle set KGS","Panelhåndteringssæt KGS","Kollektorgriffset KGS zur Montagehilfe"]
[null,221387,"Solar set basic 150/1",2678,"",null,null,null,null,null,null,221387,"Solar set basic 150/1",2678,false,null,221387,2717,2678,"sur demande",18752,2717,"Solarset Basic 150/1","Solar set basic 150/1","Kit solaire 150/2","Solarset Basic 150/3","Solarset Zonneset Basic 150/1","Solarset Basic 150/1","Solarset Basic 150/1","Solarset Basic 150/2","Solarset Basic 150/2","Solarset Basic 150/2","Solfangersæt basic 150/1"]
[null,221388,"Solar set basic 300/2",3863,"",null,null,null,null,null,null,221388,"Solar set basic 300/2",3863,false,null,221388,3583,3863,"sur demande",29241,3583,"Solarset Basic 300/2","Solar set basic 300/2","Kit solaire 300/3","Solarset Basic 300/3","Solarset Zonneset Basic 300/2","Solarset Basic 300/2","Solarset Basic 300/2","Solarset Basic 300/3","Solarset Basic 300/3","Solarset Basic 300/3","Solfangersæt basic 300/2"]
[null,230145,"LWZ 304 SOL SET","On request","",null,null,null,null,null,null,230145,"LWZ 304 SOL SET","On request",false,null,230145,16300,"On request","16.900,00","på forespørgsel",16300,"Integralgerät mit Solar LWZ 304 SOL SET","LWZ 304 SOL SET","SET LWZ 304 SOL","LWZ 304 SOL SET","Centraal ventilatietoestel  LWZ 304 SOL Set","LWZ 304 SOL SET","LWZ 304 SOL SET","LWZ 304 SOL SET","LWZ 304 SOL SET","LWZ 304 SOL SET","LWZ 304 SOL SET"]
[null,230146,"LWZ 404 SOL SET","On request","",null,null,null,null,null,null,230146,"LWZ 404 SOL SET","On request",false,null,230146,16940,"On request","17.650,00","på forespørgsel",16940,"Integralgerät mit Solar LWZ 404 SOL SET","LWZ 404 SOL SET","SET LWZ 404 SOL","LWZ 404 SOL SET","Centraal ventilatietoestel  LWZ 404 SOL Set","LWZ 404 SOL SET","LWZ 404 SOL SET","LWZ 404 SOL SET","LWZ 404 SOL SET","LWZ 404 SOL SET","LWZ 404 SOL SET"]
[null,228839,"Solar set basic WP",2421,"",null,null,null,null,null,null,228839,"Solar set basic WP",2421,false,null,228839,2619,2421,"sur demande",16956,2619,"Solar-Set Basic WP","Solar set basic WP","Kit solaire Basic WP","Solar-Set Basic WP","Solarset Zonneset Basic WP","Solar-Set Basic WP","Solar-Set Basic WP","Solar-Set Basic WP","Solar-Set Basic WP","Solar-Set Basic WP","Solfangersæt basic VP"]
[null,230152,"Solar set SBB 401 WP SOL",4292,"",null,null,null,null,null,null,230152,"Solar set SBB 401 WP SOL",4292,false,null,230152,4918,4292,"sur demande",30061,4918,"Solar-Set SBB 401 WP SOL","Solar set SBB 401 WP SOL","Kit solaire SBB 401 WP SOL","Solar-Set SBB 401 WP SOL","Solarset Zonneset SBB 401 WP SOL","Solar-Set SBB 401 WP SOL","Solar-Set SBB 401 WP SOL","Solar-Set SBB 401 WP SOL","Solar-Set SBB 401 WP SOL","Solar-Set SBB 401 WP SOL","Solfangersæt SBB 401 WP SOL"]
[null,230153,"Solar set SBB 501 WP SOL",5610,"",null,null,null,null,null,null,230153,"Solar set SBB 501 WP SOL",5610,false,null,230153,5983,5610,"sur demande",39291,5983,"Solar-Set SBB 501 WP SOL","Solar set SBB 501 WP SOL","Kit solaire SBB 501 WP SOL","Solar-Set SBB 501 WP SOL","Solarset Zonneset SBB 501 WP SOL","Solar-Set SBB 501 WP SOL","Solar-Set SBB 501 WP SOL","Solar-Set SBB 501 WP SOL","Solar-Set SBB 501 WP SOL","Solar-Set SBB 501 WP SOL","Solfangersæt SBB 401 WP SOL"]
[null,230156,"Solar set SBS 601 W SOL",7382,"",null,null,null,null,null,null,230156,"Solar set SBS 601 W SOL",7382,false,null,230156,7406,7382,"sur demande",51703,7406,"Solar-Set SBS 601 W SOL","Solar set SBS 601 W SOL","Kit solaire SBS 601 W SOL","Solar-Set SBS 601 W SOL","Solarset Zonneset SBS 601 W SOL","Solar-Set SBS 601 W SOL","Solar-Set SBS 601 W SOL","Solar-Set SBS 601 W SOL","Solar-Set SBS 601 W SOL","Solar-Set SBS 601 W SOL","Solfangersæt SBB 401 WP SOL"]
[null,230157,"Solar set SBS 801 W SOL",7511,"",null,null,null,null,null,null,230157,"Solar set SBS 801 W SOL",7511,false,null,230157,7732,7511,"sur demande",52604,7732,"Solar-Set SBS 801 W SOL","Solar set SBS 801 W SOL","Kit solaire SBS 801 W SOL","Solar-Set SBS 801 W SOL","Solarset Zonneset SBS 801 W SOL","Solar-Set SBS 801 W SOL","Solar-Set SBS 801 W SOL","Solar-Set SBS 801 W SOL","Solar-Set SBS 801 W SOL","Solar-Set SBS 801 W SOL","Solfangersæt SBB 401 WP SOL"]
[null,"------","Heating diverter valve (on side)",0,"",null,null,null,null,null,null,"------","Heating diverter valve (on side)",0,false,null,"------",0,0,"sur demande","på forespørgsel","op aanvraag","Heizungs-Umschaltventil (Bauseits)","Heating diverter valve (on side)","Vanne d'inversion chauffage","Valvola deviatrice","Verwarmings-Omschakelventiel (Bouwzijdig)","přepínací ventil vytápění (v rámci montáže)","přepínací ventil vytápění (v rámci montáže)","Zawór przełączający ogrzewania (po stronie Inwestora)","Fűtési váltószelep","Heating diverter valve (on side)","3-vejsventil (lev. af kunde)"]
[null,229908,"Air|water heat pump WPL 5 N plus",13276,{"$f":"IF(O124=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,229908,"Air|water heat pump WPL 5 N plus",13276,{"$f":"IF(AND(B124=L124,C124=M124,D124=N124),FALSE,TRUE)","v":false},null,229908,12708,13276,"sur demande",78620,12708,"Luft|Wasser-Wärmepumpe WPL 5 N plus","Air|water heat pump WPL 5 N plus","Air|water heat pump WPL 5 N plus","Air|water heat pump WPL 5 N plus","Lucht/water-warmtepompen WPL 5 N plus","Air|water heat pump WPL 5 N plus","Air|water heat pump WPL 5 N plus","Air|water heat pump WPL 5 N plus","Air|water heat pump WPL 5 N plus","Air|water heat pump WPL 5 N plus","Air|water heat pump WPL 5 N plus"]
[null,234759,"Luft|Wasser-Wärmepumpe WPL 15 ACS",8209,"",null,null,null,null,null,null,234759,"Luft|Wasser-Wärmepumpe WPL 15 ACS",8209,false,null,234759,9430,8209,"8.650,00",56228,9430,"Luft|Wasser-Wärmepumpe WPL 15 ACS","Luft|Wasser-Wärmepumpe WPL 15 ACS","Luft|Wasser-Wärmepumpe WPL 15 ACS","Luft|Wasser-Wärmepumpe WPL 15 ACS","Lucht/water-warmtepompen WPL 15 ACS","Luft|Wasser-Wärmepumpe WPL 15 AS","Luft|Wasser-Wärmepumpe WPL 15 AS","Luft|Wasser-Wärmepumpe WPL 15 AS","Luft|Wasser-Wärmepumpe WPL 15 AS","Luft|Wasser-Wärmepumpe WPL 15 AS","Luft|Wasser-Wärmepumpe WPL 15 AS"]
[null,234760,"Luft|Wasser-Wärmepumpe WPL 25 AC",9707,"",null,null,null,null,null,null,234760,"Luft|Wasser-Wärmepumpe WPL 25 AC",9707,false,null,234760,11424,9707,"10.190,00",59900,11424,"Luft|Wasser-Wärmepumpe WPL 25 AC","Luft|Wasser-Wärmepumpe WPL 25 AC","Luft|Wasser-Wärmepumpe WPL 25 AC","Luft|Wasser-Wärmepumpe WPL 25 AC","Lucht/water-warmtepompen WPL 25 AC","Luft|Wasser-Wärmepumpe WPL 25 A","Luft|Wasser-Wärmepumpe WPL 25 A","Luft|Wasser-Wärmepumpe WPL 25 A","Luft|Wasser-Wärmepumpe WPL 25 A","Luft|Wasser-Wärmepumpe WPL 25 A","Luft|Wasser-Wärmepumpe WPL 25 A"]
[null,231888,"Luft|Wasser-Wärmepumpe WPL 15 IS-2","On request","",null,null,null,null,null,null,231888,"Luft|Wasser-Wärmepumpe WPL 15 IS-2","On request",false,null,231888,11669,"On request","sur demande","på forespørgsel",11669,"Luft|Wasser-Wärmepumpe WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2","Lucht/water-warmtepompen WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2","Luft|Wasser-Wärmepumpe WPL 15 IS-2"]
[null,231889,"Luft|Wasser-Wärmepumpe WPL 25 I-2","On request","",null,null,null,null,null,null,231889,"Luft|Wasser-Wärmepumpe WPL 25 I-2","On request",false,null,231889,13642,"On request","sur demande","på forespørgsel",13642,"Luft|Wasser-Wärmepumpe WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2","Lucht/water-warmtepompen WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2","Luft|Wasser-Wärmepumpe WPL 25 I-2"]
[null,231886,"Air|water heat pump WPL 15","On request","",null,null,null,null,null,null,231886,"Air|water heat pump WPL 15","On request",false,null,231886,13694,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 15 IKS-2","Air|water heat pump WPL 15","Air|water heat pump WPL 15","Air|water heat pump WPL 15","Lucht/water-warmtepompen WPL 15 IKS-2","Air|water heat pump WPL 15","Air|water heat pump WPL 15","Air|water heat pump WPL 15","Air|water heat pump WPL 15","Air|water heat pump WPL 15","Air|water heat pump WPL 15"]
[null,231887,"Air|water heat pump WPL 25","On request","",null,null,null,null,null,null,231887,"Air|water heat pump WPL 25","On request",false,null,231887,16433,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 25 IK-2","Air|water heat pump WPL 25","Air|water heat pump WPL 25","Air|water heat pump WPL 25","Lucht/water-warmtepompen WPL 25 IK-2","Air|water heat pump WPL 25","Air|water heat pump WPL 25","Air|water heat pump WPL 25","Air|water heat pump WPL 25","Air|water heat pump WPL 25","Air|water heat pump WPL 25"]
[null,229938,"Air|water heat pump WPL 33 HT",15347,"",null,null,null,null,null,null,229938,"Air|water heat pump WPL 33 HT",15347,false,null,229938,14334,15347,"15.375,00",107116,14334,"Luft|Wasser-Wärmepumpe WPL 33 HT","Air|water heat pump WPL 33 HT","Air|water heat pump WPL 33 HT","Air|water heat pump WPL 33 HT","Lucht/water-warmtepompen WPL 33 HT","Air|water heat pump WPL 33 HT","Air|water heat pump WPL 33 HT","Air|water heat pump WPL 33 HT","Air|water heat pump WPL 33 HT","Air|water heat pump WPL 33 HT","Air|water heat pump WPL 33 HT"]
[null,230236,"Air|water heat pump WPL 10 AC",5778,"",null,null,null,null,null,null,230236,"Air|water heat pump WPL 10 AC",5778,false,null,230236,6816,5778,"7.120,00",40468,6816,"Luft|Wasser-Wärmepumpe WPL 10 AC","Air|water heat pump WPL 10 AC","Air|water heat pump WPL 10 AC","Air|water heat pump WPL 10 AC","Lucht/water-warmtepompen WPL 10 AC","Air|water heat pump WPL 10 AC","Air|water heat pump WPL 10 AC","Air|water heat pump WPL 10 AC","Air|water heat pump WPL 10 AC","Air|water heat pump WPL 10 AC","Air|water heat pump WPL 10 AC"]
[null,231788,"Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","On request","",null,null,null,null,null,null,231788,"Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","On request",false,null,231788,7200,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","WPL 10 AC - Actieset 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 1"]
[null,231789,"Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","On request","",null,null,null,null,null,null,231789,"Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","On request",false,null,231789,9450,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","WPL 10 AC - Actieset 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 2"]
[null,231790,"Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","On request","",null,null,null,null,null,null,231790,"Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","On request",false,null,231790,9100,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","WPL 10 AC - Actieset 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3","Luft|Wasser-Wärmepumpenset WPL 10 AC Set 3"]
[null,220811,"Air|water heat pump WPL 10 I",6127,"",null,null,null,null,null,null,220811,"Air|water heat pump WPL 10 I",6127,false,null,220811,8015,6127,"8.190,00",45117,8015,"Luft|Wasser-Wärmepumpe WPL 10 I","Air|water heat pump WPL 10 I","Air|water heat pump WPL 10 I","Air|water heat pump WPL 10 I","Lucht/water-warmtepompen WPL 10 I","Air|water heat pump WPL 10 I","Air|water heat pump WPL 10 I","Air|water heat pump WPL 10 I","Air|water heat pump WPL 10 I","Air|water heat pump WPL 10 I","Air|water heat pump WPL 10 I"]
[null,234655,"Air|water heat pump WPL 10 IK",8023,"",null,null,null,null,null,null,234655,"Air|water heat pump WPL 10 IK",8023,false,null,234655,10370,8023,"10.660,00",56143,10370,"Luft|Wasser-Wärmepumpe WPL 10 IK","Air|water heat pump WPL 10 IK","Air|water heat pump WPL 10 IK","Air|water heat pump WPL 10 IK","Lucht/water-warmtepompen WPL 10 IK","Air|water heat pump WPL 10 IK","Air|water heat pump WPL 10 IK","Air|water heat pump WPL 10 IK","Air|water heat pump WPL 10 IK","Air|water heat pump WPL 10 IK","Air|water heat pump WPL 10 IK"]
[null,227756,"Air|water heat pump WPL 13 E",8205,"",null,null,null,null,null,null,227756,"Air|water heat pump WPL 13 E",8205,false,null,227756,8309,8205,"9.380,00 ",38308,8309,"Luft|Wasser-Wärmepumpe WPL 13 E","Air|water heat pump WPL 13 E","Air|water heat pump WPL 13 E","Air|water heat pump WPL 13 E","Lucht/water-warmtepompen WPL 13 E","Air|water heat pump WPL 13 E","Air|water heat pump WPL 13 E","Air|water heat pump WPL 13 E","Air|water heat pump WPL 13 E","Air|water heat pump WPL 13 E","Air|water heat pump WPL 13 E"]
[null,227757,"Air|water heat pump WPL 18 E",8410,"",null,null,null,null,null,null,227757,"Air|water heat pump WPL 18 E",8410,false,null,227757,8976,8410,"9.720,00",41919,8976,"Luft|Wasser-Wärmepumpe WPL 18 E","Air|water heat pump WPL 18 E","Air|water heat pump WPL 18 E","Air|water heat pump WPL 18 E","Lucht/water-warmtepompen WPL 18 E","Air|water heat pump WPL 18 E","Air|water heat pump WPL 18 E","Air|water heat pump WPL 18 E","Air|water heat pump WPL 18 E","Air|water heat pump WPL 18 E","Air|water heat pump WPL 18 E"]
[null,227758,"Air|water heat pump WPL 23 E",8745,"",null,null,null,null,null,null,227758,"Air|water heat pump WPL 23 E",8745,false,null,227758,10461,8745,"10.050,00",45530,10461,"Luft|Wasser-Wärmepumpe WPL 23 E","Air|water heat pump WPL 23 E","Air|water heat pump WPL 23 E","Air|water heat pump WPL 23 E","Lucht/water-warmtepompen WPL 23 E","Air|water heat pump WPL 23 E","Air|water heat pump WPL 23 E","Air|water heat pump WPL 23 E","Air|water heat pump WPL 23 E","Air|water heat pump WPL 23 E","Air|water heat pump WPL 23 E"]
[null,223400,"Air|water heat pump WPL 13 cool",8368,"",null,null,null,null,null,null,223400,"Air|water heat pump WPL 13 cool",8368,false,null,223400,9408,8368,"10.720,00",54556,9408,"Luft|Wasser-Wärmepumpe WPL 13 cool","Air|water heat pump WPL 13 cool","Air|water heat pump WPL 13 cool","Air|water heat pump WPL 13 cool","Lucht/water-warmtepompen WPL 13 cool","Air|water heat pump WPL 13 cool","Air|water heat pump WPL 13 cool","Air|water heat pump WPL 13 cool","Air|water heat pump WPL 13 cool","Air|water heat pump WPL 13 cool","Air|water heat pump WPL 13 cool"]
[null,223401,"Air|water heat pump WPL 18 cool",8569,"",null,null,null,null,null,null,223401,"Air|water heat pump WPL 18 cool",8569,false,null,223401,10011,8569,"10.850,00",55167,10011,"Luft|Wasser-Wärmepumpe WPL 18 cool","Air|water heat pump WPL 18 cool","Air|water heat pump WPL 18 cool","Air|water heat pump WPL 18 cool","Lucht/water-warmtepompen WPL 18 cool","Air|water heat pump WPL 18 cool","Air|water heat pump WPL 18 cool","Air|water heat pump WPL 18 cool","Air|water heat pump WPL 18 cool","Air|water heat pump WPL 18 cool","Air|water heat pump WPL 18 cool"]
[null,223402,"Air|water heat pump WPL 23 cool",8881,"",null,null,null,null,null,null,223402,"Air|water heat pump WPL 23 cool",8881,false,null,223402,11460,8881,"11.290,00",57186,11460,"Luft|Wasser-Wärmepumpe WPL 23 cool","Air|water heat pump WPL 23 cool","Air|water heat pump WPL 23 cool","Air|water heat pump WPL 23 cool","Lucht/water-warmtepompen WPL 23 cool","Air|water heat pump WPL 23 cool","Air|water heat pump WPL 23 cool","Air|water heat pump WPL 23 cool","Air|water heat pump WPL 23 cool","Air|water heat pump WPL 23 cool","Air|water heat pump WPL 23 cool"]
[null,228835,"Air|water heat pump WPL 34 A",18229,"",null,null,null,null,null,null,228835,"Air|water heat pump WPL 34 A",18229,false,null,228835,15301,18229,"17.390,00",129600,15301,"Luft|Wasser-Wärmepumpe WPL 34","Air|water heat pump WPL 34 A","Air|water heat pump WPL 34 A","Air|water heat pump WPL 34 A","Lucht/water-warmtepompen WPL 34","Air|water heat pump WPL 34 A","Air|water heat pump WPL 34 A","Air|water heat pump WPL 34 A","Air|water heat pump WPL 34 A","Air|water heat pump WPL 34 A","Air|water heat pump WPL 34 A"]
[null,228836,"Air|water heat pump WPL 47 A",18710,"",null,null,null,null,null,null,228836,"Air|water heat pump WPL 47 A",18710,false,null,228836,16946,18710,"18.530,00",133012,16946,"Luft|Wasser-Wärmepumpe WPL 47","Air|water heat pump WPL 47 A","Air|water heat pump WPL 47 A","Air|water heat pump WPL 47 A","Lucht/water-warmtepompen WPL 47","Air|water heat pump WPL 47 A","Air|water heat pump WPL 47 A","Air|water heat pump WPL 47 A","Air|water heat pump WPL 47 A","Air|water heat pump WPL 47 A","Air|water heat pump WPL 47 A"]
[null,228837,"Air|water heat pump WPL 57 A",20309,"",null,null,null,null,null,null,228837,"Air|water heat pump WPL 57 A",20309,false,null,228837,18703,20309,"19.950,00",144381,18703,"Luft|Wasser-Wärmepumpe WPL 57","Air|water heat pump WPL 57 A","Air|water heat pump WPL 57 A","Air|water heat pump WPL 57 A","Lucht/water-warmtepompen WPL 57","Air|water heat pump WPL 57 A","Air|water heat pump WPL 57 A","Air|water heat pump WPL 57 A","Air|water heat pump WPL 57 A","Air|water heat pump WPL 57 A","Air|water heat pump WPL 57 A"]
[null,232124,"Air|water heat pump WPL 34 A SR",16245,"",null,null,null,null,null,null,232124,"Air|water heat pump WPL 34 A SR",16245,false,null,232124,15516,16245,"sur demande",111549,15516,"Luft|Wasser-Wärmepumpe WPL 34 Silber","Air|water heat pump WPL 34 A SR","Air|water heat pump WPL 34 A SR","Air|water heat pump WPL 34 A SR","Lucht/water-warmtepompen WPL 34 SR","Air|water heat pump WPL 34 A SR","Air|water heat pump WPL 34 A SR","Air|water heat pump WPL 34 A SR","Air|water heat pump WPL 34 A SR","Air|water heat pump WPL 34 A SR","Air|water heat pump WPL 34 A SR"]
[null,232125,"Air|water heat pump WPL 47 A SR",16862,"",null,null,null,null,null,null,232125,"Air|water heat pump WPL 47 A SR",16862,false,null,232125,17058,16862,"sur demande",115788,17058,"Luft|Wasser-Wärmepumpe WPL 47 Silber","Air|water heat pump WPL 47 A SR","Air|water heat pump WPL 47 A SR","Air|water heat pump WPL 47 A SR","Lucht/water-warmtepompen WPL 47 SR","Air|water heat pump WPL 47 A SR","Air|water heat pump WPL 47 A SR","Air|water heat pump WPL 47 A SR","Air|water heat pump WPL 47 A SR","Air|water heat pump WPL 47 A SR","Air|water heat pump WPL 47 A SR"]
[null,232126,"Air|water heat pump WPL 57 A SR",17408,"",null,null,null,null,null,null,232126,"Air|water heat pump WPL 57 A SR",17408,false,null,232126,18822,17408,"sur demande",119535,18822,"Luft|Wasser-Wärmepumpe WPL 57 Silber","Air|water heat pump WPL 57 A SR","Air|water heat pump WPL 57 A SR","Air|water heat pump WPL 57 A SR","Lucht/water-warmtepompen WPL 57 SR","Air|water heat pump WPL 57 A SR","Air|water heat pump WPL 57 A SR","Air|water heat pump WPL 57 A SR","Air|water heat pump WPL 57 A SR","Air|water heat pump WPL 57 A SR","Air|water heat pump WPL 57 A SR"]
[null,233749,"Hydraulikmodul HM",2640,"",null,null,null,null,null,null,233749,"Hydraulikmodul HM",2640,false,null,233749,2490,2640,"3.680,00",18084,2490,"Hydraulikmodul HM","Hydraulikmodul HM","Hydraulikmodul HM","Hydraulikmodul HM","Hydrauliekmodule HM","Hydraulikmodul HM","Hydraulikmodul HM","Hydraulikmodul HM","Hydraulikmodul HM","Hydraulikmodul HM","Hydraulikmodul HM"]
[null,232805,"Hydraulikmodul HM Trend",2160,"",null,null,null,null,null,null,232805,"Hydraulikmodul HM Trend",2160,false,null,232805,1990,2160,"2.410,00",14796,1990,"Hydraulikmodul HM Trend","Hydraulikmodul HM Trend","Hydraulikmodul HM Trend","Hydraulikmodul HM Trend","Hydrauliekmodule HM Trend","Hydraulikmodul HM Trend","Hydraulikmodul HM Trend","Hydraulikmodul HM Trend","Hydraulikmodul HM Trend","Hydraulikmodul HM Trend","Hydraulikmodul HM Trend"]
[null,232806,"Isonlierte Anschlussleiste ASL-HM",390,"",null,null,null,null,null,null,232806,"Isonlierte Anschlussleiste ASL-HM",390,false,null,232806,310,390,560,2671,310,"Isonlierte Anschlussleiste ASL-HM","Isonlierte Anschlussleiste ASL-HM","Isonlierte Anschlussleiste ASL-HM","Isonlierte Anschlussleiste ASL-HM","Geïsoleerde aansluitlijst ASL-HM","Isonlierte Anschlussleiste ASL-HM","Isonlierte Anschlussleiste ASL-HM","Isonlierte Anschlussleiste ASL-HM","Isonlierte Anschlussleiste ASL-HM","Isonlierte Anschlussleiste ASL-HM","Isonlierte Anschlussleiste ASL-HM"]
[null,233750,"Hydraulikmodul-Anschlussset AS-HM Trend",120,"",null,null,null,null,null,null,233750,"Hydraulikmodul-Anschlussset AS-HM Trend",120,false,null,233750,100,120,175,805,100,"Hydraulikmodul-Anschlussset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend","Hydrauliekmodule-Aansluitset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend","Hydraulikmodul-Anschlussset AS-HM Trend"]
[null,234264,"Speicher- und Hydraulikmodul HSBB 3",4000,"",null,null,null,null,null,null,234264,"Speicher- und Hydraulikmodul HSBB 3",4000,false,null,234264,3320,4000,"sur demande",22000,3320,"Speicher- und Hydraulikmodul HSBB 3","Speicher- und Hydraulikmodul HSBB 3","Speicher- und Hydraulikmodul HSBB 3","Speicher- und Hydraulikmodul HSBB 3","Boiler-Hydrauliek module HSBB 3","Speicher- und Hydraulikmodul HSBB 2.1","Speicher- und Hydraulikmodul HSBB 2.1","Speicher- und Hydraulikmodul HSBB 2.1","Speicher- und Hydraulikmodul HSBB 2.1","Speicher- und Hydraulikmodul HSBB 2.1","Speicher- und Hydraulikmodul HSBB 2.1"]
[null,234343,"Function module WPIC for WPL 13/18/23",4247,"",null,null,null,null,null,null,234343,"Function module WPIC for WPL 13/18/23",4247,false,null,234343,4320,4247,"5.090,00",28265,4320,"Funktionsmodul WPIC für WPL 13/18/23","Function module WPIC for WPL 13/18/23","Function module WPIC for WPL 13/18/23","Function module WPIC for WPL 13/18/23","WPL functiemodule WPIC","Function module WPIC for WPL 13/18/23","Function module WPIC for WPL 13/18/23","Function module WPIC for WPL 13/18/23","Function module WPIC for WPL 13/18/23","Function module WPIC for WPL 13/18/23","Function module WPIC for WPL 13/18/23"]
[null,74412,"Accessories WPL 13/18/23 internal installation",1059,"",null,null,null,null,null,null,74412,"Accessories WPL 13/18/23 internal installation",1059,false,null,74412,1427,1059,"1.430,00","på forespørgsel",1427,"Verkleidung WPL 13/18/23 Innenaufstellung","Accessories WPL 13/18/23 internal installation","Accessories WPL 13/18/23 internal installation","Accessories WPL 13/18/23 internal installation","Behuizing WPL 13/18/23 binnenopstelling","Accessories WPL 13/18/23 internal installation","Accessories WPL 13/18/23 internal installation","Accessories WPL 13/18/23 internal installation","Accessories WPL 13/18/23 internal installation","Accessories WPL 13/18/23 internal installation","Accessories WPL 13/18/23 internal installation"]
[null,74413,"Accessories WPL 13/18/23 external installation",1245,"",null,null,null,null,null,null,74413,"Accessories WPL 13/18/23 external installation",1245,false,null,74413,1966,1245,"1.715,00","på forespørgsel",1966,"Verkleidung WPL 13/18/23 Außenaufstellung","Accessories WPL 13/18/23 external installation","Accessories WPL 13/18/23 external installation","Accessories WPL 13/18/23 external installation","Behuizing WPL 13/18/23 buitenopstelling","Accessories WPL 13/18/23 external installation","Accessories WPL 13/18/23 external installation","Accessories WPL 13/18/23 external installation","Accessories WPL 13/18/23 external installation","Accessories WPL 13/18/23 external installation","Accessories WPL 13/18/23 external installation"]
[null,231890,"Accessories WPL 13/18/23 SR external installation",1368,"",null,null,null,null,null,null,231890,"Accessories WPL 13/18/23 SR external installation",1368,false,null,231890,2162,1368,"sur demande",8664,2162,"Verkleidung WPL 13/18/23 Außenaufstellung Silber","Accessories WPL 13/18/23 SR external installation","Accessories WPL 13/18/23 SR external installation","Accessories WPL 13/18/23 SR external installation","Behuizing WPL 13/18/23 SR omkasting ","Accessories WPL 13/18/23 SR external installation","Accessories WPL 13/18/23 SR external installation","Accessories WPL 13/18/23 SR external installation","Accessories WPL 13/18/23 SR external installation","Accessories WPL 13/18/23 SR external installation","Accessories WPL 13/18/23 SR external installation"]
[null,230206,"Accessories WPL 33 HT internal installation",1125,"",null,null,null,null,null,null,230206,"Accessories WPL 33 HT internal installation",1125,false,null,230206,1566,1125,"1.275,00",7845,1566,"Verkleidung WPL 33 HT Innenaufstellung","Accessories WPL 33 HT internal installation","Accessories WPL 33 HT internal installation","Accessories WPL 33 HT internal installation","Behuizing WPL 33 HT binnenopstelling","Accessories WPL 33 HT internal installation","Accessories WPL 33 HT internal installation","Accessories WPL 33 HT internal installation","Accessories WPL 33 HT internal installation","Accessories WPL 33 HT internal installation","Accessories WPL 33 HT internal installation"]
[null,230207,"Accessories WPL 33 HT external installation",1419,"",null,null,null,null,null,null,230207,"Accessories WPL 33 HT external installation",1419,false,null,230207,2044,1419,"1.620,00",9350,2044,"Verkleidung WPL 33 HT Außenaufstellung","Accessories WPL 33 HT external installation","Accessories WPL 33 HT external installation","Accessories WPL 33 HT external installation","Behuizing WPL 33 HT buitenopstelling","Accessories WPL 33 HT external installation","Accessories WPL 33 HT external installation","Accessories WPL 33 HT external installation","Accessories WPL 33 HT external installation","Accessories WPL 33 HT external installation","Accessories WPL 33 HT external installation"]
[null,232021,"Accessories WPL 33 HRT SR external installation",1482,"",null,null,null,null,null,null,232021,"Accessories WPL 33 HRT SR external installation",1482,false,null,232021,2248,1482,"sur demande",9402,2248,"Verkleidung WPL 33 HT Außenaufstellung Silber","Accessories WPL 33 HRT SR external installation","Accessories WPL 33 HRT SR external installation","Accessories WPL 33 HRT SR external installation","Behuizing WPL 33 HT SR buitenopstelling","Accessories WPL 33 HRT SR external installation","Accessories WPL 33 HRT SR external installation","Accessories WPL 33 HRT SR external installation","Accessories WPL 33 HRT SR external installation","Accessories WPL 33 HRT SR external installation","Accessories WPL 33 HRT SR external installation"]
[null,233836,"Außenwand-Durchführung AWG 315 silber",321,"",null,null,null,null,null,null,233836,"Außenwand-Durchführung AWG 315 silber",321,false,null,233836,399,321,455,2197,399,"Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Wanddoorvoer AWG 315 S","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber"]
[null,232955,"Außenwand-Durchführung AWG 315 grau",319,"",null,null,null,null,null,null,232955,"Außenwand-Durchführung AWG 315 grau",319,false,null,232955,399,319,450,2190,399,"Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Wanddoorvoer AWG 315 G","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau"]
[null,231039,"Air routing AWG 315 lightwell",261,"",null,null,null,null,null,null,231039,"Air routing AWG 315 lightwell",261,false,null,231039,224,261,400,1743,224,"Außenwand-Durchführung AWG 315 Lichtschacht","Air routing AWG 315 lightwell","Traversée murale AWG 315 soupirail","Air routing AWG 315 lightwell","Wanddoorvoer AWG 315 L","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell"]
[null,233837,"Außenwand-Durchführung AWG 560 H silber",447,"",null,null,null,null,null,null,233837,"Außenwand-Durchführung AWG 560 H silber",447,false,null,233837,611,447,630,3040,611,"Außenwand-Durchführung AWG 560 H silber","Außenwand-Durchführung AWG 560 H silber","Außenwand-Durchführung AWG 560 H silber","Außenwand-Durchführung AWG 560 H silber","Wanddoorvoer AWG 560 H zilver","Außenwand-Durchführung AWG 560 H silber","Außenwand-Durchführung AWG 560 H silber","Außenwand-Durchführung AWG 560 H silber","Außenwand-Durchführung AWG 560 H silber","Außenwand-Durchführung AWG 560 H silber","Außenwand-Durchführung AWG 560 H silber"]
[null,232956,"Außenwand-Durchführung AWG 560 H grau",443,"",null,null,null,null,null,null,232956,"Außenwand-Durchführung AWG 560 H grau",443,false,null,232956,611,443,640,3047,611,"Außenwand-Durchführung AWG 560 H grau","Außenwand-Durchführung AWG 560 H grau","Außenwand-Durchführung AWG 560 H grau","Außenwand-Durchführung AWG 560 H grau","Wanddoorvoer AWG 560 H grijs","Außenwand-Durchführung AWG 560 H grau","Außenwand-Durchführung AWG 560 H grau","Außenwand-Durchführung AWG 560 H grau","Außenwand-Durchführung AWG 560 H grau","Außenwand-Durchführung AWG 560 H grau","Außenwand-Durchführung AWG 560 H grau"]
[null,231041,"Air routing AWG 560 lightwell",373,"",null,null,null,null,null,null,231041,"Air routing AWG 560 lightwell",373,false,null,231041,313,373,590,2608,313,"Außenwand-Durchführung AWG 560 Lichtschacht","Air routing AWG 560 lightwell","Air routing AWG 560 lightwell","Air routing AWG 560 lightwell","Wanddoorvoer AWG 560 L","Air routing AWG 560 lightwell","Air routing AWG 560 lightwell","Air routing AWG 560 lightwell","Air routing AWG 560 lightwell","Air routing AWG 560 lightwell","Air routing AWG 560 lightwell"]
[null,233838,"Außenwand-Durchführung AWG 560 V silber",477,"",null,null,null,null,null,null,233838,"Außenwand-Durchführung AWG 560 V silber",477,false,null,233838,611,477,680,3266,611,"Außenwand-Durchführung AWG 560 V silber","Außenwand-Durchführung AWG 560 V silber","Außenwand-Durchführung AWG 560 V silber","Außenwand-Durchführung AWG 560 V silber","Wanddoorvoer AWG 560 V zilver","Außenwand-Durchführung AWG 560 V silber","Außenwand-Durchführung AWG 560 V silber","Außenwand-Durchführung AWG 560 V silber","Außenwand-Durchführung AWG 560 V silber","Außenwand-Durchführung AWG 560 V silber","Außenwand-Durchführung AWG 560 V silber"]
[null,232957,"Außenwand-Durchführung AWG 560 V grau",468,"",null,null,null,null,null,null,232957,"Außenwand-Durchführung AWG 560 V grau",468,false,null,232957,611,468,675,3218,611,"Außenwand-Durchführung AWG 560 V grau","Außenwand-Durchführung AWG 560 V grau","Außenwand-Durchführung AWG 560 V grau","Außenwand-Durchführung AWG 560 V grau","Wanddoorvoer AWG 560 V grijs","Außenwand-Durchführung AWG 560 V grau","Außenwand-Durchführung AWG 560 V grau","Außenwand-Durchführung AWG 560 V grau","Außenwand-Durchführung AWG 560 V grau","Außenwand-Durchführung AWG 560 V grau","Außenwand-Durchführung AWG 560 V grau"]
[null,231044,"Air routing AWG 600 lightwell",415,"",null,null,null,null,null,null,231044,"Air routing AWG 600 lightwell",415,false,null,231044,313,415,565,2906,313,"Außenwand-Durchführung AWG 600 Lichtschacht","Air routing AWG 600 lightwell","Air routing AWG 600 lightwell","Air routing AWG 600 lightwell","Wanddoorvoer AWG 600 L","Air routing AWG 600 lightwell","Air routing AWG 600 lightwell","Air routing AWG 600 lightwell","Air routing AWG 600 lightwell","Air routing AWG 600 lightwell","Air routing AWG 600 lightwell"]
[null,232341,"Luftleitblech für AWG 315 Lichtschacht",30,"",null,null,null,null,null,null,232341,"Luftleitblech für AWG 315 Lichtschacht",30,false,null,232341,22.8,30,45,155,23,"Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luchtgeleidingsplaat voor AWG 315 lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht"]
[null,232342,"Luftleitblech für AWG 560 Lichtschacht",34,"",null,null,null,null,null,null,232342,"Luftleitblech für AWG 560 Lichtschacht",34,false,null,232342,30,34,60,185,30,"Luftleitblech für AWG 560 Lichtschacht","Luftleitblech für AWG 560 Lichtschacht","Luftleitblech für AWG 560 Lichtschacht","Luftleitblech für AWG 560 Lichtschacht","Luchtgeleidingsplaat voor AWG 560 lichtschacht","Luftleitblech für AWG 560 Lichtschacht","Luftleitblech für AWG 560 Lichtschacht","Luftleitblech für AWG 560 Lichtschacht","Luftleitblech für AWG 560 Lichtschacht","Luftleitblech für AWG 560 Lichtschacht","Luftleitblech für AWG 560 Lichtschacht"]
[null,170018,"Silencer DN 315",138,"",null,null,null,null,null,null,170018,"Silencer DN 315",138,false,null,170018,248,138,175,909,248,"Schalldämpfer DN 315","Silencer DN 315","Amortisseur de bruit DN 315","Silencer DN 315","Geluidsdemper DN 315","Silencer DN 315","Silencer DN 315","Silencer DN 315","Silencer DN 315","Silencer DN 315","Silencer DN 315"]
[null,167120,"Hose connection plate DN 315",102,"",null,null,null,null,null,null,167120,"Hose connection plate DN 315",102,false,null,167120,215,102,145,857,215,"Schlauchanschluss-Platte DN 315","Hose connection plate DN 315","Hose connection plate DN 315","Hose connection plate DN 315","Slangaansluitplaat DN 315","Hose connection plate DN 315","Hose connection plate DN 315","Hose connection plate DN 315","Hose connection plate DN 315","Hose connection plate DN 315","Hose connection plate DN 315"]
[null,231835,"Air hose DN 315, 4m",127,"",null,null,null,null,null,null,231835,"Air hose DN 315, 4m",127,false,null,231835,228,127,215,1188,228,"Wärmegedämmter Luftschlauch DN 315, 4m","Air hose DN 315, 4m","Gaine d'air à isolation thermique DN 315, 4 m","Air hose DN 315, 4m","Luchtslang DN 315 LSWP 315-4 AL","Air hose DN 315, 4m","Air hose DN 315, 4m","Air hose DN 315, 4m","Air hose DN 315, 4m","Air hose DN 315, 4m","Air hose DN 315, 4m"]
[null,231836,"Air hose DN 560, 4m",245,"",null,null,null,null,null,null,231836,"Air hose DN 560, 4m",245,false,null,231836,436,245,345,1751,436,"Wärmegedämmter Luftschlauch DN 560, 4 m","Air hose DN 560, 4m","Air hose DN 560, 4m","Air hose DN 560, 4m","Luchtslang DN 560 LSWP 560-4 AL","Air hose DN 560, 4m","Air hose DN 560, 4m","Air hose DN 560, 4m","Air hose DN 560, 4m","Air hose DN 560, 4m","Air hose DN 560, 4m"]
[null,229286,"Condensate pump PK 9",224,"",null,null,null,null,null,null,229286,"Condensate pump PK 9",224,false,null,229286,244,224,225,1594,244,"Kondensatpumpe PK 10","Condensate pump PK 9","Condensate pump PK 9","Condensate pump PK 9","Condensaatpomp PK 10","Condensate pump PK 9","Condensate pump PK 9","Condensate pump PK 9","Condensate pump PK 9","Condensate pump PK 9","Condensate pump PK 9"]
[null,185325,"Duct silencer KSD for WPL 13/18/23",958,"",null,null,null,null,null,null,185325,"Duct silencer KSD for WPL 13/18/23",958,false,null,185325,1265,958,"1.300,00",6251,1265,"Kanal-Schalldämpfer für WPL 13/18/23","Duct silencer KSD for WPL 13/18/23","Duct silencer KSD for WPL 13/18/23","Duct silencer KSD for WPL 13/18/23","Geluiddemper KSD 13/18/23","Duct silencer KSD for WPL 13/18/23","Duct silencer KSD for WPL 13/18/23","Duct silencer KSD for WPL 13/18/23","Duct silencer KSD for WPL 13/18/23","Duct silencer KSD for WPL 13/18/23","Duct silencer KSD for WPL 13/18/23"]
[null,185370,"Duct silencer KSD for WPL 33 HT",1122,"",null,null,null,null,null,null,185370,"Duct silencer KSD for WPL 33 HT",1122,false,null,185370,1293,1122,"1.560,00",6772,1293,"Kanal-Schalldämpfer für WPL 33 HT","Duct silencer KSD for WPL 33 HT","Duct silencer KSD for WPL 33 HT","Duct silencer KSD for WPL 33 HT","Geluiddemper KSD 33","Duct silencer KSD for WPL 33 HT","Duct silencer KSD for WPL 33 HT","Duct silencer KSD for WPL 33 HT","Duct silencer KSD for WPL 33 HT","Duct silencer KSD for WPL 33 HT","Duct silencer KSD for WPL 33 HT"]
[null,222263,"Wall mounting panel 2",47,{"$f":"IF(O180=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,222263,"Wall mounting panel 2",47,false,null,222263,81,47,"sur demande",302,81,"Wandkonsole WPL 5 N plus","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2","Wandconsole 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2"]
[null,232963,"Wandkonsole WPL 10 AC",150,"",null,null,null,null,null,null,232963,"Wandkonsole WPL 10 AC",150,false,null,232963,146,150,220,1028,146,"Wandkonsole WPL 10/15/25 mit Heizband 2m","Wandkonsole WPL 10 AC","Wandkonsole WPL 10 AC","Wandkonsole WPL 10 AC","Wandconsole WPL 10/15/25 met verwarmingslint 2m","Wandkonsole WPL 10 AC","Wandkonsole WPL 10 AC","Wandkonsole WPL 10 AC","Wandkonsole WPL 10 AC","Wandkonsole WPL 10 AC","Wandkonsole WPL 10 AC"]
[null,232964,"Standkonsole Einbetonierung WPL 10 AC",463,"",null,null,null,null,null,null,232964,"Standkonsole Einbetonierung WPL 10 AC",463,false,null,232964,388,463,665,3181,388,"Standkonsole WPL 10/15/25 mit Heizband 1m","Standkonsole Einbetonierung WPL 10 AC","Standkonsole Einbetonierung WPL 10 AC","Standkonsole Einbetonierung WPL 10 AC","Vloerconsole WPL 10/15/25 met verwarmingsband 1m","Standkonsole Einbetonierung WPL 10 AC","Standkonsole Einbetonierung WPL 10 AC","Standkonsole Einbetonierung WPL 10 AC","Standkonsole Einbetonierung WPL 10 AC","Standkonsole Einbetonierung WPL 10 AC","Standkonsole Einbetonierung WPL 10 AC"]
[null,233047,"Montagekonsole Bodenaufstellung WPL 10 AC",471,"",null,null,null,null,null,null,233047,"Montagekonsole Bodenaufstellung WPL 10 AC",471,false,null,233047,372,471,"sur demande",3233,372,"Montagekonsole Bodenaufstellung WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC","Montageconsole vloeropstelling WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC","Montagekonsole Bodenaufstellung WPL 10 AC"]
[null,233622,"Hydraulisches Anschlussset AS-WP 1",118,"",null,null,null,null,null,null,233622,"Hydraulisches Anschlussset AS-WP 1",118,{"$f":"IF(AND(B184=L184,C184=M184,D184=N184),FALSE,TRUE)","v":false},null,233622,107,118,"sur demande",830,107,"Hydraulisches Anschlussset AS-WP 1","Hydraulisches Anschlussset AS-WP 1","Hydraulisches Anschlussset AS-WP 1","Hydraulisches Anschlussset AS-WP 1","Hydraulische aansluitset AS-WP 1","Hydraulisches Anschlussset AS-WP 1","Hydraulisches Anschlussset AS-WP 1","Hydraulisches Anschlussset AS-WP 1","Hydraulisches Anschlussset AS-WP 1","Hydraulisches Anschlussset AS-WP 1","Hydraulisches Anschlussset AS-WP 1"]
[null,233623,"Hydraulisches Anschlussset AS-WP 2",79,"",null,null,null,null,null,null,233623,"Hydraulisches Anschlussset AS-WP 2",79,false,null,233623,97,79,115,564,97,"Hydraulisches Anschlussset AS-WP 2","Hydraulisches Anschlussset AS-WP 2","Hydraulisches Anschlussset AS-WP 2","Hydraulisches Anschlussset AS-WP 2","Hydraulische aansluitset AS-WP 2","Hydraulisches Anschlussset AS-WP 2","Hydraulisches Anschlussset AS-WP 2","Hydraulisches Anschlussset AS-WP 2","Hydraulisches Anschlussset AS-WP 2","Hydraulisches Anschlussset AS-WP 2","Hydraulisches Anschlussset AS-WP 2"]
[null,232047,"Split line 10x1 10 m",73,"",null,null,null,null,null,null,232047,"Split line 10x1 10 m",73,false,null,232047,108,73,"sur demande",474,108,"Flüssigkeitsleitung 10x1, 10 m","Split line 10x1 10 m","Split line 10x1 10 m","Split line 10x1 10 m","Vloeistofpersleiding 10x1, 10 m","Split line 10x1 10 m","Split line 10x1 10 m","Split line 10x1 10 m","Split line 10x1 10 m","Split line 10x1 10 m","Split line 10x1 10 m"]
[null,232048,"Split line 10x1 15 m",109,"",null,null,null,null,null,null,232048,"Split line 10x1 15 m",109,false,null,232048,142,109,"sur demande",711,142,"Flüssigkeitsleitung 10x1, 15 m","Split line 10x1 15 m","Split line 10x1 15 m","Split line 10x1 15 m","Vloeistofpersleiding 10x1, 15 m","Split line 10x1 15 m","Split line 10x1 15 m","Split line 10x1 15 m","Split line 10x1 15 m","Split line 10x1 15 m","Split line 10x1 15 m"]
[null,232049,"Split line 10x1 25 m",181,"",null,null,null,null,null,null,232049,"Split line 10x1 25 m",181,false,null,232049,185,181,"sur demande",1244,185,"Flüssigkeitsleitung 10x1, 25 m","Split line 10x1 25 m","Split line 10x1 25 m","Split line 10x1 25 m","Vloeistofpersleiding 10x1, 25 m","Split line 10x1 25 m","Split line 10x1 25 m","Split line 10x1 25 m","Split line 10x1 25 m","Split line 10x1 25 m","Split line 10x1 25 m"]
[null,232050,"Split line 16x1 10 m",115,"",null,null,null,null,null,null,232050,"Split line 16x1 10 m",115,false,null,232050,151,115,"sur demande",767,151,"Sauggasleitung 16x1, 10 m","Split line 16x1 10 m","Split line 16x1 10 m","Split line 16x1 10 m","Zuiggasleiding 16x1, 10 m","Split line 16x1 10 m","Split line 16x1 10 m","Split line 16x1 10 m","Split line 16x1 10 m","Split line 16x1 10 m","Split line 16x1 10 m"]
[null,232051,"Split line 16x1 15 m",172,"",null,null,null,null,null,null,232051,"Split line 16x1 15 m",172,false,null,232051,194,172,"sur demande",1155,194,"Sauggasleitung 16x1, 15 m","Split line 16x1 15 m","Split line 16x1 15 m","Split line 16x1 15 m","Zuiggasleiding 16x1, 15 m","Split line 16x1 15 m","Split line 16x1 15 m","Split line 16x1 15 m","Split line 16x1 15 m","Split line 16x1 15 m","Split line 16x1 15 m"]
[null,232052,"Split line 16x1 25 m",287,"",null,null,null,null,null,null,232052,"Split line 16x1 25 m",287,false,null,232052,273,287,"sur demande",1922,273,"Sauggasleitung 16x1, 25 m","Split line 16x1 25 m","Split line 16x1 25 m","Split line 16x1 25 m","Zuiggasleiding 16x1, 25 m","Split line 16x1 25 m","Split line 16x1 25 m","Split line 16x1 25 m","Split line 16x1 25 m","Split line 16x1 25 m","Split line 16x1 25 m"]
[null,232053,"Split line 18x1 10 m",132,"",null,null,null,null,null,null,232053,"Split line 18x1 10 m",132,false,null,232053,169,132,"sur demande",849,169,"Sauggasleitung 18x1, 10 m","Split line 18x1 10 m","Split line 18x1 10 m","Split line 18x1 10 m","Zuiggasleiding 18x1, 10 m","Split line 18x1 10 m","Split line 18x1 10 m","Split line 18x1 10 m","Split line 18x1 10 m","Split line 18x1 10 m","Split line 18x1 10 m"]
[null,232054,"Split line 18x1 15 m",198,"",null,null,null,null,null,null,232054,"Split line 18x1 15 m",198,false,null,232054,205,198,"sur demande",1274,205,"Sauggasleitung 18x1, 15 m","Split line 18x1 15 m","Split line 18x1 15 m","Split line 18x1 15 m","Zuiggasleiding 18x1, 15 m","Split line 18x1 15 m","Split line 18x1 15 m","Split line 18x1 15 m","Split line 18x1 15 m","Split line 18x1 15 m","Split line 18x1 15 m"]
[null,232055,"Split line 18x1 25 m",329,"",null,null,null,null,null,null,232055,"Split line 18x1 25 m",329,false,null,232055,305,329,"sur demande",2123,305,"Sauggasleitung 18x1, 25 m","Split line 18x1 25 m","Split line 18x1 25 m","Split line 18x1 25 m","Zuiggasleiding 18x1, 25 m","Split line 18x1 25 m","Split line 18x1 25 m","Split line 18x1 25 m","Split line 18x1 25 m","Split line 18x1 25 m","Split line 18x1 25 m"]
[null,227557,"Insulating tape, 10 m","On request","",null,null,null,null,null,null,227557,"Insulating tape, 10 m","On request",false,null,227557,17.600000000000001,"On request","sur demande","på forespørgsel",18,"Wärmedämmband, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Isolatieband, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m"]
[null,232926,"Sole|Wasser-Wärmepumpe WPC 04",7224,"",null,null,null,null,null,null,232926,"Sole|Wasser-Wärmepumpe WPC 04",7224,false,null,232926,8169,7224,"9.370,00",36656,7709,"Sole|Wasser-Wärmepumpe WPC 04","Sole|Wasser-Wärmepumpe WPC 04","Sole|Wasser-Wärmepumpe WPC 04","Sole|Wasser-Wärmepumpe WPC 04","Glycol/water-warmtepompen WPC 04","Sole|Wasser-Wärmepumpe WPC 04","Sole|Wasser-Wärmepumpe WPC 04","Sole|Wasser-Wärmepumpe WPC 04","Sole|Wasser-Wärmepumpe WPC 04","Sole|Wasser-Wärmepumpe WPC 04","Sole|Wasser-Wärmepumpe WPC 04"]
[null,232927,"Sole|Wasser-Wärmepumpe WPC 05",7871,"",null,null,null,null,null,null,232927,"Sole|Wasser-Wärmepumpe WPC 05",7871,false,null,232927,8442,7871,"9.685,00",37888,7936,"Sole|Wasser-Wärmepumpe WPC 05","Sole|Wasser-Wärmepumpe WPC 05","Sole|Wasser-Wärmepumpe WPC 05","Sole|Wasser-Wärmepumpe WPC 05","Glycol/water-warmtepompen WPC 05","Sole|Wasser-Wärmepumpe WPC 05","Sole|Wasser-Wärmepumpe WPC 05","Sole|Wasser-Wärmepumpe WPC 05","Sole|Wasser-Wärmepumpe WPC 05","Sole|Wasser-Wärmepumpe WPC 05","Sole|Wasser-Wärmepumpe WPC 05"]
[null,232928,"Sole|Wasser-Wärmepumpe WPC 07",8127,"",null,null,null,null,null,null,232928,"Sole|Wasser-Wärmepumpe WPC 07",8127,false,null,232928,9104,8127,"10.260,00",40143,8952,"Sole|Wasser-Wärmepumpe WPC 07","Sole|Wasser-Wärmepumpe WPC 07","Sole|Wasser-Wärmepumpe WPC 07","Sole|Wasser-Wärmepumpe WPC 07","Glycol/water-warmtepompen WPC 07","Sole|Wasser-Wärmepumpe WPC 07","Sole|Wasser-Wärmepumpe WPC 07","Sole|Wasser-Wärmepumpe WPC 07","Sole|Wasser-Wärmepumpe WPC 07","Sole|Wasser-Wärmepumpe WPC 07","Sole|Wasser-Wärmepumpe WPC 07"]
[null,232929,"Sole|Wasser-Wärmepumpe WPC 10",8518,"",null,null,null,null,null,null,232929,"Sole|Wasser-Wärmepumpe WPC 10",8518,false,null,232929,9765,8518,"10.620,00",41554,9644,"Sole|Wasser-Wärmepumpe WPC 10","Sole|Wasser-Wärmepumpe WPC 10","Sole|Wasser-Wärmepumpe WPC 10","Sole|Wasser-Wärmepumpe WPC 10","Glycol/water-warmtepompen WPC 10","Sole|Wasser-Wärmepumpe WPC 10","Sole|Wasser-Wärmepumpe WPC 10","Sole|Wasser-Wärmepumpe WPC 10","Sole|Wasser-Wärmepumpe WPC 10","Sole|Wasser-Wärmepumpe WPC 10","Sole|Wasser-Wärmepumpe WPC 10"]
[null,232930,"Sole|Wasser-Wärmepumpe WPC 13",8726,"",null,null,null,null,null,null,232930,"Sole|Wasser-Wärmepumpe WPC 13",8726,false,null,232930,10593,8726,"11.040,00",43196,9805,"Sole|Wasser-Wärmepumpe WPC 13","Sole|Wasser-Wärmepumpe WPC 13","Sole|Wasser-Wärmepumpe WPC 13","Sole|Wasser-Wärmepumpe WPC 13","Glycol/water-warmtepompen WPC 13","Sole|Wasser-Wärmepumpe WPC 13","Sole|Wasser-Wärmepumpe WPC 13","Sole|Wasser-Wärmepumpe WPC 13","Sole|Wasser-Wärmepumpe WPC 13","Sole|Wasser-Wärmepumpe WPC 13","Sole|Wasser-Wärmepumpe WPC 13"]
[null,232931,"Sole|Wasser-Wärmepumpe WPC 04 cool",7969,"",null,null,null,null,null,null,232931,"Sole|Wasser-Wärmepumpe WPC 04 cool",7969,false,null,232931,9078,7969,"10.330,00","på forespørgsel",8060,"Sole|Wasser-Wärmepumpe WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool","Glycol/water-warmtepompen WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool","Sole|Wasser-Wärmepumpe WPC 04 cool"]
[null,232932,"Sole|Wasser-Wärmepumpe WPC 05 cool",8537,"",null,null,null,null,null,null,232932,"Sole|Wasser-Wärmepumpe WPC 05 cool",8537,false,null,232932,9701,8537,"10.760,00","på forespørgsel",8321,"Sole|Wasser-Wärmepumpe WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool","Glycol/water-warmtepompen WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool","Sole|Wasser-Wärmepumpe WPC 05 cool"]
[null,232933,"Sole|Wasser-Wärmepumpe WPC 07 cool",8923,"",null,null,null,null,null,null,232933,"Sole|Wasser-Wärmepumpe WPC 07 cool",8923,false,null,232933,10381,8923,"11.250,00","på forespørgsel",9573,"Sole|Wasser-Wärmepumpe WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool","Glycol/water-warmtepompen WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool","Sole|Wasser-Wärmepumpe WPC 07 cool"]
[null,232934,"Sole|Wasser-Wärmepumpe WPC 10 cool",9349,"",null,null,null,null,null,null,232934,"Sole|Wasser-Wärmepumpe WPC 10 cool",9349,false,null,232934,11045,9349,"11.595,00","på forespørgsel",10252,"Sole|Wasser-Wärmepumpe WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool","Glycol/water-warmtepompen WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool","Sole|Wasser-Wärmepumpe WPC 10 cool"]
[null,232935,"Sole|Wasser-Wärmepumpe WPC 13 cool",9545,"",null,null,null,null,null,null,232935,"Sole|Wasser-Wärmepumpe WPC 13 cool",9545,false,null,232935,11915,9545,"12.015,00","på forespørgsel",10544,"Sole|Wasser-Wärmepumpe WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool","Glycol/water-warmtepompen WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool","Sole|Wasser-Wärmepumpe WPC 13 cool"]
[null,232909,"Sole|Wasser-Wärmepumpe WPF 04",7522,"",null,null,null,null,null,null,232909,"Sole|Wasser-Wärmepumpe WPF 04",7522,false,null,232909,7674,7522,"7.910,00",34638,7674,"Sole|Wasser-Wärmepumpe WPF 04","Sole|Wasser-Wärmepumpe WPF 04","Sole|Wasser-Wärmepumpe WPF 04","Sole|Wasser-Wärmepumpe WPF 04","Glycol/water-warmtepompen WPF 04","Sole|Wasser-Wärmepumpe WPF 04","Sole|Wasser-Wärmepumpe WPF 04","Sole|Wasser-Wärmepumpe WPF 04","Sole|Wasser-Wärmepumpe WPF 04","Sole|Wasser-Wärmepumpe WPF 04","Sole|Wasser-Wärmepumpe WPF 04"]
[null,232910,"Sole|Wasser-Wärmepumpe WPF 05",7922,"",null,null,null,null,null,null,232910,"Sole|Wasser-Wärmepumpe WPF 05",7922,false,null,232910,7906,7922,"8.235,00",36075,7906,"Sole|Wasser-Wärmepumpe WPF 05","Sole|Wasser-Wärmepumpe WPF 05","Sole|Wasser-Wärmepumpe WPF 05","Sole|Wasser-Wärmepumpe WPF 05","Glycol/water-warmtepompen WPF 05","Sole|Wasser-Wärmepumpe WPF 05","Sole|Wasser-Wärmepumpe WPF 05","Sole|Wasser-Wärmepumpe WPF 05","Sole|Wasser-Wärmepumpe WPF 05","Sole|Wasser-Wärmepumpe WPF 05","Sole|Wasser-Wärmepumpe WPF 05"]
[null,232911,"Sole|Wasser-Wärmepumpe WPF 07",8347,"",null,null,null,null,null,null,232911,"Sole|Wasser-Wärmepumpe WPF 07",8347,false,null,232911,8497,8347,"8.820,00",38616,8497,"Sole|Wasser-Wärmepumpe WPF 07","Sole|Wasser-Wärmepumpe WPF 07","Sole|Wasser-Wärmepumpe WPF 07","Sole|Wasser-Wärmepumpe WPF 07","Glycol/water-warmtepompen WPF 07","Sole|Wasser-Wärmepumpe WPF 07","Sole|Wasser-Wärmepumpe WPF 07","Sole|Wasser-Wärmepumpe WPF 07","Sole|Wasser-Wärmepumpe WPF 07","Sole|Wasser-Wärmepumpe WPF 07","Sole|Wasser-Wärmepumpe WPF 07"]
[null,232912,"Sole|Wasser-Wärmepumpe WPF 10",8603,"",null,null,null,null,null,null,232912,"Sole|Wasser-Wärmepumpe WPF 10",8603,false,null,232912,9091,8603,"9.110,00",39900,9091,"Sole|Wasser-Wärmepumpe WPF 10","Sole|Wasser-Wärmepumpe WPF 10","Sole|Wasser-Wärmepumpe WPF 10","Sole|Wasser-Wärmepumpe WPF 10","Glycol/water-warmtepompen WPF 10","Sole|Wasser-Wärmepumpe WPF 10","Sole|Wasser-Wärmepumpe WPF 10","Sole|Wasser-Wärmepumpe WPF 10","Sole|Wasser-Wärmepumpe WPF 10","Sole|Wasser-Wärmepumpe WPF 10","Sole|Wasser-Wärmepumpe WPF 10"]
[null,232913,"Sole|Wasser-Wärmepumpe WPF 13",8731,"",null,null,null,null,null,null,232913,"Sole|Wasser-Wärmepumpe WPF 13",8731,false,null,232913,9750,8731,"9.530,00",41734,9750,"Sole|Wasser-Wärmepumpe WPF 13","Sole|Wasser-Wärmepumpe WPF 13","Sole|Wasser-Wärmepumpe WPF 13","Sole|Wasser-Wärmepumpe WPF 13","Glycol/water-warmtepompen WPF 13","Sole|Wasser-Wärmepumpe WPF 13","Sole|Wasser-Wärmepumpe WPF 13","Sole|Wasser-Wärmepumpe WPF 13","Sole|Wasser-Wärmepumpe WPF 13","Sole|Wasser-Wärmepumpe WPF 13","Sole|Wasser-Wärmepumpe WPF 13"]
[null,232914,"Sole|Wasser-Wärmepumpe WPF 16",8955,"",null,null,null,null,null,null,232914,"Sole|Wasser-Wärmepumpe WPF 16",8955,false,null,232914,10538,8955,"10.365,00",45377,10538,"Sole|Wasser-Wärmepumpe WPF 16","Sole|Wasser-Wärmepumpe WPF 16","Sole|Wasser-Wärmepumpe WPF 16","Sole|Wasser-Wärmepumpe WPF 16","Glycol/water-warmtepompen WPF 16","Sole|Wasser-Wärmepumpe WPF 16","Sole|Wasser-Wärmepumpe WPF 16","Sole|Wasser-Wärmepumpe WPF 16","Sole|Wasser-Wärmepumpe WPF 16","Sole|Wasser-Wärmepumpe WPF 16","Sole|Wasser-Wärmepumpe WPF 16"]
[null,232915,"Sole|Wasser-Wärmepumpe WPF 04 cool",8379,"",null,null,null,null,null,null,232915,"Sole|Wasser-Wärmepumpe WPF 04 cool",8379,false,null,232915,8363,8379,"8.810,00","på forespørgsel",8363,"Sole|Wasser-Wärmepumpe WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool","Glycol/water-warmtepompen WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool","Sole|Wasser-Wärmepumpe WPF 04 cool"]
[null,232916,"Sole|Wasser-Wärmepumpe WPF 05 cool",8603,"",null,null,null,null,null,null,232916,"Sole|Wasser-Wärmepumpe WPF 05 cool",8603,false,null,232916,9102,8603,"9.145,00","på forespørgsel",9102,"Sole|Wasser-Wärmepumpe WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool","Glycol/water-warmtepompen WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool","Sole|Wasser-Wärmepumpe WPF 05 cool"]
[null,232917,"Sole|Wasser-Wärmepumpe WPF 07 cool",8987,"",null,null,null,null,null,null,232917,"Sole|Wasser-Wärmepumpe WPF 07 cool",8987,false,null,232917,9696,8987,"9.715,00","på forespørgsel",9696,"Sole|Wasser-Wärmepumpe WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool","Glycol/water-warmtepompen WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool","Sole|Wasser-Wärmepumpe WPF 07 cool"]
[null,232918,"Sole|Wasser-Wärmepumpe WPF 10 cool",9275,"",null,null,null,null,null,null,232918,"Sole|Wasser-Wärmepumpe WPF 10 cool",9275,false,null,232918,10285,9275,"10.000,00","på forespørgsel",10285,"Sole|Wasser-Wärmepumpe WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool","Glycol/water-warmtepompen WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool","Sole|Wasser-Wärmepumpe WPF 10 cool"]
[null,232919,"Sole|Wasser-Wärmepumpe WPF 13 cool",9435,"",null,null,null,null,null,null,232919,"Sole|Wasser-Wärmepumpe WPF 13 cool",9435,false,null,232919,10947,9435,"10.430,00","på forespørgsel",10947,"Sole|Wasser-Wärmepumpe WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool","Glycol/water-warmtepompen WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool","Sole|Wasser-Wärmepumpe WPF 13 cool"]
[null,232920,"Sole|Wasser-Wärmepumpe WPF 16 cool",9627,"",null,null,null,null,null,null,232920,"Sole|Wasser-Wärmepumpe WPF 16 cool",9627,false,null,232920,11734,9627,"11.255,00","på forespørgsel",11734,"Sole|Wasser-Wärmepumpe WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool","Glycol/water-warmtepompen WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool","Sole|Wasser-Wärmepumpe WPF 16 cool"]
[null,230944,"Brine|water heat pump WPF 5 basic",4991,"",null,null,null,null,null,null,230944,"Brine|water heat pump WPF 5 basic",4991,false,null,230944,5364,4991,"5.990,00",31759,5364,"Sole|Wasser-Wärmepumpe WPF 5 basic","Brine|water heat pump WPF 5 basic","Brine|water heat pump WPF 5 basic","Brine|water heat pump WPF 5 basic","Glycol/water-warmtepompen WPF 5 basic","Brine|water heat pump WPF 5 basic","Brine|water heat pump WPF 5 basic","Brine|water heat pump WPF 5 basic","Brine|water heat pump WPF 5 basic","Brine|water heat pump WPF 5 basic","Brine|water heat pump WPF 5 basic"]
[null,230945,"Brine|water heat pump WPF 7 basic",5373,"",null,null,null,null,null,null,230945,"Brine|water heat pump WPF 7 basic",5373,false,null,230945,5822,5373,"6.440,00",34151,5822,"Sole|Wasser-Wärmepumpe WPF 7 basic","Brine|water heat pump WPF 7 basic","Brine|water heat pump WPF 7 basic","Brine|water heat pump WPF 7 basic","Glycol/water-warmtepompen WPF 7 basic","Brine|water heat pump WPF 7 basic","Brine|water heat pump WPF 7 basic","Brine|water heat pump WPF 7 basic","Brine|water heat pump WPF 7 basic","Brine|water heat pump WPF 7 basic","Brine|water heat pump WPF 7 basic"]
[null,230946,"Brine|water heat pump WPF 10 basic",5615,"",null,null,null,null,null,null,230946,"Brine|water heat pump WPF 10 basic",5615,false,null,230946,6437,5615,"6.690,00",35775,6437,"Sole|Wasser-Wärmepumpe WPF 10 basic","Brine|water heat pump WPF 10 basic","Brine|water heat pump WPF 10 basic","Brine|water heat pump WPF 10 basic","Glycol/water-warmtepompen WPF 10 basic","Brine|water heat pump WPF 10 basic","Brine|water heat pump WPF 10 basic","Brine|water heat pump WPF 10 basic","Brine|water heat pump WPF 10 basic","Brine|water heat pump WPF 10 basic","Brine|water heat pump WPF 10 basic"]
[null,230947,"Brine|water heat pump WPF 13 basic",5799,"",null,null,null,null,null,null,230947,"Brine|water heat pump WPF 13 basic",5799,false,null,230947,7050,5799,"6.940,00",36848,7050,"Sole|Wasser-Wärmepumpe WPF 13 basic","Brine|water heat pump WPF 13 basic","Brine|water heat pump WPF 13 basic","Brine|water heat pump WPF 13 basic","Glycol/water-warmtepompen WPF 13 basic","Brine|water heat pump WPF 13 basic","Brine|water heat pump WPF 13 basic","Brine|water heat pump WPF 13 basic","Brine|water heat pump WPF 13 basic","Brine|water heat pump WPF 13 basic","Brine|water heat pump WPF 13 basic"]
[null,230948,"Brine|water heat pump WPF 16 basic",6036,"",null,null,null,null,null,null,230948,"Brine|water heat pump WPF 16 basic",6036,false,null,230948,7662,6036,"7.250,00",38300,7662,"Sole|Wasser-Wärmepumpe WPF 16 basic","Brine|water heat pump WPF 16 basic","Brine|water heat pump WPF 16 basic","Brine|water heat pump WPF 16 basic","Glycol/water-warmtepompen WPF 16 basic","Brine|water heat pump WPF 16 basic","Brine|water heat pump WPF 16 basic","Brine|water heat pump WPF 16 basic","Brine|water heat pump WPF 16 basic","Brine|water heat pump WPF 16 basic","Brine|water heat pump WPF 16 basic"]
[null,185349,"Brine|water heat pump WPF 10 M",4487,"",null,null,null,null,null,null,185349,"Brine|water heat pump WPF 10 M",4487,false,null,185349,7069,4487,"6.150,00",32743,7069,"Sole|Wasser-Wärmepumpe WPF 10 M","Brine|water heat pump WPF 10 M","Brine|water heat pump WPF 10 M","Brine|water heat pump WPF 10 M","Glycol/water-warmtepompen WPF 10 M","Brine|water heat pump WPF 10 M","Brine|water heat pump WPF 10 M","Brine|water heat pump WPF 10 M","Brine|water heat pump WPF 10 M","Brine|water heat pump WPF 10 M","Brine|water heat pump WPF 10 M"]
[null,182135,"Brine|water heat pump WPF 13 M",4588,"",null,null,null,null,null,null,182135,"Brine|water heat pump WPF 13 M",4588,false,null,182135,7512,4588,"6.360,00",33830,7512,"Sole|Wasser-Wärmepumpe WPF 13 M","Brine|water heat pump WPF 13 M","Brine|water heat pump WPF 13 M","Brine|water heat pump WPF 13 M","Glycol/water-warmtepompen WPF 13 M","Brine|water heat pump WPF 13 M","Brine|water heat pump WPF 13 M","Brine|water heat pump WPF 13 M","Brine|water heat pump WPF 13 M","Brine|water heat pump WPF 13 M","Brine|water heat pump WPF 13 M"]
[null,220894,"Brine|water heat pump WPF 16 M",5017,"",null,null,null,null,null,null,220894,"Brine|water heat pump WPF 16 M",5017,false,null,220894,8455,5017,"6.725,00",36535,8455,"Sole|Wasser-Wärmepumpe WPF 16 M","Brine|water heat pump WPF 16 M","Brine|water heat pump WPF 16 M","Brine|water heat pump WPF 16 M","Glycol/water-warmtepompen WPF 16 M","Brine|water heat pump WPF 16 M","Brine|water heat pump WPF 16 M","Brine|water heat pump WPF 16 M","Brine|water heat pump WPF 16 M","Brine|water heat pump WPF 16 M","Brine|water heat pump WPF 16 M"]
[null,185365,"Brine|water heat pump WPF 20 SET",11168,"",null,null,null,null,null,null,185365,"Brine|water heat pump WPF 20 SET",11168,false,null,185365,12777,11168,"14.750,00",76407,12777,"Sole|Wasser-Wärmepumpe WPF 20 SET","Brine|water heat pump WPF 20 SET","Brine|water heat pump WPF 20 SET","Brine|water heat pump WPF 20 SET","Glycol/water-warmtepompen WPF 20 Set","Brine|water heat pump WPF 20 SET","Brine|water heat pump WPF 20 SET","Brine|water heat pump WPF 20 SET","Brine|water heat pump WPF 20 SET","Brine|water heat pump WPF 20 SET","Brine|water heat pump WPF 20 SET"]
[null,185366,"Brine|water heat pump WPF 23 SET",11340,"",null,null,null,null,null,null,185366,"Brine|water heat pump WPF 23 SET",11340,false,null,185366,13024,11340,"14.965,00",77495,13024,"Sole|Wasser-Wärmepumpe WPF 23 SET","Brine|water heat pump WPF 23 SET","Brine|water heat pump WPF 23 SET","Brine|water heat pump WPF 23 SET","Glycol/water-warmtepompen WPF 23 Set","Brine|water heat pump WPF 23 SET","Brine|water heat pump WPF 23 SET","Brine|water heat pump WPF 23 SET","Brine|water heat pump WPF 23 SET","Brine|water heat pump WPF 23 SET","Brine|water heat pump WPF 23 SET"]
[null,182139,"Brine|water heat pump WPF 26 SET",11511,"",null,null,null,null,null,null,182139,"Brine|water heat pump WPF 26 SET",11511,false,null,182139,13177,11511,"15.170,00",78583,13177,"Sole|Wasser-Wärmepumpe WPF 26 SET","Brine|water heat pump WPF 26 SET","Brine|water heat pump WPF 26 SET","Brine|water heat pump WPF 26 SET","Glycol/water-warmtepompen WPF 26 Set","Brine|water heat pump WPF 26 SET","Brine|water heat pump WPF 26 SET","Brine|water heat pump WPF 26 SET","Brine|water heat pump WPF 26 SET","Brine|water heat pump WPF 26 SET","Brine|water heat pump WPF 26 SET"]
[null,220896,"Brine|water heat pump WPF 29 SET",11911,"",null,null,null,null,null,null,220896,"Brine|water heat pump WPF 29 SET",11911,false,null,220896,14566,11911,"15.540,00",81287,14566,"Sole|Wasser-Wärmepumpe WPF 29 SET","Brine|water heat pump WPF 29 SET","Brine|water heat pump WPF 29 SET","Brine|water heat pump WPF 29 SET","Glycol/water-warmtepompen WPF 29 Set","Brine|water heat pump WPF 29 SET","Brine|water heat pump WPF 29 SET","Brine|water heat pump WPF 29 SET","Brine|water heat pump WPF 29 SET","Brine|water heat pump WPF 29 SET","Brine|water heat pump WPF 29 SET"]
[null,220897,"Brine|water heat pump WPF 32 SET",12312,"",null,null,null,null,null,null,220897,"Brine|water heat pump WPF 32 SET",12312,false,null,220897,16710,12312,"15.910,00",83991,16710,"Sole|Wasser-Wärmepumpe WPF 32 SET","Brine|water heat pump WPF 32 SET","Brine|water heat pump WPF 32 SET","Brine|water heat pump WPF 32 SET","Glycol/water-warmtepompen WPF 32 Set","Brine|water heat pump WPF 32 SET","Brine|water heat pump WPF 32 SET","Brine|water heat pump WPF 32 SET","Brine|water heat pump WPF 32 SET","Brine|water heat pump WPF 32 SET","Brine|water heat pump WPF 32 SET"]
[null,233003,"Sole|Wasser-Wärmepumpe WPF 20",10913,"",null,null,null,null,null,null,233003,"Sole|Wasser-Wärmepumpe WPF 20",10913,false,null,233003,11099,10913,"13.820,00",74932,11099,"Sole|Wasser-Wärmepumpe WPF 20","Sole|Wasser-Wärmepumpe WPF 20","Sole|Wasser-Wärmepumpe WPF 20","Sole|Wasser-Wärmepumpe WPF 20","Glycol/water-warmtepompen WPF 20","Sole|Wasser-Wärmepumpe WPF 20","Sole|Wasser-Wärmepumpe WPF 20","Sole|Wasser-Wärmepumpe WPF 20","Sole|Wasser-Wärmepumpe WPF 20","Sole|Wasser-Wärmepumpe WPF 20","Sole|Wasser-Wärmepumpe WPF 20"]
[null,233004,"Sole|Wasser-Wärmepumpe WPF 27",11921,"",null,null,null,null,null,null,233004,"Sole|Wasser-Wärmepumpe WPF 27",11921,false,null,233004,12729,11921,"15.220,00",81861,12729,"Sole|Wasser-Wärmepumpe WPF 27","Sole|Wasser-Wärmepumpe WPF 27","Sole|Wasser-Wärmepumpe WPF 27","Sole|Wasser-Wärmepumpe WPF 27","Glycol/water-warmtepompen WPF 27","Sole|Wasser-Wärmepumpe WPF 27","Sole|Wasser-Wärmepumpe WPF 27","Sole|Wasser-Wärmepumpe WPF 27","Sole|Wasser-Wärmepumpe WPF 27","Sole|Wasser-Wärmepumpe WPF 27","Sole|Wasser-Wärmepumpe WPF 27"]
[null,233005,"Sole|Wasser-Wärmepumpe WPF 35",14209,"",null,null,null,null,null,null,233005,"Sole|Wasser-Wärmepumpe WPF 35",14209,false,null,233005,15237,14209,"17.990,00",97565,15237,"Sole|Wasser-Wärmepumpe WPF 35","Sole|Wasser-Wärmepumpe WPF 35","Sole|Wasser-Wärmepumpe WPF 35","Sole|Wasser-Wärmepumpe WPF 35","Glycol/water-warmtepompen WPF 35","Sole|Wasser-Wärmepumpe WPF 35","Sole|Wasser-Wärmepumpe WPF 35","Sole|Wasser-Wärmepumpe WPF 35","Sole|Wasser-Wärmepumpe WPF 35","Sole|Wasser-Wärmepumpe WPF 35","Sole|Wasser-Wärmepumpe WPF 35"]
[null,233006,"Sole|Wasser-Wärmepumpe WPF 40",14263,"",null,null,null,null,null,null,233006,"Sole|Wasser-Wärmepumpe WPF 40",14263,false,null,233006,16970,14263,"18.390,00",97938,16970,"Sole|Wasser-Wärmepumpe WPF 40","Sole|Wasser-Wärmepumpe WPF 40","Sole|Wasser-Wärmepumpe WPF 40","Sole|Wasser-Wärmepumpe WPF 40","Glycol/water-warmtepompen WPF 40","Sole|Wasser-Wärmepumpe WPF 40","Sole|Wasser-Wärmepumpe WPF 40","Sole|Wasser-Wärmepumpe WPF 40","Sole|Wasser-Wärmepumpe WPF 40","Sole|Wasser-Wärmepumpe WPF 40","Sole|Wasser-Wärmepumpe WPF 40"]
[null,233007,"Sole|Wasser-Wärmepumpe WPF 52",17351,"",null,null,null,null,null,null,233007,"Sole|Wasser-Wärmepumpe WPF 52",17351,false,null,233007,19983,17351,"22.050,00",119140,19983,"Sole|Wasser-Wärmepumpe WPF 52","Sole|Wasser-Wärmepumpe WPF 52","Sole|Wasser-Wärmepumpe WPF 52","Sole|Wasser-Wärmepumpe WPF 52","Glycol/water-warmtepompen WPF 52","Sole|Wasser-Wärmepumpe WPF 52","Sole|Wasser-Wärmepumpe WPF 52","Sole|Wasser-Wärmepumpe WPF 52","Sole|Wasser-Wärmepumpe WPF 52","Sole|Wasser-Wärmepumpe WPF 52","Sole|Wasser-Wärmepumpe WPF 52"]
[null,233008,"Sole|Wasser-Wärmepumpe WPF 66",19285,"",null,null,null,null,null,null,233008,"Sole|Wasser-Wärmepumpe WPF 66",19285,false,null,233008,23156,19285,"24.530,00",132424,23156,"Sole|Wasser-Wärmepumpe WPF 66","Sole|Wasser-Wärmepumpe WPF 66","Sole|Wasser-Wärmepumpe WPF 66","Sole|Wasser-Wärmepumpe WPF 66","Glycol/water-warmtepompen WPF 66","Sole|Wasser-Wärmepumpe WPF 66","Sole|Wasser-Wärmepumpe WPF 66","Sole|Wasser-Wärmepumpe WPF 66","Sole|Wasser-Wärmepumpe WPF 66","Sole|Wasser-Wärmepumpe WPF 66","Sole|Wasser-Wärmepumpe WPF 66"]
[null,227760,"Connection assembly 2 x WPF 20..66","On request","",null,null,null,null,null,null,227760,"Connection assembly 2 x WPF 20..66","On request",false,null,227760,143,"On request",215,1007,143,"Bausatz vertikale Montage 2 x WPF 20..66","Connection assembly 2 x WPF 20..66","Connection assembly 2 x WPF 20..66","Connection assembly 2 x WPF 20..66","Verbindingskit WPVB","Connection assembly 2 x WPF 20..66","Connection assembly 2 x WPF 20..66","Connection assembly 2 x WPF 20..66","Connection assembly 2 x WPF 20..66","Connection assembly 2 x WPF 20..66","Connection assembly 2 x WPF 20..66"]
[null,233009,"Sole|Wasser-Wärmepumpe WPF 27 HT",12746,"",null,null,null,null,null,null,233009,"Sole|Wasser-Wärmepumpe WPF 27 HT",12746,false,null,233009,15265,12746,"17.060,00",87523,15265,"Sole|Wasser-Wärmepumpe WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT","Glycol/water-warmtepompen WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT","Sole|Wasser-Wärmepumpe WPF 27 HT"]
[null,189999,"Air/heat module LWM 250",2252,"",null,null,null,null,null,null,189999,"Air/heat module LWM 250",2252,false,null,189999,2032,2252,"sur demande",15250,2032,"Abluftmodul LWM 250","Air/heat module LWM 250","Air/heat module LWM 250","Air/heat module LWM 250","Lucht/brinemodule LWM 250","Air/heat module LWM 250","Air/heat module LWM 250","Air/heat module LWM 250","Air/heat module LWM 250","Air/heat module LWM 250","Air/heat module LWM 250"]
[null,230659,"Groundwater module GWS 1",1800,"",null,null,null,null,null,null,230659,"Groundwater module GWS 1",1800,false,null,230659,1448,1800,"sur demande",11786,1448,"Modul Grundwassernutzung GWS 1","Groundwater module GWS 1","Groundwater module GWS 1","Groundwater module GWS 1","Grondwaterstation GWS 1","Groundwater module GWS 1","Groundwater module GWS 1","Groundwater module GWS 1","Groundwater module GWS 1","Groundwater module GWS 1","Groundwater module GWS 1"]
[null,230660,"Groundwater module GWS 2",2069,"",null,null,null,null,null,null,230660,"Groundwater module GWS 2",2069,false,null,230660,1785,2069,"sur demande",13380,1785,"Modul Grundwassernutzung GWS 2","Groundwater module GWS 2","Groundwater module GWS 2","Groundwater module GWS 2","Grondwaterstation GWS 2","Groundwater module GWS 2","Groundwater module GWS 2","Groundwater module GWS 2","Groundwater module GWS 2","Groundwater module GWS 2","Groundwater module GWS 2"]
[null,232460,"Soleverteiler WPSV 25-4",621,"",null,null,null,null,null,null,232460,"Soleverteiler WPSV 25-4",621,false,null,232460,681,621,875,4254,681,"Soleverteiler WPSV 25-4","Soleverteiler WPSV 25-4","Soleverteiler WPSV 25-4","Soleverteiler WPSV 25-4","Brineverdeler WPSV 25-4","Soleverteiler WPSV 25-4","Soleverteiler WPSV 25-4","Soleverteiler WPSV 25-4","Soleverteiler WPSV 25-4","Soleverteiler WPSV 25-4","Soleverteiler WPSV 25-4"]
[null,232461,"Soleverteiler WPSV 25-6",843,"",null,null,null,null,null,null,232461,"Soleverteiler WPSV 25-6",843,false,null,232461,904,843,"1.210,00",5781,904,"Soleverteiler WPSV 25-6","Soleverteiler WPSV 25-6","Soleverteiler WPSV 25-6","Soleverteiler WPSV 25-6","Brineverdeler WPSV 25-6","Soleverteiler WPSV 25-6","Soleverteiler WPSV 25-6","Soleverteiler WPSV 25-6","Soleverteiler WPSV 25-6","Soleverteiler WPSV 25-6","Soleverteiler WPSV 25-6"]
[null,232462,"Soleverteiler WPSV 32-4",641,{"$f":"IF(O244=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,232462,"Soleverteiler WPSV 32-4",641,false,null,232462,793,641,920,4396,793,"Soleverteiler WPSV 32-4","Soleverteiler WPSV 32-4","Soleverteiler WPSV 32-4","Soleverteiler WPSV 32-4","Brineverdeler WPSV 32-4","Soleverteiler WPSV 32-4","Soleverteiler WPSV 32-4","Soleverteiler WPSV 32-4","Soleverteiler WPSV 32-4","Soleverteiler WPSV 32-4","Soleverteiler WPSV 32-4"]
[null,232463,"Soleverteiler WPSV 32-6",877,"",null,null,null,null,null,null,232463,"Soleverteiler WPSV 32-6",877,false,null,232463,1015,877,"1.250,00",6005,1015,"Soleverteiler WPSV 32-6","Soleverteiler WPSV 32-6","Soleverteiler WPSV 32-6","Soleverteiler WPSV 32-6","Brineverdeler WPSV 32-6","Soleverteiler WPSV 32-6","Soleverteiler WPSV 32-6","Soleverteiler WPSV 32-6","Soleverteiler WPSV 32-6","Soleverteiler WPSV 32-6","Soleverteiler WPSV 32-6"]
[null,232464,"Soleverteiler WPSV 40-4",697,"",null,null,null,null,null,null,232464,"Soleverteiler WPSV 40-4",697,false,null,232464,838,697,"sur demande",4775,838,"Soleverteiler WPSV 40-4","Soleverteiler WPSV 40-4","Soleverteiler WPSV 40-4","Soleverteiler WPSV 40-4","Brineverdeler WPSV 40-4","Soleverteiler WPSV 40-4","Soleverteiler WPSV 40-4","Soleverteiler WPSV 40-4","Soleverteiler WPSV 40-4","Soleverteiler WPSV 40-4","Soleverteiler WPSV 40-4"]
[null,232465,"Soleverteiler WPSV 40-6",959,"",null,null,null,null,null,null,232465,"Soleverteiler WPSV 40-6",959,false,null,232465,1078,959,"sur demande",6571,1078,"Soleverteiler WPSV 40-6","Soleverteiler WPSV 40-6","Soleverteiler WPSV 40-6","Soleverteiler WPSV 40-6","Brineverdeler WPSV 40-6","Soleverteiler WPSV 40-6","Soleverteiler WPSV 40-6","Soleverteiler WPSV 40-6","Soleverteiler WPSV 40-6","Soleverteiler WPSV 40-6","Soleverteiler WPSV 40-6"]
[null,222375,"Brine assembly WPSB 308",860,"",null,null,null,null,null,null,222375,"Brine assembly WPSB 308",860,{"$f":"IF(AND(B248=L248,C248=M248,D248=N248),FALSE,TRUE)","v":false},null,222375,1025,860,"1.140,00",6288,1025,"Solebausatz WPSB 308 E","Brine assembly WPSB 308","Brine assembly WPSB 308","Brine assembly WPSB 308","Brinebouwset WPSB 308 E","Brine assembly WPSB 308","Brine assembly WPSB 308","Brine assembly WPSB 308","Brine assembly WPSB 308","Brine assembly WPSB 308","Brine assembly WPSB 308"]
[null,232883,"Solebausatz WPSB 312 E",1200,"",null,null,null,null,null,null,232883,"Solebausatz WPSB 312 E",1200,false,null,232883,1050,1200,"1.505,00",7182,1050,"Solebausatz WPSB 312 E","Solebausatz WPSB 312 E","Solebausatz WPSB 312 E","Solebausatz WPSB 312 E","Brinebouwset WPSB 312 E","Solebausatz WPSB 312 E","Solebausatz WPSB 312 E","Solebausatz WPSB 312 E","Solebausatz WPSB 312 E","Solebausatz WPSB 312 E","Solebausatz WPSB 312 E"]
[null,232884,"Solebausatz WPSB 408 E",1611,"",null,null,null,null,null,null,232884,"Solebausatz WPSB 408 E",1611,false,null,232884,1570,1611,"2.310,00",11063,1570,"Solebausatz WPSB 408 E","Solebausatz WPSB 408 E","Solebausatz WPSB 408 E","Solebausatz WPSB 408 E","Brinebouwset WPSB 408 E","Solebausatz WPSB 408 E","Solebausatz WPSB 408 E","Solebausatz WPSB 408 E","Solebausatz WPSB 408 E","Solebausatz WPSB 408 E","Solebausatz WPSB 408 E"]
[null,233307,"Sole-Fülleinheit WPSF",263,"",null,null,null,null,null,null,233307,"Sole-Fülleinheit WPSF",263,false,null,233307,304,263,"sur demande",1773,304,"Sole-Fülleinheit WPSF","Sole-Fülleinheit WPSF","Sole-Fülleinheit WPSF","Sole-Fülleinheit WPSF","Bron vulunit WPSF","Sole-Fülleinheit WPSF","Sole-Fülleinheit WPSF","Sole-Fülleinheit WPSF","Sole-Fülleinheit WPSF","Sole-Fülleinheit WPSF","Sole-Fülleinheit WPSF"]
[null,232532,"Sole-Umwälzpumpe UPF 30/1-8 E",515,"",null,null,null,null,null,null,232532,"Sole-Umwälzpumpe UPF 30/1-8 E",515,false,null,232532,546,515,690,3539,546,"Sole-Umwälzpumpe UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E","Bronpomp UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E","Sole-Umwälzpumpe UPF 30/1-8 E"]
[null,227413,"Brine circulation pump UPF 40/1-8 E",1205,"",null,null,null,null,null,null,227413,"Brine circulation pump UPF 40/1-8 E",1205,false,null,227413,1454,1205,"1.595,00",8560,1454,"Sole-Umwälzpumpe UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E","Bronpomp UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E","Brine circulation pump UPF 40/1-8 E"]
[null,227414,"Brine circulation pump UPF 50/1-12 E",1573,"",null,null,null,null,null,null,227414,"Brine circulation pump UPF 50/1-12 E",1573,false,null,227414,1849,1573,"2.060,00",11220,1849,"Sole-Umwälzpumpe UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E","Bronpomp UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E","Brine circulation pump UPF 50/1-12 E"]
[null,221382,"Brine pressure limiter DWS 1",100,"",null,null,null,null,null,null,221382,"Brine pressure limiter DWS 1",100,false,null,221382,111,100,135,637,111,"Soledruckwächter DWS 1","Brine pressure limiter DWS 1","Brine pressure limiter DWS 1","Brine pressure limiter DWS 1","Brinedrukbewaking DWS1","Brine pressure limiter DWS 1","Brine pressure limiter DWS 1","Brine pressure limiter DWS 1","Brine pressure limiter DWS 1","Brine pressure limiter DWS 1","Brine pressure limiter DWS 1"]
[null,189981,"Expansion vessel 12l",60,"",null,null,null,null,null,null,189981,"Expansion vessel 12l",60,false,null,189981,66,60,"sur demande",383,66,"Sole-Ausdehnungsgefäß MAG 12 l","Expansion vessel 12l","Expansion vessel 12l","Expansion vessel 12l","Expansievat MAG 12","Expansion vessel 12l","Expansion vessel 12l","Expansion vessel 12l","Expansion vessel 12l","Expansion vessel 12l","Expansion vessel 12l"]
[null,227415,"Expansion vessel 18 l",62,"",null,null,null,null,null,null,227415,"Expansion vessel 18 l",62,false,null,227415,66,62,85,420,66,"Sole-Ausdehnungsgefäß MAG 18 l","Expansion vessel 18 l","Expansion vessel 18 l","Expansion vessel 18 l","Expansievat MAG 18","Expansion vessel 18 l","Expansion vessel 18 l","Expansion vessel 18 l","Expansion vessel 18 l","Expansion vessel 18 l","Expansion vessel 18 l"]
[null,227416,"Expansion vessel 25 l",62,"",null,null,null,null,null,null,227416,"Expansion vessel 25 l",62,false,null,227416,74,62,95,418,74,"Sole-Ausdehnungsgefäß MAG 25 l","Expansion vessel 25 l","Expansion vessel 25 l","Expansion vessel 25 l","Expansievat MAG 25","Expansion vessel 25 l","Expansion vessel 25 l","Expansion vessel 25 l","Expansion vessel 25 l","Expansion vessel 25 l","Expansion vessel 25 l"]
[null,227417,"Expansion vessel 50 l",99,"",null,null,null,null,null,null,227417,"Expansion vessel 50 l",99,false,null,227417,101,99,145,700,101,"Sole-Ausdehnungsgefäß MAG 50 l","Expansion vessel 50 l","Expansion vessel 50 l","Expansion vessel 50 l","Expansievat MAG 50","Expansion vessel 50 l","Expansion vessel 50 l","Expansion vessel 50 l","Expansion vessel 50 l","Expansion vessel 50 l","Expansion vessel 50 l"]
[null,231109,"Heat transfer medium MEG 10 l",63,"",null,null,null,null,null,null,231109,"Heat transfer medium MEG 10 l",63,false,null,231109,78,63,100,413,78,"Wärmeträgerflüssigkeit MEG, 10l","Heat transfer medium MEG 10 l","Heat transfer medium MEG 10 l","Heat transfer medium MEG 10 l","MEG 10 L warmtedragervloeistof ","Heat transfer medium MEG 10 l","Heat transfer medium MEG 10 l","Heat transfer medium MEG 10 l","Heat transfer medium MEG 10 l","Heat transfer medium MEG 10 l","Heat transfer medium MEG 10 l"]
[null,161696,"Heat transfer medium MEG",187,"",null,null,null,null,null,null,161696,"Heat transfer medium MEG",187,false,null,161696,225,187,245,"på forespørgsel",225,"Wärmeträgerflüssigkeit MEG, 30l","Heat transfer medium MEG","Heat transfer medium MEG","Heat transfer medium MEG","MEG 30 L Warmtedragervloeistof ","Heat transfer medium MEG","Heat transfer medium MEG","Heat transfer medium MEG","Heat transfer medium MEG","Heat transfer medium MEG","Heat transfer medium MEG"]
[null,233903,"Sole|Wasser-Wärmepumpe WPD 6 Set","On request","",null,null,null,null,null,null,233903,"Sole|Wasser-Wärmepumpe WPD 6 Set","On request",false,null,233903,9551,"On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set","Glycol/water-warmtepompen WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set","Sole|Wasser-Wärmepumpe WPD 6 Set"]
[null,233904,"Sole|Wasser-Wärmepumpe WPD 8 Set","On request","",null,null,null,null,null,null,233904,"Sole|Wasser-Wärmepumpe WPD 8 Set","On request",false,null,233904,11267,"On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set","Glycol/water-warmtepompen WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set","Sole|Wasser-Wärmepumpe WPD 8 Set"]
[null,232948,"Wasser|Wasser-Wärmepumpe WPW 06 Set","On request","",null,null,null,null,null,null,232948,"Wasser|Wasser-Wärmepumpe WPW 06 Set","On request",false,null,232948,7973,"On request","sur demande","på forespørgsel","op aanvraag","Wasser|Wasser-Wärmepumpe WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set","Water/water-warmtepompen WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set","Wasser|Wasser-Wärmepumpe WPW 06 Set"]
[null,232949,"Wasser|Wasser-Wärmepumpe WPW 07 Set","On request","",null,null,null,null,null,null,232949,"Wasser|Wasser-Wärmepumpe WPW 07 Set","On request",false,null,232949,8388,"On request","sur demande","på forespørgsel","op aanvraag","Wasser|Wasser-Wärmepumpe WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set","Water/water-warmtepompen WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set","Wasser|Wasser-Wärmepumpe WPW 07 Set"]
[null,232950,"Wasser|Wasser-Wärmepumpe WPW 10 Set","On request","",null,null,null,null,null,null,232950,"Wasser|Wasser-Wärmepumpe WPW 10 Set","On request",false,null,232950,9131,"On request","sur demande","på forespørgsel","op aanvraag","Wasser|Wasser-Wärmepumpe WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set","Water/water-warmtepompen WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set","Wasser|Wasser-Wärmepumpe WPW 10 Set"]
[null,232951,"Wasser|Wasser-Wärmepumpe WPW 13 Set","On request","",null,null,null,null,null,null,232951,"Wasser|Wasser-Wärmepumpe WPW 13 Set","On request",false,null,232951,9901,"On request","sur demande","på forespørgsel","op aanvraag","Wasser|Wasser-Wärmepumpe WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set","Water/water-warmtepompen WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set","Wasser|Wasser-Wärmepumpe WPW 13 Set"]
[null,232952,"Wasser|Wasser-Wärmepumpe WPW 18 Set","On request","",null,null,null,null,null,null,232952,"Wasser|Wasser-Wärmepumpe WPW 18 Set","On request",false,null,232952,10474,"On request","sur demande","på forespørgsel","op aanvraag","Wasser|Wasser-Wärmepumpe WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set","Water/water-warmtepompen WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set","Wasser|Wasser-Wärmepumpe WPW 18 Set"]
[null,232953,"Wasser|Wasser-Wärmepumpe WPW 22 Set","On request","",null,null,null,null,null,null,232953,"Wasser|Wasser-Wärmepumpe WPW 22 Set","On request",false,null,232953,11534,"On request","sur demande","på forespørgsel","op aanvraag","Wasser|Wasser-Wärmepumpe WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set","Water/water-warmtepompen WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set","Wasser|Wasser-Wärmepumpe WPW 22 Set"]
[null,230915,"Water|water heat pump WPW 7 basic set",7484,"",null,null,null,null,null,null,230915,"Water|water heat pump WPW 7 basic set",7484,false,null,230915,6881,7484,"sur demande",49014,"op aanvraag","Wasser|Wasser-Wärmepumpe WPW 7 basic Set","Water|water heat pump WPW 7 basic set","Water|water heat pump WPW 7 basic set","Water|water heat pump WPW 7 basic set","Water/water-warmtepompen WPW 7 basic Set","Water|water heat pump WPW 7 basic set","Water|water heat pump WPW 7 basic set","Water|water heat pump WPW 7 basic set","Water|water heat pump WPW 7 basic set","Water|water heat pump WPW 7 basic set","Water|water heat pump WPW 7 basic set"]
[null,230916,"Water|water heat pump WPW 10 basic set",7990,"",null,null,null,null,null,null,230916,"Water|water heat pump WPW 10 basic set",7990,false,null,230916,7494,7990,"sur demande",51398,"op aanvraag","Wasser|Wasser-Wärmepumpe WPW 10 basic Set","Water|water heat pump WPW 10 basic set","Water|water heat pump WPW 10 basic set","Water|water heat pump WPW 10 basic set","Water/water-warmtepompen WPW 10 basic Set","Water|water heat pump WPW 10 basic set","Water|water heat pump WPW 10 basic set","Water|water heat pump WPW 10 basic set","Water|water heat pump WPW 10 basic set","Water|water heat pump WPW 10 basic set","Water|water heat pump WPW 10 basic set"]
[null,230917,"Water|water heat pump WPW 13 basic set",8097,"",null,null,null,null,null,null,230917,"Water|water heat pump WPW 13 basic set",8097,false,null,230917,8285,8097,"sur demande",53022,"op aanvraag","Wasser|Wasser-Wärmepumpe WPW 13 basic Set","Water|water heat pump WPW 13 basic set","Water|water heat pump WPW 13 basic set","Water|water heat pump WPW 13 basic set","Water/water-warmtepompen WPW 13 basic Set","Water|water heat pump WPW 13 basic set","Water|water heat pump WPW 13 basic set","Water|water heat pump WPW 13 basic set","Water|water heat pump WPW 13 basic set","Water|water heat pump WPW 13 basic set","Water|water heat pump WPW 13 basic set"]
[null,230918,"Water|water heat pump WPW 18 basic set",8764,"",null,null,null,null,null,null,230918,"Water|water heat pump WPW 18 basic set",8764,false,null,230918,8812,8764,"sur demande",55689,"op aanvraag","Wasser|Wasser-Wärmepumpe WPW 18 basic Set","Water|water heat pump WPW 18 basic set","Water|water heat pump WPW 18 basic set","Water|water heat pump WPW 18 basic set","Water/water-warmtepompen WPW 18 basic Set","Water|water heat pump WPW 18 basic set","Water|water heat pump WPW 18 basic set","Water|water heat pump WPW 18 basic set","Water|water heat pump WPW 18 basic set","Water|water heat pump WPW 18 basic set","Water|water heat pump WPW 18 basic set"]
[null,230919,"Water|water heat pump WPW 22 basic set",8995,"",null,null,null,null,null,null,230919,"Water|water heat pump WPW 22 basic set",8995,false,null,230919,10562,8995,"sur demande",56896,"op aanvraag","Wasser|Wasser-Wärmepumpe WPW 22 basic Set","Water|water heat pump WPW 22 basic set","Water|water heat pump WPW 22 basic set","Water|water heat pump WPW 22 basic set","Water/water-warmtepompen WPW 22 basic Set","Water|water heat pump WPW 22 basic set","Water|water heat pump WPW 22 basic set","Water|water heat pump WPW 22 basic set","Water|water heat pump WPW 22 basic set","Water|water heat pump WPW 22 basic set","Water|water heat pump WPW 22 basic set"]
[null,232980,"Wärmepumpen-Manager WPMW 3",577,"",null,null,null,null,null,null,232980,"Wärmepumpen-Manager WPMW 3",577,false,null,232980,942,577,720,3010,"op aanvraag","Wärmepumpen-Manager WPMW 3","Wärmepumpen-Manager WPMW 3","Wärmepumpen-Manager WPMW 3","Wärmepumpen-Manager WPMW 3","Warmtepompmanager WPMW 3","Wärmepumpen-Manager WPMW 3","Wärmepumpen-Manager WPMW 3","Wärmepumpen-Manager WPMW 3","Wärmepumpen-Manager WPMW 3","Wärmepumpen-Manager WPMW 3","Wärmepumpen-Manager WPMW 3"]
[null,232981,"Wärmepumpen-Manager WPMS 3",420,"",null,null,null,null,null,null,232981,"Wärmepumpen-Manager WPMS 3",420,false,null,232981,866,420,580,2883,"op aanvraag","Wärmepumpen-Manager WPMS 3","Wärmepumpen-Manager WPMS 3","Wärmepumpen-Manager WPMS 3","Wärmepumpen-Manager WPMS 3","Warmtepompmanager WPMS 3","Wärmepumpen-Manager WPMS 3","Wärmepumpen-Manager WPMS 3","Wärmepumpen-Manager WPMS 3","Wärmepumpen-Manager WPMS 3","Wärmepumpen-Manager WPMS 3","Wärmepumpen-Manager WPMS 3"]
[null,230381,"Relaisbox WPM-RBS",125,"",null,null,null,null,null,null,230381,"Relaisbox WPM-RBS",125,false,null,230381,96,125,185,820,96,"Relaisbausatz für Effizienzpumpen WPM-RBS","Relaisbox WPM-RBS","Relaisbox WPM-RBS","Relaisbox WPM-RBS","Relaiskast WPM-RBS","Relaisbox WPM-RBS","Relaisbox WPM-RBS","Relaisbox WPM-RBS","Relaisbox WPM-RBS","Relaisbox WPM-RBS","Relaisbox WPM-RBS"]
[null,74519,"Mixer module MSMW",527,"",null,null,null,null,null,null,74519,"Mixer module MSMW",527,false,null,74519,749,527,720,"på forespørgsel",749,"Zusatzregler Mischer/Schwimmbad MSMW","Mixer module MSMW","Mixer module MSMW","Mixer module MSMW","Mengmodule MSMW","Mixer module MSMW","Mixer module MSMW","Mixer module MSMW","Mixer module MSMW","Mixer module MSMW","Mixer module MSMW"]
[null,74518,"Mixer module MSMS",360,"",null,null,null,null,null,null,74518,"Mixer module MSMS",360,false,null,74518,672,360,510,"på forespørgsel",672,"Zusatzregler Mischer/Schwimmbad MSMS","Mixer module MSMS","Mixer module MSMS","Mixer module MSMS","Mengmodule MSMS","Mixer module MSMS","Mixer module MSMS","Mixer module MSMS","Mixer module MSMS","Mixer module MSMS","Mixer module MSMS"]
[null,185579,"Remote control FE 7",25,"",null,null,null,null,null,null,185579,"Remote control FE 7",25,false,null,185579,85,25,40,191,85,"Fernbedienung FE 7","Remote control FE 7","Remote control FE 7","Remote control FE 7","Afstandsbediening FE 7","Remote control FE 7","Remote control FE 7","Remote control FE 7","Remote control FE 7","Remote control FE 7","Remote control FE 7"]
[null,220193,"Remote control FEK",134,"",null,null,null,null,null,null,220193,"Remote control FEK",134,false,null,220193,251,134,190,976,251,"Fernbedienung FEK","Remote control FEK","Remote control FEK","Remote control FEK","Afstandsbediening FEK","Remote control FEK","Remote control FEK","Remote control FEK","Remote control FEK","Remote control FEK","Remote control FEK"]
[null,165341,"Contact sensor AVF 6",12,"",null,null,null,null,null,null,165341,"Contact sensor AVF 6",12,false,null,165341,25.5,12,20,"på forespørgsel",26,"Anlegefühler AVF 6","Contact sensor AVF 6","Contact sensor AVF 6","Contact sensor AVF 6","Aanlegvoeler AVF 6","Contact sensor AVF 6","Contact sensor AVF 6","Contact sensor AVF 6","Contact sensor AVF 6","Contact sensor AVF 6","Contact sensor AVF 6"]
[null,165342,"Immersion sensor TF 6 A",12,"",null,null,null,null,null,null,165342,"Immersion sensor TF 6 A",12,false,null,165342,29.5,12,20,"på forespørgsel",30,"Tauchfühler TF 6 A","Immersion sensor TF 6 A","Immersion sensor TF 6 A","Immersion sensor TF 6 A","Dompelvoeler TF 6","Immersion sensor TF 6 A","Immersion sensor TF 6 A","Immersion sensor TF 6 A","Immersion sensor TF 6 A","Immersion sensor TF 6 A","Immersion sensor TF 6 A"]
[null,165339,"Outside temperature sensor AFS 2",7,"",null,null,null,null,null,null,165339,"Outside temperature sensor AFS 2",7,false,null,165339,20.6,7,10,"på forespørgsel",21,"Außenfühler AFS 2","Outside temperature sensor AFS 2","Sonde extérieure AFS 2","Outside temperature sensor AFS 2","Buitenvoeler AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2"]
[null,229336,"Internet-Service Gateway ISG web","On request","",null,null,null,null,null,null,229336,"Internet-Service Gateway ISG web","On request",false,null,229336,483,"On request","Voir tarifs mises en service p.11",4776,483,"Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Service Internet passerelle ISG web","Internet-Service Gateway ISG web","Internet-Service-Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web"]
[null,233303,"KNX IP-Software für ISG web","On request","",null,null,null,null,null,null,233303,"KNX IP-Software für ISG web","On request",false,null,233303,331.93,"On request","sur demande","på forespørgsel","op aanvraag","KNX IP-Software für ISG web","KNX IP-Software für ISG web","KNX IP-Software für ISG web","KNX IP-Software für ISG web","Software KNX","KNX IP-Software für ISG web","KNX IP-Software für ISG web","KNX IP-Software für ISG web","KNX IP-Software für ISG web","KNX IP-Software für ISG web","KNX IP-Software für ISG web"]
[null,233236,"Software für Energie Management Interface EMI","On request","",null,null,null,null,null,null,233236,"Software für Energie Management Interface EMI","On request",false,null,233236,67.900000000000006,"On request","sur demande","på forespørgsel","op aanvraag","Software für Energie Management Interface EMI","Software für Energie Management Interface EMI","Software für Energie Management Interface EMI","Software für Energie Management Interface EMI","Software Energy Management Interface EMI","Software für Energie Management Interface EMI","Software für Energie Management Interface EMI","Software für Energie Management Interface EMI","Software für Energie Management Interface EMI","Software für Energie Management Interface EMI","Software für Energie Management Interface EMI"]
[null,233493,"Internet-Service Gateway ISG plus","On request","",null,null,null,null,null,null,233493,"Internet-Service Gateway ISG plus","On request",false,null,233493,632,"On request","sur demande","på forespørgsel","op aanvraag","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus"]
[null,231166,"Data station building control system","On request","",null,null,null,null,null,null,231166,"Data station building control system","On request",false,null,231166,1677,"On request","sur demande",16536,1677,"Datenwandler Gebäudeleittechnik Data Station","Data station building control system","Data station building control system","Data station building control system","Data station","Data station building control system","Data station building control system","Data station building control system","Data station building control system","Data station building control system","Data station building control system"]
[null,189622,"Communication module DCO aktiv GSM",210,"",null,null,null,null,null,null,189622,"Communication module DCO aktiv GSM",210,false,null,189622,293,210,"sur demande",1497,293,"DFÜ-Controller DCO aktiv GSM","Communication module DCO aktiv GSM","Communication module DCO aktiv GSM","Communication module DCO aktiv GSM","Dataoverdracht DCO actief GSM","Communication module DCO aktiv GSM","Communication module DCO aktiv GSM","Communication module DCO aktiv GSM","Communication module DCO aktiv GSM","Communication module DCO aktiv GSM","Communication module DCO aktiv GSM"]
[null,223358,"Electrical distribution bar SP cool",178,"",null,null,null,null,null,null,223358,"Electrical distribution bar SP cool",178,false,null,223358,158,178,"sur demande",1267,"op aanvraag","Elektrische Verteilerleiste SP cool","Electrical distribution bar SP cool","Electrical distribution bar SP cool","Electrical distribution bar SP cool","Verdeelblok SP cool","Electrical distribution bar SP cool","Electrical distribution bar SP cool","Electrical distribution bar SP cool","Electrical distribution bar SP cool","Electrical distribution bar SP cool","Electrical distribution bar SP cool"]
[null,182206,"Warm water cylinder SBB 150 WPF",1321,"",null,null,null,null,null,null,182206,"Warm water cylinder SBB 150 WPF",1321,false,null,182206,960,1321,"1.815,00","på forespørgsel",960,"Warmwasser-Wandspeicher SBB 150 WPF","Warm water cylinder SBB 150 WPF","Warm water cylinder SBB 150 WPF","Warm water cylinder SBB 150 WPF","Warmwaterboiler SBB 150 WPF","Warm water cylinder SBB 150 WPF","Warm water cylinder SBB 150 WPF","Warm water cylinder SBB 150 WPF","Warm water cylinder SBB 150 WPF","Warm water cylinder SBB 150 WPF","Warm water cylinder SBB 150 WPF"]
[null,185306,"Cylinder connection set SAS",350,"",null,null,null,null,null,null,185306,"Cylinder connection set SAS",350,false,null,185306,318,350,505,"på forespørgsel",318,"Speicheranschlussset SBB 150 WPF","Cylinder connection set SAS","Cylinder connection set SAS","Cylinder connection set SAS","Boileraansluitset SAS","Cylinder connection set SAS","Cylinder connection set SAS","Cylinder connection set SAS","Cylinder connection set SAS","Cylinder connection set SAS","Cylinder connection set SAS"]
[null,221360,"Warm water cylinder SBB 301 WP",1886,"",null,null,null,null,null,null,221360,"Warm water cylinder SBB 301 WP",1886,false,null,221360,1772,1886,"2.260,00",9052,1772,"Warmwasserspeicher SBB 301 WP","Warm water cylinder SBB 301 WP","Warm water cylinder SBB 301 WP","Warm water cylinder SBB 301 WP","Warmwaterboiler SBB 301 WP","Warm water cylinder SBB 301 WP","Warm water cylinder SBB 301 WP","Warm water cylinder SBB 301 WP","Warm water cylinder SBB 301 WP","Warm water cylinder SBB 301 WP","Warm water cylinder SBB 301 WP"]
[null,221361,"Warm water cylinder SBB 302 WP",2255,"",null,null,null,null,null,null,221361,"Warm water cylinder SBB 302 WP",2255,false,null,221361,2027,2255,"2.660,00",11086,2027,"Warmwasserspeicher SBB 302 WP","Warm water cylinder SBB 302 WP","Warm water cylinder SBB 302 WP","Warm water cylinder SBB 302 WP","Warmwaterboiler SBB 302 WP","Warm water cylinder SBB 302 WP","Warm water cylinder SBB 302 WP","Warm water cylinder SBB 302 WP","Warm water cylinder SBB 302 WP","Warm water cylinder SBB 302 WP","Warm water cylinder SBB 302 WP"]
[null,221362,"Warm water cylinder SBB 401 WP SOL",2135,"",null,null,null,null,null,null,221362,"Warm water cylinder SBB 401 WP SOL",2135,false,null,221362,2336,2135,"2.695,00",10728,2336,"Warmwasserspeicher SBB 401 WP SOL","Warm water cylinder SBB 401 WP SOL","Ballon ECS solaire (double échangeur) 400 litres SBB 401 WP SOL","Accumulatore solare SBB 401 WP SOL","Warmwaterboiler SBB 401 WP SOL","zásobník teplé vody SBB 401 WP SOL","Zásobníkový ohrievač vody SBB 401 WP SOL","Zasobnik ciepłej wody   SBB 401 WP SOL","Melegvíztároló SBB 401 WP SOL","Käyttövesivaraaja SBB 401 WP SOL","Warm water cylinder SBB 401 WP SOL"]
[null,227534,"Warm water cylinder SBB 501 WP SOL",2435,"",null,null,null,null,null,null,227534,"Warm water cylinder SBB 501 WP SOL",2435,false,null,227534,2569,2435,"3.080,00",12903,2569,"Warmwasserspeicher SBB 501 WP SOL","Warm water cylinder SBB 501 WP SOL","Ballon ECS solaire (double échangeur) 500 litres SBB 501 WP SOL","Accumulatore solare SBB 501 WP SOL","Warmwaterboiler SBB 501 WP SOL","zásobník teplé vody SBB 501 WP SOL","Zásobníkový ohrievač vody SBB 501 WP SOL","Zasobnik ciepłej wody   SBB 501 WP SOL","Melegvíztároló SBB 501 WP SOL","Käyttövesivaraaja SBB 501 WP SOL","Warm water cylinder SBB 501 WP SOL"]
[null,232628,"Wellrohrverbinder Wärmeübertrager WRV 32",107,"",null,null,null,null,null,null,232628,"Wellrohrverbinder Wärmeübertrager WRV 32",107,false,null,232628,103,107,155,733,103,"Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","WRV 32 - Elément permettant de raccorder les échangeurs sup. et inf. des ballons SBB 401/501 WP SOL","Wellrohrverbinder Wärmeübertrager WRV 32","Doorverbinding warmtewisselaar WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32","Wellrohrverbinder Wärmeübertrager WRV 32"]
[null,233487,"Warmwasserspeicher SBB 300 WP trend",1302,"",null,null,null,null,null,null,233487,"Warmwasserspeicher SBB 300 WP trend",1302,false,null,233487,1264,1302,"1.875,00",8917,1264,"Warmwasserspeicher SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend","Warmwaterboiler SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend","Warmwasserspeicher SBB 300 WP trend"]
[null,233488,"Warmwasserspeicher SBB 400 WP trend",1768,"",null,null,null,null,null,null,233488,"Warmwasserspeicher SBB 400 WP trend",1768,false,null,233488,1629,1768,"2.385,00",12109,1629,"Warmwasserspeicher SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend","Warmwaterboiler SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend","Warmwasserspeicher SBB 400 WP trend"]
[null,233489,"Warmwasserspeicher SBB 500 WP trend",1956,"",null,null,null,null,null,null,233489,"Warmwasserspeicher SBB 500 WP trend",1956,false,null,233489,1893,1956,"2.695,00",13400,1893,"Warmwasserspeicher SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend","Warmwaterboiler SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend","Warmwasserspeicher SBB 500 WP trend"]
[null,229292,"Warm water cylinder SBB 751",2020,{"$f":"IF(O302=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,229292,"Warm water cylinder SBB 751",2020,false,null,229292,2231,2020,"2.780,00",11957,2231,"Warmwasserspeicher SBB 751","Warm water cylinder SBB 751","Warm water cylinder SBB 751","Warm water cylinder SBB 751","Warmwaterboiler SBB 751","Warm water cylinder SBB 751","Warm water cylinder SBB 751","Warm water cylinder SBB 751","Warm water cylinder SBB 751","Warm water cylinder SBB 751","Warm water cylinder SBB 751"]
[null,229294,"Warm water cylinder SBB 751 SOL",2384,"",null,null,null,null,null,null,229294,"Warm water cylinder SBB 751 SOL",2384,false,null,229294,2572,2384,"3.050,00",13693,2572,"Warmwasserspeicher SBB 751 SOL","Warm water cylinder SBB 751 SOL","Ballon ECS solaire (1 échangeur solaire) de 750 litres SBB 751 SOL ","Accumulatore solare SBB 751 SOL","Warmwaterboiler SBB 751 SOL","zásobník teplé vody SBB 751 SOL","Zásobníkový ohrievač vody SBB 751 SOL","Zasobnik ciepłej wody SBB 751 SOL","Melegvíztároló SBB 751 SOL","Käyttövesivaraaja SBB 751 SOL","Warm water cylinder SBB 751 SOL"]
[null,229293,"Warm water cylinder SBB 1001",2347,"",null,null,null,null,null,null,229293,"Warm water cylinder SBB 1001",2347,{"$f":"IF(AND(B304=L304,C304=M304,D304=N304),FALSE,TRUE)","v":false},null,229293,2546,2347,"3.080,00",16688,2546,"Warmwasserspeicher SBB 1001","Warm water cylinder SBB 1001","Warm water cylinder SBB 1001","Warm water cylinder SBB 1001","Warmwaterboiler SBB 1001","Warm water cylinder SBB 1001","Warm water cylinder SBB 1001","Warm water cylinder SBB 1001","Warm water cylinder SBB 1001","Warm water cylinder SBB 1001","Warm water cylinder SBB 1001"]
[null,229295,"Warm water cylinder SBB 1001 SOL",2868,"",null,null,null,null,null,null,229295,"Warm water cylinder SBB 1001 SOL",2868,false,null,229295,3111,2868,"3.370,00",20391,3111,"Warmwasserspeicher SBB 1001 SOL","Warm water cylinder SBB 1001 SOL","Ballon ECS solaire (1 échangeur solaire) de 1000 litres SBB 1001 SOL ","Accumulatore solare SBB 1001 SOL","Warmwaterboiler SBB 1001 SOL","zásobník teplé vody SBB 1001 SOL","Zásobníkový ohrievač vody SBB 1001 SOL","Zasobnik ciepłej wody SBB 1001 SOL","Melegvíztároló SBB 1001 SOL","Käyttövesivaraaja SBB 1001 SOL","Warm water cylinder SBB 1001 SOL"]
[null,231923,"Thermal insulation WDH 751 SBB",595,"",null,null,null,null,null,null,231923,"Thermal insulation WDH 751 SBB",595,false,null,231923,600,595,740,3837,600,"Wärmedämmung WDH 751 SBB","Thermal insulation WDH 751 SBB","Isolation renforcée WDH 751 SBB pour SBB 751 (SOL). ","Isolazione WDH 751 SBB","Isolatie WDH 751 SBB","tepelná izolace WDH 751 SBB","Tepelná izolácia WDH 751 SBB","Ocieplenie WDH 751 SBB","Hőszigetelés WDH 751 SBB","Lämmöneristys WDH 751  SBB","Thermal insulation WDH 751 SBB"]
[null,231924,"Thermal insulation WDH 1001 SBB",661,"",null,null,null,null,null,null,231924,"Thermal insulation WDH 1001 SBB",661,false,null,231924,681,661,815,4232,681,"Wärmedämmung WDH 1001 SBB","Thermal insulation WDH 1001 SBB","Isolation renforcée WDH 1001 SBB pour SBB 1001 (SOL)","Isolazione WDH 1001 SBB","Isolatie WDH 1001 SBB","tepelná izolace WDH 1001 SBB","Tepelná izolácia WDH 1001 SBB","Ocieplenie WDH 1001 SBB","Hőszigetelés WDH 1001 SBB","Lämmöneristys WDH 1001  SBB","Thermal insulation WDH 1001 SBB"]
[null,232907,"Loading station WTS 30 E",2970,"",null,null,null,null,null,null,232907,"Loading station WTS 30 E",2970,false,null,232907,3675,2970,"3.780,00",20391,3675,"Ladestation Warmwasserbereitung WTS 30 E","Loading station WTS 30 E","Station de charge WTS 30 E","stazione di carica WTS 30 E","Laadstation WTS 30 E","ohřívací stanice WTS 30 E","Výmenníková stanica WTS 30 E","Stacja ładowania WTS 30 E","Hőcserélő állomás WTS 30 E","Latausasema WTS 30 E","Loading station WTS 30 E"]
[null,232908,"Loading station WTS 40 E",4350,"",null,null,null,null,null,null,232908,"Loading station WTS 40 E",4350,false,null,232908,4775,4350,"5.455,00",29867,4775,"Ladestation Warmwasserbereitung WTS 40 E","Loading station WTS 40 E","Station de charge WTS 40 E","stazione di carica WTS 40 E","Laadstation WTS 40 E","ohřívací stanice WTS 40 E","Výmenníková stanica WTS 40 E","Stacja ładowania WTS 40 E","Hőcserélő állomás WTS 40 E","Latausasema WTS 40 E","Loading station WTS 40 E"]
[null,231910,"Warm water cylinder SBB 600 WP SOL",2991,"",null,null,null,null,null,null,231910,"Warm water cylinder SBB 600 WP SOL",2991,false,null,231910,3319,2991,"3.805,00",20949,3319,"Warmwasserspeicher SBB 600 WP SOL","Warm water cylinder SBB 600 WP SOL","Ballon ECS solaire (double échangeur) de 575 litres SBB 600 WP SOL ","Accumulatore solare SBB 600 WP SOL","Warmwaterboiler SBB 600 WP SOL","zásobník teplé vody SBB 600 WP SOL","Zásobníkový ohrievač vody SBB 600 WP SOL","Zasobnik ciepłej wody SBB 600 WP SOL","Melegvíztároló SBB 600 WP SOL","Käyttövesivaraaja SBB 600 WP SOL","Warm water cylinder SBB 600 WP SOL"]
[null,231911,"Warm water cylinder SBB 800 WP SOL",3327,"",null,null,null,null,null,null,231911,"Warm water cylinder SBB 800 WP SOL",3327,false,null,231911,3690,3327,"4.120,00",23304,3690,"Warmwasserspeicher SBB 800 WP SOL","Warm water cylinder SBB 800 WP SOL","Ballon ECS solaire (double échangeur) de 770 litres SBB 800 WP SOL ","Accumulatore solare SBB 800 WP SOL","Warmwaterboiler SBB 800 WP SOL","zásobník teplé vody SBB 800 WP SOL","Zásobníkový ohrievač vody SBB 800 WP SOL","Zasobnik ciepłej wody SBB 800 WP SOL","Melegvíztároló SBB 800 WP SOL","Käyttövesivaraaja SBB 800 WP SOL","Warm water cylinder SBB 800 WP SOL"]
[null,231912,"Warm water cylinder SBB 1000 WP SOL",3690,"",null,null,null,null,null,null,231912,"Warm water cylinder SBB 1000 WP SOL",3690,false,null,231912,4024,3690,"4.420,00",25844,4024,"Warmwasserspeicher SBB 1000 WP SOL","Warm water cylinder SBB 1000 WP SOL","Ballon ECS solaire (double échangeur) de 835 litres SBB 1000 WP SOL ","Accumulatore solare SBB 1000 WP SOL","Warmwaterboiler SBB 1000 WP SOL","zásobník teplé vody SBB 1000 WP SOL","Zásobníkový ohrievač vody SBB 1000 WP SOL","Zasobnik ciepłej wody SBB 1000 WP SOL","Melegvíztároló SBB 1000 WP SOL","Käyttövesivaraaja SBB 1000 WP SOL","Warm water cylinder SBB 1000 WP SOL"]
[null,231957,"Thermal insulation WDH 600 SBB",576,"",null,null,null,null,null,null,231957,"Thermal insulation WDH 600 SBB",576,false,null,231957,584,576,740,3837,584,"Wärmedämmung WDH 600 SBB","Thermal insulation WDH 600 SBB","Isolation WDH 600 SBB pour SBB 600 WP SOL","Isolazione WDH 600 SBB","Isolatie WDH 600 SBB","tepelná izolace WDH 600 SBB","Tepelná izolácia WDH 600 SBB","Ocieplenie WDH 600 SBB","Hőszigetelés WDH 600 SBB","Lämmöneristys WDH 600  SBB","Thermal insulation WDH 600 SBB"]
[null,231958,"Thermal insulation WDH 800 SBB",610,"",null,null,null,null,null,null,231958,"Thermal insulation WDH 800 SBB",610,false,null,231958,611,610,785,4068,611,"Wärmedämmung WDH 800 SBB","Thermal insulation WDH 800 SBB","Isolation WDH 800 SBB pour SBB 800 WP SOL","Isolazione WDH 800 SBB","Isolatie WDH 800 SBB","tepelná izolace WDH 800 SBB","Tepelná izolácia WDH 800 SBB","Ocieplenie WDH 800 SBB","Hőszigetelés WDH 800 SBB","Lämmöneristys WDH 800  SBB","Thermal insulation WDH 800 SBB"]
[null,231959,"Thermal insulation WDH 1000 SBB",674,"",null,null,null,null,null,null,231959,"Thermal insulation WDH 1000 SBB",674,false,null,231959,678,674,870,4492,678,"Wärmedämmung WDH 1000 SBB","Thermal insulation WDH 1000 SBB","Isolation WDH 1000 SBB pour SBB 1000 WP SOL","Isolazione WDH 1000 SBB","Isolatie WDH 1000 SBB","tepelná izolace WDH 1000 SBB","Tepelná izolácia WDH 1000 SBB","Ocieplenie WDH 1000 SBB","Hőszigetelés WDH 1000 SBB","Lämmöneristys WDH 1000  SBB","Thermal insulation WDH 1000 SBB"]
[null,232629,"Wellrohrverbinder Wärmeübertrager WRV 40",217,"",null,null,null,null,null,null,232629,"Wellrohrverbinder Wärmeübertrager WRV 40",217,false,null,232629,206,217,310,1490,206,"Wellrohrverbinder Wärmeübertrager WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40","Doorverbinding warmtewisselaar WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40","Wellrohrverbinder Wärmeübertrager WRV 40"]
[null,229980,"Instantaneous cylinder SBS 601 W",2230,"",null,null,null,null,null,null,229980,"Instantaneous cylinder SBS 601 W",2230,false,null,229980,2442,2230,"3.100,00",14602,2442,"Durchlaufspeicher SBS 601 W","Instantaneous cylinder SBS 601 W","Instantaneous cylinder SBS 601 W","Instantaneous cylinder SBS 601 W","Doorstroomboiler SBS 601 W","Instantaneous cylinder SBS 601 W","Instantaneous cylinder SBS 601 W","Instantaneous cylinder SBS 601 W","Instantaneous cylinder SBS 601 W","Instantaneous cylinder SBS 601 W","Instantaneous cylinder SBS 601 W"]
[null,229984,"Instantaneous cylinder SBS 601 W SOL",2628,"",null,null,null,null,null,null,229984,"Instantaneous cylinder SBS 601 W SOL",2628,false,null,229984,2879,2628,"3.465,00",17210,2879,"Durchlaufspeicher SBS 601 W SOL","Instantaneous cylinder SBS 601 W SOL","Ballon solaire combiné à production ECS instantanée SBS 601 W SOL ","Accumulatore istantaneo SBS 601 W SOL","Doorstroomboiler SBS 601 W SOL","průtokový zásobník SBS 601 W SOL","Prietokový zásobníkový ohrievač vody SBS 601 W SOL","Zasobnik przepływowy SBS 601 W SOL","Átfolyó jellegű HMV tároló SBS 601 W SOL","Läpivirtausvaraaja SBS 601 W SOL","Instantaneous cylinder SBS 601 W SOL"]
[null,229981,"Instantaneous cylinder SBS 801 W",2490,"",null,null,null,null,null,null,229981,"Instantaneous cylinder SBS 801 W",2490,false,null,229981,2726,2490,"3.195,00",16308,2726,"Durchlaufspeicher SBS 801 W","Instantaneous cylinder SBS 801 W","Instantaneous cylinder SBS 801 W","Instantaneous cylinder SBS 801 W","Doorstroomboiler SBS 801 W","Instantaneous cylinder SBS 801 W","Instantaneous cylinder SBS 801 W","Instantaneous cylinder SBS 801 W","Instantaneous cylinder SBS 801 W","Instantaneous cylinder SBS 801 W","Instantaneous cylinder SBS 801 W"]
[null,229985,"Instantaneous cylinder SBS 801 W SOL",2876,"",null,null,null,null,null,null,229985,"Instantaneous cylinder SBS 801 W SOL",2876,false,null,229985,3150,2876,"3.630,00",18834,3150,"Durchlaufspeicher SBS 801 W SOL","Instantaneous cylinder SBS 801 W SOL","Ballon solaire combiné à production ECS instantanée SBS 801 W SOL","Accumulatore istantaneo SBS 801 W SOL","Doorstroomboiler SBS 801 W SOL","průtokový zásobník SBS 801 W SOL","Prietokový zásobníkový ohrievač vody SBS 801 W SOL","Zasobnik przepływowy SBS 801 W SOL","Átfolyó jellegű HMV tároló SBS 801 W SOL","Läpivirtausvaraaja SBS 801 W SOL","Instantaneous cylinder SBS 801 W SOL"]
[null,229982,"Instantaneous cylinder SBS 1001 W",2855,"",null,null,null,null,null,null,229982,"Instantaneous cylinder SBS 1001 W",2855,false,null,229982,3128,2855,"3.540,00",18700,3128,"Durchlaufspeicher SBS 1001 W","Instantaneous cylinder SBS 1001 W","Instantaneous cylinder SBS 1001 W","Instantaneous cylinder SBS 1001 W","Doorstroomboiler SBS 1001 W","Instantaneous cylinder SBS 1001 W","Instantaneous cylinder SBS 1001 W","Instantaneous cylinder SBS 1001 W","Instantaneous cylinder SBS 1001 W","Instantaneous cylinder SBS 1001 W","Instantaneous cylinder SBS 1001 W"]
[null,229986,"Instantaneous cylinder SBS 1001 W SOL",3343,"",null,null,null,null,null,null,229986,"Instantaneous cylinder SBS 1001 W SOL",3343,false,null,229986,3661,3343,"4.060,00",21896,3661,"Durchlaufspeicher SBS 1001 W SOL","Instantaneous cylinder SBS 1001 W SOL","Ballon solaire combiné à production ECS instantanée SBS 1001 W SOL","Accumulatore istantaneo SBS 1001 W SOL","Doorstroomboiler SBS 1001 W SOL","průtokový zásobník SBS 1001 W SOL","Prietokový zásobníkový ohrievač vody SBS 1001 W SOL","Zasobnik przepływowy SBS 1001 W SOL","Átfolyó jellegű HMV tároló SBS 1001 W SOL","Läpivirtausvaraaja SBS 1001 W SOL","Instantaneous cylinder SBS 1001 W SOL"]
[null,229983,"Instantaneous cylinder SBS 1501 W",3387,"",null,null,null,null,null,null,229983,"Instantaneous cylinder SBS 1501 W",3387,false,null,229983,3707,3387,"4.340,00",22179,3707,"Durchlaufspeicher SBS 1501 W","Instantaneous cylinder SBS 1501 W","Instantaneous cylinder SBS 1501 W","Instantaneous cylinder SBS 1501 W","Doorstroomboiler SBS 1501 W","Instantaneous cylinder SBS 1501 W","Instantaneous cylinder SBS 1501 W","Instantaneous cylinder SBS 1501 W","Instantaneous cylinder SBS 1501 W","Instantaneous cylinder SBS 1501 W","Instantaneous cylinder SBS 1501 W"]
[null,229987,"Instantaneous cylinder SBS 1501 W SOL",3897,"",null,null,null,null,null,null,229987,"Instantaneous cylinder SBS 1501 W SOL",3897,false,null,229987,4267,3897,"4.875,00",25524,4267,"Durchlaufspeicher SBS 1501 W SOL","Instantaneous cylinder SBS 1501 W SOL","Ballon solaire combiné à production ECS instantanée SBS 1501 W SOL","Accumulatore istantaneo SBS 1501 W SOL","Doorstroomboiler SBS 1501 W SOL","průtokový zásobník SBS 1501 W SOL","Prietokový zásobníkový ohrievač vody SBS 1501 W SOL","Zasobnik przepływowy SBS 1501 W SOL","Átfolyó jellegű HMV tároló SBS 1501 W SOL","Läpivirtausvaraaja SBS 1501 W SOL","Instantaneous cylinder SBS 1501 W SOL"]
[null,231925,"Thermal insulation WDH 601 SBS",582,"",null,null,null,null,null,null,231925,"Thermal insulation WDH 601 SBS",582,false,null,231925,554,582,750,3881,554,"Wärmedämmung WDH 601 SBS","Thermal insulation WDH 601 SBS","Isolation renforcée WDH 601 SBS pour SBS 601 W (SOL)","Isolazione WDH 601 SBS","Isolatie WDH 601 SBS","tepelná izolace WDH 601 SBS","Tepelná izolácia WDH 601 SBS","Ocieplenie WDH 601 SBS","Hőszigetelés WDH 601 SBS","Lämmöneriste WDH 601 SBS","Thermal insulation WDH 601 SBS"]
[null,231926,"Thermal insulation WDH 801 SBS",610,"",null,null,null,null,null,null,231926,"Thermal insulation WDH 801 SBS",610,false,null,231926,610,610,785,4068,610,"Wärmedämmung WDH 801 SBS","Thermal insulation WDH 801 SBS","Isolation renforcée WDH 801 SBS pour SBS 801 W (SOL)","Isolazione WDH 801 SBS","Isolatie WDH 801 SBS","tepelná izolace WDH 801 SBS","Tepelná izolácia WDH 801 SBS","Ocieplenie WDH 801 SBS","Hőszigetelés WDH 801 SBS","Lämmöneriste WDH 801 SBS","Thermal insulation WDH 801 SBS"]
[null,231927,"Thermal insulation WDH 1001 SBS",674,"",null,null,null,null,null,null,231927,"Thermal insulation WDH 1001 SBS",674,false,null,231927,680,674,870,4492,680,"Wärmedämmung WDH 1001 SBS","Thermal insulation WDH 1001 SBS","Isolation renforcée WDH 1001 SBS pour SBS 1001 W (SOL)","Isolazione WDH 1001 SBS","Isolatie WDH 1001 SBS","tepelná izolace WDH 1001 SBS","Tepelná izolácia WDH 1001 SBS","Ocieplenie WDH 1001 SBS","Hőszigetelés WDH 1001 SBS","Lämmöneriste WDH 1001 SBS","Thermal insulation WDH 1001 SBS"]
[null,231928,"Thermal insulation WDH 1501 SBS",769,"",null,null,null,null,null,null,231928,"Thermal insulation WDH 1501 SBS",769,false,null,231928,782,769,995,5133,782,"Wärmedämmung WDH 1501 SBS","Thermal insulation WDH 1501 SBS","Isolation renforcée WDH 1501 SBS pour SBS 1501 W (SOL)","Isolazione WDH 1501 SBS","Isolatie WDH 1501 SBS","tepelná izolace WDH 1501 SBS","Tepelná izolácia WDH 1501 SBS","Ocieplenie WDH 1501 SBS","Hőszigetelés WDH 1501 SBS","Lämmöneriste WDH 1501 SBS","Thermal insulation WDH 1501 SBS"]
[null,230312,"DHW Circulation set ZW 1 1/4",94,"",null,null,null,null,null,null,230312,"DHW Circulation set ZW 1 1/4",94,false,null,230312,124,94,140,616,124,"Zirkulationsset Durchlaufspeicher ZW 1 1/4","DHW Circulation set ZW 1 1/4","Set de circulation ZW 1 1/4 pour ballons combinés SBS","Set di circolazione accumulatore combinato ZW 1 1/4","Circulatieset ZW 1 1/4","cirkulační sada k průtokovému zásobníku ZW 1 1/4","Cirkulačná sada pre prietokový zásobník ZW 1 1/4","DHW Circulation set ZW 1 1/4","Cirkulációs szett átfolyó jellegű HMV tárolóhoz ZW 1 1/4","Käyttöveden kiertokytkentä ZW 1 1/4","DHW Circulation set ZW 1 1/4"]
[null,233719,"Trinkwasser-Zirkulationspumpe UPZ",264,"",null,null,null,null,null,null,233719,"Trinkwasser-Zirkulationspumpe UPZ",264,false,null,233719,255,264,380,1842,255,"Trinkwasser-Zirkulationspumpe UPZ","Trinkwasser-Zirkulationspumpe UPZ","Trinkwasser-Zirkulationspumpe UPZ","Trinkwasser-Zirkulationspumpe UPZ","Drinkwater-Circulatiepompen UPZ","Trinkwasser-Zirkulationspumpe UPZ","Trinkwasser-Zirkulationspumpe UPZ","Trinkwasser-Zirkulationspumpe UPZ","Trinkwasser-Zirkulationspumpe UPZ","Trinkwasser-Zirkulationspumpe UPZ","Trinkwasser-Zirkulationspumpe UPZ"]
[null,56899,"Circulation pump UPS 25-60 B",153,"",null,null,null,null,null,null,56899,"Circulation pump UPS 25-60 B",153,false,null,56899,301,153,235,"på forespørgsel",301,"Bronze-Umwälzpumpe UPS 25-60 B","Circulation pump UPS 25-60 B","Circulation pump UPS 25-60 B","Circulation pump UPS 25-60 B","Circulatiepomp UP 25-60 B","Circulation pump UPS 25-60 B","Circulation pump UPS 25-60 B","Circulation pump UPS 25-60 B","Circulation pump UPS 25-60 B","Circulation pump UPS 25-60 B","Circulation pump UPS 25-60 B"]
[null,72997,"Inlet pipe 200/400 l","On request","",null,null,null,null,null,null,72997,"Inlet pipe 200/400 l","On request",false,null,72997,166,"On request","sur demande","på forespørgsel","op aanvraag","Einströmrohr Trinkwasserspeicher 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Instroombuis 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l"]
[null,72998,"Inlet pipe 600/1000 l",168,"",null,null,null,null,null,null,72998,"Inlet pipe 600/1000 l",168,false,null,72998,186,168,"sur demande","på forespørgsel",186,"Einströmrohr Trinkwasserspeicher 600/1000 l","Inlet pipe 600/1000 l","Inlet pipe 600/1000 l","Inlet pipe 600/1000 l","Instroombuis 600/1000 l","Inlet pipe 600/1000 l","Inlet pipe 600/1000 l","Inlet pipe 600/1000 l","Inlet pipe 600/1000 l","Inlet pipe 600/1000 l","Inlet pipe 600/1000 l"]
[null,70633,"Heat exchanger WT 10",778,"",null,null,null,null,null,null,70633,"Heat exchanger WT 10",778,false,null,70633,944,778,820,"på forespørgsel",944,"Wärmetauscher WT 10","Heat exchanger WT 10","Echangeur de chaleur WT 10","Scambiatore WT 10","Warmtewisselaar WT 10","tepelný výměník WT 10","Doskový výmenník tepla WT 10","Wymiennik ciepła  WT 10","Hőcserélő WT 10","Levylämmönvaihdin WT 10","Heat exchanger WT 10"]
[null,70634,"Heat exchanger WT 20",809,"",null,null,null,null,null,null,70634,"Heat exchanger WT 20",809,false,null,70634,1290,809,880,"på forespørgsel",1290,"Wärmetauscher WT 20","Heat exchanger WT 20","Echangeur de chaleur WT 20","Scambiatore WT 20","Warmtewisselaar WT 20","tepelný výměník WT 20","Doskový výmenník tepla WT 20","Wymiennik ciepła  WT 20","Hőcserélő WT 20","Levylämmönvaihdin WT 20","Heat exchanger WT 20"]
[null,71091,"Heat exchanger WT 30",1291,"",null,null,null,null,null,null,71091,"Heat exchanger WT 30",1291,false,null,71091,1609,1291,"1.400,00","på forespørgsel",1609,"Wärmetauscher WT 30","Heat exchanger WT 30","Echangeur de chaleur WT 30","Scambiatore WT 30","Warmtewisselaar WT 30","tepelný výměník WT 30","Doskový výmenník tepla WT 30","Wymiennik ciepła  WT 30","Hőcserélő WT 30","Levylämmönvaihdin WT 30","Heat exchanger WT 30"]
[null,229338,"Heat exchanger WT 40",1787,"",null,null,null,null,null,null,229338,"Heat exchanger WT 40",1787,false,null,229338,1948,1787,"1.495,00",12710,1948,"Wärmetauscher WT 40","Heat exchanger WT 40","Echangeur de chaleur WT 40","Scambiatore WT 40","Warmtewisselaar WT 40","tepelný výměník WT 40","Doskový výmenník tepla WT 40","Wymiennik ciepła  WT 40","Hőcserélő WT 40","Levylämmönvaihdin WT 40","Heat exchanger WT 40"]
[null,185443,"Buffer cylinder SBP 100",541,"",null,null,null,null,null,null,185443,"Buffer cylinder SBP 100",541,false,null,185443,659,541,615,"på forespørgsel",659,"Wandhängender Pufferspeicher SBP 100","Buffer cylinder SBP 100","Buffer cylinder SBP 100","Buffer cylinder SBP 100","Buffervat SBP 100","Buffer cylinder SBP 100","Buffer cylinder SBP 100","Buffer cylinder SBP 100","Buffer cylinder SBP 100","Buffer cylinder SBP 100","Buffer cylinder SBP 100"]
[null,227590,"Buffer cylinder SBP 200 E cool",819,"",null,null,null,null,null,null,227590,"Buffer cylinder SBP 200 E cool",819,false,null,227590,822,819,940,5237,822,"Pufferspeicher SBP 200 E cool","Buffer cylinder SBP 200 E cool","Buffer cylinder SBP 200 E cool","Buffer cylinder SBP 200 E cool","Buffervat SBP 200 E cool","Buffer cylinder SBP 200 E cool","Buffer cylinder SBP 200 E cool","Buffer cylinder SBP 200 E cool","Buffer cylinder SBP 200 E cool","Buffer cylinder SBP 200 E cool","Buffer cylinder SBP 200 E cool"]
[null,227591,"Buffer cylinder SBP 400 E cool",883,"",null,null,null,null,null,null,227591,"Buffer cylinder SBP 400 E cool",883,false,null,227591,949,883,"1.090,00",6027,949,"Pufferspeicher SBP 400 E cool","Buffer cylinder SBP 400 E cool","Buffer cylinder SBP 400 E cool","Buffer cylinder SBP 400 E cool","Buffervat SBP 400 E cool","Buffer cylinder SBP 400 E cool","Buffer cylinder SBP 400 E cool","Buffer cylinder SBP 400 E cool","Buffer cylinder SBP 400 E cool","Buffer cylinder SBP 400 E cool","Buffer cylinder SBP 400 E cool"]
[null,185458,"Buffer cylinder SBP 200 E",748,"",null,null,null,null,null,null,185458,"Buffer cylinder SBP 200 E",748,false,null,185458,750,748,865,"på forespørgsel",750,"Pufferspeicher SBP 200 E","Buffer cylinder SBP 200 E","Buffer cylinder SBP 200 E","Buffer cylinder SBP 200 E","Buffervat SBP 200 E","Buffer cylinder SBP 200 E","Buffer cylinder SBP 200 E","Buffer cylinder SBP 200 E","Buffer cylinder SBP 200 E","Buffer cylinder SBP 200 E","Buffer cylinder SBP 200 E"]
[null,220824,"Buffer cylinder SBP 400 E",819,"",null,null,null,null,null,null,220824,"Buffer cylinder SBP 400 E",819,false,null,220824,908,819,"1.015,00",5804,908,"Pufferspeicher SBP 400 E","Buffer cylinder SBP 400 E","Buffer cylinder SBP 400 E","Buffer cylinder SBP 400 E","Buffervat SBP 400 E","Buffer cylinder SBP 400 E","Buffer cylinder SBP 400 E","Buffer cylinder SBP 400 E","Buffer cylinder SBP 400 E","Buffer cylinder SBP 400 E","Buffer cylinder SBP 400 E"]
[null,185459,"Buffer cylinder SBP 700 E",1277,"",null,null,null,null,null,null,185459,"Buffer cylinder SBP 700 E",1277,false,null,185459,1477,1277,"1.675,00","på forespørgsel",1477,"Pufferspeicher SBP 700 E","Buffer cylinder SBP 700 E","Buffer cylinder SBP 700 E","Buffer cylinder SBP 700 E","Buffervat SBP 700 E","Buffer cylinder SBP 700 E","Buffer cylinder SBP 700 E","Buffer cylinder SBP 700 E","Buffer cylinder SBP 700 E","Buffer cylinder SBP 700 E","Buffer cylinder SBP 700 E"]
[null,185460,"Buffer cylinder SBP 700 E SOL",1652,"",null,null,null,null,null,null,185460,"Buffer cylinder SBP 700 E SOL",1652,false,null,185460,1799,1652,"2.100,00",10408,1799,"Pufferspeicher SBP 700 E SOL","Buffer cylinder SBP 700 E SOL","Ballon tampon solaire 700 litres SBP 700 E SOL","Accumulatore SBP 700 E SOL","Buffervat SBP 700 E SOL","akumulační zásobník SBP 700 E SOL","Akumulačný zásobník SBP 700 E SOL","Bufor SBP 700 E SOL","Puffertároló SBP 700 E SOL","Puskurivaraaja SBP 700 E SOL","Buffer cylinder SBP 700 E SOL"]
[null,227564,"Buffer cylinder SBP 1000 E",1665,"",null,null,null,null,null,null,227564,"Buffer cylinder SBP 1000 E",1665,false,null,227564,1427,1665,"1.635,00",9059,1427,"Pufferspeicher SBP 1000 E","Buffer cylinder SBP 1000 E","Buffer cylinder SBP 1000 E","Buffer cylinder SBP 1000 E","Buffervat SBP 1000 E","Buffer cylinder SBP 1000 E","Buffer cylinder SBP 1000 E","Buffer cylinder SBP 1000 E","Buffer cylinder SBP 1000 E","Buffer cylinder SBP 1000 E","Buffer cylinder SBP 1000 E"]
[null,227565,"Buffer cylinder SBP 1500 E",1974,"",null,null,null,null,null,null,227565,"Buffer cylinder SBP 1500 E",1974,false,null,227565,1625,1974,"1.850,00",10311,1625,"Pufferspeicher SBP 1500 E","Buffer cylinder SBP 1500 E","Buffer cylinder SBP 1500 E","Buffer cylinder SBP 1500 E","Buffervat SBP 1500 E","Buffer cylinder SBP 1500 E","Buffer cylinder SBP 1500 E","Buffer cylinder SBP 1500 E","Buffer cylinder SBP 1500 E","Buffer cylinder SBP 1500 E","Buffer cylinder SBP 1500 E"]
[null,227566,"Buffer cylinder SBP 1000 E SOL",2181,"",null,null,null,null,null,null,227566,"Buffer cylinder SBP 1000 E SOL",2181,false,null,227566,1849,2181,"2.365,00",13142,1849,"Pufferspeicher SBP 1000 E SOL","Buffer cylinder SBP 1000 E SOL","Ballon tampon solaire 1000 litres  SBP 1000 E SOL","Accumulatore SBP 1000 E SOL","Buffervat SBP 1000 E SOL","akumulační zásobník SBP 1000 E SOL","Akumulačný zásobník SBP 1000 E SOL","Bufor SBP 1000 E SOL","Puffertároló SBP 1000 E SOL","Puskurivaraaja SBP 1000 E SOL","Buffer cylinder SBP 1000 E SOL"]
[null,227567,"Buffer cylinder SBP 1500 E SOL",2564,"",null,null,null,null,null,null,227567,"Buffer cylinder SBP 1500 E SOL",2564,false,null,227567,2115,2564,"2.750,00",14729,2115,"Pufferspeicher SBP 1500 E SOL","Buffer cylinder SBP 1500 E SOL","Ballon tampon solaire 1500 litres SBP 1500 E SOL","Accumulatore SBP 1500 E SOL","Buffervat SBP 1500 E SOL","akumulační zásobník SBP 1500 E SOL","Akumulačný zásobník SBP 1500 E SOL","Bufor SBP 1500 E SOL","Puffertároló SBP 1500 E SOL","Puskurivaraaja SBP 1500 E SOL","Buffer cylinder SBP 1500 E SOL"]
[null,227588,"Buffer cylinder SBP 1000 E cool",2314,"",null,null,null,null,null,null,227588,"Buffer cylinder SBP 1000 E cool",2314,false,null,227588,2427,2314,"2.770,00",15407,2427,"Pufferspeicher SBP 1000 E cool","Buffer cylinder SBP 1000 E cool","Buffer cylinder SBP 1000 E cool","Buffer cylinder SBP 1000 E cool","Buffervat SBP 1000 E cool","Buffer cylinder SBP 1000 E cool","Buffer cylinder SBP 1000 E cool","Buffer cylinder SBP 1000 E cool","Buffer cylinder SBP 1000 E cool","Buffer cylinder SBP 1000 E cool","Buffer cylinder SBP 1000 E cool"]
[null,227589,"Buffer cylinder SBP 1500 E cool",2733,"",null,null,null,null,null,null,227589,"Buffer cylinder SBP 1500 E cool",2733,false,null,227589,2781,2733,"3.180,00",17671,2781,"Pufferspeicher SBP 1500 E cool","Buffer cylinder SBP 1500 E cool","Buffer cylinder SBP 1500 E cool","Buffer cylinder SBP 1500 E cool","Buffervat SBP 1500 E cool","Buffer cylinder SBP 1500 E cool","Buffer cylinder SBP 1500 E cool","Buffer cylinder SBP 1500 E cool","Buffer cylinder SBP 1500 E cool","Buffer cylinder SBP 1500 E cool","Buffer cylinder SBP 1500 E cool"]
[null,231929,"Thermal insulation WDH 1000 SBP",661,"",null,null,null,null,null,null,231929,"Thermal insulation WDH 1000 SBP",661,false,null,231929,689,661,800,4232,689,"Wärmedämmung WDH 1000 SBP","Thermal insulation WDH 1000 SBP","Isolation renforcée WDH 1000 SBP pour SBP 1000 E (SOL)","Isolazione WDH 1000 SBP","Isolatie WDH 1000 SBP","tepelná izolace WDH 1000 SBP","Tepelná izolácia WDH 1000 SBP","Ocieplenie WDH 1000 SBP","Hőszigetelés WDH 1000 SBP","Lämmöneriste WDH 1000 SBP","Thermal insulation WDH 1000 SBP"]
[null,231930,"Thermal insulation WDH 1500 SBP",761,"",null,null,null,null,null,null,231930,"Thermal insulation WDH 1500 SBP",761,false,null,231930,785,761,940,4865,785,"Wärmedämmung WDH 1500 SBP","Thermal insulation WDH 1500 SBP","Isolation renforcée WDH 1500 SBP pour SBP 1500 E (SOL)","Isolazione WDH 1500 SBP","Isolatie WDH 1500 SBP","tepelná izolace WDH 1500 SBP","Tepelná izolácia WDH 1500 SBP","Ocieplenie WDH 1500 SBP","Hőszigetelés WDH 1500 SBP","Lämmöneriste WDH 1500 SBP","Thermal insulation WDH 1500 SBP"]
[null,231921,"Thermal insulation WDH 1000 SBP cool",596,"",null,null,null,null,null,null,231921,"Thermal insulation WDH 1000 SBP cool",596,false,null,231921,614,596,740,3837,614,"Wärmedämmung WDH 1000 SBP cool","Thermal insulation WDH 1000 SBP cool","Thermal insulation WDH 1000 SBP cool","Thermal insulation WDH 1000 SBP cool","Isolatie WDH 1000 cool","Thermal insulation WDH 1000 SBP cool","Thermal insulation WDH 1000 SBP cool","Thermal insulation WDH 1000 SBP cool","Thermal insulation WDH 1000 SBP cool","Thermal insulation WDH 1000 SBP cool","Thermal insulation WDH 1000 SBP cool"]
[null,231922,"Thermal insulation WDH 1500 SBP cool",679,"",null,null,null,null,null,null,231922,"Thermal insulation WDH 1500 SBP cool",679,false,null,231922,689,679,845,4388,689,"Wärmedämmung WDH 1500 SBP cool","Thermal insulation WDH 1500 SBP cool","Thermal insulation WDH 1500 SBP cool","Thermal insulation WDH 1500 SBP cool","Isolatie WDH 1500 cool","Thermal insulation WDH 1500 SBP cool","Thermal insulation WDH 1500 SBP cool","Thermal insulation WDH 1500 SBP cool","Thermal insulation WDH 1500 SBP cool","Thermal insulation WDH 1500 SBP cool","Thermal insulation WDH 1500 SBP cool"]
[null,231739,"Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","On request","",null,null,null,null,null,null,231739,"Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","On request",false,null,231739,6623,"On request","sur demande","på forespørgsel","op aanvraag","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Buffervat SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G","Pufferspeicher mit Gas-Brennwertgerät SBP 750 G"]
[null,231750,"Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","On request","",null,null,null,null,null,null,231750,"Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","On request",false,null,231750,7156,"On request","sur demande","på forespørgsel","op aanvraag","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Buffervat SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G","Pufferspeicher mit Gas-Brennwertgerät SBP 950 G"]
[null,231884,"Dummy flange BF 80",116,"",null,null,null,null,null,null,231884,"Dummy flange BF 80",116,false,null,231884,105,116,165,775,105,"Blindflansch BF 80 für SBP 1000/1500","Dummy flange BF 80","Dummy flange BF 80","Dummy flange BF 80","Blindflens BF 80","Dummy flange BF 80","Dummy flange BF 80","Dummy flange BF 80","Dummy flange BF 80","Dummy flange BF 80","Dummy flange BF 80"]
[null,231885,"Flange reducer FG 80/2",162,"",null,null,null,null,null,null,231885,"Flange reducer FG 80/2",162,false,null,231885,151,162,"sur demande",1073,151,"Flanschreduzierung DN 80 / G 2 A","Flange reducer FG 80/2","Flange reducer FG 80/2","Flange reducer FG 80/2","Flensverloop FG 80/2","Flange reducer FG 80/2","Flange reducer FG 80/2","Flange reducer FG 80/2","Flange reducer FG 80/2","Flange reducer FG 80/2","Flange reducer FG 80/2"]
[null,232942,"Umwälzpumpe UP 25/1-7.0 E",172,"",null,null,null,null,null,null,232942,"Umwälzpumpe UP 25/1-7.0 E",172,false,null,232942,222,172,245,1177,222,"Umwälzpumpe UP 25/7.0 E","Umwälzpumpe UP 25/1-7.0 E","Umwälzpumpe UP 25/1-7.0 E","Umwälzpumpe UP 25/1-7.0 E","Circulatiepomp UP 25/7.0 E","Umwälzpumpe UP 25/1-7.0 E","Umwälzpumpe UP 25/1-7.0 E","Umwälzpumpe UP 25/1-7.0 E","Umwälzpumpe UP 25/1-7.0 E","Umwälzpumpe UP 25/1-7.0 E","Umwälzpumpe UP 25/1-7.0 E"]
[null,232943,"Umwälzpumpe UP 25/1-7.5 E",180,"",null,null,null,null,null,null,232943,"Umwälzpumpe UP 25/1-7.5 E",180,false,null,232943,247,180,260,1237,247,"Umwälzpumpe UP 25/7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Circulatiepomp UP 25/7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E"]
[null,233561,"Umwälzpumpe UP 25/1-8 E",414,"",null,null,null,null,null,null,233561,"Umwälzpumpe UP 25/1-8 E",414,false,null,233561,508,414,545,2648,508,"Umwälzpumpe UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E","Circulatiepomp UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E","Umwälzpumpe UP 25/1-8 E"]
[null,222374,"Circulation pump UP 30/1-8 E",402,"",null,null,null,null,null,null,222374,"Circulation pump UP 30/1-8 E",402,false,null,222374,510,402,575,2751,510,"Umwälzpumpe UP 30/1-8 E","Circulation pump UP 30/1-8 E","Circulation pump UP 30/1-8 E","Circulation pump UP 30/1-8 E","Circulatiepomp UP 30/1-8 E","Circulation pump UP 30/1-8 E","Circulation pump UP 30/1-8 E","Circulation pump UP 30/1-8 E","Circulation pump UP 30/1-8 E","Circulation pump UP 30/1-8 E","Circulation pump UP 30/1-8 E"]
[null,227422,"Circulation pump UP 40/1-8 E",1132,{"$f":"IF(O363=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,227422,"Circulation pump UP 40/1-8 E",1132,false,null,227422,1303,1132,"1.435,00",8076,1303,"Umwälzpumpe UP 40/1-8 E","Circulation pump UP 40/1-8 E","Circulation pump UP 40/1-8 E","Circulation pump UP 40/1-8 E","Circulatiepomp UP 40/1-8 E","Circulation pump UP 40/1-8 E","Circulation pump UP 40/1-8 E","Circulation pump UP 40/1-8 E","Circulation pump UP 40/1-8 E","Circulation pump UP 40/1-8 E","Circulation pump UP 40/1-8 E"]
[null,227423,"Circulation pump UP 50/1-12 E",1477,"",null,null,null,null,null,null,227423,"Circulation pump UP 50/1-12 E",1477,false,null,227423,1699,1477,"1.845,00",10534,1699,"Umwälzpumpe UP 50/1-12 E","Circulation pump UP 50/1-12 E","Circulation pump UP 50/1-12 E","Circulation pump UP 50/1-12 E","Circulatiepomp UP 50/1-12 E","Circulation pump UP 50/1-12 E","Circulation pump UP 50/1-12 E","Circulation pump UP 50/1-12 E","Circulation pump UP 50/1-12 E","Circulation pump UP 50/1-12 E","Circulation pump UP 50/1-12 E"]
[null,74347,"Compact installation \tWPKI-V",210,"",null,null,null,null,null,null,74347,"Compact installation \tWPKI-V",210,false,null,74347,245,210,245,"på forespørgsel",245,"Kompaktinstallation WPKI-V","Compact installation \tWPKI-V","Compact installation \tWPKI-V","Compact installation \tWPKI-V","Compacte installatie WPKI-V","Compact installation \tWPKI-V","Compact installation \tWPKI-V","Compact installation \tWPKI-V","Compact installation \tWPKI-V","Compact installation \tWPKI-V","Compact installation \tWPKI-V"]
[null,233097,"Kompaktinstallation WPKI-P E",408,"",null,null,null,null,null,null,233097,"Kompaktinstallation WPKI-P E",408,false,null,233097,406,408,580,2749,406,"Kompaktinstallation WPKI-P E","Kompaktinstallation WPKI-P E","Kompaktinstallation WPKI-P E","Kompaktinstallation WPKI-P E","Compacte installatie WPKI-P E","Kompaktinstallation WPKI-P E","Kompaktinstallation WPKI-P E","Kompaktinstallation WPKI-P E","Kompaktinstallation WPKI-P E","Kompaktinstallation WPKI-P E","Kompaktinstallation WPKI-P E"]
[null,233098,"Kompaktinstallation WPKI-H E",233,"",null,null,null,null,null,null,233098,"Kompaktinstallation WPKI-H E",233,{"$f":"IF(AND(B367=L367,C367=M367,D367=N367),FALSE,TRUE)","v":false},null,233098,291,233,335,1587,291,"Kompaktinstallation WPKI-H E","Kompaktinstallation WPKI-H E","Kompaktinstallation WPKI-H E","Kompaktinstallation WPKI-H E","Compacte installatie WPKI-H E","Kompaktinstallation WPKI-H E","Kompaktinstallation WPKI-H E","Kompaktinstallation WPKI-H E","Kompaktinstallation WPKI-H E","Kompaktinstallation WPKI-H E","Kompaktinstallation WPKI-H E"]
[null,233099,"Kompaktinstallation WPKI-W E",239,"",null,null,null,null,null,null,233099,"Kompaktinstallation WPKI-W E",239,false,null,233099,248,239,340,1617,248,"Kompaktinstallation WPKI-W E","Kompaktinstallation WPKI-W E","Kompaktinstallation WPKI-W E","Kompaktinstallation WPKI-W E","Compacte installatie WPKI-W E","Kompaktinstallation WPKI-W E","Kompaktinstallation WPKI-W E","Kompaktinstallation WPKI-W E","Kompaktinstallation WPKI-W E","Kompaktinstallation WPKI-W E","Kompaktinstallation WPKI-W E"]
[null,234763,"Compact installation WPKI 5",383,"",null,null,null,null,null,null,234763,"Compact installation WPKI 5",383,false,null,234763,420,383,470,2332,420,"Kompaktinstallation WPKI 5","Compact installation WPKI 5","Compact installation WPKI 5","Compact installation WPKI 5","Compacte installatie WPKI 5","Compact installation WPKI 5","Compact installation WPKI 5","Compact installation WPKI 5","Compact installation WPKI 5","Compact installation WPKI 5","Compact installation WPKI 5"]
[null,234764,"Compact installation BBI 5",140,"",null,null,null,null,null,null,234764,"Compact installation BBI 5",140,false,null,234764,198,140,225,849,198,"Kompaktinstallation BBI 5","Compact installation BBI 5","Compact installation BBI 5","Compact installation BBI 5","Compacte installatie BBI 5","Compact installation BBI 5","Compact installation BBI 5","Compact installation BBI 5","Compact installation BBI 5","Compact installation BBI 5","Compact installation BBI 5"]
[null,234762,"Compact installation WPKI 6",251,"",null,null,null,null,null,null,234762,"Compact installation WPKI 6",251,false,null,234762,240,251,320,1445,240,"Kompaktinstallation WPKI 6","Compact installation WPKI 6","Compact installation WPKI 6","Compact installation WPKI 6","Compacte installatie WPKI 6","Compact installation WPKI 6","Compact installation WPKI 6","Compact installation WPKI 6","Compact installation WPKI 6","Compact installation WPKI 6","Compact installation WPKI 6"]
[null,3711,"Connection components SBP",51,"",null,null,null,null,null,null,3711,"Connection components SBP",51,false,null,3711,60,51,"sur demande","på forespørgsel",60,"Einlegeteile für SBP 200/400/700","Connection components SBP","Connection components SBP","Connection components SBP","Inlegdelen SBP inlegdelen ","Connection components SBP","Connection components SBP","Connection components SBP","Connection components SBP","Connection components SBP","Connection components SBP"]
[null,233602,"Kompaktinstallation WPKI-HK E",408,"",null,null,null,null,null,null,233602,"Kompaktinstallation WPKI-HK E",408,false,null,233602,459,408,585,2840,459,"Kompaktinstallation WPKI-HK E","Kompaktinstallation WPKI-HK E","Kompaktinstallation WPKI-HK E","Kompaktinstallation WPKI-HK E","Compacte installatie WPKI-HK E","Kompaktinstallation WPKI-HK E","Kompaktinstallation WPKI-HK E","Kompaktinstallation WPKI-HK E","Kompaktinstallation WPKI-HK E","Kompaktinstallation WPKI-HK E","Kompaktinstallation WPKI-HK E"]
[null,233603,"Kompaktinstallation WPKI-HKM E",583,"",null,null,null,null,null,null,233603,"Kompaktinstallation WPKI-HKM E",583,false,null,233603,622,583,835,4051,622,"Kompaktinstallation WPKI-HKM E","Kompaktinstallation WPKI-HKM E","Kompaktinstallation WPKI-HKM E","Kompaktinstallation WPKI-HKM E","Compacte installatie WPKI-HKM E","Kompaktinstallation WPKI-HKM E","Kompaktinstallation WPKI-HKM E","Kompaktinstallation WPKI-HKM E","Kompaktinstallation WPKI-HKM E","Kompaktinstallation WPKI-HKM E","Kompaktinstallation WPKI-HKM E"]
[null,221142,"Connecting manifold WPKI-HKV",246,"",null,null,null,null,null,null,221142,"Connecting manifold WPKI-HKV",246,false,null,221142,247,246,325,1609,247,"Verbindungsverteiler WPKI-HKV","Connecting manifold WPKI-HKV","Connecting manifold WPKI-HKV","Connecting manifold WPKI-HKV","Verbindingsverdeler WPKI-HKV","Connecting manifold WPKI-HKV","Connecting manifold WPKI-HKV","Connecting manifold WPKI-HKV","Connecting manifold WPKI-HKV","Connecting manifold WPKI-HKV","Connecting manifold WPKI-HKV"]
[null,221141,"Pipe assembly kit for Buffer WPKI-RB",165,"",null,null,null,null,null,null,221141,"Pipe assembly kit for Buffer WPKI-RB",165,false,null,221141,183,165,220,1080,183,"Rohrbausatz Anschluss Pufferspeicher WPKI-RB","Pipe assembly kit for Buffer WPKI-RB","Pipe assembly kit for Buffer WPKI-RB","Pipe assembly kit for Buffer WPKI-RB","Buizenset WPKI-RB","Pipe assembly kit for Buffer WPKI-RB","Pipe assembly kit for Buffer WPKI-RB","Pipe assembly kit for Buffer WPKI-RB","Pipe assembly kit for Buffer WPKI-RB","Pipe assembly kit for Buffer WPKI-RB","Pipe assembly kit for Buffer WPKI-RB"]
[null,232943,"Umwälzpumpe UP 25/1-7.5 E",180,"",null,null,null,null,null,null,232943,"Umwälzpumpe UP 25/1-7.5 E",180,false,null,232943,247,180,260,1237,247,"Umwälzpumpe UP 25/7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Circulatiepomp UP 25/7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E","Umwälzpumpe UP 25/1-7.5 E"]
[null,221135,"Low loss header WPHW 25",308,"",null,null,null,null,null,null,221135,"Low loss header WPHW 25",308,false,null,221135,290,308,425,2026,290,"Hydraulische Weiche WPHW 25","Low loss header WPHW 25","Low loss header WPHW 25","Low loss header WPHW 25","Openverdeler WPHW 25","Low loss header WPHW 25","Low loss header WPHW 25","Low loss header WPHW 25","Low loss header WPHW 25","Low loss header WPHW 25","Low loss header WPHW 25"]
[null,74252,"Electric booster heater SBP-HF",293,"",null,null,null,null,null,null,74252,"Electric booster heater SBP-HF",293,false,null,74252,248,293,405,"på forespørgsel",248,"Elektro-Zusatzheizung SBP-HF","Electric booster heater SBP-HF","Electric booster heater SBP-HF","Electric booster heater SBP-HF","SBP-HF elektrische bijverwarming","Electric booster heater SBP-HF","Electric booster heater SBP-HF","Electric booster heater SBP-HF","Electric booster heater SBP-HF","Electric booster heater SBP-HF","Electric booster heater SBP-HF"]
[null,3769,"Electrical heating flange BGC",221,"",null,null,null,null,null,null,3769,"Electrical heating flange BGC",221,false,null,3769,357,221,"sur demande","på forespørgsel",357,"Einschraubheizkörper BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC","Verwarmingselement BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC"]
[null,75115,"Threaded immersion heater BGC/45",238,"",null,null,null,null,null,null,75115,"Threaded immersion heater BGC/45",238,false,null,75115,399,238,335,1565,399,"Einschraubheizkörper BGC/45","Threaded immersion heater BGC/45","Corps de chauffe à visser BGC","Resistenza elettrica BGC","Verwarmingselement BGC/45","šroubovací topné těleso BGC","Skrutkovacie teleso BGC","Electric threaded immersion heater BGC","Becsavarható fűtőelem BGC","Sähkövastus BGC","Threaded immersion heater BGC/45"]
[null,232029,"Einschraubheizkörper BGC 2",235,"",null,null,null,null,null,null,232029,"Einschraubheizkörper BGC 2",235,false,null,232029,386,235,"sur demande",1612,386,"Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Verwarmingselement BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2"]
[null,232030,"Einschraubheizkörper BGC 2/60",267,"",null,null,null,null,null,null,232030,"Einschraubheizkörper BGC 2/60",267,false,null,232030,435,267,"sur demande",1827,435,"Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Verwarmingselement BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60"]
[null,74233,"Pipe assembly WPRB",78,"",null,null,null,null,null,null,74233,"Pipe assembly WPRB",78,false,null,74233,107,78,115,467,107,"Rohrbausatz für elektr. Nacherwärmung WPRB","Pipe assembly WPRB","Tube d'adaptation pour BGC, WPRB","Tubo di raccordo per resistenza elettrica WPRB","Buiskit WPRB buiskit","konstrukční sada pro el.dohřev WPRB","Nadstavec pre el. Doohrev WPRB","Pipe assembly WPRB WPRB","Csőkészlet elektromos utófűtőhöz WPRB","Putkiasennussarja WPRB","Pipe assembly WPRB"]
[null,694,"Electrical heating flange FCR 28/120",774,"",null,null,null,null,null,null,694,"Electrical heating flange FCR 28/120",774,false,null,694,1227,774,"1.115,00","på forespørgsel",1227,"Elektro-Heizflansch FCR 28/120 (12 KW)","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Elektrische flens FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120"]
[null,695,"Electrical heating flange FCR 28/180",821,"",null,null,null,null,null,null,695,"Electrical heating flange FCR 28/180",821,false,null,695,1370,821,"1.395,00","på forespørgsel",1370,"Elektro-Heizflansch FCR 28/180 (18 KW)","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Elektrische flens FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180"]
[null,696,"Electrical heating flange FCR 28/760",955,"",null,null,null,null,null,null,696,"Electrical heating flange FCR 28/760",955,false,null,696,1660,955,"1.580,00","på forespørgsel",1660,"Elektro-Heizflansch FCR 28/270 (27 KW)","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Elektrische flens FCR 28/270","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760"]
[null,1502,"Electrical heating flange FCR 28/360",917,"",null,null,null,null,null,null,1502,"Electrical heating flange FCR 28/360",917,false,null,1502,1942,917,"1.520,00","på forespørgsel",1942,"Elektro-Heizflansch FCR 28/360 (36 KW)","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Elektrische flens FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360"]
[null,71332,"Electrical heating flange FCR 28/120",815,"",null,null,null,null,null,null,71332,"Electrical heating flange FCR 28/120",815,false,null,71332,1275,815,"1.375,00","på forespørgsel",1275,"Elektro-Heizflansch FCR 28/120 (6/12 KW)","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Elektrische flens FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120"]
[null,71333,"Electrical heating flange FCR 28/180",954,"",null,null,null,null,null,null,71333,"Electrical heating flange FCR 28/180",954,false,null,71333,1428,954,"1.610,00","på forespørgsel",1428,"Elektro-Heizflansch FCR 28/180 (9/18 KW)","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Elektrische flens FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180"]
[null,233511,"Filterbaugruppe FS-WP-22",61,"",null,null,null,null,null,null,233511,"Filterbaugruppe FS-WP-22",61,false,null,233511,43,61,"sur demande",406,43,"Filterbaugruppe FS-WP-22","Filterbaugruppe FS-WP-22","Filterbaugruppe FS-WP-22","Filterbaugruppe FS-WP-22","Filterbouwgroep FS-WP-22","Filterbaugruppe FS-WP-22","Filterbaugruppe FS-WP-22","Filterbaugruppe FS-WP-22","Filterbaugruppe FS-WP-22","Filterbaugruppe FS-WP-22","Filterbaugruppe FS-WP-22"]
[null,233512,"Filterbaugruppe FS-WP-28",82,"",null,null,null,null,null,null,233512,"Filterbaugruppe FS-WP-28",82,false,null,233512,66,82,"sur demande",687,66,"Filterbaugruppe FS-WP-28","Filterbaugruppe FS-WP-28","Filterbaugruppe FS-WP-28","Filterbaugruppe FS-WP-28","Filterbouwgroep FS-WP-28","Filterbaugruppe FS-WP-28","Filterbaugruppe FS-WP-28","Filterbaugruppe FS-WP-28","Filterbaugruppe FS-WP-28","Filterbaugruppe FS-WP-28","Filterbaugruppe FS-WP-28"]
[null,227420,"Heating diverter valve HUV 1",300,"",null,null,null,null,null,null,227420,"Heating diverter valve HUV 1",300,false,null,227420,310,300,425,1885,310,"Heizungsumschaltventil HUV 1","Heating diverter valve HUV 1","Heating diverter valve HUV 1","Heating diverter valve HUV 1","Omschakelventiel HUV 1","Heating diverter valve HUV 1","Heating diverter valve HUV 1","Heating diverter valve HUV 1","Heating diverter valve HUV 1","Heating diverter valve HUV 1","Heating diverter valve HUV 1"]
[null,223391,"Heating diverter valve HUV 2",708,"",null,null,null,null,null,null,223391,"Heating diverter valve HUV 2",708,false,null,223391,582,708,920,4880,582,"Heizungsumschaltventil HUV 2","Heating diverter valve HUV 2","Heating diverter valve HUV 2","Heating diverter valve HUV 2","Omschakelventiel HUV 2","Heating diverter valve HUV 2","Heating diverter valve HUV 2","Heating diverter valve HUV 2","Heating diverter valve HUV 2","Heating diverter valve HUV 2","Heating diverter valve HUV 2"]
[null,227425,"Heating diverter valve HUV 50",779,"",null,null,null,null,null,null,227425,"Heating diverter valve HUV 50",779,false,null,227425,946,779,970,5342,946,"Heizungsumschaltventil HUV 65","Heating diverter valve HUV 50","Heating diverter valve HUV 50","Heating diverter valve HUV 50","Omschakelventiel HUV 65","Heating diverter valve HUV 50","Heating diverter valve HUV 50","Heating diverter valve HUV 50","Heating diverter valve HUV 50","Heating diverter valve HUV 50","Heating diverter valve HUV 50"]
[null,227426,"Heating diverter valve HUV 80",1146,"",null,null,null,null,null,null,227426,"Heating diverter valve HUV 80",1146,false,null,227426,1456,1146,"1.495,00",7741,1456,"Heizungsumschaltventil HUV 80","Heating diverter valve HUV 80","Heating diverter valve HUV 80","Heating diverter valve HUV 80","Omschakelventiel HUV 80 ","Heating diverter valve HUV 80","Heating diverter valve HUV 80","Heating diverter valve HUV 80","Heating diverter valve HUV 80","Heating diverter valve HUV 80","Heating diverter valve HUV 80"]
[null,229645,"Three-way diverter valve HMV 1",67,"",null,null,null,null,null,null,229645,"Three-way diverter valve HMV 1",67,false,null,229645,111,67,105,432,111,"3-Wege Mischventil HMV 1","Three-way diverter valve HMV 1","Three-way diverter valve HMV 1","Three-way diverter valve HMV 1","3-Weg mengventiel HMV 1","Three-way diverter valve HMV 1","Three-way diverter valve HMV 1","Three-way diverter valve HMV 1","Three-way diverter valve HMV 1","Three-way diverter valve HMV 1","Three-way diverter valve HMV 1"]
[null,229644,"Three-way mixing valve HMV 3/4",62,"",null,null,null,null,null,null,229644,"Three-way mixing valve HMV 3/4",62,false,null,229644,107,62,95,399,107,"3-Wege Mischventil HMV 3/4","Three-way mixing valve HMV 3/4","Three-way mixing valve HMV 3/4","Three-way mixing valve HMV 3/4","3-Weg mengventiel HMV 3/4","Three-way mixing valve HMV 3/4","Three-way mixing valve HMV 3/4","Three-way mixing valve HMV 3/4","Three-way mixing valve HMV 3/4","Three-way mixing valve HMV 3/4","Three-way mixing valve HMV 3/4"]
[null,229646,"Servomotor HSM for mixing valve",231,"",null,null,null,null,null,null,229646,"Servomotor HSM for mixing valve",231,false,null,229646,407,231,345,1512,407,"Stellmotor HSM für Mischventil HMV","Servomotor HSM for mixing valve","Servomotor HSM for mixing valve","Servomotor HSM for mixing valve","Servomotor HSM","Servomotor HSM for mixing valve","Servomotor HSM for mixing valve","Servomotor HSM for mixing valve","Servomotor HSM for mixing valve","Servomotor HSM for mixing valve","Servomotor HSM for mixing valve"]
[null,233711,"Schutztemperaturregler Fußbodenheizung STB-FB",33,"",null,null,null,null,null,null,233711,"Schutztemperaturregler Fußbodenheizung STB-FB",33,false,null,233711,32.5,33,"sur demande",233,33,"Schutztemperaturregler Fußbodenheizung STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB","Beveiligingstemperatuurregelaar Vloerverwarming STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB","Schutztemperaturregler Fußbodenheizung STB-FB"]
[null,3554,"Safety temperature controller RE1 B-A","On request","",null,null,null,null,null,null,3554,"Safety temperature controller RE1 B-A","On request",false,null,3554,215,"On request","sur demande","på forespørgsel",215,"Schutztemperaturregler RE1 B-A","Safety temperature controller RE1 B-A","Safety temperature controller RE1 B-A","Safety temperature controller RE1 B-A","RE1 B-A temperatuurregelaar","Safety temperature controller RE1 B-A","Safety temperature controller RE1 B-A","Safety temperature controller RE1 B-A","Safety temperature controller RE1 B-A","Safety temperature controller RE1 B-A","Safety temperature controller RE1 B-A"]
[null,230013,"Heating descaler HZEA",222,"",null,null,null,null,null,null,230013,"Heating descaler HZEA",222,false,null,230013,240,222,240,1863,240,"Heizungs-Enthärtungsarmatur HZEA","Heating descaler HZEA","Heating descaler HZEA","Heating descaler HZEA","Onthardingsarmatuur HZEA","Heating descaler HZEA","Heating descaler HZEA","Heating descaler HZEA","Heating descaler HZEA","Heating descaler HZEA","Heating descaler HZEA"]
[null,230031,"Spare cartridge for HZEA",73,"",null,null,null,null,null,null,230031,"Spare cartridge for HZEA",73,false,null,230031,79,73,"sur demande",394,79,"Nachfüllpatrone für Enthärtungsarmatur HZEA","Spare cartridge for HZEA","Spare cartridge for HZEA","Spare cartridge for HZEA","Vervangpatroon HZEN","Spare cartridge for HZEA","Spare cartridge for HZEA","Spare cartridge for HZEA","Spare cartridge for HZEA","Spare cartridge for HZEA","Spare cartridge for HZEA"]
[null,232976,"Druckschlauch SD 25-1 G",45,"",null,null,null,null,null,null,232976,"Druckschlauch SD 25-1 G",45,false,null,232976,72,45,70,305,72,"Druckschlauch SD 25-1 G","Druckschlauch SD 25-1 G","Druckschlauch SD 25-1 G","Druckschlauch SD 25-1 G","Drukslang SD 25-1 G","Druckschlauch SD 25-1 G","Druckschlauch SD 25-1 G","Druckschlauch SD 25-1 G","Druckschlauch SD 25-1 G","Druckschlauch SD 25-1 G","Druckschlauch SD 25-1 G"]
[null,232977,"Druckschlauch SD 32-1 G",59,"",null,null,null,null,null,null,232977,"Druckschlauch SD 32-1 G",59,false,null,232977,90,59,85,397,90,"Druckschlauch SD 32-1 G","Druckschlauch SD 32-1 G","Druckschlauch SD 32-1 G","Druckschlauch SD 32-1 G","Drukslang SD 32-1 G","Druckschlauch SD 32-1 G","Druckschlauch SD 32-1 G","Druckschlauch SD 32-1 G","Druckschlauch SD 32-1 G","Druckschlauch SD 32-1 G","Druckschlauch SD 32-1 G"]
[null,233828,"Druckschlauch SD 25-2 GE",96,"",null,null,null,null,null,null,233828,"Druckschlauch SD 25-2 GE",96,false,null,233828,100,96,145,685,100,"Druckschlauch SD 25-2 GE","Druckschlauch SD 25-2 GE","Druckschlauch SD 25-2 GE","Druckschlauch SD 25-2 GE","Drukslang SD 25-2 GE","Druckschlauch SD 25-2 GE","Druckschlauch SD 25-2 GE","Druckschlauch SD 25-2 GE","Druckschlauch SD 25-2 GE","Druckschlauch SD 25-2 GE","Druckschlauch SD 25-2 GE"]
[null,232971,"Druckschlauch SD 25-2,5 GE",165,"",null,null,null,null,null,null,232971,"Druckschlauch SD 25-2,5 GE",165,false,null,232971,152,165,235,1118,152,"Druckschlauch SD 25-2.5 GE","Druckschlauch SD 25-2,5 GE","Druckschlauch SD 25-2,5 GE","Druckschlauch SD 25-2,5 GE","Drukslang SD 25-2.5 GE","Druckschlauch SD 25-2,5 GE","Druckschlauch SD 25-2,5 GE","Druckschlauch SD 25-2,5 GE","Druckschlauch SD 25-2,5 GE","Druckschlauch SD 25-2,5 GE","Druckschlauch SD 25-2,5 GE"]
[null,233829,"Druckschlauch SD 25-5 GE",210,"",null,null,null,null,null,null,233829,"Druckschlauch SD 25-5 GE",210,false,null,233829,214,210,310,1500,214,"Druckschlauch SD 25-5 GE","Druckschlauch SD 25-5 GE","Druckschlauch SD 25-5 GE","Druckschlauch SD 25-5 GE","Drukslang SD 25-5 GE","Druckschlauch SD 25-5 GE","Druckschlauch SD 25-5 GE","Druckschlauch SD 25-5 GE","Druckschlauch SD 25-5 GE","Druckschlauch SD 25-5 GE","Druckschlauch SD 25-5 GE"]
[null,233830,"Druckschlauch SD 25-10 GE",459,"",null,null,null,null,null,null,233830,"Druckschlauch SD 25-10 GE",459,false,null,233830,449,459,670,3257,449,"Druckschlauch SD 25-10 GE","Druckschlauch SD 25-10 GE","Druckschlauch SD 25-10 GE","Druckschlauch SD 25-10 GE","Drukslang SD 25-10 GE","Druckschlauch SD 25-10 GE","Druckschlauch SD 25-10 GE","Druckschlauch SD 25-10 GE","Druckschlauch SD 25-10 GE","Druckschlauch SD 25-10 GE","Druckschlauch SD 25-10 GE"]
[null,233831,"Druckschlauch SD 32-2 GE",141,"",null,null,null,null,null,null,233831,"Druckschlauch SD 32-2 GE",141,false,null,233831,141,141,210,1000,141,"Druckschlauch SD 32-2 GE","Druckschlauch SD 32-2 GE","Druckschlauch SD 32-2 GE","Druckschlauch SD 32-2 GE","Drukslang SD 32-2 GE","Druckschlauch SD 32-2 GE","Druckschlauch SD 32-2 GE","Druckschlauch SD 32-2 GE","Druckschlauch SD 32-2 GE","Druckschlauch SD 32-2 GE","Druckschlauch SD 32-2 GE"]
[null,233832,"Druckschlauch SD 32-5 GE",306,"",null,null,null,null,null,null,233832,"Druckschlauch SD 32-5 GE",306,false,null,233832,304,306,450,2167,304,"Druckschlauch SD 32-5 GE","Druckschlauch SD 32-5 GE","Druckschlauch SD 32-5 GE","Druckschlauch SD 32-5 GE","Drukslang SD 32-5 GE","Druckschlauch SD 32-5 GE","Druckschlauch SD 32-5 GE","Druckschlauch SD 32-5 GE","Druckschlauch SD 32-5 GE","Druckschlauch SD 32-5 GE","Druckschlauch SD 32-5 GE"]
[null,233833,"Druckschlauch SD 32-10 GE",528,"",null,null,null,null,null,null,233833,"Druckschlauch SD 32-10 GE",528,false,null,233833,500,528,760,3661,500,"Druckschlauch SD 32-10 GE","Druckschlauch SD 32-10 GE","Druckschlauch SD 32-10 GE","Druckschlauch SD 32-10 GE","Drukslang SD 32-10 GE","Druckschlauch SD 32-10 GE","Druckschlauch SD 32-10 GE","Druckschlauch SD 32-10 GE","Druckschlauch SD 32-10 GE","Druckschlauch SD 32-10 GE","Druckschlauch SD 32-10 GE"]
[null,74415,"Pressure hose SD 25-1",56,"",null,null,null,null,null,null,74415,"Pressure hose SD 25-1",56,false,null,74415,82,56,75,"på forespørgsel",82,"Druckschlauch SD 25-1","Pressure hose SD 25-1","Pressure hose SD 25-1","Pressure hose SD 25-1","Drukslang SD 25-1","Pressure hose SD 25-1","Pressure hose SD 25-1","Pressure hose SD 25-1","Pressure hose SD 25-1","Pressure hose SD 25-1","Pressure hose SD 25-1"]
[null,74414,"Pressure hose SD 32-1",65,"",null,null,null,null,null,null,74414,"Pressure hose SD 32-1",65,false,null,74414,98,65,95,"på forespørgsel",98,"Druckschlauch SD 32-1","Pressure hose SD 32-1","Pressure hose SD 32-1","Pressure hose SD 32-1","Drukslang SD 32-1","Pressure hose SD 32-1","Pressure hose SD 32-1","Pressure hose SD 32-1","Pressure hose SD 32-1","Pressure hose SD 32-1","Pressure hose SD 32-1"]
[null,232965,"Druckschlauch SD 25-1 E",85,"",null,null,null,null,null,null,232965,"Druckschlauch SD 25-1 E",85,false,null,232965,93,85,125,581,93,"Druckschlauch SD 25-1 E","Druckschlauch SD 25-1 E","Druckschlauch SD 25-1 E","Druckschlauch SD 25-1 E","Drukslang SD 25-1 E","Druckschlauch SD 25-1 E","Druckschlauch SD 25-1 E","Druckschlauch SD 25-1 E","Druckschlauch SD 25-1 E","Druckschlauch SD 25-1 E","Druckschlauch SD 25-1 E"]
[null,232968,"Druckschlauch SD 32-1 E",102,"",null,null,null,null,null,null,232968,"Druckschlauch SD 32-1 E",102,false,null,232968,103,102,150,697,103,"Druckschlauch SD 32-1 E","Druckschlauch SD 32-1 E","Druckschlauch SD 32-1 E","Druckschlauch SD 32-1 E","Drukslang SD 32-1 E","Druckschlauch SD 32-1 E","Druckschlauch SD 32-1 E","Druckschlauch SD 32-1 E","Druckschlauch SD 32-1 E","Druckschlauch SD 32-1 E","Druckschlauch SD 32-1 E"]
[null,232972,"Druckschlauch SD 50-1 E",203,"",null,null,null,null,null,null,232972,"Druckschlauch SD 50-1 E",203,false,null,232972,241,203,285,1378,241,"Druckschlauch SD 50-1 E","Druckschlauch SD 50-1 E","Druckschlauch SD 50-1 E","Druckschlauch SD 50-1 E","Drukslang SD 50-1 E","Druckschlauch SD 50-1 E","Druckschlauch SD 50-1 E","Druckschlauch SD 50-1 E","Druckschlauch SD 50-1 E","Druckschlauch SD 50-1 E","Druckschlauch SD 50-1 E"]
[null,232974,"Druckschlauch kürzbar SD 25-1 KE",118,"",null,null,null,null,null,null,232974,"Druckschlauch kürzbar SD 25-1 KE",118,false,null,232974,122,118,170,805,122,"Druckschlauch kürzbar SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE","Drukslang SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE","Druckschlauch kürzbar SD 25-1 KE"]
[null,232975,"Druckschlauch kürzbar SD 32-1 KE",131,"",null,null,null,null,null,null,232975,"Druckschlauch kürzbar SD 32-1 KE",131,false,null,232975,126,131,185,887,126,"Druckschlauch kürzbar SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE","Drukslang SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE","Druckschlauch kürzbar SD 32-1 KE"]
[null,3713,"Hose fitting DN 25",110,"",null,null,null,null,null,null,3713,"Hose fitting DN 25",110,false,null,3713,74,110,165,"på forespørgsel",74,"Schlauchverschraubung DN 25","Hose fitting DN 25","Hose fitting DN 25","Hose fitting DN 25","Slangschroefkoppeling DN 25","Hose fitting DN 25","Hose fitting DN 25","Hose fitting DN 25","Hose fitting DN 25","Hose fitting DN 25","Hose fitting DN 25"]
[null,70692,"Hose fitting DN 32",105,"",null,null,null,null,null,null,70692,"Hose fitting DN 32",105,false,null,70692,82,105,150,"på forespørgsel",82,"Schlauchverschraubung DN 32","Hose fitting DN 32","Hose fitting DN 32","Hose fitting DN 32","Slangschroefkoppeling DN 32","Hose fitting DN 32","Hose fitting DN 32","Hose fitting DN 32","Hose fitting DN 32","Hose fitting DN 32","Hose fitting DN 32"]
[null,227955,"Fan coil AUK 7",1169,"",null,null,null,null,null,null,227955,"Fan coil AUK 7",1169,false,null,227955,683,1169,"1.660,00",5729,683,"Gebläse-Konvektor Heizung AUK 7","Fan coil AUK 7","Fan coil AUK 7","Fan coil AUK 7","Warmtepompconvector AUK 7","Fan coil AUK 7","Fan coil AUK 7","Fan coil AUK 7","Fan coil AUK 7","Fan coil AUK 7","Fan coil AUK 7"]
[null,227956,"Fan coil AUK 14",1151,"",null,null,null,null,null,null,227956,"Fan coil AUK 14",1151,false,null,227956,764,1151,"1.715,00",6005,764,"Gebläse-Konvektor Heizung AUK 14","Fan coil AUK 14","Fan coil AUK 14","Fan coil AUK 14","Warmtepompconvector AUK 14","Fan coil AUK 14","Fan coil AUK 14","Fan coil AUK 14","Fan coil AUK 14","Fan coil AUK 14","Fan coil AUK 14"]
[null,227957,"Fan coil AUK 21",1226,"",null,null,null,null,null,null,227957,"Fan coil AUK 21",1226,false,null,227957,854,1226,"1.785,00",6452,854,"Gebläse-Konvektor Heizung AUK 21","Fan coil AUK 21","Fan coil AUK 21","Fan coil AUK 21","Warmtepompconvector AUK 21","Fan coil AUK 21","Fan coil AUK 21","Fan coil AUK 21","Fan coil AUK 21","Fan coil AUK 21","Fan coil AUK 21"]
[null,227958,"Fan coil AUK 28",1386,"",null,null,null,null,null,null,227958,"Fan coil AUK 28",1386,false,null,227958,934,1386,"1.910,00",6936,934,"Gebläse-Konvektor Heizung AUK 28","Fan coil AUK 28","Fan coil AUK 28","Fan coil AUK 28","Warmtepompconvector AUK 28","Fan coil AUK 28","Fan coil AUK 28","Fan coil AUK 28","Fan coil AUK 28","Fan coil AUK 28","Fan coil AUK 28"]
[null,227959,"Fan coil AUK 35",1430,{"$f":"IF(O426=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,227959,"Fan coil AUK 35",1430,false,null,227959,1013,1430,"1.980,00",7279,1013,"Gebläse-Konvektor Heizung AUK 35","Fan coil AUK 35","Fan coil AUK 35","Fan coil AUK 35","Warmtepompconvector AUK 35","Fan coil AUK 35","Fan coil AUK 35","Fan coil AUK 35","Fan coil AUK 35","Fan coil AUK 35","Fan coil AUK 35"]
[null,223441,"Cassette indoor unit ACKH 10",1461,"",null,null,null,null,null,null,223441,"Cassette indoor unit ACKH 10",1461,false,null,223441,2045,1461,"2.055,00",10005,2045,"Decken-Kassette Kühlung ACKH 10","Cassette indoor unit ACKH 10","Cassette indoor unit ACKH 10","Cassette indoor unit ACKH 10","Cassette-binnenunit ACKH 10","Cassette indoor unit ACKH 10","Cassette indoor unit ACKH 10","Cassette indoor unit ACKH 10","Cassette indoor unit ACKH 10","Cassette indoor unit ACKH 10","Cassette indoor unit ACKH 10"]
[null,223442,"Cassette indoor unit ACKH 12",1544,"",null,null,null,null,null,null,223442,"Cassette indoor unit ACKH 12",1544,false,null,223442,2376,1544,"2.180,00",10579,2376,"Decken-Kassette Kühlung ACKH 12","Cassette indoor unit ACKH 12","Cassette indoor unit ACKH 12","Cassette indoor unit ACKH 12","Cassette-binnenunit ACKH 12","Cassette indoor unit ACKH 12","Cassette indoor unit ACKH 12","Cassette indoor unit ACKH 12","Cassette indoor unit ACKH 12","Cassette indoor unit ACKH 12","Cassette indoor unit ACKH 12"]
[null,223443,"Cassette indoor unit ACKH 18",1594,"",null,null,null,null,null,null,223443,"Cassette indoor unit ACKH 18",1594,false,null,223443,2574,1594,"2.220,00",10922,2574,"Decken-Kassette Kühlung ACKH 18","Cassette indoor unit ACKH 18","Cassette indoor unit ACKH 18","Cassette indoor unit ACKH 18","Cassette-binnenunit ACKH 18","Cassette indoor unit ACKH 18","Cassette indoor unit ACKH 18","Cassette indoor unit ACKH 18","Cassette indoor unit ACKH 18","Cassette indoor unit ACKH 18","Cassette indoor unit ACKH 18"]
[null,189820,"Fan coil heating/cooling ACTH 20",890,"",null,null,null,null,null,null,189820,"Fan coil heating/cooling ACTH 20",890,{"$f":"IF(AND(B430=L430,C430=M430,D430=N430),FALSE,TRUE)","v":false},null,189820,923,890,"1.225,00","på forespørgsel",923,"Gebläsekonvektor Kühlung ACTH 20","Fan coil heating/cooling ACTH 20","Fan coil heating/cooling ACTH 20","Fan coil heating/cooling ACTH 20","Ventilatorconvector Verwarmen/Koelen ACTH 20","Fan coil heating/cooling ACTH 20","Fan coil heating/cooling ACTH 20","Fan coil heating/cooling ACTH 20","Fan coil heating/cooling ACTH 20","Fan coil heating/cooling ACTH 20","Fan coil heating/cooling ACTH 20"]
[null,189821,"Fan coil heating/cooling ACTH 40",966,"",null,null,null,null,null,null,189821,"Fan coil heating/cooling ACTH 40",966,false,null,189821,1040,966,"1.350,00","på forespørgsel",1040,"Gebläsekonvektor Kühlung ACTH 40","Fan coil heating/cooling ACTH 40","Fan coil heating/cooling ACTH 40","Fan coil heating/cooling ACTH 40","Ventilatorconvector Verwarmen/Koelen ACTH 40","Fan coil heating/cooling ACTH 40","Fan coil heating/cooling ACTH 40","Fan coil heating/cooling ACTH 40","Fan coil heating/cooling ACTH 40","Fan coil heating/cooling ACTH 40","Fan coil heating/cooling ACTH 40"]
[null,189822,"Fan coil heating/cooling ACTH 50",1008,"",null,null,null,null,null,null,189822,"Fan coil heating/cooling ACTH 50",1008,false,null,189822,1125,1008,"1.450,00","på forespørgsel",1125,"Gebläsekonvektor Kühlung ACTH 50","Fan coil heating/cooling ACTH 50","Fan coil heating/cooling ACTH 50","Fan coil heating/cooling ACTH 50","Ventilatorconvector Verwarmen/Koelen ACTH 50","Fan coil heating/cooling ACTH 50","Fan coil heating/cooling ACTH 50","Fan coil heating/cooling ACTH 50","Fan coil heating/cooling ACTH 50","Fan coil heating/cooling ACTH 50","Fan coil heating/cooling ACTH 50"]
[null,189861,"Console ACTH","On request","",null,null,null,null,null,null,189861,"Console ACTH","On request",false,null,189861,46.5,"On request",60,"på forespørgsel",47,"Konsole Bodenaufstellung ACTH","Console ACTH","Console ACTH","Console ACTH","Console ACTH","Console ACTH","Console ACTH","Console ACTH","Console ACTH","Console ACTH","Console ACTH"]
[null,74361,"DHW heat pump WWK 300",2849,"",null,null,null,null,null,null,74361,"DHW heat pump WWK 300",2849,false,null,74361,2724,2849,"2.690,00","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 300","DHW heat pump WWK 300","DHW heat pump WWK 300","DHW heat pump WWK 300","Warmwater-Warmtepompboiler WWK 300","DHW heat pump WWK 300","DHW heat pump WWK 300","DHW heat pump WWK 300","DHW heat pump WWK 300","DHW heat pump WWK 300","DHW heat pump WWK 300"]
[null,74362,"DHW heat pump WWK 300 SOL",3223,"",null,null,null,null,null,null,74362,"DHW heat pump WWK 300 SOL",3223,false,null,74362,3271,3223,"3.290,00","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 300 SOL","DHW heat pump WWK 300 SOL","DHW heat pump WWK 300 SOL","DHW heat pump WWK 300 SOL","Warmwater-Warmtepompboiler WWK 300 SOL","DHW heat pump WWK 300 SOL","DHW heat pump WWK 300 SOL","DHW heat pump WWK 300 SOL","DHW heat pump WWK 300 SOL","DHW heat pump WWK 300 SOL","DHW heat pump WWK 300 SOL"]
[null,231103,"DHW heat pump WWK 300 PV",3151,"",null,null,null,null,null,null,231103,"DHW heat pump WWK 300 PV",3151,false,null,231103,2893,3151,"sur demande",21709,"op aanvraag","Warmwasser-Wärmepumpe WWK 300 PV","DHW heat pump WWK 300 PV","DHW heat pump WWK 300 PV","DHW heat pump WWK 300 PV","Warmwater-Warmtepompboiler WWK 300 PV","DHW heat pump WWK 300 PV","DHW heat pump WWK 300 PV","DHW heat pump WWK 300 PV","DHW heat pump WWK 300 PV","DHW heat pump WWK 300 PV","DHW heat pump WWK 300 PV"]
[null,231208,"Warmwasser-Wärmepumpe WWK 220 electronic",3146,"",null,null,null,null,null,null,231208,"Warmwasser-Wärmepumpe WWK 220 electronic",3146,false,null,231208,2350,3146,"2.690,00",21551,"op aanvraag","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwater-Warmtepompboiler WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic","Warmwasser-Wärmepumpe WWK 220 electronic"]
[null,231210,"Warmwasser-Wärmepumpe WWK 300 electronic",3324,"",null,null,null,null,null,null,231210,"Warmwasser-Wärmepumpe WWK 300 electronic",3324,false,null,231210,2450,3324,"2.790,00",22768,"op aanvraag","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwater-Warmtepompboiler WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic","Warmwasser-Wärmepumpe WWK 300 electronic"]
[null,221470,"Ventilation device LWA 100",2786,"",null,null,null,null,null,null,221470,"Ventilation device LWA 100",2786,false,null,221470,2499,2786,"3.335,00","på forespørgsel",2499,"Warmwasser-Wärmepumpe LWA 100","Ventilation device LWA 100","LWA 100","Ventilation device LWA 100","Centraal ventilatietoestel  LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100"]
[null,233898,"Warmwasser-Wärmepumpe WWS 20","On request","",null,null,null,null,null,null,233898,"Warmwasser-Wärmepumpe WWS 20","On request",false,null,233898,2336,"On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWS 20","Warmwasser-Wärmepumpe WWS 20","Warmwasser-Wärmepumpe WWS 20","Warmwasser-Wärmepumpe WWS 20","Warmwater-Warmtepompboiler WWS 20","Warmwasser-Wärmepumpe WWS 20","Warmwasser-Wärmepumpe WWS 20","Warmwasser-Wärmepumpe WWS 20","Warmwasser-Wärmepumpe WWS 20","Warmwasser-Wärmepumpe WWS 20","Warmwasser-Wärmepumpe WWS 20"]
[null,71448,"Air duct connection WWK",180,"",null,null,null,null,null,null,71448,"Air duct connection WWK",180,false,null,71448,94,180,225,"på forespørgsel","op aanvraag","Luftkanal-Anschluss WWK","Air duct connection WWK","Air duct connection WWK","Air duct connection WWK","Luchtkanaal-Aansluiting WWK","Air duct connection WWK","Air duct connection WWK","Air duct connection WWK","Air duct connection WWK","Air duct connection WWK","Air duct connection WWK"]
[null,72997,"Inlet pipe 200/400 l","On request","",null,null,null,null,null,null,72997,"Inlet pipe 200/400 l","On request",false,null,72997,166,"On request","sur demande","på forespørgsel","op aanvraag","Einströmrohr Trinkwasserspeicher 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Instroombuis 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l","Inlet pipe 200/400 l"]
[null,233514,"Lüftungs-Integralgerät LWZ 504 SOL","On request","",null,null,null,null,null,null,233514,"Lüftungs-Integralgerät LWZ 504 SOL","On request",false,null,233514,15900,"On request","16.100,00","på forespørgsel","op aanvraag","Lüftungs-Integralgerät LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL","Centraal ventilatietoestel  LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL","Lüftungs-Integralgerät LWZ 504 SOL"]
[null,230143,"Ventilation device LWZ 304 SOL","On request","",null,null,null,null,null,null,230143,"Ventilation device LWZ 304 SOL","On request",false,null,230143,14500,"On request","14.400,00",100076,14500,"Lüftungs-Integralgerät LWZ 304 SOL","Ventilation device LWZ 304 SOL","Appareil intégral LWZ 304 SOL","Ventilation device LWZ 304 SOL","Centraal ventilatietoestel  LWZ 304 SOL","Ventilation device LWZ 304 SOL","Ventilation device LWZ 304 SOL","Ventilation device LWZ 304 SOL","Ventilation device LWZ 304 SOL","Ventilation device LWZ 304 SOL","Ventilation device LWZ 304 SOL"]
[null,230144,"Ventilation device LWZ 404 SOL","On request","",null,null,null,null,null,null,230144,"Ventilation device LWZ 404 SOL","On request",false,null,230144,15099,"On request","15.150,00",106930,15099,"Lüftungs-Integralgerät LWZ 404 SOL","Ventilation device LWZ 404 SOL","Appareil intégral LWZ 404 SOL","Ventilation device LWZ 404 SOL","Centraal ventilatietoestel  LWZ 404 SOL","Ventilation device LWZ 404 SOL","Ventilation device LWZ 404 SOL","Ventilation device LWZ 404 SOL","Ventilation device LWZ 404 SOL","Ventilation device LWZ 404 SOL","Ventilation device LWZ 404 SOL"]
[null,230145,"LWZ 304 SOL SET","On request","",null,null,null,null,null,null,230145,"LWZ 304 SOL SET","On request",false,null,230145,16300,"On request","16.900,00","på forespørgsel",16300,"Integralgerät mit Solar LWZ 304 SOL SET","LWZ 304 SOL SET","SET LWZ 304 SOL","LWZ 304 SOL SET","Centraal ventilatietoestel  LWZ 304 SOL Set","LWZ 304 SOL SET","LWZ 304 SOL SET","LWZ 304 SOL SET","LWZ 304 SOL SET","LWZ 304 SOL SET","LWZ 304 SOL SET"]
[null,230146,"LWZ 404 SOL SET","On request","",null,null,null,null,null,null,230146,"LWZ 404 SOL SET","On request",false,null,230146,16940,"On request","17.650,00","på forespørgsel",16940,"Integralgerät mit Solar LWZ 404 SOL SET","LWZ 404 SOL SET","SET LWZ 404 SOL","LWZ 404 SOL SET","Centraal ventilatietoestel  LWZ 404 SOL Set","LWZ 404 SOL SET","LWZ 404 SOL SET","LWZ 404 SOL SET","LWZ 404 SOL SET","LWZ 404 SOL SET","LWZ 404 SOL SET"]
[null,233897,"Lüftungsgerät LWZ 304 Integral","On request","",null,null,null,null,null,null,233897,"Lüftungsgerät LWZ 304 Integral","On request",false,null,233897,11200,"On request","sur demande","på forespørgsel",11200,"Lüftungsgerät LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral","Centraal ventilatietoestel  LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral","Lüftungsgerät LWZ 304 Integral"]
[null,233254,"Lüftungsgerät LWZ 304 Trend","On request","",null,null,null,null,null,null,233254,"Lüftungsgerät LWZ 304 Trend","On request",false,null,233254,11900,"On request","12.750,00","på forespørgsel",11900,"Lüftungsgerät LWZ 304 Trend","Lüftungsgerät LWZ 304 Trend","Lüftungsgerät LWZ 304 Trend","Lüftungsgerät LWZ 304 Trend","Centraal ventilatietoestel  LWZ 304 trend","Lüftungsgerät LWZ 304 Trend","Lüftungsgerät LWZ 304 Trend","Lüftungsgerät LWZ 304 Trend","Lüftungsgerät LWZ 304 Trend","Lüftungsgerät LWZ 304 Trend","Lüftungsgerät LWZ 304 Trend"]
[null,233255,"Lüftungsgerät LWZ 404 Trend","On request","",null,null,null,null,null,null,233255,"Lüftungsgerät LWZ 404 Trend","On request",false,null,233255,13500,"On request","13.500,00","på forespørgsel",13500,"Lüftungsgerät LWZ 404 Trend","Lüftungsgerät LWZ 404 Trend","Lüftungsgerät LWZ 404 Trend","Lüftungsgerät LWZ 404 Trend","Centraal ventilatietoestel  LWZ 404 trend","Lüftungsgerät LWZ 404 Trend","Lüftungsgerät LWZ 404 Trend","Lüftungsgerät LWZ 404 Trend","Lüftungsgerät LWZ 404 Trend","Lüftungsgerät LWZ 404 Trend","Lüftungsgerät LWZ 404 Trend"]
[null,227664,"Remote control FES Komfort","On request","",null,null,null,null,null,null,227664,"Remote control FES Komfort","On request",false,null,227664,291,"On request",205,1103,291,"Fernbedieneinheit FES Komfort","Remote control FES Komfort","Unité de commande à distance FES Komfort","Remote control FES Komfort","Bedieneenheid FES comfort","Remote control FES Komfort","Remote control FES Komfort","Remote control FES Komfort","Remote control FES Komfort","Remote control FES Komfort","Remote control FES Komfort"]
[null,229336,"Internet-Service Gateway ISG web","On request","",null,null,null,null,null,null,229336,"Internet-Service Gateway ISG web","On request",false,null,229336,483,"On request","Voir tarifs mises en service p.11",4776,483,"Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Service Internet passerelle ISG web","Internet-Service Gateway ISG web","Internet-Service-Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web","Internet-Service Gateway ISG web"]
[null,233493,"Internet-Service Gateway ISG plus","On request","",null,null,null,null,null,null,233493,"Internet-Service Gateway ISG plus","On request",false,null,233493,632,"On request","sur demande","på forespørgsel","op aanvraag","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus","Internet-Service Gateway ISG plus"]
[null,233836,"Außenwand-Durchführung AWG 315 silber",321,"",null,null,null,null,null,null,233836,"Außenwand-Durchführung AWG 315 silber",321,false,null,233836,399,321,455,2197,399,"Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Wanddoorvoer AWG 315 S","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber","Außenwand-Durchführung AWG 315 silber"]
[null,232955,"Außenwand-Durchführung AWG 315 grau",319,"",null,null,null,null,null,null,232955,"Außenwand-Durchführung AWG 315 grau",319,false,null,232955,399,319,450,2190,399,"Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Wanddoorvoer AWG 315 G","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau","Außenwand-Durchführung AWG 315 grau"]
[null,231039,"Air routing AWG 315 lightwell",261,"",null,null,null,null,null,null,231039,"Air routing AWG 315 lightwell",261,false,null,231039,224,261,400,1743,224,"Außenwand-Durchführung AWG 315 Lichtschacht","Air routing AWG 315 lightwell","Traversée murale AWG 315 soupirail","Air routing AWG 315 lightwell","Wanddoorvoer AWG 315 L","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell","Air routing AWG 315 lightwell"]
[null,232341,"Luftleitblech für AWG 315 Lichtschacht",30,"",null,null,null,null,null,null,232341,"Luftleitblech für AWG 315 Lichtschacht",30,false,null,232341,22.8,30,45,155,23,"Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luchtgeleidingsplaat voor AWG 315 lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht","Luftleitblech für AWG 315 Lichtschacht"]
[null,231835,"Air hose DN 315, 4m",127,"",null,null,null,null,null,null,231835,"Air hose DN 315, 4m",127,false,null,231835,228,127,215,1188,228,"Wärmegedämmter Luftschlauch DN 315, 4m","Air hose DN 315, 4m","Gaine d'air à isolation thermique DN 315, 4 m","Air hose DN 315, 4m","Luchtslang DN 315 LSWP 315-4 AL","Air hose DN 315, 4m","Air hose DN 315, 4m","Air hose DN 315, 4m","Air hose DN 315, 4m","Air hose DN 315, 4m","Air hose DN 315, 4m"]
[null,170018,"Silencer DN 315",138,"",null,null,null,null,null,null,170018,"Silencer DN 315",138,false,null,170018,248,138,175,909,248,"Schalldämpfer DN 315","Silencer DN 315","Amortisseur de bruit DN 315","Silencer DN 315","Geluidsdemper DN 315","Silencer DN 315","Silencer DN 315","Silencer DN 315","Silencer DN 315","Silencer DN 315","Silencer DN 315"]
[null,232675,"Luftumlenkhaube für Außen- und Fortluft","On request","",null,null,null,null,null,null,232675,"Luftumlenkhaube für Außen- und Fortluft","On request",false,null,232675,219,"On request","sur demande","på forespørgsel","op aanvraag","Luftumlenkhaube für Außen- und Fortluft","Luftumlenkhaube für Außen- und Fortluft","Luftumlenkhaube für Außen- und Fortluft","Luftumlenkhaube für Außen- und Fortluft","Luchtafbuigkap voor buiten- en afvoerlucht","Luftumlenkhaube für Außen- und Fortluft","Luftumlenkhaube für Außen- und Fortluft","Luftumlenkhaube für Außen- und Fortluft","Luftumlenkhaube für Außen- und Fortluft","Luftumlenkhaube für Außen- und Fortluft","Luftumlenkhaube für Außen- und Fortluft"]
[null,227665,"Summer cassette LSK 303/403","On request","",null,null,null,null,null,null,227665,"Summer cassette LSK 303/403","On request",false,null,227665,89,"On request",75,458,89,"Sommerkassette LSK 303/403","Summer cassette LSK 303/403","Cartouche été LSK 303/403","Summer cassette LSK 303/403","Zomercassette LSK 303/403","Summer cassette LSK 303/403","Summer cassette LSK 303/403","Summer cassette LSK 303/403","Summer cassette LSK 303/403","Summer cassette LSK 303/403","Summer cassette LSK 303/403"]
[null,233867,"Austausch-Enthalpie-Wärmeübertrager","On request","",null,null,null,null,null,null,233867,"Austausch-Enthalpie-Wärmeübertrager","On request",false,null,233867,1581,"On request","1.565,00","på forespørgsel","op aanvraag","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Vervangings-Enthalpie-Warmtewisselaar","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager"]
[null,233301,"Anschlussset für Zirkulationspumpe","On request","",null,null,null,null,null,null,233301,"Anschlussset für Zirkulationspumpe","On request",false,null,233301,50,"On request","sur demande","på forespørgsel","op aanvraag","Anschlussset für Zirkulationspumpe","Anschlussset für Zirkulationspumpe","Anschlussset für Zirkulationspumpe","Anschlussset für Zirkulationspumpe","Aansluitset voor circulatiepomp","Anschlussset für Zirkulationspumpe","Anschlussset für Zirkulationspumpe","Anschlussset für Zirkulationspumpe","Anschlussset für Zirkulationspumpe","Anschlussset für Zirkulationspumpe","Anschlussset für Zirkulationspumpe"]
[null,221359,"Filter mat set LWA 403, G3","On request","",null,null,null,null,null,null,221359,"Filter mat set LWA 403, G3","On request",false,null,221359,29,"On request","sur demande","på forespørgsel",29,"Filtermattenset LWA 403, G3,  10 Stück","Filter mat set LWA 403, G3","Set tapis filtrants LWA 403, G3, 10 p.","Filter mat set LWA 403, G3","Filtermatset LWA 403","Filter mat set LWA 403, G3","Filter mat set LWA 403, G3","Filter mat set LWA 403, G3","Filter mat set LWA 403, G3","Filter mat set LWA 403, G3","Filter mat set LWA 403, G3"]
[null,231330,"Filter mat set LWZ 303/403, G4","On request","",null,null,null,null,null,null,231330,"Filter mat set LWZ 303/403, G4","On request",false,null,231330,28.5,"On request","sur demande",132,29,"Filtermattenset LWZ 304/404, G4 , 10 Stück","Filter mat set LWZ 303/403, G4","Set tapis filtrants LWZ 303/403, G4, 10 p.","Filter mat set LWZ 303/403, G4","Filtermatset G4 FMS G4-10 LWZ","Filter mat set LWZ 303/403, G4","Filter mat set LWZ 303/403, G4","Filter mat set LWZ 303/403, G4","Filter mat set LWZ 303/403, G4","Filter mat set LWZ 303/403, G4","Filter mat set LWZ 303/403, G4"]
[null,231331,"Filter mat set LWZ 303/403, F5","On request","",null,null,null,null,null,null,231331,"Filter mat set LWZ 303/403, F5","On request",false,null,231331,37,"On request","sur demande",197,37,"Filtermattenset LWZ 304/404, F5 , 2 Stück","Filter mat set LWZ 303/403, F5","Set tapis filtrants LWZ 303/403, F5, 2 p.","Filter mat set LWZ 303/403, F5","Filtermatset F5 FMS F5-2 LWZ","Filter mat set LWZ 303/403, F5","Filter mat set LWZ 303/403, F5","Filter mat set LWZ 303/403, F5","Filter mat set LWZ 303/403, F5","Filter mat set LWZ 303/403, F5","Filter mat set LWZ 303/403, F5"]
[null,231332,"Filter mat set LWZ 303/403, F7","On request","",null,null,null,null,null,null,231332,"Filter mat set LWZ 303/403, F7","On request",false,null,231332,43,"On request","sur demande",460,43,"Filtermattenset LWZ 304/404, F7 , 2 Stück","Filter mat set LWZ 303/403, F7","Set tapis filtrants LWZ 303/403, F7, 2 p.","Filter mat set LWZ 303/403, F7","Filtermatset F7 FMS F7-2 LWZ","Filter mat set LWZ 303/403, F7","Filter mat set LWZ 303/403, F7","Filter mat set LWZ 303/403, F7","Filter mat set LWZ 303/403, F7","Filter mat set LWZ 303/403, F7","Filter mat set LWZ 303/403, F7"]
[null,220467,"Ventilation device LWA 403","On request","",null,null,null,null,null,null,220467,"Ventilation device LWA 403","On request",false,null,220467,10853,"On request","sur demande","på forespørgsel",10853,"Lüftungs-Integralgerät LWA 403","Ventilation device LWA 403","Appareil intégral LWA 403","Ventilation device LWA 403","Centraal ventilatietoestel LWA 403","Ventilation device LWA 403","Ventilation device LWA 403","Ventilation device LWA 403","Ventilation device LWA 403","Ventilation device LWA 403","Ventilation device LWA 403"]
[null,74264,"LWA 252",3719,"",null,null,null,null,null,null,74264,"LWA 252",3719,false,null,74264,4357,3719,"4.030,00","på forespørgsel",3531,"Warmwasser-Wärmepumpe LWA 252","LWA 252","LWA 252","LWA 252","Centraal ventilatietoestel LWA 252","LWA 252","LWA 252","LWA 252","LWA 252","LWA 252","LWA 252"]
[null,74265,"LWA 252 SOL",4142,"",null,null,null,null,null,null,74265,"LWA 252 SOL",4142,false,null,74265,5313,4142,"4.545,00","på forespørgsel",3808,"Warmwasser-Wärmepumpe LWA 252 SOL","LWA 252 SOL","LWA 252 SOL","LWA 252 SOL","Centraal ventilatietoestel LWA 252 SOL","LWA 252 SOL","LWA 252 SOL","LWA 252 SOL","LWA 252 SOL","LWA 252 SOL","LWA 252 SOL"]
[null,221470,"Ventilation device LWA 100",2786,"",null,null,null,null,null,null,221470,"Ventilation device LWA 100",2786,false,null,221470,2499,2786,"3.335,00","på forespørgsel",2499,"Warmwasser-Wärmepumpe LWA 100","Ventilation device LWA 100","LWA 100","Ventilation device LWA 100","Centraal ventilatietoestel  LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100"]
[null,170328,"Remote control RC 1",27,"",null,null,null,null,null,null,170328,"Remote control RC 1",27,false,null,170328,74,27,35,"på forespørgsel",74,"Fernbedienung RC 1","Remote control RC 1","Commande à distance RC 1","Remote control RC 1","Afstandsbediening RC 1","Remote control RC 1","Remote control RC 1","Remote control RC 1","Remote control RC 1","Remote control RC 1","Remote control RC 1"]
[null,165339,"Outside temperature sensor AFS 2",7,"",null,null,null,null,null,null,165339,"Outside temperature sensor AFS 2",7,false,null,165339,20.6,7,10,"på forespørgsel",21,"Außenfühler AFS 2","Outside temperature sensor AFS 2","Sonde extérieure AFS 2","Outside temperature sensor AFS 2","Buitenvoeler AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2","Outside temperature sensor AFS 2"]
[null,221398,"Filter mat set LWA 100",3,"",null,null,null,null,null,null,221398,"Filter mat set LWA 100",3,false,null,221398,14.4,3,30,"på forespørgsel",14,"Filtermattenset LWA 100","Filter mat set LWA 100","Tapis filtrant LWA 100","Filter mat set LWA 100","LWA 100 Filtermatset ","Filter mat set LWA 100","Filter mat set LWA 100","Filter mat set LWA 100","Filter mat set LWA 100","Filter mat set LWA 100","Filter mat set LWA 100"]
[null,233851,"Zentrales Lüftungsgerät LWZ 70 E","On request","",null,null,null,null,null,null,233851,"Zentrales Lüftungsgerät LWZ 70 E","On request",false,null,233851,2238,"On request","1.900,00","på forespørgsel","op aanvraag","Zentrales Lüftungsgerät LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E","Centrale WTW Unit LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E","Zentrales Lüftungsgerät LWZ 70 E"]
[null,233850,"Zentrales Lüftungsgerät LWZ 170 E Plus","On request","",null,null,null,null,null,null,233850,"Zentrales Lüftungsgerät LWZ 170 E Plus","On request",false,null,233850,2659,"On request","2.300,00","på forespørgsel","op aanvraag","Zentrales Lüftungsgerät LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus","Centrale WTW Unit LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus","Zentrales Lüftungsgerät LWZ 170 E Plus"]
[null,232033,"Ventilation device LWZ 370 Plus",2573,"",null,null,null,null,null,null,232033,"Ventilation device LWZ 370 Plus",2573,false,null,232033,3150,2573,"2.650,00",17597,"op aanvraag","Zentrales Lüftungsgerät LWZ 370 E Plus","Ventilation device LWZ 370 Plus","Appareil de ventilation centralisée LWZ 370 Plus","Ventilation device LWZ 370 Plus","Centrale WTW Unit LWZ 370 E Plus","Ventilation device LWZ 370 Plus","Ventilation device LWZ 370 Plus","Ventilation device LWZ 370 Plus","Ventilation device LWZ 370 Plus","Ventilation device LWZ 370 Plus","Ventilation device LWZ 370 Plus"]
[null,221234,"Ventilation device LWZ 170",2009,"",null,null,null,null,null,null,221234,"Ventilation device LWZ 170",2009,false,null,221234,2241,2009,"sur demande","på forespørgsel","op aanvraag","Zentrales Lüftungsgerät LWZ 170","Ventilation device LWZ 170","Appareil de ventilation centralisée LWZ 170","Ventilation device LWZ 170","Centrale WTW Unit LWZ 170","Ventilation device LWZ 170","Ventilation device LWZ 170","Ventilation device LWZ 170","Ventilation device LWZ 170","Ventilation device LWZ 170","Ventilation device LWZ 170"]
[null,221236,"Ventilation device LWZ 270",2340,"",null,null,null,null,null,null,221236,"Ventilation device LWZ 270",2340,false,null,221236,2866,2340,"sur demande","på forespørgsel","op aanvraag","Zentrales Lüftungsgerät LWZ 270","Ventilation device LWZ 270","Appareil de ventilation centralisée LWZ 270","Ventilation device LWZ 270","Centrale WTW Unit LWZ 270","Ventilation device LWZ 270","Ventilation device LWZ 270","Ventilation device LWZ 270","Ventilation device LWZ 270","Ventilation device LWZ 270","Ventilation device LWZ 270"]
[null,221397,"Ventilation device LWZ 100 re",2732,{"$f":"IF(O480=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,221397,"Ventilation device LWZ 100 re",2732,false,null,221397,2226,2732,"2.900,00","på forespørgsel","op aanvraag","Zentrales Lüftungsgerät LWZ 100 RE","Ventilation device LWZ 100 re","Appareil de ventilation centralisée LWZ 100 DR","Ventilation device LWZ 100 re","Centrale WTW Unit LWZ 100 RE","Ventilation device LWZ 100 re","Ventilation device LWZ 100 re","Ventilation device LWZ 100 re","Ventilation device LWZ 100 re","Ventilation device LWZ 100 re","Ventilation device LWZ 100 re"]
[null,221472,"Ventilation device LWZ 100 li",2716,"",null,null,null,null,null,null,221472,"Ventilation device LWZ 100 li",2716,false,null,221472,2226,2716,"2.900,00","på forespørgsel","op aanvraag","Zentrales Lüftungsgerät LWZ 100 LI","Ventilation device LWZ 100 li","Appareil de ventilation centralisée LWZ 100 GA","Ventilation device LWZ 100 li","Centrale WTW Unit LWZ 100 LI","Ventilation device LWZ 100 li","Ventilation device LWZ 100 li","Ventilation device LWZ 100 li","Ventilation device LWZ 100 li","Ventilation device LWZ 100 li","Ventilation device LWZ 100 li"]
[null,229978,"Ventilation device LWZ 100 plus RE",3021,"",null,null,null,null,null,null,229978,"Ventilation device LWZ 100 plus RE",3021,false,null,229978,2537,3021,"3.000,00",19787,"op aanvraag","Zentrales Lüftungsgerät LWZ 100 plus RE","Ventilation device LWZ 100 plus RE","Appareil de ventilation centralisée LWZ 100 plus DR","Ventilation device LWZ 100 plus RE","Centrale WTW Unit LWZ 100 plus RE","Ventilation device LWZ 100 plus RE","Ventilation device LWZ 100 plus RE","Ventilation device LWZ 100 plus RE","Ventilation device LWZ 100 plus RE","Ventilation device LWZ 100 plus RE","Ventilation device LWZ 100 plus RE"]
[null,229979,"Ventilation device LWZ 100 plus LI",3002,"",null,null,null,null,null,null,229979,"Ventilation device LWZ 100 plus LI",3002,{"$f":"IF(AND(B483=L483,C483=M483,D483=N483),FALSE,TRUE)","v":false},null,229979,2537,3002,"3.000,00",19847,"op aanvraag","Zentrales Lüftungsgerät LWZ 100 plus LI","Ventilation device LWZ 100 plus LI","Appareil de ventilation centralisée LWZ 100 plus GA","Ventilation device LWZ 100 plus LI","Centrale WTW Unit LWZ 100 plus LI","Ventilation device LWZ 100 plus LI","Ventilation device LWZ 100 plus LI","Ventilation device LWZ 100 plus LI","Ventilation device LWZ 100 plus LI","Ventilation device LWZ 100 plus LI","Ventilation device LWZ 100 plus LI"]
[null,189800,"Air quality sensor FEQ",188,"",null,null,null,null,null,null,189800,"Air quality sensor FEQ",188,false,null,189800,236,188,220,"på forespørgsel","op aanvraag","Luftqualitätssensor FEQ","Air quality sensor FEQ","Sonde de qualité de l'air FEQ","Air quality sensor FEQ","Luchtkwaliteitssensor FEQ","Air quality sensor FEQ","Air quality sensor FEQ","Air quality sensor FEQ","Air quality sensor FEQ","Air quality sensor FEQ","Air quality sensor FEQ"]
[null,185358,"Remote control FEZ",152,"",null,null,null,null,null,null,185358,"Remote control FEZ",152,false,null,185358,198,152,185,"på forespørgsel","op aanvraag","Fernbedienung FEZ","Remote control FEZ","Commande à distance FEZ","Remote control FEZ","Afstandsbediening FEZ","Remote control FEZ","Remote control FEZ","Remote control FEZ","Remote control FEZ","Remote control FEZ","Remote control FEZ"]
[null,222447,"Pre-heater bank LWZ 70/170/270",295,"",null,null,null,null,null,null,222447,"Pre-heater bank LWZ 70/170/270",295,false,null,222447,308,295,"sur demande","på forespørgsel","op aanvraag","Vorheizregister LWZ 70/170/270","Pre-heater bank LWZ 70/170/270","Registre de préchauffage LWZ 70/170/270","Pre-heater bank LWZ 70/170/270","Voorverwarmingsregister LWZ 70/170/270","Pre-heater bank LWZ 70/170/270","Pre-heater bank LWZ 70/170/270","Pre-heater bank LWZ 70/170/270","Pre-heater bank LWZ 70/170/270","Pre-heater bank LWZ 70/170/270","Pre-heater bank LWZ 70/170/270"]
[null,168683,"Summer cassette LWZ 170/270",154,"",null,null,null,null,null,null,168683,"Summer cassette LWZ 170/270",154,false,null,168683,212,154,"sur demande","på forespørgsel","op aanvraag","Sommerkassette LWZ 170/270","Summer cassette LWZ 170/270","Cartouche été LWZ 170/270","Summer cassette LWZ 170/270","Zomercassette LWZ 170/270","Summer cassette LWZ 170/270","Summer cassette LWZ 170/270","Summer cassette LWZ 170/270","Summer cassette LWZ 170/270","Summer cassette LWZ 170/270","Summer cassette LWZ 170/270"]
[null,227046,"Summer cassette LWZ 70",150,"",null,null,null,null,null,null,227046,"Summer cassette LWZ 70",150,false,null,227046,176,150,"sur demande",1095,"op aanvraag","Sommerkassette LWZ 70","Summer cassette LWZ 70","Cartouche été LWZ 70","Summer cassette LWZ 70","Zomercassette LWZ 70","Summer cassette LWZ 70","Summer cassette LWZ 70","Summer cassette LWZ 70","Summer cassette LWZ 70","Summer cassette LWZ 70","Summer cassette LWZ 70"]
[null,160950,"Filter mat set LWZ 170/270 plus",10,"",null,null,null,null,null,null,160950,"Filter mat set LWZ 170/270 plus",10,false,null,160950,29.5,10,30,"på forespørgsel","op aanvraag","Filtermattenset LWZ 170/270 Plus, G3 , 10 Stück","Filter mat set LWZ 170/270 plus","Set tapis filtrants LWZ 170/270 Plus, G3, 10 p.","Filter mat set LWZ 170/270 plus","Filtermattenset LWZ 170/270 Plus, G3 , 10 Stuks","Filter mat set LWZ 170/270 plus","Filter mat set LWZ 170/270 plus","Filter mat set LWZ 170/270 plus","Filter mat set LWZ 170/270 plus","Filter mat set LWZ 170/270 plus","Filter mat set LWZ 170/270 plus"]
[null,222446,"Filter mat set LWZ 70",6,"",null,null,null,null,null,null,222446,"Filter mat set LWZ 70",6,false,null,222446,24.5,6,30,"på forespørgsel","op aanvraag","Filtermattenset LWZ 70, G3, 10 Stück","Filter mat set LWZ 70","Set tapis filtrants LWZ 70, G3, 10 p.","Filter mat set LWZ 70","Filtermattenset LWZ 70, G3, 10 Stuks","Filter mat set LWZ 70","Filter mat set LWZ 70","Filter mat set LWZ 70","Filter mat set LWZ 70","Filter mat set LWZ 70","Filter mat set LWZ 70"]
[null,227658,"Filter mat set LWZ 170/270, F7",91,"",null,null,null,null,null,null,227658,"Filter mat set LWZ 170/270, F7",91,false,null,227658,70,91,120,719,"op aanvraag","Filtermattenset LWZ 170/270, F7, 2 Stück","Filter mat set LWZ 170/270, F7","Set tapis filtrants LWZ 170/270, F7, 2 p.","Filter mat set LWZ 170/270, F7","Filtermattenset LWZ 170/270, F7, 2 Stuks","Filter mat set LWZ 170/270, F7","Filter mat set LWZ 170/270, F7","Filter mat set LWZ 170/270, F7","Filter mat set LWZ 170/270, F7","Filter mat set LWZ 170/270, F7","Filter mat set LWZ 170/270, F7"]
[null,227660,"Filter mat set LWZ 70, F7",66,"",null,null,null,null,null,null,227660,"Filter mat set LWZ 70, F7",66,false,null,227660,58,66,"sur demande",554,"op aanvraag","Filtermattenset LWZ 70, F7, 2 Stück","Filter mat set LWZ 70, F7","Set tapis filtrants LWZ 70, F7, 2 p.","Filter mat set LWZ 70, F7","Filtermattenset LWZ 70, F7, 2 Stuks","Filter mat set LWZ 70, F7","Filter mat set LWZ 70, F7","Filter mat set LWZ 70, F7","Filter mat set LWZ 70, F7","Filter mat set LWZ 70, F7","Filter mat set LWZ 70, F7"]
[null,232476,"Filtermattenset LWZ 370, F5, 2 Stück",37,"",null,null,null,null,null,null,232476,"Filtermattenset LWZ 370, F5, 2 Stück",37,false,null,232476,36,37,"sur demande",254,36,"Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stuks","Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stück","Filtermattenset LWZ 370, F5, 2 Stück"]
[null,232477,"Filtermattenset LWZ 370, F7, 2 Stück",49,"",null,null,null,null,null,null,232477,"Filtermattenset LWZ 370, F7, 2 Stück",49,false,null,232477,41,49,120,338,"op aanvraag","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stuks","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stück","Filtermattenset LWZ 370, F7, 2 Stück"]
[null,232475,"Filtermattenset LWZ 370, G4, 10 Stück",15,"",null,null,null,null,null,null,232475,"Filtermattenset LWZ 370, G4, 10 Stück",15,false,null,232475,27.5,15,30,104,"op aanvraag","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stuks","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stück","Filtermattenset LWZ 370, G4, 10 Stück"]
[null,233866,"Austausch-Enthalpie-Wärmeübertrager","On request","",null,null,null,null,null,null,233866,"Austausch-Enthalpie-Wärmeübertrager","On request",false,null,233866,1581,"On request","sur demande","på forespørgsel","op aanvraag","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Vervangings-Enthalpie-Warmtewisselaar","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager","Austausch-Enthalpie-Wärmeübertrager"]
[null,223228,"Adaptor LWZ 100 to 2x DN 100",5,"",null,null,null,null,null,null,223228,"Adaptor LWZ 100 to 2x DN 100",5,false,null,223228,17.7,5,10,"på forespørgsel","op aanvraag","Übergangsstück LWZ 100 auf 2 x DN 100","Adaptor LWZ 100 to 2x DN 100","Raccord de transition LWZ 100 à 2 x DN 100","Adaptor LWZ 100 to 2x DN 100","Overgangsstuk LWZ 100 naar 2 x DN 100","Adaptor LWZ 100 to 2x DN 100","Adaptor LWZ 100 to 2x DN 100","Adaptor LWZ 100 to 2x DN 100","Adaptor LWZ 100 to 2x DN 100","Adaptor LWZ 100 to 2x DN 100","Adaptor LWZ 100 to 2x DN 100"]
[null,231336,"Übergangsstück Kombikanal EPS auf 2 x DN 100","On request","",null,null,null,null,null,null,231336,"Übergangsstück Kombikanal EPS auf 2 x DN 100","On request",false,null,231336,47,"On request",50,"på forespørgsel","op aanvraag","Übergangsstück Kombikanal EPS auf 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100","Overgangsstuk Combikanaal EPS naar 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100","Übergangsstück Kombikanal EPS auf 2 x DN 100"]
[null,223230,"Extension Combi Channel EPS",24,"",null,null,null,null,null,null,223230,"Extension Combi Channel EPS",24,false,null,223230,31,24,30,"på forespørgsel","op aanvraag","Verlängerung Kombikanal EPS","Extension Combi Channel EPS","Rallonge gaine combinée EPS","Extension Combi Channel EPS","Verlenging Combikanaal EPS","Extension Combi Channel EPS","Extension Combi Channel EPS","Extension Combi Channel EPS","Extension Combi Channel EPS","Extension Combi Channel EPS","Extension Combi Channel EPS"]
[null,222383,"Filter mat set LWZ 100",7,"",null,null,null,null,null,null,222383,"Filter mat set LWZ 100",7,false,null,222383,24.5,7,30,"på forespørgsel","op aanvraag","Filtermattenset LWZ 100, G3, 10 Stück","Filter mat set LWZ 100","Set tapis filtrants LWZ 100, G3, 10 p.","Filter mat set LWZ 100","Filtermattenset LWZ 100, G3, 10 Stuks","Filter mat set LWZ 100","Filter mat set LWZ 100","Filter mat set LWZ 100","Filter mat set LWZ 100","Filter mat set LWZ 100","Filter mat set LWZ 100"]
[null,231446,"Filter mat set LWZ 100 Plus, G4",11,"",null,null,null,null,null,null,231446,"Filter mat set LWZ 100 Plus, G4",11,false,null,231446,28.5,11,30,74,"op aanvraag","Filtermattenset LWZ 100 Plus, G4, 10 Stück","Filter mat set LWZ 100 Plus, G4","Set tapis filtrants LWZ 100 Plus, G4, 10 p.","Filter mat set LWZ 100 Plus, G4","Filtermattenset LWZ 100 Plus, G4, 10 Stuks","Filter mat set LWZ 100 Plus, G4","Filter mat set LWZ 100 Plus, G4","Filter mat set LWZ 100 Plus, G4","Filter mat set LWZ 100 Plus, G4","Filter mat set LWZ 100 Plus, G4","Filter mat set LWZ 100 Plus, G4"]
[null,231447,"Filter mat set LWZ 100, G4",11,"",null,null,null,null,null,null,231447,"Filter mat set LWZ 100, G4",11,false,null,231447,28.5,11,30,74,"op aanvraag","Filtermattenset LWZ 100 , G4, 10 Stück","Filter mat set LWZ 100, G4","Set tapis filtrants LWZ 100, G4, 10 p.","Filter mat set LWZ 100, G4","Filtermattenset LWZ 100 , G4, 10 Stuks","Filter mat set LWZ 100, G4","Filter mat set LWZ 100, G4","Filter mat set LWZ 100, G4","Filter mat set LWZ 100, G4","Filter mat set LWZ 100, G4","Filter mat set LWZ 100, G4"]
[null,231448,"Filter mat set LWZ 100, F5",73,"",null,null,null,null,null,null,231448,"Filter mat set LWZ 100, F5",73,false,null,231448,37,73,"sur demande",496,"op aanvraag","Filtermattenset LWZ 100 , F5, 2 Stück","Filter mat set LWZ 100, F5","Set tapis filtrants LWZ 100, F5, 2 p.","Filter mat set LWZ 100, F5","Filtermattenset LWZ 100 , F5, 2 Stuks","Filter mat set LWZ 100, F5","Filter mat set LWZ 100, F5","Filter mat set LWZ 100, F5","Filter mat set LWZ 100, F5","Filter mat set LWZ 100, F5","Filter mat set LWZ 100, F5"]
[null,231449,"Filter mat set LWZ 100, F7",90,"",null,null,null,null,null,null,231449,"Filter mat set LWZ 100, F7",90,false,null,231449,42.5,90,120,417,"op aanvraag","Filtermattenset LWZ 100 , F7, 2 Stück","Filter mat set LWZ 100, F7","Set tapis filtrants LWZ 100, F7, 2 p.","Filter mat set LWZ 100, F7","Filtermattenset LWZ 100 , F7, 2 Stuks","Filter mat set LWZ 100, F7","Filter mat set LWZ 100, F7","Filter mat set LWZ 100, F7","Filter mat set LWZ 100, F7","Filter mat set LWZ 100, F7","Filter mat set LWZ 100, F7"]
[null,229317,"Ventilation device LA 60 A",334,"",null,null,null,null,null,null,229317,"Ventilation device LA 60 A",334,false,null,229317,427,334,"sur demande",2101,"op aanvraag","Lüftungsgerät ohne Wärmerückgewinnung LA 60 A","Ventilation device LA 60 A","Ventilateur sans récupération de chaleur LA 60 A","Ventilation device LA 60 A","Ventilatieunit zonder warmteterugwinning LA 60 A","Ventilation device LA 60 A","Ventilation device LA 60 A","Ventilation device LA 60 A","Ventilation device LA 60 A","Ventilation device LA 60 A","Ventilation device LA 60 A"]
[null,229318,"Ventilation device LA 60 U",332,"",null,null,null,null,null,null,229318,"Ventilation device LA 60 U",332,false,null,229318,427,332,"sur demande",2049,"op aanvraag","Lüftungsgerät ohne Wärmerückgewinnung LA 60 U","Ventilation device LA 60 U","Ventilateur sans récupération de chaleur LA 60 U","Ventilation device LA 60 U","Ventilatieunit zonder warmteterugwinning LA 60 U","Ventilation device LA 60 U","Ventilation device LA 60 U","Ventilation device LA 60 U","Ventilation device LA 60 U","Ventilation device LA 60 U","Ventilation device LA 60 U"]
[null,232123,"Ventilation device LA 60 AB","On request","",null,null,null,null,null,null,232123,"Ventilation device LA 60 AB","On request",false,null,232123,470,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungsgerät ohne Wärmerückgewinnung LA 60 AB","Ventilation device LA 60 AB","Ventilateur sans récupération de chaleur LA 60 AB","Ventilation device LA 60 AB","Ventilatieunit zonder warmteterugwinning LA 60 AB","Ventilation device LA 60 AB","Ventilation device LA 60 AB","Ventilation device LA 60 AB","Ventilation device LA 60 AB","Ventilation device LA 60 AB","Ventilation device LA 60 AB"]
[null,229319,"Filter mat set LA 60, G2","On request","",null,null,null,null,null,null,229319,"Filter mat set LA 60, G2","On request",false,null,229319,23.7,"On request","sur demande","på forespørgsel","op aanvraag","Filtermattenset LA 60, G2, 5 Stück","Filter mat set LA 60, G2","Set tapis filtrants LA 60, G2, 5 p.","Filter mat set LA 60, G2","Filtermattenset LA 60, G2, 5 Stuks","Filter mat set LA 60, G2","Filter mat set LA 60, G2","Filter mat set LA 60, G2","Filter mat set LA 60, G2","Filter mat set LA 60, G2","Filter mat set LA 60, G2"]
[null,231104,"Air routing with grill LA 60","On request","",null,null,null,null,null,null,231104,"Air routing with grill LA 60","On request",false,null,231104,132,"On request","sur demande","på forespørgsel","op aanvraag","Wanddurchführung mit Außengitter LA 60","Air routing with grill LA 60","Traversée murale avec grille extérieure LA 60","Air routing with grill LA 60","Wanddoorvoer met buitenrooster LA 60","Air routing with grill LA 60","Air routing with grill LA 60","Air routing with grill LA 60","Air routing with grill LA 60","Air routing with grill LA 60","Air routing with grill LA 60"]
[null,232026,"Ventilation device LA 30 WRG","On request","",null,null,null,null,null,null,232026,"Ventilation device LA 30 WRG","On request",false,null,232026,556,"On request","sur demande",4747,"op aanvraag","Lüftungsgerät mit Wärmerückgewinnung LA 30 WRG","Ventilation device LA 30 WRG","Ventilateur avec récupération de chaleur LA 30 WRG","Ventilation device LA 30 WRG","Ventilatieunit met warmteterugwinning LA 30 WRG","Ventilation device LA 30 WRG","Ventilation device LA 30 WRG","Ventilation device LA 30 WRG","Ventilation device LA 30 WRG","Ventilation device LA 30 WRG","Ventilation device LA 30 WRG"]
[null,233019,"Geräte-Anschlussset 2 Luftverteiler","On request","",null,null,null,null,null,null,233019,"Geräte-Anschlussset 2 Luftverteiler","On request",false,null,233019,827,"On request","sur demande",3081,"op aanvraag","Geräte-Anschlussset 2 Luftverteiler","Geräte-Anschlussset 2 Luftverteiler","Geräte-Anschlussset 2 Luftverteiler","Geräte-Anschlussset 2 Luftverteiler","Toestel-aansluitset 2 luchtverdelers","Geräte-Anschlussset 2 Luftverteiler","Geräte-Anschlussset 2 Luftverteiler","Geräte-Anschlussset 2 Luftverteiler","Geräte-Anschlussset 2 Luftverteiler","Geräte-Anschlussset 2 Luftverteiler","Geräte-Anschlussset 2 Luftverteiler"]
[null,233020,"Geräte-Anschlussset 3 Luftverteiler","On request","",null,null,null,null,null,null,233020,"Geräte-Anschlussset 3 Luftverteiler","On request",false,null,233020,1044,"On request","sur demande",3934,"op aanvraag","Geräte-Anschlussset 3 Luftverteiler","Geräte-Anschlussset 3 Luftverteiler","Geräte-Anschlussset 3 Luftverteiler","Geräte-Anschlussset 3 Luftverteiler","Toestel-aansluitset 3 luchtverdelers","Geräte-Anschlussset 3 Luftverteiler","Geräte-Anschlussset 3 Luftverteiler","Geräte-Anschlussset 3 Luftverteiler","Geräte-Anschlussset 3 Luftverteiler","Geräte-Anschlussset 3 Luftverteiler","Geräte-Anschlussset 3 Luftverteiler"]
[null,233021,"Geräte-Anschlussset 4 Luftverteiler","On request","",null,null,null,null,null,null,233021,"Geräte-Anschlussset 4 Luftverteiler","On request",false,null,233021,1223,"On request","sur demande",4549,"op aanvraag","Geräte-Anschlussset 4 Luftverteiler","Geräte-Anschlussset 4 Luftverteiler","Geräte-Anschlussset 4 Luftverteiler","Geräte-Anschlussset 4 Luftverteiler","Toestel-aansluitset 4 luchtverdelers","Geräte-Anschlussset 4 Luftverteiler","Geräte-Anschlussset 4 Luftverteiler","Geräte-Anschlussset 4 Luftverteiler","Geräte-Anschlussset 4 Luftverteiler","Geräte-Anschlussset 4 Luftverteiler","Geräte-Anschlussset 4 Luftverteiler"]
[null,233022,"Set Separate Außenluftansaugung bis 2m","On request","",null,null,null,null,null,null,233022,"Set Separate Außenluftansaugung bis 2m","On request",false,null,233022,349,"On request","sur demande","på forespørgsel","op aanvraag","Set Separate Außenluftansaugung bis 2m","Set Separate Außenluftansaugung bis 2m","Set Separate Außenluftansaugung bis 2m","Set Separate Außenluftansaugung bis 2m","Set separate buitenluchtaanzuiging tot 2m","Set Separate Außenluftansaugung bis 2m","Set Separate Außenluftansaugung bis 2m","Set Separate Außenluftansaugung bis 2m","Set Separate Außenluftansaugung bis 2m","Set Separate Außenluftansaugung bis 2m","Set Separate Außenluftansaugung bis 2m"]
[null,233023,"Set Separate Außenluftansaugung bis 6m","On request","",null,null,null,null,null,null,233023,"Set Separate Außenluftansaugung bis 6m","On request",false,null,233023,429,"On request","sur demande","på forespørgsel","op aanvraag","Set Separate Außenluftansaugung bis 6m","Set Separate Außenluftansaugung bis 6m","Set Separate Außenluftansaugung bis 6m","Set Separate Außenluftansaugung bis 6m","Set separate buitenluchtaanzuiging tot 6m","Set Separate Außenluftansaugung bis 6m","Set Separate Außenluftansaugung bis 6m","Set Separate Außenluftansaugung bis 6m","Set Separate Außenluftansaugung bis 6m","Set Separate Außenluftansaugung bis 6m","Set Separate Außenluftansaugung bis 6m"]
[null,233024,"Außen-/Fortluftset Dach DN 160","On request","",null,null,null,null,null,null,233024,"Außen-/Fortluftset Dach DN 160","On request",false,null,233024,2000,"On request","sur demande","på forespørgsel","op aanvraag","Außen-/Fortluftset Dach DN 160","Außen-/Fortluftset Dach DN 160","Außen-/Fortluftset Dach DN 160","Außen-/Fortluftset Dach DN 160","Buiten-/aanvoerluchtset Dach DN 160","Außen-/Fortluftset Dach DN 160","Außen-/Fortluftset Dach DN 160","Außen-/Fortluftset Dach DN 160","Außen-/Fortluftset Dach DN 160","Außen-/Fortluftset Dach DN 160","Außen-/Fortluftset Dach DN 160"]
[null,233025,"Außen-/Fortluftset Wand DN 125","On request","",null,null,null,null,null,null,233025,"Außen-/Fortluftset Wand DN 125","On request",false,null,233025,534,"On request","sur demande",4201,"op aanvraag","Außen-/Fortluftset Wand DN 125","Außen-/Fortluftset Wand DN 125","Außen-/Fortluftset Wand DN 125","Außen-/Fortluftset Wand DN 125","Buiten-/aanvoerluchtset wand DN 125","Außen-/Fortluftset Wand DN 125","Außen-/Fortluftset Wand DN 125","Außen-/Fortluftset Wand DN 125","Außen-/Fortluftset Wand DN 125","Außen-/Fortluftset Wand DN 125","Außen-/Fortluftset Wand DN 125"]
[null,233026,"Außen-/Fortluftset Wand DN 160","On request","",null,null,null,null,null,null,233026,"Außen-/Fortluftset Wand DN 160","On request",false,null,233026,623,"On request","sur demande",4479,"op aanvraag","Außen-/Fortluftset Wand DN 160","Außen-/Fortluftset Wand DN 160","Außen-/Fortluftset Wand DN 160","Außen-/Fortluftset Wand DN 160","Buiten-/aanvoerluchtset wand DN 160","Außen-/Fortluftset Wand DN 160","Außen-/Fortluftset Wand DN 160","Außen-/Fortluftset Wand DN 160","Außen-/Fortluftset Wand DN 160","Außen-/Fortluftset Wand DN 160","Außen-/Fortluftset Wand DN 160"]
[null,233027,"Außen-/Fortluftset Wand Kombigitter","On request","",null,null,null,null,null,null,233027,"Außen-/Fortluftset Wand Kombigitter","On request",false,null,233027,364,"On request","sur demande","på forespørgsel","op aanvraag","Außen-/Fortluftset Wand Kombigitter","Außen-/Fortluftset Wand Kombigitter","Außen-/Fortluftset Wand Kombigitter","Außen-/Fortluftset Wand Kombigitter","Buiten-/aanvoerluchtset wand Kombigitter","Außen-/Fortluftset Wand Kombigitter","Außen-/Fortluftset Wand Kombigitter","Außen-/Fortluftset Wand Kombigitter","Außen-/Fortluftset Wand Kombigitter","Außen-/Fortluftset Wand Kombigitter","Außen-/Fortluftset Wand Kombigitter"]
[null,231127,"Zu- und Abluftset LVE 120","On request","",null,null,null,null,null,null,231127,"Zu- und Abluftset LVE 120","On request",false,null,231127,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVE 120","Zu- und Abluftset LVE 120","Zu- und Abluftset LVE 120","Zu- und Abluftset LVE 120","Toevoer- en afvoerset LVE 120","Zu- und Abluftset LVE 120","Zu- und Abluftset LVE 120","Zu- und Abluftset LVE 120","Zu- und Abluftset LVE 120","Zu- und Abluftset LVE 120","Zu- und Abluftset LVE 120"]
[null,231128,"Zu- und Abluftset LVE 160","On request","",null,null,null,null,null,null,231128,"Zu- und Abluftset LVE 160","On request",false,null,231128,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVE 160","Zu- und Abluftset LVE 160","Zu- und Abluftset LVE 160","Zu- und Abluftset LVE 160","Toevoer- en afvoerset LVE 160","Zu- und Abluftset LVE 160","Zu- und Abluftset LVE 160","Zu- und Abluftset LVE 160","Zu- und Abluftset LVE 160","Zu- und Abluftset LVE 160","Zu- und Abluftset LVE 160"]
[null,231129,"Zu- und Abluftset LVE 200","On request","",null,null,null,null,null,null,231129,"Zu- und Abluftset LVE 200","On request",false,null,231129,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVE 200","Zu- und Abluftset LVE 200","Zu- und Abluftset LVE 200","Zu- und Abluftset LVE 200","Toevoer- en afvoerset LVE 200","Zu- und Abluftset LVE 200","Zu- und Abluftset LVE 200","Zu- und Abluftset LVE 200","Zu- und Abluftset LVE 200","Zu- und Abluftset LVE 200","Zu- und Abluftset LVE 200"]
[null,231130,"Zu- und Abluftset LVE 240","On request","",null,null,null,null,null,null,231130,"Zu- und Abluftset LVE 240","On request",false,null,231130,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVE 240","Zu- und Abluftset LVE 240","Zu- und Abluftset LVE 240","Zu- und Abluftset LVE 240","Toevoer- en afvoerset LVE 240","Zu- und Abluftset LVE 240","Zu- und Abluftset LVE 240","Zu- und Abluftset LVE 240","Zu- und Abluftset LVE 240","Zu- und Abluftset LVE 240","Zu- und Abluftset LVE 240"]
[null,232712,"Zu- und Abluftset LVE 280","On request","",null,null,null,null,null,null,232712,"Zu- und Abluftset LVE 280","On request",false,null,232712,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVE 280","Zu- und Abluftset LVE 280","Zu- und Abluftset LVE 280","Zu- und Abluftset LVE 280","Toevoer- en afvoerset LVE 280","Zu- und Abluftset LVE 280","Zu- und Abluftset LVE 280","Zu- und Abluftset LVE 280","Zu- und Abluftset LVE 280","Zu- und Abluftset LVE 280","Zu- und Abluftset LVE 280"]
[null,223448,"Zu- und Abluftset LVS 125 Z","On request","",null,null,null,null,null,null,223448,"Zu- und Abluftset LVS 125 Z","On request",false,null,223448,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVS 125 Z","Zu- und Abluftset LVS 125 Z","Zu- und Abluftset LVS 125 Z","Zu- und Abluftset LVS 125 Z","Toevoer- en afvoerset LVS 125","Zu- und Abluftset LVS 125 Z","Zu- und Abluftset LVS 125 Z","Zu- und Abluftset LVS 125 Z","Zu- und Abluftset LVS 125 Z","Zu- und Abluftset LVS 125 Z","Zu- und Abluftset LVS 125 Z"]
[null,223449,"Zu- und Abluftset LVS 160 Z","On request",{"$f":"IF(O526=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,223449,"Zu- und Abluftset LVS 160 Z","On request",false,null,223449,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVS 160 Z","Zu- und Abluftset LVS 160 Z","Zu- und Abluftset LVS 160 Z","Zu- und Abluftset LVS 160 Z","Toevoer- en afvoerset LVS 160","Zu- und Abluftset LVS 160 Z","Zu- und Abluftset LVS 160 Z","Zu- und Abluftset LVS 160 Z","Zu- und Abluftset LVS 160 Z","Zu- und Abluftset LVS 160 Z","Zu- und Abluftset LVS 160 Z"]
[null,223450,"Zu- und Abluftset LVS 200 Z","On request","",null,null,null,null,null,null,223450,"Zu- und Abluftset LVS 200 Z","On request",false,null,223450,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVS 200 Z","Zu- und Abluftset LVS 200 Z","Zu- und Abluftset LVS 200 Z","Zu- und Abluftset LVS 200 Z","Toevoer- en afvoerset LVS 200","Zu- und Abluftset LVS 200 Z","Zu- und Abluftset LVS 200 Z","Zu- und Abluftset LVS 200 Z","Zu- und Abluftset LVS 200 Z","Zu- und Abluftset LVS 200 Z","Zu- und Abluftset LVS 200 Z"]
[null,223451,"Zu- und Abluftset LVS 240 Z","On request","",null,null,null,null,null,null,223451,"Zu- und Abluftset LVS 240 Z","On request",false,null,223451,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVS 240 Z","Zu- und Abluftset LVS 240 Z","Zu- und Abluftset LVS 240 Z","Zu- und Abluftset LVS 240 Z","Toevoer- en afvoerset LVS 240","Zu- und Abluftset LVS 240 Z","Zu- und Abluftset LVS 240 Z","Zu- und Abluftset LVS 240 Z","Zu- und Abluftset LVS 240 Z","Zu- und Abluftset LVS 240 Z","Zu- und Abluftset LVS 240 Z"]
[null,223452,"Zu- und Abluftset LVS 125 D","On request","",null,null,null,null,null,null,223452,"Zu- und Abluftset LVS 125 D","On request",false,null,223452,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVS 125 D","Zu- und Abluftset LVS 125 D","Zu- und Abluftset LVS 125 D","Zu- und Abluftset LVS 125 D","Toevoer- en afvoerset LVS 125 D","Zu- und Abluftset LVS 125 D","Zu- und Abluftset LVS 125 D","Zu- und Abluftset LVS 125 D","Zu- und Abluftset LVS 125 D","Zu- und Abluftset LVS 125 D","Zu- und Abluftset LVS 125 D"]
[null,223453,"Zu- und Abluftset LVS 160 D","On request","",null,null,null,null,null,null,223453,"Zu- und Abluftset LVS 160 D","On request",{"$f":"IF(AND(B530=L530,C530=M530,D530=N530),FALSE,TRUE)","v":false},null,223453,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVS 160 D","Zu- und Abluftset LVS 160 D","Zu- und Abluftset LVS 160 D","Zu- und Abluftset LVS 160 D","Toevoer- en afvoerset LVS 160 D","Zu- und Abluftset LVS 160 D","Zu- und Abluftset LVS 160 D","Zu- und Abluftset LVS 160 D","Zu- und Abluftset LVS 160 D","Zu- und Abluftset LVS 160 D","Zu- und Abluftset LVS 160 D"]
[null,223454,"Zu- und Abluftset LVS 200 D","On request","",null,null,null,null,null,null,223454,"Zu- und Abluftset LVS 200 D","On request",false,null,223454,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVS 200 D","Zu- und Abluftset LVS 200 D","Zu- und Abluftset LVS 200 D","Zu- und Abluftset LVS 200 D","Toevoer- en afvoerset LVS 200 D","Zu- und Abluftset LVS 200 D","Zu- und Abluftset LVS 200 D","Zu- und Abluftset LVS 200 D","Zu- und Abluftset LVS 200 D","Zu- und Abluftset LVS 200 D","Zu- und Abluftset LVS 200 D"]
[null,223455,"Zu- und Abluftset LVS 240 D","On request","",null,null,null,null,null,null,223455,"Zu- und Abluftset LVS 240 D","On request",false,null,223455,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LVS 240 D","Zu- und Abluftset LVS 240 D","Zu- und Abluftset LVS 240 D","Zu- und Abluftset LVS 240 D","Toevoer- en afvoerset LVS 240 D","Zu- und Abluftset LVS 240 D","Zu- und Abluftset LVS 240 D","Zu- und Abluftset LVS 240 D","Zu- und Abluftset LVS 240 D","Zu- und Abluftset LVS 240 D","Zu- und Abluftset LVS 240 D"]
[null,223322,"Zu- und Abluftset LFK 60 Z","On request","",null,null,null,null,null,null,223322,"Zu- und Abluftset LFK 60 Z","On request",false,null,223322,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 60 Z","Zu- und Abluftset LFK 60 Z","Zu- und Abluftset LFK 60 Z","Zu- und Abluftset LFK 60 Z","Toevoer- en afvoerset LFK 60 Z","Zu- und Abluftset LFK 60 Z","Zu- und Abluftset LFK 60 Z","Zu- und Abluftset LFK 60 Z","Zu- und Abluftset LFK 60 Z","Zu- und Abluftset LFK 60 Z","Zu- und Abluftset LFK 60 Z"]
[null,223323,"Zu- und Abluftset LFK 80 Z","On request","",null,null,null,null,null,null,223323,"Zu- und Abluftset LFK 80 Z","On request",false,null,223323,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 80 Z","Zu- und Abluftset LFK 80 Z","Zu- und Abluftset LFK 80 Z","Zu- und Abluftset LFK 80 Z","Toevoer- en afvoerset LFK 80 Z","Zu- und Abluftset LFK 80 Z","Zu- und Abluftset LFK 80 Z","Zu- und Abluftset LFK 80 Z","Zu- und Abluftset LFK 80 Z","Zu- und Abluftset LFK 80 Z","Zu- und Abluftset LFK 80 Z"]
[null,167151,"Zu- und Abluftset LFK 100 Z","On request","",null,null,null,null,null,null,167151,"Zu- und Abluftset LFK 100 Z","On request",false,null,167151,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 100 Z","Zu- und Abluftset LFK 100 Z","Zu- und Abluftset LFK 100 Z","Zu- und Abluftset LFK 100 Z","Toevoer- en afvoerset LFK 100 Z","Zu- und Abluftset LFK 100 Z","Zu- und Abluftset LFK 100 Z","Zu- und Abluftset LFK 100 Z","Zu- und Abluftset LFK 100 Z","Zu- und Abluftset LFK 100 Z","Zu- und Abluftset LFK 100 Z"]
[null,167152,"Zu- und Abluftset LFK 125 Z","On request","",null,null,null,null,null,null,167152,"Zu- und Abluftset LFK 125 Z","On request",false,null,167152,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 125 Z","Zu- und Abluftset LFK 125 Z","Zu- und Abluftset LFK 125 Z","Zu- und Abluftset LFK 125 Z","Toevoer- en afvoerset LFK 125 Z","Zu- und Abluftset LFK 125 Z","Zu- und Abluftset LFK 125 Z","Zu- und Abluftset LFK 125 Z","Zu- und Abluftset LFK 125 Z","Zu- und Abluftset LFK 125 Z","Zu- und Abluftset LFK 125 Z"]
[null,167153,"Zu- und Abluftset LFK 160 Z","On request","",null,null,null,null,null,null,167153,"Zu- und Abluftset LFK 160 Z","On request",false,null,167153,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 160 Z","Zu- und Abluftset LFK 160 Z","Zu- und Abluftset LFK 160 Z","Zu- und Abluftset LFK 160 Z","Toevoer- en afvoerset LFK 160 Z","Zu- und Abluftset LFK 160 Z","Zu- und Abluftset LFK 160 Z","Zu- und Abluftset LFK 160 Z","Zu- und Abluftset LFK 160 Z","Zu- und Abluftset LFK 160 Z","Zu- und Abluftset LFK 160 Z"]
[null,220447,"Zu- und Abluftset LFK 200 Z","On request","",null,null,null,null,null,null,220447,"Zu- und Abluftset LFK 200 Z","On request",false,null,220447,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 200 Z","Zu- und Abluftset LFK 200 Z","Zu- und Abluftset LFK 200 Z","Zu- und Abluftset LFK 200 Z","Toevoer- en afvoerset LFK 200 Z","Zu- und Abluftset LFK 200 Z","Zu- und Abluftset LFK 200 Z","Zu- und Abluftset LFK 200 Z","Zu- und Abluftset LFK 200 Z","Zu- und Abluftset LFK 200 Z","Zu- und Abluftset LFK 200 Z"]
[null,223457,"Zu- und Abluftset LFK 240 Z","On request","",null,null,null,null,null,null,223457,"Zu- und Abluftset LFK 240 Z","On request",false,null,223457,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 240 Z","Zu- und Abluftset LFK 240 Z","Zu- und Abluftset LFK 240 Z","Zu- und Abluftset LFK 240 Z","Toevoer- en afvoerset LFK 240 Z","Zu- und Abluftset LFK 240 Z","Zu- und Abluftset LFK 240 Z","Zu- und Abluftset LFK 240 Z","Zu- und Abluftset LFK 240 Z","Zu- und Abluftset LFK 240 Z","Zu- und Abluftset LFK 240 Z"]
[null,232714,"Zu- und Abluftset LFK 280 Z","On request","",null,null,null,null,null,null,232714,"Zu- und Abluftset LFK 280 Z","On request",false,null,232714,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 280 Z","Zu- und Abluftset LFK 280 Z","Zu- und Abluftset LFK 280 Z","Zu- und Abluftset LFK 280 Z","Toevoer- en afvoerset LFK 280 Z","Zu- und Abluftset LFK 280 Z","Zu- und Abluftset LFK 280 Z","Zu- und Abluftset LFK 280 Z","Zu- und Abluftset LFK 280 Z","Zu- und Abluftset LFK 280 Z","Zu- und Abluftset LFK 280 Z"]
[null,230161,"Außenluftset A1","On request","",null,null,null,null,null,null,230161,"Außenluftset A1","On request",false,null,230161,"auf Anfrage","On request","sur demande",2883,"op aanvraag","Außenluftset A1","Außenluftset A1","Außenluftset A1","Außenluftset A1","Buitenluchtset A1","Außenluftset A1","Außenluftset A1","Außenluftset A1","Außenluftset A1","Außenluftset A1","Außenluftset A1"]
[null,230162,"Außenluftset A2","On request","",null,null,null,null,null,null,230162,"Außenluftset A2","On request",false,null,230162,"auf Anfrage","On request","sur demande",3814,"op aanvraag","Außenluftset A2","Außenluftset A2","Außenluftset A2","Außenluftset A2","Buitenluchtset A2","Außenluftset A2","Außenluftset A2","Außenluftset A2","Außenluftset A2","Außenluftset A2","Außenluftset A2"]
[null,167155,"Außen- und Fortluftset FA 1","On request","",null,null,null,null,null,null,167155,"Außen- und Fortluftset FA 1","On request",false,null,167155,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Außen- und Fortluftset FA 1","Außen- und Fortluftset FA 1","Außen- und Fortluftset FA 1","Außen- und Fortluftset FA 1","Buiten- en aanvoerluchtset FA 1","Außen- und Fortluftset FA 1","Außen- und Fortluftset FA 1","Außen- und Fortluftset FA 1","Außen- und Fortluftset FA 1","Außen- und Fortluftset FA 1","Außen- und Fortluftset FA 1"]
[null,167156,"Außen- und Fortluftset FA 2","On request","",null,null,null,null,null,null,167156,"Außen- und Fortluftset FA 2","On request",false,null,167156,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Außen- und Fortluftset FA 2","Außen- und Fortluftset FA 2","Außen- und Fortluftset FA 2","Außen- und Fortluftset FA 2","Buiten- en aanvoerluchtset FA 2","Außen- und Fortluftset FA 2","Außen- und Fortluftset FA 2","Außen- und Fortluftset FA 2","Außen- und Fortluftset FA 2","Außen- und Fortluftset FA 2","Außen- und Fortluftset FA 2"]
[null,220448,"Außen- und Fortluftset FA 3","On request","",null,null,null,null,null,null,220448,"Außen- und Fortluftset FA 3","On request",false,null,220448,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Außen- und Fortluftset FA 3","Außen- und Fortluftset FA 3","Außen- und Fortluftset FA 3","Außen- und Fortluftset FA 3","Buiten- en aanvoerluchtset FA 3","Außen- und Fortluftset FA 3","Außen- und Fortluftset FA 3","Außen- und Fortluftset FA 3","Außen- und Fortluftset FA 3","Außen- und Fortluftset FA 3","Außen- und Fortluftset FA 3"]
[null,223328,"Außen- und Fortluftset FA 70","On request","",null,null,null,null,null,null,223328,"Außen- und Fortluftset FA 70","On request",false,null,223328,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Außen- und Fortluftset FA 70","Außen- und Fortluftset FA 70","Außen- und Fortluftset FA 70","Außen- und Fortluftset FA 70","Buiten- en aanvoerluchtset FA 70","Außen- und Fortluftset FA 70","Außen- und Fortluftset FA 70","Außen- und Fortluftset FA 70","Außen- und Fortluftset FA 70","Außen- und Fortluftset FA 70","Außen- und Fortluftset FA 70"]
[null,223324,"Zu- und Abluftset LFK 60 D","On request","",null,null,null,null,null,null,223324,"Zu- und Abluftset LFK 60 D","On request",false,null,223324,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 60 D","Zu- und Abluftset LFK 60 D","Zu- und Abluftset LFK 60 D","Zu- und Abluftset LFK 60 D","Toevoer- en afvoerset LFK 60 D","Zu- und Abluftset LFK 60 D","Zu- und Abluftset LFK 60 D","Zu- und Abluftset LFK 60 D","Zu- und Abluftset LFK 60 D","Zu- und Abluftset LFK 60 D","Zu- und Abluftset LFK 60 D"]
[null,223325,"Zu- und Abluftset LFK 80 D","On request","",null,null,null,null,null,null,223325,"Zu- und Abluftset LFK 80 D","On request",false,null,223325,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 80 D","Zu- und Abluftset LFK 80 D","Zu- und Abluftset LFK 80 D","Zu- und Abluftset LFK 80 D","Toevoer- en afvoerset LFK 80 D","Zu- und Abluftset LFK 80 D","Zu- und Abluftset LFK 80 D","Zu- und Abluftset LFK 80 D","Zu- und Abluftset LFK 80 D","Zu- und Abluftset LFK 80 D","Zu- und Abluftset LFK 80 D"]
[null,159265,"Zu- und Abluftset LFK 100 D","On request","",null,null,null,null,null,null,159265,"Zu- und Abluftset LFK 100 D","On request",false,null,159265,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 100 D","Zu- und Abluftset LFK 100 D","Zu- und Abluftset LFK 100 D","Zu- und Abluftset LFK 100 D","Toevoer- en afvoerset LFK 100 D","Zu- und Abluftset LFK 100 D","Zu- und Abluftset LFK 100 D","Zu- und Abluftset LFK 100 D","Zu- und Abluftset LFK 100 D","Zu- und Abluftset LFK 100 D","Zu- und Abluftset LFK 100 D"]
[null,159267,"Zu- und Abluftset LFK 125 D","On request","",null,null,null,null,null,null,159267,"Zu- und Abluftset LFK 125 D","On request",false,null,159267,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 125 D","Zu- und Abluftset LFK 125 D","Zu- und Abluftset LFK 125 D","Zu- und Abluftset LFK 125 D","Toevoer- en afvoerset LFK 125 D","Zu- und Abluftset LFK 125 D","Zu- und Abluftset LFK 125 D","Zu- und Abluftset LFK 125 D","Zu- und Abluftset LFK 125 D","Zu- und Abluftset LFK 125 D","Zu- und Abluftset LFK 125 D"]
[null,159268,"Zu- und Abluftset LFK 160 D","On request","",null,null,null,null,null,null,159268,"Zu- und Abluftset LFK 160 D","On request",false,null,159268,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 160 D","Zu- und Abluftset LFK 160 D","Zu- und Abluftset LFK 160 D","Zu- und Abluftset LFK 160 D","Toevoer- en afvoerset LFK 160 D","Zu- und Abluftset LFK 160 D","Zu- und Abluftset LFK 160 D","Zu- und Abluftset LFK 160 D","Zu- und Abluftset LFK 160 D","Zu- und Abluftset LFK 160 D","Zu- und Abluftset LFK 160 D"]
[null,223326,"Zu- und Abluftset LFK 200 D","On request","",null,null,null,null,null,null,223326,"Zu- und Abluftset LFK 200 D","On request",false,null,223326,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 200 D","Zu- und Abluftset LFK 200 D","Zu- und Abluftset LFK 200 D","Zu- und Abluftset LFK 200 D","Toevoer- en afvoerset LFK 200 D","Zu- und Abluftset LFK 200 D","Zu- und Abluftset LFK 200 D","Zu- und Abluftset LFK 200 D","Zu- und Abluftset LFK 200 D","Zu- und Abluftset LFK 200 D","Zu- und Abluftset LFK 200 D"]
[null,223456,"Zu- und Abluftset LFK 240 D","On request","",null,null,null,null,null,null,223456,"Zu- und Abluftset LFK 240 D","On request",false,null,223456,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset LFK 240 D","Zu- und Abluftset LFK 240 D","Zu- und Abluftset LFK 240 D","Zu- und Abluftset LFK 240 D","Toevoer- en afvoerset LFK 240 D","Zu- und Abluftset LFK 240 D","Zu- und Abluftset LFK 240 D","Zu- und Abluftset LFK 240 D","Zu- und Abluftset LFK 240 D","Zu- und Abluftset LFK 240 D","Zu- und Abluftset LFK 240 D"]
[null,159271,"Fortluftset F 1","On request","",null,null,null,null,null,null,159271,"Fortluftset F 1","On request",false,null,159271,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Fortluftset F 1","Fortluftset F 1","Fortluftset F 1","Fortluftset F 1","Aanvoerluchtset F 1","Fortluftset F 1","Fortluftset F 1","Fortluftset F 1","Fortluftset F 1","Fortluftset F 1","Fortluftset F 1"]
[null,159272,"Fortluftset F 2","On request","",null,null,null,null,null,null,159272,"Fortluftset F 2","On request",false,null,159272,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Fortluftset F 2","Fortluftset F 2","Fortluftset F 2","Fortluftset F 2","Aanvoerluchtset F 2","Fortluftset F 2","Fortluftset F 2","Fortluftset F 2","Fortluftset F 2","Fortluftset F 2","Fortluftset F 2"]
[null,159273,"Fortluftset F 3","On request","",null,null,null,null,null,null,159273,"Fortluftset F 3","On request",false,null,159273,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Fortluftset F 3","Fortluftset F 3","Fortluftset F 3","Fortluftset F 3","Aanvoerluchtset F 3","Fortluftset F 3","Fortluftset F 3","Fortluftset F 3","Fortluftset F 3","Fortluftset F 3","Fortluftset F 3"]
[null,223327,"Fortluftset F 100","On request","",null,null,null,null,null,null,223327,"Fortluftset F 100","On request",false,null,223327,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Fortluftset F 100","Fortluftset F 100","Fortluftset F 100","Fortluftset F 100","Aanvoerluchtset F 100","Fortluftset F 100","Fortluftset F 100","Fortluftset F 100","Fortluftset F 100","Fortluftset F 100","Fortluftset F 100"]
[null,189813,"External wall valve ALD",102,"",null,null,null,null,null,null,189813,"External wall valve ALD",102,false,null,189813,114,102,120,"på forespørgsel","op aanvraag","Außenwandventil ALD ","External wall valve ALD","Soupape pour mur extérieur ALD ","External wall valve ALD","Buitenmuurventiel ALD ","External wall valve ALD","External wall valve ALD","External wall valve ALD","External wall valve ALD","External wall valve ALD","External wall valve ALD"]
[null,189816,"Installation pipe ALD ",18,"",null,null,null,null,null,null,189816,"Installation pipe ALD ",18,false,null,189816,16.2,18,30,"på forespørgsel","op aanvraag","Montagerohr für ALD","Installation pipe ALD ","Tube de montage pour ALD","Installation pipe ALD ","Montagebuis voor ALD","Installation pipe ALD ","Installation pipe ALD ","Installation pipe ALD ","Installation pipe ALD ","Installation pipe ALD ","Installation pipe ALD "]
[null,189814,"Filter mat set ALD G3",18,"",null,null,null,null,null,null,189814,"Filter mat set ALD G3",18,false,null,189814,25.2,18,"sur demande","på forespørgsel","op aanvraag","Filtermattenset ALD, G3, 5 Sück","Filter mat set ALD G3","Set tapis filtrants ALD, G3","Filter mat set ALD G3","Filtermattenset ALD, G3","Filter mat set ALD G3","Filter mat set ALD G3","Filter mat set ALD G3","Filter mat set ALD G3","Filter mat set ALD G3","Filter mat set ALD G3"]
[null,189815,"Filter mat set ALD G2",17,"",null,null,null,null,null,null,189815,"Filter mat set ALD G2",17,false,null,189815,25.2,17,30,"på forespørgsel","op aanvraag","Filtermattenset ALD, G2, 5 Stück","Filter mat set ALD G2","Set tapis filtrants ALD, G2","Filter mat set ALD G2","Filtermattenset ALD, G2","Filter mat set ALD G2","Filter mat set ALD G2","Filter mat set ALD G2","Filter mat set ALD G2","Filter mat set ALD G2","Filter mat set ALD G2"]
[null,227925,"Filter mat ALD 160","On request","",null,null,null,null,null,null,227925,"Filter mat ALD 160","On request",false,null,227925,25.1,"On request",20,"på forespørgsel","op aanvraag","Filtermattenset ALD, F5, 3 Stück","Filter mat ALD 160","Filtre fin pour ALD 160","Filter mat ALD 160","Fijnfilter voor ALD 160","Filter mat ALD 160","Filter mat ALD 160","Filter mat ALD 160","Filter mat ALD 160","Filter mat ALD 160","Filter mat ALD 160"]
[null,227918,"Supply air valve DN 100, ceiling","On request","",null,null,null,null,null,null,227918,"Supply air valve DN 100, ceiling","On request",false,null,227918,21.2,"On request",20,"på forespørgsel","op aanvraag","Zuluftventil DN 100, Decke","Supply air valve DN 100, ceiling","Bouche d'insufflation DN 100, plafond","Supply air valve DN 100, ceiling","Toevoerventiel DN 100, plafond","Supply air valve DN 100, ceiling","Supply air valve DN 100, ceiling","Supply air valve DN 100, ceiling","Supply air valve DN 100, ceiling","Supply air valve DN 100, ceiling","Supply air valve DN 100, ceiling"]
[null,230163,"Supply air valve DN 125, ceiling","On request","",null,null,null,null,null,null,230163,"Supply air valve DN 125, ceiling","On request",false,null,230163,35,"On request",20,216,"op aanvraag","Zuluftventil DN 125, Decke","Supply air valve DN 125, ceiling","Bouche d'insufflation DN 125, plafond","Supply air valve DN 125, ceiling","Toevoerventiel DN 125, plafond","Supply air valve DN 125, ceiling","Supply air valve DN 125, ceiling","Supply air valve DN 125, ceiling","Supply air valve DN 125, ceiling","Supply air valve DN 125, ceiling","Supply air valve DN 125, ceiling"]
[null,229281,"Supply air valve DN 100, wall","On request","",null,null,null,null,null,null,229281,"Supply air valve DN 100, wall","On request",false,null,229281,77,"On request",80,"på forespørgsel","op aanvraag","Zuluftventil DN 100, Wand","Supply air valve DN 100, wall","Bouche d'insufflation DN 100, mur","Supply air valve DN 100, wall","Toevoerventiel DN 100, wand","Supply air valve DN 100, wall","Supply air valve DN 100, wall","Supply air valve DN 100, wall","Supply air valve DN 100, wall","Supply air valve DN 100, wall","Supply air valve DN 100, wall"]
[null,227917,"Exhaust air valve DN 100, ceiling/wall","On request","",null,null,null,null,null,null,227917,"Exhaust air valve DN 100, ceiling/wall","On request",false,null,227917,21.2,"On request",20,"på forespørgsel","op aanvraag","Abluftventil DN 100, Wand/Decke","Exhaust air valve DN 100, ceiling/wall","Bouche d'extraction d'air DN 100, plafond/mur","Exhaust air valve DN 100, ceiling/wall","Toevoerventiel DN 100, wand/plafond","Exhaust air valve DN 100, ceiling/wall","Exhaust air valve DN 100, ceiling/wall","Exhaust air valve DN 100, ceiling/wall","Exhaust air valve DN 100, ceiling/wall","Exhaust air valve DN 100, ceiling/wall","Exhaust air valve DN 100, ceiling/wall"]
[null,227924,"Exhaust air valve DN 125, ceiling/wall","On request","",null,null,null,null,null,null,227924,"Exhaust air valve DN 125, ceiling/wall","On request",false,null,227924,23.3,"On request",20,"på forespørgsel","op aanvraag","Abluftventil DN 125, Wand/Decke","Exhaust air valve DN 125, ceiling/wall","Bouche d'extraction d'air DN 125, plafond/mur","Exhaust air valve DN 125, ceiling/wall","Toevoerventiel DN 125, wand/plafond","Exhaust air valve DN 125, ceiling/wall","Exhaust air valve DN 125, ceiling/wall","Exhaust air valve DN 125, ceiling/wall","Exhaust air valve DN 125, ceiling/wall","Exhaust air valve DN 125, ceiling/wall","Exhaust air valve DN 125, ceiling/wall"]
[null,230960,"Filter mat set exhaust air valve DN 100","On request","",null,null,null,null,null,null,230960,"Filter mat set exhaust air valve DN 100","On request",false,null,230960,31,"On request",75,"på forespørgsel","op aanvraag","Filterset Abluftventil DN 100, G3, 5 Stück","Filter mat set exhaust air valve DN 100","Jeux de filtres bouche d'extraction d'air DN 100, G3, 5 p.","Filter mat set exhaust air valve DN 100","Filterset afvoerluchtventiel DN 100, G3, 5 stuks","Filter mat set exhaust air valve DN 100","Filter mat set exhaust air valve DN 100","Filter mat set exhaust air valve DN 100","Filter mat set exhaust air valve DN 100","Filter mat set exhaust air valve DN 100","Filter mat set exhaust air valve DN 100"]
[null,230961,"Filter mat set exhaust air valve DN 125","On request","",null,null,null,null,null,null,230961,"Filter mat set exhaust air valve DN 125","On request",false,null,230961,36,"On request",80,"på forespørgsel","op aanvraag","Filterset Abluftventil DN 125, G3, 5 Stück","Filter mat set exhaust air valve DN 125","Jeux de filtres bouche d'extraction d'air DN 125, G3, 5 p.","Filter mat set exhaust air valve DN 125","Filterset afvoerluchtventiel DN 125, G3, 5 stuks","Filter mat set exhaust air valve DN 125","Filter mat set exhaust air valve DN 125","Filter mat set exhaust air valve DN 125","Filter mat set exhaust air valve DN 125","Filter mat set exhaust air valve DN 125","Filter mat set exhaust air valve DN 125"]
[null,227920,"Wall entrances 160 VA","On request","",null,null,null,null,null,null,227920,"Wall entrances 160 VA","On request",false,null,227920,315,"On request",345,"på forespørgsel","op aanvraag","Wanddurchführung DN 160, Edelstahl","Wall entrances 160 VA","Traversée murale 160 VA","Wall entrances 160 VA","Wanddoorvoer","Wall entrances 160 VA","Wall entrances 160 VA","Wall entrances 160 VA","Wall entrances 160 VA","Wall entrances 160 VA","Wall entrances 160 VA"]
[null,71832,"Combi-air grill 125/160","On request","",null,null,null,null,null,null,71832,"Combi-air grill 125/160","On request",false,null,71832,134,"On request","sur demande","på forespørgsel","op aanvraag","Kombiluftgitter Außen-und Fortluft DN 125/160","Combi-air grill 125/160","Grille de ventilation combinée 125/160","Combi-air grill 125/160","Combi luchtrooster 125/160","Combi-air grill 125/160","Combi-air grill 125/160","Combi-air grill 125/160","Combi-air grill 125/160","Combi-air grill 125/160","Combi-air grill 125/160"]
[null,233017,"Fort- / Außenluftgitter DN 125","On request","",null,null,null,null,null,null,233017,"Fort- / Außenluftgitter DN 125","On request",false,null,233017,155,"On request",130,"på forespørgsel","op aanvraag","Fort- / Außenluftgitter DN 125","Fort- / Außenluftgitter DN 125","Fort- / Außenluftgitter DN 125","Fort- / Außenluftgitter DN 125","Aan- / buitenluchtrooster DN 125","Fort- / Außenluftgitter DN 125","Fort- / Außenluftgitter DN 125","Fort- / Außenluftgitter DN 125","Fort- / Außenluftgitter DN 125","Fort- / Außenluftgitter DN 125","Fort- / Außenluftgitter DN 125"]
[null,233018,"Fort- / Außenluftgitter DN 160","On request","",null,null,null,null,null,null,233018,"Fort- / Außenluftgitter DN 160","On request",false,null,233018,162,"On request",130,"på forespørgsel","op aanvraag","Fort- / Außenluftgitter DN 160","Fort- / Außenluftgitter DN 160","Fort- / Außenluftgitter DN 160","Fort- / Außenluftgitter DN 160","Aan- / buitenluchtrooster DN 160","Fort- / Außenluftgitter DN 160","Fort- / Außenluftgitter DN 160","Fort- / Außenluftgitter DN 160","Fort- / Außenluftgitter DN 160","Fort- / Außenluftgitter DN 160","Fort- / Außenluftgitter DN 160"]
[null,170016,"Roof duct DN 160, pitched roof","On request","",null,null,null,null,null,null,170016,"Roof duct DN 160, pitched roof","On request",false,null,170016,158,"On request",75,"på forespørgsel","op aanvraag","Kunststoff-Dachhaube mit Dacheindeckung DN 160","Roof duct DN 160, pitched roof","Traversée de toit 160, toit incliné","Roof duct DN 160, pitched roof","Dakdoorvoer 160 schuindak","Roof duct DN 160, pitched roof","Roof duct DN 160, pitched roof","Roof duct DN 160, pitched roof","Roof duct DN 160, pitched roof","Roof duct DN 160, pitched roof","Roof duct DN 160, pitched roof"]
[null,227923,"Slatted hood DN 160","On request","",null,null,null,null,null,null,227923,"Slatted hood DN 160","On request",false,null,227923,285,"On request","sur demande","på forespørgsel","op aanvraag","Lamellenhaube DN 160","Slatted hood DN 160","Tête pour traversée de toit à lamelles DN 160","Slatted hood DN 160","Lamellenmantel DN 160","Slatted hood DN 160","Slatted hood DN 160","Slatted hood DN 160","Slatted hood DN 160","Slatted hood DN 160","Slatted hood DN 160"]
[null,227922,"Roof duct DN 160 >30-45°","On request","",null,null,null,null,null,null,227922,"Roof duct DN 160 >30-45°","On request",false,null,227922,400,"On request","sur demande","på forespørgsel","op aanvraag","Dacheindeckung DN 160, 30-45°","Roof duct DN 160 >30-45°","Couverture de toit DN 160 >30-45°","Roof duct DN 160 >30-45°","Dakbedekking DN 160 >30-45°","Roof duct DN 160 >30-45°","Roof duct DN 160 >30-45°","Roof duct DN 160 >30-45°","Roof duct DN 160 >30-45°","Roof duct DN 160 >30-45°","Roof duct DN 160 >30-45°"]
[null,227921,"Roof duct DN 160 <30°","On request","",null,null,null,null,null,null,227921,"Roof duct DN 160 <30°","On request",false,null,227921,303,"On request","sur demande","på forespørgsel","op aanvraag","Dacheindeckung DN 160, 10-30°","Roof duct DN 160 <30°","Couverture de toit DN 160 <30°","Roof duct DN 160 <30°","Dakbedekking DN 160 <30°","Roof duct DN 160 <30°","Roof duct DN 160 <30°","Roof duct DN 160 <30°","Roof duct DN 160 <30°","Roof duct DN 160 <30°","Roof duct DN 160 <30°"]
[null,230962,"Stainless steel pipe DN 160, 1m","On request","",null,null,null,null,null,null,230962,"Stainless steel pipe DN 160, 1m","On request",false,null,230962,89,"On request","sur demande","på forespørgsel","op aanvraag","Edelstahlrohr DN 160, 1m","Stainless steel pipe DN 160, 1m","Tube en acier inoxydable DN 160, 1 m","Stainless steel pipe DN 160, 1m","RVS buis DN 160, 1m","Stainless steel pipe DN 160, 1m","Stainless steel pipe DN 160, 1m","Stainless steel pipe DN 160, 1m","Stainless steel pipe DN 160, 1m","Stainless steel pipe DN 160, 1m","Stainless steel pipe DN 160, 1m"]
[null,230963,"Stainless steel bow DN 160, 90°","On request","",null,null,null,null,null,null,230963,"Stainless steel bow DN 160, 90°","On request",false,null,230963,66,"On request","sur demande","på forespørgsel","op aanvraag","Edelstahlrohrbogen DN 160, 90°","Stainless steel bow DN 160, 90°","Coude en acier inoxydable DN 160, 90°","Stainless steel bow DN 160, 90°","RVS bochten DN 160, 90°","Stainless steel bow DN 160, 90°","Stainless steel bow DN 160, 90°","Stainless steel bow DN 160, 90°","Stainless steel bow DN 160, 90°","Stainless steel bow DN 160, 90°","Stainless steel bow DN 160, 90°"]
[null,161094,"Spiral duct DN 100, 2m","On request","",null,null,null,null,null,null,161094,"Spiral duct DN 100, 2m","On request",false,null,161094,16.399999999999999,"On request",15,"på forespørgsel","op aanvraag","Wickelfalzrohr DN 100, 2m","Spiral duct DN 100, 2m","Gaine plissée en spirale DN 100, 2 m","Spiral duct DN 100, 2m","Wikkelfelsbuis DN 100, 2m","Spiral duct DN 100, 2m","Spiral duct DN 100, 2m","Spiral duct DN 100, 2m","Spiral duct DN 100, 2m","Spiral duct DN 100, 2m","Spiral duct DN 100, 2m"]
[null,161095,"Spiral duct DN 125, 2m","On request","",null,null,null,null,null,null,161095,"Spiral duct DN 125, 2m","On request",false,null,161095,20.3,"On request",20,"på forespørgsel","op aanvraag","Wickelfalzrohr DN 125, 2m","Spiral duct DN 125, 2m","Gaine plissée en spirale DN 125, 2 m","Spiral duct DN 125, 2m","Wikkelfelsbuis DN 125, 2m","Spiral duct DN 125, 2m","Spiral duct DN 125, 2m","Spiral duct DN 125, 2m","Spiral duct DN 125, 2m","Spiral duct DN 125, 2m","Spiral duct DN 125, 2m"]
[null,161096,"Spiral duct DN 160, 2m","On request","",null,null,null,null,null,null,161096,"Spiral duct DN 160, 2m","On request",false,null,161096,30.5,"On request",25,"på forespørgsel","op aanvraag","Wickelfalzrohr DN 160, 2m","Spiral duct DN 160, 2m","Gaine plissée en spirale DN 160, 2 m","Spiral duct DN 160, 2m","Wikkelfelsbuis DN 160, 2m","Spiral duct DN 160, 2m","Spiral duct DN 160, 2m","Spiral duct DN 160, 2m","Spiral duct DN 160, 2m","Spiral duct DN 160, 2m","Spiral duct DN 160, 2m"]
[null,159292,"Tee DN 100 / 100","On request","",null,null,null,null,null,null,159292,"Tee DN 100 / 100","On request",false,null,159292,28.5,"On request",15,"på forespørgsel","op aanvraag","T-Stück DN 100 / 100","Tee DN 100 / 100","Raccord en T DN 100 / 100","Tee DN 100 / 100","T-stuk DN 100 / 100","Tee DN 100 / 100","Tee DN 100 / 100","Tee DN 100 / 100","Tee DN 100 / 100","Tee DN 100 / 100","Tee DN 100 / 100"]
[null,159293,"Tee DN 125 / 100","On request","",null,null,null,null,null,null,159293,"Tee DN 125 / 100","On request",false,null,159293,30.5,"On request",20,"på forespørgsel","op aanvraag","T-Stück DN 125 / 100","Tee DN 125 / 100","Raccord en T DN 125 / 100","Tee DN 125 / 100","T-stuk DN 125 / 100","Tee DN 125 / 100","Tee DN 125 / 100","Tee DN 125 / 100","Tee DN 125 / 100","Tee DN 125 / 100","Tee DN 125 / 100"]
[null,159294,"Tee DN 125 / 125","On request","",null,null,null,null,null,null,159294,"Tee DN 125 / 125","On request",false,null,159294,30.5,"On request",25,"på forespørgsel","op aanvraag","T-Stück DN 125 / 125","Tee DN 125 / 125","Raccord en T DN 125 / 125","Tee DN 125 / 125","T-stuk DN 125 / 125","Tee DN 125 / 125","Tee DN 125 / 125","Tee DN 125 / 125","Tee DN 125 / 125","Tee DN 125 / 125","Tee DN 125 / 125"]
[null,159322,"Tee DN 160 / 125","On request","",null,null,null,null,null,null,159322,"Tee DN 160 / 125","On request",false,null,159322,34,"On request",25,"på forespørgsel","op aanvraag","T-Stück DN 160 / 125","Tee DN 160 / 125","Raccord en T DN 160 / 125","Tee DN 160 / 125","T-stuk DN 160 / 125","Tee DN 160 / 125","Tee DN 160 / 125","Tee DN 160 / 125","Tee DN 160 / 125","Tee DN 160 / 125","Tee DN 160 / 125"]
[null,159323,"Tee DN 160 / 160","On request","",null,null,null,null,null,null,159323,"Tee DN 160 / 160","On request",false,null,159323,43,"On request",35,"på forespørgsel","op aanvraag","T-Stück DN 160 / 160","Tee DN 160 / 160","Raccord en T DN 160 / 160","Tee DN 160 / 160","T-stuk DN 160 / 160","Tee DN 160 / 160","Tee DN 160 / 160","Tee DN 160 / 160","Tee DN 160 / 160","Tee DN 160 / 160","Tee DN 160 / 160"]
[null,232984,"T-Stück DN 180 / 180","On request",{"$f":"IF(O588=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,232984,"T-Stück DN 180 / 180","On request",false,null,232984,42.5,"On request",40,"på forespørgsel","op aanvraag","T-Stück DN 180 / 180","T-Stück DN 180 / 180","T-Stück DN 180 / 180","T-Stück DN 180 / 180","T-stuk DN 180 / 180","T-Stück DN 180 / 180","T-Stück DN 180 / 180","T-Stück DN 180 / 180","T-Stück DN 180 / 180","T-Stück DN 180 / 180","T-Stück DN 180 / 180"]
[null,159295,"Restricted fitting DN 125 / 100","On request","",null,null,null,null,null,null,159295,"Restricted fitting DN 125 / 100","On request",false,null,159295,14.8,"On request",10,"på forespørgsel","op aanvraag","Reduzierstück DN 125 / 100","Restricted fitting DN 125 / 100","Raccord de réduction DN 125 / 100","Restricted fitting DN 125 / 100","Reduceerstuk DN 125 / 100","Restricted fitting DN 125 / 100","Restricted fitting DN 125 / 100","Restricted fitting DN 125 / 100","Restricted fitting DN 125 / 100","Restricted fitting DN 125 / 100","Restricted fitting DN 125 / 100"]
[null,159324,"Restricted fitting DN 160 / 125","On request","",null,null,null,null,null,null,159324,"Restricted fitting DN 160 / 125","On request",false,null,159324,14.8,"On request",15,"på forespørgsel","op aanvraag","Reduzierstück DN 160 / 125","Restricted fitting DN 160 / 125","Raccord de réduction DN 160 / 125","Restricted fitting DN 160 / 125","Reduceerstuk DN 160 / 125","Restricted fitting DN 160 / 125","Restricted fitting DN 160 / 125","Restricted fitting DN 160 / 125","Restricted fitting DN 160 / 125","Restricted fitting DN 160 / 125","Restricted fitting DN 160 / 125"]
[null,232711,"Reduzierstück DN 180 / 160","On request","",null,null,null,null,null,null,232711,"Reduzierstück DN 180 / 160","On request",false,null,232711,14.7,"On request",15,83,"op aanvraag","Reduzierstück DN 180 / 160","Reduzierstück DN 180 / 160","Reduzierstück DN 180 / 160","Reduzierstück DN 180 / 160","Reduceerstuk DN 180/DN 160","Reduzierstück DN 180 / 160","Reduzierstück DN 180 / 160","Reduzierstück DN 180 / 160","Reduzierstück DN 180 / 160","Reduzierstück DN 180 / 160","Reduzierstück DN 180 / 160"]
[null,159296,"Nippel DN 100","On request","",null,null,null,null,null,null,159296,"Nippel DN 100","On request",{"$f":"IF(AND(B592=L592,C592=M592,D592=N592),FALSE,TRUE)","v":false},null,159296,9.3000000000000007,"On request",5,"på forespørgsel","op aanvraag","Rohrnippel DN 100","Nippel DN 100","Raccord fileté de tube DN 100","Nippel DN 100","Buisnippel DN 100","Nippel DN 100","Nippel DN 100","Nippel DN 100","Nippel DN 100","Nippel DN 100","Nippel DN 100"]
[null,159297,"Nippel DN 125 ","On request","",null,null,null,null,null,null,159297,"Nippel DN 125 ","On request",false,null,159297,9.3000000000000007,"On request",5,"på forespørgsel","op aanvraag","Rohrnippel DN 125 ","Nippel DN 125 ","Raccord fileté de tube DN 125 ","Nippel DN 125 ","Buisnippel DN 125 ","Nippel DN 125 ","Nippel DN 125 ","Nippel DN 125 ","Nippel DN 125 ","Nippel DN 125 ","Nippel DN 125 "]
[null,159320,"Nippel DN 160","On request","",null,null,null,null,null,null,159320,"Nippel DN 160","On request",false,null,159320,9.3000000000000007,"On request",10,"på forespørgsel","op aanvraag","Rohrnippel DN 160","Nippel DN 160","Raccord fileté de tube DN 160","Nippel DN 160","Buisnippel DN 160","Nippel DN 160","Nippel DN 160","Nippel DN 160","Nippel DN 160","Nippel DN 160","Nippel DN 160"]
[null,232986,"Rohrnippel DN 180","On request","",null,null,null,null,null,null,232986,"Rohrnippel DN 180","On request",false,null,232986,10,"On request",15,"på forespørgsel","op aanvraag","Rohrnippel DN 180","Rohrnippel DN 180","Rohrnippel DN 180","Rohrnippel DN 180","Buisnippel DN 180","Rohrnippel DN 180","Rohrnippel DN 180","Rohrnippel DN 180","Rohrnippel DN 180","Rohrnippel DN 180","Rohrnippel DN 180"]
[null,159298,"Fitting DN 100","On request","",null,null,null,null,null,null,159298,"Fitting DN 100","On request",false,null,159298,5.6,"On request",5,"på forespørgsel","op aanvraag","Rohrmuffe DN 100","Fitting DN 100","Manchon DN 100","Fitting DN 100","Sok DN 100","Fitting DN 100","Fitting DN 100","Fitting DN 100","Fitting DN 100","Fitting DN 100","Fitting DN 100"]
[null,159299,"Fitting DN 125 ","On request","",null,null,null,null,null,null,159299,"Fitting DN 125 ","On request",false,null,159299,5.6,"On request",5,"på forespørgsel","op aanvraag","Rohrmuffe DN 125 ","Fitting DN 125 ","Manchon DN 125 ","Fitting DN 125 ","Sok DN 125 ","Fitting DN 125 ","Fitting DN 125 ","Fitting DN 125 ","Fitting DN 125 ","Fitting DN 125 ","Fitting DN 125 "]
[null,159326,"Fitting DN 160","On request","",null,null,null,null,null,null,159326,"Fitting DN 160","On request",false,null,159326,5.6,"On request",10,"på forespørgsel","op aanvraag","Rohrmuffe DN 160","Fitting DN 160","Manchon DN 160","Fitting DN 160","Sok DN 160","Fitting DN 160","Fitting DN 160","Fitting DN 160","Fitting DN 160","Fitting DN 160","Fitting DN 160"]
[null,232985,"Rohrmuffe DN 180","On request","",null,null,null,null,null,null,232985,"Rohrmuffe DN 180","On request",false,null,232985,6.7,"On request",10,"på forespørgsel","op aanvraag","Rohrmuffe DN 180","Rohrmuffe DN 180","Rohrmuffe DN 180","Rohrmuffe DN 180","Buissok DN 180","Rohrmuffe DN 180","Rohrmuffe DN 180","Rohrmuffe DN 180","Rohrmuffe DN 180","Rohrmuffe DN 180","Rohrmuffe DN 180"]
[null,159301,"Bow 30° DN 100","On request","",null,null,null,null,null,null,159301,"Bow 30° DN 100","On request",false,null,159301,12.8,"On request",15,"på forespørgsel","op aanvraag","Bogen 30° DN 100","Bow 30° DN 100","Coude 30° DN 100","Bow 30° DN 100","Bocht 30° DN 100","Bow 30° DN 100","Bow 30° DN 100","Bow 30° DN 100","Bow 30° DN 100","Bow 30° DN 100","Bow 30° DN 100"]
[null,159302,"Bow 45° DN 100","On request","",null,null,null,null,null,null,159302,"Bow 45° DN 100","On request",false,null,159302,14.8,"On request",15,"på forespørgsel","op aanvraag","Bogen 45° DN 100","Bow 45° DN 100","Coude 45° DN 100","Bow 45° DN 100","Bocht 45° DN 100","Bow 45° DN 100","Bow 45° DN 100","Bow 45° DN 100","Bow 45° DN 100","Bow 45° DN 100","Bow 45° DN 100"]
[null,159303,"Bow 60° DN 100","On request","",null,null,null,null,null,null,159303,"Bow 60° DN 100","On request",false,null,159303,22.2,"On request",15,"på forespørgsel","op aanvraag","Bogen 60° DN 100","Bow 60° DN 100","Coude 60° DN 100","Bow 60° DN 100","Bocht 60° DN 100","Bow 60° DN 100","Bow 60° DN 100","Bow 60° DN 100","Bow 60° DN 100","Bow 60° DN 100","Bow 60° DN 100"]
[null,159304,"Bow 90° DN 100","On request","",null,null,null,null,null,null,159304,"Bow 90° DN 100","On request",false,null,159304,16.399999999999999,"On request",15,"på forespørgsel","op aanvraag","Bogen 90° DN 100","Bow 90° DN 100","Coude 90° DN 100","Bow 90° DN 100","Bocht 90° DN 100","Bow 90° DN 100","Bow 90° DN 100","Bow 90° DN 100","Bow 90° DN 100","Bow 90° DN 100","Bow 90° DN 100"]
[null,159306,"Bow 30° DN 125","On request","",null,null,null,null,null,null,159306,"Bow 30° DN 125","On request",false,null,159306,14.8,"On request",15,"på forespørgsel","op aanvraag","Bogen 30° DN 125","Bow 30° DN 125","Coude 30° DN 125","Bow 30° DN 125","Bocht 30° DN 125","Bow 30° DN 125","Bow 30° DN 125","Bow 30° DN 125","Bow 30° DN 125","Bow 30° DN 125","Bow 30° DN 125"]
[null,159307,"Bow 45° DN 125","On request","",null,null,null,null,null,null,159307,"Bow 45° DN 125","On request",false,null,159307,16.399999999999999,"On request",15,"på forespørgsel","op aanvraag","Bogen 45° DN 125","Bow 45° DN 125","Coude 45° DN 125","Bow 45° DN 125","Bocht 45° DN 125","Bow 45° DN 125","Bow 45° DN 125","Bow 45° DN 125","Bow 45° DN 125","Bow 45° DN 125","Bow 45° DN 125"]
[null,159309,"Bow 90° DN 125","On request","",null,null,null,null,null,null,159309,"Bow 90° DN 125","On request",false,null,159309,22.2,"On request",15,"på forespørgsel","op aanvraag","Bogen 90° DN 125","Bow 90° DN 125","Coude 90° DN 125","Bow 90° DN 125","Bocht 90° DN 125","Bow 90° DN 125","Bow 90° DN 125","Bow 90° DN 125","Bow 90° DN 125","Bow 90° DN 125","Bow 90° DN 125"]
[null,167146,"Bow 30° DN 160","On request","",null,null,null,null,null,null,167146,"Bow 30° DN 160","On request",false,null,167146,26.5,"On request",20,"på forespørgsel","op aanvraag","Bogen 30° DN 160","Bow 30° DN 160","Coude 30° DN 160","Bow 30° DN 160","Bocht 30° DN 160","Bow 30° DN 160","Bow 30° DN 160","Bow 30° DN 160","Bow 30° DN 160","Bow 30° DN 160","Bow 30° DN 160"]
[null,159328,"Bow 45° DN 160","On request","",null,null,null,null,null,null,159328,"Bow 45° DN 160","On request",false,null,159328,22.2,"On request",20,"på forespørgsel","op aanvraag","Bogen 45° DN 160","Bow 45° DN 160","Coude 45° DN 160","Bow 45° DN 160","Bocht 45° DN 160","Bow 45° DN 160","Bow 45° DN 160","Bow 45° DN 160","Bow 45° DN 160","Bow 45° DN 160","Bow 45° DN 160"]
[null,159329,"Bow 90° DN 160","On request","",null,null,null,null,null,null,159329,"Bow 90° DN 160","On request",false,null,159329,22.2,"On request",25,"på forespørgsel","op aanvraag","Bogen 90° DN 160","Bow 90° DN 160","Coude 90° DN 160","Bow 90° DN 160","Bocht 90° DN 160","Bow 90° DN 160","Bow 90° DN 160","Bow 90° DN 160","Bow 90° DN 160","Bow 90° DN 160","Bow 90° DN 160"]
[null,159310,"End duct DN 100, Fitting","On request","",null,null,null,null,null,null,159310,"End duct DN 100, Fitting","On request",false,null,159310,7.4,"On request",15,"på forespørgsel","op aanvraag","Enddeckel DN 100, Muffe","End duct DN 100, Fitting","Couvercle en extrémité DN 100, manchon","End duct DN 100, Fitting","Einddeksel DN 100, Sok","End duct DN 100, Fitting","End duct DN 100, Fitting","End duct DN 100, Fitting","End duct DN 100, Fitting","End duct DN 100, Fitting","End duct DN 100, Fitting"]
[null,159311,"End duct DN 125, Fitting","On request","",null,null,null,null,null,null,159311,"End duct DN 125, Fitting","On request",false,null,159311,7.4,"On request",15,"på forespørgsel","op aanvraag","Enddeckel DN 125, Muffe","End duct DN 125, Fitting","Couvercle en extrémité DN 125, manchon","End duct DN 125, Fitting","Einddeksel DN 125, Sok","End duct DN 125, Fitting","End duct DN 125, Fitting","End duct DN 125, Fitting","End duct DN 125, Fitting","End duct DN 125, Fitting","End duct DN 125, Fitting"]
[null,167147,"End duct DN 160, Fitting","On request","",null,null,null,null,null,null,167147,"End duct DN 160, Fitting","On request",false,null,167147,11,"On request",15,"på forespørgsel","op aanvraag","Enddeckel DN 160, Muffe","End duct DN 160, Fitting","Couvercle en extrémité DN 160, manchon","End duct DN 160, Fitting","Einddeksel DN 160, Sok","End duct DN 160, Fitting","End duct DN 160, Fitting","End duct DN 160, Fitting","End duct DN 160, Fitting","End duct DN 160, Fitting","End duct DN 160, Fitting"]
[null,232112,"End duct DN 100, Nippel","On request","",null,null,null,null,null,null,232112,"End duct DN 100, Nippel","On request",false,null,232112,11.4,"On request",15,"på forespørgsel","op aanvraag","Enddeckel DN 100, Nippel","End duct DN 100, Nippel","Couvercle en extrémité DN 100, mamelon","End duct DN 100, Nippel","Einddeksel DN 100, Nippel","End duct DN 100, Nippel","End duct DN 100, Nippel","End duct DN 100, Nippel","End duct DN 100, Nippel","End duct DN 100, Nippel","End duct DN 100, Nippel"]
[null,232113,"End duct DN 125, Nippel","On request","",null,null,null,null,null,null,232113,"End duct DN 125, Nippel","On request",false,null,232113,11.4,"On request",15,"på forespørgsel","op aanvraag","Enddeckel DN 125, Nippel","End duct DN 125, Nippel","Couvercle en extrémité DN 125, mamelon","End duct DN 125, Nippel","Einddeksel DN 125, Nippel","End duct DN 125, Nippel","End duct DN 125, Nippel","End duct DN 125, Nippel","End duct DN 125, Nippel","End duct DN 125, Nippel","End duct DN 125, Nippel"]
[null,232114,"End duct DN 160, Nippel","On request","",null,null,null,null,null,null,232114,"End duct DN 160, Nippel","On request",false,null,232114,15.2,"On request",20,"på forespørgsel","op aanvraag","Enddeckel DN 160, Nippel","End duct DN 160, Nippel","Couvercle en extrémité DN 160, mamelon","End duct DN 160, Nippel","Einddeksel DN 160, Nippel","End duct DN 160, Nippel","End duct DN 160, Nippel","End duct DN 160, Nippel","End duct DN 160, Nippel","End duct DN 160, Nippel","End duct DN 160, Nippel"]
[null,159312,"End duct with cap DN 100","On request","",null,null,null,null,null,null,159312,"End duct with cap DN 100","On request",false,null,159312,39.5,"On request",20,"på forespørgsel","op aanvraag","Reinigungsdeckel DN 100","End duct with cap DN 100","Couvercle de ramonage DN 100","End duct with cap DN 100","Inspectiedeksel DN 100","End duct with cap DN 100","End duct with cap DN 100","End duct with cap DN 100","End duct with cap DN 100","End duct with cap DN 100","End duct with cap DN 100"]
[null,159313,"End duct with cap DN 125","On request","",null,null,null,null,null,null,159313,"End duct with cap DN 125","On request",false,null,159313,39.5,"On request",35,"på forespørgsel","op aanvraag","Reinigungsdeckel DN 125","End duct with cap DN 125","Couvercle de ramonage DN 125","End duct with cap DN 125","Inspectiedeksel DN 125","End duct with cap DN 125","End duct with cap DN 125","End duct with cap DN 125","End duct with cap DN 125","End duct with cap DN 125","End duct with cap DN 125"]
[null,232115,"End duct with cap DN 160","On request","",null,null,null,null,null,null,232115,"End duct with cap DN 160","On request",false,null,232115,39.5,"On request",20,"på forespørgsel","op aanvraag","Reinigungsdeckel DN 160","End duct with cap DN 160","Couvercle de ramonage DN 160","End duct with cap DN 160","Inspectiedeksel DN 160","End duct with cap DN 160","End duct with cap DN 160","End duct with cap DN 160","End duct with cap DN 160","End duct with cap DN 160","End duct with cap DN 160"]
[null,159333,"Flexible pipe DN 100","On request","",null,null,null,null,null,null,159333,"Flexible pipe DN 100","On request",false,null,159333,48,"On request",35,"på forespørgsel","op aanvraag","Flexrohr DN 100, ausziehbar auf 5m","Flexible pipe DN 100","Tube flexible DN 100, extensible sur 5 m","Flexible pipe DN 100","Flexibele buis DN 100, uittrekbaar tot 5m","Flexible pipe DN 100","Flexible pipe DN 100","Flexible pipe DN 100","Flexible pipe DN 100","Flexible pipe DN 100","Flexible pipe DN 100"]
[null,159334,"Flexible pipe DN 125","On request","",null,null,null,null,null,null,159334,"Flexible pipe DN 125","On request",false,null,159334,61,"On request",35,"på forespørgsel","op aanvraag","Flexrohr DN 125, ausziehbar auf 5m","Flexible pipe DN 125","Tube flexible DN 125, extensible sur 5 m","Flexible pipe DN 125","Flexibele buis DN 125, uittrekbaar tot 5m","Flexible pipe DN 125","Flexible pipe DN 125","Flexible pipe DN 125","Flexible pipe DN 125","Flexible pipe DN 125","Flexible pipe DN 125"]
[null,159332,"Flexible pipe DN 160","On request","",null,null,null,null,null,null,159332,"Flexible pipe DN 160","On request",false,null,159332,107,"On request",40,"på forespørgsel","op aanvraag","Flexrohr DN 160, ausziehbar auf 5m","Flexible pipe DN 160","Tube flexible DN 160, extensible sur 5 m","Flexible pipe DN 160","Flexibele buis DN 160, uittrekbaar tot 5m","Flexible pipe DN 160","Flexible pipe DN 160","Flexible pipe DN 160","Flexible pipe DN 160","Flexible pipe DN 160","Flexible pipe DN 160"]
[null,232982,"Flexrohr DN 180, ausziehbar auf 5m","On request","",null,null,null,null,null,null,232982,"Flexrohr DN 180, ausziehbar auf 5m","On request",false,null,232982,104,"On request",40,"på forespørgsel","op aanvraag","Flexrohr DN 180, ausziehbar auf 5m","Flexrohr DN 180, ausziehbar auf 5m","Flexrohr DN 180, ausziehbar auf 5m","Flexrohr DN 180, ausziehbar auf 5m","Flexibele buis DN 180, uittrekbaar tot 5m","Flexrohr DN 180, ausziehbar auf 5m","Flexrohr DN 180, ausziehbar auf 5m","Flexrohr DN 180, ausziehbar auf 5m","Flexrohr DN 180, ausziehbar auf 5m","Flexrohr DN 180, ausziehbar auf 5m","Flexrohr DN 180, ausziehbar auf 5m"]
[null,159338,"Silencer DN 100  0,6m","On request","",null,null,null,null,null,null,159338,"Silencer DN 100  0,6m","On request",false,null,159338,114,"On request",85,"på forespørgsel","op aanvraag","Schalldämpfer DN 100, 0,6m","Silencer DN 100  0,6m","Amortisseur de bruit DN 100  0,6 m","Silencer DN 100  0,6m","Geluidsdemper DN 100  0,6m","Silencer DN 100  0,6m","Silencer DN 100  0,6m","Silencer DN 100  0,6m","Silencer DN 100  0,6m","Silencer DN 100  0,6m","Silencer DN 100  0,6m"]
[null,159341,"Silencer DN 125  0,6m","On request","",null,null,null,null,null,null,159341,"Silencer DN 125  0,6m","On request",false,null,159341,141,"On request",90,"på forespørgsel","op aanvraag","Schalldämpfer DN 125, 0,6m","Silencer DN 125  0,6m","Amortisseur de bruit DN 125  0,6 m","Silencer DN 125  0,6m","Geluidsdemper DN 125  0,6m","Silencer DN 125  0,6m","Silencer DN 125  0,6m","Silencer DN 125  0,6m","Silencer DN 125  0,6m","Silencer DN 125  0,6m","Silencer DN 125  0,6m"]
[null,159342,"Silencer DN 125  0,9m","On request","",null,null,null,null,null,null,159342,"Silencer DN 125  0,9m","On request",false,null,159342,167,"On request",95,"på forespørgsel","op aanvraag","Schalldämpfer DN 125, 0,9m","Silencer DN 125  0,9m","Amortisseur de bruit DN 125  0,9 m","Silencer DN 125  0,9m","Geluidsdemper DN 125  0,9m","Silencer DN 125  0,9m","Silencer DN 125  0,9m","Silencer DN 125  0,9m","Silencer DN 125  0,9m","Silencer DN 125  0,9m","Silencer DN 125  0,9m"]
[null,159339,"Silencer DN 160  0,6m","On request","",null,null,null,null,null,null,159339,"Silencer DN 160  0,6m","On request",false,null,159339,167,"On request",100,"på forespørgsel","op aanvraag","Schalldämpfer DN 160, 0,6m","Silencer DN 160  0,6m","Amortisseur de bruit DN 160  0,6 m","Silencer DN 160  0,6m","Geluidsdemper DN 160  0,6m","Silencer DN 160  0,6m","Silencer DN 160  0,6m","Silencer DN 160  0,6m","Silencer DN 160  0,6m","Silencer DN 160  0,6m","Silencer DN 160  0,6m"]
[null,159346,"Silencer DN 160  0,9m","On request","",null,null,null,null,null,null,159346,"Silencer DN 160  0,9m","On request",false,null,159346,188,"On request",105,"på forespørgsel","op aanvraag","Schalldämpfer DN 160, 0,9m","Silencer DN 160  0,9m","Amortisseur de bruit DN 160  0,9 m","Silencer DN 160  0,9m","Geluidsdemper DN 160  0,9m","Silencer DN 160  0,9m","Silencer DN 160  0,9m","Silencer DN 160  0,9m","Silencer DN 160  0,9m","Silencer DN 160  0,9m","Silencer DN 160  0,9m"]
[null,232983,"Schalldämpfer DN 180, 0,9m","On request","",null,null,null,null,null,null,232983,"Schalldämpfer DN 180, 0,9m","On request",false,null,232983,182,"On request",120,"på forespørgsel","op aanvraag","Schalldämpfer DN 180, 0,9m","Schalldämpfer DN 180, 0,9m","Schalldämpfer DN 180, 0,9m","Schalldämpfer DN 180, 0,9m","Geluidsdemper DN 180, 0,9m","Schalldämpfer DN 180, 0,9m","Schalldämpfer DN 180, 0,9m","Schalldämpfer DN 180, 0,9m","Schalldämpfer DN 180, 0,9m","Schalldämpfer DN 180, 0,9m","Schalldämpfer DN 180, 0,9m"]
[null,167148,"Silencer DN 100","On request","",null,null,null,null,null,null,167148,"Silencer DN 100","On request",false,null,167148,81,"On request",50,"på forespørgsel","op aanvraag","Telefonie-Schalldämpfer DN 100","Silencer DN 100","Piège à sons DN 100","Silencer DN 100","Geluidsdemper flexibel DN 100","Silencer DN 100","Silencer DN 100","Silencer DN 100","Silencer DN 100","Silencer DN 100","Silencer DN 100"]
[null,159343,"Silencer DN 125","On request","",null,null,null,null,null,null,159343,"Silencer DN 125","On request",false,null,159343,83,"On request",55,"på forespørgsel","op aanvraag","Telefonie-Schalldämpfer DN 125","Silencer DN 125","Piège à sons DN 125","Silencer DN 125","Geluidsdemper flexibel DN 125","Silencer DN 125","Silencer DN 125","Silencer DN 125","Silencer DN 125","Silencer DN 125","Silencer DN 125"]
[null,185666,"Silencer for pipe DN 100","On request","",null,null,null,null,null,null,185666,"Silencer for pipe DN 100","On request",false,null,185666,30,"On request","sur demande","på forespørgsel","op aanvraag","Schalldämpfelement DN 100, 4 Stück","Silencer for pipe DN 100","Élément d'isolation acoustique DN 100, 4 p.","Silencer for pipe DN 100","Geluidsdemperelement DN 100, 4 stuks","Silencer for pipe DN 100","Silencer for pipe DN 100","Silencer for pipe DN 100","Silencer for pipe DN 100","Silencer for pipe DN 100","Silencer for pipe DN 100"]
[null,233012,"Schalldämpfer rechteckig DN 160, 0,5m","On request","",null,null,null,null,null,null,233012,"Schalldämpfer rechteckig DN 160, 0,5m","On request",false,null,233012,149,"On request",180,"på forespørgsel","op aanvraag","Schalldämpfer rechteckig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m","Geluidsdemper rechthoekig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m","Schalldämpfer rechteckig DN 160, 0,5m"]
[null,233013,"Schalldämpfer rechteckig DN 160, 1m","On request","",null,null,null,null,null,null,233013,"Schalldämpfer rechteckig DN 160, 1m","On request",false,null,233013,247,"On request",315,"på forespørgsel","op aanvraag","Schalldämpfer rechteckig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m","Geluidsdemper rechthoekig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m","Schalldämpfer rechteckig DN 160, 1m"]
[null,233014,"Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","On request","",null,null,null,null,null,null,233014,"Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","On request",false,null,233014,449,"On request",525,"på forespørgsel","op aanvraag","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Geluidsdemper rechthoekig DN 160, 1m, 90°-aansluiting","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss","Schalldämpfer rechteckig DN 160, 1m, 90°-Anschluss"]
[null,231111,"LVE flexible pipe, 20m","On request","",null,null,null,null,null,null,231111,"LVE flexible pipe, 20m","On request",false,null,231111,253,"On request",230,"på forespørgsel","op aanvraag","LVE Flexibler Kunststoffkanal, 20m","LVE flexible pipe, 20m","LVE goulotte plastique souple, 20 m","LVE flexible pipe, 20m","LVE Flexibel Kunststofkanaal, 20m","LVE flexible pipe, 20m","LVE flexible pipe, 20m","LVE flexible pipe, 20m","LVE flexible pipe, 20m","LVE flexible pipe, 20m","LVE flexible pipe, 20m"]
[null,231126,"LVE central air distributor","On request","",null,null,null,null,null,null,231126,"LVE central air distributor","On request",false,null,231126,208,"On request",125,"på forespørgsel","op aanvraag","LVE Zentraler Luftverteiler","LVE central air distributor","LVE distributeur d'air centralisé","LVE central air distributor","LVE Centrale luchtverdeler","LVE central air distributor","LVE central air distributor","LVE central air distributor","LVE central air distributor","LVE central air distributor","LVE central air distributor"]
[null,231457,"LVE cover for central air distributor","On request","",null,null,null,null,null,null,231457,"LVE cover for central air distributor","On request",false,null,231457,66,"On request",65,"på forespørgsel","op aanvraag","LVE Verteilerabdeckung für Fußbodeneinbau","LVE cover for central air distributor","LVE cache de distributeur d'air pour montage dans le sol","LVE cover for central air distributor","LVE Vedelerafdekking voor vloerinbouw","LVE cover for central air distributor","LVE cover for central air distributor","LVE cover for central air distributor","LVE cover for central air distributor","LVE cover for central air distributor","LVE cover for central air distributor"]
[null,231119,"LVE extension air distributor connection","On request","",null,null,null,null,null,null,231119,"LVE extension air distributor connection","On request",false,null,231119,24.1,"On request",25,"på forespørgsel","op aanvraag","LVE Verlängerung Verteileranschluss, 0,1 m","LVE extension air distributor connection","LVE rallonge de raccordement de distributeur d'air, 4 p.","LVE extension air distributor connection","LVE Verlenging verdeleraansluiting, 4 stuks","LVE extension air distributor connection","LVE extension air distributor connection","LVE extension air distributor connection","LVE extension air distributor connection","LVE extension air distributor connection","LVE extension air distributor connection"]
[null,233030,"LVE Verlängerung Verteileranschluss, 0,5 m","On request","",null,null,null,null,null,null,233030,"LVE Verlängerung Verteileranschluss, 0,5 m","On request",false,null,233030,15.8,"On request",65,"på forespørgsel","op aanvraag","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlenging verdeleraansluiting, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m","LVE Verlängerung Verteileranschluss, 0,5 m"]
[null,233031,"LVE Verlängerung Verteileranschluss Bogen 45°","On request","",null,null,null,null,null,null,233031,"LVE Verlängerung Verteileranschluss Bogen 45°","On request",false,null,233031,15.8,"On request",55,"på forespørgsel","op aanvraag","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlenging verdeleraansluiting bocht 45°","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlängerung Verteileranschluss Bogen 45°","LVE Verlängerung Verteileranschluss Bogen 45°"]
[null,231125,"LVE air outlet floor","On request","",null,null,null,null,null,null,231125,"LVE air outlet floor","On request",false,null,231125,44,"On request","sur demande","på forespørgsel","op aanvraag","LVE Fußbodenauslass","LVE air outlet floor","LVE bouche d'aération au sol","LVE air outlet floor","LVE Vloerverwarmings uitstroom","LVE air outlet floor","LVE air outlet floor","LVE air outlet floor","LVE air outlet floor","LVE air outlet floor","LVE air outlet floor"]
[null,231124,"LVE air outlet wall/ceiling","On request","",null,null,null,null,null,null,231124,"LVE air outlet wall/ceiling","On request",false,null,231124,33,"On request",45,"på forespørgsel","op aanvraag","LVE Wand-/Deckenauslass","LVE air outlet wall/ceiling","LVE bouche d'aération murale et au plafond","LVE air outlet wall/ceiling","LVE Wand-/Plafond uitstroom","LVE air outlet wall/ceiling","LVE air outlet wall/ceiling","LVE air outlet wall/ceiling","LVE air outlet wall/ceiling","LVE air outlet wall/ceiling","LVE air outlet wall/ceiling"]
[null,233029,"LVE Verlängerung Wand-/Deckenauslass","On request","",null,null,null,null,null,null,233029,"LVE Verlängerung Wand-/Deckenauslass","On request",false,null,233029,13.3,"On request",20,"på forespørgsel","op aanvraag","LVE Verlängerung Wand-/Deckenauslass","LVE Verlängerung Wand-/Deckenauslass","LVE Verlängerung Wand-/Deckenauslass","LVE Verlängerung Wand-/Deckenauslass","LVE Verlenging Wand-/Plafonf uitstroom","LVE Verlängerung Wand-/Deckenauslass","LVE Verlängerung Wand-/Deckenauslass","LVE Verlängerung Wand-/Deckenauslass","LVE Verlängerung Wand-/Deckenauslass","LVE Verlängerung Wand-/Deckenauslass","LVE Verlängerung Wand-/Deckenauslass"]
[null,231123,"LVE Bow 90° high","On request","",null,null,null,null,null,null,231123,"LVE Bow 90° high","On request",false,null,231123,16.3,"On request",25,"på forespørgsel","op aanvraag","LVE Bogen 90° hoch","LVE Bow 90° high","LVE coude 90° haut","LVE Bow 90° high","LVE Bocht 90° hoog","LVE Bow 90° high","LVE Bow 90° high","LVE Bow 90° high","LVE Bow 90° high","LVE Bow 90° high","LVE Bow 90° high"]
[null,231122,"LVE Bow 90° flat","On request","",null,null,null,null,null,null,231122,"LVE Bow 90° flat","On request",false,null,231122,16.3,"On request",25,"på forespørgsel","op aanvraag","LVE Bogen 90° flach","LVE Bow 90° flat","LVE coude 90° plat","LVE Bow 90° flat","LVE Bocht 90° plat","LVE Bow 90° flat","LVE Bow 90° flat","LVE Bow 90° flat","LVE Bow 90° flat","LVE Bow 90° flat","LVE Bow 90° flat"]
[null,231121,"LVE Bow 45° flat","On request","",null,null,null,null,null,null,231121,"LVE Bow 45° flat","On request",false,null,231121,16.3,"On request",20,"på forespørgsel","op aanvraag","LVE Bogen 45° flach","LVE Bow 45° flat","LVE coude 45° plat","LVE Bow 45° flat","LVE Bocht 45° plat","LVE Bow 45° flat","LVE Bow 45° flat","LVE Bow 45° flat","LVE Bow 45° flat","LVE Bow 45° flat","LVE Bow 45° flat"]
[null,231120,"LVE Adapter piece redirecting 180°","On request","",null,null,null,null,null,null,231120,"LVE Adapter piece redirecting 180°","On request",false,null,231120,16.3,"On request",20,"på forespørgsel","op aanvraag","LVE Übergangsstück Lagewechsel Kanal","LVE Adapter piece redirecting 180°","LVE raccord transition changement de direction 180°","LVE Adapter piece redirecting 180°","LVE Overgangsstuk Richtingswissel 180°","LVE Adapter piece redirecting 180°","LVE Adapter piece redirecting 180°","LVE Adapter piece redirecting 180°","LVE Adapter piece redirecting 180°","LVE Adapter piece redirecting 180°","LVE Adapter piece redirecting 180°"]
[null,231117,"LVE fitting for pipes","On request","",null,null,null,null,null,null,231117,"LVE fitting for pipes","On request",false,null,231117,21.9,"On request",20,"på forespørgsel","op aanvraag","LVE Adapter Anschluss Kanal, 5 Stück","LVE fitting for pipes","LVE adaptateur fixation de tube, 5 p.","LVE fitting for pipes","LVE Adaptor buisbevestiging, 5 stuks","LVE fitting for pipes","LVE fitting for pipes","LVE fitting for pipes","LVE fitting for pipes","LVE fitting for pipes","LVE fitting for pipes"]
[null,231116,"LVE End duct","On request","",null,null,null,null,null,null,231116,"LVE End duct","On request",false,null,231116,21.9,"On request",15,"på forespørgsel","op aanvraag","LVE Enddeckel, 5 Stück","LVE End duct","LVE couvercle en extrémité, 5 p.","LVE End duct","LVE Einddeksel, 5 stuks","LVE End duct","LVE End duct","LVE End duct","LVE End duct","LVE End duct","LVE End duct"]
[null,231787,"LVE fitting für bows","On request","",null,null,null,null,null,null,231787,"LVE fitting für bows","On request",false,null,231787,28,"On request",35,"på forespørgsel","op aanvraag","LVE Adapter Anschluss Formteil, 5 Stück","LVE fitting für bows","LVE pièce de raccordement de pièces moulées, 5 p.","LVE fitting für bows","LVE Verbindingsstuk voor vormdelen, 5 stuks","LVE fitting für bows","LVE fitting für bows","LVE fitting für bows","LVE fitting für bows","LVE fitting für bows","LVE fitting für bows"]
[null,231113,"LVE pipe clamp","On request","",null,null,null,null,null,null,231113,"LVE pipe clamp","On request",false,null,231113,16.3,"On request",20,"på forespørgsel","op aanvraag","LVE Befestigungsklammer Kanal, 10 Stück","LVE pipe clamp","LVE clip de fixation de goulotte, 10 p.","LVE pipe clamp","LVE Bevestigingsklemmen kanaal, 10 stuks","LVE pipe clamp","LVE pipe clamp","LVE pipe clamp","LVE pipe clamp","LVE pipe clamp","LVE pipe clamp"]
[null,231112,"LVE fitting for pipe-extension","On request",{"$f":"IF(O652=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,231112,"LVE fitting for pipe-extension","On request",false,null,231112,24.1,"On request",25,"på forespørgsel","op aanvraag","LVE Adapter Rohrverlängerung, 5 Stück","LVE fitting for pipe-extension","LVE adaptateur rallonge de tube, 5 p.","LVE fitting for pipe-extension","LVE Adaptor buisverlenging, 5 stuks","LVE fitting for pipe-extension","LVE fitting for pipe-extension","LVE fitting for pipe-extension","LVE fitting for pipe-extension","LVE fitting for pipe-extension","LVE fitting for pipe-extension"]
[null,233032,"LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","On request","",null,null,null,null,null,null,233032,"LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","On request",false,null,233032,29.5,"On request",30,"på forespørgsel","op aanvraag","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Overgangsstuk naar LVS-Kunststofbuis DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75","LVE Übergangsstück auf LVS-Kunststoffrohr DN 75"]
[null,231969,"LVE air grill floor - stainless steel 1","On request","",null,null,null,null,null,null,231969,"LVE air grill floor - stainless steel 1","On request",false,null,231969,88,"On request","sur demande","på forespørgsel","op aanvraag","LVE Gitter Boden, Design Welle, Edelstahl","LVE air grill floor - stainless steel 1","LVE grille de sol, design onde, acier inoxydable","LVE air grill floor - stainless steel 1","LVE Vloerrooster, Golf design, RVS","LVE air grill floor - stainless steel 1","LVE air grill floor - stainless steel 1","LVE air grill floor - stainless steel 1","LVE air grill floor - stainless steel 1","LVE air grill floor - stainless steel 1","LVE air grill floor - stainless steel 1"]
[null,231970,"LVE air grill floor - stainless steel 2","On request","",null,null,null,null,null,null,231970,"LVE air grill floor - stainless steel 2","On request",false,null,231970,88,"On request","sur demande","på forespørgsel","op aanvraag","LVE Gitter Boden, Design Natur, Edelstahl","LVE air grill floor - stainless steel 2","LVE grille de sol, design nature, acier inoxydable","LVE air grill floor - stainless steel 2","LVE Vloerrooster, Natuur design, RVS","LVE air grill floor - stainless steel 2","LVE air grill floor - stainless steel 2","LVE air grill floor - stainless steel 2","LVE air grill floor - stainless steel 2","LVE air grill floor - stainless steel 2","LVE air grill floor - stainless steel 2"]
[null,231971,"LVE air grill floor - stainless steel 3","On request","",null,null,null,null,null,null,231971,"LVE air grill floor - stainless steel 3","On request",{"$f":"IF(AND(B656=L656,C656=M656,D656=N656),FALSE,TRUE)","v":false},null,231971,66,"On request","sur demande","på forespørgsel","op aanvraag","LVE Gitter Boden, Design Kreis, Edelstahl","LVE air grill floor - stainless steel 3","LVE grille de sol, design cercle, acier inoxydable","LVE air grill floor - stainless steel 3","LVE Vloerrooster, Kruis design, RVS","LVE air grill floor - stainless steel 3","LVE air grill floor - stainless steel 3","LVE air grill floor - stainless steel 3","LVE air grill floor - stainless steel 3","LVE air grill floor - stainless steel 3","LVE air grill floor - stainless steel 3"]
[null,231115,"LVE air grill floor - stainless steel 4","On request","",null,null,null,null,null,null,231115,"LVE air grill floor - stainless steel 4","On request",false,null,231115,66,"On request","sur demande","på forespørgsel","op aanvraag","LVE Gitter Boden, Design Langloch, Edelstahl","LVE air grill floor - stainless steel 4","LVE grille de sol, design trou oblong, acier inoxydable","LVE air grill floor - stainless steel 4","LVE Vloerrooster, Rechthoek design, RVS","LVE air grill floor - stainless steel 4","LVE air grill floor - stainless steel 4","LVE air grill floor - stainless steel 4","LVE air grill floor - stainless steel 4","LVE air grill floor - stainless steel 4","LVE air grill floor - stainless steel 4"]
[null,231972,"LVE air grill floor - stainless steel 5","On request","",null,null,null,null,null,null,231972,"LVE air grill floor - stainless steel 5","On request",false,null,231972,53,"On request","sur demande","på forespørgsel","op aanvraag","LVE Gitter Boden, Design Kreis, Edelstahl steckbar","LVE air grill floor - stainless steel 5","LVE grille de sol, design cercle, acier inoxydable enfichable","LVE air grill floor - stainless steel 5","LVE Vloerrooster, Kruis design, RVS koppelbaar","LVE air grill floor - stainless steel 5","LVE air grill floor - stainless steel 5","LVE air grill floor - stainless steel 5","LVE air grill floor - stainless steel 5","LVE air grill floor - stainless steel 5","LVE air grill floor - stainless steel 5"]
[null,231973,"LVE air grill floor - white","On request","",null,null,null,null,null,null,231973,"LVE air grill floor - white","On request",false,null,231973,53,"On request","sur demande","på forespørgsel","op aanvraag","LVE Gitter Boden, Design Kreis, weiß lackiert","LVE air grill floor - white","LVE grille de sol, design cercle, laquée blanc","LVE air grill floor - white","LVE Vloerrooster, Kruis design, wit gelakt","LVE air grill floor - white","LVE air grill floor - white","LVE air grill floor - white","LVE air grill floor - white","LVE air grill floor - white","LVE air grill floor - white"]
[null,231974,"LVE air grill wall/ceiling - stainless steel 1","On request","",null,null,null,null,null,null,231974,"LVE air grill wall/ceiling - stainless steel 1","On request",false,null,231974,32.5,"On request",40,"på forespørgsel","op aanvraag","LVE Gitter Wand/Decke, Design Welle, Edelstahl","LVE air grill wall/ceiling - stainless steel 1","LVE grille mur/plafond, design onde, acier inoxydable","LVE air grill wall/ceiling - stainless steel 1","LVE Wand/plafond rooster, Golf design, RVS","LVE air grill wall/ceiling - stainless steel 1","LVE air grill wall/ceiling - stainless steel 1","LVE air grill wall/ceiling - stainless steel 1","LVE air grill wall/ceiling - stainless steel 1","LVE air grill wall/ceiling - stainless steel 1","LVE air grill wall/ceiling - stainless steel 1"]
[null,231975,"LVE air grill wall/ceiling - stainless steel 2","On request","",null,null,null,null,null,null,231975,"LVE air grill wall/ceiling - stainless steel 2","On request",false,null,231975,32.5,"On request",40,"på forespørgsel","op aanvraag","LVE Gitter Wand/Decke, Design Natur, Edelstahl","LVE air grill wall/ceiling - stainless steel 2","LVE grille mur/plafond, design nature, acier inoxydable","LVE air grill wall/ceiling - stainless steel 2","LVE Wand/plafond rooster, Natuur design, RVS","LVE air grill wall/ceiling - stainless steel 2","LVE air grill wall/ceiling - stainless steel 2","LVE air grill wall/ceiling - stainless steel 2","LVE air grill wall/ceiling - stainless steel 2","LVE air grill wall/ceiling - stainless steel 2","LVE air grill wall/ceiling - stainless steel 2"]
[null,231114,"LVE air grill wall/ceiling - stainless steel 3","On request","",null,null,null,null,null,null,231114,"LVE air grill wall/ceiling - stainless steel 3","On request",false,null,231114,21.9,"On request",40,"på forespørgsel","op aanvraag","LVE Gitter Wand/Decke, Design Langloch, Edelstahl","LVE air grill wall/ceiling - stainless steel 3","LVE grille mur/plafond, design trou oblong, acier inoxydable","LVE air grill wall/ceiling - stainless steel 3","LVE Wand/plafond rooster, Rechthoek design, RVS","LVE air grill wall/ceiling - stainless steel 3","LVE air grill wall/ceiling - stainless steel 3","LVE air grill wall/ceiling - stainless steel 3","LVE air grill wall/ceiling - stainless steel 3","LVE air grill wall/ceiling - stainless steel 3","LVE air grill wall/ceiling - stainless steel 3"]
[null,231976,"LVE air grill wall/ceiling - stainless steel 4","On request","",null,null,null,null,null,null,231976,"LVE air grill wall/ceiling - stainless steel 4","On request",false,null,231976,21.9,"On request",40,"på forespørgsel","op aanvraag","LVE Gitter Wand/Decke, Design Kreis, Edelstahl","LVE air grill wall/ceiling - stainless steel 4","LVE grille mur/plafond, design circuit, acier inoxydable","LVE air grill wall/ceiling - stainless steel 4","LVE Wand/plafond rooster, Kruis design, RVS","LVE air grill wall/ceiling - stainless steel 4","LVE air grill wall/ceiling - stainless steel 4","LVE air grill wall/ceiling - stainless steel 4","LVE air grill wall/ceiling - stainless steel 4","LVE air grill wall/ceiling - stainless steel 4","LVE air grill wall/ceiling - stainless steel 4"]
[null,231977,"LVE air grill wall/ceiling - white","On request","",null,null,null,null,null,null,231977,"LVE air grill wall/ceiling - white","On request",false,null,231977,21.9,"On request",40,"på forespørgsel","op aanvraag","LVE Gitter Wand/Decke, Design Kreis, weiß lackiert","LVE air grill wall/ceiling - white","LVE grille mur/plafond, design circuit, laquée blanc","LVE air grill wall/ceiling - white","LVE Wand/plafond rooster, Kruis design, wit gelakt ","LVE air grill wall/ceiling - white","LVE air grill wall/ceiling - white","LVE air grill wall/ceiling - white","LVE air grill wall/ceiling - white","LVE air grill wall/ceiling - white","LVE air grill wall/ceiling - white"]
[null,233408,"LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","On request","",null,null,null,null,null,null,233408,"LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","On request",false,null,233408,21.4,"On request","sur demande","på forespørgsel","op aanvraag","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE rooster Wand/Plafond, Rechthoekig design, wit gelakt","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert","LVE Gitter Wand/Decke, Design Langloch, weiß lackiert"]
[null,232022,"LVE Luftleitblech für Deckengitter","On request","",null,null,null,null,null,null,232022,"LVE Luftleitblech für Deckengitter","On request",false,null,232022,19.2,"On request",20,92,"op aanvraag","LVE Luftleitblech für Deckengitter","LVE Luftleitblech für Deckengitter","LVE Luftleitblech für Deckengitter","LVE Luftleitblech für Deckengitter","LVE Luchtgeleidingsplaat voor plafond rooster","LVE Luftleitblech für Deckengitter","LVE Luftleitblech für Deckengitter","LVE Luftleitblech für Deckengitter","LVE Luftleitblech für Deckengitter","LVE Luftleitblech für Deckengitter","LVE Luftleitblech für Deckengitter"]
[null,227652,"LVS central air distributor, 4 connections","On request","",null,null,null,null,null,null,227652,"LVS central air distributor, 4 connections","On request",false,null,227652,53,"On request","sur demande","på forespørgsel","op aanvraag","LVS Zentraler Luftverteiler, 4-fach","LVS central air distributor, 4 connections","LVS distributeur d'air centralisé, 4 connexions","LVS central air distributor, 4 connections","LVS Centrale luchtverdeler, 4-voudig","LVS central air distributor, 4 connections","LVS central air distributor, 4 connections","LVS central air distributor, 4 connections","LVS central air distributor, 4 connections","LVS central air distributor, 4 connections","LVS central air distributor, 4 connections"]
[null,232117,"LVS central air distributor, 8 connections","On request","",null,null,null,null,null,null,232117,"LVS central air distributor, 8 connections","On request",false,null,232117,163,"On request","sur demande","på forespørgsel","op aanvraag","LVS Zentraler Luftverteiler, 8-fach","LVS central air distributor, 8 connections","LVS distributeur d'air centralisé, 8 connexions","LVS central air distributor, 8 connections","LVS Centrale luchtverdeler, 8-voudig","LVS central air distributor, 8 connections","LVS central air distributor, 8 connections","LVS central air distributor, 8 connections","LVS central air distributor, 8 connections","LVS central air distributor, 8 connections","LVS central air distributor, 8 connections"]
[null,232118,"LVS central air distributor, 12 connections","On request","",null,null,null,null,null,null,232118,"LVS central air distributor, 12 connections","On request",false,null,232118,248,"On request","sur demande","på forespørgsel","op aanvraag","LVS Zentraler Luftverteiler, 12-fach","LVS central air distributor, 12 connections","LVS distributeur d'air centralisé, 12 connexions","LVS central air distributor, 12 connections","LVS Centrale luchtverdeler, 12-voudig","LVS central air distributor, 12 connections","LVS central air distributor, 12 connections","LVS central air distributor, 12 connections","LVS central air distributor, 12 connections","LVS central air distributor, 12 connections","LVS central air distributor, 12 connections"]
[null,232121,"LVS set for lateral connection","On request","",null,null,null,null,null,null,232121,"LVS set for lateral connection","On request",false,null,232121,97,"On request","sur demande","på forespørgsel","op aanvraag","LVS Zubehörset seitlicher Verteileranschluss","LVS set for lateral connection","LVS set d'accessoires raccord latéral de distributeur","LVS set for lateral connection","LVS Toebehorenset zijdelingse verdeleraansluiting","LVS set for lateral connection","LVS set for lateral connection","LVS set for lateral connection","LVS set for lateral connection","LVS set for lateral connection","LVS set for lateral connection"]
[null,223311,"LVS air oulet","On request","",null,null,null,null,null,null,223311,"LVS air oulet","On request",false,null,223311,31,"On request","sur demande","på forespørgsel","op aanvraag","LVS Auslass-/Einlassgehäuse","LVS air oulet","LVS boîtier de sortie/d'entrée","LVS air oulet","LVS Uitlaat-/Inlaatbehuizing","LVS air oulet","LVS air oulet","LVS air oulet","LVS air oulet","LVS air oulet","LVS air oulet"]
[null,223312,"LVS air outlet precast deck","On request","",null,null,null,null,null,null,223312,"LVS air outlet precast deck","On request",false,null,223312,41.5,"On request","sur demande","på forespørgsel","op aanvraag","LVS Auslass-/Einlassgehäuse Filigrandecke","LVS air outlet precast deck","LVS boîtier de sortie/d'entrée couverture en éléments préfabriqués","LVS air outlet precast deck","LVS Uitlaat-/Inlaatbehuizing Filigraanafdekking","LVS air outlet precast deck","LVS air outlet precast deck","LVS air outlet precast deck","LVS air outlet precast deck","LVS air outlet precast deck","LVS air outlet precast deck"]
[null,227653,"LVS air outlet small","On request","",null,null,null,null,null,null,227653,"LVS air outlet small","On request",false,null,227653,29.5,"On request","sur demande","på forespørgsel","op aanvraag","LVS Auslass-/Einlassgehäuse klein","LVS air outlet small","LVS boîtier de sortie/d'entrée petit","LVS air outlet small","LVS Uitlaat-/Inlaatbehuizing klein","LVS air outlet small","LVS air outlet small","LVS air outlet small","LVS air outlet small","LVS air outlet small","LVS air outlet small"]
[null,223313,"LVS air grille - standard","On request","",null,null,null,null,null,null,223313,"LVS air grille - standard","On request",false,null,223313,24.7,"On request","sur demande","på forespørgsel","op aanvraag","LVS Luftdurchlassgitter Standard","LVS air grille - standard","LVS grille d'aération standard","LVS air grille - standard","LVS Luchtdoorlaatrooster Standaard","LVS air grille - standard","LVS air grille - standard","LVS air grille - standard","LVS air grille - standard","LVS air grille - standard","LVS air grille - standard"]
[null,223315,"LVS air grille - white","On request","",null,null,null,null,null,null,223315,"LVS air grille - white","On request",false,null,223315,49.5,"On request","sur demande","på forespørgsel","op aanvraag","LVS Luftdurchlassgitter Stahlblech weiß lackiert","LVS air grille - white","LVS grille d'aération tôle d'acier laquée blanc","LVS air grille - white","LVS Luchtdoorlaatrooster staalplaat wit gelakt","LVS air grille - white","LVS air grille - white","LVS air grille - white","LVS air grille - white","LVS air grille - white","LVS air grille - white"]
[null,223314,"LVS air grille - stainless steel","On request","",null,null,null,null,null,null,223314,"LVS air grille - stainless steel","On request",false,null,223314,49.5,"On request","sur demande","på forespørgsel","op aanvraag","LVS Luftdurchlassgitter Edelstahl","LVS air grille - stainless steel","LVS grille d'aération acier inoxydable","LVS air grille - stainless steel","LVS Luchtdoorlaatrooster RVS","LVS air grille - stainless steel","LVS air grille - stainless steel","LVS air grille - stainless steel","LVS air grille - stainless steel","LVS air grille - stainless steel","LVS air grille - stainless steel"]
[null,227656,"LVS air grille - stainles steel design","On request","",null,null,null,null,null,null,227656,"LVS air grille - stainles steel design","On request",false,null,227656,53,"On request","sur demande","på forespørgsel","op aanvraag","LVS Luftdurchlassgitter Edelstahl Design","LVS air grille - stainles steel design","LVS grille d'aération acier inoxydable design","LVS air grille - stainles steel design","LVS Luchtdoorlaatrooster RVS Design","LVS air grille - stainles steel design","LVS air grille - stainles steel design","LVS air grille - stainles steel design","LVS air grille - stainles steel design","LVS air grille - stainles steel design","LVS air grille - stainles steel design"]
[null,223318,"LVS connection fitting","On request","",null,null,null,null,null,null,223318,"LVS connection fitting","On request",false,null,223318,49.5,"On request","sur demande","på forespørgsel","op aanvraag","LVS Anschlussadapter, 5 Stück","LVS connection fitting","LVS adaptateur de raccordement, 5 p.","LVS connection fitting","LVS Aansluitadaptor, 5 stuks","LVS connection fitting","LVS connection fitting","LVS connection fitting","LVS connection fitting","LVS connection fitting","LVS connection fitting"]
[null,227654,"LVS connection fitting small","On request","",null,null,null,null,null,null,227654,"LVS connection fitting small","On request",false,null,227654,47,"On request","sur demande","på forespørgsel","op aanvraag","LVS Anschlussadapter klein, 5 Stück","LVS connection fitting small","LVS adaptateur de raccordement petit, 5 p.","LVS connection fitting small","LVS Aansluitadaptor klein, 5 stuks","LVS connection fitting small","LVS connection fitting small","LVS connection fitting small","LVS connection fitting small","LVS connection fitting small","LVS connection fitting small"]
[null,223319,"LVS End duct","On request","",null,null,null,null,null,null,223319,"LVS End duct","On request",false,null,223319,62,"On request","sur demande","på forespørgsel","op aanvraag","LVS Enddeckel, 10 Stück","LVS End duct","LVS couvercle en extrémité, 10 p.","LVS End duct","LVS Einddeksel, 10 stuks","LVS End duct","LVS End duct","LVS End duct","LVS End duct","LVS End duct","LVS End duct"]
[null,227655,"LVS End duct small","On request","",null,null,null,null,null,null,227655,"LVS End duct small","On request",false,null,227655,61,"On request","sur demande","på forespørgsel","op aanvraag","LVS Enddeckel klein, 10 Stück","LVS End duct small","LVS couvercle en extrémité petit, 10 p.","LVS End duct small","LVS Einddeksel klein, 10 stuks","LVS End duct small","LVS End duct small","LVS End duct small","LVS End duct small","LVS End duct small","LVS End duct small"]
[null,224897,"LVS fitting for pipe-extension","On request","",null,null,null,null,null,null,224897,"LVS fitting for pipe-extension","On request",false,null,224897,24.5,"On request","sur demande","på forespørgsel","op aanvraag","LVS Adapter Rohrverlängerung, 5 Stück","LVS fitting for pipe-extension","LVS adaptateur rallonge de tube, 5 p.","LVS fitting for pipe-extension","LVS Adaptor buisverlenging, 5 stuks","LVS fitting for pipe-extension","LVS fitting for pipe-extension","LVS fitting for pipe-extension","LVS fitting for pipe-extension","LVS fitting for pipe-extension","LVS fitting for pipe-extension"]
[null,223321,"LVS flexible pipe DN 75, 25 m","On request","",null,null,null,null,null,null,223321,"LVS flexible pipe DN 75, 25 m","On request",false,null,223321,185,"On request",100,"på forespørgsel","op aanvraag","LVS Flexibles Kunststoffrohr DN 75, 25 m","LVS flexible pipe DN 75, 25 m","LVS tube en matière synthétique souple DN 75, 25 m","LVS flexible pipe DN 75, 25 m","LVS Flexibele kunststofbuis DN 75, 25 m","LVS flexible pipe DN 75, 25 m","LVS flexible pipe DN 75, 25 m","LVS flexible pipe DN 75, 25 m","LVS flexible pipe DN 75, 25 m","LVS flexible pipe DN 75, 25 m","LVS flexible pipe DN 75, 25 m"]
[null,227650,"LVS Redirection piece DN 75 to DN 100","On request","",null,null,null,null,null,null,227650,"LVS Redirection piece DN 75 to DN 100","On request",false,null,227650,31,"On request","sur demande","på forespørgsel","op aanvraag","LVS Umlenkstück DN 75 auf DN 100","LVS Redirection piece DN 75 to DN 100","LVS déflecteur DN 75 à DN 100","LVS Redirection piece DN 75 to DN 100","LVS Afbuigstuk DN 75 naar DN 100","LVS Redirection piece DN 75 to DN 100","LVS Redirection piece DN 75 to DN 100","LVS Redirection piece DN 75 to DN 100","LVS Redirection piece DN 75 to DN 100","LVS Redirection piece DN 75 to DN 100","LVS Redirection piece DN 75 to DN 100"]
[null,232116,"LVS Redirection piece 2 x DN 75 to DN 100","On request","",null,null,null,null,null,null,232116,"LVS Redirection piece 2 x DN 75 to DN 100","On request",false,null,232116,52,"On request","sur demande","på forespørgsel","op aanvraag","LVS Umlenkstück 2 x DN 75 auf DN 100","LVS Redirection piece 2 x DN 75 to DN 100","LVS déflecteur 2 x DN 75 à DN 100","LVS Redirection piece 2 x DN 75 to DN 100","LVS Afbuigstuk 2 x DN 75 naar DN 100","LVS Redirection piece 2 x DN 75 to DN 100","LVS Redirection piece 2 x DN 75 to DN 100","LVS Redirection piece 2 x DN 75 to DN 100","LVS Redirection piece 2 x DN 75 to DN 100","LVS Redirection piece 2 x DN 75 to DN 100","LVS Redirection piece 2 x DN 75 to DN 100"]
[null,227651,"LVS Adapter piece 2 x DN 75 to LFK 50 x 150","On request","",null,null,null,null,null,null,227651,"LVS Adapter piece 2 x DN 75 to LFK 50 x 150","On request",false,null,227651,42.5,"On request","sur demande","på forespørgsel","op aanvraag","LVS Übergangsstück 2 x DN 75 auf LFK 50 x 150","LVS Adapter piece 2 x DN 75 to LFK 50 x 150","LVS déflecteur 2 x DN 75 à LFK 50 x 150","LVS Adapter piece 2 x DN 75 to LFK 50 x 150","LVS Overgangsstuk 2 x DN 75 naar LFK 50 x 150","LVS Adapter piece 2 x DN 75 to LFK 50 x 150","LVS Adapter piece 2 x DN 75 to LFK 50 x 150","LVS Adapter piece 2 x DN 75 to LFK 50 x 150","LVS Adapter piece 2 x DN 75 to LFK 50 x 150","LVS Adapter piece 2 x DN 75 to LFK 50 x 150","LVS Adapter piece 2 x DN 75 to LFK 50 x 150"]
[null,220565,"Central air distributor LFK","On request","",null,null,null,null,null,null,220565,"Central air distributor LFK","On request",false,null,220565,281,"On request","sur demande","på forespørgsel","op aanvraag","Zentraler Luftverteiler LFK","Central air distributor LFK","Distributeur d'air centralisé LFK","Central air distributor LFK","Centrale luchtverdeler LFK","Central air distributor LFK","Central air distributor LFK","Central air distributor LFK","Central air distributor LFK","Central air distributor LFK","Central air distributor LFK"]
[null,220566,"Flat pipework 100 x 50, 2m","On request","",null,null,null,null,null,null,220566,"Flat pipework 100 x 50, 2m","On request",false,null,220566,23.1,"On request","sur demande","på forespørgsel","op aanvraag","Flachkanal 100 x 50, 2m","Flat pipework 100 x 50, 2m","Gaine plate 100 x 50, 2 m","Flat pipework 100 x 50, 2m","Platkanaal 100 x 50, 2m","Flat pipework 100 x 50, 2m","Flat pipework 100 x 50, 2m","Flat pipework 100 x 50, 2m","Flat pipework 100 x 50, 2m","Flat pipework 100 x 50, 2m","Flat pipework 100 x 50, 2m"]
[null,220567,"Flat pipework 150 x 50, 2m","On request","",null,null,null,null,null,null,220567,"Flat pipework 150 x 50, 2m","On request",false,null,220567,28.5,"On request","sur demande","på forespørgsel","op aanvraag","Flachkanal 150 x 50, 2m","Flat pipework 150 x 50, 2m","Gaine plate 150 x 50, 2 m","Flat pipework 150 x 50, 2m","Platkanaal 150 x 50, 2m","Flat pipework 150 x 50, 2m","Flat pipework 150 x 50, 2m","Flat pipework 150 x 50, 2m","Flat pipework 150 x 50, 2m","Flat pipework 150 x 50, 2m","Flat pipework 150 x 50, 2m"]
[null,221483,"Flat pipework 200 x 50, 2m","On request","",null,null,null,null,null,null,221483,"Flat pipework 200 x 50, 2m","On request",false,null,221483,31,"On request","sur demande","på forespørgsel","op aanvraag","Flachkanal 200 x 50, 2m","Flat pipework 200 x 50, 2m","Gaine plate 200 x 50, 2 m","Flat pipework 200 x 50, 2m","Platkanaal 200 x 50, 2m","Flat pipework 200 x 50, 2m","Flat pipework 200 x 50, 2m","Flat pipework 200 x 50, 2m","Flat pipework 200 x 50, 2m","Flat pipework 200 x 50, 2m","Flat pipework 200 x 50, 2m"]
[null,220568,"Nippel 100 x 50","On request","",null,null,null,null,null,null,220568,"Nippel 100 x 50","On request",false,null,220568,3.8,"On request","sur demande","på forespørgsel","op aanvraag","Nippel 100 x 50","Nippel 100 x 50","Mamelon 100 x 50","Nippel 100 x 50","Nippel 100 x 50","Nippel 100 x 50","Nippel 100 x 50","Nippel 100 x 50","Nippel 100 x 50","Nippel 100 x 50","Nippel 100 x 50"]
[null,220569,"Nippel 150 x 50","On request","",null,null,null,null,null,null,220569,"Nippel 150 x 50","On request",false,null,220569,4.7,"On request","sur demande","på forespørgsel","op aanvraag","Nippel 150 x 50","Nippel 150 x 50","Mamelon 150 x 50","Nippel 150 x 50","Nippel 150 x 50","Nippel 150 x 50","Nippel 150 x 50","Nippel 150 x 50","Nippel 150 x 50","Nippel 150 x 50","Nippel 150 x 50"]
[null,221484,"Nippel 200 x 50","On request","",null,null,null,null,null,null,221484,"Nippel 200 x 50","On request",false,null,221484,5.6,"On request","sur demande","på forespørgsel","op aanvraag","Nippel 200 x 50","Nippel 200 x 50","Mamelon 200 x 50","Nippel 200 x 50","Nippel 200 x 50","Nippel 200 x 50","Nippel 200 x 50","Nippel 200 x 50","Nippel 200 x 50","Nippel 200 x 50","Nippel 200 x 50"]
[null,220570,"Fitting 100 x 50","On request","",null,null,null,null,null,null,220570,"Fitting 100 x 50","On request",false,null,220570,3.8,"On request","sur demande","på forespørgsel","op aanvraag","Muffe 100 x 50","Fitting 100 x 50","Manchon 100 x 50","Fitting 100 x 50","Sok 100 x 50","Fitting 100 x 50","Fitting 100 x 50","Fitting 100 x 50","Fitting 100 x 50","Fitting 100 x 50","Fitting 100 x 50"]
[null,220571,"Fitting 150 x 50","On request","",null,null,null,null,null,null,220571,"Fitting 150 x 50","On request",false,null,220571,5.6,"On request","sur demande","på forespørgsel","op aanvraag","Muffe 150 x 50","Fitting 150 x 50","Manchon 150 x 50","Fitting 150 x 50","Sok 150 x 50","Fitting 150 x 50","Fitting 150 x 50","Fitting 150 x 50","Fitting 150 x 50","Fitting 150 x 50","Fitting 150 x 50"]
[null,221485,"Fitting 200 x 50","On request","",null,null,null,null,null,null,221485,"Fitting 200 x 50","On request",false,null,221485,6.9,"On request","sur demande","på forespørgsel","op aanvraag","Muffe 200 x 50","Fitting 200 x 50","Manchon 200 x 50","Fitting 200 x 50","Sok 200 x 50","Fitting 200 x 50","Fitting 200 x 50","Fitting 200 x 50","Fitting 200 x 50","Fitting 200 x 50","Fitting 200 x 50"]
[null,220572,"Bow 100 x 50, 90° flat","On request","",null,null,null,null,null,null,220572,"Bow 100 x 50, 90° flat","On request",false,null,220572,16.399999999999999,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 100 x 50, 90° flach","Bow 100 x 50, 90° flat","Coude 100 x 50, 90° plat","Bow 100 x 50, 90° flat","Bocht 100 x 50, 90° plat","Bow 100 x 50, 90° flat","Bow 100 x 50, 90° flat","Bow 100 x 50, 90° flat","Bow 100 x 50, 90° flat","Bow 100 x 50, 90° flat","Bow 100 x 50, 90° flat"]
[null,220573,"Bow 150 x 50, 90° flat","On request","",null,null,null,null,null,null,220573,"Bow 150 x 50, 90° flat","On request",false,null,220573,20.3,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 150 x 50, 90° flach","Bow 150 x 50, 90° flat","Coude 150 x 50, 90° plat","Bow 150 x 50, 90° flat","Bocht 150 x 50, 90° plat","Bow 150 x 50, 90° flat","Bow 150 x 50, 90° flat","Bow 150 x 50, 90° flat","Bow 150 x 50, 90° flat","Bow 150 x 50, 90° flat","Bow 150 x 50, 90° flat"]
[null,221486,"Bow 200 x 50, 90° flat","On request","",null,null,null,null,null,null,221486,"Bow 200 x 50, 90° flat","On request",false,null,221486,22.8,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 200 x 50, 90° flach","Bow 200 x 50, 90° flat","Coude 200 x 50, 90° plat","Bow 200 x 50, 90° flat","Bocht 200 x 50, 90° plat","Bow 200 x 50, 90° flat","Bow 200 x 50, 90° flat","Bow 200 x 50, 90° flat","Bow 200 x 50, 90° flat","Bow 200 x 50, 90° flat","Bow 200 x 50, 90° flat"]
[null,220574,"Bow 100 x 50, 90° high","On request","",null,null,null,null,null,null,220574,"Bow 100 x 50, 90° high","On request",false,null,220574,16.399999999999999,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 100 x 50, 90° hoch","Bow 100 x 50, 90° high","Coude 100 x 50, 90° haut","Bow 100 x 50, 90° high","Bocht 100 x 50, 90° hoog","Bow 100 x 50, 90° high","Bow 100 x 50, 90° high","Bow 100 x 50, 90° high","Bow 100 x 50, 90° high","Bow 100 x 50, 90° high","Bow 100 x 50, 90° high"]
[null,220575,"Bow 150 x 50, 90° high","On request","",null,null,null,null,null,null,220575,"Bow 150 x 50, 90° high","On request",false,null,220575,20.3,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 150 x 50, 90° hoch","Bow 150 x 50, 90° high","Coude 150 x 50, 90° haut","Bow 150 x 50, 90° high","Bocht 150 x 50, 90° hoog","Bow 150 x 50, 90° high","Bow 150 x 50, 90° high","Bow 150 x 50, 90° high","Bow 150 x 50, 90° high","Bow 150 x 50, 90° high","Bow 150 x 50, 90° high"]
[null,221487,"Bow 200 x 50, 90° high","On request","",null,null,null,null,null,null,221487,"Bow 200 x 50, 90° high","On request",false,null,221487,22.8,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 200 x 50, 90° hoch","Bow 200 x 50, 90° high","Coude 200 x 50, 90° haut","Bow 200 x 50, 90° high","Bocht 200 x 50, 90° hoog","Bow 200 x 50, 90° high","Bow 200 x 50, 90° high","Bow 200 x 50, 90° high","Bow 200 x 50, 90° high","Bow 200 x 50, 90° high","Bow 200 x 50, 90° high"]
[null,220576,"Bow 100 x 50, 45° flat","On request","",null,null,null,null,null,null,220576,"Bow 100 x 50, 45° flat","On request",false,null,220576,16.399999999999999,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 100 x 50, 45° flach","Bow 100 x 50, 45° flat","Coude 100 x 50, 45° plat","Bow 100 x 50, 45° flat","Bocht 100 x 50, 45° plat","Bow 100 x 50, 45° flat","Bow 100 x 50, 45° flat","Bow 100 x 50, 45° flat","Bow 100 x 50, 45° flat","Bow 100 x 50, 45° flat","Bow 100 x 50, 45° flat"]
[null,220577,"Bow 150 x 50, 45° flat","On request","",null,null,null,null,null,null,220577,"Bow 150 x 50, 45° flat","On request",false,null,220577,20.3,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 150 x 50, 45° flach","Bow 150 x 50, 45° flat","Coude 150 x 50, 45° plat","Bow 150 x 50, 45° flat","Bocht 150 x 50, 45° plat","Bow 150 x 50, 45° flat","Bow 150 x 50, 45° flat","Bow 150 x 50, 45° flat","Bow 150 x 50, 45° flat","Bow 150 x 50, 45° flat","Bow 150 x 50, 45° flat"]
[null,221488,"Bow 200 x 50, 45° flat","On request","",null,null,null,null,null,null,221488,"Bow 200 x 50, 45° flat","On request",false,null,221488,22.8,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 200 x 50, 45° flach","Bow 200 x 50, 45° flat","Coude 200 x 50, 45° plat","Bow 200 x 50, 45° flat","Bocht 200 x 50, 45° plat","Bow 200 x 50, 45° flat","Bow 200 x 50, 45° flat","Bow 200 x 50, 45° flat","Bow 200 x 50, 45° flat","Bow 200 x 50, 45° flat","Bow 200 x 50, 45° flat"]
[null,221229,"Branch piece 100 x 50 to DN 100","On request","",null,null,null,null,null,null,221229,"Branch piece 100 x 50 to DN 100","On request",false,null,221229,39.5,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 100 x 50 auf DN 100","Branch piece 100 x 50 to DN 100","Pièce de dérivation 100 x 50 à DN 100","Branch piece 100 x 50 to DN 100","T-stuk 100 x 50 naar DN 100","Branch piece 100 x 50 to DN 100","Branch piece 100 x 50 to DN 100","Branch piece 100 x 50 to DN 100","Branch piece 100 x 50 to DN 100","Branch piece 100 x 50 to DN 100","Branch piece 100 x 50 to DN 100"]
[null,221230,"Branch piece 150 x 50 to DN 100","On request","",null,null,null,null,null,null,221230,"Branch piece 150 x 50 to DN 100","On request",false,null,221230,39.5,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 150 x 50 auf DN 100","Branch piece 150 x 50 to DN 100","Pièce de dérivation 150 x 50 à DN 100","Branch piece 150 x 50 to DN 100","T-stuk 150 x 50 naar DN 100","Branch piece 150 x 50 to DN 100","Branch piece 150 x 50 to DN 100","Branch piece 150 x 50 to DN 100","Branch piece 150 x 50 to DN 100","Branch piece 150 x 50 to DN 100","Branch piece 150 x 50 to DN 100"]
[null,220578,"Branch piece 150 x 50 to DN 125","On request","",null,null,null,null,null,null,220578,"Branch piece 150 x 50 to DN 125","On request",false,null,220578,28,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 150 x 50 auf DN 125","Branch piece 150 x 50 to DN 125","Pièce de dérivation 150 x 50 à DN 125","Branch piece 150 x 50 to DN 125","T-stuk 150 x 50 naar DN 125","Branch piece 150 x 50 to DN 125","Branch piece 150 x 50 to DN 125","Branch piece 150 x 50 to DN 125","Branch piece 150 x 50 to DN 125","Branch piece 150 x 50 to DN 125","Branch piece 150 x 50 to DN 125"]
[null,221489,"Branch piece 200 x 50 to DN 125","On request","",null,null,null,null,null,null,221489,"Branch piece 200 x 50 to DN 125","On request",false,null,221489,29.5,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 200 x 50 auf DN 125","Branch piece 200 x 50 to DN 125","Pièce de dérivation 200 x 50 à DN 125","Branch piece 200 x 50 to DN 125","T-stuk 200 x 50 naar DN 125","Branch piece 200 x 50 to DN 125","Branch piece 200 x 50 to DN 125","Branch piece 200 x 50 to DN 125","Branch piece 200 x 50 to DN 125","Branch piece 200 x 50 to DN 125","Branch piece 200 x 50 to DN 125"]
[null,221231,"Branch piece 150/150/150 flat","On request","",null,null,null,null,null,null,221231,"Branch piece 150/150/150 flat","On request",false,null,221231,24,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 150/150/150 flach","Branch piece 150/150/150 flat","Pièce de dérivation 150/150/150 plate","Branch piece 150/150/150 flat","T-stuk 150/150/150 plat","Branch piece 150/150/150 flat","Branch piece 150/150/150 flat","Branch piece 150/150/150 flat","Branch piece 150/150/150 flat","Branch piece 150/150/150 flat","Branch piece 150/150/150 flat"]
[null,220579,"Branch piece 150/150/100 flat","On request","",null,null,null,null,null,null,220579,"Branch piece 150/150/100 flat","On request",false,null,220579,20.3,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 150/150/100 flach","Branch piece 150/150/100 flat","Pièce de dérivation 150/150/100 plate","Branch piece 150/150/100 flat","T-stuk 150/150/100 plat","Branch piece 150/150/100 flat","Branch piece 150/150/100 flat","Branch piece 150/150/100 flat","Branch piece 150/150/100 flat","Branch piece 150/150/100 flat","Branch piece 150/150/100 flat"]
[null,221490,"Branch piece 200/200/100 flat","On request","",null,null,null,null,null,null,221490,"Branch piece 200/200/100 flat","On request",false,null,221490,21,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 200/200/100 flach","Branch piece 200/200/100 flat","Pièce de dérivation 200/200/100 plate","Branch piece 200/200/100 flat","T-stuk 200/200/100 plat","Branch piece 200/200/100 flat","Branch piece 200/200/100 flat","Branch piece 200/200/100 flat","Branch piece 200/200/100 flat","Branch piece 200/200/100 flat","Branch piece 200/200/100 flat"]
[null,232989,"Abzweigstück 200/150/150 flach","On request","",null,null,null,null,null,null,232989,"Abzweigstück 200/150/150 flach","On request",false,null,232989,27.5,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 200/200/150 flach","Abzweigstück 200/150/150 flach","Abzweigstück 200/150/150 flach","Abzweigstück 200/150/150 flach","T-stuk 200/150/150 plat","Abzweigstück 200/150/150 flach","Abzweigstück 200/150/150 flach","Abzweigstück 200/150/150 flach","Abzweigstück 200/150/150 flach","Abzweigstück 200/150/150 flach","Abzweigstück 200/150/150 flach"]
[null,220580,"Branch piece 150/100/100 flat","On request",{"$f":"IF(O714=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,220580,"Branch piece 150/100/100 flat","On request",false,null,220580,34,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 150/100/100 flach","Branch piece 150/100/100 flat","Pièce de dérivation 150/100/100 plate","Branch piece 150/100/100 flat","T-stuk 150/100/100 plat","Branch piece 150/100/100 flat","Branch piece 150/100/100 flat","Branch piece 150/100/100 flat","Branch piece 150/100/100 flat","Branch piece 150/100/100 flat","Branch piece 150/100/100 flat"]
[null,221491,"Branch piece 200/100/100 flat","On request","",null,null,null,null,null,null,221491,"Branch piece 200/100/100 flat","On request",false,null,221491,41,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück 200/100/100 flach","Branch piece 200/100/100 flat","Pièce de dérivation 200/100/100 plate","Branch piece 200/100/100 flat","T-stuk 200/100/100 plat","Branch piece 200/100/100 flat","Branch piece 200/100/100 flat","Branch piece 200/100/100 flat","Branch piece 200/100/100 flat","Branch piece 200/100/100 flat","Branch piece 200/100/100 flat"]
[null,220597,"Silencer 100 x 50  1m","On request","",null,null,null,null,null,null,220597,"Silencer 100 x 50  1m","On request",false,null,220597,108,"On request","sur demande","på forespørgsel","op aanvraag","Telefonieschalldämpfer 100 x 50  1m","Silencer 100 x 50  1m","Piège à son 100 x 50  1 m","Silencer 100 x 50  1m","Geluiddemper 100 x 50  1m","Silencer 100 x 50  1m","Silencer 100 x 50  1m","Silencer 100 x 50  1m","Silencer 100 x 50  1m","Silencer 100 x 50  1m","Silencer 100 x 50  1m"]
[null,220598,"Silencer 150 x 50  1m","On request","",null,null,null,null,null,null,220598,"Silencer 150 x 50  1m","On request",false,null,220598,114,"On request","sur demande","på forespørgsel","op aanvraag","Telefonieschalldämpfer 150 x 50  1m","Silencer 150 x 50  1m","Piège à son 150 x 50  1 m","Silencer 150 x 50  1m","Geluiddemper 150 x 50  1m","Silencer 150 x 50  1m","Silencer 150 x 50  1m","Silencer 150 x 50  1m","Silencer 150 x 50  1m","Silencer 150 x 50  1m","Silencer 150 x 50  1m"]
[null,221492,"Silencer 200 x 50  1m","On request","",null,null,null,null,null,null,221492,"Silencer 200 x 50  1m","On request",{"$f":"IF(AND(B718=L718,C718=M718,D718=N718),FALSE,TRUE)","v":false},null,221492,156,"On request","sur demande","på forespørgsel","op aanvraag","Telefonieschalldämpfer 200 x 50  1m","Silencer 200 x 50  1m","Piège à son 200 x 50  1 m","Silencer 200 x 50  1m","Geluiddemper 200 x 50  1m","Silencer 200 x 50  1m","Silencer 200 x 50  1m","Silencer 200 x 50  1m","Silencer 200 x 50  1m","Silencer 200 x 50  1m","Silencer 200 x 50  1m"]
[null,220599,"Redirection piece 100 x 50 to DN 100, 350 mm","On request","",null,null,null,null,null,null,220599,"Redirection piece 100 x 50 to DN 100, 350 mm","On request",false,null,220599,34,"On request","sur demande","på forespørgsel","op aanvraag","Umlenkstück 100 x 50 auf DN 100, 350 mm lang","Redirection piece 100 x 50 to DN 100, 350 mm","Déflecteur 100 x 50 à DN 100, longueur 350 mm","Redirection piece 100 x 50 to DN 100, 350 mm","Afbuigstuk 100 x 50 naar DN 100, 350 mm lang","Redirection piece 100 x 50 to DN 100, 350 mm","Redirection piece 100 x 50 to DN 100, 350 mm","Redirection piece 100 x 50 to DN 100, 350 mm","Redirection piece 100 x 50 to DN 100, 350 mm","Redirection piece 100 x 50 to DN 100, 350 mm","Redirection piece 100 x 50 to DN 100, 350 mm"]
[null,220600,"Redirection piece 150 x 50 to DN 100, 350 mm","On request","",null,null,null,null,null,null,220600,"Redirection piece 150 x 50 to DN 100, 350 mm","On request",false,null,220600,34.5,"On request","sur demande","på forespørgsel","op aanvraag","Umlenkstück 150 x 50 auf DN 100, 350 mm lang","Redirection piece 150 x 50 to DN 100, 350 mm","Déflecteur 150 x 50 à DN 100, longueur 350 mm","Redirection piece 150 x 50 to DN 100, 350 mm","Afbuigstuk 150 x 50 naar DN 100, 350 mm lang","Redirection piece 150 x 50 to DN 100, 350 mm","Redirection piece 150 x 50 to DN 100, 350 mm","Redirection piece 150 x 50 to DN 100, 350 mm","Redirection piece 150 x 50 to DN 100, 350 mm","Redirection piece 150 x 50 to DN 100, 350 mm","Redirection piece 150 x 50 to DN 100, 350 mm"]
[null,220601,"Redirection piece 150 x 50 to DN 125, 350 mm","On request","",null,null,null,null,null,null,220601,"Redirection piece 150 x 50 to DN 125, 350 mm","On request",false,null,220601,36,"On request","sur demande","på forespørgsel","op aanvraag","Umlenkstück 150 x 50 auf DN 125, 350 mm lang","Redirection piece 150 x 50 to DN 125, 350 mm","Déflecteur 150 x 50 à DN 125, longueur 350 mm","Redirection piece 150 x 50 to DN 125, 350 mm","Afbuigstuk 150 x 50 naar DN 125, 350 mm lang","Redirection piece 150 x 50 to DN 125, 350 mm","Redirection piece 150 x 50 to DN 125, 350 mm","Redirection piece 150 x 50 to DN 125, 350 mm","Redirection piece 150 x 50 to DN 125, 350 mm","Redirection piece 150 x 50 to DN 125, 350 mm","Redirection piece 150 x 50 to DN 125, 350 mm"]
[null,232987,"Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","On request","",null,null,null,null,null,null,232987,"Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","On request",false,null,232987,40.5,"On request","sur demande","på forespørgsel","op aanvraag","Umlenkstück 200 x 50 auf DN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","Afbuigstuk 2000 x 50 naarDN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang","Umlenkstück 2000 x 50 auf DN 125, 350 mm lang"]
[null,220602,"Redirection piece 100 x 50 to DN 100, Nippel","On request","",null,null,null,null,null,null,220602,"Redirection piece 100 x 50 to DN 100, Nippel","On request",false,null,220602,22.2,"On request","sur demande","på forespørgsel","op aanvraag","Umlenkstück 100 x 50 auf DN 100, Nippelende","Redirection piece 100 x 50 to DN 100, Nippel","Déflecteur 100 x 50 à DN 100, fin à mamelon","Redirection piece 100 x 50 to DN 100, Nippel","Afbuigstuk 100 x 50 naar DN 100, Nippeleinde","Redirection piece 100 x 50 to DN 100, Nippel","Redirection piece 100 x 50 to DN 100, Nippel","Redirection piece 100 x 50 to DN 100, Nippel","Redirection piece 100 x 50 to DN 100, Nippel","Redirection piece 100 x 50 to DN 100, Nippel","Redirection piece 100 x 50 to DN 100, Nippel"]
[null,220603,"Redirection piece 150 x 50 to DN 100, Nippel","On request","",null,null,null,null,null,null,220603,"Redirection piece 150 x 50 to DN 100, Nippel","On request",false,null,220603,23.1,"On request","sur demande","på forespørgsel","op aanvraag","Umlenkstück 150 x 50 auf DN 100, Nippelende","Redirection piece 150 x 50 to DN 100, Nippel","Déflecteur 150 x 50 à DN 100, fin à mamelon","Redirection piece 150 x 50 to DN 100, Nippel","Afbuigstuk 150 x 50 naar DN 100, Nippeleinde","Redirection piece 150 x 50 to DN 100, Nippel","Redirection piece 150 x 50 to DN 100, Nippel","Redirection piece 150 x 50 to DN 100, Nippel","Redirection piece 150 x 50 to DN 100, Nippel","Redirection piece 150 x 50 to DN 100, Nippel","Redirection piece 150 x 50 to DN 100, Nippel"]
[null,220604,"Redirection piece 150 x 50 to DN 125, Nippel","On request","",null,null,null,null,null,null,220604,"Redirection piece 150 x 50 to DN 125, Nippel","On request",false,null,220604,28,"On request","sur demande","på forespørgsel","op aanvraag","Umlenkstück 150 x 50 auf DN 125, Nippelende","Redirection piece 150 x 50 to DN 125, Nippel","Déflecteur 150 x 50 à DN 125, fin à mamelon","Redirection piece 150 x 50 to DN 125, Nippel","Afbuigstuk 150 x 50 naar DN 125, Nippeleinde","Redirection piece 150 x 50 to DN 125, Nippel","Redirection piece 150 x 50 to DN 125, Nippel","Redirection piece 150 x 50 to DN 125, Nippel","Redirection piece 150 x 50 to DN 125, Nippel","Redirection piece 150 x 50 to DN 125, Nippel","Redirection piece 150 x 50 to DN 125, Nippel"]
[null,220605,"Air distributor connection 100 x 50","On request","",null,null,null,null,null,null,220605,"Air distributor connection 100 x 50","On request",false,null,220605,38.5,"On request","sur demande","på forespørgsel","op aanvraag","Verteileranschluss 100 x 50, 2 Stück","Air distributor connection 100 x 50","Raccord de distributeur 100 x 50, 2 p.","Air distributor connection 100 x 50","Verdeleraansluiting 100 x 50, 2 stuks","Air distributor connection 100 x 50","Air distributor connection 100 x 50","Air distributor connection 100 x 50","Air distributor connection 100 x 50","Air distributor connection 100 x 50","Air distributor connection 100 x 50"]
[null,220606,"Air distributor connection 150 x 50","On request","",null,null,null,null,null,null,220606,"Air distributor connection 150 x 50","On request",false,null,220606,19.2,"On request","sur demande","på forespørgsel","op aanvraag","Verteileranschluss 150 x 50","Air distributor connection 150 x 50","Raccord de distributeur 150 x 50","Air distributor connection 150 x 50","Verdeleraansluiting 150 x 50","Air distributor connection 150 x 50","Air distributor connection 150 x 50","Air distributor connection 150 x 50","Air distributor connection 150 x 50","Air distributor connection 150 x 50","Air distributor connection 150 x 50"]
[null,221493,"Air distributor connection 200 x 50","On request","",null,null,null,null,null,null,221493,"Air distributor connection 200 x 50","On request",false,null,221493,19.899999999999999,"On request","sur demande","på forespørgsel","op aanvraag","Verteileranschluss 200 x 50","Air distributor connection 200 x 50","Raccord de distributeur 200 x 50","Air distributor connection 200 x 50","Verdeleraansluiting 200 x 50","Air distributor connection 200 x 50","Air distributor connection 200 x 50","Air distributor connection 200 x 50","Air distributor connection 200 x 50","Air distributor connection 200 x 50","Air distributor connection 200 x 50"]
[null,221223,"Branch piece horizontal DN 100 to 50x150","On request","",null,null,null,null,null,null,221223,"Branch piece horizontal DN 100 to 50x150","On request",false,null,221223,36,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück horizontal DN 100 auf 50x150","Branch piece horizontal DN 100 to 50x150","Pièce de dérivation horizontale DN 100 à 50x150","Branch piece horizontal DN 100 to 50x150","T-stuk horizontal DN 100 naar 50x150","Branch piece horizontal DN 100 to 50x150","Branch piece horizontal DN 100 to 50x150","Branch piece horizontal DN 100 to 50x150","Branch piece horizontal DN 100 to 50x150","Branch piece horizontal DN 100 to 50x150","Branch piece horizontal DN 100 to 50x150"]
[null,221224,"Branch piece horizontal DN 125 to 50x150","On request","",null,null,null,null,null,null,221224,"Branch piece horizontal DN 125 to 50x150","On request",false,null,221224,38.5,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück horizontal DN 125 auf 50x150","Branch piece horizontal DN 125 to 50x150","Pièce de dérivation horizontale DN 125 à 50x150","Branch piece horizontal DN 125 to 50x150","T-stuk horizontal DN 125 naar 50x150","Branch piece horizontal DN 125 to 50x150","Branch piece horizontal DN 125 to 50x150","Branch piece horizontal DN 125 to 50x150","Branch piece horizontal DN 125 to 50x150","Branch piece horizontal DN 125 to 50x150","Branch piece horizontal DN 125 to 50x150"]
[null,221225,"Branch piece horizontal DN 160 to 50x150 ","On request","",null,null,null,null,null,null,221225,"Branch piece horizontal DN 160 to 50x150 ","On request",false,null,221225,39.5,"On request","sur demande","på forespørgsel","op aanvraag","Abzweigstück horizontal DN 160 auf 50x150 ","Branch piece horizontal DN 160 to 50x150 ","Pièce de dérivation horizontale DN 160 à 50x150 ","Branch piece horizontal DN 160 to 50x150 ","T-stuk horizontal DN 160 naar 50x150 ","Branch piece horizontal DN 160 to 50x150 ","Branch piece horizontal DN 160 to 50x150 ","Branch piece horizontal DN 160 to 50x150 ","Branch piece horizontal DN 160 to 50x150 ","Branch piece horizontal DN 160 to 50x150 ","Branch piece horizontal DN 160 to 50x150 "]
[null,221226,"Adapter piece DN 100 to 50x100 ","On request","",null,null,null,null,null,null,221226,"Adapter piece DN 100 to 50x100 ","On request",false,null,221226,43,"On request","sur demande","på forespørgsel","op aanvraag","Übergangsstück DN 100 auf 50x100 ","Adapter piece DN 100 to 50x100 ","Pièce de transition DN 100 à 50x100 ","Adapter piece DN 100 to 50x100 ","Overgangsstuk DN 100 naar 50x100 ","Adapter piece DN 100 to 50x100 ","Adapter piece DN 100 to 50x100 ","Adapter piece DN 100 to 50x100 ","Adapter piece DN 100 to 50x100 ","Adapter piece DN 100 to 50x100 ","Adapter piece DN 100 to 50x100 "]
[null,221227,"Adapter piece DN 100 to 50x150","On request","",null,null,null,null,null,null,221227,"Adapter piece DN 100 to 50x150","On request",false,null,221227,43,"On request","sur demande","på forespørgsel","op aanvraag","Übergangsstück DN 100 auf 50x150","Adapter piece DN 100 to 50x150","Pièce de transition DN 100 à 50x150","Adapter piece DN 100 to 50x150","Overgangsstuk DN 100 naar 50x150","Adapter piece DN 100 to 50x150","Adapter piece DN 100 to 50x150","Adapter piece DN 100 to 50x150","Adapter piece DN 100 to 50x150","Adapter piece DN 100 to 50x150","Adapter piece DN 100 to 50x150"]
[null,221228,"Restricted fitting 150 x 50 to 100 x 50","On request","",null,null,null,null,null,null,221228,"Restricted fitting 150 x 50 to 100 x 50","On request",false,null,221228,22.2,"On request","sur demande","på forespørgsel","op aanvraag","Reduzierstück 150 x 50 auf 100 x 50","Restricted fitting 150 x 50 to 100 x 50","Raccord de réduction 150 x 50 à 100 x 50","Restricted fitting 150 x 50 to 100 x 50","Reduceerstuk 150 x 50 naar 100 x 50","Restricted fitting 150 x 50 to 100 x 50","Restricted fitting 150 x 50 to 100 x 50","Restricted fitting 150 x 50 to 100 x 50","Restricted fitting 150 x 50 to 100 x 50","Restricted fitting 150 x 50 to 100 x 50","Restricted fitting 150 x 50 to 100 x 50"]
[null,232988,"Reduzierstück 200 x 50 auf 150 x 50","On request","",null,null,null,null,null,null,232988,"Reduzierstück 200 x 50 auf 150 x 50","On request",false,null,232988,23.1,"On request","sur demande","på forespørgsel","op aanvraag","Reduzierstück 200 x 50 auf 150 x 50","Reduzierstück 200 x 50 auf 150 x 50","Reduzierstück 200 x 50 auf 150 x 50","Reduzierstück 200 x 50 auf 150 x 50","Reduceerstuk 200 x 50 naar 150 x 50","Reduzierstück 200 x 50 auf 150 x 50","Reduzierstück 200 x 50 auf 150 x 50","Reduzierstück 200 x 50 auf 150 x 50","Reduzierstück 200 x 50 auf 150 x 50","Reduzierstück 200 x 50 auf 150 x 50","Reduzierstück 200 x 50 auf 150 x 50"]
[null,221232,"End duct 100 x 50","On request","",null,null,null,null,null,null,221232,"End duct 100 x 50","On request",false,null,221232,4.9000000000000004,"On request","sur demande","på forespørgsel","op aanvraag","Enddeckel 100 x 50","End duct 100 x 50","Couvercle en extrémité 100 x 50","End duct 100 x 50","Einddeksel 100 x 50","End duct 100 x 50","End duct 100 x 50","End duct 100 x 50","End duct 100 x 50","End duct 100 x 50","End duct 100 x 50"]
[null,221233,"End duct 150 x 50","On request","",null,null,null,null,null,null,221233,"End duct 150 x 50","On request",false,null,221233,4.9000000000000004,"On request","sur demande","på forespørgsel","op aanvraag","Enddeckel 150 x 50","End duct 150 x 50","Couvercle en extrémité 150 x 50","End duct 150 x 50","Einddeksel 150 x 50","End duct 150 x 50","End duct 150 x 50","End duct 150 x 50","End duct 150 x 50","End duct 150 x 50","End duct 150 x 50"]
[null,230955,"Insulation hose DN 100, 4m","On request","",null,null,null,null,null,null,230955,"Insulation hose DN 100, 4m","On request",false,null,230955,79,"On request",80,"på forespørgsel","op aanvraag","Dämmschlauch DN 100, schwitzwasserisoliert, 4m","Insulation hose DN 100, 4m","Flexible isolant DN 100, isolé contre la condensation, 4 m","Insulation hose DN 100, 4m","Geïsoleerdeslang DN 100, condens isolerend, 4m","Insulation hose DN 100, 4m","Insulation hose DN 100, 4m","Insulation hose DN 100, 4m","Insulation hose DN 100, 4m","Insulation hose DN 100, 4m","Insulation hose DN 100, 4m"]
[null,159347,"Insulation hose DN 125, 4m","On request","",null,null,null,null,null,null,159347,"Insulation hose DN 125, 4m","On request",false,null,159347,96,"On request",85,"på forespørgsel","op aanvraag","Dämmschlauch DN 125, schwitzwasserisoliert, 4m","Insulation hose DN 125, 4m","Flexible isolant DN 125, isolé contre la condensation, 4 m","Insulation hose DN 125, 4m","Geïsoleerdeslang DN 125, condens isolerend, 4m","Insulation hose DN 125, 4m","Insulation hose DN 125, 4m","Insulation hose DN 125, 4m","Insulation hose DN 125, 4m","Insulation hose DN 125, 4m","Insulation hose DN 125, 4m"]
[null,170013,"Insulation hose DN 160, 4m","On request","",null,null,null,null,null,null,170013,"Insulation hose DN 160, 4m","On request",false,null,170013,156,"On request",95,"på forespørgsel","op aanvraag","Dämmschlauch DN 160, schwitzwasserisoliert, 4m","Insulation hose DN 160, 4m","Flexible isolant DN 160, isolé contre la condensation, 4 m","Insulation hose DN 160, 4m","Geïsoleerdeslang DN 160, condens isolerend, 4m","Insulation hose DN 160, 4m","Insulation hose DN 160, 4m","Insulation hose DN 160, 4m","Insulation hose DN 160, 4m","Insulation hose DN 160, 4m","Insulation hose DN 160, 4m"]
[null,159348,"Punched tape 10m","On request","",null,null,null,null,null,null,159348,"Punched tape 10m","On request",false,null,159348,19.399999999999999,"On request",20,"på forespørgsel","op aanvraag","Stahllochband verzinkt, 10m","Punched tape 10m","Ruban acier percé zingué, 10 m","Punched tape 10m","Geperforeerde staalband verzinkt, 10m","Punched tape 10m","Punched tape 10m","Punched tape 10m","Punched tape 10m","Punched tape 10m","Punched tape 10m"]
[null,227948,"Duct tape 10m","On request","",null,null,null,null,null,null,227948,"Duct tape 10m","On request",false,null,227948,20.100000000000001,"On request",20,"på forespørgsel","op aanvraag","Klebeband, alukaschiert mit Schutzfolie, 10m","Duct tape 10m","Ruban adhésif, laminé alu avec film protecteur, 10 m","Duct tape 10m","Kleefband, Gealuminiseerd met beschermfolie, 10m","Duct tape 10m","Duct tape 10m","Duct tape 10m","Duct tape 10m","Duct tape 10m","Duct tape 10m"]
[null,170015,"Heater battery DN 160","On request","",null,null,null,null,null,null,170015,"Heater battery DN 160","On request",false,null,170015,612,"On request",815,"på forespørgsel","op aanvraag","Heizregister DN 160","Heater battery DN 160","Registre de chauffage DN 160","Heater battery DN 160","Verwarmingstregister DN 160","Heater battery DN 160","Heater battery DN 160","Heater battery DN 160","Heater battery DN 160","Heater battery DN 160","Heater battery DN 160"]
[null,233015,"Filterbox Grobfilter DN 160","On request","",null,null,null,null,null,null,233015,"Filterbox Grobfilter DN 160","On request",false,null,233015,85,"On request",85,"på forespørgsel","op aanvraag","Filterbox Grobfilter DN 160","Filterbox Grobfilter DN 160","Filterbox Grobfilter DN 160","Filterbox Grobfilter DN 160","Filterbox Groffilter DN 160","Filterbox Grobfilter DN 160","Filterbox Grobfilter DN 160","Filterbox Grobfilter DN 160","Filterbox Grobfilter DN 160","Filterbox Grobfilter DN 160","Filterbox Grobfilter DN 160"]
[null,233028,"Filtermattenset G4, 5 Stück","On request","",null,null,null,null,null,null,233028,"Filtermattenset G4, 5 Stück","On request",false,null,233028,37,"On request",90,"på forespørgsel","op aanvraag","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 stuks","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 Stück","Filtermattenset G4, 5 Stück"]
[null,233016,"Filterbox Feinfilter DN 160","On request","",null,null,null,null,null,null,233016,"Filterbox Feinfilter DN 160","On request",false,null,233016,155,"On request",315,"på forespørgsel","op aanvraag","Filterbox Feinfilter DN 160","Filterbox Feinfilter DN 160","Filterbox Feinfilter DN 160","Filterbox Feinfilter DN 160","Filterbox Fijnfilter DN 160","Filterbox Feinfilter DN 160","Filterbox Feinfilter DN 160","Filterbox Feinfilter DN 160","Filterbox Feinfilter DN 160","Filterbox Feinfilter DN 160","Filterbox Feinfilter DN 160"]
[null,171475,"Filter cassette F5 for filter box DN 160","On request","",null,null,null,null,null,null,171475,"Filter cassette F5 for filter box DN 160","On request",false,null,171475,29.5,"On request","sur demande","på forespørgsel","op aanvraag","Filterkassette F5 für Filterbox DN 160","Filter cassette F5 for filter box DN 160","Cartouche à filtre F5 pour boîte à filtre DN 160","Filter cassette F5 for filter box DN 160","Filtercassette F5 voor filterbox DN 160","Filter cassette F5 for filter box DN 160","Filter cassette F5 for filter box DN 160","Filter cassette F5 for filter box DN 160","Filter cassette F5 for filter box DN 160","Filter cassette F5 for filter box DN 160","Filter cassette F5 for filter box DN 160"]
[null,171474,"Filter cassette F7 for filter box DN 160","On request","",null,null,null,null,null,null,171474,"Filter cassette F7 for filter box DN 160","On request",false,null,171474,33.5,"On request",60,"på forespørgsel","op aanvraag","Filterkassette F7 für Filterbox DN 160","Filter cassette F7 for filter box DN 160","Cartouche à filtre F7 pour boîte à filtre DN 160","Filter cassette F7 for filter box DN 160","Filterkassette F7 voor filterbox DN 160","Filter cassette F7 for filter box DN 160","Filter cassette F7 for filter box DN 160","Filter cassette F7 for filter box DN 160","Filter cassette F7 for filter box DN 160","Filter cassette F7 for filter box DN 160","Filter cassette F7 for filter box DN 160"]
[null,233868,"Filterkassette F7-LP für Filterbox DN 160","On request","",null,null,null,null,null,null,233868,"Filterkassette F7-LP für Filterbox DN 160","On request",false,null,233868,43.5,"On request","sur demande","på forespørgsel","op aanvraag","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP voor filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160","Filterkassette F7-LP für Filterbox DN 160"]
[null,233869,"Filterkassette F9 für Filterbox DN 160","On request","",null,null,null,null,null,null,233869,"Filterkassette F9 für Filterbox DN 160","On request",false,null,233869,52,"On request","sur demande","på forespørgsel","op aanvraag","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 voor filterbox DN 160","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 für Filterbox DN 160","Filterkassette F9 für Filterbox DN 160"]
[null,233870,"Filterkassette VOC für Filterbox DN 160","On request","",null,null,null,null,null,null,233870,"Filterkassette VOC für Filterbox DN 160","On request",false,null,233870,139,"On request","sur demande","på forespørgsel","op aanvraag","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC voor filterbox DN 160","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC für Filterbox DN 160","Filterkassette VOC für Filterbox DN 160"]
[null,274166,"Batterie-Wechselrichter WRS SB 3600 SE","On request","",null,null,null,null,null,null,274166,"Batterie-Wechselrichter WRS SB 3600 SE","On request",false,null,274166,8000,"On request","sur demande","på forespørgsel","op aanvraag","Batterie-Wechselrichter WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE","Omvormer WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE","Batterie-Wechselrichter WRS SB 3600 SE"]
[null,274167,"Batterie-Wechselrichter WRS SB 5000 SE","On request","",null,null,null,null,null,null,274167,"Batterie-Wechselrichter WRS SB 5000 SE","On request",false,null,274167,8450,"On request","sur demande","på forespørgsel","op aanvraag","Batterie-Wechselrichter WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE","Omvormer WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE","Batterie-Wechselrichter WRS SB 5000 SE"]
[null,273344,"Wechselrichter WRS STP 15000 TL","On request","",null,null,null,null,null,null,273344,"Wechselrichter WRS STP 15000 TL","On request",false,null,273344,5450,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 15000 TL","Wechselrichter WRS STP 15000 TL","Wechselrichter WRS STP 15000 TL","Wechselrichter WRS STP 15000 TL","Omvormer Sunny Tripower WRS STP15000TL","Wechselrichter WRS STP 15000 TL","Wechselrichter WRS STP 15000 TL","Wechselrichter WRS STP 15000 TL","Wechselrichter WRS STP 15000 TL","Wechselrichter WRS STP 15000 TL","Wechselrichter WRS STP 15000 TL"]
[null,273343,"Wechselrichter WRS STP 17000 TL","On request","",null,null,null,null,null,null,273343,"Wechselrichter WRS STP 17000 TL","On request",false,null,273343,5850,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 17000 TL","Wechselrichter WRS STP 17000 TL","Wechselrichter WRS STP 17000 TL","Wechselrichter WRS STP 17000 TL","Omvormer Sunny Tripower WRS STP17000TL","Wechselrichter WRS STP 17000 TL","Wechselrichter WRS STP 17000 TL","Wechselrichter WRS STP 17000 TL","Wechselrichter WRS STP 17000 TL","Wechselrichter WRS STP 17000 TL","Wechselrichter WRS STP 17000 TL"]
[null,273595,"Wechselrichter WRS STP 5000 TL","On request","",null,null,null,null,null,null,273595,"Wechselrichter WRS STP 5000 TL","On request",false,null,273595,2700,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 5000 TL","Wechselrichter WRS STP 5000 TL","Wechselrichter WRS STP 5000 TL","Wechselrichter WRS STP 5000 TL","Omvormer Sunny Tripower WRS STP5000TL","Wechselrichter WRS STP 5000 TL","Wechselrichter WRS STP 5000 TL","Wechselrichter WRS STP 5000 TL","Wechselrichter WRS STP 5000 TL","Wechselrichter WRS STP 5000 TL","Wechselrichter WRS STP 5000 TL"]
[null,273357,"Wechselrichter WRS STP 6000 TL","On request","",null,null,null,null,null,null,273357,"Wechselrichter WRS STP 6000 TL","On request",false,null,273357,3000,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 6000 TL","Wechselrichter WRS STP 6000 TL","Wechselrichter WRS STP 6000 TL","Wechselrichter WRS STP 6000 TL","Omvormer Sunny Tripower WRS STP6000TL","Wechselrichter WRS STP 6000 TL","Wechselrichter WRS STP 6000 TL","Wechselrichter WRS STP 6000 TL","Wechselrichter WRS STP 6000 TL","Wechselrichter WRS STP 6000 TL","Wechselrichter WRS STP 6000 TL"]
[null,273356,"Wechselrichter WRS STP 7000 TL","On request","",null,null,null,null,null,null,273356,"Wechselrichter WRS STP 7000 TL","On request",false,null,273356,3200,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 7000 TL","Wechselrichter WRS STP 7000 TL","Wechselrichter WRS STP 7000 TL","Wechselrichter WRS STP 7000 TL","Omvormer Sunny Tripower WRS STP7000TL","Wechselrichter WRS STP 7000 TL","Wechselrichter WRS STP 7000 TL","Wechselrichter WRS STP 7000 TL","Wechselrichter WRS STP 7000 TL","Wechselrichter WRS STP 7000 TL","Wechselrichter WRS STP 7000 TL"]
[null,273355,"Wechselrichter WRS STP 8000 TL","On request","",null,null,null,null,null,null,273355,"Wechselrichter WRS STP 8000 TL","On request",false,null,273355,3400,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 8000 TL","Wechselrichter WRS STP 8000 TL","Wechselrichter WRS STP 8000 TL","Wechselrichter WRS STP 8000 TL","Omvormer Sunny Tripower WRS STP8000TL","Wechselrichter WRS STP 8000 TL","Wechselrichter WRS STP 8000 TL","Wechselrichter WRS STP 8000 TL","Wechselrichter WRS STP 8000 TL","Wechselrichter WRS STP 8000 TL","Wechselrichter WRS STP 8000 TL"]
[null,273354,"Wechselrichter WRS STP 9000 TL","On request","",null,null,null,null,null,null,273354,"Wechselrichter WRS STP 9000 TL","On request",false,null,273354,3600,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 9000 TL","Wechselrichter WRS STP 9000 TL","Wechselrichter WRS STP 9000 TL","Wechselrichter WRS STP 9000 TL","Omvormer Sunny Tripower  WRS STP9000TL","Wechselrichter WRS STP 9000 TL","Wechselrichter WRS STP 9000 TL","Wechselrichter WRS STP 9000 TL","Wechselrichter WRS STP 9000 TL","Wechselrichter WRS STP 9000 TL","Wechselrichter WRS STP 9000 TL"]
[null,273596,"Wechselrichter WRS SB 3000 TL","On request","",null,null,null,null,null,null,273596,"Wechselrichter WRS SB 3000 TL","On request",false,null,273596,1925,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 3000 TL","Wechselrichter WRS SB 3000 TL","Wechselrichter WRS SB 3000 TL","Wechselrichter WRS SB 3000 TL","Omvormer Sunny Boy WRS SB 3000TL","Wechselrichter WRS SB 3000 TL","Wechselrichter WRS SB 3000 TL","Wechselrichter WRS SB 3000 TL","Wechselrichter WRS SB 3000 TL","Wechselrichter WRS SB 3000 TL","Wechselrichter WRS SB 3000 TL"]
[null,273589,"Wechselrichter WRS SB 3600 TL","On request","",null,null,null,null,null,null,273589,"Wechselrichter WRS SB 3600 TL","On request",false,null,273589,1950,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 3600 TL","Wechselrichter WRS SB 3600 TL","Wechselrichter WRS SB 3600 TL","Wechselrichter WRS SB 3600 TL","Omvormer Sunny Boy WRS SB 3600TL","Wechselrichter WRS SB 3600 TL","Wechselrichter WRS SB 3600 TL","Wechselrichter WRS SB 3600 TL","Wechselrichter WRS SB 3600 TL","Wechselrichter WRS SB 3600 TL","Wechselrichter WRS SB 3600 TL"]
[null,273588,"Wechselrichter WRS SB 4000 TL","On request","",null,null,null,null,null,null,273588,"Wechselrichter WRS SB 4000 TL","On request",false,null,273588,2050,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 4000 TL","Wechselrichter WRS SB 4000 TL","Wechselrichter WRS SB 4000 TL","Wechselrichter WRS SB 4000 TL","Omvormer Sunny Boy WRS SB 4000TL","Wechselrichter WRS SB 4000 TL","Wechselrichter WRS SB 4000 TL","Wechselrichter WRS SB 4000 TL","Wechselrichter WRS SB 4000 TL","Wechselrichter WRS SB 4000 TL","Wechselrichter WRS SB 4000 TL"]
[null,273587,"Wechselrichter WRS SB 5000 TL","On request","",null,null,null,null,null,null,273587,"Wechselrichter WRS SB 5000 TL","On request",false,null,273587,2350,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 5000 TL","Wechselrichter WRS SB 5000 TL","Wechselrichter WRS SB 5000 TL","Wechselrichter WRS SB 5000 TL","Omvormer Sunny Boy WRS SB 5000TL","Wechselrichter WRS SB 5000 TL","Wechselrichter WRS SB 5000 TL","Wechselrichter WRS SB 5000 TL","Wechselrichter WRS SB 5000 TL","Wechselrichter WRS SB 5000 TL","Wechselrichter WRS SB 5000 TL"]
[null,273591,"Wechselrichter WRS SB 2500 TLST","On request","",null,null,null,null,null,null,273591,"Wechselrichter WRS SB 2500 TLST","On request",false,null,273591,1800,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 2500 TLST","Wechselrichter WRS SB 2500 TLST","Wechselrichter WRS SB 2500 TLST","Wechselrichter WRS SB 2500 TLST","Omvormer Sunny Boy WRS SB 2500TLST","Wechselrichter WRS SB 2500 TLST","Wechselrichter WRS SB 2500 TLST","Wechselrichter WRS SB 2500 TLST","Wechselrichter WRS SB 2500 TLST","Wechselrichter WRS SB 2500 TLST","Wechselrichter WRS SB 2500 TLST"]
[null,273590,"Wechselrichter WRS SB 3000 TLST","On request","",null,null,null,null,null,null,273590,"Wechselrichter WRS SB 3000 TLST","On request",false,null,273590,1900,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 3000 TLST","Wechselrichter WRS SB 3000 TLST","Wechselrichter WRS SB 3000 TLST","Wechselrichter WRS SB 3000 TLST","Omvormer Sunny Boy WRS SB 3000TLST","Wechselrichter WRS SB 3000 TLST","Wechselrichter WRS SB 3000 TLST","Wechselrichter WRS SB 3000 TLST","Wechselrichter WRS SB 3000 TLST","Wechselrichter WRS SB 3000 TLST","Wechselrichter WRS SB 3000 TLST"]
[null,273594,"Wechselrichter WRS SB 1300 TL","On request","",null,null,null,null,null,null,273594,"Wechselrichter WRS SB 1300 TL","On request",false,null,273594,1050,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 1300 TL","Wechselrichter WRS SB 1300 TL","Wechselrichter WRS SB 1300 TL","Wechselrichter WRS SB 1300 TL","Omvormer Sunny Boy WRS SB 1300TL","Wechselrichter WRS SB 1300 TL","Wechselrichter WRS SB 1300 TL","Wechselrichter WRS SB 1300 TL","Wechselrichter WRS SB 1300 TL","Wechselrichter WRS SB 1300 TL","Wechselrichter WRS SB 1300 TL"]
[null,273593,"Wechselrichter WRS SB 1600 TL","On request",{"$f":"IF(O768=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,273593,"Wechselrichter WRS SB 1600 TL","On request",false,null,273593,1150,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 1600 TL","Wechselrichter WRS SB 1600 TL","Wechselrichter WRS SB 1600 TL","Wechselrichter WRS SB 1600 TL","Omvormer Sunny Boy WRS SB 1600TL","Wechselrichter WRS SB 1600 TL","Wechselrichter WRS SB 1600 TL","Wechselrichter WRS SB 1600 TL","Wechselrichter WRS SB 1600 TL","Wechselrichter WRS SB 1600 TL","Wechselrichter WRS SB 1600 TL"]
[null,273592,"Wechselrichter WRS SB 2100 TL","On request","",null,null,null,null,null,null,273592,"Wechselrichter WRS SB 2100 TL","On request",false,null,273592,1300,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS SB 2100 TL","Wechselrichter WRS SB 2100 TL","Wechselrichter WRS SB 2100 TL","Wechselrichter WRS SB 2100 TL","Omvormer Sunny Boy  WRS SB 2100TL","Wechselrichter WRS SB 2100 TL","Wechselrichter WRS SB 2100 TL","Wechselrichter WRS SB 2100 TL","Wechselrichter WRS SB 2100 TL","Wechselrichter WRS SB 2100 TL","Wechselrichter WRS SB 2100 TL"]
[null,273679,"Sunny Home Manager ZS HM","On request","",null,null,null,null,null,null,273679,"Sunny Home Manager ZS HM","On request",{"$f":"IF(AND(B770=L770,C770=M770,D770=N770),FALSE,TRUE)","v":false},null,273679,470,"On request","sur demande","på forespørgsel","op aanvraag","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM","Sunny Home Manager ZS HM"]
[null,273680,"Sunny Home Manager ZS HM START","On request","",null,null,null,null,null,null,273680,"Sunny Home Manager ZS HM START","On request",false,null,273680,740,"On request","sur demande","på forespørgsel","op aanvraag","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START","Sunny Home Manager ZS HM START"]
[null,273681,"Bluetooth-Funksteckdose für Sunny Home Manager","On request","",null,null,null,null,null,null,273681,"Bluetooth-Funksteckdose für Sunny Home Manager","On request",false,null,273681,183,"On request","sur demande","på forespørgsel","op aanvraag","Bluetooth-Funksteckdose für Sunny Home Manager","Bluetooth-Funksteckdose für Sunny Home Manager","Bluetooth-Funksteckdose für Sunny Home Manager","Bluetooth-Funksteckdose für Sunny Home Manager","Radiografische insteekdoos (Bluetooth) ZS BT-SOCKET","Bluetooth-Funksteckdose für Sunny Home Manager","Bluetooth-Funksteckdose für Sunny Home Manager","Bluetooth-Funksteckdose für Sunny Home Manager","Bluetooth-Funksteckdose für Sunny Home Manager","Bluetooth-Funksteckdose für Sunny Home Manager","Bluetooth-Funksteckdose für Sunny Home Manager"]
[null,274170,"Smart Energy Meter für Sunny Home Manager","On request","",null,null,null,null,null,null,274170,"Smart Energy Meter für Sunny Home Manager","On request",false,null,274170,460,"On request","sur demande","på forespørgsel","op aanvraag","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter ZS EM","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter für Sunny Home Manager","Smart Energy Meter für Sunny Home Manager"]
[null,273682,"Auslesekopf D0 Meteradapter","On request","",null,null,null,null,null,null,273682,"Auslesekopf D0 Meteradapter","On request",false,null,273682,95,"On request","sur demande","på forespørgsel","op aanvraag","Auslesekopf D0 Meteradapter","Auslesekopf D0 Meteradapter","Auslesekopf D0 Meteradapter","Auslesekopf D0 Meteradapter","DO-Meteradapter (Uitleeskop Teller) ZS HM-DO","Auslesekopf D0 Meteradapter","Auslesekopf D0 Meteradapter","Auslesekopf D0 Meteradapter","Auslesekopf D0 Meteradapter","Auslesekopf D0 Meteradapter","Auslesekopf D0 Meteradapter"]
[null,273683,"Webbox Bluetooth","On request","",null,null,null,null,null,null,273683,"Webbox Bluetooth","On request",false,null,273683,633,"On request","sur demande","på forespørgsel","op aanvraag","Webbox Bluetooth","Webbox Bluetooth","Webbox Bluetooth","Webbox Bluetooth","Webbox Bluetooth ZS","Webbox Bluetooth","Webbox Bluetooth","Webbox Bluetooth","Webbox Bluetooth","Webbox Bluetooth","Webbox Bluetooth"]
[null,273678,"Netz- und Anlagenschutz SMA","On request","",null,null,null,null,null,null,273678,"Netz- und Anlagenschutz SMA","On request",false,null,273678,624,"On request","sur demande","på forespørgsel","op aanvraag","Netz- und Anlagenschutz SMA","Netz- und Anlagenschutz SMA","Netz- und Anlagenschutz SMA","Netz- und Anlagenschutz SMA","Grid Gate ZS","Netz- und Anlagenschutz SMA","Netz- und Anlagenschutz SMA","Netz- und Anlagenschutz SMA","Netz- und Anlagenschutz SMA","Netz- und Anlagenschutz SMA","Netz- und Anlagenschutz SMA"]
[null,273677,"Cluster Controller","On request","",null,null,null,null,null,null,273677,"Cluster Controller","On request",false,null,273677,1462,"On request","sur demande","på forespørgsel","op aanvraag","Cluster Controller","Cluster Controller","Cluster Controller","Cluster Controller","Cluster Controller ZS","Cluster Controller","Cluster Controller","Cluster Controller","Cluster Controller","Cluster Controller","Cluster Controller"]
[null,273812,"Netzteil für Cluster Controller","On request","",null,null,null,null,null,null,273812,"Netzteil für Cluster Controller","On request",false,null,273812,74,"On request","sur demande","på forespørgsel","op aanvraag","Netzteil für Cluster Controller","Netzteil für Cluster Controller","Netzteil für Cluster Controller","Netzteil für Cluster Controller","Cluster Controller Netdeel ZS","Netzteil für Cluster Controller","Netzteil für Cluster Controller","Netzteil für Cluster Controller","Netzteil für Cluster Controller","Netzteil für Cluster Controller","Netzteil für Cluster Controller"]
[null,274164,"Teleskopschiene 2,0 m","On request","",null,null,null,null,null,null,274164,"Teleskopschiene 2,0 m","On request",false,null,274164,12.6,"On request","sur demande","på forespørgsel","op aanvraag","Teleskopschiene 2,0 m","Teleskopschiene 2,0 m","Teleskopschiene 2,0 m","Teleskopschiene 2,0 m","Telescoopverlenging 0,6 m","Teleskopschiene 2,0 m","Teleskopschiene 2,0 m","Teleskopschiene 2,0 m","Teleskopschiene 2,0 m","Teleskopschiene 2,0 m","Teleskopschiene 2,0 m"]
[null,273304,"Schienenverbinder 2,0 m","On request","",null,null,null,null,null,null,273304,"Schienenverbinder 2,0 m","On request",false,null,273304,3.7,"On request","sur demande","på forespørgsel","op aanvraag","Schienenverbinder 2,0 m","Schienenverbinder 2,0 m","Schienenverbinder 2,0 m","Schienenverbinder 2,0 m","Verbinderprofiel","Schienenverbinder 2,0 m","Schienenverbinder 2,0 m","Schienenverbinder 2,0 m","Schienenverbinder 2,0 m","Schienenverbinder 2,0 m","Schienenverbinder 2,0 m"]
[null,273324,"Endhalter, 10 Stück","On request","",null,null,null,null,null,null,273324,"Endhalter, 10 Stück","On request",false,null,273324,8.5,"On request","sur demande","på forespørgsel","op aanvraag","Modulhalter Endhalter, 10 Stück","Endhalter, 10 Stück","Endhalter, 10 Stück","Endhalter, 10 Stück","Eindhouder, 10 stuks","Endhalter, 10 Stück","Endhalter, 10 Stück","Endhalter, 10 Stück","Endhalter, 10 Stück","Endhalter, 10 Stück","Endhalter, 10 Stück"]
[null,273360,"Modulhalter Mittelklemme, 40 Sück","On request","",null,null,null,null,null,null,273360,"Modulhalter Mittelklemme, 40 Sück","On request",false,null,273360,29.5,"On request","sur demande","på forespørgsel","op aanvraag","Modulhalter Mittelklemme, 40 Sück","Modulhalter Mittelklemme, 40 Sück","Modulhalter Mittelklemme, 40 Sück","Modulhalter Mittelklemme, 40 Sück","Modulehouder middelklemmen, 40 stuks","Modulhalter Mittelklemme, 40 Sück","Modulhalter Mittelklemme, 40 Sück","Modulhalter Mittelklemme, 40 Sück","Modulhalter Mittelklemme, 40 Sück","Modulhalter Mittelklemme, 40 Sück","Modulhalter Mittelklemme, 40 Sück"]
[null,273326,"Kreuzschienenverbinder, 20 Stück","On request","",null,null,null,null,null,null,273326,"Kreuzschienenverbinder, 20 Stück","On request",false,null,273326,15,"On request","sur demande","på forespørgsel","op aanvraag","Kreuzschienenverbinder, 20 Stück","Kreuzschienenverbinder, 20 Stück","Kreuzschienenverbinder, 20 Stück","Kreuzschienenverbinder, 20 Stück","Rail connector kruis, 20 stuks","Kreuzschienenverbinder, 20 Stück","Kreuzschienenverbinder, 20 Stück","Kreuzschienenverbinder, 20 Stück","Kreuzschienenverbinder, 20 Stück","Kreuzschienenverbinder, 20 Stück","Kreuzschienenverbinder, 20 Stück"]
[null,273327,"Arretierungsclip, 20 Stück","On request","",null,null,null,null,null,null,273327,"Arretierungsclip, 20 Stück","On request",false,null,273327,8,"On request","sur demande","på forespørgsel","op aanvraag","Arretierungsclip, 20 Stück","Arretierungsclip, 20 Stück","Arretierungsclip, 20 Stück","Arretierungsclip, 20 Stück","Borgingsclip, 20 stuks","Arretierungsclip, 20 Stück","Arretierungsclip, 20 Stück","Arretierungsclip, 20 Stück","Arretierungsclip, 20 Stück","Arretierungsclip, 20 Stück","Arretierungsclip, 20 Stück"]
[null,274146,"Sparrenanker Pfannendach","On request","",null,null,null,null,null,null,274146,"Sparrenanker Pfannendach","On request",false,null,274146,7.4,"On request","sur demande","på forespørgsel","op aanvraag","Dachbefestigung Pfannendach","Sparrenanker Pfannendach","Sparrenanker Pfannendach","Sparrenanker Pfannendach","Sparrenanker pannendak","Sparrenanker Pfannendach","Sparrenanker Pfannendach","Sparrenanker Pfannendach","Sparrenanker Pfannendach","Sparrenanker Pfannendach","Sparrenanker Pfannendach"]
[null,274148,"Dachbefestigung Pfannendach Variabel","On request","",null,null,null,null,null,null,274148,"Dachbefestigung Pfannendach Variabel","On request",false,null,274148,8.9,"On request","sur demande","på forespørgsel","op aanvraag","Dachbefestigung Pfannendach Variabel","Dachbefestigung Pfannendach Variabel","Dachbefestigung Pfannendach Variabel","Dachbefestigung Pfannendach Variabel","Sparrenanker pannendak vario","Dachbefestigung Pfannendach Variabel","Dachbefestigung Pfannendach Variabel","Dachbefestigung Pfannendach Variabel","Dachbefestigung Pfannendach Variabel","Dachbefestigung Pfannendach Variabel","Dachbefestigung Pfannendach Variabel"]
[null,273931,"Dachhaken Biberschwanzpfanne","On request","",null,null,null,null,null,null,273931,"Dachhaken Biberschwanzpfanne","On request",false,null,273931,10.8,"On request","sur demande","på forespørgsel","op aanvraag","Dachbefestigung Biberschwanzpfanne","Dachhaken Biberschwanzpfanne","Dachhaken Biberschwanzpfanne","Dachhaken Biberschwanzpfanne","Dakhaken Zwaluwstaartpannen","Dachhaken Biberschwanzpfanne","Dachhaken Biberschwanzpfanne","Dachhaken Biberschwanzpfanne","Dachhaken Biberschwanzpfanne","Dachhaken Biberschwanzpfanne","Dachhaken Biberschwanzpfanne"]
[null,273790,"Dachhaken Schieferdach","On request","",null,null,null,null,null,null,273790,"Dachhaken Schieferdach","On request",false,null,273790,10.25,"On request","sur demande","på forespørgsel","op aanvraag","Dachbefestigung Schieferdach","Dachhaken Schieferdach","Dachhaken Schieferdach","Dachhaken Schieferdach","Dakhaken leiendak","Dachhaken Schieferdach","Dachhaken Schieferdach","Dachhaken Schieferdach","Dachhaken Schieferdach","Dachhaken Schieferdach","Dachhaken Schieferdach"]
[null,274199,"Trapezblechschiene","On request","",null,null,null,null,null,null,274199,"Trapezblechschiene","On request",false,null,274199,4.12,"On request","sur demande","på forespørgsel","op aanvraag","Trapezblechschiene","Trapezblechschiene","Trapezblechschiene","Trapezblechschiene","Dakplaatklem","Trapezblechschiene","Trapezblechschiene","Trapezblechschiene","Trapezblechschiene","Trapezblechschiene","Trapezblechschiene"]
[null,273338,"Holzschraube Senkkopf, 100 Stück","On request","",null,null,null,null,null,null,273338,"Holzschraube Senkkopf, 100 Stück","On request",false,null,273338,19.2,"On request","sur demande","på forespørgsel","op aanvraag","Holzschraube Senkkopf, 100 Stück","Holzschraube Senkkopf, 100 Stück","Holzschraube Senkkopf, 100 Stück","Holzschraube Senkkopf, 100 Stück","Houtschroef verzonken kop, 100 stuks","Holzschraube Senkkopf, 100 Stück","Holzschraube Senkkopf, 100 Stück","Holzschraube Senkkopf, 100 Stück","Holzschraube Senkkopf, 100 Stück","Holzschraube Senkkopf, 100 Stück","Holzschraube Senkkopf, 100 Stück"]
[null,273339,"Holzschraube Torx Tellerkopf, 100 Stück","On request","",null,null,null,null,null,null,273339,"Holzschraube Torx Tellerkopf, 100 Stück","On request",false,null,273339,54,"On request","sur demande","på forespørgsel","op aanvraag","Holzschraube Tellerkopf, 100 Stück","Holzschraube Torx Tellerkopf, 100 Stück","Holzschraube Torx Tellerkopf, 100 Stück","Holzschraube Torx Tellerkopf, 100 Stück","Houtschroef Torx bollekop, 100 stuks","Holzschraube Torx Tellerkopf, 100 Stück","Holzschraube Torx Tellerkopf, 100 Stück","Holzschraube Torx Tellerkopf, 100 Stück","Holzschraube Torx Tellerkopf, 100 Stück","Holzschraube Torx Tellerkopf, 100 Stück","Holzschraube Torx Tellerkopf, 100 Stück"]
[null,273340,"Stockschraube M10x200, 20 Stück","On request",{"$f":"IF(O792=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,273340,"Stockschraube M10x200, 20 Stück","On request",false,null,273340,86,"On request","sur demande","på forespørgsel","op aanvraag","Stockschraube M10x200, 20 Stück","Stockschraube M10x200, 20 Stück","Stockschraube M10x200, 20 Stück","Stockschraube M10x200, 20 Stück","Stokschroeven M10x200, 20 stuks","Stockschraube M10x200, 20 Stück","Stockschraube M10x200, 20 Stück","Stockschraube M10x200, 20 Stück","Stockschraube M10x200, 20 Stück","Stockschraube M10x200, 20 Stück","Stockschraube M10x200, 20 Stück"]
[null,273341,"Stockschraube M12x250, 20 Stück","On request","",null,null,null,null,null,null,273341,"Stockschraube M12x250, 20 Stück","On request",false,null,273341,121,"On request","sur demande","på forespørgsel","op aanvraag","Stockschraube M12x250, 20 Stück","Stockschraube M12x250, 20 Stück","Stockschraube M12x250, 20 Stück","Stockschraube M12x250, 20 Stück","Stokschroeven M12x250, 20 stuks","Stockschraube M12x250, 20 Stück","Stockschraube M12x250, 20 Stück","Stockschraube M12x250, 20 Stück","Stockschraube M12x250, 20 Stück","Stockschraube M12x250, 20 Stück","Stockschraube M12x250, 20 Stück"]
[null,273283,"Montagewanne Flachdach CS Plus","On request","",null,null,null,null,null,null,273283,"Montagewanne Flachdach CS Plus","On request",false,null,273283,83,"On request","sur demande","på forespørgsel","op aanvraag","Montagewanne Flachdach CS Plus","Montagewanne Flachdach CS Plus","Montagewanne Flachdach CS Plus","Montagewanne Flachdach CS Plus","Montagebak CS (15°)","Montagewanne Flachdach CS Plus","Montagewanne Flachdach CS Plus","Montagewanne Flachdach CS Plus","Montagewanne Flachdach CS Plus","Montagewanne Flachdach CS Plus","Montagewanne Flachdach CS Plus"]
[null,273284,"Windführung für Montagewanne CS Plus","On request","",null,null,null,null,null,null,273284,"Windführung für Montagewanne CS Plus","On request",{"$f":"IF(AND(B795=L795,C795=M795,D795=N795),FALSE,TRUE)","v":false},null,273284,41,"On request","sur demande","på forespørgsel","op aanvraag","Windführung für Montagewanne CS Plus","Windführung für Montagewanne CS Plus","Windführung für Montagewanne CS Plus","Windführung für Montagewanne CS Plus","Streamliner voor Montageframe CS","Windführung für Montagewanne CS Plus","Windführung für Montagewanne CS Plus","Windführung für Montagewanne CS Plus","Windführung für Montagewanne CS Plus","Windführung für Montagewanne CS Plus","Windführung für Montagewanne CS Plus"]
[null,273318,"Solarleitung 1x4 mm², 50m","On request","",null,null,null,null,null,null,273318,"Solarleitung 1x4 mm², 50m","On request",false,null,273318,49,"On request","sur demande","på forespørgsel","op aanvraag","Solarleitung 1x4 mm², 50m","Solarleitung 1x4 mm², 50m","Solarleitung 1x4 mm², 50m","Solarleitung 1x4 mm², 50m","Solarleiding 1x4 mm², 50m","Solarleitung 1x4 mm², 50m","Solarleitung 1x4 mm², 50m","Solarleitung 1x4 mm², 50m","Solarleitung 1x4 mm², 50m","Solarleitung 1x4 mm², 50m","Solarleitung 1x4 mm², 50m"]
[null,273319,"Solarleitung 1x4 mm², 100m","On request","",null,null,null,null,null,null,273319,"Solarleitung 1x4 mm², 100m","On request",false,null,273319,98,"On request","sur demande","på forespørgsel","op aanvraag","Solarleitung 1x4 mm², 100m","Solarleitung 1x4 mm², 100m","Solarleitung 1x4 mm², 100m","Solarleitung 1x4 mm², 100m","Solarleiding 1x4 mm², 100m","Solarleitung 1x4 mm², 100m","Solarleitung 1x4 mm², 100m","Solarleitung 1x4 mm², 100m","Solarleitung 1x4 mm², 100m","Solarleitung 1x4 mm², 100m","Solarleitung 1x4 mm², 100m"]
[null,273358,"Solarleitung 1x4 mm², 500m","On request","",null,null,null,null,null,null,273358,"Solarleitung 1x4 mm², 500m","On request",false,null,273358,490,"On request","sur demande","på forespørgsel","op aanvraag","Solarleitung 1x4 mm², 500m","Solarleitung 1x4 mm², 500m","Solarleitung 1x4 mm², 500m","Solarleitung 1x4 mm², 500m","Solarleiding 1x4 mm², 500m","Solarleitung 1x4 mm², 500m","Solarleitung 1x4 mm², 500m","Solarleitung 1x4 mm², 500m","Solarleitung 1x4 mm², 500m","Solarleitung 1x4 mm², 500m","Solarleitung 1x4 mm², 500m"]
[null,273320,"Solarleitung 1x6 mm², 50m","On request","",null,null,null,null,null,null,273320,"Solarleitung 1x6 mm², 50m","On request",false,null,273320,69,"On request","sur demande","på forespørgsel","op aanvraag","Solarleitung 1x6 mm², 50m","Solarleitung 1x6 mm², 50m","Solarleitung 1x6 mm², 50m","Solarleitung 1x6 mm², 50m","Solarleiding 1x6 mm², 50m","Solarleitung 1x6 mm², 50m","Solarleitung 1x6 mm², 50m","Solarleitung 1x6 mm², 50m","Solarleitung 1x6 mm², 50m","Solarleitung 1x6 mm², 50m","Solarleitung 1x6 mm², 50m"]
[null,273321,"Solarleitung 1x6 mm², 100m","On request","",null,null,null,null,null,null,273321,"Solarleitung 1x6 mm², 100m","On request",false,null,273321,138,"On request","sur demande","på forespørgsel","op aanvraag","Solarleitung 1x6 mm², 100m","Solarleitung 1x6 mm², 100m","Solarleitung 1x6 mm², 100m","Solarleitung 1x6 mm², 100m","Solarleiding 1x6 mm², 100m","Solarleitung 1x6 mm², 100m","Solarleitung 1x6 mm², 100m","Solarleitung 1x6 mm², 100m","Solarleitung 1x6 mm², 100m","Solarleitung 1x6 mm², 100m","Solarleitung 1x6 mm², 100m"]
[null,273359,"Solarleitung 1x6 mm², 500m","On request","",null,null,null,null,null,null,273359,"Solarleitung 1x6 mm², 500m","On request",false,null,273359,690,"On request","sur demande","på forespørgsel","op aanvraag","Solarleitung 1x6 mm², 500m","Solarleitung 1x6 mm², 500m","Solarleitung 1x6 mm², 500m","Solarleitung 1x6 mm², 500m","Solarleiding 1x6 mm², 500m","Solarleitung 1x6 mm², 500m","Solarleitung 1x6 mm², 500m","Solarleitung 1x6 mm², 500m","Solarleitung 1x6 mm², 500m","Solarleitung 1x6 mm², 500m","Solarleitung 1x6 mm², 500m"]
[null,273322,"Solarleitung 1x10 mm², 50m","On request","",null,null,null,null,null,null,273322,"Solarleitung 1x10 mm², 50m","On request",false,null,273322,115,"On request","sur demande","på forespørgsel","op aanvraag","Solarleitung 1x10 mm², 50m","Solarleitung 1x10 mm², 50m","Solarleitung 1x10 mm², 50m","Solarleitung 1x10 mm², 50m","Solarleiding 1x10 mm², 50m","Solarleitung 1x10 mm², 50m","Solarleitung 1x10 mm², 50m","Solarleitung 1x10 mm², 50m","Solarleitung 1x10 mm², 50m","Solarleitung 1x10 mm², 50m","Solarleitung 1x10 mm², 50m"]
[null,273323,"Solarleitung 1x10 mm², 100m","On request","",null,null,null,null,null,null,273323,"Solarleitung 1x10 mm², 100m","On request",false,null,273323,230,"On request","sur demande","på forespørgsel","op aanvraag","Solarleitung 1x10 mm², 100m","Solarleitung 1x10 mm², 100m","Solarleitung 1x10 mm², 100m","Solarleitung 1x10 mm², 100m","Solarleiding 1x10 mm², 100m","Solarleitung 1x10 mm², 100m","Solarleitung 1x10 mm², 100m","Solarleitung 1x10 mm², 100m","Solarleitung 1x10 mm², 100m","Solarleitung 1x10 mm², 100m","Solarleitung 1x10 mm², 100m"]
[null,273656,"Adapterset APH-H4","On request","",null,null,null,null,null,null,273656,"Adapterset APH-H4","On request",false,null,273656,9.15,"On request","sur demande","på forespørgsel","op aanvraag","Adapterset Solarkabel Amphenol","Adapterset APH-H4","Adapterset APH-H4","Adapterset APH-H4","Adapterset APH-H4","Adapterset APH-H4","Adapterset APH-H4","Adapterset APH-H4","Adapterset APH-H4","Adapterset APH-H4","Adapterset APH-H4"]
[null,273655,"Entriegelungswerkzeug APH-H4","On request","",null,null,null,null,null,null,273655,"Entriegelungswerkzeug APH-H4","On request",false,null,273655,1.05,"On request","sur demande","på forespørgsel","op aanvraag","Entriegelungswerkzeug Solarkabel","Entriegelungswerkzeug APH-H4","Entriegelungswerkzeug APH-H4","Entriegelungswerkzeug APH-H4","Ontgrendelingsgereedschap APH-H4","Entriegelungswerkzeug APH-H4","Entriegelungswerkzeug APH-H4","Entriegelungswerkzeug APH-H4","Entriegelungswerkzeug APH-H4","Entriegelungswerkzeug APH-H4","Entriegelungswerkzeug APH-H4"]
[null,273310,"TEGREON 1202 WWK (12x Module TEGREON)","On request","",null,null,null,null,null,null,273310,"TEGREON 1202 WWK (12x Module TEGREON)","On request",false,null,273310,7800,"On request","sur demande","på forespørgsel","op aanvraag","PV-Set TEGREON 1202 WWK (2 Reihen x 6 Module)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)"]
[null,273311,"TEGREON 1202 WWK (12x Module TEGREON)","On request","",null,null,null,null,null,null,273311,"TEGREON 1202 WWK (12x Module TEGREON)","On request",false,null,273311,7900,"On request","sur demande","på forespørgsel","op aanvraag","PV-Set TEGREON 1202 WWK (3 Reihen x 4 Module)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)","TEGREON 1202 WWK (12x Module TEGREON)"]
[null,273312,"TEGREON 1601 WWK (16x Module TEGREON)","On request","",null,null,null,null,null,null,273312,"TEGREON 1601 WWK (16x Module TEGREON)","On request",false,null,273312,9300,"On request","sur demande","på forespørgsel","op aanvraag","PV-Set TEGREON 1601 WWK (2 Reihen x 8 Module)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)","TEGREON 1601 WWK (16x Module TEGREON)"]
[null,273313,"TEGREON 1602 WWK (16x Module TEGREON)","On request","",null,null,null,null,null,null,273313,"TEGREON 1602 WWK (16x Module TEGREON)","On request",false,null,273313,9400,"On request","sur demande","på forespørgsel","op aanvraag","PV-Set TEGREON 1602 WWK (4 Reihen x 4 Module)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)","TEGREON 1602 WWK (16x Module TEGREON)"]
[null,273314,"TEGREON 2001 WWK (20x Module TEGREON)","On request","",null,null,null,null,null,null,273314,"TEGREON 2001 WWK (20x Module TEGREON)","On request",false,null,273314,11000,"On request","sur demande","på forespørgsel","op aanvraag","PV-Set TEGREON 2001 WWK (2 Reihen x 10 Module)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)","TEGREON 2001 WWK (20x Module TEGREON)"]
[null,273315,"TEGREON 2002 WWK (20x Module TEGREON)","On request","",null,null,null,null,null,null,273315,"TEGREON 2002 WWK (20x Module TEGREON)","On request",false,null,273315,11100,"On request","sur demande","på forespørgsel","op aanvraag","PV-Set TEGREON 2002 WWK (4 Reihen x 5 Module)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)","TEGREON 2002 WWK (20x Module TEGREON)"]
[null,233228,"Integralgerät mit Photovoltaik LWZ 304 PV SET","On request","",null,null,null,null,null,null,233228,"Integralgerät mit Photovoltaik LWZ 304 PV SET","On request",false,null,233228,18362.400000000001,"On request","sur demande","på forespørgsel","op aanvraag","Integralgerät mit Photovoltaik LWZ 304 PV SET","Integralgerät mit Photovoltaik LWZ 304 PV SET","Integralgerät mit Photovoltaik LWZ 304 PV SET","Integralgerät mit Photovoltaik LWZ 304 PV SET","Centraal ventilatietoestel  LWZ 304 PV Set","Integralgerät mit Photovoltaik LWZ 304 PV SET","Integralgerät mit Photovoltaik LWZ 304 PV SET","Integralgerät mit Photovoltaik LWZ 304 PV SET","Integralgerät mit Photovoltaik LWZ 304 PV SET","Integralgerät mit Photovoltaik LWZ 304 PV SET","Integralgerät mit Photovoltaik LWZ 304 PV SET"]
[null,233229,"Integralgerät mit Photovoltaik LWZ 404 PV SET","On request","",null,null,null,null,null,null,233229,"Integralgerät mit Photovoltaik LWZ 404 PV SET","On request",false,null,233229,19399.400000000001,"On request","sur demande","på forespørgsel","op aanvraag","Integralgerät mit Photovoltaik LWZ 404 PV SET","Integralgerät mit Photovoltaik LWZ 404 PV SET","Integralgerät mit Photovoltaik LWZ 404 PV SET","Integralgerät mit Photovoltaik LWZ 404 PV SET","Centraal ventilatietoestel  LWZ 404 PV Set","Integralgerät mit Photovoltaik LWZ 404 PV SET","Integralgerät mit Photovoltaik LWZ 404 PV SET","Integralgerät mit Photovoltaik LWZ 404 PV SET","Integralgerät mit Photovoltaik LWZ 404 PV SET","Integralgerät mit Photovoltaik LWZ 404 PV SET","Integralgerät mit Photovoltaik LWZ 404 PV SET"]
[null,223240,"Transportable air dryer LFW 12 C","On request","",null,null,null,null,null,null,223240,"Transportable air dryer LFW 12 C","On request",false,null,223240,446,"On request","sur demande","på forespørgsel","op aanvraag","Luftentfeuchter LFW 12 C","Transportable air dryer LFW 12 C","Transportable air dryer LFW 12 C","Transportable air dryer LFW 12 C","Luchtontvochtiger LFW 12 C","Transportable air dryer LFW 12 C","Transportable air dryer LFW 12 C","Transportable air dryer LFW 12 C","Transportable air dryer LFW 12 C","Transportable air dryer LFW 12 C","Transportable air dryer LFW 12 C"]
[null,231593,"Transportable air dryer LF 21","On request","",null,null,null,null,null,null,231593,"Transportable air dryer LF 21","On request",false,null,231593,445,"On request","sur demande","på forespørgsel","op aanvraag","Mobiler Luftentfeuchter LF 21","Transportable air dryer LF 21","Transportable air dryer LF 21","Transportable air dryer LF 21","Mobiele Luchtontvochtiger LF 21","Transportable air dryer LF 21","Transportable air dryer LF 21","Transportable air dryer LF 21","Transportable air dryer LF 21","Transportable air dryer LF 21","Transportable air dryer LF 21"]
[null,227151,"Transportable air conditioning unit ACP 24","On request","",null,null,null,null,null,null,227151,"Transportable air conditioning unit ACP 24","On request",false,null,227151,1072,"On request","sur demande","på forespørgsel","op aanvraag","Mobiles Kompakt-Raumklimagerät ACP 24","Transportable air conditioning unit ACP 24","Transportable air conditioning unit ACP 24","Transportable air conditioning unit ACP 24","Mobiele compacte Airco-unit ACP 24","Transportable air conditioning unit ACP 24","Transportable air conditioning unit ACP 24","Transportable air conditioning unit ACP 24","Transportable air conditioning unit ACP 24","Transportable air conditioning unit ACP 24","Transportable air conditioning unit ACP 24"]
[null,233751,"Mobiles Kompakt-Raumklimagerät ACP 29 plus","On request","",null,null,null,null,null,null,233751,"Mobiles Kompakt-Raumklimagerät ACP 29 plus","On request",false,null,233751,785,"On request","sur demande","på forespørgsel","op aanvraag","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiele compacte Airco-unit ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus","Mobiles Kompakt-Raumklimagerät ACP 29 plus"]
[null,227153,"ACP 24 wall mounting set","On request","",null,null,null,null,null,null,227153,"ACP 24 wall mounting set","On request",false,null,227153,86,"On request","sur demande","på forespørgsel","op aanvraag","ACP 24 Wandmontageset","ACP 24 wall mounting set","ACP 24 wall mounting set","ACP 24 wall mounting set","ACP 24 Wandmontageset","ACP 24 wall mounting set","ACP 24 wall mounting set","ACP 24 wall mounting set","ACP 24 wall mounting set","ACP 24 wall mounting set","ACP 24 wall mounting set"]
[null,227550,"Telescope wall entrances ACP 24","On request","",null,null,null,null,null,null,227550,"Telescope wall entrances ACP 24","On request",false,null,227550,63,"On request","sur demande","på forespørgsel","op aanvraag","Teleskop-Wanddurchführung ACP 24","Telescope wall entrances ACP 24","Telescope wall entrances ACP 24","Telescope wall entrances ACP 24","Telescopische wanddoorvoer ACP 24","Telescope wall entrances ACP 24","Telescope wall entrances ACP 24","Telescope wall entrances ACP 24","Telescope wall entrances ACP 24","Telescope wall entrances ACP 24","Telescope wall entrances ACP 24"]
[null,233588,"Singlesplit-Raumklimagerät CAWR 25 exklusiv","On request","",null,null,null,null,null,null,233588,"Singlesplit-Raumklimagerät CAWR 25 exklusiv","On request",false,null,233588,2059,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit Airco-unit CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv","Singlesplit-Raumklimagerät CAWR 25 exklusiv"]
[null,233589,"Singlesplit-Raumklimagerät CAWR 35 exklusiv","On request","",null,null,null,null,null,null,233589,"Singlesplit-Raumklimagerät CAWR 35 exklusiv","On request",false,null,233589,2359,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit Airco-unit CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv","Singlesplit-Raumklimagerät CAWR 35 exklusiv"]
[null,233590,"Singlesplit-Raumklimagerät CAWR 50 exklusiv","On request","",null,null,null,null,null,null,233590,"Singlesplit-Raumklimagerät CAWR 50 exklusiv","On request",false,null,233590,2795,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit Airco-unit CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv","Singlesplit-Raumklimagerät CAWR 50 exklusiv"]
[null,232630,"Singlesplit-Raumklimagerät CAWR 25 premium","On request","",null,null,null,null,null,null,232630,"Singlesplit-Raumklimagerät CAWR 25 premium","On request",false,null,232630,1815,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit Airco-unit CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium","Singlesplit-Raumklimagerät CAWR 25 premium"]
[null,232631,"Singlesplit-Raumklimagerät CAWR 35 premium","On request","",null,null,null,null,null,null,232631,"Singlesplit-Raumklimagerät CAWR 35 premium","On request",false,null,232631,2106,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit Airco-unit CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium","Singlesplit-Raumklimagerät CAWR 35 premium"]
[null,232632,"Singlesplit-Raumklimagerät CAWR 50 premium","On request","",null,null,null,null,null,null,232632,"Singlesplit-Raumklimagerät CAWR 50 premium","On request",false,null,232632,2568,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit Airco-unit CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium","Singlesplit-Raumklimagerät CAWR 50 premium"]
[null,232990,"Singlesplit-Raumklimagerät CAWR 25 trend","On request","",null,null,null,null,null,null,232990,"Singlesplit-Raumklimagerät CAWR 25 trend","On request",false,null,232990,1392,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit Airco-unit CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend","Singlesplit-Raumklimagerät CAWR 25 trend"]
[null,232991,"Singlesplit-Raumklimagerät CAWR 35 trend","On request","",null,null,null,null,null,null,232991,"Singlesplit-Raumklimagerät CAWR 35 trend","On request",false,null,232991,1535,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit Airco-unit CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend","Singlesplit-Raumklimagerät CAWR 35 trend"]
[null,232992,"Singlesplit-Raumklimagerät CAWR 50 trend","On request","",null,null,null,null,null,null,232992,"Singlesplit-Raumklimagerät CAWR 50 trend","On request",false,null,232992,2113,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit Airco-unit CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend","Singlesplit-Raumklimagerät CAWR 50 trend"]
[null,232639,"Singlesplit-Raumklimagerät CACR 25 premium","On request","",null,null,null,null,null,null,232639,"Singlesplit-Raumklimagerät CACR 25 premium","On request",false,null,232639,2817,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit Airco-unit CAWR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium","Singlesplit-Raumklimagerät CACR 25 premium"]
[null,232640,"Singlesplit-Raumklimagerät CACR 35 premium","On request","",null,null,null,null,null,null,232640,"Singlesplit-Raumklimagerät CACR 35 premium","On request",false,null,232640,3315,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit Airco-unit CAWR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium","Singlesplit-Raumklimagerät CACR 35 premium"]
[null,232641,"Singlesplit-Raumklimagerät CACR 50 premium","On request","",null,null,null,null,null,null,232641,"Singlesplit-Raumklimagerät CACR 50 premium","On request",false,null,232641,3846,"On request","sur demande","på forespørgsel","op aanvraag","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit Airco-unit CAWR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium","Singlesplit-Raumklimagerät CACR 50 premium"]
[null,232648,"Multisplit-Außengerät CUR 2-53 premium","On request","",null,null,null,null,null,null,232648,"Multisplit-Außengerät CUR 2-53 premium","On request",false,null,232648,2554,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Buitenunit CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium","Multisplit-Außengerät CUR 2-53 premium"]
[null,232649,"Multisplit-Außengerät CUR 3-54 premium","On request","",null,null,null,null,null,null,232649,"Multisplit-Außengerät CUR 3-54 premium","On request",false,null,232649,3094,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Buitenunit CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium","Multisplit-Außengerät CUR 3-54 premium"]
[null,232650,"Multisplit-Außengerät CUR 4-72 premium","On request","",null,null,null,null,null,null,232650,"Multisplit-Außengerät CUR 4-72 premium","On request",false,null,232650,4262,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Buitenunit CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium","Multisplit-Außengerät CUR 4-72 premium"]
[null,232651,"Multisplit-Außengerät CUR 5-102 premium","On request","",null,null,null,null,null,null,232651,"Multisplit-Außengerät CUR 5-102 premium","On request",false,null,232651,6317,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Buitenunit CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium","Multisplit-Außengerät CUR 5-102 premium"]
[null,230800,"Multisplit-Outdoor unit CUR 5-100i premium","On request","",null,null,null,null,null,null,230800,"Multisplit-Outdoor unit CUR 5-100i premium","On request",false,null,230800,5927,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Außengerät CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium","Multisplit-Buitenunit CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium","Multisplit-Outdoor unit CUR 5-100i premium"]
[null,232652,"Multisplit-Außengerät CUR 6-122 premium","On request","",null,null,null,null,null,null,232652,"Multisplit-Außengerät CUR 6-122 premium","On request",false,null,232652,7438,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Buitenunit CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium","Multisplit-Außengerät CUR 6-122 premium"]
[null,232653,"Multisplit-Innengerät Wand Wand ACW 18 exklusiv","On request","",null,null,null,null,null,null,232653,"Multisplit-Innengerät Wand Wand ACW 18 exklusiv","On request",false,null,232653,703,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Binnenunit ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv","Multisplit-Innengerät Wand Wand ACW 18 exklusiv"]
[null,232654,"Multisplit-Innengerät Wand ACW 22 exklusiv","On request","",null,null,null,null,null,null,232654,"Multisplit-Innengerät Wand ACW 22 exklusiv","On request",false,null,232654,726,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Binnenunit ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv","Multisplit-Innengerät Wand ACW 22 exklusiv"]
[null,232655,"Multisplit-Innengerät Wand ACW 25 exklusiv","On request","",null,null,null,null,null,null,232655,"Multisplit-Innengerät Wand ACW 25 exklusiv","On request",false,null,232655,782,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Binnenunit ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv","Multisplit-Innengerät Wand ACW 25 exklusiv"]
[null,232656,"Multisplit-Innengerät Wand ACW 35 exklusiv","On request","",null,null,null,null,null,null,232656,"Multisplit-Innengerät Wand ACW 35 exklusiv","On request",false,null,232656,909,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Binnenunit ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv","Multisplit-Innengerät Wand ACW 35 exklusiv"]
[null,232657,"Multisplit-Innengerät Wand ACW 50 exklusiv","On request","",null,null,null,null,null,null,232657,"Multisplit-Innengerät Wand ACW 50 exklusiv","On request",false,null,232657,1103,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Binnenunit ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv","Multisplit-Innengerät Wand ACW 50 exklusiv"]
[null,232633,"Multisplit-Innengerät Wand ACW 25 premium","On request","",null,null,null,null,null,null,232633,"Multisplit-Innengerät Wand ACW 25 premium","On request",false,null,232633,646,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Binnenunit ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium","Multisplit-Innengerät Wand ACW 25 premium"]
[null,232634,"Multisplit-Innengerät Wand ACW 35 premium","On request","",null,null,null,null,null,null,232634,"Multisplit-Innengerät Wand ACW 35 premium","On request",false,null,232634,776,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Binnenunit ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium","Multisplit-Innengerät Wand ACW 35 premium"]
[null,232635,"Multisplit-Innengerät Wand ACW 50 premium","On request","",null,null,null,null,null,null,232635,"Multisplit-Innengerät Wand ACW 50 premium","On request",false,null,232635,977,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Binnenunit ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium","Multisplit-Innengerät Wand ACW 50 premium"]
[null,232642,"Multisplit-Innengerät Decke ACK 25 premium","On request","",null,null,null,null,null,null,232642,"Multisplit-Innengerät Decke ACK 25 premium","On request",false,null,232642,1589,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Binnenunit ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium","Multisplit-Innengerät Decke ACK 25 premium"]
[null,232643,"Multisplit-Innengerät Decke ACK 35 premium","On request","",null,null,null,null,null,null,232643,"Multisplit-Innengerät Decke ACK 35 premium","On request",false,null,232643,1909,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Binnenunit ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium","Multisplit-Innengerät Decke ACK 35 premium"]
[null,232644,"Multisplit-Innengerät Decke ACK 50 premium","On request","",null,null,null,null,null,null,232644,"Multisplit-Innengerät Decke ACK 50 premium","On request",false,null,232644,2173,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Binnenunit ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium","Multisplit-Innengerät Decke ACK 50 premium"]
[null,230780,"Multisplit-Indoor unit ACK 25i premium","On request","",null,null,null,null,null,null,230780,"Multisplit-Indoor unit ACK 25i premium","On request",false,null,230780,1499,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Decke ACK 25i premium","Multisplit-Indoor unit ACK 25i premium","Multisplit-Indoor unit ACK 25i premium","Multisplit-Indoor unit ACK 25i premium","Multisplit-Binnenunit ACK 25i premium","Multisplit-Indoor unit ACK 25i premium","Multisplit-Indoor unit ACK 25i premium","Multisplit-Indoor unit ACK 25i premium","Multisplit-Indoor unit ACK 25i premium","Multisplit-Indoor unit ACK 25i premium","Multisplit-Indoor unit ACK 25i premium"]
[null,230781,"Multisplit-Indoor unit ACK 35i premium","On request",{"$f":"IF(O850=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,230781,"Multisplit-Indoor unit ACK 35i premium","On request",false,null,230781,1800,"On request","sur demande","på forespørgsel","op aanvraag","Multisplit-Innengerät Decke ACK 35i premium","Multisplit-Indoor unit ACK 35i premium","Multisplit-Indoor unit ACK 35i premium","Multisplit-Indoor unit ACK 35i premium","Multisplit-Binnenunit ACK 35i premium","Multisplit-Indoor unit ACK 35i premium","Multisplit-Indoor unit ACK 35i premium","Multisplit-Indoor unit ACK 35i premium","Multisplit-Indoor unit ACK 35i premium","Multisplit-Indoor unit ACK 35i premium","Multisplit-Indoor unit ACK 35i premium"]
[null,169972,"Split line 6x1 mm, 5 m","On request","",null,null,null,null,null,null,169972,"Split line 6x1 mm, 5 m","On request",false,null,169972,82,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 6x1 mm, 5 m","Split line 6x1 mm, 5 m","Split line 6x1 mm, 5 m","Split line 6x1 mm, 5 m","Vloeistofpersleiding 6x1 mm, 5 m","Split line 6x1 mm, 5 m","Split line 6x1 mm, 5 m","Split line 6x1 mm, 5 m","Split line 6x1 mm, 5 m","Split line 6x1 mm, 5 m","Split line 6x1 mm, 5 m"]
[null,139291,"Split line 6x1 mm, 10 m","On request","",null,null,null,null,null,null,139291,"Split line 6x1 mm, 10 m","On request",false,null,139291,104,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 6x1 mm, 10 m","Split line 6x1 mm, 10 m","Split line 6x1 mm, 10 m","Split line 6x1 mm, 10 m","Vloeistofpersleiding 6x1 mm, 10 m","Split line 6x1 mm, 10 m","Split line 6x1 mm, 10 m","Split line 6x1 mm, 10 m","Split line 6x1 mm, 10 m","Split line 6x1 mm, 10 m","Split line 6x1 mm, 10 m"]
[null,169973,"Split line 6x1 mm, 15 m","On request","",null,null,null,null,null,null,169973,"Split line 6x1 mm, 15 m","On request",false,null,169973,128,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 6x1 mm, 15 m","Split line 6x1 mm, 15 m","Split line 6x1 mm, 15 m","Split line 6x1 mm, 15 m","Vloeistofpersleiding 6x1 mm, 15 m","Split line 6x1 mm, 15 m","Split line 6x1 mm, 15 m","Split line 6x1 mm, 15 m","Split line 6x1 mm, 15 m","Split line 6x1 mm, 15 m","Split line 6x1 mm, 15 m"]
[null,223459,"Split line 6x1 mm, 30 m","On request","",null,null,null,null,null,null,223459,"Split line 6x1 mm, 30 m","On request",{"$f":"IF(AND(B854=L854,C854=M854,D854=N854),FALSE,TRUE)","v":false},null,223459,187,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 6x1 mm, 30 m","Split line 6x1 mm, 30 m","Split line 6x1 mm, 30 m","Split line 6x1 mm, 30 m","Vloeistofpersleiding 6x1 mm, 30 m","Split line 6x1 mm, 30 m","Split line 6x1 mm, 30 m","Split line 6x1 mm, 30 m","Split line 6x1 mm, 30 m","Split line 6x1 mm, 30 m","Split line 6x1 mm, 30 m"]
[null,114942,"Split line 10x1 mm, 5 m","On request","",null,null,null,null,null,null,114942,"Split line 10x1 mm, 5 m","On request",false,null,114942,92,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 10x1 mm, 5 m","Split line 10x1 mm, 5 m","Split line 10x1 mm, 5 m","Split line 10x1 mm, 5 m","Zuiggasleiding 10x1 mm, 5 m","Split line 10x1 mm, 5 m","Split line 10x1 mm, 5 m","Split line 10x1 mm, 5 m","Split line 10x1 mm, 5 m","Split line 10x1 mm, 5 m","Split line 10x1 mm, 5 m"]
[null,117996,"Split line 10x1 mm, 10 m","On request","",null,null,null,null,null,null,117996,"Split line 10x1 mm, 10 m","On request",false,null,117996,116,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 10x1 mm, 10 m","Split line 10x1 mm, 10 m","Split line 10x1 mm, 10 m","Split line 10x1 mm, 10 m","Zuiggasleiding 10x1 mm, 10 m","Split line 10x1 mm, 10 m","Split line 10x1 mm, 10 m","Split line 10x1 mm, 10 m","Split line 10x1 mm, 10 m","Split line 10x1 mm, 10 m","Split line 10x1 mm, 10 m"]
[null,169974,"Split line 10x1 mm, 15 m","On request","",null,null,null,null,null,null,169974,"Split line 10x1 mm, 15 m","On request",false,null,169974,151,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 10x1 mm, 15 m","Split line 10x1 mm, 15 m","Split line 10x1 mm, 15 m","Split line 10x1 mm, 15 m","Zuiggasleiding 10x1 mm, 15 m","Split line 10x1 mm, 15 m","Split line 10x1 mm, 15 m","Split line 10x1 mm, 15 m","Split line 10x1 mm, 15 m","Split line 10x1 mm, 15 m","Split line 10x1 mm, 15 m"]
[null,223460,"Split line 10x1 mm, 30 m","On request","",null,null,null,null,null,null,223460,"Split line 10x1 mm, 30 m","On request",false,null,223460,221,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 10x1 mm, 30 m","Split line 10x1 mm, 30 m","Split line 10x1 mm, 30 m","Split line 10x1 mm, 30 m","Zuiggasleiding 10x1 mm, 30 m","Split line 10x1 mm, 30 m","Split line 10x1 mm, 30 m","Split line 10x1 mm, 30 m","Split line 10x1 mm, 30 m","Split line 10x1 mm, 30 m","Split line 10x1 mm, 30 m"]
[null,169975,"Split line 12x1 mm, 5 m","On request","",null,null,null,null,null,null,169975,"Split line 12x1 mm, 5 m","On request",false,null,169975,104,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 12x1 mm, 5 m","Split line 12x1 mm, 5 m","Split line 12x1 mm, 5 m","Split line 12x1 mm, 5 m","Zuiggasleiding 12x1 mm, 5 m","Split line 12x1 mm, 5 m","Split line 12x1 mm, 5 m","Split line 12x1 mm, 5 m","Split line 12x1 mm, 5 m","Split line 12x1 mm, 5 m","Split line 12x1 mm, 5 m"]
[null,139292,"Split line 12x1 mm, 10 m","On request","",null,null,null,null,null,null,139292,"Split line 12x1 mm, 10 m","On request",false,null,139292,154,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 12x1 mm, 10 m","Split line 12x1 mm, 10 m","Split line 12x1 mm, 10 m","Split line 12x1 mm, 10 m","Zuiggasleiding 12x1 mm, 10 m","Split line 12x1 mm, 10 m","Split line 12x1 mm, 10 m","Split line 12x1 mm, 10 m","Split line 12x1 mm, 10 m","Split line 12x1 mm, 10 m","Split line 12x1 mm, 10 m"]
[null,169976,"Split line 12x1 mm, 15 m","On request","",null,null,null,null,null,null,169976,"Split line 12x1 mm, 15 m","On request",false,null,169976,209,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 12x1 mm, 15 m","Split line 12x1 mm, 15 m","Split line 12x1 mm, 15 m","Split line 12x1 mm, 15 m","Zuiggasleiding 12x1 mm, 15 m","Split line 12x1 mm, 15 m","Split line 12x1 mm, 15 m","Split line 12x1 mm, 15 m","Split line 12x1 mm, 15 m","Split line 12x1 mm, 15 m","Split line 12x1 mm, 15 m"]
[null,223461,"Split line 12x1 mm, 30 m","On request","",null,null,null,null,null,null,223461,"Split line 12x1 mm, 30 m","On request",false,null,223461,305,"On request","sur demande","på forespørgsel","op aanvraag","Splitleitungen 12x1 mm, 30 m","Split line 12x1 mm, 30 m","Split line 12x1 mm, 30 m","Split line 12x1 mm, 30 m","Zuiggasleiding 12x1 mm, 30 m","Split line 12x1 mm, 30 m","Split line 12x1 mm, 30 m","Split line 12x1 mm, 30 m","Split line 12x1 mm, 30 m","Split line 12x1 mm, 30 m","Split line 12x1 mm, 30 m"]
[null,47614,"Union nut 6 mm","On request","",null,null,null,null,null,null,47614,"Union nut 6 mm","On request",false,null,47614,2.7,"On request","sur demande","på forespørgsel","op aanvraag","Überwurfmutter 6 mm","Union nut 6 mm","Union nut 6 mm","Union nut 6 mm","Wartel 6 mm","Union nut 6 mm","Union nut 6 mm","Union nut 6 mm","Union nut 6 mm","Union nut 6 mm","Union nut 6 mm"]
[null,31479,"Union nut 10 mm","On request","",null,null,null,null,null,null,31479,"Union nut 10 mm","On request",false,null,31479,2.7,"On request","sur demande","på forespørgsel","op aanvraag","Überwurfmutter 10 mm","Union nut 10 mm","Union nut 10 mm","Union nut 10 mm","Wartel 10 mm","Union nut 10 mm","Union nut 10 mm","Union nut 10 mm","Union nut 10 mm","Union nut 10 mm","Union nut 10 mm"]
[null,31474,"Union nut 12 mm","On request","",null,null,null,null,null,null,31474,"Union nut 12 mm","On request",false,null,31474,2.7,"On request","sur demande","på forespørgsel","op aanvraag","Überwurfmutter 12 mm","Union nut 12 mm","Union nut 12 mm","Union nut 12 mm","Wartel 12 mm","Union nut 12 mm","Union nut 12 mm","Union nut 12 mm","Union nut 12 mm","Union nut 12 mm","Union nut 12 mm"]
[null,71735,"Fitting 6 mm","On request","",null,null,null,null,null,null,71735,"Fitting 6 mm","On request",false,null,71735,5.0999999999999996,"On request","sur demande","på forespørgsel","op aanvraag","Verbindungsnippel 6 mm","Fitting 6 mm","Fitting 6 mm","Fitting 6 mm","Verbindingsnippel 6 mm","Fitting 6 mm","Fitting 6 mm","Fitting 6 mm","Fitting 6 mm","Fitting 6 mm","Fitting 6 mm"]
[null,71736,"Fitting 10 mm","On request","",null,null,null,null,null,null,71736,"Fitting 10 mm","On request",false,null,71736,6.6,"On request","sur demande","på forespørgsel","op aanvraag","Verbindungsnippel 10 mm","Fitting 10 mm","Fitting 10 mm","Fitting 10 mm","Verbindingsnippel 10 mm","Fitting 10 mm","Fitting 10 mm","Fitting 10 mm","Fitting 10 mm","Fitting 10 mm","Fitting 10 mm"]
[null,71737,"Fitting 12 mm","On request","",null,null,null,null,null,null,71737,"Fitting 12 mm","On request",false,null,71737,8.5,"On request","sur demande","på forespørgsel","op aanvraag","Verbindungsnippel 12 mm","Fitting 12 mm","Fitting 12 mm","Fitting 12 mm","Verbindingsnippel 12 mm","Fitting 12 mm","Fitting 12 mm","Fitting 12 mm","Fitting 12 mm","Fitting 12 mm","Fitting 12 mm"]
[null,227557,"Insulating tape, 10 m","On request","",null,null,null,null,null,null,227557,"Insulating tape, 10 m","On request",false,null,227557,17.600000000000001,"On request","sur demande","på forespørgsel",18,"Wärmedämmband, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Isolatieband, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m","Insulating tape, 10 m"]
[null,182148,"In-wall box for installation 1","On request","",null,null,null,null,null,null,182148,"In-wall box for installation 1","On request",false,null,182148,12.6,"On request","sur demande","på forespørgsel","op aanvraag","Klima-Wandbox 1","In-wall box for installation 1","In-wall box for installation 1","In-wall box for installation 1","Klima-Wandbox 1","In-wall box for installation 1","In-wall box for installation 1","In-wall box for installation 1","In-wall box for installation 1","In-wall box for installation 1","In-wall box for installation 1"]
[null,227556,"In-wall box for installation 2","On request","",null,null,null,null,null,null,227556,"In-wall box for installation 2","On request",false,null,227556,14.4,"On request","sur demande","på forespørgsel","op aanvraag","Klima-Wandbox 2","In-wall box for installation 2","In-wall box for installation 2","In-wall box for installation 2","Klima-Wandbox 2","In-wall box for installation 2","In-wall box for installation 2","In-wall box for installation 2","In-wall box for installation 2","In-wall box for installation 2","In-wall box for installation 2"]
[null,182145,"Wall mounting panel 1","On request","",null,null,null,null,null,null,182145,"Wall mounting panel 1","On request",false,null,182145,81,"On request","sur demande","på forespørgsel","op aanvraag","Wandkonsole 1","Wall mounting panel 1","Wall mounting panel 1","Wall mounting panel 1","Wandconsole 1","Wall mounting panel 1","Wall mounting panel 1","Wall mounting panel 1","Wall mounting panel 1","Wall mounting panel 1","Wall mounting panel 1"]
[null,222263,"Wall mounting panel 2",47,"",null,null,null,null,null,null,222263,"Wall mounting panel 2",47,false,null,222263,81,47,"sur demande",302,81,"Wandkonsole 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2","Wandconsole 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2","Wall mounting panel 2"]
[null,227558,"Mounting rail CUR","On request","",null,null,null,null,null,null,227558,"Mounting rail CUR","On request",false,null,227558,35,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene CUR","Mounting rail CUR","Mounting rail CUR","Mounting rail CUR","Montagerail CUR","Mounting rail CUR","Mounting rail CUR","Mounting rail CUR","Mounting rail CUR","Mounting rail CUR","Mounting rail CUR"]
[null,153504,"Vibration damper floor","On request","",null,null,null,null,null,null,153504,"Vibration damper floor","On request",false,null,153504,26,"On request","sur demande","på forespørgsel","op aanvraag","Schwingungsdämpfer Boden, 4 Stück","Vibration damper floor","Vibration damper floor","Vibration damper floor","Geluidsdemper vloer, 4 stuks","Vibration damper floor","Vibration damper floor","Vibration damper floor","Vibration damper floor","Vibration damper floor","Vibration damper floor"]
[null,227555," vibration damper console","On request","",null,null,null,null,null,null,227555," vibration damper console","On request",false,null,227555,17.399999999999999,"On request","sur demande","på forespørgsel","op aanvraag","Schwingungsdämpfer Konsole, 4 Stück"," vibration damper console"," vibration damper console"," vibration damper console","Geluidsdemper console, 4 stuks"," vibration damper console"," vibration damper console"," vibration damper console"," vibration damper console"," vibration damper console"," vibration damper console"]
[null,171853,"Condensate pump PK 8","On request","",null,null,null,null,null,null,171853,"Condensate pump PK 8","On request",false,null,171853,254,"On request","sur demande","på forespørgsel","op aanvraag","Kondensatpumpe PK 8","Condensate pump PK 8","Condensate pump PK 8","Condensate pump PK 8","Condensaatpomp PK 8","Condensate pump PK 8","Condensate pump PK 8","Condensate pump PK 8","Condensate pump PK 8","Condensate pump PK 8","Condensate pump PK 8"]
[null,230802,"Communication port ACCI","On request","",null,null,null,null,null,null,230802,"Communication port ACCI","On request",false,null,230802,176,"On request","sur demande","på forespørgsel","op aanvraag","Kommunikationsschnittstelle ACCI","Communication port ACCI","Communication port ACCI","Communication port ACCI","Communicatie interfacekabel  ACCI","Communication port ACCI","Communication port ACCI","Communication port ACCI","Communication port ACCI","Communication port ACCI","Communication port ACCI"]
[null,230803,"Communication cable ACCA","On request","",null,null,null,null,null,null,230803,"Communication cable ACCA","On request",false,null,230803,27.5,"On request","sur demande","på forespørgsel","op aanvraag","Kommunikationskabel ACCA","Communication cable ACCA","Communication cable ACCA","Communication cable ACCA","Communicatiekabel ACCA","Communication cable ACCA","Communication cable ACCA","Communication cable ACCA","Communication cable ACCA","Communication cable ACCA","Communication cable ACCA"]
[null,232841,"Wärmeübergabestation TWS 8","On request","",null,null,null,null,null,null,232841,"Wärmeübergabestation TWS 8","On request",false,null,232841,1056,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation TWS 8","Wärmeübergabestation TWS 8","Wärmeübergabestation TWS 8","Wärmeübergabestation TWS 8","Warmteovergavestation TWS 8","Wärmeübergabestation TWS 8","Wärmeübergabestation TWS 8","Wärmeübergabestation TWS 8","Wärmeübergabestation TWS 8","Wärmeübergabestation TWS 8","Wärmeübergabestation TWS 8"]
[null,232842,"Wärmeübergabestation TWS 10","On request","",null,null,null,null,null,null,232842,"Wärmeübergabestation TWS 10","On request",false,null,232842,1097,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation TWS 10","Wärmeübergabestation TWS 10","Wärmeübergabestation TWS 10","Wärmeübergabestation TWS 10","Warmteovergavestation TWS 10","Wärmeübergabestation TWS 10","Wärmeübergabestation TWS 10","Wärmeübergabestation TWS 10","Wärmeübergabestation TWS 10","Wärmeübergabestation TWS 10","Wärmeübergabestation TWS 10"]
[null,231085,"Heat transfer station TWS 12","On request","",null,null,null,null,null,null,231085,"Heat transfer station TWS 12","On request",false,null,231085,1133,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation TWS 12","Heat transfer station TWS 12","Heat transfer station TWS 12","Heat transfer station TWS 12","Warmteovergavestation TWS 12","Heat transfer station TWS 12","Heat transfer station TWS 12","Heat transfer station TWS 12","Heat transfer station TWS 12","Heat transfer station TWS 12","Heat transfer station TWS 12"]
[null,231086,"Heat transfer station TWS 16","On request","",null,null,null,null,null,null,231086,"Heat transfer station TWS 16","On request",false,null,231086,1373,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation TWS 16","Heat transfer station TWS 16","Heat transfer station TWS 16","Heat transfer station TWS 16","Warmteovergavestation TWS 16","Heat transfer station TWS 16","Heat transfer station TWS 16","Heat transfer station TWS 16","Heat transfer station TWS 16","Heat transfer station TWS 16","Heat transfer station TWS 16"]
[null,232843,"Wärmeübergabestation TWS 10 G","On request","",null,null,null,null,null,null,232843,"Wärmeübergabestation TWS 10 G","On request",false,null,232843,1512,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation TWS 10 G","Wärmeübergabestation TWS 10 G","Wärmeübergabestation TWS 10 G","Wärmeübergabestation TWS 10 G","Warmteovergavestation TWS 10 G","Wärmeübergabestation TWS 10 G","Wärmeübergabestation TWS 10 G","Wärmeübergabestation TWS 10 G","Wärmeübergabestation TWS 10 G","Wärmeübergabestation TWS 10 G","Wärmeübergabestation TWS 10 G"]
[null,232844,"Wärmeübergabestation WS 2-8","On request","",null,null,null,null,null,null,232844,"Wärmeübergabestation WS 2-8","On request",false,null,232844,1136,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 2-8","Wärmeübergabestation WS 2-8","Wärmeübergabestation WS 2-8","Wärmeübergabestation WS 2-8","Warmteovergavestation WS 2-8","Wärmeübergabestation WS 2-8","Wärmeübergabestation WS 2-8","Wärmeübergabestation WS 2-8","Wärmeübergabestation WS 2-8","Wärmeübergabestation WS 2-8","Wärmeübergabestation WS 2-8"]
[null,232845,"Wärmeübergabestation WS 2-10","On request","",null,null,null,null,null,null,232845,"Wärmeübergabestation WS 2-10","On request",false,null,232845,1171,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 2-10","Wärmeübergabestation WS 2-10","Wärmeübergabestation WS 2-10","Wärmeübergabestation WS 2-10","Warmteovergavestation WS 2-10","Wärmeübergabestation WS 2-10","Wärmeübergabestation WS 2-10","Wärmeübergabestation WS 2-10","Wärmeübergabestation WS 2-10","Wärmeübergabestation WS 2-10","Wärmeübergabestation WS 2-10"]
[null,231087,"Heat transfer station WS 2-12","On request","",null,null,null,null,null,null,231087,"Heat transfer station WS 2-12","On request",false,null,231087,1189,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 2-12","Heat transfer station WS 2-12","Heat transfer station WS 2-12","Heat transfer station WS 2-12","Warmteovergavestation WS 2-12","Heat transfer station WS 2-12","Heat transfer station WS 2-12","Heat transfer station WS 2-12","Heat transfer station WS 2-12","Heat transfer station WS 2-12","Heat transfer station WS 2-12"]
[null,231088,"Heat transfer station WS 2-16","On request","",null,null,null,null,null,null,231088,"Heat transfer station WS 2-16","On request",false,null,231088,1408,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 2-16","Heat transfer station WS 2-16","Heat transfer station WS 2-16","Heat transfer station WS 2-16","Warmteovergavestation WS 2-16","Heat transfer station WS 2-16","Heat transfer station WS 2-16","Heat transfer station WS 2-16","Heat transfer station WS 2-16","Heat transfer station WS 2-16","Heat transfer station WS 2-16"]
[null,232847,"Wärmeübergabestation WS 2-10 G","On request","",null,null,null,null,null,null,232847,"Wärmeübergabestation WS 2-10 G","On request",false,null,232847,1668,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 2-10 G","Wärmeübergabestation WS 2-10 G","Wärmeübergabestation WS 2-10 G","Wärmeübergabestation WS 2-10 G","Warmteovergavestation WS 2-10 G","Wärmeübergabestation WS 2-10 G","Wärmeübergabestation WS 2-10 G","Wärmeübergabestation WS 2-10 G","Wärmeübergabestation WS 2-10 G","Wärmeübergabestation WS 2-10 G","Wärmeübergabestation WS 2-10 G"]
[null,232849,"Wärmeübergabestation WS 2plus-8","On request","",null,null,null,null,null,null,232849,"Wärmeübergabestation WS 2plus-8","On request",false,null,232849,1894,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 2plus-8","Wärmeübergabestation WS 2plus-8","Wärmeübergabestation WS 2plus-8","Wärmeübergabestation WS 2plus-8","Warmteovergavestation WS 2plus-8","Wärmeübergabestation WS 2plus-8","Wärmeübergabestation WS 2plus-8","Wärmeübergabestation WS 2plus-8","Wärmeübergabestation WS 2plus-8","Wärmeübergabestation WS 2plus-8","Wärmeübergabestation WS 2plus-8"]
[null,232850,"Wärmeübergabestation WS 2plus-10","On request","",null,null,null,null,null,null,232850,"Wärmeübergabestation WS 2plus-10","On request",false,null,232850,1987,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 2plus-10","Wärmeübergabestation WS 2plus-10","Wärmeübergabestation WS 2plus-10","Wärmeübergabestation WS 2plus-10","Warmteovergavestation WS 2plus-10","Wärmeübergabestation WS 2plus-10","Wärmeübergabestation WS 2plus-10","Wärmeübergabestation WS 2plus-10","Wärmeübergabestation WS 2plus-10","Wärmeübergabestation WS 2plus-10","Wärmeübergabestation WS 2plus-10"]
[null,232848,"Wärmeübergabestation WS 2plus-10 G","On request","",null,null,null,null,null,null,232848,"Wärmeübergabestation WS 2plus-10 G","On request",false,null,232848,2284,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G","Warmteovergavestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G","Wärmeübergabestation WS 2plus-10 G"]
[null,231089,"Heat transfer station WS 4-16","On request","",null,null,null,null,null,null,231089,"Heat transfer station WS 4-16","On request",false,null,231089,1711,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation WS 4-16","Heat transfer station WS 4-16","Heat transfer station WS 4-16","Heat transfer station WS 4-16","Warmteovergavestation WS 4-16","Heat transfer station WS 4-16","Heat transfer station WS 4-16","Heat transfer station WS 4-16","Heat transfer station WS 4-16","Heat transfer station WS 4-16","Heat transfer station WS 4-16"]
[null,231096,"Heat transfer station cover WS 2-AP","On request","",null,null,null,null,null,null,231096,"Heat transfer station cover WS 2-AP","On request",false,null,231096,129,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Gehäuse WS 2-AP","Heat transfer station cover WS 2-AP","Heat transfer station cover WS 2-AP","Heat transfer station cover WS 2-AP","Warmteovergavestation behuizing WS 2-AP","Heat transfer station cover WS 2-AP","Heat transfer station cover WS 2-AP","Heat transfer station cover WS 2-AP","Heat transfer station cover WS 2-AP","Heat transfer station cover WS 2-AP","Heat transfer station cover WS 2-AP"]
[null,231098,"Heat transfer station cover WS 4-AP","On request","",null,null,null,null,null,null,231098,"Heat transfer station cover WS 4-AP","On request",false,null,231098,186,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Gehäuse WS 4-AP","Heat transfer station cover WS 4-AP","Heat transfer station cover WS 4-AP","Heat transfer station cover WS 4-AP","Warmteovergavestation behuizing WS 4-AP","Heat transfer station cover WS 4-AP","Heat transfer station cover WS 4-AP","Heat transfer station cover WS 4-AP","Heat transfer station cover WS 4-AP","Heat transfer station cover WS 4-AP","Heat transfer station cover WS 4-AP"]
[null,232851,"Wärmeübergabestation Gehäuse WS 2 plus APL","On request","",null,null,null,null,null,null,232851,"Wärmeübergabestation Gehäuse WS 2 plus APL","On request",false,null,232851,158,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Gehäuse WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL","Warmteovergavestation behuizing WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL","Wärmeübergabestation Gehäuse WS 2 plus APL"]
[null,232852,"Wärmeübergabestation Gehäuse WS 2 plus APK","On request","",null,null,null,null,null,null,232852,"Wärmeübergabestation Gehäuse WS 2 plus APK","On request",false,null,232852,136,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Gehäuse WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK","Warmteovergavestation behuizing WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK","Wärmeübergabestation Gehäuse WS 2 plus APK"]
[null,231097,"Heat transfer station cover WS 2-UP","On request","",null,null,null,null,null,null,231097,"Heat transfer station cover WS 2-UP","On request",false,null,231097,170,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Gehäuse WS 2-UP","Heat transfer station cover WS 2-UP","Heat transfer station cover WS 2-UP","Heat transfer station cover WS 2-UP","Warmteovergavestation behuizing WS 2-UP","Heat transfer station cover WS 2-UP","Heat transfer station cover WS 2-UP","Heat transfer station cover WS 2-UP","Heat transfer station cover WS 2-UP","Heat transfer station cover WS 2-UP","Heat transfer station cover WS 2-UP"]
[null,231099,"Heat transfer station cover WS 4-UP","On request","",null,null,null,null,null,null,231099,"Heat transfer station cover WS 4-UP","On request",false,null,231099,235,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Gehäuse WS 4-UP","Heat transfer station cover WS 4-UP","Heat transfer station cover WS 4-UP","Heat transfer station cover WS 4-UP","Warmteovergavestation behuizing WS 4-UP","Heat transfer station cover WS 4-UP","Heat transfer station cover WS 4-UP","Heat transfer station cover WS 4-UP","Heat transfer station cover WS 4-UP","Heat transfer station cover WS 4-UP","Heat transfer station cover WS 4-UP"]
[null,232853,"Wärmeübergabestation Gehäuse WS 2 plus UPL","On request","",null,null,null,null,null,null,232853,"Wärmeübergabestation Gehäuse WS 2 plus UPL","On request",false,null,232853,241,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Gehäuse WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL","Warmteovergavestation behuizing WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL","Wärmeübergabestation Gehäuse WS 2 plus UPL"]
[null,232854,"Wärmeübergabestation Gehäuse WS 2 plus UPK","On request","",null,null,null,null,null,null,232854,"Wärmeübergabestation Gehäuse WS 2 plus UPK","On request",false,null,232854,170,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Gehäuse WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK","Warmteovergavestation behuizing WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK","Wärmeübergabestation Gehäuse WS 2 plus UPK"]
[null,233757,"Wärmeübergabestation Regelung WS-RT","On request","",null,null,null,null,null,null,233757,"Wärmeübergabestation Regelung WS-RT","On request",false,null,233757,112,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Regelung WS-RT","Wärmeübergabestation Regelung WS-RT","Wärmeübergabestation Regelung WS-RT","Wärmeübergabestation Regelung WS-RT","Warmteovergavestation regeling WS-RT","Wärmeübergabestation Regelung WS-RT","Wärmeübergabestation Regelung WS-RT","Wärmeübergabestation Regelung WS-RT","Wärmeübergabestation Regelung WS-RT","Wärmeübergabestation Regelung WS-RT","Wärmeübergabestation Regelung WS-RT"]
[null,233758,"Wärmeübergabestation Stellantrieb WS-ST","On request","",null,null,null,null,null,null,233758,"Wärmeübergabestation Stellantrieb WS-ST","On request",false,null,233758,70,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Stellantrieb WS-ST","Wärmeübergabestation Stellantrieb WS-ST","Wärmeübergabestation Stellantrieb WS-ST","Wärmeübergabestation Stellantrieb WS-ST","Warmteovergavestation afsluiteraandrijving WS-ST","Wärmeübergabestation Stellantrieb WS-ST","Wärmeübergabestation Stellantrieb WS-ST","Wärmeübergabestation Stellantrieb WS-ST","Wärmeübergabestation Stellantrieb WS-ST","Wärmeübergabestation Stellantrieb WS-ST","Wärmeübergabestation Stellantrieb WS-ST"]
[null,231100,"Heat transfer station controler WS-RT","On request","",null,null,null,null,null,null,231100,"Heat transfer station controler WS-RT","On request",false,null,231100,77,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Regelung WS-RT (Auslaufmodell)","Heat transfer station controler WS-RT","Heat transfer station controler WS-RT","Heat transfer station controler WS-RT","Warmteovergavestation regeling WS-RT (oud)","Heat transfer station controler WS-RT","Heat transfer station controler WS-RT","Heat transfer station controler WS-RT","Heat transfer station controler WS-RT","Heat transfer station controler WS-RT","Heat transfer station controler WS-RT"]
[null,231186,"Heat transfer station servomotor WS-ST","On request","",null,null,null,null,null,null,231186,"Heat transfer station servomotor WS-ST","On request",false,null,231186,46,"On request","sur demande","på forespørgsel","op aanvraag","Wärmeübergabestation Stellantrieb WS-ST (Auslaufmodell)","Heat transfer station servomotor WS-ST","Heat transfer station servomotor WS-ST","Heat transfer station servomotor WS-ST","Warmteovergavestation afsluiteraandrijving WS-ST (oud)","Heat transfer station servomotor WS-ST","Heat transfer station servomotor WS-ST","Heat transfer station servomotor WS-ST","Heat transfer station servomotor WS-ST","Heat transfer station servomotor WS-ST","Heat transfer station servomotor WS-ST"]
[null,232855,"Heizkreisverteiler HKV 4/9, 4 Heizkreise","On request","",null,null,null,null,null,null,232855,"Heizkreisverteiler HKV 4/9, 4 Heizkreise","On request",false,null,232855,530,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Vloerverdeler HKV 4/9, 4 groepen","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Heizkreisverteiler HKV 4/9, 4 Heizkreise","Heizkreisverteiler HKV 4/9, 4 Heizkreise"]
[null,232856,"Heizkreisverteiler HKV 6/9, 6 Heizkreise","On request","",null,null,null,null,null,null,232856,"Heizkreisverteiler HKV 6/9, 6 Heizkreise","On request",false,null,232856,633,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Vloerverdeler HKV 6/9, 6 groepen","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Heizkreisverteiler HKV 6/9, 6 Heizkreise","Heizkreisverteiler HKV 6/9, 6 Heizkreise"]
[null,232857,"Heizkreisverteiler HKV 8/9, 8 Heizkreise","On request","",null,null,null,null,null,null,232857,"Heizkreisverteiler HKV 8/9, 8 Heizkreise","On request",false,null,232857,734,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Vloerverdeler HKV 8/9, 8 groepen","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Heizkreisverteiler HKV 8/9, 8 Heizkreise","Heizkreisverteiler HKV 8/9, 8 Heizkreise"]
[null,232858,"Montageschiene AL 9","On request","",null,null,null,null,null,null,232858,"Montageschiene AL 9","On request",false,null,232858,155,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene AL 9","Montageschiene AL 9","Montageschiene AL 9","Montageschiene AL 9","Montagerail AL 9","Montageschiene AL 9","Montageschiene AL 9","Montageschiene AL 9","Montageschiene AL 9","Montageschiene AL 9","Montageschiene AL 9"]
[null,232859,"Überströmventil WS-ÜV","On request","",null,null,null,null,null,null,232859,"Überströmventil WS-ÜV","On request",false,null,232859,189,"On request","sur demande","på forespørgsel","op aanvraag","Überströmventil WS-ÜV","Überströmventil WS-ÜV","Überströmventil WS-ÜV","Überströmventil WS-ÜV","Overstroomventiel WS-ÜV","Überströmventil WS-ÜV","Überströmventil WS-ÜV","Überströmventil WS-ÜV","Überströmventil WS-ÜV","Überströmventil WS-ÜV","Überströmventil WS-ÜV"]
[null,227489,"Instantaneous water heater DHE 18 SL 25A","On request",{"$f":"IF(O911=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,227489,"Instantaneous water heater DHE 18 SL 25A","On request",{"$f":"IF(AND(B911=L911,C911=M911,D911=N911),FALSE,TRUE)","v":false},null,227489,762,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A","Doorstromer DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A","Instantaneous water heater DHE 18 SL 25A"]
[null,227490,"Instantaneous water heater DHE 18/21/24 SL","On request","",null,null,null,null,null,null,227490,"Instantaneous water heater DHE 18/21/24 SL","On request",false,null,227490,762,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL","Doorstromer DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL","Instantaneous water heater DHE 18/21/24 SL"]
[null,227491,"Instantaneous water heater DHE 27 SL","On request","",null,null,null,null,null,null,227491,"Instantaneous water heater DHE 27 SL","On request",false,null,227491,762,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHE 27 SL","Instantaneous water heater DHE 27 SL","Instantaneous water heater DHE 27 SL","Instantaneous water heater DHE 27 SL","Doorstromer DHE 27 SL","Instantaneous water heater DHE 27 SL","Instantaneous water heater DHE 27 SL","Instantaneous water heater DHE 27 SL","Instantaneous water heater DHE 27 SL","Instantaneous water heater DHE 27 SL","Instantaneous water heater DHE 27 SL"]
[null,233306,"Durchlauferhitzer DHE 18/21/24 SL LABS","On request","",null,null,null,null,null,null,233306,"Durchlauferhitzer DHE 18/21/24 SL LABS","On request",false,null,233306,874,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS","Doorstromer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS","Durchlauferhitzer DHE 18/21/24 SL LABS"]
[null,233678,"Durchlauferhitzer DEL 18/21/24 SL","On request","",null,null,null,null,null,null,233678,"Durchlauferhitzer DEL 18/21/24 SL","On request",false,null,233678,618,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL","Doorstromer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL","Durchlauferhitzer DEL 18/21/24 SL"]
[null,233679,"Durchlauferhitzer DEL 27 SL","On request","",null,null,null,null,null,null,233679,"Durchlauferhitzer DEL 27 SL","On request",false,null,233679,618,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DEL 27 SL","Durchlauferhitzer DEL 27 SL","Durchlauferhitzer DEL 27 SL","Durchlauferhitzer DEL 27 SL","Doorstromer DEL 27 SL","Durchlauferhitzer DEL 27 SL","Durchlauferhitzer DEL 27 SL","Durchlauferhitzer DEL 27 SL","Durchlauferhitzer DEL 27 SL","Durchlauferhitzer DEL 27 SL","Durchlauferhitzer DEL 27 SL"]
[null,232008,"Durchlauferhitzer DHB-E 11 SL","On request","",null,null,null,null,null,null,232008,"Durchlauferhitzer DHB-E 11 SL","On request",false,null,232008,489,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL","Doorstromer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL","Durchlauferhitzer DHB-E 11 SL"]
[null,232009,"Durchlauferhitzer DHB-E 13 SL","On request","",null,null,null,null,null,null,232009,"Durchlauferhitzer DHB-E 13 SL","On request",false,null,232009,489,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL","Doorstromer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL","Durchlauferhitzer DHB-E 13 SL"]
[null,232010,"Durchlauferhitzer DHB-E 18 SL 25A","On request","",null,null,null,null,null,null,232010,"Durchlauferhitzer DHB-E 18 SL 25A","On request",false,null,232010,489,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A","Doorstromer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A","Durchlauferhitzer DHB-E 18 SL 25A"]
[null,232011,"Durchlauferhitzer DHB-E 18/21/24 SL","On request","",null,null,null,null,null,null,232011,"Durchlauferhitzer DHB-E 18/21/24 SL","On request",false,null,232011,489,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL","Doorstromer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL","Durchlauferhitzer DHB-E 18/21/24 SL"]
[null,232012,"Durchlauferhitzer DHB-E 27 SL","On request","",null,null,null,null,null,null,232012,"Durchlauferhitzer DHB-E 27 SL","On request",false,null,232012,489,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL","Doorstromer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL","Durchlauferhitzer DHB-E 27 SL"]
[null,227608,"Instantaneous water heater DHB 18 ST","On request","",null,null,null,null,null,null,227608,"Instantaneous water heater DHB 18 ST","On request",false,null,227608,326,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB 18 ST","Instantaneous water heater DHB 18 ST","Instantaneous water heater DHB 18 ST","Instantaneous water heater DHB 18 ST","Doorstromer DHB 18 ST","Instantaneous water heater DHB 18 ST","Instantaneous water heater DHB 18 ST","Instantaneous water heater DHB 18 ST","Instantaneous water heater DHB 18 ST","Instantaneous water heater DHB 18 ST","Instantaneous water heater DHB 18 ST"]
[null,227609,"Instantaneous water heater DHB 21 ST","On request","",null,null,null,null,null,null,227609,"Instantaneous water heater DHB 21 ST","On request",false,null,227609,326,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB 21 ST","Instantaneous water heater DHB 21 ST","Instantaneous water heater DHB 21 ST","Instantaneous water heater DHB 21 ST","Doorstromer DHB 21 ST","Instantaneous water heater DHB 21 ST","Instantaneous water heater DHB 21 ST","Instantaneous water heater DHB 21 ST","Instantaneous water heater DHB 21 ST","Instantaneous water heater DHB 21 ST","Instantaneous water heater DHB 21 ST"]
[null,227610,"Instantaneous water heater DHB 24 ST","On request","",null,null,null,null,null,null,227610,"Instantaneous water heater DHB 24 ST","On request",false,null,227610,326,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB 24 ST","Instantaneous water heater DHB 24 ST","Instantaneous water heater DHB 24 ST","Instantaneous water heater DHB 24 ST","Doorstromer DHB 24 ST","Instantaneous water heater DHB 24 ST","Instantaneous water heater DHB 24 ST","Instantaneous water heater DHB 24 ST","Instantaneous water heater DHB 24 ST","Instantaneous water heater DHB 24 ST","Instantaneous water heater DHB 24 ST"]
[null,227611,"Instantaneous water heater DHB 27 ST","On request","",null,null,null,null,null,null,227611,"Instantaneous water heater DHB 27 ST","On request",false,null,227611,326,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB 27 ST","Instantaneous water heater DHB 27 ST","Instantaneous water heater DHB 27 ST","Instantaneous water heater DHB 27 ST","Doorstromer DHB 27 ST","Instantaneous water heater DHB 27 ST","Instantaneous water heater DHB 27 ST","Instantaneous water heater DHB 27 ST","Instantaneous water heater DHB 27 ST","Instantaneous water heater DHB 27 ST","Instantaneous water heater DHB 27 ST"]
[null,231999,"Instantaneous water heater HDB-E 12 control","On request","",null,null,null,null,null,null,231999,"Instantaneous water heater HDB-E 12 control","On request",false,null,231999,274,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer HDB-E 12","Instantaneous water heater HDB-E 12 control","Instantaneous water heater HDB-E 12 control","Instantaneous water heater HDB-E 12 control","Doorstromer HDB-E 12 control","Instantaneous water heater HDB-E 12 control","Instantaneous water heater HDB-E 12 control","Instantaneous water heater HDB-E 12 control","Instantaneous water heater HDB-E 12 control","Instantaneous water heater HDB-E 12 control","Instantaneous water heater HDB-E 12 control"]
[null,232000,"Instantaneous water heater HDB-E 18 control","On request","",null,null,null,null,null,null,232000,"Instantaneous water heater HDB-E 18 control","On request",false,null,232000,274,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer HDB-E 18","Instantaneous water heater HDB-E 18 control","Instantaneous water heater HDB-E 18 control","Instantaneous water heater HDB-E 18 control","Doorstromer HDB-E 18 control","Instantaneous water heater HDB-E 18 control","Instantaneous water heater HDB-E 18 control","Instantaneous water heater HDB-E 18 control","Instantaneous water heater HDB-E 18 control","Instantaneous water heater HDB-E 18 control","Instantaneous water heater HDB-E 18 control"]
[null,232001,"Instantaneous water heater HDB-E 21 control","On request","",null,null,null,null,null,null,232001,"Instantaneous water heater HDB-E 21 control","On request",false,null,232001,274,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer HDB-E 21","Instantaneous water heater HDB-E 21 control","Instantaneous water heater HDB-E 21 control","Instantaneous water heater HDB-E 21 control","Doorstromer HDB-E 21 control","Instantaneous water heater HDB-E 21 control","Instantaneous water heater HDB-E 21 control","Instantaneous water heater HDB-E 21 control","Instantaneous water heater HDB-E 21 control","Instantaneous water heater HDB-E 21 control","Instantaneous water heater HDB-E 21 control"]
[null,232002,"Instantaneous water heater HDB-E 24 control","On request","",null,null,null,null,null,null,232002,"Instantaneous water heater HDB-E 24 control","On request",false,null,232002,274,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer HDB-E 24","Instantaneous water heater HDB-E 24 control","Instantaneous water heater HDB-E 24 control","Instantaneous water heater HDB-E 24 control","Doorstromer HDB-E 24 control","Instantaneous water heater HDB-E 24 control","Instantaneous water heater HDB-E 24 control","Instantaneous water heater HDB-E 24 control","Instantaneous water heater HDB-E 24 control","Instantaneous water heater HDB-E 24 control","Instantaneous water heater HDB-E 24 control"]
[null,74301,"Instantaneous water heater DHF 13 C",307,"",null,null,null,null,null,null,74301,"Instantaneous water heater DHF 13 C",307,false,null,74301,370,307,505,"på forespørgsel",428,"Durchlauferhitzer DHF 13 C","Instantaneous water heater DHF 13 C","Instantaneous water heater DHF 13 C","Instantaneous water heater DHF 13 C","Hydraulische Doorstromer DHF 13 C","Instantaneous water heater DHF 13 C","Instantaneous water heater DHF 13 C","Instantaneous water heater DHF 13 C","Instantaneous water heater DHF 13 C","Instantaneous water heater DHF 13 C","Instantaneous water heater DHF 13 C"]
[null,74302,"Instantaneous water heater DHF 15 C",302,"",null,null,null,null,null,null,74302,"Instantaneous water heater DHF 15 C",302,false,null,74302,370,302,505,"på forespørgsel",428,"Durchlauferhitzer DHF 15 C","Instantaneous water heater DHF 15 C","Instantaneous water heater DHF 15 C","Instantaneous water heater DHF 15 C","Hydraulische Doorstromer DHF 15 C","Instantaneous water heater DHF 15 C","Instantaneous water heater DHF 15 C","Instantaneous water heater DHF 15 C","Instantaneous water heater DHF 15 C","Instantaneous water heater DHF 15 C","Instantaneous water heater DHF 15 C"]
[null,74303,"Instantaneous water heater DHF 18 C",304,"",null,null,null,null,null,null,74303,"Instantaneous water heater DHF 18 C",304,false,null,74303,370,304,505,"på forespørgsel",428,"Durchlauferhitzer DHF 18 C","Instantaneous water heater DHF 18 C","Instantaneous water heater DHF 18 C","Instantaneous water heater DHF 18 C","Hydraulische Doorstromer DHF 18 C","Instantaneous water heater DHF 18 C","Instantaneous water heater DHF 18 C","Instantaneous water heater DHF 18 C","Instantaneous water heater DHF 18 C","Instantaneous water heater DHF 18 C","Instantaneous water heater DHF 18 C"]
[null,74304,"Instantaneous water heater DHF 21 C",305,"",null,null,null,null,null,null,74304,"Instantaneous water heater DHF 21 C",305,false,null,74304,370,305,505,"på forespørgsel",428,"Durchlauferhitzer DHF 21 C","Instantaneous water heater DHF 21 C","Instantaneous water heater DHF 21 C","Instantaneous water heater DHF 21 C","Hydraulische Doorstromer DHF 21 C","Instantaneous water heater DHF 21 C","Instantaneous water heater DHF 21 C","Instantaneous water heater DHF 21 C","Instantaneous water heater DHF 21 C","Instantaneous water heater DHF 21 C","Instantaneous water heater DHF 21 C"]
[null,74305,"Instantaneous water heater DHF 24 C",309,"",null,null,null,null,null,null,74305,"Instantaneous water heater DHF 24 C",309,false,null,74305,370,309,505,"på forespørgsel",428,"Durchlauferhitzer DHF 24 C","Instantaneous water heater DHF 24 C","Instantaneous water heater DHF 24 C","Instantaneous water heater DHF 24 C","Hydraulische Doorstromer DHF 24 C","Instantaneous water heater DHF 24 C","Instantaneous water heater DHF 24 C","Instantaneous water heater DHF 24 C","Instantaneous water heater DHF 24 C","Instantaneous water heater DHF 24 C","Instantaneous water heater DHF 24 C"]
[null,222419,"Wireless remote control FFB 1 SL",266,"",null,null,null,null,null,null,222419,"Wireless remote control FFB 1 SL",266,false,null,222419,170,266,"sur demande","på forespørgsel",170,"Fernbedienung FFB 1 SL","Wireless remote control FFB 1 SL","Wireless remote control FFB 1 SL","Wireless remote control FFB 1 SL","Afstandsbediening FFB 1 SL","Wireless remote control FFB 1 SL","Wireless remote control FFB 1 SL","Wireless remote control FFB 1 SL","Wireless remote control FFB 1 SL","Wireless remote control FFB 1 SL","Wireless remote control FFB 1 SL"]
[null,223340,"Wireless remote control FFB 2 SL",188,"",null,null,null,null,null,null,223340,"Wireless remote control FFB 2 SL",188,false,null,223340,111,188,"sur demande","på forespørgsel",111,"Fernbedienung FFB 2 SL","Wireless remote control FFB 2 SL","Wireless remote control FFB 2 SL","Wireless remote control FFB 2 SL","Afstandsbediening FFB 2 SL","Wireless remote control FFB 2 SL","Wireless remote control FFB 2 SL","Wireless remote control FFB 2 SL","Wireless remote control FFB 2 SL","Wireless remote control FFB 2 SL","Wireless remote control FFB 2 SL"]
[null,169478,"Wireless remote control FFB 1",156,"",null,null,null,null,null,null,169478,"Wireless remote control FFB 1",156,false,null,169478,"auf Anfrage",156,"sur demande","på forespørgsel",173,"Fernbedienung FFB 1","Wireless remote control FFB 1","Wireless remote control FFB 1","Wireless remote control FFB 1","Afstandsbediening FFB 1","Wireless remote control FFB 1","Wireless remote control FFB 1","Wireless remote control FFB 1","Wireless remote control FFB 1","Wireless remote control FFB 1","Wireless remote control FFB 1"]
[null,169482,"Wireless remote control FFB 2",95,"",null,null,null,null,null,null,169482,"Wireless remote control FFB 2",95,false,null,169482,"auf Anfrage",95,"sur demande","på forespørgsel",114,"Fernbedienung FFB 2","Wireless remote control FFB 2","Wireless remote control FFB 2","Wireless remote control FFB 2","Afstandsbediening FFB 2","Wireless remote control FFB 2","Wireless remote control FFB 2","Wireless remote control FFB 2","Wireless remote control FFB 2","Wireless remote control FFB 2","Wireless remote control FFB 2"]
[null,221333,"Hard-wired remote control FB 1 SL",78,"",null,null,null,null,null,null,221333,"Hard-wired remote control FB 1 SL",78,false,null,221333,86,78,"sur demande","på forespørgsel",86,"Fernbedienung FB 1 SL","Hard-wired remote control FB 1 SL","Hard-wired remote control FB 1 SL","Hard-wired remote control FB 1 SL","Afstandsbediening FB 1 SL","Hard-wired remote control FB 1 SL","Hard-wired remote control FB 1 SL","Hard-wired remote control FB 1 SL","Hard-wired remote control FB 1 SL","Hard-wired remote control FB 1 SL","Hard-wired remote control FB 1 SL"]
[null,232613,"Einhebel-Wandarmatur MEKD",143,"",null,null,null,null,null,null,232613,"Einhebel-Wandarmatur MEKD",143,false,null,232613,156,143,"sur demande","på forespørgsel",156,"Einhebel-Wandarmatur MEKD","Einhebel-Wandarmatur MEKD","Einhebel-Wandarmatur MEKD","Einhebel-Wandarmatur MEKD","Eenhandel-Wandarmatuur MEKD","Einhebel-Wandarmatur MEKD","Einhebel-Wandarmatur MEKD","Einhebel-Wandarmatur MEKD","Einhebel-Wandarmatur MEKD","Einhebel-Wandarmatur MEKD","Einhebel-Wandarmatur MEKD"]
[null,232614,"Einhebel-Wandarmatur WEBD",191,"",null,null,null,null,null,null,232614,"Einhebel-Wandarmatur WEBD",191,false,null,232614,242,191,"sur demande","på forespørgsel",242,"Einhebel-Wandarmatur MEBD","Einhebel-Wandarmatur WEBD","Einhebel-Wandarmatur WEBD","Einhebel-Wandarmatur WEBD","Eenhandel-Wandarmatuur WEBD","Einhebel-Wandarmatur WEBD","Einhebel-Wandarmatur WEBD","Einhebel-Wandarmatur WEBD","Einhebel-Wandarmatur WEBD","Einhebel-Wandarmatur WEBD","Einhebel-Wandarmatur WEBD"]
[null,220291,"Mounting frame DH..","On request","",null,null,null,null,null,null,220291,"Mounting frame DH..","On request",false,null,220291,58.4,"On request","sur demande","på forespørgsel",58,"Universal-Montagerahmen Durchlauferhitzer","Mounting frame DH..","Mounting frame DH..","Mounting frame DH..","Universeel montageframe DH..","Mounting frame DH..","Mounting frame DH..","Mounting frame DH..","Mounting frame DH..","Mounting frame DH..","Mounting frame DH.."]
[null,222378,"Mounting frame DHF-C","On request","",null,null,null,null,null,null,222378,"Mounting frame DHF-C","On request",false,null,222378,68.7,"On request","sur demande","på forespørgsel",69,"Universal-Montagerahmen DHF-C","Mounting frame DHF-C","Mounting frame DHF-C","Mounting frame DHF-C","Montageframe DHF-C","Mounting frame DHF-C","Mounting frame DHF-C","Mounting frame DHF-C","Mounting frame DHF-C","Mounting frame DHF-C","Mounting frame DHF-C"]
[null,220290,"Offset installation DH..","On request","",null,null,null,null,null,null,220290,"Offset installation DH..","On request",false,null,220290,126,"On request","sur demande","på forespørgsel",126,"Rohrbausatz für Versatzmontage","Offset installation DH..","Offset installation DH..","Offset installation DH..","Leidingset DH..Versch. montage","Offset installation DH..","Offset installation DH..","Offset installation DH..","Offset installation DH..","Offset installation DH..","Offset installation DH.."]
[null,220510,"Gas boiler replacement DH..","On request","",null,null,null,null,null,null,220510,"Gas boiler replacement DH..","On request",false,null,220510,94.1,"On request","sur demande","på forespørgsel",94,"Rohrbausatz für Gas-Wasserheizer-Austausch","Gas boiler replacement DH..","Gas boiler replacement DH..","Gas boiler replacement DH..","Leidingset DH..Geiserverv.","Gas boiler replacement DH..","Gas boiler replacement DH..","Gas boiler replacement DH..","Gas boiler replacement DH..","Gas boiler replacement DH..","Gas boiler replacement DH.."]
[null,74019,"Assembly for surface mounting","On request","",null,null,null,null,null,null,74019,"Assembly for surface mounting","On request",false,null,74019,24,"On request","sur demande","på forespørgsel",24,"Montageset Aufputzinstallation Kupferrohr Löt","Assembly for surface mounting","Assembly for surface mounting","Assembly for surface mounting","Montageset Bouwset opbouw","Assembly for surface mounting","Assembly for surface mounting","Assembly for surface mounting","Assembly for surface mounting","Assembly for surface mounting","Assembly for surface mounting"]
[null,222380,"Assembly for surface mounting Cu Press.","On request","",null,null,null,null,null,null,222380,"Assembly for surface mounting Cu Press.","On request",false,null,222380,24,"On request","sur demande","på forespørgsel",24,"Montageset Aufputzinstallation Kupferrohr Press","Assembly for surface mounting Cu Press.","Assembly for surface mounting Cu Press.","Assembly for surface mounting Cu Press.","Bouwset opbouwinstallatie Cu Press.","Assembly for surface mounting Cu Press.","Assembly for surface mounting Cu Press.","Assembly for surface mounting Cu Press.","Assembly for surface mounting Cu Press.","Assembly for surface mounting Cu Press.","Assembly for surface mounting Cu Press."]
[null,222381,"Assembly for surface mounting Ku Press.","On request","",null,null,null,null,null,null,222381,"Assembly for surface mounting Ku Press.","On request",false,null,222381,24,"On request","sur demande","på forespørgsel",24,"Montageset Aufputzinstallation Kunststoffrohr Press","Assembly for surface mounting Ku Press.","Assembly for surface mounting Ku Press.","Assembly for surface mounting Ku Press.","Bouwset opbouwinstallatie Ku Press.","Assembly for surface mounting Ku Press.","Assembly for surface mounting Ku Press.","Assembly for surface mounting Ku Press.","Assembly for surface mounting Ku Press.","Assembly for surface mounting Ku Press.","Assembly for surface mounting Ku Press."]
[null,74326,"Plug G 1/2","On request","",null,null,null,null,null,null,74326,"Plug G 1/2","On request",false,null,74326,6.3,"On request","sur demande","på forespørgsel",6,"Bausatz Wasserstopfen G 1/2, 2 Stück","Plug G 1/2","Plug G 1/2","Plug G 1/2","Bouwset Stop G ½","Plug G 1/2","Plug G 1/2","Plug G 1/2","Plug G 1/2","Plug G 1/2","Plug G 1/2"]
[null,159876,"Plug-in adaptor DHB","On request","",null,null,null,null,null,null,159876,"Plug-in adaptor DHB","On request",false,null,159876,16.8,"On request","sur demande","på forespørgsel",17,"Steckadapter für DHB-Austausch","Plug-in adaptor DHB","Plug-in adaptor DHB","Plug-in adaptor DHB","Leidingset DHB Steekadapter ","Plug-in adaptor DHB","Plug-in adaptor DHB","Plug-in adaptor DHB","Plug-in adaptor DHB","Plug-in adaptor DHB","Plug-in adaptor DHB"]
[null,70565,"Undersink kit DH..","On request","",null,null,null,null,null,null,70565,"Undersink kit DH..","On request",false,null,70565,68.7,"On request","sur demande","på forespørgsel",69,"Rohrbausatz Untertischgerät","Undersink kit DH..","Undersink kit DH..","Undersink kit DH..","Bouwset onderbouw DH..","Undersink kit DH..","Undersink kit DH..","Undersink kit DH..","Undersink kit DH..","Undersink kit DH..","Undersink kit DH.."]
[null,2280,"Measuring jug","On request","",null,null,null,null,null,null,2280,"Measuring jug","On request",false,null,2280,34.200000000000003,"On request","sur demande","på forespørgsel",34,"Messbecher","Measuring jug","Measuring jug","Measuring jug","Montage-/reparatiehulp Maatbeker","Measuring jug","Measuring jug","Measuring jug","Measuring jug","Measuring jug","Measuring jug"]
[null,2283,"Thermometer","On request","",null,null,null,null,null,null,2283,"Thermometer","On request",false,null,2283,27.3,"On request","sur demande","på forespørgsel",27,"Taschen-Thermometer","Thermometer","Thermometer","Thermometer","Montage-/reparatiehulp Thermometer","Thermometer","Thermometer","Thermometer","Thermometer","Thermometer","Thermometer"]
[null,1786,"Automatic maximum demand controller LR-1-A",32,"",null,null,null,null,null,null,1786,"Automatic maximum demand controller LR-1-A",32,false,null,1786,41.5,32,"sur demande","på forespørgsel",42,"Lastabwurf-Relais LR-1-A","Automatic maximum demand controller LR-1-A","Automatic maximum demand controller LR-1-A","Automatic maximum demand controller LR-1-A","Stroomkeuzesrelais LR-1-A","Automatic maximum demand controller LR-1-A","Automatic maximum demand controller LR-1-A","Automatic maximum demand controller LR-1-A","Automatic maximum demand controller LR-1-A","Automatic maximum demand controller LR-1-A","Automatic maximum demand controller LR-1-A"]
[null,73864,"Central-Thermostat ZTA 3/4",103,"",null,null,null,null,null,null,73864,"Central-Thermostat ZTA 3/4",103,false,null,73864,101,103,150,"på forespørgsel",101,"Zentralthermostatarmatur ZTA 3/4","Central-Thermostat ZTA 3/4","Mitigeur thermostatique ZTA 3/4","Termostato principale ZTA 3/4","Thermostaat armatuur ZTA 3/4","centrální termostat ZTA 3/4","Centrálny termostat ZTA 3/4","Central-Thermostat ZTA 3/4","Központi termosztát ZTA 3/4","Keskustermostaatti ZTA 3/4","Central-Thermostat ZTA 3/4"]
[null,223409,"DHB-E oven connection set LRH 11/13","On request","",null,null,null,null,null,null,223409,"DHB-E oven connection set LRH 11/13","On request",false,null,223409,94,"On request","sur demande","på forespørgsel",94,"DHB-E Herd Anschluss-SET LRH 11/13","DHB-E oven connection set LRH 11/13","DHB-E oven connection set LRH 11/13","DHB-E oven connection set LRH 11/13","Fornuisaansluitset LRH 11/13","DHB-E oven connection set LRH 11/13","DHB-E oven connection set LRH 11/13","DHB-E oven connection set LRH 11/13","DHB-E oven connection set LRH 11/13","DHB-E oven connection set LRH 11/13","DHB-E oven connection set LRH 11/13"]
[null,230770,"Durchlauferhitzer DCE 11/13 compact",180,"",null,null,null,null,null,null,230770,"Durchlauferhitzer DCE 11/13 compact",180,false,null,230770,236,180,"sur demande","på forespørgsel",273,"Durchlauferhitzer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact","Doorstromer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact","Durchlauferhitzer DCE 11/13 compact"]
[null,230771,"Durchlauferhitzer DCE 11/13 compact RC",234,"",null,null,null,null,null,null,230771,"Durchlauferhitzer DCE 11/13 compact RC",234,false,null,230771,309,234,"sur demande","på forespørgsel",347,"Durchlauferhitzer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC","Doorstromer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC","Durchlauferhitzer DCE 11/13 compact RC"]
[null,233048,"DCE Herd Anschluss-SET LRH 11/13.1",465,"",null,null,null,null,null,null,233048,"DCE Herd Anschluss-SET LRH 11/13.1",465,false,null,233048,94,465,"sur demande","på forespørgsel",94,"DCE Herd Anschluss-SET LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1","DCE Haard aansluitset LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1","DCE Herd Anschluss-SET LRH 11/13.1"]
[null,231001,"Mini instantaneous water heater DEM 3 electronic",213,"",null,null,null,null,null,null,231001,"Mini instantaneous water heater DEM 3 electronic",213,false,null,231001,223,213,"sur demande","på forespørgsel",225,"Kleindurchlauferhitzer DEM 3","Mini instantaneous water heater DEM 3 electronic","Mini instantaneous water heater DEM 3 electronic","Mini instantaneous water heater DEM 3 electronic","Mini-doorstromer DEM 3 electronic","Mini instantaneous water heater DEM 3 electronic","Mini instantaneous water heater DEM 3 electronic","Mini instantaneous water heater DEM 3 electronic","Mini instantaneous water heater DEM 3 electronic","Mini instantaneous water heater DEM 3 electronic","Mini instantaneous water heater DEM 3 electronic"]
[null,231002,"Mini instantaneous water heater DEM 3/4/6 electronic",199,"",null,null,null,null,null,null,231002,"Mini instantaneous water heater DEM 3/4/6 electronic",199,false,null,231002,223,199,"sur demande","på forespørgsel",225,"Kleindurchlauferhitzer DEM 4","Mini instantaneous water heater DEM 3/4/6 electronic","Mini instantaneous water heater DEM 3/4/6 electronic","Mini instantaneous water heater DEM 3/4/6 electronic","Mini-doorstromer DEM 4 electronic","Mini instantaneous water heater DEM 3/4/6 electronic","Mini instantaneous water heater DEM 3/4/6 electronic","Mini instantaneous water heater DEM 3/4/6 electronic","Mini instantaneous water heater DEM 3/4/6 electronic","Mini instantaneous water heater DEM 3/4/6 electronic","Mini instantaneous water heater DEM 3/4/6 electronic"]
[null,231215,"Mini instantaneous water heater DEM 6 electronic",200,"",null,null,null,null,null,null,231215,"Mini instantaneous water heater DEM 6 electronic",200,false,null,231215,223,200,"sur demande","på forespørgsel",225,"Kleindurchlauferhitzer DEM 6","Mini instantaneous water heater DEM 6 electronic","Mini instantaneous water heater DEM 6 electronic","Mini instantaneous water heater DEM 6 electronic","Mini-doorstromer DEM 6 electronic","Mini instantaneous water heater DEM 6 electronic","Mini instantaneous water heater DEM 6 electronic","Mini instantaneous water heater DEM 6 electronic","Mini instantaneous water heater DEM 6 electronic","Mini instantaneous water heater DEM 6 electronic","Mini instantaneous water heater DEM 6 electronic"]
[null,232769,"Kleindurchlauferhitzer DEM 7",218,"",null,null,null,null,null,null,232769,"Kleindurchlauferhitzer DEM 7",218,false,null,232769,223,218,"sur demande","på forespørgsel",225,"Kleindurchlauferhitzer DEM 7","Kleindurchlauferhitzer DEM 7","Kleindurchlauferhitzer DEM 7","Kleindurchlauferhitzer DEM 7","Mini-doorstromer DEM 7 electronic","Kleindurchlauferhitzer DEM 7","Kleindurchlauferhitzer DEM 7","Kleindurchlauferhitzer DEM 7","Kleindurchlauferhitzer DEM 7","Kleindurchlauferhitzer DEM 7","Kleindurchlauferhitzer DEM 7"]
[null,185411,"Mini instantaneous water heater DNM 3",110,"",null,null,null,null,null,null,185411,"Mini instantaneous water heater DNM 3",110,false,null,185411,108,110,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DNM 3","Mini instantaneous water heater DNM 3","Mini instantaneous water heater DNM 3","Mini instantaneous water heater DNM 3","Minidoorstromer DNM 3","Mini instantaneous water heater DNM 3","Mini instantaneous water heater DNM 3","Mini instantaneous water heater DNM 3","Mini instantaneous water heater DNM 3","Mini instantaneous water heater DNM 3","Mini instantaneous water heater DNM 3"]
[null,185415,"Mini instantaneous water heater DNM 4",111,"",null,null,null,null,null,null,185415,"Mini instantaneous water heater DNM 4",111,false,null,185415,119,111,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DNM 4","Mini instantaneous water heater DNM 4","Mini instantaneous water heater DNM 4","Mini instantaneous water heater DNM 4","Minidoorstromer DNM 4","Mini instantaneous water heater DNM 4","Mini instantaneous water heater DNM 4","Mini instantaneous water heater DNM 4","Mini instantaneous water heater DNM 4","Mini instantaneous water heater DNM 4","Mini instantaneous water heater DNM 4"]
[null,185418,"Mini instantaneous water heater DNM 6",114,"",null,null,null,null,null,null,185418,"Mini instantaneous water heater DNM 6",114,false,null,185418,124,114,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DNM 6","Mini instantaneous water heater DNM 6","Mini instantaneous water heater DNM 6","Mini instantaneous water heater DNM 6","Minidoorstromer DNM 6","Mini instantaneous water heater DNM 6","Mini instantaneous water heater DNM 6","Mini instantaneous water heater DNM 6","Mini instantaneous water heater DNM 6","Mini instantaneous water heater DNM 6","Mini instantaneous water heater DNM 6"]
[null,185412,"Mini instantaneous water heater DNM 3 + MAW",163,"",null,null,null,null,null,null,185412,"Mini instantaneous water heater DNM 3 + MAW",163,false,null,185412,163,163,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW","Minidoorstromer DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW","Mini instantaneous water heater DNM 3 + MAW"]
[null,185413,"Mini instantaneous water heater DNM 3 + MAZ",182,"",null,null,null,null,null,null,185413,"Mini instantaneous water heater DNM 3 + MAZ",182,false,null,185413,163,182,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ","Minidoorstromer DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ","Mini instantaneous water heater DNM 3 + MAZ"]
[null,185414,"Mini instantaneous water heater DNM 3 + MAE",240,"",null,null,null,null,null,null,185414,"Mini instantaneous water heater DNM 3 + MAE",240,false,null,185414,210,240,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE","Minidoorstromer DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE","Mini instantaneous water heater DNM 3 + MAE"]
[null,185474,"Wall mounted mixer tap MAW",52,{"$f":"IF(O970=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,185474,"Wall mounted mixer tap MAW",52,false,null,185474,70,52,"sur demande","på forespørgsel","op aanvraag","Zweigriff-Armatur MAW","Wall mounted mixer tap MAW","Wall mounted mixer tap MAW","Wall mounted mixer tap MAW","Tweegreeps-Armatuur MAW","Wall mounted mixer tap MAW","Wall mounted mixer tap MAW","Wall mounted mixer tap MAW","Wall mounted mixer tap MAW","Wall mounted mixer tap MAW","Wall mounted mixer tap MAW"]
[null,185475,"Single hole mixer tap MAZ",70,"",null,null,null,null,null,null,185475,"Single hole mixer tap MAZ",70,false,null,185475,72,70,"sur demande","på forespørgsel","op aanvraag","Zweigriff-Armatur MAZ","Single hole mixer tap MAZ","Single hole mixer tap MAZ","Single hole mixer tap MAZ","Tweegreeps-Armatuur MAZ","Single hole mixer tap MAZ","Single hole mixer tap MAZ","Single hole mixer tap MAZ","Single hole mixer tap MAZ","Single hole mixer tap MAZ","Single hole mixer tap MAZ"]
[null,185476,"Mono-lever mixer tap MAE",126,"",null,null,null,null,null,null,185476,"Mono-lever mixer tap MAE",126,false,null,185476,139,126,"sur demande","på forespørgsel","op aanvraag","Einhebel-Mischarmatur MAE","Mono-lever mixer tap MAE","Mono-lever mixer tap MAE","Mono-lever mixer tap MAE","Eenhandel-Mengarmatuur MAE","Mono-lever mixer tap MAE","Mono-lever mixer tap MAE","Mono-lever mixer tap MAE","Mono-lever mixer tap MAE","Mono-lever mixer tap MAE","Mono-lever mixer tap MAE"]
[null,220813,"Mini instantaneous water heater DHM 3",155,"",null,null,null,null,null,null,220813,"Mini instantaneous water heater DHM 3",155,false,null,220813,167,155,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DHM 3","Mini instantaneous water heater DHM 3","Mini instantaneous water heater DHM 3","Mini instantaneous water heater DHM 3","Mini-doorstromer DHM 3","Mini instantaneous water heater DHM 3","Mini instantaneous water heater DHM 3","Mini instantaneous water heater DHM 3","Mini instantaneous water heater DHM 3","Mini instantaneous water heater DHM 3","Mini instantaneous water heater DHM 3"]
[null,220814,"Mini instantaneous water heater DHM 4",141,"",null,null,null,null,null,null,220814,"Mini instantaneous water heater DHM 4",141,{"$f":"IF(AND(B974=L974,C974=M974,D974=N974),FALSE,TRUE)","v":false},null,220814,175,141,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DHM 4","Mini instantaneous water heater DHM 4","Mini instantaneous water heater DHM 4","Mini instantaneous water heater DHM 4","Mini-doorstromer DHM 4","Mini instantaneous water heater DHM 4","Mini instantaneous water heater DHM 4","Mini instantaneous water heater DHM 4","Mini instantaneous water heater DHM 4","Mini instantaneous water heater DHM 4","Mini instantaneous water heater DHM 4"]
[null,185473,"Mini instantaneous water heater DHM 6",143,"",null,null,null,null,null,null,185473,"Mini instantaneous water heater DHM 6",143,false,null,185473,181,143,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DHM 6","Mini instantaneous water heater DHM 6","Mini instantaneous water heater DHM 6","Mini instantaneous water heater DHM 6","Mini-doorstromer DHM 6","Mini instantaneous water heater DHM 6","Mini instantaneous water heater DHM 6","Mini instantaneous water heater DHM 6","Mini instantaneous water heater DHM 6","Mini instantaneous water heater DHM 6","Mini instantaneous water heater DHM 6"]
[null,232789,"Kleindurchlauferhitzer DHM 7",159,"",null,null,null,null,null,null,232789,"Kleindurchlauferhitzer DHM 7",159,false,null,232789,181,159,"sur demande","på forespørgsel","op aanvraag","Kleindurchlauferhitzer DHM 7","Kleindurchlauferhitzer DHM 7","Kleindurchlauferhitzer DHM 7","Kleindurchlauferhitzer DHM 7","Mini-doorstromer DHM 7","Kleindurchlauferhitzer DHM 7","Kleindurchlauferhitzer DHM 7","Kleindurchlauferhitzer DHM 7","Kleindurchlauferhitzer DHM 7","Kleindurchlauferhitzer DHM 7","Kleindurchlauferhitzer DHM 7"]
[null,230957,"Senso fitting WEH",674,"",null,null,null,null,null,null,230957,"Senso fitting WEH",674,false,null,230957,544,674,"sur demande","på forespørgsel",544,"Sensor-Armatur WEH","Senso fitting WEH","Senso fitting WEH","Senso fitting WEH","Sensor armatuur WEH","Senso fitting WEH","Senso fitting WEH","Senso fitting WEH","Senso fitting WEH","Senso fitting WEH","Senso fitting WEH"]
[null,74286,"Water boiler EBK 5 G",262,"",null,null,null,null,null,null,74286,"Water boiler EBK 5 G",262,false,null,74286,254,262,"sur demande","på forespørgsel",356,"Kochendwassergerät EBK 5 G","Water boiler EBK 5 G","Water boiler EBK 5 G","Water boiler EBK 5 G","Kokendwatertoestel EBK 5 G","Water boiler EBK 5 G","Water boiler EBK 5 G","Water boiler EBK 5 G","Water boiler EBK 5 G","Water boiler EBK 5 G","Water boiler EBK 5 G"]
[null,74287,"Water boiler EBK 5 GA",252,"",null,null,null,null,null,null,74287,"Water boiler EBK 5 GA",252,false,null,74287,254,252,"sur demande","på forespørgsel",346,"Kochendwassergerät EBK 5 GA","Water boiler EBK 5 GA","Water boiler EBK 5 GA","Water boiler EBK 5 GA","Kokendwatertoestel EBK 5 GA","Water boiler EBK 5 GA","Water boiler EBK 5 GA","Water boiler EBK 5 GA","Water boiler EBK 5 GA","Water boiler EBK 5 GA","Water boiler EBK 5 GA"]
[null,74288,"Water boiler EBK 5 K",202,"",null,null,null,null,null,null,74288,"Water boiler EBK 5 K",202,false,null,74288,217,202,"sur demande","på forespørgsel",288,"Kochendwassergerät EBK 5 K","Water boiler EBK 5 K","Water boiler EBK 5 K","Water boiler EBK 5 K","Kokendwatertoestel EBK 5 K","Water boiler EBK 5 K","Water boiler EBK 5 K","Water boiler EBK 5 K","Water boiler EBK 5 K","Water boiler EBK 5 K","Water boiler EBK 5 K"]
[null,74289,"Water boiler KBA 5 KA",194,"",null,null,null,null,null,null,74289,"Water boiler KBA 5 KA",194,false,null,74289,213,194,"sur demande","på forespørgsel",255,"Kochendwassergerät KBA 5 KA","Water boiler KBA 5 KA","Water boiler KBA 5 KA","Water boiler KBA 5 KA","Kokendwatertoestel KBA 5 KA","Water boiler KBA 5 KA","Water boiler KBA 5 KA","Water boiler KBA 5 KA","Water boiler KBA 5 KA","Water boiler KBA 5 KA","Water boiler KBA 5 KA"]
[null,169951,"Drain valve for EBK 5 G/K",75,"",null,null,null,null,null,null,169951,"Drain valve for EBK 5 G/K",75,false,null,169951,72.099999999999994,75,"sur demande","på forespørgsel",72,"Ablaufarmatur EBK 5 G, EBK 5 K","Drain valve for EBK 5 G/K","Drain valve for EBK 5 G/K","Drain valve for EBK 5 G/K","Vervang aftapkraan EBK 5 G/K","Drain valve for EBK 5 G/K","Drain valve for EBK 5 G/K","Drain valve for EBK 5 G/K","Drain valve for EBK 5 G/K","Drain valve for EBK 5 G/K","Drain valve for EBK 5 G/K"]
[null,166491,"Drain valve for EBK 5 GSA/GA, KBA 5 KA",54,"",null,null,null,null,null,null,166491,"Drain valve for EBK 5 GSA/GA, KBA 5 KA",54,false,null,166491,65.400000000000006,54,"sur demande","på forespørgsel",65,"Ablaufarmatur EBK 5 GA, KBA 5 KA","Drain valve for EBK 5 GSA/GA, KBA 5 KA","Drain valve for EBK 5 GSA/GA, KBA 5 KA","Drain valve for EBK 5 GSA/GA, KBA 5 KA","Vervang aftapkraan EBK 5","Drain valve for EBK 5 GSA/GA, KBA 5 KA","Drain valve for EBK 5 GSA/GA, KBA 5 KA","Drain valve for EBK 5 GSA/GA, KBA 5 KA","Drain valve for EBK 5 GSA/GA, KBA 5 KA","Drain valve for EBK 5 GSA/GA, KBA 5 KA","Drain valve for EBK 5 GSA/GA, KBA 5 KA"]
[null,3770,"Drain valve for EBK 5 C",45,"",null,null,null,null,null,null,3770,"Drain valve for EBK 5 C",45,false,null,3770,65.400000000000006,45,"sur demande","på forespørgsel",66,"Ablaufarmatur EBK 5 C","Drain valve for EBK 5 C","Drain valve for EBK 5 C","Drain valve for EBK 5 C","Vervang aftapkraan EBK 5 C","Drain valve for EBK 5 C","Drain valve for EBK 5 C","Drain valve for EBK 5 C","Drain valve for EBK 5 C","Drain valve for EBK 5 C","Drain valve for EBK 5 C"]
[null,128907,"Outlet 120mm white",32,"",null,null,null,null,null,null,128907,"Outlet 120mm white",32,false,null,128907,27.3,32,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 200 mm weiß","Outlet 120mm white","Outlet 120mm white","Outlet 120mm white","Schwenkarm 200 mm wit","Outlet 120mm white","Outlet 120mm white","Outlet 120mm white","Outlet 120mm white","Outlet 120mm white","Outlet 120mm white"]
[null,128908,"Outlet 200mm white",28,"",null,null,null,null,null,null,128908,"Outlet 200mm white",28,false,null,128908,30.6,28,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 250 mm weiß","Outlet 200mm white","Outlet 200mm white","Outlet 200mm white","Schwenkarm 250 mm wit","Outlet 200mm white","Outlet 200mm white","Outlet 200mm white","Outlet 200mm white","Outlet 200mm white","Outlet 200mm white"]
[null,128909,"Outlet 300mm white",31,"",null,null,null,null,null,null,128909,"Outlet 300mm white",31,false,null,128909,34.200000000000003,31,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 300 mm weiß","Outlet 300mm white","Outlet 300mm white","Outlet 300mm white","Schwenkarm 300 mm wit","Outlet 300mm white","Outlet 300mm white","Outlet 300mm white","Outlet 300mm white","Outlet 300mm white","Outlet 300mm white"]
[null,128910,"Outlet 400mm white",26,"",null,null,null,null,null,null,128910,"Outlet 400mm white",26,false,null,128910,34.200000000000003,26,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 400 mm weiß","Outlet 400mm white","Outlet 400mm white","Outlet 400mm white","Schwenkarm 400 mm wit","Outlet 400mm white","Outlet 400mm white","Outlet 400mm white","Outlet 400mm white","Outlet 400mm white","Outlet 400mm white"]
[null,6075,"Outlet 120mm chrome",10,"",null,null,null,null,null,null,6075,"Outlet 120mm chrome",10,false,null,6075,16.8,10,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 120 mm verchromt","Outlet 120mm chrome","Outlet 120mm chrome","Outlet 120mm chrome","Schwenkarm 120 mm verchroomd","Outlet 120mm chrome","Outlet 120mm chrome","Outlet 120mm chrome","Outlet 120mm chrome","Outlet 120mm chrome","Outlet 120mm chrome"]
[null,6082,"Outlet 200mm chrome",14,"",null,null,null,null,null,null,6082,"Outlet 200mm chrome",14,false,null,6082,24,14,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 200 mm verchromt","Outlet 200mm chrome","Outlet 200mm chrome","Outlet 200mm chrome","Schwenkarm 200 mm verchroomd","Outlet 200mm chrome","Outlet 200mm chrome","Outlet 200mm chrome","Outlet 200mm chrome","Outlet 200mm chrome","Outlet 200mm chrome"]
[null,28923,"Outlet 250mm chrome",15,"",null,null,null,null,null,null,28923,"Outlet 250mm chrome",15,false,null,28923,27.3,15,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 250 mm verchromt","Outlet 250mm chrome","Outlet 250mm chrome","Outlet 250mm chrome","Schwenkarm 250 mm verchroomd","Outlet 250mm chrome","Outlet 250mm chrome","Outlet 250mm chrome","Outlet 250mm chrome","Outlet 250mm chrome","Outlet 250mm chrome"]
[null,6085,"Outlet 300mm chrome",17,"",null,null,null,null,null,null,6085,"Outlet 300mm chrome",17,false,null,6085,34.200000000000003,17,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 300 mm verchromt","Outlet 300mm chrome","Outlet 300mm chrome","Outlet 300mm chrome","Schwenkarm 300 mm verchroomd","Outlet 300mm chrome","Outlet 300mm chrome","Outlet 300mm chrome","Outlet 300mm chrome","Outlet 300mm chrome","Outlet 300mm chrome"]
[null,6087,"Outlet 400mm chrome",19,"",null,null,null,null,null,null,6087,"Outlet 400mm chrome",19,false,null,6087,34.200000000000003,19,"sur demande","på forespørgsel","op aanvraag","Schwenkarm EBK 400 mm verchromt","Outlet 400mm chrome","Outlet 400mm chrome","Outlet 400mm chrome","Schwenkarm 400 mm verchroomd","Outlet 400mm chrome","Outlet 400mm chrome","Outlet 400mm chrome","Outlet 400mm chrome","Outlet 400mm chrome","Outlet 400mm chrome"]
[null,232252,"Kochendwasserautomat SNU Hot inkl. Armatur",657,"",null,null,null,null,null,null,232252,"Kochendwasserautomat SNU Hot inkl. Armatur",657,false,null,232252,621,657,"sur demande","på forespørgsel","op aanvraag ","Heißwasserautomat SNU Hot","Kochendwasserautomat SNU Hot inkl. Armatur","Kochendwasserautomat SNU Hot inkl. Armatur","Kochendwasserautomat SNU Hot inkl. Armatur","Heetwaterautomaat SNU Hot incl. armatuur","Kochendwasserautomat SNU Hot inkl. Armatur","Kochendwasserautomat SNU Hot inkl. Armatur","Kochendwasserautomat SNU Hot inkl. Armatur","Kochendwasserautomat SNU Hot inkl. Armatur","Kochendwasserautomat SNU Hot inkl. Armatur","Kochendwasserautomat SNU Hot inkl. Armatur"]
[null,233231,"Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","On request","",null,null,null,null,null,null,233231,"Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","On request",false,null,233231,158,"On request","sur demande","på forespørgsel",158,"Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Ontkalkingsfilter Basis FKB (zonder filtercontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)","Entkalkungsfilter Basis FKB (ohne Filterkontrolle)"]
[null,233232,"Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","On request","",null,null,null,null,null,null,233232,"Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","On request",false,null,233232,197,"On request","sur demande","på forespørgsel",197,"Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Ontkalkingsfilter Comfort FKC (met Filtercontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)","Entkalkungsfilter Comfort FKC (mit Filterkontrolle)"]
[null,233230,"Ersatz-Filterkartuschen Entkalkung, 3 Stück","On request","",null,null,null,null,null,null,233230,"Ersatz-Filterkartuschen Entkalkung, 3 Stück","On request",false,null,233230,164,"On request","sur demande","på forespørgsel",164,"Ersatz-Filterkartuschen Entkalkung, 3 Stück","Ersatz-Filterkartuschen Entkalkung, 3 Stück","Ersatz-Filterkartuschen Entkalkung, 3 Stück","Ersatz-Filterkartuschen Entkalkung, 3 Stück","Reserve-Filterkaarsen Ontkalken, 3 stuks","Ersatz-Filterkartuschen Entkalkung, 3 Stück","Ersatz-Filterkartuschen Entkalkung, 3 Stück","Ersatz-Filterkartuschen Entkalkung, 3 Stück","Ersatz-Filterkartuschen Entkalkung, 3 Stück","Ersatz-Filterkartuschen Entkalkung, 3 Stück","Ersatz-Filterkartuschen Entkalkung, 3 Stück"]
[null,231251,"Wall mounted cylinder SHZ 30 LCD",561,"",null,null,null,null,null,null,231251,"Wall mounted cylinder SHZ 30 LCD",561,false,null,231251,712,561,"1.010,00","på forespørgsel",779,"Warmwasser-Wandspeicher SHZ 30 LCD","Wall mounted cylinder SHZ 30 LCD","Wall mounted cylinder SHZ 30 LCD","Wall mounted cylinder SHZ 30 LCD","Wandboiler SHZ 30 LCD ECO","Wall mounted cylinder SHZ 30 LCD","Wall mounted cylinder SHZ 30 LCD","Wall mounted cylinder SHZ 30 LCD","Wall mounted cylinder SHZ 30 LCD","Wall mounted cylinder SHZ 30 LCD","Wall mounted cylinder SHZ 30 LCD"]
[null,231252,"Wall mounted cylinder SHZ 50 LCD",588,"",null,null,null,null,null,null,231252,"Wall mounted cylinder SHZ 50 LCD",588,false,null,231252,758,588,"1.125,00","på forespørgsel",926,"Warmwasser-Wandspeicher SHZ 50 LCD","Wall mounted cylinder SHZ 50 LCD","Wall mounted cylinder SHZ 50 LCD","Wall mounted cylinder SHZ 50 LCD","Wandboiler SHZ 50 LCD ECO","Wall mounted cylinder SHZ 50 LCD","Wall mounted cylinder SHZ 50 LCD","Wall mounted cylinder SHZ 50 LCD","Wall mounted cylinder SHZ 50 LCD","Wall mounted cylinder SHZ 50 LCD","Wall mounted cylinder SHZ 50 LCD"]
[null,231253,"Wall mounted cylinder SHZ 80 LCD",630,"",null,null,null,null,null,null,231253,"Wall mounted cylinder SHZ 80 LCD",630,false,null,231253,712,630,"1.195,00","på forespørgsel",1136,"Warmwasser-Wandspeicher SHZ 80 LCD","Wall mounted cylinder SHZ 80 LCD","Wall mounted cylinder SHZ 80 LCD","Wall mounted cylinder SHZ 80 LCD","Wandboiler SHZ 80 LCD ECO","Wall mounted cylinder SHZ 80 LCD","Wall mounted cylinder SHZ 80 LCD","Wall mounted cylinder SHZ 80 LCD","Wall mounted cylinder SHZ 80 LCD","Wall mounted cylinder SHZ 80 LCD","Wall mounted cylinder SHZ 80 LCD"]
[null,231254,"Wall mounted cylinder SHZ 100 LCD",637,"",null,null,null,null,null,null,231254,"Wall mounted cylinder SHZ 100 LCD",637,false,null,231254,725,637,"1.215,00","på forespørgsel",1222,"Warmwasser-Wandspeicher SHZ 100 LCD","Wall mounted cylinder SHZ 100 LCD","Wall mounted cylinder SHZ 100 LCD","Wall mounted cylinder SHZ 100 LCD","Wandboiler SHZ 100 LCD ECO","Wall mounted cylinder SHZ 100 LCD","Wall mounted cylinder SHZ 100 LCD","Wall mounted cylinder SHZ 100 LCD","Wall mounted cylinder SHZ 100 LCD","Wall mounted cylinder SHZ 100 LCD","Wall mounted cylinder SHZ 100 LCD"]
[null,231255,"Wall mounted cylinder SHZ 120 LCD",681,"",null,null,null,null,null,null,231255,"Wall mounted cylinder SHZ 120 LCD",681,false,null,231255,1005,681,"1.285,00","på forespørgsel",1442,"Warmwasser-Wandspeicher SHZ 120 LCD","Wall mounted cylinder SHZ 120 LCD","Wall mounted cylinder SHZ 120 LCD","Wall mounted cylinder SHZ 120 LCD","Wandboiler SHZ 120 LCD ECO","Wall mounted cylinder SHZ 120 LCD","Wall mounted cylinder SHZ 120 LCD","Wall mounted cylinder SHZ 120 LCD","Wall mounted cylinder SHZ 120 LCD","Wall mounted cylinder SHZ 120 LCD","Wall mounted cylinder SHZ 120 LCD"]
[null,231256,"Wall mounted cylinder SHZ 150 LCD",733,"",null,null,null,null,null,null,231256,"Wall mounted cylinder SHZ 150 LCD",733,false,null,231256,1061,733,"1.365,00","på forespørgsel",1678,"Warmwasser-Wandspeicher SHZ 150 LCD","Wall mounted cylinder SHZ 150 LCD","Wall mounted cylinder SHZ 150 LCD","Wall mounted cylinder SHZ 150 LCD","Wandboiler SHZ 150 LCD ECO","Wall mounted cylinder SHZ 150 LCD","Wall mounted cylinder SHZ 150 LCD","Wall mounted cylinder SHZ 150 LCD","Wall mounted cylinder SHZ 150 LCD","Wall mounted cylinder SHZ 150 LCD","Wall mounted cylinder SHZ 150 LCD"]
[null,73047,"Warm water cylinder SH 30 S",516,"",null,null,null,null,null,null,73047,"Warm water cylinder SH 30 S",516,false,null,73047,676,516,"sur demande","på forespørgsel",742,"Warmwasser-Wandspeicher SH 30 S","Warm water cylinder SH 30 S","Warm water cylinder SH 30 S","Warm water cylinder SH 30 S","Wandboiler SH 30 S","Warm water cylinder SH 30 S","Warm water cylinder SH 30 S","Warm water cylinder SH 30 S","Warm water cylinder SH 30 S","Warm water cylinder SH 30 S","Warm water cylinder SH 30 S"]
[null,73048,"Warm water cylinder SH 50 S",546,"",null,null,null,null,null,null,73048,"Warm water cylinder SH 50 S",546,false,null,73048,714,546,"sur demande","på forespørgsel",782,"Warmwasser-Wandspeicher SH 50 S","Warm water cylinder SH 50 S","Warm water cylinder SH 50 S","Warm water cylinder SH 50 S","Wandboiler SH 50 S","Warm water cylinder SH 50 S","Warm water cylinder SH 50 S","Warm water cylinder SH 50 S","Warm water cylinder SH 50 S","Warm water cylinder SH 50 S","Warm water cylinder SH 50 S"]
[null,73049,"Warm water cylinder SH 80 S",590,"",null,null,null,null,null,null,73049,"Warm water cylinder SH 80 S",590,false,null,73049,678,590,"sur demande","på forespørgsel",861,"Warmwasser-Wandspeicher SH 80 S","Warm water cylinder SH 80 S","Warm water cylinder SH 80 S","Warm water cylinder SH 80 S","Wandboiler SH 80 S","Warm water cylinder SH 80 S","Warm water cylinder SH 80 S","Warm water cylinder SH 80 S","Warm water cylinder SH 80 S","Warm water cylinder SH 80 S","Warm water cylinder SH 80 S"]
[null,73050,"Warm water cylinder SH 100 S",602,"",null,null,null,null,null,null,73050,"Warm water cylinder SH 100 S",602,false,null,73050,693,602,"sur demande","på forespørgsel",867,"Warmwasser-Wandspeicher SH 100 S","Warm water cylinder SH 100 S","Warm water cylinder SH 100 S","Warm water cylinder SH 100 S","Wandboiler SH 100 S","Warm water cylinder SH 100 S","Warm water cylinder SH 100 S","Warm water cylinder SH 100 S","Warm water cylinder SH 100 S","Warm water cylinder SH 100 S","Warm water cylinder SH 100 S"]
[null,73051,"Warm water cylinder SH 120 S",651,"",null,null,null,null,null,null,73051,"Warm water cylinder SH 120 S",651,false,null,73051,965,651,"sur demande","på forespørgsel",931,"Warmwasser-Wandspeicher SH 120 S","Warm water cylinder SH 120 S","Warm water cylinder SH 120 S","Warm water cylinder SH 120 S","Wandboiler SH 120 S","Warm water cylinder SH 120 S","Warm water cylinder SH 120 S","Warm water cylinder SH 120 S","Warm water cylinder SH 120 S","Warm water cylinder SH 120 S","Warm water cylinder SH 120 S"]
[null,73052,"Warm water cylinder SH 150 S",701,"",null,null,null,null,null,null,73052,"Warm water cylinder SH 150 S",701,false,null,73052,1017,701,"sur demande","på forespørgsel",995,"Warmwasser-Wandspeicher SH 150 S","Warm water cylinder SH 150 S","Warm water cylinder SH 150 S","Warm water cylinder SH 150 S","Wandboiler SH 150 S","Warm water cylinder SH 150 S","Warm water cylinder SH 150 S","Warm water cylinder SH 150 S","Warm water cylinder SH 150 S","Warm water cylinder SH 150 S","Warm water cylinder SH 150 S"]
[null,73111,"Wall mounted cylinder HFA-Z 30","On request","",null,null,null,null,null,null,73111,"Wall mounted cylinder HFA-Z 30","On request",false,null,73111,604,"On request",825,"på forespørgsel","op aanvraag","Warmwasser-Wandspeicher HFA-Z 30","Wall mounted cylinder HFA-Z 30","Wall mounted cylinder HFA-Z 30","Wall mounted cylinder HFA-Z 30","Wandboiler HFA-Z 30","Wall mounted cylinder HFA-Z 30","Wall mounted cylinder HFA-Z 30","Wall mounted cylinder HFA-Z 30","Wall mounted cylinder HFA-Z 30","Wall mounted cylinder HFA-Z 30","Wall mounted cylinder HFA-Z 30"]
[null,74467,"Wall mounted cylinder HFA-Z 80","On request","",null,null,null,null,null,null,74467,"Wall mounted cylinder HFA-Z 80","On request",false,null,74467,545,"On request",925,"på forespørgsel","op aanvraag","Warmwasser-Wandspeicher HFA-Z 80","Wall mounted cylinder HFA-Z 80","Wall mounted cylinder HFA-Z 80","Wall mounted cylinder HFA-Z 80","Wandboiler HFA-Z 80","Wall mounted cylinder HFA-Z 80","Wall mounted cylinder HFA-Z 80","Wall mounted cylinder HFA-Z 80","Wall mounted cylinder HFA-Z 80","Wall mounted cylinder HFA-Z 80","Wall mounted cylinder HFA-Z 80"]
[null,73112,"Wall mounted cylinder HFA/EB 80 Z","On request","",null,null,null,null,null,null,73112,"Wall mounted cylinder HFA/EB 80 Z","On request",false,null,73112,560,"On request",880,"på forespørgsel","op aanvraag","Warmwasser-Wandspeicher HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z","Wandboiler HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z","Wall mounted cylinder HFA/EB 80 Z"]
[null,74469,"Wall mounted cylinder HFA-Z 100","On request","",null,null,null,null,null,null,74469,"Wall mounted cylinder HFA-Z 100","On request",false,null,74469,573,"On request",935,"på forespørgsel","op aanvraag","Warmwasser-Wandspeicher HFA-Z 100","Wall mounted cylinder HFA-Z 100","Wall mounted cylinder HFA-Z 100","Wall mounted cylinder HFA-Z 100","Wandboiler HFA-Z 100","Wall mounted cylinder HFA-Z 100","Wall mounted cylinder HFA-Z 100","Wall mounted cylinder HFA-Z 100","Wall mounted cylinder HFA-Z 100","Wall mounted cylinder HFA-Z 100","Wall mounted cylinder HFA-Z 100"]
[null,73114,"Wall mounted cylinder HFA-Z 150","On request","",null,null,null,null,null,null,73114,"Wall mounted cylinder HFA-Z 150","On request",false,null,73114,750,"On request","1.075,00","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher HFA-Z 150","Wall mounted cylinder HFA-Z 150","Wall mounted cylinder HFA-Z 150","Wall mounted cylinder HFA-Z 150","Wandboiler HFA-Z 150","Wall mounted cylinder HFA-Z 150","Wall mounted cylinder HFA-Z 150","Wall mounted cylinder HFA-Z 150","Wall mounted cylinder HFA-Z 150","Wall mounted cylinder HFA-Z 150","Wall mounted cylinder HFA-Z 150"]
[null,73062,"Wall mounted cylinder SNZ 80 S","On request","",null,null,null,null,null,null,73062,"Wall mounted cylinder SNZ 80 S","On request",false,null,73062,984,"On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher SNZ 80 S","Wall mounted cylinder SNZ 80 S","Wall mounted cylinder SNZ 80 S","Wall mounted cylinder SNZ 80 S","Wandboiler SNZ 80 S","Wall mounted cylinder SNZ 80 S","Wall mounted cylinder SNZ 80 S","Wall mounted cylinder SNZ 80 S","Wall mounted cylinder SNZ 80 S","Wall mounted cylinder SNZ 80 S","Wall mounted cylinder SNZ 80 S"]
[null,73059,"Wall mounted cylinder SHD 30 S",771,"",null,null,null,null,null,null,73059,"Wall mounted cylinder SHD 30 S",771,false,null,73059,1097,771,"1.150,00","på forespørgsel",1141,"Durchlaufspeicher SHD 30 S","Wall mounted cylinder SHD 30 S","Wall mounted cylinder SHD 30 S","Wall mounted cylinder SHD 30 S","Doorstroomboiler SHD 30 S","Wall mounted cylinder SHD 30 S","Wall mounted cylinder SHD 30 S","Wall mounted cylinder SHD 30 S","Wall mounted cylinder SHD 30 S","Wall mounted cylinder SHD 30 S","Wall mounted cylinder SHD 30 S"]
[null,73060,"Wall mounted cylinder SHD 100 S",854,"",null,null,null,null,null,null,73060,"Wall mounted cylinder SHD 100 S",854,false,null,73060,1450,854,"1.270,00","på forespørgsel",1381,"Durchlaufspeicher SHD 100 S","Wall mounted cylinder SHD 100 S","Wall mounted cylinder SHD 100 S","Wall mounted cylinder SHD 100 S","Doorstroomboiler SHD 100 S","Wall mounted cylinder SHD 100 S","Wall mounted cylinder SHD 100 S","Wall mounted cylinder SHD 100 S","Wall mounted cylinder SHD 100 S","Wall mounted cylinder SHD 100 S","Wall mounted cylinder SHD 100 S"]
[null,221470,"Ventilation device LWA 100",2786,"",null,null,null,null,null,null,221470,"Ventilation device LWA 100",2786,false,null,221470,2499,2786,"3.335,00","på forespørgsel",2499,"Warmwasser-Wärmepumpe LWA 100","Ventilation device LWA 100","LWA 100","Ventilation device LWA 100","Centraal ventilatietoestel  LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100","Ventilation device LWA 100"]
[null,233480,"Sicherheitsgruppe KV 30",83,"",null,null,null,null,null,null,233480,"Sicherheitsgruppe KV 30",83,false,null,233480,94,83,"sur demande","på forespørgsel",94,"Sicherheitsgruppe KV 30","Sicherheitsgruppe KV 30","Sicherheitsgruppe KV 30","Sicherheitsgruppe KV 30","Veiligheidsgroep KV 30","Sicherheitsgruppe KV 30","Sicherheitsgruppe KV 30","Sicherheitsgruppe KV 30","Sicherheitsgruppe KV 30","Sicherheitsgruppe KV 30","Sicherheitsgruppe KV 30"]
[null,233481,"Sicherheitsgruppe KV 40",127,"",null,null,null,null,null,null,233481,"Sicherheitsgruppe KV 40",127,false,null,233481,136,127,"sur demande","på forespørgsel",136,"Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Veiligheidsgroep KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40"]
[null,74143,"Cover KV","On request","",null,null,null,null,null,null,74143,"Cover KV","On request",false,null,74143,47,"On request","sur demande","på forespørgsel",47,"Abdeckhaube KV","Cover KV","Cover KV","Cover KV","KV Afdekkap ","Cover KV","Cover KV","Cover KV","Cover KV","Cover KV","Cover KV"]
[null,221123,"Small water heater SN 5 SL","On request","",null,null,null,null,null,null,221123,"Small water heater SN 5 SL","On request",false,null,221123,160,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SN 5 SL","Small water heater SN 5 SL","Small water heater SN 5 SL","Small water heater SN 5 SL","Kleine boiler drukloos SN 5 SL","Small water heater SN 5 SL","Small water heater SN 5 SL","Small water heater SN 5 SL","Small water heater SN 5 SL","Small water heater SN 5 SL","Small water heater SN 5 SL"]
[null,221115,"Small water heater SNU 5 SL","On request","",null,null,null,null,null,null,221115,"Small water heater SNU 5 SL","On request",false,null,221115,144,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SNU 5 SL","Small water heater SNU 5 SL","Small water heater SNU 5 SL","Small water heater SNU 5 SL","Kleine boiler drukloos SNU 5 SL","Small water heater SNU 5 SL","Small water heater SNU 5 SL","Small water heater SNU 5 SL","Small water heater SNU 5 SL","Small water heater SNU 5 SL","Small water heater SNU 5 SL"]
[null,221116,"Small water heater SNU 5 SL 1 KW","On request","",null,null,null,null,null,null,221116,"Small water heater SNU 5 SL 1 KW","On request",false,null,221116,164,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SNU 5 SL, 1 KW","Small water heater SNU 5 SL 1 KW","Small water heater SNU 5 SL 1 KW","Small water heater SNU 5 SL 1 KW","Kleine boiler drukloos SNU 5 SL 1 KW","Small water heater SNU 5 SL 1 KW","Small water heater SNU 5 SL 1 KW","Small water heater SNU 5 SL 1 KW","Small water heater SNU 5 SL 1 KW","Small water heater SNU 5 SL 1 KW","Small water heater SNU 5 SL 1 KW"]
[null,222191,"Small water heater SN 10 SL","On request","",null,null,null,null,null,null,222191,"Small water heater SN 10 SL","On request",false,null,222191,283,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SN 10 SL","Small water heater SN 10 SL","Small water heater SN 10 SL","Small water heater SN 10 SL","Kleine boiler drukloos SN 10 SL","Small water heater SN 10 SL","Small water heater SN 10 SL","Small water heater SN 10 SL","Small water heater SN 10 SL","Small water heater SN 10 SL","Small water heater SN 10 SL"]
[null,222197,"Small water heater SNU 10 SL","On request","",null,null,null,null,null,null,222197,"Small water heater SNU 10 SL","On request",false,null,222197,287,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SNU 10 SL","Small water heater SNU 10 SL","Small water heater SNU 10 SL","Small water heater SNU 10 SL","Kleine boiler drukloos SNU 10 SL","Small water heater SNU 10 SL","Small water heater SNU 10 SL","Small water heater SNU 10 SL","Small water heater SNU 10 SL","Small water heater SNU 10 SL","Small water heater SNU 10 SL"]
[null,222202,"Small water heater SN 15 SL 2 KW","On request","",null,null,null,null,null,null,222202,"Small water heater SN 15 SL 2 KW","On request",false,null,222202,455,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SN 15 SL, 2 KW","Small water heater SN 15 SL 2 KW","Small water heater SN 15 SL 2 KW","Small water heater SN 15 SL 2 KW","Kleine boiler drukloos SN 15 SL 2 KW","Small water heater SN 15 SL 2 KW","Small water heater SN 15 SL 2 KW","Small water heater SN 15 SL 2 KW","Small water heater SN 15 SL 2 KW","Small water heater SN 15 SL 2 KW","Small water heater SN 15 SL 2 KW"]
[null,222203,"Small water heater SN 15 SL 3,3 KW",182,"",null,null,null,null,null,null,222203,"Small water heater SN 15 SL 3,3 KW",182,false,null,222203,463,182,490,"på forespørgsel","op aanvraag","Kleinspeicher SN 15 SL, 3,3 KW","Small water heater SN 15 SL 3,3 KW","Small water heater SN 15 SL 3,3 KW","Small water heater SN 15 SL 3,3 KW","Kleine boiler drukloos SN 15 SL 3,3 KW","Small water heater SN 15 SL 3,3 KW","Small water heater SN 15 SL 3,3 KW","Small water heater SN 15 SL 3,3 KW","Small water heater SN 15 SL 3,3 KW","Small water heater SN 15 SL 3,3 KW","Small water heater SN 15 SL 3,3 KW"]
[null,221120,"Small water heater SNU 5 SL + WST-W","On request","",null,null,null,null,null,null,221120,"Small water heater SNU 5 SL + WST-W","On request",false,null,221120,166,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W","Kleine boiler drukloos SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W","Small water heater SNU 5 SL + WST-W"]
[null,222173,"Small water heater SNU 5 SL + MAE-K",258,{"$f":"IF(O1030=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,222173,"Small water heater SNU 5 SL + MAE-K",258,false,null,222173,214,258,435,"på forespørgsel","op aanvraag","Kleinspeicher SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K","Kleine boiler drukloos SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K","Small water heater SNU 5 SL + MAE-K"]
[null,222172,"Small water heater ",218,"",null,null,null,null,null,null,222172,"Small water heater ",218,false,null,222172,192,218,370,"på forespørgsel","op aanvraag","Kleinspeicher SNU 5 SL + MAE-W","Small water heater ","Small water heater ","Small water heater ","Kleine boiler drukloos SNU 5 SL + MAE-W","Small water heater ","Small water heater ","Small water heater ","Small water heater ","Small water heater ","Small water heater "]
[null,222175,"Small water heater UFP 5 t","On request","",null,null,null,null,null,null,222175,"Small water heater UFP 5 t","On request",false,null,222175,84,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher UFP 5 t","Small water heater UFP 5 t","Small water heater UFP 5 t","Small water heater UFP 5 t","Kleine boiler drukloos UFP 5 t","Small water heater UFP 5 t","Small water heater UFP 5 t","Small water heater UFP 5 t","Small water heater UFP 5 t","Small water heater UFP 5 t","Small water heater UFP 5 t"]
[null,222158,"Small water heater UFP 5 h",93,"",null,null,null,null,null,null,222158,"Small water heater UFP 5 h",93,false,null,222158,99,93,160,"på forespørgsel","op aanvraag","Kleinspeicher UFP 5 h","Small water heater UFP 5 h","Small water heater UFP 5 h","Small water heater UFP 5 h","Kleine boiler drukloos UFP 5 h","Small water heater UFP 5 h","Small water heater UFP 5 h","Small water heater UFP 5 h","Small water heater UFP 5 h","Small water heater UFP 5 h","Small water heater UFP 5 h"]
[null,232804,"Kleinspeicher drucklos UFP 5 t LABS","On request","",null,null,null,null,null,null,232804,"Kleinspeicher drucklos UFP 5 t LABS","On request",{"$f":"IF(AND(B1034=L1034,C1034=M1034,D1034=N1034),FALSE,TRUE)","v":false},null,232804,99,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS","Kleine boiler drukloos UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS","Kleinspeicher drucklos UFP 5 t LABS"]
[null,233076,"Kleinspeicher UFP 5 h LABS","On request","",null,null,null,null,null,null,233076,"Kleinspeicher UFP 5 h LABS","On request",false,null,233076,134,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher UFP 5 h LABS","Kleinspeicher UFP 5 h LABS","Kleinspeicher UFP 5 h LABS","Kleinspeicher UFP 5 h LABS","Kleine boiler drukloos UFP 5 h LABS","Kleinspeicher UFP 5 h LABS","Kleinspeicher UFP 5 h LABS","Kleinspeicher UFP 5 h LABS","Kleinspeicher UFP 5 h LABS","Kleinspeicher UFP 5 h LABS","Kleinspeicher UFP 5 h LABS"]
[null,222177,"Small water heater UFP 5 t + TWS 2","On request","",null,null,null,null,null,null,222177,"Small water heater UFP 5 t + TWS 2","On request",false,null,222177,119,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2","Kleine boiler drukloos UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2","Small water heater UFP 5 t + TWS 2"]
[null,222159,"Small water heater UFP 5 h + VL","On request","",null,null,null,null,null,null,222159,"Small water heater UFP 5 h + VL","On request",false,null,222159,138,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher UFP 5 h + VL","Small water heater UFP 5 h + VL","Small water heater UFP 5 h + VL","Small water heater UFP 5 h + VL","Kleine boiler drukloos UFP 5 h + VL","Small water heater UFP 5 h + VL","Small water heater UFP 5 h + VL","Small water heater UFP 5 h + VL","Small water heater UFP 5 h + VL","Small water heater UFP 5 h + VL","Small water heater UFP 5 h + VL"]
[null,232045,"Small water heater UFP 5 t + Mischarmatur EMK","On request","",null,null,null,null,null,null,232045,"Small water heater UFP 5 t + Mischarmatur EMK","On request",false,null,232045,144,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher UFP 5 t + EMK","Small water heater UFP 5 t + Mischarmatur EMK","Small water heater UFP 5 t + Mischarmatur EMK","Small water heater UFP 5 t + Mischarmatur EMK","Kleine boiler drukloos UFP 5 t + Mengarmatuur EMK","Small water heater UFP 5 t + Mischarmatur EMK","Small water heater UFP 5 t + Mischarmatur EMK","Small water heater UFP 5 t + Mischarmatur EMK","Small water heater UFP 5 t + Mischarmatur EMK","Small water heater UFP 5 t + Mischarmatur EMK","Small water heater UFP 5 t + Mischarmatur EMK"]
[null,232046,"Small water heater UFP 5 t + Mischarmatur EMW","On request","",null,null,null,null,null,null,232046,"Small water heater UFP 5 t + Mischarmatur EMW","On request",false,null,232046,132,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher UFP 5 t + EMW","Small water heater UFP 5 t + Mischarmatur EMW","Small water heater UFP 5 t + Mischarmatur EMW","Small water heater UFP 5 t + Mischarmatur EMW","Kleine boiler drukloos UFP 5 t + Mengarmatuur EMW","Small water heater UFP 5 t + Mischarmatur EMW","Small water heater UFP 5 t + Mischarmatur EMW","Small water heater UFP 5 t + Mischarmatur EMW","Small water heater UFP 5 t + Mischarmatur EMW","Small water heater UFP 5 t + Mischarmatur EMW","Small water heater UFP 5 t + Mischarmatur EMW"]
[null,222205,"Shower boiler EB 15 SL 2 KW","On request","",null,null,null,null,null,null,222205,"Shower boiler EB 15 SL 2 KW","On request",false,null,222205,499,"On request","sur demande","på forespørgsel","op aanvraag","Duschboiler EB 15 SL, 2 KW","Shower boiler EB 15 SL 2 KW","Shower boiler EB 15 SL 2 KW","Shower boiler EB 15 SL 2 KW","Doucheboiler EB 15 SL 2 KW","Shower boiler EB 15 SL 2 KW","Shower boiler EB 15 SL 2 KW","Shower boiler EB 15 SL 2 KW","Shower boiler EB 15 SL 2 KW","Shower boiler EB 15 SL 2 KW","Shower boiler EB 15 SL 2 KW"]
[null,222206,"Shower boiler EB 15 SL 3,3 KW","On request","",null,null,null,null,null,null,222206,"Shower boiler EB 15 SL 3,3 KW","On request",false,null,222206,508,"On request","sur demande","på forespørgsel","op aanvraag","Duschboiler EB 15 SL, 3,3 KW","Shower boiler EB 15 SL 3,3 KW","Shower boiler EB 15 SL 3,3 KW","Shower boiler EB 15 SL 3,3 KW","Doucheboiler EB 15 SL 3,3 KW","Shower boiler EB 15 SL 3,3 KW","Shower boiler EB 15 SL 3,3 KW","Shower boiler EB 15 SL 3,3 KW","Shower boiler EB 15 SL 3,3 KW","Shower boiler EB 15 SL 3,3 KW","Shower boiler EB 15 SL 3,3 KW"]
[null,232620,"Temperierarmatur WST",84,"",null,null,null,null,null,null,232620,"Temperierarmatur WST",84,false,null,232620,85,84,155,"på forespørgsel","op aanvraag","Temperierarmatur WST","Temperierarmatur WST","Temperierarmatur WST","Temperierarmatur WST","Mengarmatuur WST Serie Elnor Twin","Temperierarmatur WST","Temperierarmatur WST","Temperierarmatur WST","Temperierarmatur WST","Temperierarmatur WST","Temperierarmatur WST"]
[null,232604,"Temperierarmatur WUT",87,"",null,null,null,null,null,null,232604,"Temperierarmatur WUT",87,false,null,232604,97,87,160,"på forespørgsel","op aanvraag","Temperierarmatur WUT","Temperierarmatur WUT","Temperierarmatur WUT","Temperierarmatur WUT","Mengarmatuur WUT Serie Elnor Twin","Temperierarmatur WUT","Temperierarmatur WUT","Temperierarmatur WUT","Temperierarmatur WUT","Temperierarmatur WUT","Temperierarmatur WUT"]
[null,232612,"Einhebel-Mischarmatur MEW",121,"",null,null,null,null,null,null,232612,"Einhebel-Mischarmatur MEW",121,false,null,232612,163,121,215,"på forespørgsel","op aanvraag","Einhebel-Mischarmatur MEW","Einhebel-Mischarmatur MEW","Einhebel-Mischarmatur MEW","Einhebel-Mischarmatur MEW","Eenhandel mengarmatuur MEW","Einhebel-Mischarmatur MEW","Einhebel-Mischarmatur MEW","Einhebel-Mischarmatur MEW","Einhebel-Mischarmatur MEW","Einhebel-Mischarmatur MEW","Einhebel-Mischarmatur MEW"]
[null,232741,"Einhebel-Mischarmatur MEWC",96,"",null,null,null,null,null,null,232741,"Einhebel-Mischarmatur MEWC",96,false,null,232741,163,96,170,"på forespørgsel","op aanvraag","Einhebel-Mischarmatur MEWC","Einhebel-Mischarmatur MEWC","Einhebel-Mischarmatur MEWC","Einhebel-Mischarmatur MEWC","Eenhandel mengarmatuur MEWC","Einhebel-Mischarmatur MEWC","Einhebel-Mischarmatur MEWC","Einhebel-Mischarmatur MEWC","Einhebel-Mischarmatur MEWC","Einhebel-Mischarmatur MEWC","Einhebel-Mischarmatur MEWC"]
[null,232611,"Einhebel-Mischarmatur MES",100,"",null,null,null,null,null,null,232611,"Einhebel-Mischarmatur MES",100,false,null,232611,163,100,175,"på forespørgsel","op aanvraag","Einhebel-Mischarmatur MES","Einhebel-Mischarmatur MES","Einhebel-Mischarmatur MES","Einhebel-Mischarmatur MES","Eenhandel mengarmatuur MES","Einhebel-Mischarmatur MES","Einhebel-Mischarmatur MES","Einhebel-Mischarmatur MES","Einhebel-Mischarmatur MES","Einhebel-Mischarmatur MES","Einhebel-Mischarmatur MES"]
[null,230956,"Sensor fitting WEN",733,"",null,null,null,null,null,null,230956,"Sensor fitting WEN",733,false,null,230956,604,733,"1.240,00","på forespørgsel","op aanvraag","Sensor-Armatur WEN","Sensor fitting WEN","Sensor fitting WEN","Sensor fitting WEN","Sensor-Armatuur WEN","Sensor fitting WEN","Sensor fitting WEN","Sensor fitting WEN","Sensor fitting WEN","Sensor fitting WEN","Sensor fitting WEN"]
[null,232605,"Zweigriffarmatur WKM",126,"",null,null,null,null,null,null,232605,"Zweigriffarmatur WKM",126,false,null,232605,156,126,215,"på forespørgsel","op aanvraag","Zweigriffarmatur WKM","Zweigriffarmatur WKM","Zweigriffarmatur WKM","Zweigriffarmatur WKM","Tweegreepsarmatuur WKM","Zweigriffarmatur WKM","Zweigriffarmatur WKM","Zweigriffarmatur WKM","Zweigriffarmatur WKM","Zweigriffarmatur WKM","Zweigriffarmatur WKM"]
[null,232606,"Zweigriffarmatur WDM",139,"",null,null,null,null,null,null,232606,"Zweigriffarmatur WDM",139,false,null,232606,168,139,"sur demande","på forespørgsel","op aanvraag","Zweigriffarmatur WDM","Zweigriffarmatur WDM","Zweigriffarmatur WDM","Zweigriffarmatur WDM","Tweegreepsarmatuur WDM","Zweigriffarmatur WDM","Zweigriffarmatur WDM","Zweigriffarmatur WDM","Zweigriffarmatur WDM","Zweigriffarmatur WDM","Zweigriffarmatur WDM"]
[null,232607,"Zweigriffarmatur WBM",189,"",null,null,null,null,null,null,232607,"Zweigriffarmatur WBM",189,false,null,232607,249,189,"sur demande","på forespørgsel","op aanvraag","Zweigriffarmatur WBM","Zweigriffarmatur WBM","Zweigriffarmatur WBM","Zweigriffarmatur WBM","Tweegreepsarmatuur WBM","Zweigriffarmatur WBM","Zweigriffarmatur WBM","Zweigriffarmatur WBM","Zweigriffarmatur WBM","Zweigriffarmatur WBM","Zweigriffarmatur WBM"]
[null,232608,"Einhebel-Mischarmatur MEK",152,"",null,null,null,null,null,null,232608,"Einhebel-Mischarmatur MEK",152,false,null,232608,222,152,"sur demande","på forespørgsel","op aanvraag","Einhebel-Mischarmatur MEK","Einhebel-Mischarmatur MEK","Einhebel-Mischarmatur MEK","Einhebel-Mischarmatur MEK","Eenhandel mengarmatuur MEK","Einhebel-Mischarmatur MEK","Einhebel-Mischarmatur MEK","Einhebel-Mischarmatur MEK","Einhebel-Mischarmatur MEK","Einhebel-Mischarmatur MEK","Einhebel-Mischarmatur MEK"]
[null,232609,"Einhebel-Mischarmatur MED",146,"",null,null,null,null,null,null,232609,"Einhebel-Mischarmatur MED",146,false,null,232609,222,146,"sur demande","på forespørgsel","op aanvraag","Einhebel-Mischarmatur MED","Einhebel-Mischarmatur MED","Einhebel-Mischarmatur MED","Einhebel-Mischarmatur MED","Eenhandel mengarmatuur MED","Einhebel-Mischarmatur MED","Einhebel-Mischarmatur MED","Einhebel-Mischarmatur MED","Einhebel-Mischarmatur MED","Einhebel-Mischarmatur MED","Einhebel-Mischarmatur MED"]
[null,232610,"Einhebel-Mischarmatur MEB",192,"",null,null,null,null,null,null,232610,"Einhebel-Mischarmatur MEB",192,false,null,232610,292,192,"sur demande","på forespørgsel","op aanvraag","Einhebel-Mischarmatur MEB","Einhebel-Mischarmatur MEB","Einhebel-Mischarmatur MEB","Einhebel-Mischarmatur MEB","Eenhandel mengarmatuur MEB","Einhebel-Mischarmatur MEB","Einhebel-Mischarmatur MEB","Einhebel-Mischarmatur MEB","Einhebel-Mischarmatur MEB","Einhebel-Mischarmatur MEB","Einhebel-Mischarmatur MEB"]
[null,6629,"Connection pipe 500 mm",17,"",null,null,null,null,null,null,6629,"Connection pipe 500 mm",17,false,null,6629,24,17,"sur demande","på forespørgsel","op aanvraag","Anschlussrohr 500 mm","Connection pipe 500 mm","Connection pipe 500 mm","Connection pipe 500 mm","Aansluitleiding 500 mm","Connection pipe 500 mm","Connection pipe 500 mm","Connection pipe 500 mm","Connection pipe 500 mm","Connection pipe 500 mm","Connection pipe 500 mm"]
[null,734,"U/heavy",113,"",null,null,null,null,null,null,734,"U/heavy",113,false,null,734,156,113,"sur demande","på forespørgsel","op aanvraag","Anschlusszubehör U/schwer","U/heavy","U/heavy","U/heavy","U/zwaar","U/heavy","U/heavy","U/heavy","U/heavy","U/heavy","U/heavy"]
[null,222152,"Small water heater SHU 5 SL","On request","",null,null,null,null,null,null,222152,"Small water heater SHU 5 SL","On request",false,null,222152,455,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SHU 5 SL","Small water heater SHU 5 SL","Small water heater SHU 5 SL","Small water heater SHU 5 SL","Kleine boiler drukvast SHU 5 SL","Small water heater SHU 5 SL","Small water heater SHU 5 SL","Small water heater SHU 5 SL","Small water heater SHU 5 SL","Small water heater SHU 5 SL","Small water heater SHU 5 SL"]
[null,229472,"Small water heater SHU 10 SL","On request","",null,null,null,null,null,null,229472,"Small water heater SHU 10 SL","On request",false,null,229472,486,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SHU 10 SL","Small water heater SHU 10 SL","Small water heater SHU 10 SL","Small water heater SHU 10 SL","Kleine boiler drukvast SHU 10 SL","Small water heater SHU 10 SL","Small water heater SHU 10 SL","Small water heater SHU 10 SL","Small water heater SHU 10 SL","Small water heater SHU 10 SL","Small water heater SHU 10 SL"]
[null,229475,"Small water heater SH 10 SL","On request","",null,null,null,null,null,null,229475,"Small water heater SH 10 SL","On request",false,null,229475,486,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SH 10 SL","Small water heater SH 10 SL","Small water heater SH 10 SL","Small water heater SH 10 SL","Kleine boiler drukvast SH 10 SL","Small water heater SH 10 SL","Small water heater SH 10 SL","Small water heater SH 10 SL","Small water heater SH 10 SL","Small water heater SH 10 SL","Small water heater SH 10 SL"]
[null,229477,"Small water heater SH 15 SL","On request","",null,null,null,null,null,null,229477,"Small water heater SH 15 SL","On request",false,null,229477,685,"On request","sur demande","på forespørgsel","op aanvraag","Kleinspeicher SH 15 SL","Small water heater SH 15 SL","Small water heater SH 15 SL","Small water heater SH 15 SL","Kleine boiler drukvast SH 15 SL","Small water heater SH 15 SL","Small water heater SH 15 SL","Small water heater SH 15 SL","Small water heater SH 15 SL","Small water heater SH 15 SL","Small water heater SH 15 SL"]
[null,229479,"Small water heater SH 15 SL 3.3 kW",272,"",null,null,null,null,null,null,229479,"Small water heater SH 15 SL 3.3 kW",272,false,null,229479,696,272,720,"på forespørgsel","op aanvraag","Kleinspeicher SH 15 SL, 3,3 KW","Small water heater SH 15 SL 3.3 kW","Small water heater SH 15 SL 3.3 kW","Small water heater SH 15 SL 3.3 kW","Kleine boiler drukvast SH 15 SL 3,3 KW","Small water heater SH 15 SL 3.3 kW","Small water heater SH 15 SL 3.3 kW","Small water heater SH 15 SL 3.3 kW","Small water heater SH 15 SL 3.3 kW","Small water heater SH 15 SL 3.3 kW","Small water heater SH 15 SL 3.3 kW"]
[null,73499,"Safety assembly SVMT",155,"",null,null,null,null,null,null,73499,"Safety assembly SVMT",155,false,null,73499,170,155,"sur demande","på forespørgsel","op aanvraag","Sicherheitsgruppe SVMT","Safety assembly SVMT","Safety assembly SVMT","Safety assembly SVMT","Veiligheidsgroep SVMT","Safety assembly SVMT","Safety assembly SVMT","Safety assembly SVMT","Safety assembly SVMT","Safety assembly SVMT","Safety assembly SVMT"]
[null,70558,"Tees",25,"",null,null,null,null,null,null,70558,"Tees",25,false,null,70558,31.5,25,"sur demande","på forespørgsel","op aanvraag","Sicherheitsgruppe T-Stücke","Tees","Tees","Tees","Veiligheidsgroep T-Stuk","Tees","Tees","Tees","Tees","Tees","Tees"]
[null,233481,"Sicherheitsgruppe KV 40",127,"",null,null,null,null,null,null,233481,"Sicherheitsgruppe KV 40",127,false,null,233481,136,127,"sur demande","på forespørgsel",136,"Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Veiligheidsgroep KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40","Sicherheitsgruppe KV 40"]
[null,233482,"Sicherheitsgruppe KV 307",85,"",null,null,null,null,null,null,233482,"Sicherheitsgruppe KV 307",85,false,null,233482,109,85,"sur demande","på forespørgsel",109,"Sicherheitsgruppe KV 307","Sicherheitsgruppe KV 307","Sicherheitsgruppe KV 307","Sicherheitsgruppe KV 307","Veiligheidsgroep KV 307","Sicherheitsgruppe KV 307","Sicherheitsgruppe KV 307","Sicherheitsgruppe KV 307","Sicherheitsgruppe KV 307","Sicherheitsgruppe KV 307","Sicherheitsgruppe KV 307"]
[null,230764,"Safety assembly ZRT 2",58,"",null,null,null,null,null,null,230764,"Safety assembly ZRT 2",58,false,null,230764,100,58,"sur demande","på forespørgsel",100,"Sicherheitsgruppe SRT 2","Safety assembly ZRT 2","Safety assembly ZRT 2","Safety assembly ZRT 2","Veiligheidsgroep SRT 2","Safety assembly ZRT 2","Safety assembly ZRT 2","Safety assembly ZRT 2","Safety assembly ZRT 2","Safety assembly ZRT 2","Safety assembly ZRT 2"]
[null,223219,"Permanent connection set","On request","",null,null,null,null,null,null,223219,"Permanent connection set","On request",false,null,223219,16.8,"On request","sur demande","på forespørgsel","op aanvraag","Bausatz Festanschluss Kleinspeicher","Permanent connection set","Permanent connection set","Permanent connection set","Bouwset vaste aansluiting","Permanent connection set","Permanent connection set","Permanent connection set","Permanent connection set","Permanent connection set","Permanent connection set"]
[null,74196,"Storage heater HT 80 S","On request","",null,null,null,null,null,null,74196,"Storage heater HT 80 S","On request",false,null,74196,2002,"On request","sur demande","på forespørgsel","op aanvraag","Tischspeicher HT 80 S","Storage heater HT 80 S","Storage heater HT 80 S","Storage heater HT 80 S","Tafelmodel boiler HT 80 S","Storage heater HT 80 S","Storage heater HT 80 S","Storage heater HT 80 S","Storage heater HT 80 S","Storage heater HT 80 S","Storage heater HT 80 S"]
[null,74197,"Full casing HT 80 S","On request","",null,null,null,null,null,null,74197,"Full casing HT 80 S","On request",false,null,74197,180,"On request","sur demande","på forespørgsel","op aanvraag","Vollverkleidung HT 80 S","Full casing HT 80 S","Full casing HT 80 S","Full casing HT 80 S","Ommanteling HT 80 S","Full casing HT 80 S","Full casing HT 80 S","Full casing HT 80 S","Full casing HT 80 S","Full casing HT 80 S","Full casing HT 80 S"]
[null,182120,"Warm water cylinder SHW 200 S",1113,"",null,null,null,null,null,null,182120,"Warm water cylinder SHW 200 S",1113,false,null,182120,1542,1113,"sur demande","på forespørgsel",1549,"Warmwasser-Standspeicher SHW 200 S","Warm water cylinder SHW 200 S","Warm water cylinder SHW 200 S","Warm water cylinder SHW 200 S","Staande boiler SHW 200 S","Warm water cylinder SHW 200 S","Warm water cylinder SHW 200 S","Warm water cylinder SHW 200 S","Warm water cylinder SHW 200 S","Warm water cylinder SHW 200 S","Warm water cylinder SHW 200 S"]
[null,182121,"Warm water cylinder SHW 300 S",1138,"",null,null,null,null,null,null,182121,"Warm water cylinder SHW 300 S",1138,false,null,182121,1693,1138,"sur demande","på forespørgsel",1644,"Warmwasser-Standspeicher SHW 300 S","Warm water cylinder SHW 300 S","Warm water cylinder SHW 300 S","Warm water cylinder SHW 300 S","Staande boiler SHW 300 S","Warm water cylinder SHW 300 S","Warm water cylinder SHW 300 S","Warm water cylinder SHW 300 S","Warm water cylinder SHW 300 S","Warm water cylinder SHW 300 S","Warm water cylinder SHW 300 S"]
[null,182122,"Warm water cylinder SHW 400 S",1242,"",null,null,null,null,null,null,182122,"Warm water cylinder SHW 400 S",1242,false,null,182122,2058,1242,"sur demande","på forespørgsel",1798,"Warmwasser-Standspeicher SHW 400 S","Warm water cylinder SHW 400 S","Warm water cylinder SHW 400 S","Warm water cylinder SHW 400 S","Staande boiler SHW 400 S","Warm water cylinder SHW 400 S","Warm water cylinder SHW 400 S","Warm water cylinder SHW 400 S","Warm water cylinder SHW 400 S","Warm water cylinder SHW 400 S","Warm water cylinder SHW 400 S"]
[null,185352,"Warm water cylinder SHW 300 WS","On request","",null,null,null,null,null,null,185352,"Warm water cylinder SHW 300 WS","On request",false,null,185352,2628,"On request","sur demande","på forespørgsel",2371,"Warmwasser-Standspeicher SHW 300 WS","Warm water cylinder SHW 300 WS","Warm water cylinder SHW 300 WS","Warm water cylinder SHW 300 WS","Staande boiler SHW 300 WS","Warm water cylinder SHW 300 WS","Warm water cylinder SHW 300 WS","Warm water cylinder SHW 300 WS","Warm water cylinder SHW 300 WS","Warm water cylinder SHW 300 WS","Warm water cylinder SHW 300 WS"]
[null,185353,"Warm water cylinder SHW 400 WS","On request","",null,null,null,null,null,null,185353,"Warm water cylinder SHW 400 WS","On request",false,null,185353,3014,"On request","sur demande","på forespørgsel",2587,"Warmwasser-Standspeicher SHW 400 WS","Warm water cylinder SHW 400 WS","Warm water cylinder SHW 400 WS","Warm water cylinder SHW 400 WS","Staande boiler SHW 400 WS","Warm water cylinder SHW 400 WS","Warm water cylinder SHW 400 WS","Warm water cylinder SHW 400 WS","Warm water cylinder SHW 400 WS","Warm water cylinder SHW 400 WS","Warm water cylinder SHW 400 WS"]
[null,71264,"Warm water cylinder HSTP 200","On request","",null,null,null,null,null,null,71264,"Warm water cylinder HSTP 200","On request",false,null,71264,1314,"On request","sur demande","på forespørgsel",1330,"Warmwasser-Standspeicher HSTP 200","Warm water cylinder HSTP 200","Warm water cylinder HSTP 200","Warm water cylinder HSTP 200","Staande boiler HSTP 200","Warm water cylinder HSTP 200","Warm water cylinder HSTP 200","Warm water cylinder HSTP 200","Warm water cylinder HSTP 200","Warm water cylinder HSTP 200","Warm water cylinder HSTP 200"]
[null,71267,"Warm water cylinder HSTP 300","On request","",null,null,null,null,null,null,71267,"Warm water cylinder HSTP 300","On request",false,null,71267,1463,"On request","sur demande","på forespørgsel",1481,"Warmwasser-Standspeicher HSTP 300","Warm water cylinder HSTP 300","Warm water cylinder HSTP 300","Warm water cylinder HSTP 300","Staande boiler HSTP 300","Warm water cylinder HSTP 300","Warm water cylinder HSTP 300","Warm water cylinder HSTP 300","Warm water cylinder HSTP 300","Warm water cylinder HSTP 300","Warm water cylinder HSTP 300"]
[null,71270,"Warm water cylinder HSTP 400","On request","",null,null,null,null,null,null,71270,"Warm water cylinder HSTP 400","On request",false,null,71270,1777,"On request","sur demande","på forespørgsel",1801,"Warmwasser-Standspeicher HSTP 400","Warm water cylinder HSTP 400","Warm water cylinder HSTP 400","Warm water cylinder HSTP 400","Staande boiler HSTP 400","Warm water cylinder HSTP 400","Warm water cylinder HSTP 400","Warm water cylinder HSTP 400","Warm water cylinder HSTP 400","Warm water cylinder HSTP 400","Warm water cylinder HSTP 400"]
[null,1414,"Warm water cylinder SHO AC 600 7,5",1703,"",null,null,null,null,null,null,1414,"Warm water cylinder SHO AC 600 7,5",1703,false,null,1414,3241,1703,"sur demande","på forespørgsel",3241,"Warmwasser-Standspeicher SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5","Staande boiler SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5","Warm water cylinder SHO AC 600 7,5"]
[null,3352,"Warm water cylinder SHO AC 600 6/12",1853,"",null,null,null,null,null,null,3352,"Warm water cylinder SHO AC 600 6/12",1853,false,null,3352,3381,1853,"sur demande","på forespørgsel",3381,"Warmwasser-Standspeicher SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12","Staande boiler SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12","Warm water cylinder SHO AC 600 6/12"]
[null,1415,"Warm water cylinder SHO AC 1000 12",2894,"",null,null,null,null,null,null,1415,"Warm water cylinder SHO AC 1000 12",2894,false,null,1415,4429,2894,"sur demande","på forespørgsel",4429,"Warmwasser-Standspeicher SHO AC 1000 12","Warm water cylinder SHO AC 1000 12","Warm water cylinder SHO AC 1000 12","Warm water cylinder SHO AC 1000 12","Staande boiler SHO AC 1000 12","Warm water cylinder SHO AC 1000 12","Warm water cylinder SHO AC 1000 12","Warm water cylinder SHO AC 1000 12","Warm water cylinder SHO AC 1000 12","Warm water cylinder SHO AC 1000 12","Warm water cylinder SHO AC 1000 12"]
[null,3353,"Warm water cylinder SHO AC 1000 9/18",3106,"",null,null,null,null,null,null,3353,"Warm water cylinder SHO AC 1000 9/18",3106,false,null,3353,4572,3106,"sur demande","på forespørgsel",4572,"Warmwasser-Standspeicher SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18","Staande boiler SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18","Warm water cylinder SHO AC 1000 9/18"]
[null,185354,"Warm water cylinder SB 302 S",1118,"",null,null,null,null,null,null,185354,"Warm water cylinder SB 302 S",1118,false,null,185354,1271,1118,"1.905,00","på forespørgsel",1417,"Warmwasser-Standspeicher SB 302 S","Warm water cylinder SB 302 S","Warm water cylinder SB 302 S","Warm water cylinder SB 302 S","Tapwatervat SB 302 S","Warm water cylinder SB 302 S","Warm water cylinder SB 302 S","Warm water cylinder SB 302 S","Warm water cylinder SB 302 S","Warm water cylinder SB 302 S","Warm water cylinder SB 302 S"]
[null,185355,"Warm water cylinder SB 402 S",1263,"",null,null,null,null,null,null,185355,"Warm water cylinder SB 402 S",1263,false,null,185355,1728,1263,"2.160,00","på forespørgsel",1545,"Warmwasser-Standspeicher SB 402 S","Warm water cylinder SB 402 S","Warm water cylinder SB 402 S","Warm water cylinder SB 402 S","Tapwatervat SB 402 S","Warm water cylinder SB 402 S","Warm water cylinder SB 402 S","Warm water cylinder SB 402 S","Warm water cylinder SB 402 S","Warm water cylinder SB 402 S","Warm water cylinder SB 402 S"]
[null,71554,"Warm water cylinder SB 602 AC",1350,"",null,null,null,null,null,null,71554,"Warm water cylinder SB 602 AC",1350,false,null,71554,2852,1350,"2.295,00","på forespørgsel",2852,"Warmwasser-Standspeicher SB 602 AC","Warm water cylinder SB 602 AC","Warm water cylinder SB 602 AC","Warm water cylinder SB 602 AC","Tapwatervat SB 602 AC","Warm water cylinder SB 602 AC","Warm water cylinder SB 602 AC","Warm water cylinder SB 602 AC","Warm water cylinder SB 602 AC","Warm water cylinder SB 602 AC","Warm water cylinder SB 602 AC"]
[null,71282,"Warm water cylinder SB 1002 AC",2410,"",null,null,null,null,null,null,71282,"Warm water cylinder SB 1002 AC",2410,false,null,71282,3095,2410,"4.050,00","på forespørgsel",3125,"Warmwasser-Standspeicher SB 1002 AC","Warm water cylinder SB 1002 AC","Warm water cylinder SB 1002 AC","Warm water cylinder SB 1002 AC","Tapwatervat SB 1002 AC","Warm water cylinder SB 1002 AC","Warm water cylinder SB 1002 AC","Warm water cylinder SB 1002 AC","Warm water cylinder SB 1002 AC","Warm water cylinder SB 1002 AC","Warm water cylinder SB 1002 AC"]
[null,3039,"Warm water cylinder SB 650/3 AC",1924,"",null,null,null,null,null,null,3039,"Warm water cylinder SB 650/3 AC",1924,false,null,3039,2927,1924,"3.305,00","på forespørgsel",2927,"Warmwasser-Standspeicher SB 650/3 AC","Warm water cylinder SB 650/3 AC","Warm water cylinder SB 650/3 AC","Warm water cylinder SB 650/3 AC","Tapwatervat SB 650/3 AC","Warm water cylinder SB 650/3 AC","Warm water cylinder SB 650/3 AC","Warm water cylinder SB 650/3 AC","Warm water cylinder SB 650/3 AC","Warm water cylinder SB 650/3 AC","Warm water cylinder SB 650/3 AC"]
[null,691,"Electrical heating flange FCR 18/60",673,"",null,null,null,null,null,null,691,"Electrical heating flange FCR 18/60",673,false,null,691,851,673,"sur demande","på forespørgsel",851,"Elektro-Heizflansch FCR 18/60","Electrical heating flange FCR 18/60","Electrical heating flange FCR 18/60","Electrical heating flange FCR 18/60","Elektrische flens FCR 18/60","Electrical heating flange FCR 18/60","Electrical heating flange FCR 18/60","Electrical heating flange FCR 18/60","Electrical heating flange FCR 18/60","Electrical heating flange FCR 18/60","Electrical heating flange FCR 18/60"]
[null,692,"Electrical heating flange FCR 18/90",733,"",null,null,null,null,null,null,692,"Electrical heating flange FCR 18/90",733,false,null,692,927,733,"sur demande","på forespørgsel",927,"Elektro-Heizflansch FCR 18/90","Electrical heating flange FCR 18/90","Electrical heating flange FCR 18/90","Electrical heating flange FCR 18/90","Elektrische flens FCR 18/60","Electrical heating flange FCR 18/90","Electrical heating flange FCR 18/90","Electrical heating flange FCR 18/90","Electrical heating flange FCR 18/90","Electrical heating flange FCR 18/90","Electrical heating flange FCR 18/90"]
[null,71330,"Electrical heating flange FCR 21/60",418,"",null,null,null,null,null,null,71330,"Electrical heating flange FCR 21/60",418,false,null,71330,965,418,"sur demande","på forespørgsel",965,"Elektro-Heizflansch FCR 21/60","Electrical heating flange FCR 21/60","Electrical heating flange FCR 21/60","Electrical heating flange FCR 21/60","Elektrische flens FCR 21/60","Electrical heating flange FCR 21/60","Electrical heating flange FCR 21/60","Electrical heating flange FCR 21/60","Electrical heating flange FCR 21/60","Electrical heating flange FCR 21/60","Electrical heating flange FCR 21/60"]
[null,71331,"Electrical heating flange FCR 21/120",382,{"$f":"IF(O1089=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,71331,"Electrical heating flange FCR 21/120",382,false,null,71331,928,382,795,"på forespørgsel",928,"Elektro-Heizflansch FCR 21/120","Electrical heating flange FCR 21/120","Electrical heating flange FCR 21/120","Electrical heating flange FCR 21/120","Elektrische flens FCR 21/120","Electrical heating flange FCR 21/120","Electrical heating flange FCR 21/120","Electrical heating flange FCR 21/120","Electrical heating flange FCR 21/120","Electrical heating flange FCR 21/120","Electrical heating flange FCR 21/120"]
[null,694,"Electrical heating flange FCR 28/120",774,"",null,null,null,null,null,null,694,"Electrical heating flange FCR 28/120",774,false,null,694,1227,774,"1.115,00","på forespørgsel",1227,"Elektro-Heizflansch FCR 28/120 (12 KW)","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Elektrische flens FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120"]
[null,695,"Electrical heating flange FCR 28/180",821,"",null,null,null,null,null,null,695,"Electrical heating flange FCR 28/180",821,false,null,695,1370,821,"1.395,00","på forespørgsel",1370,"Elektro-Heizflansch FCR 28/180 (18 KW)","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Elektrische flens FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180"]
[null,696,"Electrical heating flange FCR 28/760",955,"",null,null,null,null,null,null,696,"Electrical heating flange FCR 28/760",955,false,null,696,1660,955,"1.580,00","på forespørgsel",1660,"Elektro-Heizflansch FCR 28/270 (27 KW)","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Elektrische flens FCR 28/270","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760","Electrical heating flange FCR 28/760"]
[null,1502,"Electrical heating flange FCR 28/360",917,"",null,null,null,null,null,null,1502,"Electrical heating flange FCR 28/360",917,{"$f":"IF(AND(B1093=L1093,C1093=M1093,D1093=N1093),FALSE,TRUE)","v":false},null,1502,1942,917,"1.520,00","på forespørgsel",1942,"Elektro-Heizflansch FCR 28/360 (36 KW)","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Elektrische flens FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360","Electrical heating flange FCR 28/360"]
[null,71332,"Electrical heating flange FCR 28/120",815,"",null,null,null,null,null,null,71332,"Electrical heating flange FCR 28/120",815,false,null,71332,1275,815,"1.375,00","på forespørgsel",1275,"Elektro-Heizflansch FCR 28/120 (6/12 KW)","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Elektrische flens FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120","Electrical heating flange FCR 28/120"]
[null,71333,"Electrical heating flange FCR 28/180",954,"",null,null,null,null,null,null,71333,"Electrical heating flange FCR 28/180",954,false,null,71333,1428,954,"1.610,00","på forespørgsel",1428,"Elektro-Heizflansch FCR 28/180 (9/18 KW)","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Elektrische flens FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180","Electrical heating flange FCR 28/180"]
[null,3769,"Electrical heating flange BGC",221,"",null,null,null,null,null,null,3769,"Electrical heating flange BGC",221,false,null,3769,357,221,"sur demande","på forespørgsel",357,"Einschraubheizkörper BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC","Verwarmingselement BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC","Electrical heating flange BGC"]
[null,75115,"Threaded immersion heater BGC/45",238,"",null,null,null,null,null,null,75115,"Threaded immersion heater BGC/45",238,false,null,75115,399,238,335,1565,399,"Einschraubheizkörper BGC/45","Threaded immersion heater BGC/45","Corps de chauffe à visser BGC","Resistenza elettrica BGC","Verwarmingselement BGC/45","šroubovací topné těleso BGC","Skrutkovacie teleso BGC","Electric threaded immersion heater BGC","Becsavarható fűtőelem BGC","Sähkövastus BGC","Threaded immersion heater BGC/45"]
[null,232029,"Einschraubheizkörper BGC 2",235,"",null,null,null,null,null,null,232029,"Einschraubheizkörper BGC 2",235,false,null,232029,386,235,"sur demande",1612,386,"Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Verwarmingselement BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2","Einschraubheizkörper BGC 2"]
[null,232030,"Einschraubheizkörper BGC 2/60",267,"",null,null,null,null,null,null,232030,"Einschraubheizkörper BGC 2/60",267,false,null,232030,435,267,"sur demande",1827,435,"Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Verwarmingselement BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60","Einschraubheizkörper BGC 2/60"]
[null,76102,"Dummy flange B21",87,"",null,null,null,null,null,null,76102,"Dummy flange B21",87,false,null,76102,128,87,150,"på forespørgsel",128,"Blindflansch B 21","Dummy flange B21","Dummy flange B21","Dummy flange B21","Blindflens B 21","Dummy flange B21","Dummy flange B21","Dummy flange B21","Dummy flange B21","Dummy flange B21","Dummy flange B21"]
[null,76103,"Dummy flange B28",158,"",null,null,null,null,null,null,76103,"Dummy flange B28",158,false,null,76103,146,158,270,"på forespørgsel",146,"Blindflansch B 28","Dummy flange B28","Dummy flange B28","Dummy flange B28","Blindflens B 28","Dummy flange B28","Dummy flange B28","Dummy flange B28","Dummy flange B28","Dummy flange B28","Dummy flange B28"]
[null,1663,"Dummy flange GF 18",42,"",null,null,null,null,null,null,1663,"Dummy flange GF 18",42,false,null,1663,167,42,"sur demande","på forespørgsel",167,"Gegenflansch GF 18","Dummy flange GF 18","Dummy flange GF 18","Dummy flange GF 18","Tegenflens GF 18","Dummy flange GF 18","Dummy flange GF 18","Dummy flange GF 18","Dummy flange GF 18","Dummy flange GF 18","Dummy flange GF 18"]
[null,1664,"Dummy flange GF 28",70,"",null,null,null,null,null,null,1664,"Dummy flange GF 28",70,false,null,1664,300,70,"sur demande","på forespørgsel",300,"Gegenflansch GF 28","Dummy flange GF 28","Dummy flange GF 28","Dummy flange GF 28","Tegenflens GF 28","Dummy flange GF 28","Dummy flange GF 28","Dummy flange GF 28","Dummy flange GF 28","Dummy flange GF 28","Dummy flange GF 28"]
[null,76062,"Heat exchanger WTW 21/13",683,"",null,null,null,null,null,null,76062,"Heat exchanger WTW 21/13",683,false,null,76062,689,683,"1.150,00","på forespørgsel",689,"Heizungs-Wärmeaustauscher WTW 21/13","Heat exchanger WTW 21/13","Heat exchanger WTW 21/13","Heat exchanger WTW 21/13","Warmtewisselaar WTW 21/13","Heat exchanger WTW 21/13","Heat exchanger WTW 21/13","Heat exchanger WTW 21/13","Heat exchanger WTW 21/13","Heat exchanger WTW 21/13","Heat exchanger WTW 21/13"]
[null,76098,"Heat exchanger WTW 28/18",934,"",null,null,null,null,null,null,76098,"Heat exchanger WTW 28/18",934,false,null,76098,928,934,"sur demande","på forespørgsel",928,"Heizungs-Wärmeaustauscher WTW 28/18","Heat exchanger WTW 28/18","Heat exchanger WTW 28/18","Heat exchanger WTW 28/18","Warmtewisselaar WTW 28/18","Heat exchanger WTW 28/18","Heat exchanger WTW 28/18","Heat exchanger WTW 28/18","Heat exchanger WTW 28/18","Heat exchanger WTW 28/18","Heat exchanger WTW 28/18"]
[null,76099,"Heat exchanger WTW 28/23",1017,"",null,null,null,null,null,null,76099,"Heat exchanger WTW 28/23",1017,false,null,76099,999,1017,"1.735,00","på forespørgsel",999,"Heizungs-Wärmeaustauscher WTW 28/23","Heat exchanger WTW 28/23","Heat exchanger WTW 28/23","Heat exchanger WTW 28/23","Warmtewisselaar WTW 28/23","Heat exchanger WTW 28/23","Heat exchanger WTW 28/23","Heat exchanger WTW 28/23","Heat exchanger WTW 28/23","Heat exchanger WTW 28/23","Heat exchanger WTW 28/23"]
[null,72119,"Refrigerant heat exchanger WTFS 21/13",1193,"",null,null,null,null,null,null,72119,"Refrigerant heat exchanger WTFS 21/13",1193,false,null,72119,1151,1193,"sur demande","på forespørgsel",1151,"Kältemittel-Wärmeaustauscher WTFS 21/13","Refrigerant heat exchanger WTFS 21/13","Refrigerant heat exchanger WTFS 21/13","Refrigerant heat exchanger WTFS 21/13","Warmtewisselaar WTFS 21/13","Refrigerant heat exchanger WTFS 21/13","Refrigerant heat exchanger WTFS 21/13","Refrigerant heat exchanger WTFS 21/13","Refrigerant heat exchanger WTFS 21/13","Refrigerant heat exchanger WTFS 21/13","Refrigerant heat exchanger WTFS 21/13"]
[null,72118,"Refrigerant heat exchanger WTFS 28/23",1445,"",null,null,null,null,null,null,72118,"Refrigerant heat exchanger WTFS 28/23",1445,false,null,72118,1425,1445,"sur demande","på forespørgsel",1425,"Kältemittel-Wärmeaustauscher WTFS 28/23","Refrigerant heat exchanger WTFS 28/23","Refrigerant heat exchanger WTFS 28/23","Refrigerant heat exchanger WTFS 28/23","Warmtewisselaar WTFS 28/23","Refrigerant heat exchanger WTFS 28/23","Refrigerant heat exchanger WTFS 28/23","Refrigerant heat exchanger WTFS 28/23","Refrigerant heat exchanger WTFS 28/23","Refrigerant heat exchanger WTFS 28/23","Refrigerant heat exchanger WTFS 28/23"]
[null,74370,"Safety assembly ZH 1",131,"",null,null,null,null,null,null,74370,"Safety assembly ZH 1",131,false,null,74370,130,131,"sur demande","på forespørgsel","op aanvraag","Sicherheitsgruppe Standspeicher ZH 1","Safety assembly ZH 1","Safety assembly ZH 1","Safety assembly ZH 1","Veiligheidsgroep ZH 1","Safety assembly ZH 1","Safety assembly ZH 1","Safety assembly ZH 1","Safety assembly ZH 1","Safety assembly ZH 1","Safety assembly ZH 1"]
[null,74371,"Pressure reducing valve DMV/ZH 1",101,"",null,null,null,null,null,null,74371,"Pressure reducing valve DMV/ZH 1",101,false,null,74371,90,101,"sur demande","på forespørgsel",90,"Druckminderventil DMV / ZH 1","Pressure reducing valve DMV/ZH 1","Pressure reducing valve DMV/ZH 1","Pressure reducing valve DMV/ZH 1","Drukreduceer DMV / ZH 1","Pressure reducing valve DMV/ZH 1","Pressure reducing valve DMV/ZH 1","Pressure reducing valve DMV/ZH 1","Pressure reducing valve DMV/ZH 1","Pressure reducing valve DMV/ZH 1","Pressure reducing valve DMV/ZH 1"]
[null,74373,"Safety valve S 1/2-6",13,"",null,null,null,null,null,null,74373,"Safety valve S 1/2-6",13,false,null,74373,14.6,13,"sur demande","på forespørgsel",15,"Sicherheitsventil SV 1/2-6","Safety valve S 1/2-6","Safety valve S 1/2-6","Safety valve S 1/2-6","Veiligheidsklep SV 1/2-6","Safety valve S 1/2-6","Safety valve S 1/2-6","Safety valve S 1/2-6","Safety valve S 1/2-6","Safety valve S 1/2-6","Safety valve S 1/2-6"]
[null,74374,"Safety valve S 3/4-6",20,"",null,null,null,null,null,null,74374,"Safety valve S 3/4-6",20,false,null,74374,23.7,20,"sur demande","på forespørgsel",24,"Sicherheitsventil SV 3/4-6","Safety valve S 3/4-6","Safety valve S 3/4-6","Safety valve S 3/4-6","Veiligheidsklep SV 3/4-6","Safety valve S 3/4-6","Safety valve S 3/4-6","Safety valve S 3/4-6","Safety valve S 3/4-6","Safety valve S 3/4-6","Safety valve S 3/4-6"]
[null,74375,"Safety valve S 3/4-10",18,"",null,null,null,null,null,null,74375,"Safety valve S 3/4-10",18,false,null,74375,23.7,18,"sur demande","på forespørgsel",24,"Sicherheitsventil SV 3/4-10","Safety valve S 3/4-10","Safety valve S 3/4-10","Safety valve S 3/4-10","Veiligheidsklep SV 3/4-10","Safety valve S 3/4-10","Safety valve S 3/4-10","Safety valve S 3/4-10","Safety valve S 3/4-10","Safety valve S 3/4-10","Safety valve S 3/4-10"]
[null,232875,"Wärmedämmung für SHO AC 600",456,"",null,null,null,null,null,null,232875,"Wärmedämmung für SHO AC 600",456,false,null,232875,564,456,"sur demande","på forespørgsel",564,"Wärmedämmung für SHO AC 600","Wärmedämmung für SHO AC 600","Wärmedämmung für SHO AC 600","Wärmedämmung für SHO AC 600","Isolatie SHO AC 600","Wärmedämmung für SHO AC 600","Wärmedämmung für SHO AC 600","Wärmedämmung für SHO AC 600","Wärmedämmung für SHO AC 600","Wärmedämmung für SHO AC 600","Wärmedämmung für SHO AC 600"]
[null,232876,"Wärmedämmung für SHO AC 1000",564,"",null,null,null,null,null,null,232876,"Wärmedämmung für SHO AC 1000",564,false,null,232876,725,564,"sur demande","på forespørgsel",725,"Wärmedämmung für SHO AC 1000","Wärmedämmung für SHO AC 1000","Wärmedämmung für SHO AC 1000","Wärmedämmung für SHO AC 1000","Isolatie SHO AC 1000","Wärmedämmung für SHO AC 1000","Wärmedämmung für SHO AC 1000","Wärmedämmung für SHO AC 1000","Wärmedämmung für SHO AC 1000","Wärmedämmung für SHO AC 1000","Wärmedämmung für SHO AC 1000"]
[null,232877,"Wärmedämmung für SB 602 AC",480,"",null,null,null,null,null,null,232877,"Wärmedämmung für SB 602 AC",480,false,null,232877,590,480,845,"på forespørgsel",590,"Wärmedämmung für SB 602 AC","Wärmedämmung für SB 602 AC","Wärmedämmung für SB 602 AC","Wärmedämmung für SB 602 AC","Isolatie SB 602 AC","Wärmedämmung für SB 602 AC","Wärmedämmung für SB 602 AC","Wärmedämmung für SB 602 AC","Wärmedämmung für SB 602 AC","Wärmedämmung für SB 602 AC","Wärmedämmung für SB 602 AC"]
[null,232878,"Wärmedämmung für SB 1002 AC",591,"",null,null,null,null,null,null,232878,"Wärmedämmung für SB 1002 AC",591,false,null,232878,760,591,"1.080,00","på forespørgsel",760,"Wärmedämmung für SB 1002 AC","Wärmedämmung für SB 1002 AC","Wärmedämmung für SB 1002 AC","Wärmedämmung für SB 1002 AC","Isolatie SB 1002 AC","Wärmedämmung für SB 1002 AC","Wärmedämmung für SB 1002 AC","Wärmedämmung für SB 1002 AC","Wärmedämmung für SB 1002 AC","Wärmedämmung für SB 1002 AC","Wärmedämmung für SB 1002 AC"]
[null,232879,"Wärmedämmung für SB 650/3 AC",486,"",null,null,null,null,null,null,232879,"Wärmedämmung für SB 650/3 AC",486,false,null,232879,578,486,875,"på forespørgsel",578,"Wärmedämmung für SB 650/3 AC","Wärmedämmung für SB 650/3 AC","Wärmedämmung für SB 650/3 AC","Wärmedämmung für SB 650/3 AC","Isolatie SB 650/3 AC","Wärmedämmung für SB 650/3 AC","Wärmedämmung für SB 650/3 AC","Wärmedämmung für SB 650/3 AC","Wärmedämmung für SB 650/3 AC","Wärmedämmung für SB 650/3 AC","Wärmedämmung für SB 650/3 AC"]
[null,58990,"Temperature controller RWF 1N-A","On request","",null,null,null,null,null,null,58990,"Temperature controller RWF 1N-A","On request",false,null,58990,105.9,"On request","sur demande","på forespørgsel",106,"Temperaturregler Standspeicher RWF 1N-A","Temperature controller RWF 1N-A","Temperature controller RWF 1N-A","Temperature controller RWF 1N-A","Thermostaat RWF 1N-A","Temperature controller RWF 1N-A","Temperature controller RWF 1N-A","Temperature controller RWF 1N-A","Temperature controller RWF 1N-A","Temperature controller RWF 1N-A","Temperature controller RWF 1N-A"]
[null,143498,"Replacement anode G 3/4",78,"",null,null,null,null,null,null,143498,"Replacement anode G 3/4",78,false,null,143498,114.9,78,"sur demande","på forespørgsel",115,"Ersatzanode 3/4","Replacement anode G 3/4","Replacement anode G 3/4","Replacement anode G 3/4","Vervanganode 3/4","Replacement anode G 3/4","Replacement anode G 3/4","Replacement anode G 3/4","Replacement anode G 3/4","Replacement anode G 3/4","Replacement anode G 3/4"]
[null,143499,"Replacement anode G 1 1/4",133,"",null,null,null,null,null,null,143499,"Replacement anode G 1 1/4",133,false,null,143499,150.6,133,"sur demande","på forespørgsel",151,"Ersatzanode 1 1/4","Replacement anode G 1 1/4","Replacement anode G 1 1/4","Replacement anode G 1 1/4","Vervanganode 1 1/4","Replacement anode G 1 1/4","Replacement anode G 1 1/4","Replacement anode G 1 1/4","Replacement anode G 1 1/4","Replacement anode G 1 1/4","Replacement anode G 1 1/4"]
[null,74464,"Hand dryer HTT 4 WS",264,"",null,null,null,null,null,null,74464,"Hand dryer HTT 4 WS",264,false,null,74464,350,264,465,"på forespørgsel",436,"Händetrockner HTT 4 WS","Hand dryer HTT 4 WS","Hand dryer HTT 4 WS","Hand dryer HTT 4 WS","Handendroger HTT 4 WS","Hand dryer HTT 4 WS","Hand dryer HTT 4 WS","Hand dryer HTT 4 WS","Hand dryer HTT 4 WS","Hand dryer HTT 4 WS","Hand dryer HTT 4 WS"]
[null,74465,"Hand dryer HTT 5 WS",345,"",null,null,null,null,null,null,74465,"Hand dryer HTT 5 WS",345,false,null,74465,437,345,605,"på forespørgsel",552,"Händetrockner HTT 5 WS","Hand dryer HTT 5 WS","Hand dryer HTT 5 WS","Hand dryer HTT 5 WS","Handendroger HTT 5 WS","Hand dryer HTT 5 WS","Hand dryer HTT 5 WS","Hand dryer HTT 5 WS","Hand dryer HTT 5 WS","Hand dryer HTT 5 WS","Hand dryer HTT 5 WS"]
[null,182053,"Hand dryer HTT 5 SM",344,"",null,null,null,null,null,null,182053,"Hand dryer HTT 5 SM",344,false,null,182053,561,344,605,"på forespørgsel",552,"Händetrockner HTT 5 SM","Hand dryer HTT 5 SM","Hand dryer HTT 5 SM","Hand dryer HTT 5 SM","Handendroger HTT 5 SM","Hand dryer HTT 5 SM","Hand dryer HTT 5 SM","Hand dryer HTT 5 SM","Hand dryer HTT 5 SM","Hand dryer HTT 5 SM","Hand dryer HTT 5 SM"]
[null,182052,"Hand dryer HTT 5 AM",343,"",null,null,null,null,null,null,182052,"Hand dryer HTT 5 AM",343,false,null,182052,561,343,605,"på forespørgsel",552,"Händetrockner HTT 5 AM","Hand dryer HTT 5 AM","Hand dryer HTT 5 AM","Hand dryer HTT 5 AM","Handendroger HTT 5 AM","Hand dryer HTT 5 AM","Hand dryer HTT 5 AM","Hand dryer HTT 5 AM","Hand dryer HTT 5 AM","Hand dryer HTT 5 AM","Hand dryer HTT 5 AM"]
[null,231582,"Hand dryer highspeed Ultronic S",436,"",null,null,null,null,null,null,231582,"Hand dryer highspeed Ultronic S",436,false,null,231582,590,436,770,"på forespørgsel",582,"Händetrockner Highspeed Ultronic S","Hand dryer highspeed Ultronic S","Hand dryer highspeed Ultronic S","Hand dryer highspeed Ultronic S","Handendroger Ultronic S","Hand dryer highspeed Ultronic S","Hand dryer highspeed Ultronic S","Hand dryer highspeed Ultronic S","Hand dryer highspeed Ultronic S","Hand dryer highspeed Ultronic S","Hand dryer highspeed Ultronic S"]
[null,231583,"Hand dryer highspeed Ultronic W",316,"",null,null,null,null,null,null,231583,"Hand dryer highspeed Ultronic W",316,false,null,231583,454,316,560,"på forespørgsel",448,"Händetrockner Highspeed Ultronic W","Hand dryer highspeed Ultronic W","Hand dryer highspeed Ultronic W","Hand dryer highspeed Ultronic W","Handendroger Ultronic W","Hand dryer highspeed Ultronic W","Hand dryer highspeed Ultronic W","Hand dryer highspeed Ultronic W","Hand dryer highspeed Ultronic W","Hand dryer highspeed Ultronic W","Hand dryer highspeed Ultronic W"]
[null,74484,"Standard storage heater ETS 200",571,"",null,null,null,null,null,null,74484,"Standard storage heater ETS 200",571,false,null,74484,812,571,"sur demande","på forespørgsel",812,"Wärmespeicher-Standard ETS 200","Standard storage heater ETS 200","Standard storage heater ETS 200","Standard storage heater ETS 200","Accumulatiekachel ETS 200","Standard storage heater ETS 200","Standard storage heater ETS 200","Standard storage heater ETS 200","Standard storage heater ETS 200","Standard storage heater ETS 200","Standard storage heater ETS 200"]
[null,74485,"Standard storage heater ETS 300",628,"",null,null,null,null,null,null,74485,"Standard storage heater ETS 300",628,false,null,74485,1008,628,"sur demande","på forespørgsel",1008,"Wärmespeicher-Standard ETS 300","Standard storage heater ETS 300","Standard storage heater ETS 300","Standard storage heater ETS 300","Accumulatiekachel ETS 300","Standard storage heater ETS 300","Standard storage heater ETS 300","Standard storage heater ETS 300","Standard storage heater ETS 300","Standard storage heater ETS 300","Standard storage heater ETS 300"]
[null,74486,"Standard storage heater ETS 400",721,"",null,null,null,null,null,null,74486,"Standard storage heater ETS 400",721,false,null,74486,1159,721,"sur demande","på forespørgsel",1159,"Wärmespeicher-Standard ETS 400","Standard storage heater ETS 400","Standard storage heater ETS 400","Standard storage heater ETS 400","Accumulatiekachel ETS 400","Standard storage heater ETS 400","Standard storage heater ETS 400","Standard storage heater ETS 400","Standard storage heater ETS 400","Standard storage heater ETS 400","Standard storage heater ETS 400"]
[null,74487,"Standard storage heater ETS 500",793,"",null,null,null,null,null,null,74487,"Standard storage heater ETS 500",793,false,null,74487,1295,793,"sur demande","på forespørgsel",1295,"Wärmespeicher-Standard ETS 500","Standard storage heater ETS 500","Standard storage heater ETS 500","Standard storage heater ETS 500","Accumulatiekachel ETS 500","Standard storage heater ETS 500","Standard storage heater ETS 500","Standard storage heater ETS 500","Standard storage heater ETS 500","Standard storage heater ETS 500","Standard storage heater ETS 500"]
[null,74488,"Standard storage heater ETS 600",877,"",null,null,null,null,null,null,74488,"Standard storage heater ETS 600",877,false,null,74488,1464,877,"sur demande","på forespørgsel",1464,"Wärmespeicher-Standard ETS 600","Standard storage heater ETS 600","Standard storage heater ETS 600","Standard storage heater ETS 600","Accumulatiekachel ETS 600","Standard storage heater ETS 600","Standard storage heater ETS 600","Standard storage heater ETS 600","Standard storage heater ETS 600","Standard storage heater ETS 600","Standard storage heater ETS 600"]
[null,74489,"Standard storage heater ETS 700",976,"",null,null,null,null,null,null,74489,"Standard storage heater ETS 700",976,false,null,74489,1769,976,"sur demande","på forespørgsel",1769,"Wärmespeicher-Standard ETS 700","Standard storage heater ETS 700","Standard storage heater ETS 700","Standard storage heater ETS 700","Accumulatiekachel ETS 700","Standard storage heater ETS 700","Standard storage heater ETS 700","Standard storage heater ETS 700","Standard storage heater ETS 700","Standard storage heater ETS 700","Standard storage heater ETS 700"]
[null,74391,"Wall mounted storage heater ETW 120","On request","",null,null,null,null,null,null,74391,"Wall mounted storage heater ETW 120","On request",false,null,74391,921,"On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher Wand ETW 120","Wall mounted storage heater ETW 120","Wall mounted storage heater ETW 120","Wall mounted storage heater ETW 120","Accumulatiekachel ETW 120","Wall mounted storage heater ETW 120","Wall mounted storage heater ETW 120","Wall mounted storage heater ETW 120","Wall mounted storage heater ETW 120","Wall mounted storage heater ETW 120","Wall mounted storage heater ETW 120"]
[null,74392,"Wall mounted storage heater ETW 180","On request","",null,null,null,null,null,null,74392,"Wall mounted storage heater ETW 180","On request",false,null,74392,1009,"On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher Wand ETW 180","Wall mounted storage heater ETW 180","Wall mounted storage heater ETW 180","Wall mounted storage heater ETW 180","Accumulatiekachel ETW 180","Wall mounted storage heater ETW 180","Wall mounted storage heater ETW 180","Wall mounted storage heater ETW 180","Wall mounted storage heater ETW 180","Wall mounted storage heater ETW 180","Wall mounted storage heater ETW 180"]
[null,74393,"Wall mounted storage heater ETW 240","On request","",null,null,null,null,null,null,74393,"Wall mounted storage heater ETW 240","On request",false,null,74393,1187,"On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher Wand ETW 240","Wall mounted storage heater ETW 240","Wall mounted storage heater ETW 240","Wall mounted storage heater ETW 240","Accumulatiekachel ETW 240","Wall mounted storage heater ETW 240","Wall mounted storage heater ETW 240","Wall mounted storage heater ETW 240","Wall mounted storage heater ETW 240","Wall mounted storage heater ETW 240","Wall mounted storage heater ETW 240"]
[null,74394,"Wall mounted storage heater ETW 300","On request","",null,null,null,null,null,null,74394,"Wall mounted storage heater ETW 300","On request",false,null,74394,1295,"On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher Wand ETW 300","Wall mounted storage heater ETW 300","Wall mounted storage heater ETW 300","Wall mounted storage heater ETW 300","Accumulatiekachel ETW 300","Wall mounted storage heater ETW 300","Wall mounted storage heater ETW 300","Wall mounted storage heater ETW 300","Wall mounted storage heater ETW 300","Wall mounted storage heater ETW 300","Wall mounted storage heater ETW 300"]
[null,74395,"Wall mounted storage heater ETW 360","On request","",null,null,null,null,null,null,74395,"Wall mounted storage heater ETW 360","On request",false,null,74395,1418,"On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher Wand ETW 360","Wall mounted storage heater ETW 360","Wall mounted storage heater ETW 360","Wall mounted storage heater ETW 360","Accumulatiekachel ETW 360","Wall mounted storage heater ETW 360","Wall mounted storage heater ETW 360","Wall mounted storage heater ETW 360","Wall mounted storage heater ETW 360","Wall mounted storage heater ETW 360","Wall mounted storage heater ETW 360"]
[null,74396,"Wall mounted storage heater ETW 420","On request","",null,null,null,null,null,null,74396,"Wall mounted storage heater ETW 420","On request",false,null,74396,1550,"On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher Wand ETW 420","Wall mounted storage heater ETW 420","Wall mounted storage heater ETW 420","Wall mounted storage heater ETW 420","Accumulatiekachel ETW 420","Wall mounted storage heater ETW 420","Wall mounted storage heater ETW 420","Wall mounted storage heater ETW 420","Wall mounted storage heater ETW 420","Wall mounted storage heater ETW 420","Wall mounted storage heater ETW 420"]
[null,74397,"Wall mounted storage heater ETW 480","On request","",null,null,null,null,null,null,74397,"Wall mounted storage heater ETW 480","On request",false,null,74397,1688,"On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher Wand ETW 480","Wall mounted storage heater ETW 480","Wall mounted storage heater ETW 480","Wall mounted storage heater ETW 480","Accumulatiekachel ETW 480","Wall mounted storage heater ETW 480","Wall mounted storage heater ETW 480","Wall mounted storage heater ETW 480","Wall mounted storage heater ETW 480","Wall mounted storage heater ETW 480","Wall mounted storage heater ETW 480"]
[null,182015,"Assembly 2-line ZK 2","On request","",null,null,null,null,null,null,182015,"Assembly 2-line ZK 2","On request",false,null,182015,67,"On request","sur demande","på forespørgsel","op aanvraag","Bausatz Zweikreis für ETW","Assembly 2-line ZK 2","Assembly 2-line ZK 2","Assembly 2-line ZK 2","ZK 2 Bouwset Tweespan","Assembly 2-line ZK 2","Assembly 2-line ZK 2","Assembly 2-line ZK 2","Assembly 2-line ZK 2","Assembly 2-line ZK 2","Assembly 2-line ZK 2"]
[null,74490,"Storage heater low ETT 350","On request","",null,null,null,null,null,null,74490,"Storage heater low ETT 350","On request",false,null,74490,1148,"On request","sur demande","på forespørgsel","op aanvraag","Niedrig-Wärmespeicher ETT 350","Storage heater low ETT 350","Storage heater low ETT 350","Storage heater low ETT 350","Lage accumulatiekachel ETT 350","Storage heater low ETT 350","Storage heater low ETT 350","Storage heater low ETT 350","Storage heater low ETT 350","Storage heater low ETT 350","Storage heater low ETT 350"]
[null,74491,"Storage heater low ETT 500","On request","",null,null,null,null,null,null,74491,"Storage heater low ETT 500","On request",false,null,74491,1475,"On request","sur demande","på forespørgsel","op aanvraag","Niedrig-Wärmespeicher ETT 500","Storage heater low ETT 500","Storage heater low ETT 500","Storage heater low ETT 500","Lage accumulatiekachel ETT 500","Storage heater low ETT 500","Storage heater low ETT 500","Storage heater low ETT 500","Storage heater low ETT 500","Storage heater low ETT 500","Storage heater low ETT 500"]
[null,182026,"Room temperature controller RTI-E 3",58,"",null,null,null,null,null,null,182026,"Room temperature controller RTI-E 3",58,false,null,182026,98,58,105,"på forespørgsel",98,"Raumtemperaturregler RTI-E 3","Room temperature controller RTI-E 3","Room temperature controller RTI-E 3","Room temperature controller RTI-E 3","Temperatuurregelaar RTI-E3","Room temperature controller RTI-E 3","Room temperature controller RTI-E 3","Room temperature controller RTI-E 3","Room temperature controller RTI-E 3","Room temperature controller RTI-E 3","Room temperature controller RTI-E 3"]
[null,182027,"Room temperature controller RTI-EP 2",96,"",null,null,null,null,null,null,182027,"Room temperature controller RTI-EP 2",96,false,null,182027,147,96,170,"på forespørgsel",147,"Raumtemperaturregler RTI-EP 2","Room temperature controller RTI-EP 2","Room temperature controller RTI-EP 2","Room temperature controller RTI-EP 2","Temperatuurregelaar RTI-EP2","Room temperature controller RTI-EP 2","Room temperature controller RTI-EP 2","Room temperature controller RTI-EP 2","Room temperature controller RTI-EP 2","Room temperature controller RTI-EP 2","Room temperature controller RTI-EP 2"]
[null,182103,"Booster heater ETW 120, ETS 200",57,"",null,null,null,null,null,null,182103,"Booster heater ETW 120, ETS 200",57,false,null,182103,61,57,"sur demande","på forespørgsel",61,"Zusatzheizung für ETW 120, ETS 200","Booster heater ETW 120, ETS 200","Booster heater ETW 120, ETS 200","Booster heater ETW 120, ETS 200","Aanvullende verwarming ETW 120, ETS 200","Booster heater ETW 120, ETS 200","Booster heater ETW 120, ETS 200","Booster heater ETW 120, ETS 200","Booster heater ETW 120, ETS 200","Booster heater ETW 120, ETS 200","Booster heater ETW 120, ETS 200"]
[null,182104,"Booster heater ETW 180, ETS 300",54,"",null,null,null,null,null,null,182104,"Booster heater ETW 180, ETS 300",54,false,null,182104,63,54,"sur demande","på forespørgsel",63,"Zusatzheizung für ETW 180, ETS 300","Booster heater ETW 180, ETS 300","Booster heater ETW 180, ETS 300","Booster heater ETW 180, ETS 300","Aanvullende verwarming ETW 180, ETS 300","Booster heater ETW 180, ETS 300","Booster heater ETW 180, ETS 300","Booster heater ETW 180, ETS 300","Booster heater ETW 180, ETS 300","Booster heater ETW 180, ETS 300","Booster heater ETW 180, ETS 300"]
[null,182105,"Booster heater ETW 240, ETS 400",55,"",null,null,null,null,null,null,182105,"Booster heater ETW 240, ETS 400",55,false,null,182105,65,55,"sur demande","på forespørgsel",65,"Zusatzheizung für ETW 240, ETS 400","Booster heater ETW 240, ETS 400","Booster heater ETW 240, ETS 400","Booster heater ETW 240, ETS 400","Aanvullende verwarming ETW 240, ETS 400","Booster heater ETW 240, ETS 400","Booster heater ETW 240, ETS 400","Booster heater ETW 240, ETS 400","Booster heater ETW 240, ETS 400","Booster heater ETW 240, ETS 400","Booster heater ETW 240, ETS 400"]
[null,182106,"Booster heater ETW 300, ETS 500, ETT 350",61,"",null,null,null,null,null,null,182106,"Booster heater ETW 300, ETS 500, ETT 350",61,false,null,182106,69,61,"sur demande","på forespørgsel",69,"Zusatzheizung für ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350","Aanvullende verwarming ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350","Booster heater ETW 300, ETS 500, ETT 350"]
[null,182107,"Booster heater ETW 360","On request","",null,null,null,null,null,null,182107,"Booster heater ETW 360","On request",false,null,182107,78,"On request","sur demande","på forespørgsel","op aanvraag","Zusatzheizung für ETW 360","Booster heater ETW 360","Booster heater ETW 360","Booster heater ETW 360","Aanvullende verwarming ETW 360","Booster heater ETW 360","Booster heater ETW 360","Booster heater ETW 360","Booster heater ETW 360","Booster heater ETW 360","Booster heater ETW 360"]
[null,220900,"Booster heater ETS 600",68,"",null,null,null,null,null,null,220900,"Booster heater ETS 600",68,false,null,220900,78,68,"sur demande","på forespørgsel",78,"Zusatzheizung für ETS 600","Booster heater ETS 600","Booster heater ETS 600","Booster heater ETS 600","Aanvullende verwarming ETS 600","Booster heater ETS 600","Booster heater ETS 600","Booster heater ETS 600","Booster heater ETS 600","Booster heater ETS 600","Booster heater ETS 600"]
[null,182108,"Booster heater ETS 700, ETT 500",71,{"$f":"IF(O1152=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,182108,"Booster heater ETS 700, ETT 500",71,false,null,182108,82,71,"sur demande","på forespørgsel",82,"Zusatzheizung für ETS 700, ETT 500","Booster heater ETS 700, ETT 500","Booster heater ETS 700, ETT 500","Booster heater ETS 700, ETT 500","Aanvullende verwarming ETS 700, ETT 500 ","Booster heater ETS 700, ETT 500","Booster heater ETS 700, ETT 500","Booster heater ETS 700, ETT 500","Booster heater ETS 700, ETT 500","Booster heater ETS 700, ETT 500","Booster heater ETS 700, ETT 500"]
[null,185276,"Booster heater ETW 420","On request","",null,null,null,null,null,null,185276,"Booster heater ETW 420","On request",false,null,185276,82,"On request","sur demande","på forespørgsel","op aanvraag","Zusatzheizung für ETW 420","Booster heater ETW 420","Booster heater ETW 420","Booster heater ETW 420","Aanvullende verwarming ETW 420","Booster heater ETW 420","Booster heater ETW 420","Booster heater ETW 420","Booster heater ETW 420","Booster heater ETW 420","Booster heater ETW 420"]
[null,182109,"Booster heater ETW 480","On request","",null,null,null,null,null,null,182109,"Booster heater ETW 480","On request",false,null,182109,91,"On request","sur demande","på forespørgsel","op aanvraag","Zusatzheizung für ETW 480","Booster heater ETW 480","Booster heater ETW 480","Booster heater ETW 480","Aanvullende verwarming ETW 480","Booster heater ETW 480","Booster heater ETW 480","Booster heater ETW 480","Booster heater ETW 480","Booster heater ETW 480","Booster heater ETW 480"]
[null,171362,"Adjuster cap controller",1,"",null,null,null,null,null,null,171362,"Adjuster cap controller",1,false,null,171362,0.9,1,"sur demande","på forespørgsel",1,"Abdeckkappe für Laderegler","Adjuster cap controller","Adjuster cap controller","Adjuster cap controller","Afdekkap ET..Kap laadregelaar ","Adjuster cap controller","Adjuster cap controller","Adjuster cap controller","Adjuster cap controller","Adjuster cap controller","Adjuster cap controller"]
[null,182028,"Vario panel ETS",72,"",null,null,null,null,null,null,182028,"Vario panel ETS",72,{"$f":"IF(AND(B1156=L1156,C1156=M1156,D1156=N1156),FALSE,TRUE)","v":false},null,182028,93,72,160,"på forespørgsel",93,"Vario-Konsole für ETS, ETT","Vario panel ETS","Vario panel ETS","Vario panel ETS","Vario-console ETS, ETT Vario-console ","Vario panel ETS","Vario panel ETS","Vario panel ETS","Vario panel ETS","Vario panel ETS","Vario panel ETS"]
[null,182102,"Vario panel ETW, ETA","On request","",null,null,null,null,null,null,182102,"Vario panel ETW, ETA","On request",false,null,182102,91,"On request",130,"på forespørgsel","op aanvraag","Vario-Konsole für ETW, ETA","Vario panel ETW, ETA","Vario panel ETW, ETA","Vario panel ETW, ETA","Vario-Konsole ETW, ETA","Vario panel ETW, ETA","Vario panel ETW, ETA","Vario panel ETW, ETA","Vario panel ETW, ETA","Vario panel ETW, ETA","Vario panel ETW, ETA"]
[null,182101,"Support panel ETW, ETA","On request","",null,null,null,null,null,null,182101,"Support panel ETW, ETA","On request",false,null,182101,46.5,"On request",55,"på forespørgsel","op aanvraag","Stützkonsole für ETW, ETA","Support panel ETW, ETA","Support panel ETW, ETA","Support panel ETW, ETA","Vloerconsole ETW, ETA","Support panel ETW, ETA","Support panel ETW, ETA","Support panel ETW, ETA","Support panel ETW, ETA","Support panel ETW, ETA","Support panel ETW, ETA"]
[null,182110,"Htg. circ. < 8h ETS 200",58,"",null,null,null,null,null,null,182110,"Htg. circ. < 8h ETS 200",58,false,null,182110,39,58,"sur demande","på forespørgsel",39,"Heizkörper für ETS 200, Lademodell < 8h","Htg. circ. < 8h ETS 200","Htg. circ. < 8h ETS 200","Htg. circ. < 8h ETS 200","Radiatorbouwset ETS 200 Verw.< 8h ","Htg. circ. < 8h ETS 200","Htg. circ. < 8h ETS 200","Htg. circ. < 8h ETS 200","Htg. circ. < 8h ETS 200","Htg. circ. < 8h ETS 200","Htg. circ. < 8h ETS 200"]
[null,182111,"Htg. circ. < 8h ETS 300",64,"",null,null,null,null,null,null,182111,"Htg. circ. < 8h ETS 300",64,false,null,182111,46.5,64,"sur demande","på forespørgsel",47,"Heizkörper für ETS 300, Lademodell < 8h","Htg. circ. < 8h ETS 300","Htg. circ. < 8h ETS 300","Htg. circ. < 8h ETS 300","Radiatorbouwset ETS 300 Verw.< 8h ","Htg. circ. < 8h ETS 300","Htg. circ. < 8h ETS 300","Htg. circ. < 8h ETS 300","Htg. circ. < 8h ETS 300","Htg. circ. < 8h ETS 300","Htg. circ. < 8h ETS 300"]
[null,182112,"Htg. circ. < 8h ETS 400",71,"",null,null,null,null,null,null,182112,"Htg. circ. < 8h ETS 400",71,false,null,182112,53,71,"sur demande","på forespørgsel",53,"Heizkörper für ETS 400, Lademodell < 8h","Htg. circ. < 8h ETS 400","Htg. circ. < 8h ETS 400","Htg. circ. < 8h ETS 400","Radiatorbouwset ETS 400 Verw.< 8h ","Htg. circ. < 8h ETS 400","Htg. circ. < 8h ETS 400","Htg. circ. < 8h ETS 400","Htg. circ. < 8h ETS 400","Htg. circ. < 8h ETS 400","Htg. circ. < 8h ETS 400"]
[null,182113,"Htg. circ. < 8h ETS 500",88,"",null,null,null,null,null,null,182113,"Htg. circ. < 8h ETS 500",88,false,null,182113,56,88,"sur demande","på forespørgsel",56,"Heizkörper für ETS 500, Lademodell < 8h","Htg. circ. < 8h ETS 500","Htg. circ. < 8h ETS 500","Htg. circ. < 8h ETS 500","Radiatorbouwset ETS 500 Verw.< 8h ","Htg. circ. < 8h ETS 500","Htg. circ. < 8h ETS 500","Htg. circ. < 8h ETS 500","Htg. circ. < 8h ETS 500","Htg. circ. < 8h ETS 500","Htg. circ. < 8h ETS 500"]
[null,182114,"Htg. circ. < 8h ETS 600",84,"",null,null,null,null,null,null,182114,"Htg. circ. < 8h ETS 600",84,false,null,182114,65,84,"sur demande","på forespørgsel",65,"Heizkörper für ETS 600, Lademodell < 8h","Htg. circ. < 8h ETS 600","Htg. circ. < 8h ETS 600","Htg. circ. < 8h ETS 600","Radiatorbouwset ETS 600 Verw.< 8h ","Htg. circ. < 8h ETS 600","Htg. circ. < 8h ETS 600","Htg. circ. < 8h ETS 600","Htg. circ. < 8h ETS 600","Htg. circ. < 8h ETS 600","Htg. circ. < 8h ETS 600"]
[null,182115,"Htg. circ. < 8h ETS 700",130,"",null,null,null,null,null,null,182115,"Htg. circ. < 8h ETS 700",130,false,null,182115,69,130,"sur demande","på forespørgsel",69,"Heizkörper für ETS 700, Lademodell < 8h","Htg. circ. < 8h ETS 700","Htg. circ. < 8h ETS 700","Htg. circ. < 8h ETS 700","Radiatorbouwset ETS 700 Verw.< 8h ","Htg. circ. < 8h ETS 700","Htg. circ. < 8h ETS 700","Htg. circ. < 8h ETS 700","Htg. circ. < 8h ETS 700","Htg. circ. < 8h ETS 700","Htg. circ. < 8h ETS 700"]
[null,182116,"Htg. circ. < 8h ETT 350","On request","",null,null,null,null,null,null,182116,"Htg. circ. < 8h ETT 350","On request",false,null,182116,56,"On request","sur demande","på forespørgsel","op aanvraag","Heizkörper für ETT 350, Lademodell < 8h","Htg. circ. < 8h ETT 350","Htg. circ. < 8h ETT 350","Htg. circ. < 8h ETT 350","Verwarmingselement-bouwset < 8h ETT 350","Htg. circ. < 8h ETT 350","Htg. circ. < 8h ETT 350","Htg. circ. < 8h ETT 350","Htg. circ. < 8h ETT 350","Htg. circ. < 8h ETT 350","Htg. circ. < 8h ETT 350"]
[null,182117,"Htg. circ. < 8h ETT 500","On request","",null,null,null,null,null,null,182117,"Htg. circ. < 8h ETT 500","On request",false,null,182117,69,"On request","sur demande","på forespørgsel","op aanvraag","Heizkörper für ETT 500, Lademodell < 8h","Htg. circ. < 8h ETT 500","Htg. circ. < 8h ETT 500","Htg. circ. < 8h ETT 500","Verwarmingselement-bouwset < 8h ETT 500","Htg. circ. < 8h ETT 500","Htg. circ. < 8h ETT 500","Htg. circ. < 8h ETT 500","Htg. circ. < 8h ETT 500","Htg. circ. < 8h ETT 500","Htg. circ. < 8h ETT 500"]
[null,223221,"Storage heater low ETH 60","On request","",null,null,null,null,null,null,223221,"Storage heater low ETH 60","On request",false,null,223221,2158,"On request","sur demande","på forespørgsel","op aanvraag","Hoch-Wärmespeicher ETH 60","Storage heater low ETH 60","Storage heater low ETH 60","Storage heater low ETH 60","Hoge-accumulatiekachel ETH 60","Storage heater low ETH 60","Storage heater low ETH 60","Storage heater low ETH 60","Storage heater low ETH 60","Storage heater low ETH 60","Storage heater low ETH 60"]
[null,231954,"Room temerature controller RTI-EH","On request","",null,null,null,null,null,null,231954,"Room temerature controller RTI-EH","On request",false,null,231954,232,"On request","sur demande","på forespørgsel","op aanvraag","Raumtemperaturregler RTI-EH","Room temerature controller RTI-EH","Room temerature controller RTI-EH","Room temerature controller RTI-EH","Thermostaat RTI-EH","Room temerature controller RTI-EH","Room temerature controller RTI-EH","Room temerature controller RTI-EH","Room temerature controller RTI-EH","Room temerature controller RTI-EH","Room temerature controller RTI-EH"]
[null,223224,"Zusatzheizung für ETH","On request","",null,null,null,null,null,null,223224,"Zusatzheizung für ETH","On request",false,null,223224,70,"On request","sur demande","på forespørgsel","op aanvraag","Zusatzheizung für ETH","Zusatzheizung für ETH","Zusatzheizung für ETH","Zusatzheizung für ETH","Aanvullende verwarming voor ETH","Zusatzheizung für ETH","Zusatzheizung für ETH","Zusatzheizung für ETH","Zusatzheizung für ETH","Zusatzheizung für ETH","Zusatzheizung für ETH"]
[null,148621,"Kitchen storage heater ETK 300","On request","",null,null,null,null,null,null,148621,"Kitchen storage heater ETK 300","On request",false,null,148621,1673,"On request","sur demande","på forespørgsel","op aanvraag","Küchen-Wärmespeicher ETK 300","Kitchen storage heater ETK 300","Kitchen storage heater ETK 300","Kitchen storage heater ETK 300","Keuken-accumulatiekachel ETK 300","Kitchen storage heater ETK 300","Kitchen storage heater ETK 300","Kitchen storage heater ETK 300","Kitchen storage heater ETK 300","Kitchen storage heater ETK 300","Kitchen storage heater ETK 300"]
[null,148629,"Cover for ETK 300","On request","",null,null,null,null,null,null,148629,"Cover for ETK 300","On request",false,null,148629,238,"On request","sur demande","på forespørgsel","op aanvraag","Verkleidung ETK 300","Cover for ETK 300","Cover for ETK 300","Cover for ETK 300","Behuizing ETK 300","Cover for ETK 300","Cover for ETK 300","Cover for ETK 300","Cover for ETK 300","Cover for ETK 300","Cover for ETK 300"]
[null,189809,"Booster heater ETK 300","On request","",null,null,null,null,null,null,189809,"Booster heater ETK 300","On request",false,null,189809,83,"On request","sur demande","på forespørgsel","op aanvraag","Zusatzheizung ETK 300","Booster heater ETK 300","Booster heater ETK 300","Booster heater ETK 300","Aanvullende verwarming ETK 300","Booster heater ETK 300","Booster heater ETK 300","Booster heater ETK 300","Booster heater ETK 300","Booster heater ETK 300","Booster heater ETK 300"]
[null,187900,"Charge control EAC 4","On request","",null,null,null,null,null,null,187900,"Charge control EAC 4","On request",false,null,187900,470,"On request","sur demande","på forespørgsel",470,"Aufladesteuerung EAC 4","Charge control EAC 4","Charge control EAC 4","Charge control EAC 4","Oplaadsturing EAC 4","Charge control EAC 4","Charge control EAC 4","Charge control EAC 4","Charge control EAC 4","Charge control EAC 4","Charge control EAC 4"]
[null,187901,"Charge control EAS 4","On request","",null,null,null,null,null,null,187901,"Charge control EAS 4","On request",false,null,187901,273,"On request","sur demande","på forespørgsel",273,"Aufladesteuerung EAS 4","Charge control EAS 4","Charge control EAS 4","Charge control EAS 4","Oplaadsturing EAS 4","Charge control EAS 4","Charge control EAS 4","Charge control EAS 4","Charge control EAS 4","Charge control EAS 4","Charge control EAS 4"]
[null,187902,"Group control unit ZSE 4","On request","",null,null,null,null,null,null,187902,"Group control unit ZSE 4","On request",false,null,187902,212,"On request","sur demande","på forespørgsel",212,"Aufladesteuerung ZSE 4","Group control unit ZSE 4","Group control unit ZSE 4","Group control unit ZSE 4","Groepstuurtoestel ZSE 4","Group control unit ZSE 4","Group control unit ZSE 4","Group control unit ZSE 4","Group control unit ZSE 4","Group control unit ZSE 4","Group control unit ZSE 4"]
[null,2050,"Load resistor BW 5","On request","",null,null,null,null,null,null,2050,"Load resistor BW 5","On request",false,null,2050,39,"On request","sur demande","på forespørgsel",39,"Belastungswiderstand BW 5","Load resistor BW 5","Load resistor BW 5","Load resistor BW 5","Belastingsweerstand BW 5","Load resistor BW 5","Load resistor BW 5","Load resistor BW 5","Load resistor BW 5","Load resistor BW 5","Load resistor BW 5"]
[null,223344,"Room temperature controller RTA-S UP",33,"",null,null,null,null,null,null,223344,"Room temperature controller RTA-S UP",33,false,null,223344,41.5,33,"sur demande","på forespørgsel","op aanvraag","Raumtemperaturregler RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Ruimtetemp. regelaar RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP"]
[null,223345,"Room temperature controller RTZ-S UP",38,"",null,null,null,null,null,null,223345,"Room temperature controller RTZ-S UP",38,false,null,223345,52,38,"sur demande","på forespørgsel",52,"Raumtemperaturregler RTZ-S UP","Room temperature controller RTZ-S UP","Room temperature controller RTZ-S UP","Room temperature controller RTZ-S UP","Ruimtetemp. regelaar RTZ-S UP","Room temperature controller RTZ-S UP","Room temperature controller RTZ-S UP","Room temperature controller RTZ-S UP","Room temperature controller RTZ-S UP","Room temperature controller RTZ-S UP","Room temperature controller RTZ-S UP"]
[null,231061,"Room temperature controller RTA-S2",21,"",null,null,null,null,null,null,231061,"Room temperature controller RTA-S2",21,false,null,231061,30,21,50,"på forespørgsel","op aanvraag","Raumtemperaturregler RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Ruimtetemp. regelaar RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2"]
[null,231063,"Room temperature controller RTNZ-S2",30,"",null,null,null,null,null,null,231063,"Room temperature controller RTNZ-S2",30,false,null,231063,46.5,30,85,"på forespørgsel",47,"Raumtemperaturregler RTNZ-S2","Room temperature controller RTNZ-S2","Room temperature controller RTNZ-S2","Room temperature controller RTNZ-S2","Ruimtetemp. regelaar RTNZ-S2","Room temperature controller RTNZ-S2","Room temperature controller RTNZ-S2","Room temperature controller RTNZ-S2","Room temperature controller RTNZ-S2","Room temperature controller RTNZ-S2","Room temperature controller RTNZ-S2"]
[null,73494,"Room temperature controller RTP-S",147,"",null,null,null,null,null,null,73494,"Room temperature controller RTP-S",147,false,null,73494,108,147,205,"på forespørgsel",108,"Raumtemperaturregler RTP-S","Room temperature controller RTP-S","Room temperature controller RTP-S","Room temperature controller RTP-S","Ruimtetemp. regelaar RTP-S","Room temperature controller RTP-S","Room temperature controller RTP-S","Room temperature controller RTP-S","Room temperature controller RTP-S","Room temperature controller RTP-S","Room temperature controller RTP-S"]
[null,73495,"Room temperature controller RTPZ-S",188,"",null,null,null,null,null,null,73495,"Room temperature controller RTPZ-S",188,false,null,73495,130,188,250,"på forespørgsel",130,"Raumtemperaturregler RTPZ-S","Room temperature controller RTPZ-S","Room temperature controller RTPZ-S","Room temperature controller RTPZ-S","Ruimtetemp. regelaar RTPZ-S","Room temperature controller RTPZ-S","Room temperature controller RTPZ-S","Room temperature controller RTPZ-S","Room temperature controller RTPZ-S","Room temperature controller RTPZ-S","Room temperature controller RTPZ-S"]
[null,233642,"Natursteinheizung Typ Galaxis MHG 35 E",574,"",null,null,null,null,null,null,233642,"Natursteinheizung Typ Galaxis MHG 35 E",574,false,null,233642,541,574,945,"på forespørgsel","op aanvraag","Natursteinheizung Typ Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E","Natuursteenverwarming Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E","Natursteinheizung Typ Galaxis MHG 35 E"]
[null,233643,"Natursteinheizung Typ Galaxis MHG 65 E",574,"",null,null,null,null,null,null,233643,"Natursteinheizung Typ Galaxis MHG 65 E",574,false,null,233643,580,574,"1.010,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E","Natuursteenverwarming Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E","Natursteinheizung Typ Galaxis MHG 65 E"]
[null,233644,"Natursteinheizung Typ Galaxis MHG 85 E",710,"",null,null,null,null,null,null,233644,"Natursteinheizung Typ Galaxis MHG 85 E",710,false,null,233644,671,710,"1.170,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E","Natuursteenverwarming Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E","Natursteinheizung Typ Galaxis MHG 85 E"]
[null,233645,"Natursteinheizung Typ Galaxis MHG 115 E",759,"",null,null,null,null,null,null,233645,"Natursteinheizung Typ Galaxis MHG 115 E",759,false,null,233645,717,759,"1.245,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E","Natuursteenverwarming Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E","Natursteinheizung Typ Galaxis MHG 115 E"]
[null,233646,"Natursteinheizung Typ Galaxis MHG 145 E",793,"",null,null,null,null,null,null,233646,"Natursteinheizung Typ Galaxis MHG 145 E",793,false,null,233646,749,793,"1.300,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E","Natuursteenverwarming Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E","Natursteinheizung Typ Galaxis MHG 145 E"]
[null,233647,"Natursteinheizung Typ Galaxis MHG 165 E",972,"",null,null,null,null,null,null,233647,"Natursteinheizung Typ Galaxis MHG 165 E",972,false,null,233647,917,972,"1.595,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E","Natuursteenverwarming Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E","Natursteinheizung Typ Galaxis MHG 165 E"]
[null,233648,"Natursteinheizung Typ Jura MHJ 35 E",574,"",null,null,null,null,null,null,233648,"Natursteinheizung Typ Jura MHJ 35 E",574,false,null,233648,541,574,950,"på forespørgsel","op aanvraag","Natursteinheizung Typ Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E","Natuursteenverwarming Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E","Natursteinheizung Typ Jura MHJ 35 E"]
[null,233649,"Natursteinheizung Typ Jura MHJ 65 E",614,"",null,null,null,null,null,null,233649,"Natursteinheizung Typ Jura MHJ 65 E",614,false,null,233649,580,614,"1.005,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E","Natuursteenverwarming Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E","Natursteinheizung Typ Jura MHJ 65 E"]
[null,233650,"Natursteinheizung Typ Jura MHJ 85 E",710,"",null,null,null,null,null,null,233650,"Natursteinheizung Typ Jura MHJ 85 E",710,false,null,233650,671,710,"1.170,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E","Natuursteenverwarming Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E","Natursteinheizung Typ Jura MHJ 85 E"]
[null,233651,"Natursteinheizung Typ Jura MHJ 115 E",759,"",null,null,null,null,null,null,233651,"Natursteinheizung Typ Jura MHJ 115 E",759,false,null,233651,717,759,"1.245,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E","Natuursteenverwarming Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E","Natursteinheizung Typ Jura MHJ 115 E"]
[null,233652,"Natursteinheizung Typ Jura MHJ 145 E",793,"",null,null,null,null,null,null,233652,"Natursteinheizung Typ Jura MHJ 145 E",793,false,null,233652,749,793,"1.300,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E","Natuursteenverwarming Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E","Natursteinheizung Typ Jura MHJ 145 E"]
[null,233653,"Natursteinheizung Typ Jura MHJ 165 E",972,"",null,null,null,null,null,null,233653,"Natursteinheizung Typ Jura MHJ 165 E",972,false,null,233653,917,972,"1.595,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E","Natuursteenverwarming Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E","Natursteinheizung Typ Jura MHJ 165 E"]
[null,233654,"Natursteinheizung Typ Sahara MHS 35 E",574,"",null,null,null,null,null,null,233654,"Natursteinheizung Typ Sahara MHS 35 E",574,false,null,233654,541,574,945,"på forespørgsel","op aanvraag","Natursteinheizung Typ Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E","Natuursteenverwarming Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E","Natursteinheizung Typ Sahara MHS 35 E"]
[null,233655,"Natursteinheizung Typ Sahara MHS 65 E",614,"",null,null,null,null,null,null,233655,"Natursteinheizung Typ Sahara MHS 65 E",614,false,null,233655,580,614,"1.010,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E","Natuursteenverwarming Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E","Natursteinheizung Typ Sahara MHS 65 E"]
[null,233656,"Natursteinheizung Typ Sahara MHS 85 E",710,"",null,null,null,null,null,null,233656,"Natursteinheizung Typ Sahara MHS 85 E",710,false,null,233656,671,710,"1.170,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E","Natuursteenverwarming Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E","Natursteinheizung Typ Sahara MHS 85 E"]
[null,233657,"Natursteinheizung Typ Sahara MHS 115 E",759,"",null,null,null,null,null,null,233657,"Natursteinheizung Typ Sahara MHS 115 E",759,false,null,233657,717,759,"1.245,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E","Natuursteenverwarming Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E","Natursteinheizung Typ Sahara MHS 115 E"]
[null,233658,"Natursteinheizung Typ Sahara MHS 145 E",793,"",null,null,null,null,null,null,233658,"Natursteinheizung Typ Sahara MHS 145 E",793,false,null,233658,749,793,"1.300,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E","Natuursteenverwarming Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E","Natursteinheizung Typ Sahara MHS 145 E"]
[null,233659,"Natursteinheizung Typ Sahara MHS 165 E",972,"",null,null,null,null,null,null,233659,"Natursteinheizung Typ Sahara MHS 165 E",972,false,null,233659,917,972,"1.595,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E","Natuursteenverwarming Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E","Natursteinheizung Typ Sahara MHS 165 E"]
[null,233660,"Natursteinheizung Typ Prinos MHP 35 E",605,"",null,null,null,null,null,null,233660,"Natursteinheizung Typ Prinos MHP 35 E",605,false,null,233660,635,605,995,"på forespørgsel","op aanvraag","Natursteinheizung Typ Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E","Natuursteenverwarming Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E","Natursteinheizung Typ Prinos MHP 35 E"]
[null,233661,"Natursteinheizung Typ Prinos MHP 65 E",677,"",null,null,null,null,null,null,233661,"Natursteinheizung Typ Prinos MHP 65 E",677,false,null,233661,711,677,"1.110,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E","Natuursteenverwarming Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E","Natursteinheizung Typ Prinos MHP 65 E"]
[null,233662,"Natursteinheizung Typ Prinos MHP 85 E",761,"",null,null,null,null,null,null,233662,"Natursteinheizung Typ Prinos MHP 85 E",761,false,null,233662,797,761,"1.245,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E","Natuursteenverwarming Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E","Natursteinheizung Typ Prinos MHP 85 E"]
[null,233663,"Natursteinheizung Typ Prinos MHP 115 E",810,"",null,null,null,null,null,null,233663,"Natursteinheizung Typ Prinos MHP 115 E",810,false,null,233663,850,810,"1.330,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E","Natuursteenverwarming Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E","Natursteinheizung Typ Prinos MHP 115 E"]
[null,233664,"Natursteinheizung Typ Prinos MHP 145 E",861,"",null,null,null,null,null,null,233664,"Natursteinheizung Typ Prinos MHP 145 E",861,false,null,233664,902,861,"1.410,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E","Natuursteenverwarming Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E","Natursteinheizung Typ Prinos MHP 145 E"]
[null,233665,"Natursteinheizung Typ Prinos MHP 165 E",1013,"",null,null,null,null,null,null,233665,"Natursteinheizung Typ Prinos MHP 165 E",1013,false,null,233665,1062,1013,"1.660,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E","Natuursteenverwarming Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E","Natursteinheizung Typ Prinos MHP 165 E"]
[null,233666,"Natursteinheizung Speckstein SPH 35 E",701,"",null,null,null,null,null,null,233666,"Natursteinheizung Speckstein SPH 35 E",701,false,null,233666,760,701,"1.150,00","på forespørgsel","op aanvraag","Natursteinheizung Speckstein SPH 35 E","Natursteinheizung Speckstein SPH 35 E","Natursteinheizung Speckstein SPH 35 E","Natursteinheizung Speckstein SPH 35 E","Natuursteenverwarming SPH 35 E","Natursteinheizung Speckstein SPH 35 E","Natursteinheizung Speckstein SPH 35 E","Natursteinheizung Speckstein SPH 35 E","Natursteinheizung Speckstein SPH 35 E","Natursteinheizung Speckstein SPH 35 E","Natursteinheizung Speckstein SPH 35 E"]
[null,233667,"Natursteinheizung Speckstein SPH 65 E",736,"",null,null,null,null,null,null,233667,"Natursteinheizung Speckstein SPH 65 E",736,false,null,233667,797,736,"1.210,00","på forespørgsel","op aanvraag","Natursteinheizung Speckstein SPH 65 E","Natursteinheizung Speckstein SPH 65 E","Natursteinheizung Speckstein SPH 65 E","Natursteinheizung Speckstein SPH 65 E","Natuursteenverwarming SPH 65 E","Natursteinheizung Speckstein SPH 65 E","Natursteinheizung Speckstein SPH 65 E","Natursteinheizung Speckstein SPH 65 E","Natursteinheizung Speckstein SPH 65 E","Natursteinheizung Speckstein SPH 65 E","Natursteinheizung Speckstein SPH 65 E"]
[null,233668,"Natursteinheizung Speckstein SPH 85 E",880,"",null,null,null,null,null,null,233668,"Natursteinheizung Speckstein SPH 85 E",880,false,null,233668,953,880,"1.445,00","på forespørgsel","op aanvraag","Natursteinheizung Speckstein SPH 85 E","Natursteinheizung Speckstein SPH 85 E","Natursteinheizung Speckstein SPH 85 E","Natursteinheizung Speckstein SPH 85 E","Natuursteenverwarming SPH 85 E","Natursteinheizung Speckstein SPH 85 E","Natursteinheizung Speckstein SPH 85 E","Natursteinheizung Speckstein SPH 85 E","Natursteinheizung Speckstein SPH 85 E","Natursteinheizung Speckstein SPH 85 E","Natursteinheizung Speckstein SPH 85 E"]
[null,233669,"Natursteinheizung Speckstein SPH 115 E",946,"",null,null,null,null,null,null,233669,"Natursteinheizung Speckstein SPH 115 E",946,false,null,233669,1024,946,"1.555,00","på forespørgsel","op aanvraag","Natursteinheizung Speckstein SPH 115 E","Natursteinheizung Speckstein SPH 115 E","Natursteinheizung Speckstein SPH 115 E","Natursteinheizung Speckstein SPH 115 E","Natuursteenverwarming SPH 115 E","Natursteinheizung Speckstein SPH 115 E","Natursteinheizung Speckstein SPH 115 E","Natursteinheizung Speckstein SPH 115 E","Natursteinheizung Speckstein SPH 115 E","Natursteinheizung Speckstein SPH 115 E","Natursteinheizung Speckstein SPH 115 E"]
[null,233670,"Natursteinheizung Speckstein SPH 145 E",1014,"",null,null,null,null,null,null,233670,"Natursteinheizung Speckstein SPH 145 E",1014,false,null,233670,1098,1014,"1.660,00","på forespørgsel","op aanvraag","Natursteinheizung Speckstein SPH 145 E","Natursteinheizung Speckstein SPH 145 E","Natursteinheizung Speckstein SPH 145 E","Natursteinheizung Speckstein SPH 145 E","Natuursteenverwarming SPH 145 E","Natursteinheizung Speckstein SPH 145 E","Natursteinheizung Speckstein SPH 145 E","Natursteinheizung Speckstein SPH 145 E","Natursteinheizung Speckstein SPH 145 E","Natursteinheizung Speckstein SPH 145 E","Natursteinheizung Speckstein SPH 145 E"]
[null,233671,"Natursteinheizung Speckstein SPH 165 E",1141,"",null,null,null,null,null,null,233671,"Natursteinheizung Speckstein SPH 165 E",1141,false,null,233671,1236,1141,"1.870,00","på forespørgsel","op aanvraag","Natursteinheizung Speckstein SPH 165 E","Natursteinheizung Speckstein SPH 165 E","Natursteinheizung Speckstein SPH 165 E","Natursteinheizung Speckstein SPH 165 E","Natuursteenverwarming SPH 165 E","Natursteinheizung Speckstein SPH 165 E","Natursteinheizung Speckstein SPH 165 E","Natursteinheizung Speckstein SPH 165 E","Natursteinheizung Speckstein SPH 165 E","Natursteinheizung Speckstein SPH 165 E","Natursteinheizung Speckstein SPH 165 E"]
[null,233672,"Natursteinheizung Typ Varios MHV 35 E",542,"",null,null,null,null,null,null,233672,"Natursteinheizung Typ Varios MHV 35 E",542,false,null,233672,486,542,910,"på forespørgsel","op aanvraag","Natursteinheizung Typ Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E","Natuursteenverwarming Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E","Natursteinheizung Typ Varios MHV 35 E"]
[null,233673,"Natursteinheizung Typ Varios MHV 65 E",582,{"$f":"IF(O1214=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,233673,"Natursteinheizung Typ Varios MHV 65 E",582,false,null,233673,522,582,955,"på forespørgsel","op aanvraag","Natursteinheizung Typ Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E","Natuursteenverwarming Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E","Natursteinheizung Typ Varios MHV 65 E"]
[null,233674,"Natursteinheizung Typ Varios MHV 85 E",679,"",null,null,null,null,null,null,233674,"Natursteinheizung Typ Varios MHV 85 E",679,false,null,233674,610,679,"1.115,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E","Natuursteenverwarming Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E","Natursteinheizung Typ Varios MHV 85 E"]
[null,233675,"Natursteinheizung Typ Varios MHV 115 E",725,"",null,null,null,null,null,null,233675,"Natursteinheizung Typ Varios MHV 115 E",725,false,null,233675,650,725,"1.190,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E","Natuursteenverwarming Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E","Natursteinheizung Typ Varios MHV 115 E"]
[null,233676,"Natursteinheizung Typ Varios MHV 145 E",770,"",null,null,null,null,null,null,233676,"Natursteinheizung Typ Varios MHV 145 E",770,false,null,233676,689,770,"1.265,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E","Natuursteenverwarming Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E","Natursteinheizung Typ Varios MHV 145 E"]
[null,233677,"Natursteinheizung Typ Varios MHV 165 E",898,"",null,null,null,null,null,null,233677,"Natursteinheizung Typ Varios MHV 165 E",898,{"$f":"IF(AND(B1218=L1218,C1218=M1218,D1218=N1218),FALSE,TRUE)","v":false},null,233677,806,898,"1.475,00","på forespørgsel","op aanvraag","Natursteinheizung Typ Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E","Natuursteenverwarming Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E","Natursteinheizung Typ Varios MHV 165 E"]
[null,223344,"Room temperature controller RTA-S UP",33,"",null,null,null,null,null,null,223344,"Room temperature controller RTA-S UP",33,false,null,223344,41.5,33,"sur demande","på forespørgsel","op aanvraag","Raumtemperaturregler RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Ruimtetemp. regelaar RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP","Room temperature controller RTA-S UP"]
[null,223343,"Room temperature controller RTA 3600 UP",77,"",null,null,null,null,null,null,223343,"Room temperature controller RTA 3600 UP",77,false,null,223343,41.5,77,"sur demande","på forespørgsel","op aanvraag","Raumtemperaturregler RTA 3600 UP","Room temperature controller RTA 3600 UP","Room temperature controller RTA 3600 UP","Room temperature controller RTA 3600 UP","Ruimtetemp. regelaar RTA 3600 UP","Room temperature controller RTA 3600 UP","Room temperature controller RTA 3600 UP","Room temperature controller RTA 3600 UP","Room temperature controller RTA 3600 UP","Room temperature controller RTA 3600 UP","Room temperature controller RTA 3600 UP"]
[null,231061,"Room temperature controller RTA-S2",21,"",null,null,null,null,null,null,231061,"Room temperature controller RTA-S2",21,false,null,231061,30,21,50,"på forespørgsel","op aanvraag","Raumtemperaturregler RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Ruimtetemp. regelaar RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2","Room temperature controller RTA-S2"]
[null,231062,"Room temperature controller RTA 3000 S2",17,"",null,null,null,null,null,null,231062,"Room temperature controller RTA 3000 S2",17,false,null,231062,37.5,17,"sur demande","på forespørgsel","op aanvraag","Raumtemperaturregler RTA 3000 S2","Room temperature controller RTA 3000 S2","Room temperature controller RTA 3000 S2","Room temperature controller RTA 3000 S2","Ruimtetemp. regelaar RTA 3000 S2","Room temperature controller RTA 3000 S2","Room temperature controller RTA 3000 S2","Room temperature controller RTA 3000 S2","Room temperature controller RTA 3000 S2","Room temperature controller RTA 3000 S2","Room temperature controller RTA 3000 S2"]
[null,185605,"Accessory set comfort FT-C",201,"",null,null,null,null,null,null,185605,"Accessory set comfort FT-C",201,false,null,185605,206,201,"sur demande","på forespørgsel","op aanvraag","Sonderzubehör FT-C set","Accessory set comfort FT-C","Accessory set comfort FT-C","Accessory set comfort FT-C","Speciale toebehoren FT-C set","Accessory set comfort FT-C","Accessory set comfort FT-C","Accessory set comfort FT-C","Accessory set comfort FT-C","Accessory set comfort FT-C","Accessory set comfort FT-C"]
[null,185604,"Accessory set standard FT-S",150,"",null,null,null,null,null,null,185604,"Accessory set standard FT-S",150,false,null,185604,150,150,"sur demande","på forespørgsel","op aanvraag","Sonderzubehör FT-S set","Accessory set standard FT-S","Accessory set standard FT-S","Accessory set standard FT-S","Speciale toebehoren FT-S set","Accessory set standard FT-S","Accessory set standard FT-S","Accessory set standard FT-S","Accessory set standard FT-S","Accessory set standard FT-S","Accessory set standard FT-S"]
[null,231065,"UFH temperature controller RTF-Z2",150,"",null,null,null,null,null,null,231065,"UFH temperature controller RTF-Z2",150,false,null,231065,174,150,"sur demande","på forespørgsel","op aanvraag","Fußboden-Temperaturregler RTF-Z2","UFH temperature controller RTF-Z2","UFH temperature controller RTF-Z2","UFH temperature controller RTF-Z2","Vloerverwarmings thermostaat RTF-Z2","UFH temperature controller RTF-Z2","UFH temperature controller RTF-Z2","UFH temperature controller RTF-Z2","UFH temperature controller RTF-Z2","UFH temperature controller RTF-Z2","UFH temperature controller RTF-Z2"]
[null,185547,"UFH temperature controller RTF",101,"",null,null,null,null,null,null,185547,"UFH temperature controller RTF",101,false,null,185547,121,101,"sur demande","på forespørgsel","op aanvraag","Fußboden-Temperaturregler RTF","UFH temperature controller RTF","UFH temperature controller RTF","UFH temperature controller RTF","Vloerverwarmings thermostaat RTF","UFH temperature controller RTF","UFH temperature controller RTF","UFH temperature controller RTF","UFH temperature controller RTF","UFH temperature controller RTF","UFH temperature controller RTF"]
[null,223346,"UFH temperature controller RTF-AP 2",69,"",null,null,null,null,null,null,223346,"UFH temperature controller RTF-AP 2",69,false,null,223346,111,69,"sur demande","på forespørgsel","op aanvraag","Fußboden-Temperaturregler RTF-AP 2","UFH temperature controller RTF-AP 2","UFH temperature controller RTF-AP 2","UFH temperature controller RTF-AP 2","Vloerverwarmings thermostaat RTF-AP 2","UFH temperature controller RTF-AP 2","UFH temperature controller RTF-AP 2","UFH temperature controller RTF-AP 2","UFH temperature controller RTF-AP 2","UFH temperature controller RTF-AP 2","UFH temperature controller RTF-AP 2"]
[null,233856,"Bad-/Handtuchheizkörper BHE 75 Classic",441,"",null,null,null,null,null,null,233856,"Bad-/Handtuchheizkörper BHE 75 Classic",441,false,null,233856,515,441,"sur demande","på forespørgsel","op aanvraag","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/handdoekradiator BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic","Bad-/Handtuchheizkörper BHE 75 Classic"]
[null,233857,"Bad-/Handtuchheizkörper BHE 100 Classic",511,"",null,null,null,null,null,null,233857,"Bad-/Handtuchheizkörper BHE 100 Classic",511,false,null,233857,562,511,"sur demande","på forespørgsel","op aanvraag","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/handdoekradiator BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic","Bad-/Handtuchheizkörper BHE 100 Classic"]
[null,233858,"Bad-/Handtuchheizkörper BHE 175 Classic",552,"",null,null,null,null,null,null,233858,"Bad-/Handtuchheizkörper BHE 175 Classic",552,false,null,233858,623,552,"sur demande","på forespørgsel","op aanvraag","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/handdoekradiator BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic","Bad-/Handtuchheizkörper BHE 175 Classic"]
[null,233859,"Bad-/Handtuchheizkörper BHE 100 Style",544,"",null,null,null,null,null,null,233859,"Bad-/Handtuchheizkörper BHE 100 Style",544,false,null,233859,670,544,"sur demande","på forespørgsel","op aanvraag","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/handdoekradiator BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style","Bad-/Handtuchheizkörper BHE 100 Style"]
[null,71815,"Wall mounted convector CON 10 S",153,"",null,null,null,null,null,null,71815,"Wall mounted convector CON 10 S",153,false,null,71815,198,153,"sur demande","på forespørgsel",223,"Wand-Konvektor CON 10 S","Wall mounted convector CON 10 S","Wall mounted convector CON 10 S","Wall mounted convector CON 10 S","Wandconvector CON 10 S","Wall mounted convector CON 10 S","Wall mounted convector CON 10 S","Wall mounted convector CON 10 S","Wall mounted convector CON 10 S","Wall mounted convector CON 10 S","Wall mounted convector CON 10 S"]
[null,71816,"Wall mounted convector CON 15 S",163,"",null,null,null,null,null,null,71816,"Wall mounted convector CON 15 S",163,false,null,71816,207,163,"sur demande","på forespørgsel",250,"Wand-Konvektor CON 15 S","Wall mounted convector CON 15 S","Wall mounted convector CON 15 S","Wall mounted convector CON 15 S","Wandconvector CON 15 S","Wall mounted convector CON 15 S","Wall mounted convector CON 15 S","Wall mounted convector CON 15 S","Wall mounted convector CON 15 S","Wall mounted convector CON 15 S","Wall mounted convector CON 15 S"]
[null,71817,"Wall mounted convector CON 20 S",170,"",null,null,null,null,null,null,71817,"Wall mounted convector CON 20 S",170,false,null,71817,226,170,"sur demande","på forespørgsel",262,"Wand-Konvektor CON 20 S","Wall mounted convector CON 20 S","Wall mounted convector CON 20 S","Wall mounted convector CON 20 S","Wandconvector CON 20 S","Wall mounted convector CON 20 S","Wall mounted convector CON 20 S","Wall mounted convector CON 20 S","Wall mounted convector CON 20 S","Wall mounted convector CON 20 S","Wall mounted convector CON 20 S"]
[null,71818,"Wall mounted convector CON 30 S",235,"",null,null,null,null,null,null,71818,"Wall mounted convector CON 30 S",235,false,null,71818,255,235,"sur demande","på forespørgsel",338,"Wand-Konvektor CON 30 S","Wall mounted convector CON 30 S","Wall mounted convector CON 30 S","Wall mounted convector CON 30 S","Wandconvector CON 30 S","Wall mounted convector CON 30 S","Wall mounted convector CON 30 S","Wall mounted convector CON 30 S","Wall mounted convector CON 30 S","Wall mounted convector CON 30 S","Wall mounted convector CON 30 S"]
[null,71819,"Wall mounted convector CON 10 ZS",193,"",null,null,null,null,null,null,71819,"Wall mounted convector CON 10 ZS",193,false,null,71819,245,193,"sur demande","på forespørgsel",282,"Wand-Konvektor CON 10 ZS","Wall mounted convector CON 10 ZS","Wall mounted convector CON 10 ZS","Wall mounted convector CON 10 ZS","Wandconvector CON 10 ZS","Wall mounted convector CON 10 ZS","Wall mounted convector CON 10 ZS","Wall mounted convector CON 10 ZS","Wall mounted convector CON 10 ZS","Wall mounted convector CON 10 ZS","Wall mounted convector CON 10 ZS"]
[null,71820,"Wall mounted convector CON 15 ZS",206,"",null,null,null,null,null,null,71820,"Wall mounted convector CON 15 ZS",206,false,null,71820,259,206,"sur demande","på forespørgsel",298,"Wand-Konvektor CON 15 ZS","Wall mounted convector CON 15 ZS","Wall mounted convector CON 15 ZS","Wall mounted convector CON 15 ZS","Wandconvector CON 15 ZS","Wall mounted convector CON 15 ZS","Wall mounted convector CON 15 ZS","Wall mounted convector CON 15 ZS","Wall mounted convector CON 15 ZS","Wall mounted convector CON 15 ZS","Wall mounted convector CON 15 ZS"]
[null,71821,"Wall mounted convector CON 20 ZS",214,"",null,null,null,null,null,null,71821,"Wall mounted convector CON 20 ZS",214,false,null,71821,277,214,"sur demande","på forespørgsel",325,"Wand-Konvektor CON 20 ZS","Wall mounted convector CON 20 ZS","Wall mounted convector CON 20 ZS","Wall mounted convector CON 20 ZS","Wandconvector CON 20 ZS","Wall mounted convector CON 20 ZS","Wall mounted convector CON 20 ZS","Wall mounted convector CON 20 ZS","Wall mounted convector CON 20 ZS","Wall mounted convector CON 20 ZS","Wall mounted convector CON 20 ZS"]
[null,71822,"Wall mounted convector CON 30 ZS",278,"",null,null,null,null,null,null,71822,"Wall mounted convector CON 30 ZS",278,false,null,71822,306,278,"sur demande","på forespørgsel",390,"Wand-Konvektor CON 30 ZS","Wall mounted convector CON 30 ZS","Wall mounted convector CON 30 ZS","Wall mounted convector CON 30 ZS","Wandconvector CON 30 ZS","Wall mounted convector CON 30 ZS","Wall mounted convector CON 30 ZS","Wall mounted convector CON 30 ZS","Wall mounted convector CON 30 ZS","Wall mounted convector CON 30 ZS","Wall mounted convector CON 30 ZS"]
[null,72464,"Towel-holder for CON 15","On request","",null,null,null,null,null,null,72464,"Towel-holder for CON 15","On request",false,null,72464,41,"On request","sur demande","på forespørgsel",41,"Handtuchhalter CON 15","Towel-holder for CON 15","Towel-holder for CON 15","Towel-holder for CON 15","Handdoekhouder CON 15 Handdoekhouder","Towel-holder for CON 15","Towel-holder for CON 15","Towel-holder for CON 15","Towel-holder for CON 15","Towel-holder for CON 15","Towel-holder for CON 15"]
[null,72465,"Towel-holder for CON 20","On request","",null,null,null,null,null,null,72465,"Towel-holder for CON 20","On request",false,null,72465,44,"On request","sur demande","på forespørgsel",44,"Handtuchhalter CON 20","Towel-holder for CON 20","Towel-holder for CON 20","Towel-holder for CON 20","Handdoekhouder CON 20 Handdoekhouder ","Towel-holder for CON 20","Towel-holder for CON 20","Towel-holder for CON 20","Towel-holder for CON 20","Towel-holder for CON 20","Towel-holder for CON 20"]
[null,72466,"Towel-holder for CON 30","On request","",null,null,null,null,null,null,72466,"Towel-holder for CON 30","On request",false,null,72466,49,"On request","sur demande","på forespørgsel",49,"Handtuchhalter CON 30","Towel-holder for CON 30","Towel-holder for CON 30","Towel-holder for CON 30","Handdoekhouder CON 30 Handdoekhouder ","Towel-holder for CON 30","Towel-holder for CON 30","Towel-holder for CON 30","Towel-holder for CON 30","Towel-holder for CON 30","Towel-holder for CON 30"]
[null,220716,"Wall mounted convector CNS 50 S",76,"",null,null,null,null,null,null,220716,"Wall mounted convector CNS 50 S",76,false,null,220716,113,76,"sur demande","på forespørgsel",116,"Wand-Konvektor CNS 50 S","Wall mounted convector CNS 50 S","Wall mounted convector CNS 50 S","Wall mounted convector CNS 50 S","Wandconvector CNS 50 S","Wall mounted convector CNS 50 S","Wall mounted convector CNS 50 S","Wall mounted convector CNS 50 S","Wall mounted convector CNS 50 S","Wall mounted convector CNS 50 S","Wall mounted convector CNS 50 S"]
[null,220717,"Wall mounted convector CNS 75 S",83,"",null,null,null,null,null,null,220717,"Wall mounted convector CNS 75 S",83,false,null,220717,124,83,"sur demande","på forespørgsel",122,"Wand-Konvektor CNS 75 S","Wall mounted convector CNS 75 S","Wall mounted convector CNS 75 S","Wall mounted convector CNS 75 S","Wandconvector CNS 75 S","Wall mounted convector CNS 75 S","Wall mounted convector CNS 75 S","Wall mounted convector CNS 75 S","Wall mounted convector CNS 75 S","Wall mounted convector CNS 75 S","Wall mounted convector CNS 75 S"]
[null,220718,"Wall mounted convector CNS 100 S",83,"",null,null,null,null,null,null,220718,"Wall mounted convector CNS 100 S",83,false,null,220718,129,83,"sur demande","på forespørgsel",129,"Wand-Konvektor CNS 100 S","Wall mounted convector CNS 100 S","Wall mounted convector CNS 100 S","Wall mounted convector CNS 100 S","Wandconvector CNS 100 S","Wall mounted convector CNS 100 S","Wall mounted convector CNS 100 S","Wall mounted convector CNS 100 S","Wall mounted convector CNS 100 S","Wall mounted convector CNS 100 S","Wall mounted convector CNS 100 S"]
[null,220720,"Wall mounted convector CNS 150 S",96,"",null,null,null,null,null,null,220720,"Wall mounted convector CNS 150 S",96,false,null,220720,136,96,"sur demande","på forespørgsel",140,"Wand-Konvektor CNS 150 S","Wall mounted convector CNS 150 S","Wall mounted convector CNS 150 S","Wall mounted convector CNS 150 S","Wandconvector CNS 150 S","Wall mounted convector CNS 150 S","Wall mounted convector CNS 150 S","Wall mounted convector CNS 150 S","Wall mounted convector CNS 150 S","Wall mounted convector CNS 150 S","Wall mounted convector CNS 150 S"]
[null,220722,"Wall mounted convector CNS 200 S",109,"",null,null,null,null,null,null,220722,"Wall mounted convector CNS 200 S",109,false,null,220722,145,109,"sur demande","på forespørgsel",159,"Wand-Konvektor CNS 200 S","Wall mounted convector CNS 200 S","Wall mounted convector CNS 200 S","Wall mounted convector CNS 200 S","Wandconvector CNS 200 S","Wall mounted convector CNS 200 S","Wall mounted convector CNS 200 S","Wall mounted convector CNS 200 S","Wall mounted convector CNS 200 S","Wall mounted convector CNS 200 S","Wall mounted convector CNS 200 S"]
[null,220723,"Wall mounted convector CNS 250 S",138,"",null,null,null,null,null,null,220723,"Wall mounted convector CNS 250 S",138,false,null,220723,166,138,"sur demande","på forespørgsel",174,"Wand-Konvektor CNS 250 S","Wall mounted convector CNS 250 S","Wall mounted convector CNS 250 S","Wall mounted convector CNS 250 S","Wandconvector CNS 250 S","Wall mounted convector CNS 250 S","Wall mounted convector CNS 250 S","Wall mounted convector CNS 250 S","Wall mounted convector CNS 250 S","Wall mounted convector CNS 250 S","Wall mounted convector CNS 250 S"]
[null,220724,"Wall mounted convector CNS 300 S",154,"",null,null,null,null,null,null,220724,"Wall mounted convector CNS 300 S",154,false,null,220724,189,154,"sur demande","på forespørgsel",188,"Wand-Konvektor CNS 300 S","Wall mounted convector CNS 300 S","Wall mounted convector CNS 300 S","Wall mounted convector CNS 300 S","Wandconvector CNS 300 S","Wall mounted convector CNS 300 S","Wall mounted convector CNS 300 S","Wall mounted convector CNS 300 S","Wall mounted convector CNS 300 S","Wall mounted convector CNS 300 S","Wall mounted convector CNS 300 S"]
[null,229740,"Wall mounted convector CNS 50 SE",104,"",null,null,null,null,null,null,229740,"Wall mounted convector CNS 50 SE",104,false,null,229740,153,104,"sur demande","på forespørgsel",152,"Wand-Konvektor CNS 50 SE","Wall mounted convector CNS 50 SE","Wall mounted convector CNS 50 SE","Wall mounted convector CNS 50 SE","Convector CNS 50 SE","Wall mounted convector CNS 50 SE","Wall mounted convector CNS 50 SE","Wall mounted convector CNS 50 SE","Wall mounted convector CNS 50 SE","Wall mounted convector CNS 50 SE","Wall mounted convector CNS 50 SE"]
[null,229741,"Wall mounted convector CNS 75 SE",111,"",null,null,null,null,null,null,229741,"Wall mounted convector CNS 75 SE",111,false,null,229741,160,111,"sur demande","på forespørgsel",160,"Wand-Konvektor CNS 75 SE","Wall mounted convector CNS 75 SE","Wall mounted convector CNS 75 SE","Wall mounted convector CNS 75 SE","Convector CNS 75 SE","Wall mounted convector CNS 75 SE","Wall mounted convector CNS 75 SE","Wall mounted convector CNS 75 SE","Wall mounted convector CNS 75 SE","Wall mounted convector CNS 75 SE","Wall mounted convector CNS 75 SE"]
[null,229742,"Wall mounted convector CNS 100 SE",111,"",null,null,null,null,null,null,229742,"Wall mounted convector CNS 100 SE",111,false,null,229742,164,111,"sur demande","på forespørgsel",164,"Wand-Konvektor CNS 100 SE","Wall mounted convector CNS 100 SE","Wall mounted convector CNS 100 SE","Wall mounted convector CNS 100 SE","Convector CNS 100 SE","Wall mounted convector CNS 100 SE","Wall mounted convector CNS 100 SE","Wall mounted convector CNS 100 SE","Wall mounted convector CNS 100 SE","Wall mounted convector CNS 100 SE","Wall mounted convector CNS 100 SE"]
[null,229744,"Wall mounted convector CNS 150 SE",123,{"$f":"IF(O1253=TRUE,\"O\",\"\")","v":""},null,null,null,null,null,null,229744,"Wall mounted convector CNS 150 SE",123,false,null,229744,170,123,"sur demande","på forespørgsel",177,"Wand-Konvektor CNS 150 SE","Wall mounted convector CNS 150 SE","Wall mounted convector CNS 150 SE","Wall mounted convector CNS 150 SE","Convector CNS 150 SE","Wall mounted convector CNS 150 SE","Wall mounted convector CNS 150 SE","Wall mounted convector CNS 150 SE","Wall mounted convector CNS 150 SE","Wall mounted convector CNS 150 SE","Wall mounted convector CNS 150 SE"]
[null,229746,"Wall mounted convector CNS 200 SE",137,"",null,null,null,null,null,null,229746,"Wall mounted convector CNS 200 SE",137,false,null,229746,177,137,"sur demande","på forespørgsel",193,"Wand-Konvektor CNS 200 SE","Wall mounted convector CNS 200 SE","Wall mounted convector CNS 200 SE","Wall mounted convector CNS 200 SE","Convector CNS 200 SE","Wall mounted convector CNS 200 SE","Wall mounted convector CNS 200 SE","Wall mounted convector CNS 200 SE","Wall mounted convector CNS 200 SE","Wall mounted convector CNS 200 SE","Wall mounted convector CNS 200 SE"]
[null,229747,"Wall mounted convector CNS 250 SE",167,"",null,null,null,null,null,null,229747,"Wall mounted convector CNS 250 SE",167,false,null,229747,199,167,"sur demande","på forespørgsel",207,"Wand-Konvektor CNS 250 SE","Wall mounted convector CNS 250 SE","Wall mounted convector CNS 250 SE","Wall mounted convector CNS 250 SE","Convector CNS 250 SE","Wall mounted convector CNS 250 SE","Wall mounted convector CNS 250 SE","Wall mounted convector CNS 250 SE","Wall mounted convector CNS 250 SE","Wall mounted convector CNS 250 SE","Wall mounted convector CNS 250 SE"]
[null,229748,"Wall mounted convector CNS 300 SE",182,"",null,null,null,null,null,null,229748,"Wall mounted convector CNS 300 SE",182,false,null,229748,220,182,"sur demande","på forespørgsel",221,"Wand-Konvektor CNS 300 SE","Wall mounted convector CNS 300 SE","Wall mounted convector CNS 300 SE","Wall mounted convector CNS 300 SE","Convector CNS 300 SE","Wall mounted convector CNS 300 SE","Wall mounted convector CNS 300 SE","Wall mounted convector CNS 300 SE","Wall mounted convector CNS 300 SE","Wall mounted convector CNS 300 SE","Wall mounted convector CNS 300 SE"]
[null,74376,"Freestanding convector CS 20",66,"",null,null,null,null,null,null,74376,"Freestanding convector CS 20",66,{"$f":"IF(AND(B1257=L1257,C1257=M1257,D1257=N1257),FALSE,TRUE)","v":false},null,74376,89,66,"sur demande","på forespørgsel",113,"Stand-Konvektor CS 20","Freestanding convector CS 20","Freestanding convector CS 20","Freestanding convector CS 20","Stand convector CS 20","Freestanding convector CS 20","Freestanding convector CS 20","Freestanding convector CS 20","Freestanding convector CS 20","Freestanding convector CS 20","Freestanding convector CS 20"]
[null,74377,"Freestanding convector CS 20 L",83,"",null,null,null,null,null,null,74377,"Freestanding convector CS 20 L",83,false,null,74377,111,83,"sur demande","på forespørgsel",141,"Stand-Konvektor CS 20 L","Freestanding convector CS 20 L","Freestanding convector CS 20 L","Freestanding convector CS 20 L","Stand convector CS 20 L","Freestanding convector CS 20 L","Freestanding convector CS 20 L","Freestanding convector CS 20 L","Freestanding convector CS 20 L","Freestanding convector CS 20 L","Freestanding convector CS 20 L"]
[null,71793,"Quick-response heater CK 20 S",115,"",null,null,null,null,null,null,71793,"Quick-response heater CK 20 S",115,false,null,71793,128,115,205,"på forespørgsel",172,"Schnellheizer CK 20 S","Quick-response heater CK 20 S","Quick-response heater CK 20 S","Quick-response heater CK 20 S","Convector CK 20 S","Quick-response heater CK 20 S","Quick-response heater CK 20 S","Quick-response heater CK 20 S","Quick-response heater CK 20 S","Quick-response heater CK 20 S","Quick-response heater CK 20 S"]
[null,71795,"Quick-response heater CKZ 20 S",154,"",null,null,null,null,null,null,71795,"Quick-response heater CKZ 20 S",154,false,null,71795,174,154,290,"på forespørgsel",224,"Schnellheizer CKZ 20 S","Quick-response heater CKZ 20 S","Quick-response heater CKZ 20 S","Quick-response heater CKZ 20 S","Convector CKZ 20 S","Quick-response heater CKZ 20 S","Quick-response heater CKZ 20 S","Quick-response heater CKZ 20 S","Quick-response heater CKZ 20 S","Quick-response heater CKZ 20 S","Quick-response heater CKZ 20 S"]
[null,72633,"Quick-response heater CKR 20 S",136,"",null,null,null,null,null,null,72633,"Quick-response heater CKR 20 S",136,false,null,72633,189,136,240,"på forespørgsel",212,"Schnellheizer CKR 20 S","Quick-response heater CKR 20 S","Quick-response heater CKR 20 S","Quick-response heater CKR 20 S","Convector CKR 20 S","Quick-response heater CKR 20 S","Quick-response heater CKR 20 S","Quick-response heater CKR 20 S","Quick-response heater CKR 20 S","Quick-response heater CKR 20 S","Quick-response heater CKR 20 S"]
[null,230344,"Quick-response heater CKT 20 S",146,"",null,null,null,null,null,null,230344,"Quick-response heater CKT 20 S",146,false,null,230344,174,146,"sur demande","på forespørgsel",209,"Schnellheizer CKT 20 S","Quick-response heater CKT 20 S","Quick-response heater CKT 20 S","Quick-response heater CKT 20 S","Convector CKT 20 S","Quick-response heater CKT 20 S","Quick-response heater CKT 20 S","Quick-response heater CKT 20 S","Quick-response heater CKT 20 S","Quick-response heater CKT 20 S","Quick-response heater CKT 20 S"]
[null,185274,"Quick-response heater CBS 20 S",79,"",null,null,null,null,null,null,185274,"Quick-response heater CBS 20 S",79,false,null,185274,89,79,145,"på forespørgsel",89,"Schnellheizer CBS 20 S","Quick-response heater CBS 20 S","Quick-response heater CBS 20 S","Quick-response heater CBS 20 S","Snelverwarmer CBS 20 S","Quick-response heater CBS 20 S","Quick-response heater CBS 20 S","Quick-response heater CBS 20 S","Quick-response heater CBS 20 S","Quick-response heater CBS 20 S","Quick-response heater CBS 20 S"]
[null,73685,"Small frost protection heater CFK 5",37,"",null,null,null,null,null,null,73685,"Small frost protection heater CFK 5",37,false,null,73685,54,37,"sur demande","på forespørgsel",54,"Frostschutz-Kleinheizgerät CFK 5","Small frost protection heater CFK 5","Small frost protection heater CFK 5","Small frost protection heater CFK 5","Vorstbeschermer CFK 5","Small frost protection heater CFK 5","Small frost protection heater CFK 5","Small frost protection heater CFK 5","Small frost protection heater CFK 5","Small frost protection heater CFK 5","Small frost protection heater CFK 5"]
[null,229339,"IR quartz heater IW 120",43,"",null,null,null,null,null,null,229339,"IR quartz heater IW 120",43,false,null,229339,71,43,"sur demande","på forespørgsel",69,"Infrarot-Quarzstrahler IW 120","IR quartz heater IW 120","IR quartz heater IW 120","IR quartz heater IW 120","Infrarood-straler IW 120","IR quartz heater IW 120","IR quartz heater IW 120","IR quartz heater IW 120","IR quartz heater IW 120","IR quartz heater IW 120","IR quartz heater IW 120"]
[null,229340,"IR quartz heater IW 180",43,"",null,null,null,null,null,null,229340,"IR quartz heater IW 180",43,false,null,229340,79,43,"sur demande","på forespørgsel",75,"Infrarot-Quarzstrahler IW 180","IR quartz heater IW 180","IR quartz heater IW 180","IR quartz heater IW 180","Infrarood-straler IW 180","IR quartz heater IW 180","IR quartz heater IW 180","IR quartz heater IW 180","IR quartz heater IW 180","IR quartz heater IW 180","IR quartz heater IW 180"]
[null,240587,"Calculation heat demand building","On request","",null,null,null,null,null,null,240587,"Calculation heat demand building","On request",false,null,240587,189,"On request","sur demande","på forespørgsel","op aanvraag","Heizlastberechnung Einfamilienhaus","Calculation heat demand building","Calcul de la charge calorifique selon DIN 12831","Calculation heat demand building","Warmteverliesberekening woning","Calculation heat demand building","Calculation heat demand building","Calculation heat demand building","Calculation heat demand building","Calculation heat demand building","Calculation heat demand building"]
[null,303540,"Heizlastberechnung Mehrfamilienhaus","On request","",null,null,null,null,null,null,303540,"Heizlastberechnung Mehrfamilienhaus","On request",false,null,303540,349,"On request","sur demande","på forespørgsel","op aanvraag","Heizlastberechnung Mehrfamilienhaus","Heizlastberechnung Mehrfamilienhaus","Heizlastberechnung Mehrfamilienhaus","Heizlastberechnung Mehrfamilienhaus","Warmteverliesberekening appartementen complex","Heizlastberechnung Mehrfamilienhaus","Heizlastberechnung Mehrfamilienhaus","Heizlastberechnung Mehrfamilienhaus","Heizlastberechnung Mehrfamilienhaus","Heizlastberechnung Mehrfamilienhaus","Heizlastberechnung Mehrfamilienhaus"]
[null,303541,"Heizlastberechnung Nichtwohngebäude","On request","",null,null,null,null,null,null,303541,"Heizlastberechnung Nichtwohngebäude","On request",false,null,303541,340,"On request","sur demande","på forespørgsel","op aanvraag","Heizlastberechnung Nichtwohngebäude","Heizlastberechnung Nichtwohngebäude","Heizlastberechnung Nichtwohngebäude","Heizlastberechnung Nichtwohngebäude","Warmteverliesberekening utiliteit","Heizlastberechnung Nichtwohngebäude","Heizlastberechnung Nichtwohngebäude","Heizlastberechnung Nichtwohngebäude","Heizlastberechnung Nichtwohngebäude","Heizlastberechnung Nichtwohngebäude","Heizlastberechnung Nichtwohngebäude"]
[null,240588,"Engineering heat pump system","On request","",null,null,null,null,null,null,240588,"Engineering heat pump system","On request",false,null,240588,360,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Wärmepumpe Wohngebäude","Engineering heat pump system","Engineering heat pump system","Engineering heat pump system","Planningsberekening warmtepomp woning","Engineering heat pump system","Engineering heat pump system","Engineering heat pump system","Engineering heat pump system","Engineering heat pump system","Engineering heat pump system"]
[null,303542,"Planungsleistung Wärmepumpe Nichtwohngebäude","On request","",null,null,null,null,null,null,303542,"Planungsleistung Wärmepumpe Nichtwohngebäude","On request",false,null,303542,900,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Wärmepumpe Nichtwohngebäude","Planungsleistung Wärmepumpe Nichtwohngebäude","Planungsleistung Wärmepumpe Nichtwohngebäude","Planungsleistung Wärmepumpe Nichtwohngebäude","Planningsberekening warmtepomp utiliteit","Planungsleistung Wärmepumpe Nichtwohngebäude","Planungsleistung Wärmepumpe Nichtwohngebäude","Planungsleistung Wärmepumpe Nichtwohngebäude","Planungsleistung Wärmepumpe Nichtwohngebäude","Planungsleistung Wärmepumpe Nichtwohngebäude","Planungsleistung Wärmepumpe Nichtwohngebäude"]
[null,313466,"Planungsleistung Wärmepumpe Direktverdampfer","On request","",null,null,null,null,null,null,313466,"Planungsleistung Wärmepumpe Direktverdampfer","On request",false,null,313466,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Wärmepumpe Direktverdampfer","Planungsleistung Wärmepumpe Direktverdampfer","Planungsleistung Wärmepumpe Direktverdampfer","Planungsleistung Wärmepumpe Direktverdampfer","Planningsberekening warmtepomp directverdamper","Planungsleistung Wärmepumpe Direktverdampfer","Planungsleistung Wärmepumpe Direktverdampfer","Planungsleistung Wärmepumpe Direktverdampfer","Planungsleistung Wärmepumpe Direktverdampfer","Planungsleistung Wärmepumpe Direktverdampfer","Planungsleistung Wärmepumpe Direktverdampfer"]
[null,303543,"Planungsleistung Schaltschrankbau/Leittechnik","On request","",null,null,null,null,null,null,303543,"Planungsleistung Schaltschrankbau/Leittechnik","On request",false,null,303543,950,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Schaltschrankbau/Leittechnik","Planungsleistung Schaltschrankbau/Leittechnik","Planungsleistung Schaltschrankbau/Leittechnik","Planungsleistung Schaltschrankbau/Leittechnik","Planningsberekening schakelkasten/kabeltechniek","Planungsleistung Schaltschrankbau/Leittechnik","Planungsleistung Schaltschrankbau/Leittechnik","Planungsleistung Schaltschrankbau/Leittechnik","Planungsleistung Schaltschrankbau/Leittechnik","Planungsleistung Schaltschrankbau/Leittechnik","Planungsleistung Schaltschrankbau/Leittechnik"]
[null,240592,"Engineering air ventilation system","On request","",null,null,null,null,null,null,240592,"Engineering air ventilation system","On request",false,null,240592,360,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Lüftungstechnik","Engineering air ventilation system","Études de ventilation","Engineering air ventilation system","Planningsberekening ventilatie","Engineering air ventilation system","Engineering air ventilation system","Engineering air ventilation system","Engineering air ventilation system","Engineering air ventilation system","Engineering air ventilation system"]
[null,240590,"Engineering air conditioning system","On request","",null,null,null,null,null,null,240590,"Engineering air conditioning system","On request",false,null,240590,210,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Klimatechnik","Engineering air conditioning system","Engineering air conditioning system","Engineering air conditioning system","Planningsberekening airconditioning","Engineering air conditioning system","Engineering air conditioning system","Engineering air conditioning system","Engineering air conditioning system","Engineering air conditioning system","Engineering air conditioning system"]
[null,240591,"Engineering solar system","On request","",null,null,null,null,null,null,240591,"Engineering solar system","On request",false,null,240591,215,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Solartechnik und Photovoltaik","Engineering solar system","Solaire - performances","Solar-Planungsleistung","Planningsberekening Solartechniek en PV techniek","Solar-Planungsleistung","Solar-Planungsleistung","Solar-Planungsleistung","Solar-Planungsleistung","Solar-Planungsleistung","Engineering solar system"]
[null,303544,"Planung Trinkwassersystem bis 20 Wohneinheiten","On request","",null,null,null,null,null,null,303544,"Planung Trinkwassersystem bis 20 Wohneinheiten","On request",false,null,303544,360,"On request","sur demande","på forespørgsel","op aanvraag","Planung Trinkwassersystem bis 20 Wohneinheiten","Planung Trinkwassersystem bis 20 Wohneinheiten","Planung Trinkwassersystem bis 20 Wohneinheiten","Planung Trinkwassersystem bis 20 Wohneinheiten","Planning drinkwatersysteem tot 20 wooneenheden","Planung Trinkwassersystem bis 20 Wohneinheiten","Planung Trinkwassersystem bis 20 Wohneinheiten","Planung Trinkwassersystem bis 20 Wohneinheiten","Planung Trinkwassersystem bis 20 Wohneinheiten","Planung Trinkwassersystem bis 20 Wohneinheiten","Planung Trinkwassersystem bis 20 Wohneinheiten"]
[null,303545,"Planung Trinkwassersystem größer 20 Wohneinheiten","On request","",null,null,null,null,null,null,303545,"Planung Trinkwassersystem größer 20 Wohneinheiten","On request",false,null,303545,900,"On request","sur demande","på forespørgsel","op aanvraag","Planung Trinkwassersystem größer 20 Wohneinheiten","Planung Trinkwassersystem größer 20 Wohneinheiten","Planung Trinkwassersystem größer 20 Wohneinheiten","Planung Trinkwassersystem größer 20 Wohneinheiten","Planning drinkwatersysteem groter dan 20 wooneenheden","Planung Trinkwassersystem größer 20 Wohneinheiten","Planung Trinkwassersystem größer 20 Wohneinheiten","Planung Trinkwassersystem größer 20 Wohneinheiten","Planung Trinkwassersystem größer 20 Wohneinheiten","Planung Trinkwassersystem größer 20 Wohneinheiten","Planung Trinkwassersystem größer 20 Wohneinheiten"]
[null,303546,"Planungsleistung Wirtschaftlichkeitsbetrachtung","On request","",null,null,null,null,null,null,303546,"Planungsleistung Wirtschaftlichkeitsbetrachtung","On request",false,null,303546,210,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planningsberekening rendabiliteit","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planungsleistung Wirtschaftlichkeitsbetrachtung","Planungsleistung Wirtschaftlichkeitsbetrachtung"]
[null,303547,"Planungsleistung Erstellung Energieausweis","On request","",null,null,null,null,null,null,303547,"Planungsleistung Erstellung Energieausweis","On request",false,null,303547,110,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Erstellung Energieausweis","Planungsleistung Erstellung Energieausweis","Planungsleistung Erstellung Energieausweis","Planungsleistung Erstellung Energieausweis","Planningsberekening creëren energie-certificaat","Planungsleistung Erstellung Energieausweis","Planungsleistung Erstellung Energieausweis","Planungsleistung Erstellung Energieausweis","Planungsleistung Erstellung Energieausweis","Planungsleistung Erstellung Energieausweis","Planungsleistung Erstellung Energieausweis"]
[null,283722,"Commissioning heat pump","On request","",null,null,null,null,null,null,283722,"Commissioning heat pump","On request",false,null,283722,405,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Wärmepumpen nur Hzg/WWB","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump","Ingebruikname Warmtepomp","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump"]
[null,294381,"Inbetriebnahme Wärmepumpe nach Estrichaufheizung","On request","",null,null,null,null,null,null,294381,"Inbetriebnahme Wärmepumpe nach Estrichaufheizung","On request",false,null,294381,225,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Ingebruikname warmtepomp na opwarmprogramma","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung"]
[null,286777,"Commissioning heat pump","On request","",null,null,null,null,null,null,286777,"Commissioning heat pump","On request",false,null,286777,520,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme WPL 34...57, WPF 20...66","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump","Ingebruikname WPL 34...57, WPF 20...66","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump","Commissioning heat pump"]
[null,283724,"Commissioning heat pump - additional module","On request","",null,null,null,null,null,null,283724,"Commissioning heat pump - additional module","On request",false,null,283724,135,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme zusätzliches WP-Modul","Commissioning heat pump - additional module","Commissioning heat pump - additional module","Commissioning heat pump - additional module","Ingebruikname extra Warmtepomp-Module","Commissioning heat pump - additional module","Commissioning heat pump - additional module","Commissioning heat pump - additional module","Commissioning heat pump - additional module","Commissioning heat pump - additional module","Commissioning heat pump - additional module"]
[null,283725,"Commissioning LWM 250","On request","",null,null,null,null,null,null,283725,"Commissioning LWM 250","On request",false,null,283725,188,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme LWM 250","Commissioning LWM 250","Mise en service LWM 250","Commissioning LWM 250","Ingebruikname LWM 250","Commissioning LWM 250","Commissioning LWM 250","Commissioning LWM 250","Commissioning LWM 250","Commissioning LWM 250","Commissioning LWM 250"]
[null,293133,"Inbetriebnahme Kühlfunktion Wärmepumpe","On request","",null,null,null,null,null,null,293133,"Inbetriebnahme Kühlfunktion Wärmepumpe","On request",false,null,293133,90,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Ingebruikname Cool-functie","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe"]
[null,293134,"Inbetriebnahme Solarfunktion Wärmepumpe","On request","",null,null,null,null,null,null,293134,"Inbetriebnahme Solarfunktion Wärmepumpe","On request",false,null,293134,116,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Ingebruikname Solar-functie","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe"]
[null,287082,"Commissioning heat pump split lines","On request","",null,null,null,null,null,null,287082,"Commissioning heat pump split lines","On request",false,null,287082,350,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Splitleitungen Wärmepumpe","Commissioning heat pump split lines","Commissioning heat pump split lines","Commissioning heat pump split lines","Ingebruikname Warmtepompen splitleidingen","Commissioning heat pump split lines","Commissioning heat pump split lines","Commissioning heat pump split lines","Commissioning heat pump split lines","Commissioning heat pump split lines","Commissioning heat pump split lines"]
[null,313465,"Inbetriebnahme Wärmepumpe Direktverdampfer","On request","",null,null,null,null,null,null,313465,"Inbetriebnahme Wärmepumpe Direktverdampfer","On request",false,null,313465,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbedrijfname Warmtepomp Directverdamper","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbetriebnahme Wärmepumpe Direktverdampfer","Inbetriebnahme Wärmepumpe Direktverdampfer"]
[null,283723,"Commissioning LWZ 303/403 SOL","On request","",null,null,null,null,null,null,283723,"Commissioning LWZ 303/403 SOL","On request",false,null,283723,440,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme LWZ 303/304/403/404 SOL","Commissioning LWZ 303/403 SOL","Mise en service LWZ 303/403 SOL","Commissioning LWZ 303/403 SOL","Ingebruikname LWZ 303/403 SOL","Commissioning LWZ 303/403 SOL","Commissioning LWZ 303/403 SOL","Commissioning LWZ 303/403 SOL","Commissioning LWZ 303/403 SOL","Commissioning LWZ 303/403 SOL","Commissioning LWZ 303/403 SOL"]
[null,294381,"Inbetriebnahme Wärmepumpe nach Estrichaufheizung","On request","",null,null,null,null,null,null,294381,"Inbetriebnahme Wärmepumpe nach Estrichaufheizung","On request",false,null,294381,225,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Ingebruikname warmtepomp na opwarmprogramma","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung","Inbetriebnahme Wärmepumpe nach Estrichaufheizung"]
[null,283731,"Commissioning LWZ 100/LWZ 70","On request","",null,null,null,null,null,null,283731,"Commissioning LWZ 100/LWZ 70","On request",false,null,283731,260,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme LWZ 100/LWZ 70","Commissioning LWZ 100/LWZ 70","Mise en service LWZ 100 LWZ 70","Commissioning LWZ 100/LWZ 70","Ingebruikname LWZ 100/LWZ 70","Commissioning LWZ 100/LWZ 70","Commissioning LWZ 100/LWZ 70","Commissioning LWZ 100/LWZ 70","Commissioning LWZ 100/LWZ 70","Commissioning LWZ 100/LWZ 70","Commissioning LWZ 100/LWZ 70"]
[null,283728,"Commissioning LWA 252 SOL","On request","",null,null,null,null,null,null,283728,"Commissioning LWA 252 SOL","On request",false,null,283728,355,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme LWZ 170/270/370 Plus","Commissioning LWA 252 SOL","Mise en service LWA 252 SOL","Commissioning LWA 252 SOL","Ingebruikname LWA 252 SOL/WM300","Commissioning LWA 252 SOL","Commissioning LWA 252 SOL","Commissioning LWA 252 SOL","Commissioning LWA 252 SOL","Commissioning LWA 252 SOL","Commissioning LWA 252 SOL"]
[null,303646,"Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","On request","",null,null,null,null,null,null,303646,"Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","On request",false,null,303646,20,"On request","sur demande","på forespørgsel","op aanvraag","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","IJken aanvoer-/afvoer ventielen (bij overige systemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)","Einmessen Zuluft-/Abluftventil (bei Fremdsystemen)"]
[null,293133,"Inbetriebnahme Kühlfunktion Wärmepumpe","On request","",null,null,null,null,null,null,293133,"Inbetriebnahme Kühlfunktion Wärmepumpe","On request",false,null,293133,90,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Ingebruikname Cool-functie","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe","Inbetriebnahme Kühlfunktion Wärmepumpe"]
[null,293134,"Inbetriebnahme Solarfunktion Wärmepumpe","On request","",null,null,null,null,null,null,293134,"Inbetriebnahme Solarfunktion Wärmepumpe","On request",false,null,293134,116,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Ingebruikname Solar-functie","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe","Inbetriebnahme Solarfunktion Wärmepumpe"]
[null,283743,"Commissioning additional indoor unit","On request","",null,null,null,null,null,null,283743,"Commissioning additional indoor unit","On request",false,null,283743,69,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Klimaanlage Innengerät","Commissioning additional indoor unit","Commissioning additional indoor unit","Commissioning additional indoor unit","Ingebruikname extra binnenopstelling","Commissioning additional indoor unit","Commissioning additional indoor unit","Commissioning additional indoor unit","Commissioning additional indoor unit","Commissioning additional indoor unit","Commissioning additional indoor unit"]
[null,285129,"Leak test air conditioning system","On request","",null,null,null,null,null,null,285129,"Leak test air conditioning system","On request",false,null,285129,198,"On request","sur demande","på forespørgsel","op aanvraag","Dichtheitsprüfung Klimaanlage","Leak test air conditioning system","Leak test air conditioning system","Leak test air conditioning system","Dichtheidscontrolle airco installatie","Leak test air conditioning system","Leak test air conditioning system","Leak test air conditioning system","Leak test air conditioning system","Leak test air conditioning system","Leak test air conditioning system"]
[null,283733,"Commissioning solar system","On request","",null,null,null,null,null,null,283733,"Commissioning solar system","On request",false,null,283733,260,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Solaranlage","Commissioning solar system","Mise en service solaire","Inbetriebnahme Solar","Ingebruikname Solar i.c.m warmtepomp","Inbetriebnahme Solar","Inbetriebnahme Solar","Inbetriebnahme Solar","Inbetriebnahme Solar","Inbetriebnahme Solar","Commissioning solar system"]
[null,296190,"Inbetriebnahme Data Station Gebäudeleittechnik","On request","",null,null,null,null,null,null,296190,"Inbetriebnahme Data Station Gebäudeleittechnik","On request",false,null,296190,990,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Data Station Gebäudeleittechnik","Inbetriebnahme Data Station Gebäudeleittechnik","Inbetriebnahme Data Station Gebäudeleittechnik","Inbetriebnahme Data Station Gebäudeleittechnik","Ingebruikname Data Station (Gebouwbeheersysteem)","Inbetriebnahme Data Station Gebäudeleittechnik","Inbetriebnahme Data Station Gebäudeleittechnik","Inbetriebnahme Data Station Gebäudeleittechnik","Inbetriebnahme Data Station Gebäudeleittechnik","Inbetriebnahme Data Station Gebäudeleittechnik","Inbetriebnahme Data Station Gebäudeleittechnik"]
[null,298662,"Inbetriebnahme ISG web","On request","",null,null,null,null,null,null,298662,"Inbetriebnahme ISG web","On request",false,null,298662,100,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme ISG web","Inbetriebnahme ISG web","Inbetriebnahme ISG web","Inbetriebnahme ISG web","Ingebruikname ISG web","Inbetriebnahme ISG web","Inbetriebnahme ISG web","Inbetriebnahme ISG web","Inbetriebnahme ISG web","Inbetriebnahme ISG web","Inbetriebnahme ISG web"]
[null,297848,"ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","On request","",null,null,null,null,null,null,297848,"ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","On request",false,null,297848,0,"On request","sur demande","på forespørgsel","op aanvraag","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Gebruiksduur 3 Jaar)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)","ISG Servicewelt Basis (Nutzungsdauer 3 Jahre)"]
[null,297849,"ISG Servicewelt Plus (Jahresbeitrag)","On request","",null,null,null,null,null,null,297849,"ISG Servicewelt Plus (Jahresbeitrag)","On request",false,null,297849,49,"On request","sur demande","på forespørgsel","op aanvraag","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jaarbijdrage)","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jahresbeitrag)","ISG Servicewelt Plus (Jahresbeitrag)"]
[null,233303,"Softwareerweiterung KNX IP für ISG web","On request","",null,null,null,null,null,null,233303,"Softwareerweiterung KNX IP für ISG web","On request",false,null,233303,331.93,"On request","sur demande","på forespørgsel","op aanvraag","Softwareerweiterung KNX IP für ISG web","Softwareerweiterung KNX IP für ISG web","Softwareerweiterung KNX IP für ISG web","Softwareerweiterung KNX IP für ISG web","Software KNX","Softwareerweiterung KNX IP für ISG web","Softwareerweiterung KNX IP für ISG web","Softwareerweiterung KNX IP für ISG web","Softwareerweiterung KNX IP für ISG web","Softwareerweiterung KNX IP für ISG web","Softwareerweiterung KNX IP für ISG web"]
[null,233236,"Softwareerweiterung EMI für ISG web","On request","",null,null,null,null,null,null,233236,"Softwareerweiterung EMI für ISG web","On request",false,null,233236,67.900000000000006,"On request","sur demande","på forespørgsel","op aanvraag","Softwareerweiterung EMI für ISG web","Softwareerweiterung EMI für ISG web","Softwareerweiterung EMI für ISG web","Softwareerweiterung EMI für ISG web","Software Energy Management Interface EMI","Softwareerweiterung EMI für ISG web","Softwareerweiterung EMI für ISG web","Softwareerweiterung EMI für ISG web","Softwareerweiterung EMI für ISG web","Softwareerweiterung EMI für ISG web","Softwareerweiterung EMI für ISG web"]
[null,267225,"Vermietung Elektroheizmobil MH 20.2","On request","",null,null,null,null,null,null,267225,"Vermietung Elektroheizmobil MH 20.2","On request",false,null,267225,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Vermietung Elektroheizmobil MH 20.2","Vermietung Elektroheizmobil MH 20.2","Vermietung Elektroheizmobil MH 20.2","Vermietung Elektroheizmobil MH 20.2","Verhuur Elektroverwarmingsunit MH 20.2","Vermietung Elektroheizmobil MH 20.2","Vermietung Elektroheizmobil MH 20.2","Vermietung Elektroheizmobil MH 20.2","Vermietung Elektroheizmobil MH 20.2","Vermietung Elektroheizmobil MH 20.2","Vermietung Elektroheizmobil MH 20.2"]
[null,313393,"Verkauf Elektroheizmobil MH 19.2","On request","",null,null,null,null,null,null,313393,"Verkauf Elektroheizmobil MH 19.2","On request",false,null,313393,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Verkauf Elektroheizmobil MH 19.2","Verkauf Elektroheizmobil MH 19.2","Verkauf Elektroheizmobil MH 19.2","Verkauf Elektroheizmobil MH 19.2","Verkoop Elektroverwarmingsunit MH 19.2","Verkauf Elektroheizmobil MH 19.2","Verkauf Elektroheizmobil MH 19.2","Verkauf Elektroheizmobil MH 19.2","Verkauf Elektroheizmobil MH 19.2","Verkauf Elektroheizmobil MH 19.2","Verkauf Elektroheizmobil MH 19.2"]
[null,313394,"Verkauf Elektroheizmobil MH 20.2","On request","",null,null,null,null,null,null,313394,"Verkauf Elektroheizmobil MH 20.2","On request",false,null,313394,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Verkauf Elektroheizmobil MH 20.2","Verkauf Elektroheizmobil MH 20.2","Verkauf Elektroheizmobil MH 20.2","Verkauf Elektroheizmobil MH 20.2","Verkoop Elektroverwarmingsunit MH 20.2","Verkauf Elektroheizmobil MH 20.2","Verkauf Elektroheizmobil MH 20.2","Verkauf Elektroheizmobil MH 20.2","Verkauf Elektroheizmobil MH 20.2","Verkauf Elektroheizmobil MH 20.2","Verkauf Elektroheizmobil MH 20.2"]
[null,233871,"Luft|Wasser-Wärmepumpe WPL 08 S Trend","On request",null,null,null,null,null,null,null,233871,"Luft|Wasser-Wärmepumpe WPL 08 S Trend","On request",false,null,233871,"auf Anfrage","On request","N.C","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 08 S Trend","Luft|Wasser-Wärmepumpe WPL 08 S Trend","Luft|Wasser-Wärmepumpe WPL 08 S Trend","Luft|Wasser-Wärmepumpe WPL 08 S Trend","Lucht/water-warmtepompen WPL 08 S Trend"]
[null,233872,"Luft|Wasser-Wärmepumpe WPL 12 S Trend","On request",null,null,null,null,null,null,null,233872,"Luft|Wasser-Wärmepumpe WPL 12 S Trend","On request",false,null,233872,"auf Anfrage","On request","N.C","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 12 S Trend","Luft|Wasser-Wärmepumpe WPL 12 S Trend","Luft|Wasser-Wärmepumpe WPL 12 S Trend","Luft|Wasser-Wärmepumpe WPL 12 S Trend","Lucht/water-warmtepompen WPL 12 S Trend"]
[null,233873,"Luft|Wasser-Wärmepumpe WPL 16 S Trend","On request",null,null,null,null,null,null,null,233873,"Luft|Wasser-Wärmepumpe WPL 16 S Trend","On request",false,null,233873,"auf Anfrage","On request","N.C","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 16 S Trend","Luft|Wasser-Wärmepumpe WPL 16 S Trend","Luft|Wasser-Wärmepumpe WPL 16 S Trend","Luft|Wasser-Wärmepumpe WPL 16 S Trend","Lucht/water-warmtepompen WPL 16 S Trend"]
[null,233876,"Luft|Wasser-Wärmepumpe WPL 22 Trend","On request",null,null,null,null,null,null,null,233876,"Luft|Wasser-Wärmepumpe WPL 22 Trend","On request",false,null,233876,"auf Anfrage","On request","N.C","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 22 Trend","Luft|Wasser-Wärmepumpe WPL 22 Trend","Luft|Wasser-Wärmepumpe WPL 22 Trend","Luft|Wasser-Wärmepumpe WPL 22 Trend","Lucht/water-warmtepompen WPL 22 Trend"]
[null,233877,"Luft|Wasser-Wärmepumpe WPL 28 Trend","On request",null,null,null,null,null,null,null,233877,"Luft|Wasser-Wärmepumpe WPL 28 Trend","On request",false,null,233877,"auf Anfrage","On request","N.C","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 28 Trend","Luft|Wasser-Wärmepumpe WPL 28 Trend","Luft|Wasser-Wärmepumpe WPL 28 Trend","Luft|Wasser-Wärmepumpe WPL 28 Trend","Lucht/water-warmtepompen WPL 28 Trend"]
[null,233878,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 1","On request",null,null,null,null,null,null,null,233878,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 1","On request",false,null,233878,8300,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 1","Lucht/water-warmtepompen WPL 08 S Trend Set 1"]
[null,233879,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 1","On request",null,null,null,null,null,null,null,233879,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 1","On request",false,null,233879,8990,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 1","Lucht/water-warmtepompen WPL 12 S Trend Set 1"]
[null,233880,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 1","On request",null,null,null,null,null,null,null,233880,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 1","On request",false,null,233880,10250,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 1","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 1","Lucht/water-warmtepompen WPL 16 S Trend Set 1"]
[null,233883,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 1","On request",null,null,null,null,null,null,null,233883,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 1","On request",false,null,233883,12200,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 1","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 1","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 1","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 1","Lucht/water-warmtepompen WPL 22 Trend Set 1"]
[null,233884,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 1","On request",null,null,null,null,null,null,null,233884,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 1","On request",false,null,233884,14150,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 1","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 1","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 1","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 1","Lucht/water-warmtepompen WPL 28 Trend Set 1"]
[null,233885,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 2","On request",null,null,null,null,null,null,null,233885,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 2","On request",false,null,233885,9500,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 2","Lucht/water-warmtepompen WPL 08 S Trend Set 2"]
[null,233886,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 2","On request",null,null,null,null,null,null,null,233886,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 2","On request",false,null,233886,10190,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 2","Lucht/water-warmtepompen WPL 12 S Trend Set 2"]
[null,233887,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 2","On request",null,null,null,null,null,null,null,233887,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 2","On request",{"$f":"IF(AND(B1321=L1321,C1321=M1321,D1321=N1321),FALSE,TRUE)","v":false},null,233887,11850,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 2","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 2","Lucht/water-warmtepompen WPL 16 S Trend Set 2"]
[null,233890,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 2","On request",null,null,null,null,null,null,null,233890,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 2","On request",false,null,233890,13800,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 2","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 2","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 2","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 2","Lucht/water-warmtepompen WPL 22 Trend Set 2"]
[null,233891,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 2","On request",null,null,null,null,null,null,null,233891,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 2","On request",false,null,233891,15750,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 2","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 2","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 2","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 2","Lucht/water-warmtepompen WPL 28 Trend Set 2"]
[null,234729,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 3","On request",null,null,null,null,null,null,null,234729,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 3","On request",false,null,234729,10500,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 3","Lucht/water-warmtepompen WPL 08 S Trend Set 3"]
[null,234730,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 3","On request",null,null,null,null,null,null,null,234730,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 3","On request",false,null,234730,11190,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 3","Lucht/water-warmtepompen WPL 12 S Trend Set 3"]
[null,234731,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 3","On request",null,null,null,null,null,null,null,234731,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 3","On request",false,null,234731,12850,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 3","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 3","Lucht/water-warmtepompen WPL 16 S Trend Set 3"]
[null,234733,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 3","On request",null,null,null,null,null,null,null,234733,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 3","On request",false,null,234733,14800,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 3","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 3","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 3","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 3","Lucht/water-warmtepompen WPL 22 Trend Set 3"]
[null,234734,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 3","On request",null,null,null,null,null,null,null,234734,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 3","On request",false,null,234734,16750,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 3","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 3","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 3","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 3","Lucht/water-warmtepompen WPL 28 Trend Set 3"]
[null,234735,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 4","On request",null,null,null,null,null,null,null,234735,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 4","On request",false,null,234735,9700,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 4","Lucht/water-warmtepompen WPL 08 S Trend Set 4"]
[null,234736,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 4","On request",null,null,null,null,null,null,null,234736,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 4","On request",false,null,234736,10390,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 4","Lucht/water-warmtepompen WPL 12 S Trend Set 4"]
[null,234737,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 4","On request",null,null,null,null,null,null,null,234737,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 4","On request",false,null,234737,11850,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 4","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 4","Lucht/water-warmtepompen WPL 16 S Trend Set 4"]
[null,234739,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 4","On request",null,null,null,null,null,null,null,234739,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 4","On request",false,null,234739,13800,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 4","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 4","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 4","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 4","Lucht/water-warmtepompen WPL 22 Trend Set 4"]
[null,234740,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 4","On request",null,null,null,null,null,null,null,234740,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 4","On request",false,null,234740,15750,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 4","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 4","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 4","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 4","Lucht/water-warmtepompen WPL 28 Trend Set 4"]
[null,234741,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 5","On request",null,null,null,null,null,null,null,234741,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 5","On request",false,null,234741,10100,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 5","Lucht/water-warmtepompen WPL 08 S Trend Set 5"]
[null,234742,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 5","On request",null,null,null,null,null,null,null,234742,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 5","On request",false,null,234742,10790,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 5","Lucht/water-warmtepompen WPL 12 S Trend Set 5"]
[null,234743,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 5","On request",null,null,null,null,null,null,null,234743,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 5","On request",false,null,234743,12250,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 5","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 5","Lucht/water-warmtepompen WPL 16 S Trend Set 5"]
[null,234745,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 5","On request",null,null,null,null,null,null,null,234745,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 5","On request",false,null,234745,14200,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 5","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 5","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 5","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 5","Lucht/water-warmtepompen WPL 22 Trend Set 5"]
[null,234746,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 5","On request",null,null,null,null,null,null,null,234746,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 5","On request",false,null,234746,16150,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 5","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 5","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 5","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 5","Lucht/water-warmtepompen WPL 28 Trend Set 5"]
[null,234747,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 6","On request",null,null,null,null,null,null,null,234747,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 6","On request",false,null,234747,11100,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 6","Lucht/water-warmtepompen WPL 08 S Trend Set 6"]
[null,234748,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 6","On request",null,null,null,null,null,null,null,234748,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 6","On request",false,null,234748,11790,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 6","Lucht/water-warmtepompen WPL 12 S Trend Set 6"]
[null,234749,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 6","On request",null,null,null,null,null,null,null,234749,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 6","On request",false,null,234749,13250,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 6","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 6","Lucht/water-warmtepompen WPL 16 S Trend Set 6"]
[null,234751,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 6","On request",null,null,null,null,null,null,null,234751,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 6","On request",false,null,234751,15200,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 6","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 6","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 6","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 6","Lucht/water-warmtepompen WPL 22 Trend Set 6"]
[null,234752,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 6","On request",null,null,null,null,null,null,null,234752,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 6","On request",false,null,234752,17150,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 6","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 6","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 6","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 6","Lucht/water-warmtepompen WPL 28 Trend Set 6"]
[null,234753,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 7","On request",null,null,null,null,null,null,null,234753,"Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 7","On request",false,null,234753,12300,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 08 S Trend Set 7","Lucht/water-warmtepompen WPL 08 S Trend Set 7"]
[null,234754,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 7","On request",null,null,null,null,null,null,null,234754,"Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 7","On request",false,null,234754,12990,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 12 S Trend Set 7","Lucht/water-warmtepompen WPL 12 S Trend Set 7"]
[null,234755,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 7","On request",null,null,null,null,null,null,null,234755,"Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 7","On request",false,null,234755,14450,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 7","Luft|Wasser-Wärmepumpe WPL 16 S Trend Set 7","Lucht/water-warmtepompen WPL 16 S Trend Set 7"]
[null,234757,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 7","On request",null,null,null,null,null,null,null,234757,"Luft|Wasser-Wärmepumpe WPL 22 Trend Set 7","On request",false,null,234757,16400,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 7","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 7","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 7","Luft|Wasser-Wärmepumpe WPL 22 Trend Set 7","Lucht/water-warmtepompen WPL 22 Trend Set 7"]
[null,234758,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 7","On request",null,null,null,null,null,null,null,234758,"Luft|Wasser-Wärmepumpe WPL 28 Trend Set 7","On request",false,null,234758,18350,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 7","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 7","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 7","Luft|Wasser-Wärmepumpe WPL 28 Trend Set 7","Lucht/water-warmtepompen WPL 28 Trend Set 7"]
[null,233510,"Integral-Speicher HSBC 200","On request",null,null,null,null,null,null,null,233510,"Integral-Speicher HSBC 200","On request",false,null,233510,3695,"On request","5.390,00","på forespørgsel",3695,"Integral-Speicher HSBC 200","Integral-Speicher HSBC 200","Integral-Speicher HSBC 200","Integral-Speicher HSBC 200","Integral-Speicher HSBC 200"]
[null,234648,"Pumpenbaugruppe Mischerkreis für HSBC 200","On request",null,null,null,null,null,null,null,234648,"Pumpenbaugruppe Mischerkreis für HSBC 200","On request",false,null,234648,495,"On request",695,"på forespørgsel",495,"Pumpenbaugruppe Mischerkreis für HSBC 200","Pumpenbaugruppe Mischerkreis für HSBC 200","Pumpenbaugruppe Mischerkreis für HSBC 200","Pumpenbaugruppe Mischerkreis für HSBC 200","Pumpenbaugruppe Mischerkreis für HSBC 200"]
[null,234646,"Wärmegedämmter Luftschlauch DN 315, 4m","On request",null,null,null,null,null,null,null,234646,"Wärmegedämmter Luftschlauch DN 315, 4m","On request",false,null,234646,240,"On request",180,"på forespørgsel",240,"Wärmegedämmter Luftschlauch DN 315, 4m","Wärmegedämmter Luftschlauch DN 315, 4m","Wärmegedämmter Luftschlauch DN 315, 4m","Wärmegedämmter Luftschlauch DN 315, 4m","Wärmegedämmter Luftschlauch DN 315, 4m"]
[null,234647,"Wärmegedämmter Luftschlauch DN 560, 4 m","On request",null,null,null,null,null,null,null,234647,"Wärmegedämmter Luftschlauch DN 560, 4 m","On request",false,null,234647,445,"On request",435,"på forespørgsel",445,"Wärmegedämmter Luftschlauch DN 560, 4 m","Wärmegedämmter Luftschlauch DN 560, 4 m","Wärmegedämmter Luftschlauch DN 560, 4 m","Wärmegedämmter Luftschlauch DN 560, 4 m","Wärmegedämmter Luftschlauch DN 560, 4 m"]
[null,234722,"Wandkonsole WPL 15/25 AC mit Heizband 2m","On request",null,null,null,null,null,null,null,234722,"Wandkonsole WPL 15/25 AC mit Heizband 2m","On request",false,null,234722,298,"On request",445,"på forespørgsel",298,"Wandkonsole WPL 15/25 AC mit Heizband 2m","Wandkonsole WPL 15/25 AC mit Heizband 2m","Wandkonsole WPL 15/25 AC mit Heizband 2m","Wandkonsole WPL 15/25 AC mit Heizband 2m","Wandkonsole WPL 15/25 AC mit Heizband 2m"]
[null,316303,"Modbus TCP/IP Software für ISG web","On request",null,null,null,null,null,null,null,316303,"Modbus TCP/IP Software für ISG web","On request",false,null,316303,290,"On request","sur demande","på forespørgsel","op aanvraag","Modbus TCP/IP Software für ISG web","Modbus TCP/IP Software für ISG web","Modbus TCP/IP Software für ISG web","Modbus TCP/IP Software für ISG web","Modbus TCP/IP Software für ISG web"]
[null,234348,"Warmwasserspeicher SBBE 301 WP","On request",null,null,null,null,null,null,null,234348,"Warmwasserspeicher SBBE 301 WP","On request",false,null,234348,1872,"On request","2.450,00","på forespørgsel",1872,"Warmwasserspeicher SBBE 301 WP","Warmwasserspeicher SBBE 301 WP","Warmwasserspeicher SBBE 301 WP","Warmwasserspeicher SBBE 301 WP","Warmwaterboiler  SBBE 301 WP"]
[null,234349,"Warmwasserspeicher SBBE 302 WP","On request",null,null,null,null,null,null,null,234349,"Warmwasserspeicher SBBE 302 WP","On request",false,null,234349,2127,"On request","2.850,00","på forespørgsel",2127,"Warmwasserspeicher SBBE 302 WP","Warmwasserspeicher SBBE 302 WP","Warmwasserspeicher SBBE 302 WP","Warmwasserspeicher SBBE 302 WP","Warmwaterboiler  SBBE 302 WP"]
[null,234350,"Warmwasserspeicher SBBE 401 WP SOL","On request",null,null,null,null,null,null,null,234350,"Warmwasserspeicher SBBE 401 WP SOL","On request",false,null,234350,2436,"On request","2.885,00","på forespørgsel",2436,"Warmwasserspeicher SBBE 401 WP SOL","Warmwasserspeicher SBBE 401 WP SOL","Warmwasserspeicher SBBE 401 WP SOL","Warmwasserspeicher SBBE 401 WP SOL","Warmwaterboiler  SBBE 401 WP SOL"]
[null,234351,"Warmwasserspeicher SBBE 501 WP SOL","On request",null,null,null,null,null,null,null,234351,"Warmwasserspeicher SBBE 501 WP SOL","On request",false,null,234351,2669,"On request","3.250,00","på forespørgsel",2669,"Warmwasserspeicher SBBE 501 WP SOL","Warmwasserspeicher SBBE 501 WP SOL","Warmwasserspeicher SBBE 501 WP SOL","Warmwasserspeicher SBBE 501 WP SOL","Warmwaterboiler  SBBE 501 WP SOL"]
[null,234515,"Rohrbausatz für Warmwasserspeicher RBS 301","On request",null,null,null,null,null,null,null,234515,"Rohrbausatz für Warmwasserspeicher RBS 301","On request",false,null,234515,287,"On request",375,"på forespørgsel",287,"Rohrbausatz für Warmwasserspeicher RBS 301","Rohrbausatz für Warmwasserspeicher RBS 301","Rohrbausatz für Warmwasserspeicher RBS 301","Rohrbausatz für Warmwasserspeicher RBS 301","Rohrbausatz für Warmwasserspeicher RBS 301"]
[null,234516,"Rohrbausatz für Warmwasserspeicher RBS 302","On request",null,null,null,null,null,null,null,234516,"Rohrbausatz für Warmwasserspeicher RBS 302","On request",false,null,234516,287,"On request",375,"på forespørgsel",287,"Rohrbausatz für Warmwasserspeicher RBS 302","Rohrbausatz für Warmwasserspeicher RBS 302","Rohrbausatz für Warmwasserspeicher RBS 302","Rohrbausatz für Warmwasserspeicher RBS 302","Rohrbausatz für Warmwasserspeicher RBS 302"]
[null,234511,"Rohrbausatz für Warmwasserspeicher RBS 401","On request",null,null,null,null,null,null,null,234511,"Rohrbausatz für Warmwasserspeicher RBS 401","On request",false,null,234511,347,"On request",500,"på forespørgsel",347,"Rohrbausatz für Warmwasserspeicher RBS 401","Rohrbausatz für Warmwasserspeicher RBS 401","Rohrbausatz für Warmwasserspeicher RBS 401","Rohrbausatz für Warmwasserspeicher RBS 401","Rohrbausatz für Warmwasserspeicher RBS 401"]
[null,234512,"Rohrbausatz für Warmwasserspeicher RBS 401.2","On request",null,null,null,null,null,null,null,234512,"Rohrbausatz für Warmwasserspeicher RBS 401.2","On request",false,null,234512,347,"On request",585,"på forespørgsel",347,"Rohrbausatz für Warmwasserspeicher RBS 401.2","Rohrbausatz für Warmwasserspeicher RBS 401.2","Rohrbausatz für Warmwasserspeicher RBS 401.2","Rohrbausatz für Warmwasserspeicher RBS 401.2","Rohrbausatz für Warmwasserspeicher RBS 401.2"]
[null,234513,"Rohrbausatz für Warmwasserspeicher RBS 501","On request",null,null,null,null,null,null,null,234513,"Rohrbausatz für Warmwasserspeicher RBS 501","On request",false,null,234513,397,"On request",500,"på forespørgsel",397,"Rohrbausatz für Warmwasserspeicher RBS 501","Rohrbausatz für Warmwasserspeicher RBS 501","Rohrbausatz für Warmwasserspeicher RBS 501","Rohrbausatz für Warmwasserspeicher RBS 501","Rohrbausatz für Warmwasserspeicher RBS 501"]
[null,234514,"Rohrbausatz für Warmwasserspeicher RBS 501.2","On request",null,null,null,null,null,null,null,234514,"Rohrbausatz für Warmwasserspeicher RBS 501.2","On request",false,null,234514,397,"On request",585,"på forespørgsel",397,"Rohrbausatz für Warmwasserspeicher RBS 501.2","Rohrbausatz für Warmwasserspeicher RBS 501.2","Rohrbausatz für Warmwasserspeicher RBS 501.2","Rohrbausatz für Warmwasserspeicher RBS 501.2","Rohrbausatz für Warmwasserspeicher RBS 501.2"]
[null,233510,"Integral-Speicher HSBC 200","On request",null,null,null,null,null,null,null,233510,"Integral-Speicher HSBC 200","On request",false,null,233510,3695,"On request","5.390,00","på forespørgsel",3695,"Integral-Speicher HSBC 200","Integral-Speicher HSBC 200","Integral-Speicher HSBC 200","Integral-Speicher HSBC 200","Integral-Speicher HSBC 200"]
[null,234648,"Pumpenbaugruppe Mischerkreis für HSBC 200","On request",null,null,null,null,null,null,null,234648,"Pumpenbaugruppe Mischerkreis für HSBC 200","On request",false,null,234648,495,"On request",695,"på forespørgsel",495,"Pumpenbaugruppe Mischerkreis für HSBC 200","Pumpenbaugruppe Mischerkreis für HSBC 200","Pumpenbaugruppe Mischerkreis für HSBC 200","Pumpenbaugruppe Mischerkreis für HSBC 200","Pumpenbaugruppe Mischerkreis für HSBC 200"]
[null,"ATEC-01","Abgas-Komplettsystem für SBP 750/950 G","On request",null,null,null,null,null,null,null,"ATEC-01","Abgas-Komplettsystem für SBP 750/950 G","On request",false,null,"ATEC-01","auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Abgas-Komplettsystem für SBP 750/950 G","Abgas-Komplettsystem für SBP 750/950 G","Abgas-Komplettsystem für SBP 750/950 G","Abgas-Komplettsystem für SBP 750/950 G","Abgas-Komplettsystem montagefertig für SBP-Gas"]
[null,233583,"Warmwasser-Wärmepumpe WWK 300 electronic SOL","On request",null,null,null,null,null,null,null,233583,"Warmwasser-Wärmepumpe WWK 300 electronic SOL","On request",false,null,233583,2950,"On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 300 electronic SOL","Warmwasser-Wärmepumpe WWK 300 electronic SOL","Warmwasser-Wärmepumpe WWK 300 electronic SOL","Warmwasser-Wärmepumpe WWK 300 electronic SOL","Warmwater-Warmtepompboiler WWK 300 electronic SOL"]
[null,230949,"Warmwasser-Wärmepumpe WWK 221 electronic","On request",null,null,null,null,null,null,null,230949,"Warmwasser-Wärmepumpe WWK 221 electronic","On request",false,null,230949,2650,"On request","2.490,00","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 221 electronic","Warmwasser-Wärmepumpe WWK 221 electronic","Warmwasser-Wärmepumpe WWK 221 electronic","Warmwasser-Wärmepumpe WWK 221 electronic","Warmwater-Warmtepompboiler WWK 221 electronic"]
[null,230950,"Warmwasser-Wärmepumpe WWK 301 electronic","On request",null,null,null,null,null,null,null,230950,"Warmwasser-Wärmepumpe WWK 301 electronic","On request",false,null,230950,2750,"On request","2.590,00","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 301 electronic","Warmwasser-Wärmepumpe WWK 301 electronic","Warmwasser-Wärmepumpe WWK 301 electronic","Warmwasser-Wärmepumpe WWK 301 electronic","Warmwater-Warmtepompboiler WWK 301 electronic"]
[null,233584,"Warmwasser-Wärmepumpe WWK 301 electronic SOL","On request",null,null,null,null,null,null,null,233584,"Warmwasser-Wärmepumpe WWK 301 electronic SOL","On request",false,null,233584,3250,"On request","3.390,00","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 301 electronic SOL","Warmwasser-Wärmepumpe WWK 301 electronic SOL","Warmwasser-Wärmepumpe WWK 301 electronic SOL","Warmwasser-Wärmepumpe WWK 301 electronic SOL","Warmwater-Warmtepompboiler WWK 301 electronic SOL"]
[null,233920,"Schaltschrank 2 Wärmepumpen (Heizen)","On request",null,null,null,null,null,null,null,233920,"Schaltschrank 2 Wärmepumpen (Heizen)","On request",false,null,233920,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 2 Wärmepumpen (Heizen)","Schaltschrank 2 Wärmepumpen (Heizen)","Schaltschrank 2 Wärmepumpen (Heizen)","Schaltschrank 2 Wärmepumpen (Heizen)","Schaltschrank 2 Wärmepumpen (Heizen)"]
[null,233921,"Schaltschrank 2 Wärmepumpen (Heizen/GLT)","On request",null,null,null,null,null,null,null,233921,"Schaltschrank 2 Wärmepumpen (Heizen/GLT)","On request",false,null,233921,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 2 Wärmepumpen (Heizen/GLT)","Schaltschrank 2 Wärmepumpen (Heizen/GLT)","Schaltschrank 2 Wärmepumpen (Heizen/GLT)","Schaltschrank 2 Wärmepumpen (Heizen/GLT)","Schaltschrank 2 Wärmepumpen (Heizen/GLT)"]
[null,233922,"Schaltschrank 2 Wärmepumpen (Heizen/Kühlen)","On request",null,null,null,null,null,null,null,233922,"Schaltschrank 2 Wärmepumpen (Heizen/Kühlen)","On request",false,null,233922,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen)"]
[null,233923,"Schaltschrank 2 Wärmepumpen (Heizen/Kühlen/GLT)","On request",null,null,null,null,null,null,null,233923,"Schaltschrank 2 Wärmepumpen (Heizen/Kühlen/GLT)","On request",false,null,233923,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 2 Wärmepumpen (Heizen/Kühlen/GLT)"]
[null,233924,"Schaltschrank 3 Wärmepumpen (Heizen)","On request",null,null,null,null,null,null,null,233924,"Schaltschrank 3 Wärmepumpen (Heizen)","On request",false,null,233924,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 3 Wärmepumpen (Heizen)","Schaltschrank 3 Wärmepumpen (Heizen)","Schaltschrank 3 Wärmepumpen (Heizen)","Schaltschrank 3 Wärmepumpen (Heizen)","Schaltschrank 3 Wärmepumpen (Heizen)"]
[null,233925,"Schaltschrank 3 Wärmepumpen (Heizen/GLT)","On request",null,null,null,null,null,null,null,233925,"Schaltschrank 3 Wärmepumpen (Heizen/GLT)","On request",false,null,233925,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 3 Wärmepumpen (Heizen/GLT)","Schaltschrank 3 Wärmepumpen (Heizen/GLT)","Schaltschrank 3 Wärmepumpen (Heizen/GLT)","Schaltschrank 3 Wärmepumpen (Heizen/GLT)","Schaltschrank 3 Wärmepumpen (Heizen/GLT)"]
[null,233926,"Schaltschrank 3 Wärmepumpen (Heizen/Kühlen)","On request",null,null,null,null,null,null,null,233926,"Schaltschrank 3 Wärmepumpen (Heizen/Kühlen)","On request",false,null,233926,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen)"]
[null,233927,"Schaltschrank 3 Wärmepumpen (Heizen/Kühlen/GLT)","On request",null,null,null,null,null,null,null,233927,"Schaltschrank 3 Wärmepumpen (Heizen/Kühlen/GLT)","On request",false,null,233927,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 3 Wärmepumpen (Heizen/Kühlen/GLT)"]
[null,233928,"Schaltschrank 4 Wärmepumpen (Heizen)","On request",null,null,null,null,null,null,null,233928,"Schaltschrank 4 Wärmepumpen (Heizen)","On request",false,null,233928,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 4 Wärmepumpen (Heizen)","Schaltschrank 4 Wärmepumpen (Heizen)","Schaltschrank 4 Wärmepumpen (Heizen)","Schaltschrank 4 Wärmepumpen (Heizen)","Schaltschrank 4 Wärmepumpen (Heizen)"]
[null,233929,"Schaltschrank 4 Wärmepumpen (Heizen/GLT)","On request",null,null,null,null,null,null,null,233929,"Schaltschrank 4 Wärmepumpen (Heizen/GLT)","On request",false,null,233929,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 4 Wärmepumpen (Heizen/GLT)","Schaltschrank 4 Wärmepumpen (Heizen/GLT)","Schaltschrank 4 Wärmepumpen (Heizen/GLT)","Schaltschrank 4 Wärmepumpen (Heizen/GLT)","Schaltschrank 4 Wärmepumpen (Heizen/GLT)"]
[null,233930,"Schaltschrank 4 Wärmepumpen (Heizen/Kühlen)","On request",null,null,null,null,null,null,null,233930,"Schaltschrank 4 Wärmepumpen (Heizen/Kühlen)","On request",false,null,233930,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen)"]
[null,233931,"Schaltschrank 4 Wärmepumpen (Heizen/Kühlen/GLT)","On request",null,null,null,null,null,null,null,233931,"Schaltschrank 4 Wärmepumpen (Heizen/Kühlen/GLT)","On request",false,null,233931,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 4 Wärmepumpen (Heizen/Kühlen/GLT)"]
[null,233932,"Schaltschrank 5 Wärmepumpen (Heizen)","On request",null,null,null,null,null,null,null,233932,"Schaltschrank 5 Wärmepumpen (Heizen)","On request",false,null,233932,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 5 Wärmepumpen (Heizen)","Schaltschrank 5 Wärmepumpen (Heizen)","Schaltschrank 5 Wärmepumpen (Heizen)","Schaltschrank 5 Wärmepumpen (Heizen)","Schaltschrank 5 Wärmepumpen (Heizen)"]
[null,233933,"Schaltschrank 5 Wärmepumpen (Heizen/GLT)","On request",null,null,null,null,null,null,null,233933,"Schaltschrank 5 Wärmepumpen (Heizen/GLT)","On request",{"$f":"IF(AND(B1385=L1385,C1385=M1385,D1385=N1385),FALSE,TRUE)","v":false},null,233933,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 5 Wärmepumpen (Heizen/GLT)","Schaltschrank 5 Wärmepumpen (Heizen/GLT)","Schaltschrank 5 Wärmepumpen (Heizen/GLT)","Schaltschrank 5 Wärmepumpen (Heizen/GLT)","Schaltschrank 5 Wärmepumpen (Heizen/GLT)"]
[null,233934,"Schaltschrank 5 Wärmepumpen (Heizen/Kühlen)","On request",null,null,null,null,null,null,null,233934,"Schaltschrank 5 Wärmepumpen (Heizen/Kühlen)","On request",false,null,233934,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen)"]
[null,233935,"Schaltschrank 5 Wärmepumpen (Heizen/Kühlen/GLT)","On request",null,null,null,null,null,null,null,233935,"Schaltschrank 5 Wärmepumpen (Heizen/Kühlen/GLT)","On request",false,null,233935,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 5 Wärmepumpen (Heizen/Kühlen/GLT)"]
[null,233936,"Schaltschrank 6 Wärmepumpen (Heizen)","On request",null,null,null,null,null,null,null,233936,"Schaltschrank 6 Wärmepumpen (Heizen)","On request",false,null,233936,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 6 Wärmepumpen (Heizen)","Schaltschrank 6 Wärmepumpen (Heizen)","Schaltschrank 6 Wärmepumpen (Heizen)","Schaltschrank 6 Wärmepumpen (Heizen)","Schaltschrank 6 Wärmepumpen (Heizen)"]
[null,233937,"Schaltschrank 6 Wärmepumpen (Heizen/GLT)","On request",null,null,null,null,null,null,null,233937,"Schaltschrank 6 Wärmepumpen (Heizen/GLT)","On request",false,null,233937,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 6 Wärmepumpen (Heizen/GLT)","Schaltschrank 6 Wärmepumpen (Heizen/GLT)","Schaltschrank 6 Wärmepumpen (Heizen/GLT)","Schaltschrank 6 Wärmepumpen (Heizen/GLT)","Schaltschrank 6 Wärmepumpen (Heizen/GLT)"]
[null,233938,"Schaltschrank 6 Wärmepumpen (Heizen/Kühlen)","On request",null,null,null,null,null,null,null,233938,"Schaltschrank 6 Wärmepumpen (Heizen/Kühlen)","On request",false,null,233938,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen)","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen)"]
[null,233939,"Schaltschrank 6 Wärmepumpen (Heizen/Kühlen/GLT)","On request",null,null,null,null,null,null,null,233939,"Schaltschrank 6 Wärmepumpen (Heizen/Kühlen/GLT)","On request",false,null,233939,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen/GLT)","Schaltschrank 6 Wärmepumpen (Heizen/Kühlen/GLT)"]
[null,233940,"Schaltschrank 6 x WPF 66 (Heizen)","On request",null,null,null,null,null,null,null,233940,"Schaltschrank 6 x WPF 66 (Heizen)","On request",false,null,233940,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 6 x WPF 66 (Heizen)","Schaltschrank 6 x WPF 66 (Heizen)","Schaltschrank 6 x WPF 66 (Heizen)","Schaltschrank 6 x WPF 66 (Heizen)","Schaltschrank 6 x WPF 66 (Heizen)"]
[null,233941,"Schaltschrank 6 x WPF 66 (Heizen/GLT)","On request",null,null,null,null,null,null,null,233941,"Schaltschrank 6 x WPF 66 (Heizen/GLT)","On request",false,null,233941,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 6 x WPF 66 (Heizen/GLT)","Schaltschrank 6 x WPF 66 (Heizen/GLT)","Schaltschrank 6 x WPF 66 (Heizen/GLT)","Schaltschrank 6 x WPF 66 (Heizen/GLT)","Schaltschrank 6 x WPF 66 (Heizen/GLT)"]
[null,233942,"Schaltschrank 6 x WPF 66 (Heizen/Kühlen)","On request",null,null,null,null,null,null,null,233942,"Schaltschrank 6 x WPF 66 (Heizen/Kühlen)","On request",false,null,233942,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 6 x WPF 66 (Heizen/Kühlen)","Schaltschrank 6 x WPF 66 (Heizen/Kühlen)","Schaltschrank 6 x WPF 66 (Heizen/Kühlen)","Schaltschrank 6 x WPF 66 (Heizen/Kühlen)","Schaltschrank 6 x WPF 66 (Heizen/Kühlen)"]
[null,233943,"Schaltschrank 6 x WPF 66 (Heizen/Kühlen/GLT)","On request",null,null,null,null,null,null,null,233943,"Schaltschrank 6 x WPF 66 (Heizen/Kühlen/GLT)","On request",false,null,233943,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Schaltschrank 6 x WPF 66 (Heizen/Kühlen/GLT)","Schaltschrank 6 x WPF 66 (Heizen/Kühlen/GLT)","Schaltschrank 6 x WPF 66 (Heizen/Kühlen/GLT)","Schaltschrank 6 x WPF 66 (Heizen/Kühlen/GLT)","Schaltschrank 6 x WPF 66 (Heizen/Kühlen/GLT)"]
[null,234383,"Luft|Wasser-Wärmepumpe WPL 10 AC Set 4","On request",null,null,null,null,null,null,null,234383,"Luft|Wasser-Wärmepumpe WPL 10 AC Set 4","On request",false,null,234383,6700,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 10 AC Set 4","Luft|Wasser-Wärmepumpe WPL 10 AC Set 4","Luft|Wasser-Wärmepumpe WPL 10 AC Set 4","Luft|Wasser-Wärmepumpe WPL 10 AC Set 4","Luft|Wasser-Wärmepumpe WPL 10 AC Set 4"]
[null,234384,"Luft|Wasser-Wärmepumpe WPL 10 AC Set 5","On request",null,null,null,null,null,null,null,234384,"Luft|Wasser-Wärmepumpe WPL 10 AC Set 5","On request",false,null,234384,8850,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 10 AC Set 5","Luft|Wasser-Wärmepumpe WPL 10 AC Set 5","Luft|Wasser-Wärmepumpe WPL 10 AC Set 5","Luft|Wasser-Wärmepumpe WPL 10 AC Set 5","Luft|Wasser-Wärmepumpe WPL 10 AC Set 5"]
[null,234385,"Luft|Wasser-Wärmepumpe WPL 10 AC Set 6","On request",null,null,null,null,null,null,null,234385,"Luft|Wasser-Wärmepumpe WPL 10 AC Set 6","On request",false,null,234385,7850,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 10 AC Set 6","Luft|Wasser-Wärmepumpe WPL 10 AC Set 6","Luft|Wasser-Wärmepumpe WPL 10 AC Set 6","Luft|Wasser-Wärmepumpe WPL 10 AC Set 6","Luft|Wasser-Wärmepumpe WPL 10 AC Set 6"]
[null,234386,"Luft|Wasser-Wärmepumpe WPL 10 AC Set 7","On request",null,null,null,null,null,null,null,234386,"Luft|Wasser-Wärmepumpe WPL 10 AC Set 7","On request",false,null,234386,10020,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 10 AC Set 7","Luft|Wasser-Wärmepumpe WPL 10 AC Set 7","Luft|Wasser-Wärmepumpe WPL 10 AC Set 7","Luft|Wasser-Wärmepumpe WPL 10 AC Set 7","Luft|Wasser-Wärmepumpe WPL 10 AC Set 7"]
[null,234387,"Luft|Wasser-Wärmepumpe WPL 15 AS Set 1","On request",null,null,null,null,null,null,null,234387,"Luft|Wasser-Wärmepumpe WPL 15 AS Set 1","On request",false,null,234387,9830,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 15 AS Set 1","Luft|Wasser-Wärmepumpe WPL 15 AS Set 1","Luft|Wasser-Wärmepumpe WPL 15 AS Set 1","Luft|Wasser-Wärmepumpe WPL 15 AS Set 1","Luft|Wasser-Wärmepumpe WPL 15 AS Set 1"]
[null,234388,"Luft|Wasser-Wärmepumpe WPL 15 AS Set 2","On request",null,null,null,null,null,null,null,234388,"Luft|Wasser-Wärmepumpe WPL 15 AS Set 2","On request",false,null,234388,12160,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 15 AS Set 2","Luft|Wasser-Wärmepumpe WPL 15 AS Set 2","Luft|Wasser-Wärmepumpe WPL 15 AS Set 2","Luft|Wasser-Wärmepumpe WPL 15 AS Set 2","Luft|Wasser-Wärmepumpe WPL 15 AS Set 2"]
[null,234389,"Luft|Wasser-Wärmepumpe WPL 15 AS Set 3","On request",null,null,null,null,null,null,null,234389,"Luft|Wasser-Wärmepumpe WPL 15 AS Set 3","On request",false,null,234389,11050,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 15 AS Set 3","Luft|Wasser-Wärmepumpe WPL 15 AS Set 3","Luft|Wasser-Wärmepumpe WPL 15 AS Set 3","Luft|Wasser-Wärmepumpe WPL 15 AS Set 3","Luft|Wasser-Wärmepumpe WPL 15 AS Set 3"]
[null,234390,"Luft|Wasser-Wärmepumpe WPL 15 AS Set 4","On request",null,null,null,null,null,null,null,234390,"Luft|Wasser-Wärmepumpe WPL 15 AS Set 4","On request",false,null,234390,13020,"On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 15 AS Set 4","Luft|Wasser-Wärmepumpe WPL 15 AS Set 4","Luft|Wasser-Wärmepumpe WPL 15 AS Set 4","Luft|Wasser-Wärmepumpe WPL 15 AS Set 4","Luft|Wasser-Wärmepumpe WPL 15 AS Set 4"]
[null,234646,"Wärmegedämmter Luftschlauch DN 315, 4m","On request",null,null,null,null,null,null,null,234646,"Wärmegedämmter Luftschlauch DN 315, 4m","On request",false,null,234646,240,"On request",180,"på forespørgsel",240,"Wärmegedämmter Luftschlauch DN 315, 4m","Wärmegedämmter Luftschlauch DN 315, 4m","Wärmegedämmter Luftschlauch DN 315, 4m","Wärmegedämmter Luftschlauch DN 315, 4m","Wärmegedämmter Luftschlauch DN 315, 4m"]
[null,234866,"4-Stufen Schalter mit LED","On request",null,null,null,null,null,null,null,234866,"4-Stufen Schalter mit LED","On request",false,null,234866,58,"On request",40,"på forespørgsel","op aanvraag","4-Stufen Schalter mit LED","4-Stufen Schalter mit LED","4-Stufen Schalter mit LED","4-Stufen Schalter mit LED","4-Stufen Schalter mit LED"]
[null,234656,"Dezentrales Lüftungsgerät LA 50","On request",null,null,null,null,null,null,null,234656,"Dezentrales Lüftungsgerät LA 50","On request",false,null,234656,232,"On request","sur demande","på forespørgsel","op aanvraag","Dezentrales Lüftungsgerät LA 50","Dezentrales Lüftungsgerät LA 50","Dezentrales Lüftungsgerät LA 50","Dezentrales Lüftungsgerät LA 50","Ventilatieunit zonder warmteterugwinning LA 50"]
[null,234182,"Komfort-Bedieneinheit RCT für LA 30/50/60","On request",null,null,null,null,null,null,null,234182,"Komfort-Bedieneinheit RCT für LA 30/50/60","On request",false,null,234182,437,"On request","sur demande","på forespørgsel","op aanvraag","Komfort-Bedieneinheit RCT für LA 30/50/60","Komfort-Bedieneinheit RCT für LA 30/50/60","Komfort-Bedieneinheit RCT für LA 30/50/60","Komfort-Bedieneinheit RCT für LA 30/50/60","Komfort-Bedieneinheit für LA 50/60"]
[null,234182,"Komfort-Bedieneinheit RCT für LA 30/50/60","On request",null,null,null,null,null,null,null,234182,"Komfort-Bedieneinheit RCT für LA 30/50/60","On request",false,null,234182,437,"On request","sur demande","på forespørgsel","op aanvraag","Komfort-Bedieneinheit RCT für LA 30/50/60","Komfort-Bedieneinheit RCT für LA 30/50/60","Komfort-Bedieneinheit RCT für LA 30/50/60","Komfort-Bedieneinheit RCT für LA 30/50/60","Komfort-Bedieneinheit für LA 50/60"]
[null,234181,"Bedieneinheit 3-stufig für LA 30/50","On request",null,null,null,null,null,null,null,234181,"Bedieneinheit 3-stufig für LA 30/50","On request",false,null,234181,33,"On request","sur demande","på forespørgsel","op aanvraag","Bedieneinheit 3-stufig für LA 30/50","Bedieneinheit 3-stufig für LA 30/50","Bedieneinheit 3-stufig für LA 30/50","Bedieneinheit 3-stufig für LA 30/50","Bedieneinheit 3-stufig für LA 30 WRG"]
[null,234179,"Zentralsteuerungseinheit für 6 x LA 30/50","On request",null,null,null,null,null,null,null,234179,"Zentralsteuerungseinheit für 6 x LA 30/50","On request",false,null,234179,99,"On request","sur demande","på forespørgsel","op aanvraag","Zentralsteuerungseinheit für 6 x LA 30/50","Zentralsteuerungseinheit für 6 x LA 30/50","Zentralsteuerungseinheit für 6 x LA 30/50","Zentralsteuerungseinheit für 6 x LA 30/50","Centrale sturingsunit voor 6 x LA 30 WRG"]
[null,234180,"Zentralsteuerungseinheit für 10 x LA 30/50","On request",null,null,null,null,null,null,null,234180,"Zentralsteuerungseinheit für 10 x LA 30/50","On request",false,null,234180,109,"On request","sur demande","på forespørgsel","op aanvraag","Zentralsteuerungseinheit für 10 x LA 30/50","Zentralsteuerungseinheit für 10 x LA 30/50","Zentralsteuerungseinheit für 10 x LA 30/50","Zentralsteuerungseinheit für 10 x LA 30/50","Centrale sturingsunit voor 10 x LA 30 WRG"]
[null,234106,"Reduzierstück DN 200 / 160","On request",null,null,null,null,null,null,null,234106,"Reduzierstück DN 200 / 160","On request",false,null,234106,19,"On request","sur demande","på forespørgsel","op aanvraag","Reduzierstück DN 200 / 160","Reduzierstück DN 200 / 160","Reduzierstück DN 200 / 160","Reduzierstück DN 200 / 160","Reduceerstuk DN 200 / 160"]
[null,234107,"Rohrnippel DN 200","On request",null,null,null,null,null,null,null,234107,"Rohrnippel DN 200","On request",false,null,234107,10.5,"On request","sur demande","på forespørgsel","op aanvraag","Rohrnippel DN 200","Rohrnippel DN 200","Rohrnippel DN 200","Rohrnippel DN 200","Buisnippel DN 200"]
[null,234105,"Rohrmuffe DN 200","On request",null,null,null,null,null,null,null,234105,"Rohrmuffe DN 200","On request",false,null,234105,7.1,"On request","sur demande","på forespørgsel","op aanvraag","Rohrmuffe DN 200","Rohrmuffe DN 200","Rohrmuffe DN 200","Rohrmuffe DN 200","Buissok DN 200"]
[null,234104,"Bogen 90° DN 200","On request",null,null,null,null,null,null,null,234104,"Bogen 90° DN 200","On request",false,null,234104,28,"On request","sur demande","på forespørgsel","op aanvraag","Bogen 90° DN 200","Bogen 90° DN 200","Bogen 90° DN 200","Bogen 90° DN 200","Bocht 90° DN 200"]
[null,234492,"LVS Luftverteiler Aufputz, 9-fach","On request",null,null,null,null,null,null,null,234492,"LVS Luftverteiler Aufputz, 9-fach","On request",false,null,234492,250,"On request","sur demande","på forespørgsel","op aanvraag","LVS Luftverteiler Aufputz, 9-fach","LVS Luftverteiler Aufputz, 9-fach","LVS Luftverteiler Aufputz, 9-fach","LVS Luftverteiler Aufputz, 9-fach","LVS Luftverteiler Aufputz, 9-fach"]
[null,234493,"LVS Schallgedämmter Luftverteiler Aufputz, 9-fach","On request",null,null,null,null,null,null,null,234493,"LVS Schallgedämmter Luftverteiler Aufputz, 9-fach","On request",false,null,234493,460,"On request","sur demande","på forespørgsel","op aanvraag","LVS Schallgedämmter Luftverteiler Aufputz, 9-fach","LVS Schallgedämmter Luftverteiler Aufputz, 9-fach","LVS Schallgedämmter Luftverteiler Aufputz, 9-fach","LVS Schallgedämmter Luftverteiler Aufputz, 9-fach","LVS Schallgedämmter Luftverteiler Aufputz, 9-fach"]
[null,234495,"LVS Einstellplatte 9-fach für Luftverteiler VTS 9","On request",null,null,null,null,null,null,null,234495,"LVS Einstellplatte 9-fach für Luftverteiler VTS 9","On request",false,null,234495,180,"On request","sur demande","på forespørgsel","op aanvraag","LVS Einstellplatte 9-fach für Luftverteiler VTS 9","LVS Einstellplatte 9-fach für Luftverteiler VTS 9","LVS Einstellplatte 9-fach für Luftverteiler VTS 9","LVS Einstellplatte 9-fach für Luftverteiler VTS 9","LVS Einstellplatte 9-fach für Luftverteiler VTS 9"]
[null,234496,"LVS Einsteller DN 75 für Luftverteiler VTS 9","On request",null,null,null,null,null,null,null,234496,"LVS Einsteller DN 75 für Luftverteiler VTS 9","On request",false,null,234496,24,"On request","sur demande","på forespørgsel","op aanvraag","LVS Einsteller DN 75 für Luftverteiler VTS 9","LVS Einsteller DN 75 für Luftverteiler VTS 9","LVS Einsteller DN 75 für Luftverteiler VTS 9","LVS Einsteller DN 75 für Luftverteiler VTS 9","LVS Einsteller DN 75 für Luftverteiler VTS 9"]
[null,234494,"LVS Übergangsstück 75mm auf 90mm","On request",null,null,null,null,null,null,null,234494,"LVS Übergangsstück 75mm auf 90mm","On request",false,null,234494,19,"On request","sur demande","på forespørgsel","op aanvraag","LVS Übergangsstück 75mm auf 90mm","LVS Übergangsstück 75mm auf 90mm","LVS Übergangsstück 75mm auf 90mm","LVS Übergangsstück 75mm auf 90mm","LVS Übergangsstück 75mm auf 90mm"]
[null,234022,"Wärmegedämmter Luftschlauch DN 160, 4m","On request",null,null,null,null,null,null,null,234022,"Wärmegedämmter Luftschlauch DN 160, 4m","On request",false,null,234022,72,"On request",50,"på forespørgsel","op aanvraag","Wärmegedämmter Luftschlauch DN 160, 4m","Wärmegedämmter Luftschlauch DN 160, 4m","Wärmegedämmter Luftschlauch DN 160, 4m","Wärmegedämmter Luftschlauch DN 160, 4m","Wärmegedämmter Luftschlauch DN 160, 4m"]
[null,234023,"Wärmegedämmter Luftschlauch DN 200, 4m","On request",null,null,null,null,null,null,null,234023,"Wärmegedämmter Luftschlauch DN 200, 4m","On request",false,null,234023,88,"On request",55,"på forespørgsel","op aanvraag","Wärmegedämmter Luftschlauch DN 200, 4m","Wärmegedämmter Luftschlauch DN 200, 4m","Wärmegedämmter Luftschlauch DN 200, 4m","Wärmegedämmter Luftschlauch DN 200, 4m","Wärmegedämmter Luftschlauch DN 200, 4m"]
[null,234108,"Befestigungsschelle für Luftschlauch DN 160","On request",null,null,null,null,null,null,null,234108,"Befestigungsschelle für Luftschlauch DN 160","On request",false,null,234108,3.5,"On request","sur demande","på forespørgsel","op aanvraag","Befestigungsschelle für Luftschlauch DN 160","Befestigungsschelle für Luftschlauch DN 160","Befestigungsschelle für Luftschlauch DN 160","Befestigungsschelle für Luftschlauch DN 160","Befestigungsschelle für Luftschlauch DN 160"]
[null,234109,"Befestigungsschelle für Luftschlauch DN 200","On request",null,null,null,null,null,null,null,234109,"Befestigungsschelle für Luftschlauch DN 200","On request",false,null,234109,4,"On request","sur demande","på forespørgsel","op aanvraag","Befestigungsschelle für Luftschlauch DN 200","Befestigungsschelle für Luftschlauch DN 200","Befestigungsschelle für Luftschlauch DN 200","Befestigungsschelle für Luftschlauch DN 200","Befestigungsschelle für Luftschlauch DN 200"]
[null,234893,"Lüftungs-Basisset LVE bis 100 m²","On request",null,null,null,null,null,null,null,234893,"Lüftungs-Basisset LVE bis 100 m²","On request",false,null,234893,1050,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVE bis 100 m²","Lüftungs-Basisset LVE bis 100 m²","Lüftungs-Basisset LVE bis 100 m²","Lüftungs-Basisset LVE bis 100 m²","Lüftungs-Basisset LVE bis 100 m²"]
[null,234894,"Lüftungs-Basisset LVE bis 130 m²","On request",null,null,null,null,null,null,null,234894,"Lüftungs-Basisset LVE bis 130 m²","On request",false,null,234894,1500,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVE bis 130 m²","Lüftungs-Basisset LVE bis 130 m²","Lüftungs-Basisset LVE bis 130 m²","Lüftungs-Basisset LVE bis 130 m²","Lüftungs-Basisset LVE bis 130 m²"]
[null,234895,"Lüftungs-Basisset LVE bis 160 m²","On request",null,null,null,null,null,null,null,234895,"Lüftungs-Basisset LVE bis 160 m²","On request",false,null,234895,1880,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVE bis 160 m²","Lüftungs-Basisset LVE bis 160 m²","Lüftungs-Basisset LVE bis 160 m²","Lüftungs-Basisset LVE bis 160 m²","Lüftungs-Basisset LVE bis 160 m²"]
[null,234896,"Lüftungs-Basisset LVE bis 190 m²","On request",null,null,null,null,null,null,null,234896,"Lüftungs-Basisset LVE bis 190 m²","On request",false,null,234896,2300,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVE bis 190 m²","Lüftungs-Basisset LVE bis 190 m²","Lüftungs-Basisset LVE bis 190 m²","Lüftungs-Basisset LVE bis 190 m²","Lüftungs-Basisset LVE bis 190 m²"]
[null,234897,"Lüftungs-Basisset LVE bis 220 m²","On request",null,null,null,null,null,null,null,234897,"Lüftungs-Basisset LVE bis 220 m²","On request",false,null,234897,2550,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVE bis 220 m²","Lüftungs-Basisset LVE bis 220 m²","Lüftungs-Basisset LVE bis 220 m²","Lüftungs-Basisset LVE bis 220 m²","Lüftungs-Basisset LVE bis 220 m²"]
[null,234898,"Lüftungs-Basisset LVE bis 250 m²","On request",null,null,null,null,null,null,null,234898,"Lüftungs-Basisset LVE bis 250 m²","On request",false,null,234898,2850,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVE bis 250 m²","Lüftungs-Basisset LVE bis 250 m²","Lüftungs-Basisset LVE bis 250 m²","Lüftungs-Basisset LVE bis 250 m²","Lüftungs-Basisset LVE bis 250 m²"]
[null,317146,"Lüftungs-Zubehörset LVE bis 100 m²","On request",null,null,null,null,null,null,null,317146,"Lüftungs-Zubehörset LVE bis 100 m²","On request",false,null,317146,420,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVE bis 100 m²","Lüftungs-Zubehörset LVE bis 100 m²","Lüftungs-Zubehörset LVE bis 100 m²","Lüftungs-Zubehörset LVE bis 100 m²","Lüftungs-Zubehörset LVE bis 100 m²"]
[null,317147,"Lüftungs-Zubehörset LVE bis 130 m²","On request",null,null,null,null,null,null,null,317147,"Lüftungs-Zubehörset LVE bis 130 m²","On request",false,null,317147,600,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVE bis 130 m²","Lüftungs-Zubehörset LVE bis 130 m²","Lüftungs-Zubehörset LVE bis 130 m²","Lüftungs-Zubehörset LVE bis 130 m²","Lüftungs-Zubehörset LVE bis 130 m²"]
[null,317148,"Lüftungs-Zubehörset LVE bis 160 m²","On request",null,null,null,null,null,null,null,317148,"Lüftungs-Zubehörset LVE bis 160 m²","On request",false,null,317148,750,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVE bis 160 m²","Lüftungs-Zubehörset LVE bis 160 m²","Lüftungs-Zubehörset LVE bis 160 m²","Lüftungs-Zubehörset LVE bis 160 m²","Lüftungs-Zubehörset LVE bis 160 m²"]
[null,317149,"Lüftungs-Zubehörset LVE bis 190 m²","On request",null,null,null,null,null,null,null,317149,"Lüftungs-Zubehörset LVE bis 190 m²","On request",false,null,317149,920,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVE bis 190 m²","Lüftungs-Zubehörset LVE bis 190 m²","Lüftungs-Zubehörset LVE bis 190 m²","Lüftungs-Zubehörset LVE bis 190 m²","Lüftungs-Zubehörset LVE bis 190 m²"]
[null,317150,"Lüftungs-Zubehörset LVE bis 220 m²","On request",null,null,null,null,null,null,null,317150,"Lüftungs-Zubehörset LVE bis 220 m²","On request",false,null,317150,1020,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVE bis 220 m²","Lüftungs-Zubehörset LVE bis 220 m²","Lüftungs-Zubehörset LVE bis 220 m²","Lüftungs-Zubehörset LVE bis 220 m²","Lüftungs-Zubehörset LVE bis 220 m²"]
[null,317151,"Lüftungs-Zubehörset LVE bis 250 m²","On request",null,null,null,null,null,null,null,317151,"Lüftungs-Zubehörset LVE bis 250 m²","On request",false,null,317151,1140,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVE bis 250 m²","Lüftungs-Zubehörset LVE bis 250 m²","Lüftungs-Zubehörset LVE bis 250 m²","Lüftungs-Zubehörset LVE bis 250 m²","Lüftungs-Zubehörset LVE bis 250 m²"]
[null,234899,"Lüftungs-Basisset LVS bis 100 m²","On request",null,null,null,null,null,null,null,234899,"Lüftungs-Basisset LVS bis 100 m²","On request",false,null,234899,1180,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVS bis 100 m²","Lüftungs-Basisset LVS bis 100 m²","Lüftungs-Basisset LVS bis 100 m²","Lüftungs-Basisset LVS bis 100 m²","Lüftungs-Basisset LVS bis 100 m²"]
[null,234900,"Lüftungs-Basisset LVS bis 130 m²","On request",null,null,null,null,null,null,null,234900,"Lüftungs-Basisset LVS bis 130 m²","On request",false,null,234900,1780,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVS bis 130 m²","Lüftungs-Basisset LVS bis 130 m²","Lüftungs-Basisset LVS bis 130 m²","Lüftungs-Basisset LVS bis 130 m²","Lüftungs-Basisset LVS bis 130 m²"]
[null,234901,"Lüftungs-Basisset LVS bis 160 m²","On request",null,null,null,null,null,null,null,234901,"Lüftungs-Basisset LVS bis 160 m²","On request",false,null,234901,2020,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVS bis 160 m²","Lüftungs-Basisset LVS bis 160 m²","Lüftungs-Basisset LVS bis 160 m²","Lüftungs-Basisset LVS bis 160 m²","Lüftungs-Basisset LVS bis 160 m²"]
[null,234902,"Lüftungs-Basisset LVS bis 190 m²","On request",null,null,null,null,null,null,null,234902,"Lüftungs-Basisset LVS bis 190 m²","On request",false,null,234902,2500,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVS bis 190 m²","Lüftungs-Basisset LVS bis 190 m²","Lüftungs-Basisset LVS bis 190 m²","Lüftungs-Basisset LVS bis 190 m²","Lüftungs-Basisset LVS bis 190 m²"]
[null,234903,"Lüftungs-Basisset LVS bis 220 m²","On request",null,null,null,null,null,null,null,234903,"Lüftungs-Basisset LVS bis 220 m²","On request",false,null,234903,2750,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVS bis 220 m²","Lüftungs-Basisset LVS bis 220 m²","Lüftungs-Basisset LVS bis 220 m²","Lüftungs-Basisset LVS bis 220 m²","Lüftungs-Basisset LVS bis 220 m²"]
[null,234904,"Lüftungs-Basisset LVS bis 250 m²","On request",null,null,null,null,null,null,null,234904,"Lüftungs-Basisset LVS bis 250 m²","On request",false,null,234904,3200,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset LVS bis 250 m²","Lüftungs-Basisset LVS bis 250 m²","Lüftungs-Basisset LVS bis 250 m²","Lüftungs-Basisset LVS bis 250 m²","Lüftungs-Basisset LVS bis 250 m²"]
[null,317152,"Lüftungs-Zubehörset LVS bis 100 m²","On request",null,null,null,null,null,null,null,317152,"Lüftungs-Zubehörset LVS bis 100 m²","On request",false,null,317152,300,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVS bis 100 m²","Lüftungs-Zubehörset LVS bis 100 m²","Lüftungs-Zubehörset LVS bis 100 m²","Lüftungs-Zubehörset LVS bis 100 m²","Lüftungs-Zubehörset LVS bis 100 m²"]
[null,317153,"Lüftungs-Zubehörset LVS bis 130 m²","On request",null,null,null,null,null,null,null,317153,"Lüftungs-Zubehörset LVS bis 130 m²","On request",false,null,317153,450,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVS bis 130 m²","Lüftungs-Zubehörset LVS bis 130 m²","Lüftungs-Zubehörset LVS bis 130 m²","Lüftungs-Zubehörset LVS bis 130 m²","Lüftungs-Zubehörset LVS bis 130 m²"]
[null,317154,"Lüftungs-Zubehörset LVS bis 160 m²","On request",null,null,null,null,null,null,null,317154,"Lüftungs-Zubehörset LVS bis 160 m²","On request",false,null,317154,510,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVS bis 160 m²","Lüftungs-Zubehörset LVS bis 160 m²","Lüftungs-Zubehörset LVS bis 160 m²","Lüftungs-Zubehörset LVS bis 160 m²","Lüftungs-Zubehörset LVS bis 160 m²"]
[null,317155,"Lüftungs-Zubehörset LVS bis 190 m²","On request",null,null,null,null,null,null,null,317155,"Lüftungs-Zubehörset LVS bis 190 m²","On request",false,null,317155,625,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVS bis 190 m²","Lüftungs-Zubehörset LVS bis 190 m²","Lüftungs-Zubehörset LVS bis 190 m²","Lüftungs-Zubehörset LVS bis 190 m²","Lüftungs-Zubehörset LVS bis 190 m²"]
[null,317156,"Lüftungs-Zubehörset LVS bis 220 m²","On request",null,null,null,null,null,null,null,317156,"Lüftungs-Zubehörset LVS bis 220 m²","On request",false,null,317156,690,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVS bis 220 m²","Lüftungs-Zubehörset LVS bis 220 m²","Lüftungs-Zubehörset LVS bis 220 m²","Lüftungs-Zubehörset LVS bis 220 m²","Lüftungs-Zubehörset LVS bis 220 m²"]
[null,317157,"Lüftungs-Zubehörset LVS bis 250 m²","On request",null,null,null,null,null,null,null,317157,"Lüftungs-Zubehörset LVS bis 250 m²","On request",false,null,317157,800,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Zubehörset LVS bis 250 m²","Lüftungs-Zubehörset LVS bis 250 m²","Lüftungs-Zubehörset LVS bis 250 m²","Lüftungs-Zubehörset LVS bis 250 m²","Lüftungs-Zubehörset LVS bis 250 m²"]
[null,234905,"Lüftungs-Basisset Flachkanal bis 70 m²","On request",null,null,null,null,null,null,null,234905,"Lüftungs-Basisset Flachkanal bis 70 m²","On request",{"$f":"IF(AND(B1449=L1449,C1449=M1449,D1449=N1449),FALSE,TRUE)","v":false},null,234905,1340,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset Flachkanal bis 70 m²","Lüftungs-Basisset Flachkanal bis 70 m²","Lüftungs-Basisset Flachkanal bis 70 m²","Lüftungs-Basisset Flachkanal bis 70 m²","Lüftungs-Basisset Flachkanal bis 70 m²"]
[null,234906,"Lüftungs-Basisset Flachkanal bis 100 m²","On request",null,null,null,null,null,null,null,234906,"Lüftungs-Basisset Flachkanal bis 100 m²","On request",false,null,234906,1518,"On request","sur demande","på forespørgsel","op aanvraag","Lüftungs-Basisset Flachkanal bis 100 m²","Lüftungs-Basisset Flachkanal bis 100 m²","Lüftungs-Basisset Flachkanal bis 100 m²","Lüftungs-Basisset Flachkanal bis 100 m²","Lüftungs-Basisset Flachkanal bis 100 m²"]
[null,234497,"Zu- und Abluftset VTS 120 Z","On request",null,null,null,null,null,null,null,234497,"Zu- und Abluftset VTS 120 Z","On request",false,null,234497,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset VTS 120 Z","Zu- und Abluftset VTS 120 Z","Zu- und Abluftset VTS 120 Z","Zu- und Abluftset VTS 120 Z","Zu- und Abluftset VTS 120 Z"]
[null,234498,"Zu- und Abluftset VTS 160 Z","On request",null,null,null,null,null,null,null,234498,"Zu- und Abluftset VTS 160 Z","On request",false,null,234498,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset VTS 160 Z","Zu- und Abluftset VTS 160 Z","Zu- und Abluftset VTS 160 Z","Zu- und Abluftset VTS 160 Z","Zu- und Abluftset VTS 160 Z"]
[null,234499,"Zu- und Abluftset VTS 200 Z","On request",null,null,null,null,null,null,null,234499,"Zu- und Abluftset VTS 200 Z","On request",false,null,234499,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset VTS 200 Z","Zu- und Abluftset VTS 200 Z","Zu- und Abluftset VTS 200 Z","Zu- und Abluftset VTS 200 Z","Zu- und Abluftset VTS 200 Z"]
[null,234500,"Zu- und Abluftset VTS 240 Z","On request",null,null,null,null,null,null,null,234500,"Zu- und Abluftset VTS 240 Z","On request",false,null,234500,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Zu- und Abluftset VTS 240 Z","Zu- und Abluftset VTS 240 Z","Zu- und Abluftset VTS 240 Z","Zu- und Abluftset VTS 240 Z","Zu- und Abluftset VTS 240 Z"]
[null,230141,"Solar-Regelung SOM 6 Plus","On request",null,null,null,null,null,null,null,230141,"Solar-Regelung SOM 6 Plus","On request",false,null,230141,244,"On request","sur demande","på forespørgsel",244,"Solar-Regelung SOM 6 Plus","Solar-Regelung SOM 6 Plus","Solar-Regelung SOM 6 Plus","Solar-Regelung SOM 6 Plus","Solar regeling SOM 6 plus"]
[null,230142,"Solar-Regelung SOM 7 Plus","On request",null,null,null,null,null,null,null,230142,"Solar-Regelung SOM 7 Plus","On request",false,null,230142,486,"On request","sur demande","på forespørgsel",486,"Solar-Regelung SOM 7 Plus","Solar-Regelung SOM 7 Plus","Solar-Regelung SOM 7 Plus","Solar-Regelung SOM 7 Plus","Solar regeling SOM 7 plus"]
[null,234350,"Warmwasserspeicher SBBE 401 WP SOL","On request",null,null,null,null,null,null,null,234350,"Warmwasserspeicher SBBE 401 WP SOL","On request",false,null,234350,2436,"On request","2.885,00","på forespørgsel",2436,"Warmwasserspeicher SBBE 401 WP SOL","Warmwasserspeicher SBBE 401 WP SOL","Warmwasserspeicher SBBE 401 WP SOL","Warmwasserspeicher SBBE 401 WP SOL","Warmwaterboiler  SBBE 401 WP SOL"]
[null,234351,"Warmwasserspeicher SBBE 501 WP SOL","On request",null,null,null,null,null,null,null,234351,"Warmwasserspeicher SBBE 501 WP SOL","On request",false,null,234351,2669,"On request","3.250,00","på forespørgsel",2669,"Warmwasserspeicher SBBE 501 WP SOL","Warmwasserspeicher SBBE 501 WP SOL","Warmwasserspeicher SBBE 501 WP SOL","Warmwasserspeicher SBBE 501 WP SOL","Warmwaterboiler  SBBE 501 WP SOL"]
[null,234511,"Rohrbausatz für Warmwasserspeicher RBS 401","On request",null,null,null,null,null,null,null,234511,"Rohrbausatz für Warmwasserspeicher RBS 401","On request",false,null,234511,347,"On request",500,"på forespørgsel",347,"Rohrbausatz für Warmwasserspeicher RBS 401","Rohrbausatz für Warmwasserspeicher RBS 401","Rohrbausatz für Warmwasserspeicher RBS 401","Rohrbausatz für Warmwasserspeicher RBS 401","Rohrbausatz für Warmwasserspeicher RBS 401"]
[null,234513,"Rohrbausatz für Warmwasserspeicher RBS 501","On request",null,null,null,null,null,null,null,234513,"Rohrbausatz für Warmwasserspeicher RBS 501","On request",false,null,234513,397,"On request",500,"på forespørgsel",397,"Rohrbausatz für Warmwasserspeicher RBS 501","Rohrbausatz für Warmwasserspeicher RBS 501","Rohrbausatz für Warmwasserspeicher RBS 501","Rohrbausatz für Warmwasserspeicher RBS 501","Rohrbausatz für Warmwasserspeicher RBS 501"]
[null,274179,"Photovoltaikmodul TEGREON 260 P","On request",null,null,null,null,null,null,null,274179,"Photovoltaikmodul TEGREON 260 P","On request",false,null,274179,278.85000000000002,"On request","sur demande","på forespørgsel","op aanvraag","Photovoltaikmodul TEGREON 260 P","Photovoltaikmodul TEGREON 260 P","Photovoltaikmodul TEGREON 260 P","Photovoltaikmodul TEGREON 260 P","Fotovoltalische module TEGREON 260 P"]
[null,274180,"Photovoltaikmodul TEGREON 265 P","On request",null,null,null,null,null,null,null,274180,"Photovoltaikmodul TEGREON 265 P","On request",false,null,274180,284.20999999999998,"On request","sur demande","på forespørgsel","op aanvraag","Photovoltaikmodul TEGREON 265 P","Photovoltaikmodul TEGREON 265 P","Photovoltaikmodul TEGREON 265 P","Photovoltaikmodul TEGREON 265 P","Fotovoltalische module TEGREON 265 P"]
[null,274194,"Garantieverlängerung Batterie auf 7 Jahre","On request",null,null,null,null,null,null,null,274194,"Garantieverlängerung Batterie auf 7 Jahre","On request",false,null,274194,600,"On request","sur demande","på forespørgsel","op aanvraag","Garantieverlängerung Batterie auf 7 Jahre","Garantieverlängerung Batterie auf 7 Jahre","Garantieverlängerung Batterie auf 7 Jahre","Garantieverlängerung Batterie auf 7 Jahre","Garantieverlängerung Batterie auf 7 Jahre"]
[null,274181,"Wechselrichter WRS STP 10000 TL","On request",null,null,null,null,null,null,null,274181,"Wechselrichter WRS STP 10000 TL","On request",false,null,274181,3900,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 10000 TL","Wechselrichter WRS STP 10000 TL","Wechselrichter WRS STP 10000 TL","Wechselrichter WRS STP 10000 TL","Wechselrichter WRS STP 10000 TL"]
[null,274182,"Wechselrichter WRS STP 12000 TL","On request",null,null,null,null,null,null,null,274182,"Wechselrichter WRS STP 12000 TL","On request",false,null,274182,4450,"On request","sur demande","på forespørgsel","op aanvraag","Wechselrichter WRS STP 12000 TL","Wechselrichter WRS STP 12000 TL","Wechselrichter WRS STP 12000 TL","Wechselrichter WRS STP 12000 TL","Wechselrichter WRS STP 12000 TL"]
[null,274195,"Power Control Modul ZS PCM-A","On request",null,null,null,null,null,null,null,274195,"Power Control Modul ZS PCM-A","On request",false,null,274195,170,"On request","sur demande","på forespørgsel","op aanvraag","Power Control Modul ZS PCM-A","Power Control Modul ZS PCM-A","Power Control Modul ZS PCM-A","Power Control Modul ZS PCM-A","Power Control Modul ZS PCM-A"]
[null,274196,"Power Control Modul ZS PCM-B","On request",null,null,null,null,null,null,null,274196,"Power Control Modul ZS PCM-B","On request",false,null,274196,170,"On request","sur demande","på forespørgsel","op aanvraag","Power Control Modul ZS PCM-B","Power Control Modul ZS PCM-B","Power Control Modul ZS PCM-B","Power Control Modul ZS PCM-B","Power Control Modul ZS PCM-B"]
[null,274186,"Systemträgerschiene 1,2 m","On request",null,null,null,null,null,null,null,274186,"Systemträgerschiene 1,2 m","On request",false,null,274186,12,"On request","sur demande","på forespørgsel","op aanvraag","Systemträgerschiene 1,2 m","Systemträgerschiene 1,2 m","Systemträgerschiene 1,2 m","Systemträgerschiene 1,2 m","Systemträgerschiene 1,2 m"]
[null,274187,"Systemträgerschiene 1,9 m","On request",null,null,null,null,null,null,null,274187,"Systemträgerschiene 1,9 m","On request",false,null,274187,18,"On request","sur demande","på forespørgsel","op aanvraag","Systemträgerschiene 1,9 m","Systemträgerschiene 1,9 m","Systemträgerschiene 1,9 m","Systemträgerschiene 1,9 m","Systemträgerschiene 1,9 m"]
[null,274188,"Systemträgerschiene 2,5 m","On request",null,null,null,null,null,null,null,274188,"Systemträgerschiene 2,5 m","On request",false,null,274188,24,"On request","sur demande","på forespørgsel","op aanvraag","Systemträgerschiene 2,5 m","Systemträgerschiene 2,5 m","Systemträgerschiene 2,5 m","Systemträgerschiene 2,5 m","Systemträgerschiene 2,5 m"]
[null,274189,"Systemträgerschiene 3,1 m","On request",null,null,null,null,null,null,null,274189,"Systemträgerschiene 3,1 m","On request",false,null,274189,23,"On request","sur demande","på forespørgsel","op aanvraag","Systemträgerschiene 3,1 m","Systemträgerschiene 3,1 m","Systemträgerschiene 3,1 m","Systemträgerschiene 3,1 m","Systemträgerschiene 3,1 m"]
[null,234657,"Wohnungsstation Grundmodul WS-1","On request",null,null,null,null,null,null,null,234657,"Wohnungsstation Grundmodul WS-1","On request",false,null,234657,1136,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WS-1","Wohnungsstation Grundmodul WS-1","Wohnungsstation Grundmodul WS-1","Wohnungsstation Grundmodul WS-1","Wohnungsstation Grundmodul WS-1"]
[null,234658,"Wohnungsstation Grundmodul WS-2","On request",null,null,null,null,null,null,null,234658,"Wohnungsstation Grundmodul WS-2","On request",false,null,234658,1171,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WS-2","Wohnungsstation Grundmodul WS-2","Wohnungsstation Grundmodul WS-2","Wohnungsstation Grundmodul WS-2","Wohnungsstation Grundmodul WS-2"]
[null,234659,"Wohnungsstation Grundmodul WS-3","On request",null,null,null,null,null,null,null,234659,"Wohnungsstation Grundmodul WS-3","On request",false,null,234659,1189,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WS-3","Wohnungsstation Grundmodul WS-3","Wohnungsstation Grundmodul WS-3","Wohnungsstation Grundmodul WS-3","Wohnungsstation Grundmodul WS-3"]
[null,234660,"Wohnungsstation Grundmodul WS-4","On request",null,null,null,null,null,null,null,234660,"Wohnungsstation Grundmodul WS-4","On request",false,null,234660,1408,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WS-4","Wohnungsstation Grundmodul WS-4","Wohnungsstation Grundmodul WS-4","Wohnungsstation Grundmodul WS-4","Wohnungsstation Grundmodul WS-4"]
[null,234661,"Wohnungsstation Grundmodul WSP-1","On request",null,null,null,null,null,null,null,234661,"Wohnungsstation Grundmodul WSP-1","On request",false,null,234661,1330,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WSP-1","Wohnungsstation Grundmodul WSP-1","Wohnungsstation Grundmodul WSP-1","Wohnungsstation Grundmodul WSP-1","Wohnungsstation Grundmodul WSP-1"]
[null,234662,"Wohnungsstation Grundmodul WSP-2","On request",null,null,null,null,null,null,null,234662,"Wohnungsstation Grundmodul WSP-2","On request",false,null,234662,1650,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WSP-2","Wohnungsstation Grundmodul WSP-2","Wohnungsstation Grundmodul WSP-2","Wohnungsstation Grundmodul WSP-2","Wohnungsstation Grundmodul WSP-2"]
[null,234663,"Wohnungsstation Grundmodul WSP-3","On request",null,null,null,null,null,null,null,234663,"Wohnungsstation Grundmodul WSP-3","On request",false,null,234663,1720,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WSP-3","Wohnungsstation Grundmodul WSP-3","Wohnungsstation Grundmodul WSP-3","Wohnungsstation Grundmodul WSP-3","Wohnungsstation Grundmodul WSP-3"]
[null,234664,"Wohnungsstation Grundmodul WSG-1","On request",null,null,null,null,null,null,null,234664,"Wohnungsstation Grundmodul WSG-1","On request",false,null,234664,1650,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WSG-1","Wohnungsstation Grundmodul WSG-1","Wohnungsstation Grundmodul WSG-1","Wohnungsstation Grundmodul WSG-1","Wohnungsstation Grundmodul WSG-1"]
[null,234665,"Wohnungsstation Grundmodul WSG-2","On request",null,null,null,null,null,null,null,234665,"Wohnungsstation Grundmodul WSG-2","On request",false,null,234665,1950,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WSG-2","Wohnungsstation Grundmodul WSG-2","Wohnungsstation Grundmodul WSG-2","Wohnungsstation Grundmodul WSG-2","Wohnungsstation Grundmodul WSG-2"]
[null,234666,"Wohnungsstation Grundmodul WSG-3","On request",null,null,null,null,null,null,null,234666,"Wohnungsstation Grundmodul WSG-3","On request",false,null,234666,2050,"On request","sur demande","på forespørgsel","op aanvraag","Wohnungsstation Grundmodul WSG-3","Wohnungsstation Grundmodul WSG-3","Wohnungsstation Grundmodul WSG-3","Wohnungsstation Grundmodul WSG-3","Wohnungsstation Grundmodul WSG-3"]
[null,234667,"Zubehör Heizkreis thermostatisch E1-HKT","On request",null,null,null,null,null,null,null,234667,"Zubehör Heizkreis thermostatisch E1-HKT","On request",false,null,234667,600,"On request","sur demande","på forespørgsel","op aanvraag","Zubehör Heizkreis thermostatisch E1-HKT","Zubehör Heizkreis thermostatisch E1-HKT","Zubehör Heizkreis thermostatisch E1-HKT","Zubehör Heizkreis thermostatisch E1-HKT","Zubehör Heizkreis thermostatisch E1-HKT"]
[null,234668,"Zubehör Heizkreis elektrisch E1-HKE","On request",null,null,null,null,null,null,null,234668,"Zubehör Heizkreis elektrisch E1-HKE","On request",false,null,234668,1050,"On request","sur demande","på forespørgsel","op aanvraag","Zubehör Heizkreis elektrisch E1-HKE","Zubehör Heizkreis elektrisch E1-HKE","Zubehör Heizkreis elektrisch E1-HKE","Zubehör Heizkreis elektrisch E1-HKE","Zubehör Heizkreis elektrisch E1-HKE"]
[null,234669,"Zubehör Heizkreis ungemischt E2-HKU","On request",null,null,null,null,null,null,null,234669,"Zubehör Heizkreis ungemischt E2-HKU","On request",false,null,234669,110,"On request","sur demande","på forespørgsel","op aanvraag","Zubehör Heizkreis ungemischt E2-HKU","Zubehör Heizkreis ungemischt E2-HKU","Zubehör Heizkreis ungemischt E2-HKU","Zubehör Heizkreis ungemischt E2-HKU","Zubehör Heizkreis ungemischt E2-HKU"]
[null,234670,"Aufputzgehäuse E3-GAK1","On request",null,null,null,null,null,null,null,234670,"Aufputzgehäuse E3-GAK1","On request",false,null,234670,129,"On request","sur demande","på forespørgsel","op aanvraag","Aufputzgehäuse E3-GAK1","Aufputzgehäuse E3-GAK1","Aufputzgehäuse E3-GAK1","Aufputzgehäuse E3-GAK1","Aufputzgehäuse E3-GAK1"]
[null,234671,"Unterputzgehäuse E3-GUK1","On request",null,null,null,null,null,null,null,234671,"Unterputzgehäuse E3-GUK1","On request",false,null,234671,180,"On request","sur demande","på forespørgsel","op aanvraag","Unterputzgehäuse E3-GUK1","Unterputzgehäuse E3-GUK1","Unterputzgehäuse E3-GUK1","Unterputzgehäuse E3-GUK1","Unterputzgehäuse E3-GUK1"]
[null,234672,"Aufputzgehäuse E3-GAK2","On request",null,null,null,null,null,null,null,234672,"Aufputzgehäuse E3-GAK2","On request",false,null,234672,155,"On request","sur demande","på forespørgsel","op aanvraag","Aufputzgehäuse E3-GAK2","Aufputzgehäuse E3-GAK2","Aufputzgehäuse E3-GAK2","Aufputzgehäuse E3-GAK2","Aufputzgehäuse E3-GAK2"]
[null,234673,"Aufputzgehäuse E3-GAL1","On request",null,null,null,null,null,null,null,234673,"Aufputzgehäuse E3-GAL1","On request",false,null,234673,180,"On request","sur demande","på forespørgsel","op aanvraag","Aufputzgehäuse E3-GAL1","Aufputzgehäuse E3-GAL1","Aufputzgehäuse E3-GAL1","Aufputzgehäuse E3-GAL1","Aufputzgehäuse E3-GAL1"]
[null,234674,"Unterputzgehäuse E3-GUK2","On request",null,null,null,null,null,null,null,234674,"Unterputzgehäuse E3-GUK2","On request",false,null,234674,190,"On request","sur demande","på forespørgsel","op aanvraag","Unterputzgehäuse E3-GUK2","Unterputzgehäuse E3-GUK2","Unterputzgehäuse E3-GUK2","Unterputzgehäuse E3-GUK2","Unterputzgehäuse E3-GUK2"]
[null,234675,"Unterputzgehäuse, E3-GUL1","On request",null,null,null,null,null,null,null,234675,"Unterputzgehäuse, E3-GUL1","On request",false,null,234675,260,"On request","sur demande","på forespørgsel","op aanvraag","Unterputzgehäuse, E3-GUL1","Unterputzgehäuse, E3-GUL1","Unterputzgehäuse, E3-GUL1","Unterputzgehäuse, E3-GUL1","Unterputzgehäuse, E3-GUL1"]
[null,234676,"Unterputzgehäuse, E3-GUL2","On request",null,null,null,null,null,null,null,234676,"Unterputzgehäuse, E3-GUL2","On request",false,null,234676,290,"On request","sur demande","på forespørgsel","op aanvraag","Unterputzgehäuse, E3-GUL2","Unterputzgehäuse, E3-GUL2","Unterputzgehäuse, E3-GUL2","Unterputzgehäuse, E3-GUL2","Unterputzgehäuse, E3-GUL2"]
[null,234677,"Aufputzgehäuse E3-GAL2","On request",null,null,null,null,null,null,null,234677,"Aufputzgehäuse E3-GAL2","On request",false,null,234677,235,"On request","sur demande","på forespørgsel","op aanvraag","Aufputzgehäuse E3-GAL2","Aufputzgehäuse E3-GAL2","Aufputzgehäuse E3-GAL2","Aufputzgehäuse E3-GAL2","Aufputzgehäuse E3-GAL2"]
[null,234678,"Zirkulationspumpe E4-ZP","On request",null,null,null,null,null,null,null,234678,"Zirkulationspumpe E4-ZP","On request",false,null,234678,337,"On request","sur demande","på forespørgsel","op aanvraag","Zirkulationspumpe E4-ZP","Zirkulationspumpe E4-ZP","Zirkulationspumpe E4-ZP","Zirkulationspumpe E4-ZP","Zirkulationspumpe E4-ZP"]
[null,234679,"Montageschiene E5-MS-6","On request",null,null,null,null,null,null,null,234679,"Montageschiene E5-MS-6","On request",false,null,234679,110,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene E5-MS-6","Montageschiene E5-MS-6","Montageschiene E5-MS-6","Montageschiene E5-MS-6","Montageschiene E5-MS-6"]
[null,234680,"Montageschiene E5-MS-7","On request",null,null,null,null,null,null,null,234680,"Montageschiene E5-MS-7","On request",false,null,234680,120,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene E5-MS-7","Montageschiene E5-MS-7","Montageschiene E5-MS-7","Montageschiene E5-MS-7","Montageschiene E5-MS-7"]
[null,234681,"Montageschiene E5-MS-8","On request",null,null,null,null,null,null,null,234681,"Montageschiene E5-MS-8","On request",false,null,234681,140,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene E5-MS-8","Montageschiene E5-MS-8","Montageschiene E5-MS-8","Montageschiene E5-MS-8","Montageschiene E5-MS-8"]
[null,234875,"Montageschiene E5-MS-9","On request",null,null,null,null,null,null,null,234875,"Montageschiene E5-MS-9","On request",false,null,234875,165,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene E5-MS-9","Montageschiene E5-MS-9","Montageschiene E5-MS-9","Montageschiene E5-MS-9","Montageschiene E5-MS-9"]
[null,234682,"Montageschiene E5-MS10","On request",null,null,null,null,null,null,null,234682,"Montageschiene E5-MS10","On request",false,null,234682,175,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene E5-MS10","Montageschiene E5-MS10","Montageschiene E5-MS10","Montageschiene E5-MS10","Montageschiene E5-MS10"]
[null,234683,"Heizkreisverteiler E6-HKV 2","On request",null,null,null,null,null,null,null,234683,"Heizkreisverteiler E6-HKV 2","On request",false,null,234683,350,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 2","Heizkreisverteiler E6-HKV 2","Heizkreisverteiler E6-HKV 2","Heizkreisverteiler E6-HKV 2","Heizkreisverteiler E6-HKV 2"]
[null,234684,"Heizkreisverteiler E6-HKV 3","On request",null,null,null,null,null,null,null,234684,"Heizkreisverteiler E6-HKV 3","On request",false,null,234684,380,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 3","Heizkreisverteiler E6-HKV 3","Heizkreisverteiler E6-HKV 3","Heizkreisverteiler E6-HKV 3","Heizkreisverteiler E6-HKV 3"]
[null,234685,"Heizkreisverteiler E6-HKV 4","On request",null,null,null,null,null,null,null,234685,"Heizkreisverteiler E6-HKV 4","On request",false,null,234685,420,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 4","Heizkreisverteiler E6-HKV 4","Heizkreisverteiler E6-HKV 4","Heizkreisverteiler E6-HKV 4","Heizkreisverteiler E6-HKV 4"]
[null,234686,"Heizkreisverteiler E6-HKV 5","On request",null,null,null,null,null,null,null,234686,"Heizkreisverteiler E6-HKV 5","On request",false,null,234686,450,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 5","Heizkreisverteiler E6-HKV 5","Heizkreisverteiler E6-HKV 5","Heizkreisverteiler E6-HKV 5","Heizkreisverteiler E6-HKV 5"]
[null,234687,"Heizkreisverteiler E6-HKV 6","On request",null,null,null,null,null,null,null,234687,"Heizkreisverteiler E6-HKV 6","On request",false,null,234687,480,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 6","Heizkreisverteiler E6-HKV 6","Heizkreisverteiler E6-HKV 6","Heizkreisverteiler E6-HKV 6","Heizkreisverteiler E6-HKV 6"]
[null,234688,"Heizkreisverteiler E6-HKV 7","On request",null,null,null,null,null,null,null,234688,"Heizkreisverteiler E6-HKV 7","On request",false,null,234688,510,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 7","Heizkreisverteiler E6-HKV 7","Heizkreisverteiler E6-HKV 7","Heizkreisverteiler E6-HKV 7","Heizkreisverteiler E6-HKV 7"]
[null,234689,"Heizkreisverteiler E6-HKV 8","On request",null,null,null,null,null,null,null,234689,"Heizkreisverteiler E6-HKV 8","On request",false,null,234689,540,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 8","Heizkreisverteiler E6-HKV 8","Heizkreisverteiler E6-HKV 8","Heizkreisverteiler E6-HKV 8","Heizkreisverteiler E6-HKV 8"]
[null,234690,"Heizkreisverteiler E6-HKV 9","On request",null,null,null,null,null,null,null,234690,"Heizkreisverteiler E6-HKV 9","On request",false,null,234690,580,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 9","Heizkreisverteiler E6-HKV 9","Heizkreisverteiler E6-HKV 9","Heizkreisverteiler E6-HKV 9","Heizkreisverteiler E6-HKV 9"]
[null,234691,"Heizkreisverteiler E6-HKV 10","On request",null,null,null,null,null,null,null,234691,"Heizkreisverteiler E6-HKV 10","On request",false,null,234691,610,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 10","Heizkreisverteiler E6-HKV 10","Heizkreisverteiler E6-HKV 10","Heizkreisverteiler E6-HKV 10","Heizkreisverteiler E6-HKV 10"]
[null,234692,"Heizkreisverteiler E6-HKV 12","On request",null,null,null,null,null,null,null,234692,"Heizkreisverteiler E6-HKV 12","On request",false,null,234692,650,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler E6-HKV 12","Heizkreisverteiler E6-HKV 12","Heizkreisverteiler E6-HKV 12","Heizkreisverteiler E6-HKV 12","Heizkreisverteiler E6-HKV 12"]
[null,234693,"Wärmedämmung Rohrleitung E7-WDR1","On request",null,null,null,null,null,null,null,234693,"Wärmedämmung Rohrleitung E7-WDR1","On request",false,null,234693,120,"On request","sur demande","på forespørgsel","op aanvraag","Wärmedämmung Rohrleitung E7-WDR1","Wärmedämmung Rohrleitung E7-WDR1","Wärmedämmung Rohrleitung E7-WDR1","Wärmedämmung Rohrleitung E7-WDR1","Wärmedämmung Rohrleitung E7-WDR1"]
[null,234694,"Wärmedämmung Rohrleitung E7-WDR2","On request",null,null,null,null,null,null,null,234694,"Wärmedämmung Rohrleitung E7-WDR2","On request",{"$f":"IF(AND(B1510=L1510,C1510=M1510,D1510=N1510),FALSE,TRUE)","v":false},null,234694,50,"On request","sur demande","på forespørgsel","op aanvraag","Wärmedämmung Rohrleitung E7-WDR2","Wärmedämmung Rohrleitung E7-WDR2","Wärmedämmung Rohrleitung E7-WDR2","Wärmedämmung Rohrleitung E7-WDR2","Wärmedämmung Rohrleitung E7-WDR2"]
[null,234695,"Entleerungsset E8-ES","On request",null,null,null,null,null,null,null,234695,"Entleerungsset E8-ES","On request",false,null,234695,80,"On request","sur demande","på forespørgsel","op aanvraag","Entleerungsset E8-ES","Entleerungsset E8-ES","Entleerungsset E8-ES","Entleerungsset E8-ES","Entleerungsset E8-ES"]
[null,234696,"Anlegetemperaturregler E9-ATR","On request",null,null,null,null,null,null,null,234696,"Anlegetemperaturregler E9-ATR","On request",false,null,234696,98,"On request","sur demande","på forespørgsel","op aanvraag","Anlegetemperaturregler E9-ATR","Anlegetemperaturregler E9-ATR","Anlegetemperaturregler E9-ATR","Anlegetemperaturregler E9-ATR","Anlegetemperaturregler E9-ATR"]
[null,234697,"Reglerklemmleiste  E10-RKL","On request",null,null,null,null,null,null,null,234697,"Reglerklemmleiste  E10-RKL","On request",false,null,234697,195,"On request","sur demande","på forespørgsel","op aanvraag","Reglerklemmleiste  E10-RKL","Reglerklemmleiste  E10-RKL","Reglerklemmleiste  E10-RKL","Reglerklemmleiste  E10-RKL","Reglerklemmleiste  E10-RKL"]
[null,234698,"Kaltwasserzähler Passstück E11-KP","On request",null,null,null,null,null,null,null,234698,"Kaltwasserzähler Passstück E11-KP","On request",false,null,234698,25,"On request","sur demande","på forespørgsel","op aanvraag","Kaltwasserzähler Passstück E11-KP","Kaltwasserzähler Passstück E11-KP","Kaltwasserzähler Passstück E11-KP","Kaltwasserzähler Passstück E11-KP","Kaltwasserzähler Passstück E11-KP"]
[null,234699,"Kaltwasserzähler Passstück E11-KPA","On request",null,null,null,null,null,null,null,234699,"Kaltwasserzähler Passstück E11-KPA","On request",false,null,234699,65,"On request","sur demande","på forespørgsel","op aanvraag","Kaltwasserzähler Passstück E11-KPA","Kaltwasserzähler Passstück E11-KPA","Kaltwasserzähler Passstück E11-KPA","Kaltwasserzähler Passstück E11-KPA","Kaltwasserzähler Passstück E11-KPA"]
[null,234835,"Aufputzgehäuse Z3-GAK1","On request",null,null,null,null,null,null,null,234835,"Aufputzgehäuse Z3-GAK1","On request",false,null,234835,129,"On request","sur demande","på forespørgsel","op aanvraag","Aufputzgehäuse Z3-GAK1","Aufputzgehäuse Z3-GAK1","Aufputzgehäuse Z3-GAK1","Aufputzgehäuse Z3-GAK1","Aufputzgehäuse Z3-GAK1"]
[null,234837,"Aufputzgehäuse Z3-GAK2","On request",null,null,null,null,null,null,null,234837,"Aufputzgehäuse Z3-GAK2","On request",false,null,234837,155,"On request","sur demande","på forespørgsel","op aanvraag","Aufputzgehäuse Z3-GAK2","Aufputzgehäuse Z3-GAK2","Aufputzgehäuse Z3-GAK2","Aufputzgehäuse Z3-GAK2","Aufputzgehäuse Z3-GAK2"]
[null,234838,"Aufputzgehäuse Z3-GAL1","On request",null,null,null,null,null,null,null,234838,"Aufputzgehäuse Z3-GAL1","On request",false,null,234838,180,"On request","sur demande","på forespørgsel","op aanvraag","Aufputzgehäuse Z3-GAL1","Aufputzgehäuse Z3-GAL1","Aufputzgehäuse Z3-GAL1","Aufputzgehäuse Z3-GAL1","Aufputzgehäuse Z3-GAL1"]
[null,234842,"Aufputzgehäuse Z3-GAL2","On request",null,null,null,null,null,null,null,234842,"Aufputzgehäuse Z3-GAL2","On request",false,null,234842,235,"On request","sur demande","på forespørgsel","op aanvraag","Aufputzgehäuse Z3-GAL2","Aufputzgehäuse Z3-GAL2","Aufputzgehäuse Z3-GAL2","Aufputzgehäuse Z3-GAL2","Aufputzgehäuse Z3-GAL2"]
[null,234836,"Unterputzgehäuse Z3-GUK1","On request",null,null,null,null,null,null,null,234836,"Unterputzgehäuse Z3-GUK1","On request",false,null,234836,180,"On request","sur demande","på forespørgsel","op aanvraag","Unterputzgehäuse Z3-GUK1","Unterputzgehäuse Z3-GUK1","Unterputzgehäuse Z3-GUK1","Unterputzgehäuse Z3-GUK1","Unterputzgehäuse Z3-GUK1"]
[null,234839,"Unterputzgehäuse Z3-GUK2","On request",null,null,null,null,null,null,null,234839,"Unterputzgehäuse Z3-GUK2","On request",false,null,234839,190,"On request","sur demande","på forespørgsel","op aanvraag","Unterputzgehäuse Z3-GUK2","Unterputzgehäuse Z3-GUK2","Unterputzgehäuse Z3-GUK2","Unterputzgehäuse Z3-GUK2","Unterputzgehäuse Z3-GUK2"]
[null,234840,"Unterputzgehäuse, Z3-GUL1","On request",null,null,null,null,null,null,null,234840,"Unterputzgehäuse, Z3-GUL1","On request",false,null,234840,260,"On request","sur demande","på forespørgsel","op aanvraag","Unterputzgehäuse, Z3-GUL1","Unterputzgehäuse, Z3-GUL1","Unterputzgehäuse, Z3-GUL1","Unterputzgehäuse, Z3-GUL1","Unterputzgehäuse, Z3-GUL1"]
[null,234841,"Unterputzgehäuse, Z3-GUL2","On request",null,null,null,null,null,null,null,234841,"Unterputzgehäuse, Z3-GUL2","On request",false,null,234841,290,"On request","sur demande","på forespørgsel","op aanvraag","Unterputzgehäuse, Z3-GUL2","Unterputzgehäuse, Z3-GUL2","Unterputzgehäuse, Z3-GUL2","Unterputzgehäuse, Z3-GUL2","Unterputzgehäuse, Z3-GUL2"]
[null,234845,"Montageschiene Z5-MS-6","On request",null,null,null,null,null,null,null,234845,"Montageschiene Z5-MS-6","On request",false,null,234845,110,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene Z5-MS-6","Montageschiene Z5-MS-6","Montageschiene Z5-MS-6","Montageschiene Z5-MS-6","Montageschiene Z5-MS-6"]
[null,234846,"Montageschiene Z5-MS-7","On request",null,null,null,null,null,null,null,234846,"Montageschiene Z5-MS-7","On request",false,null,234846,120,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene Z5-MS-7","Montageschiene Z5-MS-7","Montageschiene Z5-MS-7","Montageschiene Z5-MS-7","Montageschiene Z5-MS-7"]
[null,234847,"Montageschiene Z5-MS-8","On request",null,null,null,null,null,null,null,234847,"Montageschiene Z5-MS-8","On request",false,null,234847,140,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene Z5-MS-8","Montageschiene Z5-MS-8","Montageschiene Z5-MS-8","Montageschiene Z5-MS-8","Montageschiene Z5-MS-8"]
[null,234859,"Montageschiene Z5-MS-9","On request",null,null,null,null,null,null,null,234859,"Montageschiene Z5-MS-9","On request",false,null,234859,165,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene Z5-MS-9","Montageschiene Z5-MS-9","Montageschiene Z5-MS-9","Montageschiene Z5-MS-9","Montageschiene Z5-MS-9"]
[null,234848,"Montageschiene Z5-MS10","On request",null,null,null,null,null,null,null,234848,"Montageschiene Z5-MS10","On request",false,null,234848,175,"On request","sur demande","på forespørgsel","op aanvraag","Montageschiene Z5-MS10","Montageschiene Z5-MS10","Montageschiene Z5-MS10","Montageschiene Z5-MS10","Montageschiene Z5-MS10"]
[null,234849,"Heizkreisverteiler Z6-HKV 2","On request",null,null,null,null,null,null,null,234849,"Heizkreisverteiler Z6-HKV 2","On request",false,null,234849,350,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 2","Heizkreisverteiler Z6-HKV 2","Heizkreisverteiler Z6-HKV 2","Heizkreisverteiler Z6-HKV 2","Heizkreisverteiler Z6-HKV 2"]
[null,234850,"Heizkreisverteiler Z6-HKV 3","On request",null,null,null,null,null,null,null,234850,"Heizkreisverteiler Z6-HKV 3","On request",false,null,234850,380,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 3","Heizkreisverteiler Z6-HKV 3","Heizkreisverteiler Z6-HKV 3","Heizkreisverteiler Z6-HKV 3","Heizkreisverteiler Z6-HKV 3"]
[null,234851,"Heizkreisverteiler Z6-HKV 4","On request",null,null,null,null,null,null,null,234851,"Heizkreisverteiler Z6-HKV 4","On request",false,null,234851,420,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 4","Heizkreisverteiler Z6-HKV 4","Heizkreisverteiler Z6-HKV 4","Heizkreisverteiler Z6-HKV 4","Heizkreisverteiler Z6-HKV 4"]
[null,234852,"Heizkreisverteiler Z6-HKV 5","On request",null,null,null,null,null,null,null,234852,"Heizkreisverteiler Z6-HKV 5","On request",false,null,234852,450,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 5","Heizkreisverteiler Z6-HKV 5","Heizkreisverteiler Z6-HKV 5","Heizkreisverteiler Z6-HKV 5","Heizkreisverteiler Z6-HKV 5"]
[null,234853,"Heizkreisverteiler Z6-HKV 6","On request",null,null,null,null,null,null,null,234853,"Heizkreisverteiler Z6-HKV 6","On request",false,null,234853,480,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 6","Heizkreisverteiler Z6-HKV 6","Heizkreisverteiler Z6-HKV 6","Heizkreisverteiler Z6-HKV 6","Heizkreisverteiler Z6-HKV 6"]
[null,234854,"Heizkreisverteiler Z6-HKV 7","On request",null,null,null,null,null,null,null,234854,"Heizkreisverteiler Z6-HKV 7","On request",false,null,234854,510,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 7","Heizkreisverteiler Z6-HKV 7","Heizkreisverteiler Z6-HKV 7","Heizkreisverteiler Z6-HKV 7","Heizkreisverteiler Z6-HKV 7"]
[null,234855,"Heizkreisverteiler Z6-HKV 8","On request",null,null,null,null,null,null,null,234855,"Heizkreisverteiler Z6-HKV 8","On request",false,null,234855,540,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 8","Heizkreisverteiler Z6-HKV 8","Heizkreisverteiler Z6-HKV 8","Heizkreisverteiler Z6-HKV 8","Heizkreisverteiler Z6-HKV 8"]
[null,234856,"Heizkreisverteiler Z6-HKV 9","On request",null,null,null,null,null,null,null,234856,"Heizkreisverteiler Z6-HKV 9","On request",false,null,234856,580,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 9","Heizkreisverteiler Z6-HKV 9","Heizkreisverteiler Z6-HKV 9","Heizkreisverteiler Z6-HKV 9","Heizkreisverteiler Z6-HKV 9"]
[null,234857,"Heizkreisverteiler Z6-HKV 10","On request",null,null,null,null,null,null,null,234857,"Heizkreisverteiler Z6-HKV 10","On request",false,null,234857,610,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 10","Heizkreisverteiler Z6-HKV 10","Heizkreisverteiler Z6-HKV 10","Heizkreisverteiler Z6-HKV 10","Heizkreisverteiler Z6-HKV 10"]
[null,234858,"Heizkreisverteiler Z6-HKV 12","On request",null,null,null,null,null,null,null,234858,"Heizkreisverteiler Z6-HKV 12","On request",false,null,234858,650,"On request","sur demande","på forespørgsel","op aanvraag","Heizkreisverteiler Z6-HKV 12","Heizkreisverteiler Z6-HKV 12","Heizkreisverteiler Z6-HKV 12","Heizkreisverteiler Z6-HKV 12","Heizkreisverteiler Z6-HKV 12"]
[null,234843,"Netzpumpenmodul NPM 3-G","On request",null,null,null,null,null,null,null,234843,"Netzpumpenmodul NPM 3-G","On request",false,null,234843,3000,"On request","sur demande","på forespørgsel","op aanvraag","Netzpumpenmodul NPM 3-G","Netzpumpenmodul NPM 3-G","Netzpumpenmodul NPM 3-G","Netzpumpenmodul NPM 3-G","Netwerk pompmodule NPM 3-G"]
[null,234844,"Netzpumpenmodul NPM 6-G","On request",null,null,null,null,null,null,null,234844,"Netzpumpenmodul NPM 6-G","On request",false,null,234844,3250,"On request","sur demande","på forespørgsel","op aanvraag","Netzpumpenmodul NPM 6-G","Netzpumpenmodul NPM 6-G","Netzpumpenmodul NPM 6-G","Netzpumpenmodul NPM 6-G","Netwerk pompmodule NPM 6-G"]
[null,234890,"Netzpumpenmodul NPM 10-G","On request",null,null,null,null,null,null,null,234890,"Netzpumpenmodul NPM 10-G","On request",false,null,234890,4650,"On request","sur demande","på forespørgsel","op aanvraag","Netzpumpenmodul NPM 10-G","Netzpumpenmodul NPM 10-G","Netzpumpenmodul NPM 10-G","Netzpumpenmodul NPM 10-G","Netwerk pompmodule NPM 10-G"]
[null,234872,"Netzpumpenmodul NPM 3-U","On request",null,null,null,null,null,null,null,234872,"Netzpumpenmodul NPM 3-U","On request",false,null,234872,2500,"On request","sur demande","på forespørgsel","op aanvraag","Netzpumpenmodul NPM 3-U","Netzpumpenmodul NPM 3-U","Netzpumpenmodul NPM 3-U","Netzpumpenmodul NPM 3-U","Netwerk pompmodule NPM 3-U"]
[null,234873,"Netzpumpenmodul NPM 6-U","On request",null,null,null,null,null,null,null,234873,"Netzpumpenmodul NPM 6-U","On request",false,null,234873,2750,"On request","sur demande","på forespørgsel","op aanvraag","Netzpumpenmodul NPM 6-U","Netzpumpenmodul NPM 6-U","Netzpumpenmodul NPM 6-U","Netzpumpenmodul NPM 6-U","Netwerk pompmodule NPM 6-U"]
[null,234874,"Netzpumpenmodul NPM 10-U","On request",null,null,null,null,null,null,null,234874,"Netzpumpenmodul NPM 10-U","On request",false,null,234874,3800,"On request","sur demande","på forespørgsel","op aanvraag","Netzpumpenmodul NPM 10-U","Netzpumpenmodul NPM 10-U","Netzpumpenmodul NPM 10-U","Netzpumpenmodul NPM 10-U","Netwerk pompmodule NPM 10-U"]
[null,234805,"Regelung für Netzpumpenmodul R1-NPM-G","On request",null,null,null,null,null,null,null,234805,"Regelung für Netzpumpenmodul R1-NPM-G","On request",false,null,234805,890,"On request","sur demande","på forespørgsel","op aanvraag","Regelung für Netzpumpenmodul R1-NPM-G","Regelung für Netzpumpenmodul R1-NPM-G","Regelung für Netzpumpenmodul R1-NPM-G","Regelung für Netzpumpenmodul R1-NPM-G","Regelung für Netzpumpenmodul R1-NPM-G"]
[null,234467,"Durchlauferhitzer DHE Connect 18/21/24","On request",null,null,null,null,null,null,null,234467,"Durchlauferhitzer DHE Connect 18/21/24","On request",false,null,234467,862,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHE Connect 18/21/24","Durchlauferhitzer DHE Connect 18/21/24","Durchlauferhitzer DHE Connect 18/21/24","Durchlauferhitzer DHE Connect 18/21/24","Doorstromer DHE Connect 18/21/24"]
[null,234468,"Durchlauferhitzer DHE Connect 27","On request",null,null,null,null,null,null,null,234468,"Durchlauferhitzer DHE Connect 27","On request",false,null,234468,862,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHE Connect 27","Durchlauferhitzer DHE Connect 27","Durchlauferhitzer DHE Connect 27","Durchlauferhitzer DHE Connect 27","Doorstromer DHE Connect 27"]
[null,234459,"Durchlauferhitzer DHE Touch 18/21/24","On request",null,null,null,null,null,null,null,234459,"Durchlauferhitzer DHE Touch 18/21/24","On request",false,null,234459,762,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHE Touch 18/21/24","Durchlauferhitzer DHE Touch 18/21/24","Durchlauferhitzer DHE Touch 18/21/24","Durchlauferhitzer DHE Touch 18/21/24","Doorstromer DHE Touch 18/21/24"]
[null,234460,"Durchlauferhitzer DHE Touch 27","On request",null,null,null,null,null,null,null,234460,"Durchlauferhitzer DHE Touch 27","On request",false,null,234460,762,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHE Touch 27","Durchlauferhitzer DHE Touch 27","Durchlauferhitzer DHE Touch 27","Durchlauferhitzer DHE Touch 27","Doorstromer DHE Touch 27"]
[null,234832,"Funkfernbedienung Wandgehäuse FFB W Set","On request",null,null,null,null,null,null,null,234832,"Funkfernbedienung Wandgehäuse FFB W Set","On request",false,null,234832,69,"On request","sur demande","på forespørgsel","op aanvraag","Funkfernbedienung Wandgehäuse FFB W Set","Funkfernbedienung Wandgehäuse FFB W Set","Funkfernbedienung Wandgehäuse FFB W Set","Funkfernbedienung Wandgehäuse FFB W Set","Funkfernbedienung Wandgehäuse FFB W Set"]
[null,234475,"Funkfernbedienung Standgehäuse FFB T Set","On request",null,null,null,null,null,null,null,234475,"Funkfernbedienung Standgehäuse FFB T Set","On request",false,null,234475,69,"On request","sur demande","på forespørgsel","op aanvraag","Funkfernbedienung Standgehäuse FFB T Set","Funkfernbedienung Standgehäuse FFB T Set","Funkfernbedienung Standgehäuse FFB T Set","Funkfernbedienung Standgehäuse FFB T Set","Funkfernbedienung Standgehäuse FFB T Set"]
[null,234476,"Funkfernbedienung Standgehäuse FFB T Plus Set","On request",null,null,null,null,null,null,null,234476,"Funkfernbedienung Standgehäuse FFB T Plus Set","On request",false,null,234476,189,"On request","sur demande","på forespørgsel","op aanvraag","Funkfernbedienung Standgehäuse FFB T Plus Set","Funkfernbedienung Standgehäuse FFB T Plus Set","Funkfernbedienung Standgehäuse FFB T Plus Set","Funkfernbedienung Standgehäuse FFB T Plus Set","Funkfernbedienung Standgehäuse FFB T Plus Set"]
[null,234478,"Funkfernbedienung Wandgehäuse FFB 4 EU","On request",null,null,null,null,null,null,null,234478,"Funkfernbedienung Wandgehäuse FFB 4 EU","On request",false,null,234478,69,"On request","sur demande","på forespørgsel","op aanvraag","Funkfernbedienung Wandgehäuse FFB 4 EU","Funkfernbedienung Wandgehäuse FFB 4 EU","Funkfernbedienung Wandgehäuse FFB 4 EU","Funkfernbedienung Wandgehäuse FFB 4 EU","Funkfernbedienung Wandgehäuse FFB 4 EU"]
[null,232792,"Durchlauferhitzer DCE 11/13 H","On request",null,null,null,null,null,null,null,232792,"Durchlauferhitzer DCE 11/13 H","On request",false,null,232792,236,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DCE 11/13 H","Durchlauferhitzer DCE 11/13 H","Durchlauferhitzer DCE 11/13 H","Durchlauferhitzer DCE 11/13 H","Doorstromer DCE 11/13 H"]
[null,232794,"Durchlauferhitzer DCE 11/13 H + MEKD","On request",null,null,null,null,null,null,null,232794,"Durchlauferhitzer DCE 11/13 H + MEKD","On request",false,null,232794,358,"On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DCE 11/13 H + MEKD","Durchlauferhitzer DCE 11/13 H + MEKD","Durchlauferhitzer DCE 11/13 H + MEKD","Durchlauferhitzer DCE 11/13 H + MEKD","Doorstromer DCE 11/13 H + MEKD"]
[null,231064,"Raumtemperaturregler RTU-S UP","On request",null,null,null,null,null,null,null,231064,"Raumtemperaturregler RTU-S UP","On request",false,null,231064,150,"On request","sur demande","på forespørgsel","op aanvraag","Raumtemperaturregler RTU-S UP","Raumtemperaturregler RTU-S UP","Raumtemperaturregler RTU-S UP","Raumtemperaturregler RTU-S UP","Ruimtetemp. regelaar  RTU-S UP"]
[null,234417,"Funk-Raumtemperaturregler SRC C digital","On request",null,null,null,null,null,null,null,234417,"Funk-Raumtemperaturregler SRC C digital","On request",false,null,234417,168,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC C digital","Funk-Raumtemperaturregler SRC C digital","Funk-Raumtemperaturregler SRC C digital","Funk-Raumtemperaturregler SRC C digital","Funk-Ruimtetemp. regelaar  SRC C digital"]
[null,234418,"Funk-Raumtemperaturregler SRC C analog","On request",null,null,null,null,null,null,null,234418,"Funk-Raumtemperaturregler SRC C analog","On request",false,null,234418,85,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC C analog","Funk-Raumtemperaturregler SRC C analog","Funk-Raumtemperaturregler SRC C analog","Funk-Raumtemperaturregler SRC C analog","Funk-Ruimtetemp. regelaar  SRC C analog"]
[null,234420,"Funk-Raumtemperaturregler SRC R UP","On request",null,null,null,null,null,null,null,234420,"Funk-Raumtemperaturregler SRC R UP","On request",false,null,234420,159,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC R UP","Funk-Raumtemperaturregler SRC R UP","Funk-Raumtemperaturregler SRC R UP","Funk-Raumtemperaturregler SRC R UP","Funk-Ruimtetemp. regelaar  SRC R UP"]
[null,234421,"Funk-Raumtemperaturregler SRC R AP","On request",null,null,null,null,null,null,null,234421,"Funk-Raumtemperaturregler SRC R AP","On request",false,null,234421,107,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC R AP","Funk-Raumtemperaturregler SRC R AP","Funk-Raumtemperaturregler SRC R AP","Funk-Raumtemperaturregler SRC R AP","Funk-Ruimtetemp. regelaar  SRC R AP"]
[null,234422,"Strahlungsheizung Glas-Schwarz RHB 300","On request",null,null,null,null,null,null,null,234422,"Strahlungsheizung Glas-Schwarz RHB 300","On request",false,null,234422,505,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Glas-Schwarz RHB 300","Strahlungsheizung Glas-Schwarz RHB 300","Strahlungsheizung Glas-Schwarz RHB 300","Strahlungsheizung Glas-Schwarz RHB 300","Strahlungsheizung Glas-Schwarz RHB 300"]
[null,234423,"Strahlungsheizung Glas-Schwarz RHB 500","On request",null,null,null,null,null,null,null,234423,"Strahlungsheizung Glas-Schwarz RHB 500","On request",false,null,234423,654,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Glas-Schwarz RHB 500","Strahlungsheizung Glas-Schwarz RHB 500","Strahlungsheizung Glas-Schwarz RHB 500","Strahlungsheizung Glas-Schwarz RHB 500","Strahlungsheizung Glas-Schwarz RHB 500"]
[null,234424,"Strahlungsheizung Glas-Schwarz RHB 700","On request",null,null,null,null,null,null,null,234424,"Strahlungsheizung Glas-Schwarz RHB 700","On request",false,null,234424,788,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Glas-Schwarz RHB 700","Strahlungsheizung Glas-Schwarz RHB 700","Strahlungsheizung Glas-Schwarz RHB 700","Strahlungsheizung Glas-Schwarz RHB 700","Strahlungsheizung Glas-Schwarz RHB 700"]
[null,234425,"Strahlungsheizung Glas-Schwarz RHB 900","On request",null,null,null,null,null,null,null,234425,"Strahlungsheizung Glas-Schwarz RHB 900","On request",false,null,234425,929,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Glas-Schwarz RHB 900","Strahlungsheizung Glas-Schwarz RHB 900","Strahlungsheizung Glas-Schwarz RHB 900","Strahlungsheizung Glas-Schwarz RHB 900","Strahlungsheizung Glas-Schwarz RHB 900"]
[null,234426,"Strahlungsheizung Glas-Weiß RHW 300","On request",null,null,null,null,null,null,null,234426,"Strahlungsheizung Glas-Weiß RHW 300","On request",false,null,234426,505,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Glas-Weiß RHW 300","Strahlungsheizung Glas-Weiß RHW 300","Strahlungsheizung Glas-Weiß RHW 300","Strahlungsheizung Glas-Weiß RHW 300","Strahlungsheizung Glas-Weiß RHW 300"]
[null,234427,"Strahlungsheizung Glas-Weiß RHW 500","On request",null,null,null,null,null,null,null,234427,"Strahlungsheizung Glas-Weiß RHW 500","On request",false,null,234427,654,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Glas-Weiß RHW 500","Strahlungsheizung Glas-Weiß RHW 500","Strahlungsheizung Glas-Weiß RHW 500","Strahlungsheizung Glas-Weiß RHW 500","Strahlungsheizung Glas-Weiß RHW 500"]
[null,234428,"Strahlungsheizung Glas-Weiß RHW 700","On request",null,null,null,null,null,null,null,234428,"Strahlungsheizung Glas-Weiß RHW 700","On request",false,null,234428,788,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Glas-Weiß RHW 700","Strahlungsheizung Glas-Weiß RHW 700","Strahlungsheizung Glas-Weiß RHW 700","Strahlungsheizung Glas-Weiß RHW 700","Strahlungsheizung Glas-Weiß RHW 700"]
[null,234429,"Strahlungsheizung Glas-Weiß RHW 900","On request",null,null,null,null,null,null,null,234429,"Strahlungsheizung Glas-Weiß RHW 900","On request",false,null,234429,929,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Glas-Weiß RHW 900","Strahlungsheizung Glas-Weiß RHW 900","Strahlungsheizung Glas-Weiß RHW 900","Strahlungsheizung Glas-Weiß RHW 900","Strahlungsheizung Glas-Weiß RHW 900"]
[null,234430,"Strahlungsheizung Spiegel RHM 300","On request",null,null,null,null,null,null,null,234430,"Strahlungsheizung Spiegel RHM 300","On request",false,null,234430,608,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Spiegel RHM 300","Strahlungsheizung Spiegel RHM 300","Strahlungsheizung Spiegel RHM 300","Strahlungsheizung Spiegel RHM 300","Strahlungsheizung Spiegel RHM 300"]
[null,234431,"Strahlungsheizung Spiegel RHM 500","On request",null,null,null,null,null,null,null,234431,"Strahlungsheizung Spiegel RHM 500","On request",false,null,234431,877,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Spiegel RHM 500","Strahlungsheizung Spiegel RHM 500","Strahlungsheizung Spiegel RHM 500","Strahlungsheizung Spiegel RHM 500","Strahlungsheizung Spiegel RHM 500"]
[null,234432,"Strahlungsheizung Spiegel RHM 700","On request",null,null,null,null,null,null,null,234432,"Strahlungsheizung Spiegel RHM 700","On request",false,null,234432,1152,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Spiegel RHM 700","Strahlungsheizung Spiegel RHM 700","Strahlungsheizung Spiegel RHM 700","Strahlungsheizung Spiegel RHM 700","Strahlungsheizung Spiegel RHM 700"]
[null,234433,"Strahlungsheizung Spiegel RHM 900","On request",null,null,null,null,null,null,null,234433,"Strahlungsheizung Spiegel RHM 900","On request",false,null,234433,1415,"On request","sur demande","på forespørgsel","op aanvraag","Strahlungsheizung Spiegel RHM 900","Strahlungsheizung Spiegel RHM 900","Strahlungsheizung Spiegel RHM 900","Strahlungsheizung Spiegel RHM 900","Strahlungsheizung Spiegel RHM 900"]
[null,231064,"Raumtemperaturregler RTU-S UP","On request",null,null,null,null,null,null,null,231064,"Raumtemperaturregler RTU-S UP","On request",false,null,231064,150,"On request","sur demande","på forespørgsel","op aanvraag","Raumtemperaturregler RTU-S UP","Raumtemperaturregler RTU-S UP","Raumtemperaturregler RTU-S UP","Raumtemperaturregler RTU-S UP","Ruimtetemp. regelaar  RTU-S UP"]
[null,234417,"Funk-Raumtemperaturregler SRC C digital","On request",null,null,null,null,null,null,null,234417,"Funk-Raumtemperaturregler SRC C digital","On request",{"$f":"IF(AND(B1574=L1574,C1574=M1574,D1574=N1574),FALSE,TRUE)","v":false},null,234417,168,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC C digital","Funk-Raumtemperaturregler SRC C digital","Funk-Raumtemperaturregler SRC C digital","Funk-Raumtemperaturregler SRC C digital","Funk-Ruimtetemp. regelaar  SRC C digital"]
[null,234418,"Funk-Raumtemperaturregler SRC C analog","On request",null,null,null,null,null,null,null,234418,"Funk-Raumtemperaturregler SRC C analog","On request",false,null,234418,85,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC C analog","Funk-Raumtemperaturregler SRC C analog","Funk-Raumtemperaturregler SRC C analog","Funk-Raumtemperaturregler SRC C analog","Funk-Ruimtetemp. regelaar  SRC C analog"]
[null,234419,"Funk-Raumtemperaturregler SRC R S","On request",null,null,null,null,null,null,null,234419,"Funk-Raumtemperaturregler SRC R S","On request",false,null,234419,159,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC R S","Funk-Raumtemperaturregler SRC R S","Funk-Raumtemperaturregler SRC R S","Funk-Raumtemperaturregler SRC R S","Funk-Ruimtetemp. regelaar  SRC R S"]
[null,234420,"Funk-Raumtemperaturregler SRC R UP","On request",null,null,null,null,null,null,null,234420,"Funk-Raumtemperaturregler SRC R UP","On request",false,null,234420,159,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC R UP","Funk-Raumtemperaturregler SRC R UP","Funk-Raumtemperaturregler SRC R UP","Funk-Raumtemperaturregler SRC R UP","Funk-Ruimtetemp. regelaar  SRC R UP"]
[null,234421,"Funk-Raumtemperaturregler SRC R AP","On request",null,null,null,null,null,null,null,234421,"Funk-Raumtemperaturregler SRC R AP","On request",false,null,234421,107,"On request","sur demande","på forespørgsel","op aanvraag","Funk-Raumtemperaturregler SRC R AP","Funk-Raumtemperaturregler SRC R AP","Funk-Raumtemperaturregler SRC R AP","Funk-Raumtemperaturregler SRC R AP","Funk-Ruimtetemp. regelaar  SRC R AP"]
[null,234287,"Fußbodentemperierung FTT 160 C","On request",null,null,null,null,null,null,null,234287,"Fußbodentemperierung FTT 160 C","On request",false,null,234287,85,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 160 C","Fußbodentemperierung FTT 160 C","Fußbodentemperierung FTT 160 C","Fußbodentemperierung FTT 160 C","Fußbodentemperierung FTT 160 C"]
[null,234288,"Fußbodentemperierung FTT 240 C","On request",null,null,null,null,null,null,null,234288,"Fußbodentemperierung FTT 240 C","On request",false,null,234288,110,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 240 C","Fußbodentemperierung FTT 240 C","Fußbodentemperierung FTT 240 C","Fußbodentemperierung FTT 240 C","Fußbodentemperierung FTT 240 C"]
[null,234289,"Fußbodentemperierung FTT 320 C","On request",null,null,null,null,null,null,null,234289,"Fußbodentemperierung FTT 320 C","On request",false,null,234289,134,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 320 C","Fußbodentemperierung FTT 320 C","Fußbodentemperierung FTT 320 C","Fußbodentemperierung FTT 320 C","Fußbodentemperierung FTT 320 C"]
[null,234290,"Fußbodentemperierung FTT 400 C","On request",null,null,null,null,null,null,null,234290,"Fußbodentemperierung FTT 400 C","On request",false,null,234290,174,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 400 C","Fußbodentemperierung FTT 400 C","Fußbodentemperierung FTT 400 C","Fußbodentemperierung FTT 400 C","Fußbodentemperierung FTT 400 C"]
[null,234291,"Fußbodentemperierung FTT 480 C","On request",null,null,null,null,null,null,null,234291,"Fußbodentemperierung FTT 480 C","On request",false,null,234291,202,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 480 C","Fußbodentemperierung FTT 480 C","Fußbodentemperierung FTT 480 C","Fußbodentemperierung FTT 480 C","Fußbodentemperierung FTT 480 C"]
[null,234292,"Fußbodentemperierung FTT 640 C","On request",null,null,null,null,null,null,null,234292,"Fußbodentemperierung FTT 640 C","On request",false,null,234292,263,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 640 C","Fußbodentemperierung FTT 640 C","Fußbodentemperierung FTT 640 C","Fußbodentemperierung FTT 640 C","Fußbodentemperierung FTT 640 C"]
[null,234293,"Fußbodentemperierung FTT 800 C","On request",null,null,null,null,null,null,null,234293,"Fußbodentemperierung FTT 800 C","On request",false,null,234293,323,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 800 C","Fußbodentemperierung FTT 800 C","Fußbodentemperierung FTT 800 C","Fußbodentemperierung FTT 800 C","Fußbodentemperierung FTT 800 C"]
[null,234294,"Fußbodentemperierung FTT 960 C","On request",null,null,null,null,null,null,null,234294,"Fußbodentemperierung FTT 960 C","On request",false,null,234294,387,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 960 C","Fußbodentemperierung FTT 960 C","Fußbodentemperierung FTT 960 C","Fußbodentemperierung FTT 960 C","Fußbodentemperierung FTT 960 C"]
[null,234295,"Fußbodentemperierung FTT 1120 C","On request",null,null,null,null,null,null,null,234295,"Fußbodentemperierung FTT 1120 C","On request",false,null,234295,451,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTT 1120 C","Fußbodentemperierung FTT 1120 C","Fußbodentemperierung FTT 1120 C","Fußbodentemperierung FTT 1120 C","Fußbodentemperierung FTT 1120 C"]
[null,234834,"Fußbodentemperierung FTB 160","On request",null,null,null,null,null,null,null,234834,"Fußbodentemperierung FTB 160","On request",false,null,234834,96,"On request","sur demande","på forespørgsel","op aanvraag","Fußbodentemperierung FTB 160","Fußbodentemperierung FTB 160","Fußbodentemperierung FTB 160","Fußbodentemperierung FTB 160","Fußbodentemperierung FTB 160"]
[null,233882,"Infrarot-Heizstrahler IA 2054 extreme","On request",null,null,null,null,null,null,null,233882,"Infrarot-Heizstrahler IA 2054 extreme","On request",false,null,233882,365,"On request","sur demande","på forespørgsel","op aanvraag","Infrarot-Heizstrahler IA 2054 extreme","Infrarot-Heizstrahler IA 2054 extreme","Infrarot-Heizstrahler IA 2054 extreme","Infrarot-Heizstrahler IA 2054 extreme","Infrarot-Heizstrahler IA 2054 extreme"]
[null,233889,"Infrarot-Heizstrahler IA 2024 outdoor","On request",null,null,null,null,null,null,null,233889,"Infrarot-Heizstrahler IA 2024 outdoor","On request",false,null,233889,269,"On request","sur demande","på forespørgsel","op aanvraag","Infrarot-Heizstrahler IA 2024 outdoor","Infrarot-Heizstrahler IA 2024 outdoor","Infrarot-Heizstrahler IA 2024 outdoor","Infrarot-Heizstrahler IA 2024 outdoor","Infrarot-Heizstrahler IA 2024 outdoor"]
[null,233875,"Funkempfänger für Infrarot-Heizstrahler IA","On request",null,null,null,null,null,null,null,233875,"Funkempfänger für Infrarot-Heizstrahler IA","On request",false,null,233875,200,"On request","sur demande","på forespørgsel","op aanvraag","Funkempfänger für Infrarot-Heizstrahler IA","Funkempfänger für Infrarot-Heizstrahler IA","Funkempfänger für Infrarot-Heizstrahler IA","Funkempfänger für Infrarot-Heizstrahler IA","Funkempfänger für Infrarot-Heizstrahler IA"]
[null,234728,"Fernbedienung für Infrarot-Heizstrahler IA","On request",null,null,null,null,null,null,null,234728,"Fernbedienung für Infrarot-Heizstrahler IA","On request",false,null,234728,109,"On request","sur demande","på forespørgsel","op aanvraag","Fernbedienung für Infrarot-Heizstrahler IA","Fernbedienung für Infrarot-Heizstrahler IA","Fernbedienung für Infrarot-Heizstrahler IA","Fernbedienung für Infrarot-Heizstrahler IA","Fernbedienung für Infrarot-Heizstrahler IA"]
[null,317118,"Planungsleistung Lüftungstechnik 2D","On request",null,null,null,null,null,null,null,317118,"Planungsleistung Lüftungstechnik 2D","On request",false,null,317118,240,"On request","sur demande","på forespørgsel","op aanvraag","Planungsleistung Lüftungstechnik 2D","Planungsleistung Lüftungstechnik 2D","Planungsleistung Lüftungstechnik 2D","Planungsleistung Lüftungstechnik 2D","Planungsleistung Lüftungstechnik 2D"]
[null,317028,"Inbetriebnahme Lüftungsanlage Fremdhersteller","On request",null,null,null,null,null,null,null,317028,"Inbetriebnahme Lüftungsanlage Fremdhersteller","On request",false,null,317028,200,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Lüftungsanlage Fremdhersteller","Inbetriebnahme Lüftungsanlage Fremdhersteller","Inbetriebnahme Lüftungsanlage Fremdhersteller","Inbetriebnahme Lüftungsanlage Fremdhersteller","Inbetriebnahme Lüftungsanlage Fremdhersteller"]
[null,315441,"Inbetriebnahme ISG mit EMI und SMA","On request",null,null,null,null,null,null,null,315441,"Inbetriebnahme ISG mit EMI und SMA","On request",false,null,315441,480,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme ISG mit EMI und SMA","Inbetriebnahme ISG mit EMI und SMA","Inbetriebnahme ISG mit EMI und SMA","Inbetriebnahme ISG mit EMI und SMA","Inbetriebnahme ISG mit EMI und SMA"]
[null,315442,"Inbetriebnahme ISG plus mit SG ready","On request",null,null,null,null,null,null,null,315442,"Inbetriebnahme ISG plus mit SG ready","On request",false,null,315442,180,"On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme ISG plus mit SG ready","Inbetriebnahme ISG plus mit SG ready","Inbetriebnahme ISG plus mit SG ready","Inbetriebnahme ISG plus mit SG ready","Inbetriebnahme ISG plus mit SG ready"]
[null,317839,"ISG Webmonitoring für Fachhandwerker","On request",null,null,null,null,null,null,null,317839,"ISG Webmonitoring für Fachhandwerker","On request",false,null,317839,159,"On request","sur demande","på forespørgsel","op aanvraag","ISG Webmonitoring für Fachhandwerker","ISG Webmonitoring für Fachhandwerker","ISG Webmonitoring für Fachhandwerker","ISG Webmonitoring für Fachhandwerker","ISG Webmonitoring für Fachhandwerker"]
[null,316303,"Modbus TCP/IP Software für ISG web","On request",null,null,null,null,null,null,null,316303,"Modbus TCP/IP Software für ISG web","On request",false,null,316303,290,"On request","sur demande","på forespørgsel","op aanvraag","Modbus TCP/IP Software für ISG web","Modbus TCP/IP Software für ISG web","Modbus TCP/IP Software für ISG web","Modbus TCP/IP Software für ISG web","Modbus TCP/IP Software für ISG web"]
[null,313743,"Inbetriebnahme SBP 750/950 G","On request",null,null,null,null,null,null,null,313743,"Inbetriebnahme SBP 750/950 G","On request",false,null,313743,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme SBP 750/950 G","Inbetriebnahme SBP 750/950 G","Inbetriebnahme SBP 750/950 G","Inbetriebnahme SBP 750/950 G","Inbetriebnahme SBP 750/950 G"]
[null,313328,"Inbetriebnahme Netzpumpenmodul","On request",null,null,null,null,null,null,null,313328,"Inbetriebnahme Netzpumpenmodul","On request",false,null,313328,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Netzpumpenmodul","Inbetriebnahme Netzpumpenmodul","Inbetriebnahme Netzpumpenmodul","Inbetriebnahme Netzpumpenmodul","Inbetriebnahme Netzpumpenmodul"]
[null,313329,"Inbetriebnahme Wohnungsstation","On request",null,null,null,null,null,null,null,313329,"Inbetriebnahme Wohnungsstation","On request",false,null,313329,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Inbetriebnahme Wohnungsstation","Inbetriebnahme Wohnungsstation","Inbetriebnahme Wohnungsstation","Inbetriebnahme Wohnungsstation","Inbetriebnahme Wärmeübergabestation"]
[null,317840,"Wartungsvertrag Wärmepumpe (Jahresbeitrag)","On request",null,null,null,null,null,null,null,317840,"Wartungsvertrag Wärmepumpe (Jahresbeitrag)","On request",false,null,317840,180,"On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag Wärmepumpe (Jahresbeitrag)","Wartungsvertrag Wärmepumpe (Jahresbeitrag)","Wartungsvertrag Wärmepumpe (Jahresbeitrag)","Wartungsvertrag Wärmepumpe (Jahresbeitrag)","Wartungsvertrag Wärmepumpe (Jahresbeitrag)"]
[null,317841,"Wartungsvertrag Lüftungsintegralgerät (Jahresbeitrag)","On request",null,null,null,null,null,null,null,317841,"Wartungsvertrag Lüftungsintegralgerät (Jahresbeitrag)","On request",false,null,317841,210,"On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag Lüftungsintegralgerät (Jahresbeitrag)","Wartungsvertrag Lüftungsintegralgerät (Jahresbeitrag)","Wartungsvertrag Lüftungsintegralgerät (Jahresbeitrag)","Wartungsvertrag Lüftungsintegralgerät (Jahresbeitrag)","Wartungsvertrag Lüftungsintegralgerät (Jahresbeitrag)"]
[null,317842,"Wartungsvertrag-Plus Wärmepumpe (Jahresbeitrag)","On request",null,null,null,null,null,null,null,317842,"Wartungsvertrag-Plus Wärmepumpe (Jahresbeitrag)","On request",false,null,317842,200,"On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag-Plus Wärmepumpe (Jahresbeitrag)","Wartungsvertrag-Plus Wärmepumpe (Jahresbeitrag)","Wartungsvertrag-Plus Wärmepumpe (Jahresbeitrag)","Wartungsvertrag-Plus Wärmepumpe (Jahresbeitrag)","Wartungsvertrag-Plus Wärmepumpe (Jahresbeitrag)"]
[null,317843,"Wartungsvertrag-Plus Lüftungsintegralgerät (Jahresbeitrag)","On request",null,null,null,null,null,null,null,317843,"Wartungsvertrag-Plus Lüftungsintegralgerät (Jahresbeitrag)","On request",false,null,317843,240,"On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag-Plus Lüftungsintegralgerät (Jahresbeitrag)","Wartungsvertrag-Plus Lüftungsintegralgerät (Jahresbeitrag)","Wartungsvertrag-Plus Lüftungsintegralgerät (Jahresbeitrag)","Wartungsvertrag-Plus Lüftungsintegralgerät (Jahresbeitrag)","Wartungsvertrag-Plus Lüftungsintegralgerät (Jahresbeitrag)"]
[null,317844,"Rund-um-Sorglos' Wärmepumpe (Jahresbeitrag)","On request",null,null,null,null,null,null,null,317844,"Rund-um-Sorglos' Wärmepumpe (Jahresbeitrag)","On request",false,null,317844,250,"On request","sur demande","på forespørgsel","op aanvraag","Rund-um-Sorglos' Wärmepumpe (Jahresbeitrag)","Rund-um-Sorglos' Wärmepumpe (Jahresbeitrag)","Rund-um-Sorglos' Wärmepumpe (Jahresbeitrag)","Rund-um-Sorglos' Wärmepumpe (Jahresbeitrag)","Rund-um-Sorglos' Wärmepumpe (Jahresbeitrag)"]
[null,317845,"Rund-um-Sorglos' Lüftungsintegralgerät (Jahresbeitrag)","On request",null,null,null,null,null,null,null,317845,"Rund-um-Sorglos' Lüftungsintegralgerät (Jahresbeitrag)","On request",false,null,317845,290,"On request","sur demande","på forespørgsel","op aanvraag","Rund-um-Sorglos' Lüftungsintegralgerät (Jahresbeitrag)","Rund-um-Sorglos' Lüftungsintegralgerät (Jahresbeitrag)","Rund-um-Sorglos' Lüftungsintegralgerät (Jahresbeitrag)","Rund-um-Sorglos' Lüftungsintegralgerät (Jahresbeitrag)","Rund-um-Sorglos' Lüftungsintegralgerät (Jahresbeitrag)"]
[null,317846,"Dichtigkeitsprüfung Heizungsanlage","On request",null,null,null,null,null,null,null,317846,"Dichtigkeitsprüfung Heizungsanlage","On request",false,null,317846,90,"On request","sur demande","på forespørgsel","op aanvraag","Dichtigkeitsprüfung Heizungsanlage","Dichtigkeitsprüfung Heizungsanlage","Dichtigkeitsprüfung Heizungsanlage","Dichtigkeitsprüfung Heizungsanlage","Dichtigkeitsprüfung Heizungsanlage"]
[null,294265,"Wartungsvertrag WPC/WPF (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294265,"Wartungsvertrag WPC/WPF (Jahresbeitrag)","On request",false,null,294265,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag WPC/WPF (Jahresbeitrag)","Wartungsvertrag WPC/WPF (Jahresbeitrag)","Wartungsvertrag WPC/WPF (Jahresbeitrag)","Wartungsvertrag WPC/WPF (Jahresbeitrag)","Wartungsvertrag WPC/WPF (Jahresbeitrag)"]
[null,294266,"Wartungsvertrag WPC/WPF Folgemodul (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294266,"Wartungsvertrag WPC/WPF Folgemodul (Jahresbeitrag)","On request",false,null,294266,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag WPC/WPF Folgemodul (Jahresbeitrag)","Wartungsvertrag WPC/WPF Folgemodul (Jahresbeitrag)","Wartungsvertrag WPC/WPF Folgemodul (Jahresbeitrag)","Wartungsvertrag WPC/WPF Folgemodul (Jahresbeitrag)","Wartungsvertrag WPC/WPF Folgemodul (Jahresbeitrag)"]
[null,294267,"Wartungsvertrag WPF-G / WPL-G (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294267,"Wartungsvertrag WPF-G / WPL-G (Jahresbeitrag)","On request",false,null,294267,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag WPF-G / WPL-G (Jahresbeitrag)","Wartungsvertrag WPF-G / WPL-G (Jahresbeitrag)","Wartungsvertrag WPF-G / WPL-G (Jahresbeitrag)","Wartungsvertrag WPF-G / WPL-G (Jahresbeitrag)","Wartungsvertrag WPF-G / WPL-G (Jahresbeitrag)"]
[null,294268,"Wartungsvertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294268,"Wartungsvertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","On request",false,null,294268,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","Wartungsvertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","Wartungsvertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","Wartungsvertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","Wartungsvertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)"]
[null,294269,"Wartungsvertrag WPL (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294269,"Wartungsvertrag WPL (Jahresbeitrag)","On request",false,null,294269,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag WPL (Jahresbeitrag)","Wartungsvertrag WPL (Jahresbeitrag)","Wartungsvertrag WPL (Jahresbeitrag)","Wartungsvertrag WPL (Jahresbeitrag)","Wartungsvertrag WPL (Jahresbeitrag)"]
[null,294270,"Wartungsvertrag WPL Folgemodul (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294270,"Wartungsvertrag WPL Folgemodul (Jahresbeitrag)","On request",false,null,294270,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag WPL Folgemodul (Jahresbeitrag)","Wartungsvertrag WPL Folgemodul (Jahresbeitrag)","Wartungsvertrag WPL Folgemodul (Jahresbeitrag)","Wartungsvertrag WPL Folgemodul (Jahresbeitrag)","Wartungsvertrag WPL Folgemodul (Jahresbeitrag)"]
[null,294271,"Wartungsvertrag LWZ 304/404 (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294271,"Wartungsvertrag LWZ 304/404 (Jahresbeitrag)","On request",false,null,294271,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag LWZ 304/404 (Jahresbeitrag)","Wartungsvertrag LWZ 304/404 (Jahresbeitrag)","Wartungsvertrag LWZ 304/404 (Jahresbeitrag)","Wartungsvertrag LWZ 304/404 (Jahresbeitrag)","Wartungsvertrag LWZ 304/404 (Jahresbeitrag)"]
[null,313455,"Wartungsvertrag LWZ 304/404, LWA 403 Folgemodul (Jahresbeitrag)","On request",null,null,null,null,null,null,null,313455,"Wartungsvertrag LWZ 304/404, LWA 403 Folgemodul (Jahresbeitrag)","On request",false,null,313455,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag LWZ 304/404, LWA 403 Folgemodul (Jahresbeitrag)","Wartungsvertrag LWZ 304/404, LWA 403 Folgemodul (Jahresbeitrag)","Wartungsvertrag LWZ 304/404, LWA 403 Folgemodul (Jahresbeitrag)","Wartungsvertrag LWZ 304/404, LWA 403 Folgemodul (Jahresbeitrag)","Wartungsvertrag LWZ 304/404, LWA 403 Folgemodul (Jahresbeitrag)"]
[null,304059,"Wartungsvertrag LWA 100, LWA 252 (Jahresbeitrag)","On request",null,null,null,null,null,null,null,304059,"Wartungsvertrag LWA 100, LWA 252 (Jahresbeitrag)","On request",false,null,304059,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag LWA 100, LWA 252 (Jahresbeitrag)","Wartungsvertrag LWA 100, LWA 252 (Jahresbeitrag)","Wartungsvertrag LWA 100, LWA 252 (Jahresbeitrag)","Wartungsvertrag LWA 100, LWA 252 (Jahresbeitrag)","Wartungsvertrag LWA 100, LWA 252 (Jahresbeitrag)"]
[null,304060,"Wartungsvertrag LWZ 70…370 (Jahresbeitrag)","On request",null,null,null,null,null,null,null,304060,"Wartungsvertrag LWZ 70…370 (Jahresbeitrag)","On request",false,null,304060,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag LWZ 70…370 (Jahresbeitrag)","Wartungsvertrag LWZ 70…370 (Jahresbeitrag)","Wartungsvertrag LWZ 70…370 (Jahresbeitrag)","Wartungsvertrag LWZ 70…370 (Jahresbeitrag)","Wartungsvertrag LWZ 70…370 (Jahresbeitrag)"]
[null,313326,"Wartungsvertrag LWZ 70…370 mit WP (Jahresbeitrag)","On request",null,null,null,null,null,null,null,313326,"Wartungsvertrag LWZ 70…370 mit WP (Jahresbeitrag)","On request",false,null,313326,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag LWZ 70…370 mit WP (Jahresbeitrag)","Wartungsvertrag LWZ 70…370 mit WP (Jahresbeitrag)","Wartungsvertrag LWZ 70…370 mit WP (Jahresbeitrag)","Wartungsvertrag LWZ 70…370 mit WP (Jahresbeitrag)","Wartungsvertrag LWZ 70…370 mit WP (Jahresbeitrag)"]
[null,304061,"Wartungsvertrag Klima Außengerät (Jahresbeitrag)","On request",null,null,null,null,null,null,null,304061,"Wartungsvertrag Klima Außengerät (Jahresbeitrag)","On request",false,null,304061,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag Klima Außengerät (Jahresbeitrag)","Wartungsvertrag Klima Außengerät (Jahresbeitrag)","Wartungsvertrag Klima Außengerät (Jahresbeitrag)","Wartungsvertrag Klima Außengerät (Jahresbeitrag)","Wartungsvertrag Klima Außengerät (Jahresbeitrag)"]
[null,313327,"Wartungsvertrag Klima weiteres Außengerät (Jahresbeitrag)","On request",null,null,null,null,null,null,null,313327,"Wartungsvertrag Klima weiteres Außengerät (Jahresbeitrag)","On request",false,null,313327,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag Klima weiteres Außengerät (Jahresbeitrag)","Wartungsvertrag Klima weiteres Außengerät (Jahresbeitrag)","Wartungsvertrag Klima weiteres Außengerät (Jahresbeitrag)","Wartungsvertrag Klima weiteres Außengerät (Jahresbeitrag)","Wartungsvertrag Klima weiteres Außengerät (Jahresbeitrag)"]
[null,304062,"Wartungsvertrag Klima Innengerät (Jahresbeitrag)","On request",null,null,null,null,null,null,null,304062,"Wartungsvertrag Klima Innengerät (Jahresbeitrag)","On request",false,null,304062,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wartungsvertrag Klima Innengerät (Jahresbeitrag)","Wartungsvertrag Klima Innengerät (Jahresbeitrag)","Wartungsvertrag Klima Innengerät (Jahresbeitrag)","Wartungsvertrag Klima Innengerät (Jahresbeitrag)","Wartungsvertrag Klima Innengerät (Jahresbeitrag)"]
[null,294248,"Servicevertrag WPC/WPF (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294248,"Servicevertrag WPC/WPF (Jahresbeitrag)","On request",false,null,294248,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPC/WPF (Jahresbeitrag)","Servicevertrag WPC/WPF (Jahresbeitrag)","Servicevertrag WPC/WPF (Jahresbeitrag)","Servicevertrag WPC/WPF (Jahresbeitrag)","Servicevertrag WPC/WPF (Jahresbeitrag)"]
[null,294250,"Servicevertrag WPC/WPF (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,294250,"Servicevertrag WPC/WPF (Monatl. Beitrag)","On request",false,null,294250,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPC/WPF (Monatl. Beitrag)","Servicevertrag WPC/WPF (Monatl. Beitrag)","Servicevertrag WPC/WPF (Monatl. Beitrag)","Servicevertrag WPC/WPF (Monatl. Beitrag)","Servicevertrag WPC/WPF (Monatl. Beitrag)"]
[null,294251,"Servicevertrag WPC/WPF Folgemodul (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294251,"Servicevertrag WPC/WPF Folgemodul (Jahresbeitrag)","On request",false,null,294251,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPC/WPF Folgemodul (Jahresbeitrag)","Servicevertrag WPC/WPF Folgemodul (Jahresbeitrag)","Servicevertrag WPC/WPF Folgemodul (Jahresbeitrag)","Servicevertrag WPC/WPF Folgemodul (Jahresbeitrag)","Servicevertrag WPC/WPF Folgemodul (Jahresbeitrag)"]
[null,294252,"Servicevertrag WPC/WPF Folgemodul (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,294252,"Servicevertrag WPC/WPF Folgemodul (Monatl. Beitrag)","On request",false,null,294252,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPC/WPF Folgemodul (Monatl. Beitrag)","Servicevertrag WPC/WPF Folgemodul (Monatl. Beitrag)","Servicevertrag WPC/WPF Folgemodul (Monatl. Beitrag)","Servicevertrag WPC/WPF Folgemodul (Monatl. Beitrag)","Servicevertrag WPC/WPF Folgemodul (Monatl. Beitrag)"]
[null,294253,"Servicevertrag WPF-G / WPL-G (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294253,"Servicevertrag WPF-G / WPL-G (Jahresbeitrag)","On request",false,null,294253,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPF-G / WPL-G (Jahresbeitrag)","Servicevertrag WPF-G / WPL-G (Jahresbeitrag)","Servicevertrag WPF-G / WPL-G (Jahresbeitrag)","Servicevertrag WPF-G / WPL-G (Jahresbeitrag)","Servicevertrag WPF-G / WPL-G (Jahresbeitrag)"]
[null,294255,"Servicevertrag WPF-G / WPL-G (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,294255,"Servicevertrag WPF-G / WPL-G (Monatl. Beitrag)","On request",false,null,294255,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPF-G / WPL-G (Monatl. Beitrag)","Servicevertrag WPF-G / WPL-G (Monatl. Beitrag)","Servicevertrag WPF-G / WPL-G (Monatl. Beitrag)","Servicevertrag WPF-G / WPL-G (Monatl. Beitrag)","Servicevertrag WPF-G / WPL-G (Monatl. Beitrag)"]
[null,294256,"Servicevertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294256,"Servicevertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","On request",false,null,294256,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","Servicevertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","Servicevertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","Servicevertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)","Servicevertrag WPF-G / WPL-G Folgemodul (Jahresbeitrag)"]
[null,294257,"Servicevertrag WPF-G / WPL-G Folgemodul (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,294257,"Servicevertrag WPF-G / WPL-G Folgemodul (Monatl. Beitrag)","On request",false,null,294257,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPF-G / WPL-G Folgemodul (Monatl. Beitrag)","Servicevertrag WPF-G / WPL-G Folgemodul (Monatl. Beitrag)","Servicevertrag WPF-G / WPL-G Folgemodul (Monatl. Beitrag)","Servicevertrag WPF-G / WPL-G Folgemodul (Monatl. Beitrag)","Servicevertrag WPF-G / WPL-G Folgemodul (Monatl. Beitrag)"]
[null,294258,"Servicevertrag WPL (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294258,"Servicevertrag WPL (Jahresbeitrag)","On request",false,null,294258,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPL (Jahresbeitrag)","Servicevertrag WPL (Jahresbeitrag)","Servicevertrag WPL (Jahresbeitrag)","Servicevertrag WPL (Jahresbeitrag)","Servicevertrag WPL (Jahresbeitrag)"]
[null,294259,"Servicevertrag WPL (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,294259,"Servicevertrag WPL (Monatl. Beitrag)","On request",false,null,294259,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPL (Monatl. Beitrag)","Servicevertrag WPL (Monatl. Beitrag)","Servicevertrag WPL (Monatl. Beitrag)","Servicevertrag WPL (Monatl. Beitrag)","Servicevertrag WPL (Monatl. Beitrag)"]
[null,294260,"Servicevertrag WPL Folgemodul (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294260,"Servicevertrag WPL Folgemodul (Jahresbeitrag)","On request",false,null,294260,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPL Folgemodul (Jahresbeitrag)","Servicevertrag WPL Folgemodul (Jahresbeitrag)","Servicevertrag WPL Folgemodul (Jahresbeitrag)","Servicevertrag WPL Folgemodul (Jahresbeitrag)","Servicevertrag WPL Folgemodul (Jahresbeitrag)"]
[null,294261,"Servicevertrag WPL Folgemodul (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,294261,"Servicevertrag WPL Folgemodul (Monatl. Beitrag)","On request",false,null,294261,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WPL Folgemodul (Monatl. Beitrag)","Servicevertrag WPL Folgemodul (Monatl. Beitrag)","Servicevertrag WPL Folgemodul (Monatl. Beitrag)","Servicevertrag WPL Folgemodul (Monatl. Beitrag)","Servicevertrag WPL Folgemodul (Monatl. Beitrag)"]
[null,294262,"Servicevertrag LWZ 304/404 LWA 403 (Jahresbeitrag)","On request",null,null,null,null,null,null,null,294262,"Servicevertrag LWZ 304/404 LWA 403 (Jahresbeitrag)","On request",false,null,294262,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag LWZ 304/404 LWA 403 (Jahresbeitrag)","Servicevertrag LWZ 304/404 LWA 403 (Jahresbeitrag)","Servicevertrag LWZ 304/404 LWA 403 (Jahresbeitrag)","Servicevertrag LWZ 304/404 LWA 403 (Jahresbeitrag)","Servicevertrag LWZ 304/403 LWA 403 (Jahresbeitrag)"]
[null,294263,"Servicevertrag LWZ 304/404 LWA 403 (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,294263,"Servicevertrag LWZ 304/404 LWA 403 (Monatl. Beitrag)","On request",false,null,294263,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag LWZ 304/404 LWA 403 (Monatl. Beitrag)","Servicevertrag LWZ 304/404 LWA 403 (Monatl. Beitrag)","Servicevertrag LWZ 304/404 LWA 403 (Monatl. Beitrag)","Servicevertrag LWZ 304/404 LWA 403 (Monatl. Beitrag)","Servicevertrag LWZ 304/403 LWA 403 (Monatl. Beitrag)"]
[null,304589,"Servicevertrag WWK/WWP (Jahresbeitrag)","On request",null,null,null,null,null,null,null,304589,"Servicevertrag WWK/WWP (Jahresbeitrag)","On request",false,null,304589,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WWK/WWP (Jahresbeitrag)","Servicevertrag WWK/WWP (Jahresbeitrag)","Servicevertrag WWK/WWP (Jahresbeitrag)","Servicevertrag WWK/WWP (Jahresbeitrag)","Servicevertrag WWK/WWP (Jahresbeitrag)"]
[null,304590,"Servicevertrag WWK/WWP (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,304590,"Servicevertrag WWK/WWP (Monatl. Beitrag)","On request",{"$f":"IF(AND(B1638=L1638,C1638=M1638,D1638=N1638),FALSE,TRUE)","v":false},null,304590,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WWK/WWP (Monatl. Beitrag)","Servicevertrag WWK/WWP (Monatl. Beitrag)","Servicevertrag WWK/WWP (Monatl. Beitrag)","Servicevertrag WWK/WWP (Monatl. Beitrag)","Servicevertrag WWK/WWP (Monatl. Beitrag)"]
[null,313323,"Servicevertrag WWK/WWP mit Wärmepumpe (Jahresbeitrag)","On request",null,null,null,null,null,null,null,313323,"Servicevertrag WWK/WWP mit Wärmepumpe (Jahresbeitrag)","On request",false,null,313323,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WWK/WWP mit Wärmepumpe (Jahresbeitrag)","Servicevertrag WWK/WWP mit Wärmepumpe (Jahresbeitrag)","Servicevertrag WWK/WWP mit Wärmepumpe (Jahresbeitrag)","Servicevertrag WWK/WWP mit Wärmepumpe (Jahresbeitrag)","Servicevertrag WWK/WWP mit Wärmepumpe (Jahresbeitrag)"]
[null,313324,"Servicevertrag WWK/WWP mit Wärmepumpe (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,313324,"Servicevertrag WWK/WWP mit Wärmepumpe (Monatl. Beitrag)","On request",false,null,313324,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag WWK/WWP mit Wärmepumpe (Monatl. Beitrag)","Servicevertrag WWK/WWP mit Wärmepumpe (Monatl. Beitrag)","Servicevertrag WWK/WWP mit Wärmepumpe (Monatl. Beitrag)","Servicevertrag WWK/WWP mit Wärmepumpe (Monatl. Beitrag)","Servicevertrag WWK/WWP mit Wärmepumpe (Monatl. Beitrag)"]
[null,304591,"Servicevertrag LWZ 70...370, LWA 252 (Jahresbeitrag)","On request",null,null,null,null,null,null,null,304591,"Servicevertrag LWZ 70...370, LWA 252 (Jahresbeitrag)","On request",false,null,304591,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag LWZ 70...370, LWA 252 (Jahresbeitrag)","Servicevertrag LWZ 70...370, LWA 252 (Jahresbeitrag)","Servicevertrag LWZ 70...370, LWA 252 (Jahresbeitrag)","Servicevertrag LWZ 70...370, LWA 252 (Jahresbeitrag)","Servicevertrag LWZ 70...370, LWA 252 (Jahresbeitrag)"]
[null,304592,"Servicevertrag LWZ 70...370, LWA 252 (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,304592,"Servicevertrag LWZ 70...370, LWA 252 (Monatl. Beitrag)","On request",false,null,304592,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag LWZ 70...370, LWA 252 (Monatl. Beitrag)","Servicevertrag LWZ 70...370, LWA 252 (Monatl. Beitrag)","Servicevertrag LWZ 70...370, LWA 252 (Monatl. Beitrag)","Servicevertrag LWZ 70...370, LWA 252 (Monatl. Beitrag)","Servicevertrag LWZ 70...370, LWA 252 (Monatl. Beitrag)"]
[null,304593,"Servicevertrag LWZ 70...370 mit Wärmepumpe (Jahresbeitrag)","On request",null,null,null,null,null,null,null,304593,"Servicevertrag LWZ 70...370 mit Wärmepumpe (Jahresbeitrag)","On request",false,null,304593,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag LWZ 70...370 mit Wärmepumpe (Jahresbeitrag)","Servicevertrag LWZ 70...370 mit Wärmepumpe (Jahresbeitrag)","Servicevertrag LWZ 70...370 mit Wärmepumpe (Jahresbeitrag)","Servicevertrag LWZ 70...370 mit Wärmepumpe (Jahresbeitrag)","Servicevertrag LWZ 70...370 mit Wärmepumpe (Jahresbeitrag)"]
[null,304594,"Servicevertrag LWZ 70...370 mit Wärmepumpe (Monatl. Beitrag)","On request",null,null,null,null,null,null,null,304594,"Servicevertrag LWZ 70...370 mit Wärmepumpe (Monatl. Beitrag)","On request",false,null,304594,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Servicevertrag LWZ 70...370 mit Wärmepumpe (Monatl. Beitrag)","Servicevertrag LWZ 70...370 mit Wärmepumpe (Monatl. Beitrag)","Servicevertrag LWZ 70...370 mit Wärmepumpe (Monatl. Beitrag)","Servicevertrag LWZ 70...370 mit Wärmepumpe (Monatl. Beitrag)","Servicevertrag LWZ 70...370 mit Wärmepumpe (Monatl. Beitrag)"]
[null,289708,"Garantieverlängerung WP-Bestandsgerät auf 5 Jahre","On request",null,null,null,null,null,null,null,289708,"Garantieverlängerung WP-Bestandsgerät auf 5 Jahre","On request",false,null,289708,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Garantieverlängerung WP-Bestandsgerät auf 5 Jahre","Garantieverlängerung WP-Bestandsgerät auf 5 Jahre","Garantieverlängerung WP-Bestandsgerät auf 5 Jahre","Garantieverlängerung WP-Bestandsgerät auf 5 Jahre","Garantieverlängerung WP-Bestandsgerät auf 5 Jahre"]
[null,294368,"Inspektion Systemtechnik-Anlage","On request",null,null,null,null,null,null,null,294368,"Inspektion Systemtechnik-Anlage","On request",false,null,294368,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Inspektion Systemtechnik-Anlage","Inspektion Systemtechnik-Anlage","Inspektion Systemtechnik-Anlage","Inspektion Systemtechnik-Anlage","Inspektion Systemtechnik-Anlage"]
[null,313325,"Kamera-Inspektion Luftverteilsystem","On request",null,null,null,null,null,null,null,313325,"Kamera-Inspektion Luftverteilsystem","On request",false,null,313325,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Kamera-Inspektion Luftverteilsystem","Kamera-Inspektion Luftverteilsystem","Kamera-Inspektion Luftverteilsystem","Kamera-Inspektion Luftverteilsystem","Kamera-Inspektion Luftverteilsystem"]
[null,293912,"Einmalige Wartung WPC/WPF","On request",null,null,null,null,null,null,null,293912,"Einmalige Wartung WPC/WPF","On request",false,null,293912,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung WPC/WPF","Einmalige Wartung WPC/WPF","Einmalige Wartung WPC/WPF","Einmalige Wartung WPC/WPF","Einmalige Wartung WPC/WPF"]
[null,293913,"Einmalige Wartung WPC/WPF Folgemodul ","On request",null,null,null,null,null,null,null,293913,"Einmalige Wartung WPC/WPF Folgemodul ","On request",false,null,293913,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung WPC/WPF Folgemodul ","Einmalige Wartung WPC/WPF Folgemodul ","Einmalige Wartung WPC/WPF Folgemodul ","Einmalige Wartung WPC/WPF Folgemodul ","Einmalige Wartung WPC/WPF Folgemodul "]
[null,293914,"Einmalige Wartung WPF-G / WPL-G","On request",null,null,null,null,null,null,null,293914,"Einmalige Wartung WPF-G / WPL-G","On request",false,null,293914,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung WPF-G / WPL-G","Einmalige Wartung WPF-G / WPL-G","Einmalige Wartung WPF-G / WPL-G","Einmalige Wartung WPF-G / WPL-G","Einmalige Wartung WPF-G / WPL-G"]
[null,293915,"Einmalige Wartung WPF-G / WPL-G Folgemodul","On request",null,null,null,null,null,null,null,293915,"Einmalige Wartung WPF-G / WPL-G Folgemodul","On request",false,null,293915,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung WPF-G / WPL-G Folgemodul","Einmalige Wartung WPF-G / WPL-G Folgemodul","Einmalige Wartung WPF-G / WPL-G Folgemodul","Einmalige Wartung WPF-G / WPL-G Folgemodul","Einmalige Wartung WPF-G / WPL-G Folgemodul"]
[null,293916,"Einmalige Wartung LWM 250","On request",null,null,null,null,null,null,null,293916,"Einmalige Wartung LWM 250","On request",false,null,293916,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung LWM 250","Einmalige Wartung LWM 250","Einmalige Wartung LWM 250","Einmalige Wartung LWM 250","Einmalige Wartung LWM 250"]
[null,293917,"Einmalige Wartung WPL","On request",null,null,null,null,null,null,null,293917,"Einmalige Wartung WPL","On request",false,null,293917,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung WPL","Einmalige Wartung WPL","Einmalige Wartung WPL","Einmalige Wartung WPL","Einmalige Wartung WPL"]
[null,293918,"Einmalige Wartung WPL Folgemodul","On request",null,null,null,null,null,null,null,293918,"Einmalige Wartung WPL Folgemodul","On request",false,null,293918,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung WPL Folgemodul","Einmalige Wartung WPL Folgemodul","Einmalige Wartung WPL Folgemodul","Einmalige Wartung WPL Folgemodul","Einmalige Wartung WPL Folgemodul"]
[null,293926,"Einmalige Wartung LWZ 304/404, LWA 403","On request",null,null,null,null,null,null,null,293926,"Einmalige Wartung LWZ 304/404, LWA 403","On request",false,null,293926,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung LWZ 304/404, LWA 403","Einmalige Wartung LWZ 304/404, LWA 403","Einmalige Wartung LWZ 304/404, LWA 403","Einmalige Wartung LWZ 304/404, LWA 403","Einmalige Wartung LWZ 304/404, LWA 403"]
[null,293928,"Einmalige Wartung LWZ 70…370","On request",null,null,null,null,null,null,null,293928,"Einmalige Wartung LWZ 70…370","On request",false,null,293928,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung LWZ 70…370","Einmalige Wartung LWZ 70…370","Einmalige Wartung LWZ 70…370","Einmalige Wartung LWZ 70…370","Einmalige Wartung LWZ 70…370"]
[null,293924,"Einmalige Wartung LWA 100, LWA 252","On request",null,null,null,null,null,null,null,293924,"Einmalige Wartung LWA 100, LWA 252","On request",false,null,293924,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung LWA 100, LWA 252","Einmalige Wartung LWA 100, LWA 252","Einmalige Wartung LWA 100, LWA 252","Einmalige Wartung LWA 100, LWA 252","Einmalige Wartung LWA 100, LWA 252"]
[null,293925,"Einmalige Wartung Lüftung (je Ventil)","On request",null,null,null,null,null,null,null,293925,"Einmalige Wartung Lüftung (je Ventil)","On request",false,null,293925,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung Lüftung (je Ventil)","Einmalige Wartung Lüftung (je Ventil)","Einmalige Wartung Lüftung (je Ventil)","Einmalige Wartung Lüftung (je Ventil)","Einmalige Wartung Lüftung (je Ventil)"]
[null,293922,"Einmalige Wartung Klima Außengerät","On request",null,null,null,null,null,null,null,293922,"Einmalige Wartung Klima Außengerät","On request",false,null,293922,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung Klima Außengerät","Einmalige Wartung Klima Außengerät","Einmalige Wartung Klima Außengerät","Einmalige Wartung Klima Außengerät","Einmalige Wartung Klima Außengerät"]
[null,293923,"Einmalige Wartung Klima Innengerät","On request",null,null,null,null,null,null,null,293923,"Einmalige Wartung Klima Innengerät","On request",false,null,293923,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung Klima Innengerät","Einmalige Wartung Klima Innengerät","Einmalige Wartung Klima Innengerät","Einmalige Wartung Klima Innengerät","Einmalige Wartung Klima Innengerät"]
[null,313330,"Einmalige Wartung Netzpumpenmodul","On request",null,null,null,null,null,null,null,313330,"Einmalige Wartung Netzpumpenmodul","On request",false,null,313330,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung Netzpumpenmodul","Einmalige Wartung Netzpumpenmodul","Einmalige Wartung Netzpumpenmodul","Einmalige Wartung Netzpumpenmodul","Einmalige Wartung Netzpumpenmodul"]
[null,313331,"Einmalige Wartung Wohnungsstation","On request",null,null,null,null,null,null,null,313331,"Einmalige Wartung Wohnungsstation","On request",false,null,313331,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Einmalige Wartung Wohnungsstation","Einmalige Wartung Wohnungsstation","Einmalige Wartung Wohnungsstation","Einmalige Wartung Wohnungsstation","Einmalige Wartung Wärmeübergabestation"]
[null,"EWS-01","Bohrung Erdwärmesonde","On request",null,null,null,null,null,null,null,"EWS-01","Bohrung Erdwärmesonde","On request",false,null,"EWS-01","auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Bohrung Erdwärmesonde","Bohrung Erdwärmesonde","Bohrung Erdwärmesonde","Bohrung Erdwärmesonde","Boring aardwarmtesonde"]
[null,"EWS-02","Bohrgutentsorgung","On request",null,null,null,null,null,null,null,"EWS-02","Bohrgutentsorgung","On request",false,null,"EWS-02","auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Bohrgutentsorgung","Bohrgutentsorgung","Bohrgutentsorgung","Bohrgutentsorgung","Booremulsie verwijdering"]
[null,"EWS-03","Anbindung Erdwärmesonde","On request",null,null,null,null,null,null,null,"EWS-03","Anbindung Erdwärmesonde","On request",false,null,"EWS-03","auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Anbindung Erdwärmesonde","Anbindung Erdwärmesonde","Anbindung Erdwärmesonde","Anbindung Erdwärmesonde","Aankoppelen aardwarmtecollector"]
[null,"EWS-04","Soleseitige Inneninstallation","On request",null,null,null,null,null,null,null,"EWS-04","Soleseitige Inneninstallation","On request",false,null,"EWS-04","auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Soleseitige Inneninstallation","Soleseitige Inneninstallation","Soleseitige Inneninstallation","Soleseitige Inneninstallation","Bronzijdige binneninstallatie"]
[null,"EWS-05","Installation mit Solebausatz","On request",null,null,null,null,null,null,null,"EWS-05","Installation mit Solebausatz","On request",false,null,"EWS-05","auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Installation mit Solebausatz","Installation mit Solebausatz","Installation mit Solebausatz","Installation mit Solebausatz","Installatie met pompbouwgroep"]
[null,"Belimo1","Umschaltventil Fa. Belimo Typ H7100N","On request",null,null,null,null,null,null,null,"Belimo1","Umschaltventil Fa. Belimo Typ H7100N","On request",false,null,"Belimo1","bauseits","On request","sur demande","på forespørgsel","bauseits","Umschaltventil Fa. Belimo Typ H7100N","Umschaltventil Fa. Belimo Typ H7100N","Umschaltventil Fa. Belimo Typ H7100N","Umschaltventil Fa. Belimo Typ H7100N","Omschakelventiel Belimo type H7100N"]
[null,"Belimo2","Umschaltventil Fa. Belimo Typ H7125N","On request",null,null,null,null,null,null,null,"Belimo2","Umschaltventil Fa. Belimo Typ H7125N","On request",false,null,"Belimo2","bauseits","On request","sur demande","på forespørgsel","bauseits","Umschaltventil Fa. Belimo Typ H7125N","Umschaltventil Fa. Belimo Typ H7125N","Umschaltventil Fa. Belimo Typ H7125N","Umschaltventil Fa. Belimo Typ H7125N","Omschakelventiel Belimo type H7125N"]
[null,"Belimo3","Umschaltventil Fa. Belimo Typ H7150N","On request",null,null,null,null,null,null,null,"Belimo3","Umschaltventil Fa. Belimo Typ H7150N","On request",false,null,"Belimo3","bauseits","On request","sur demande","på forespørgsel","bauseits","Umschaltventil Fa. Belimo Typ H7150N","Umschaltventil Fa. Belimo Typ H7150N","Umschaltventil Fa. Belimo Typ H7150N","Umschaltventil Fa. Belimo Typ H7150N","Omschakelventiel Belimo type H7150N"]
[null,"Belimo4","Motorantrieb Fa. Belimo Typ AV230-3","On request",null,null,null,null,null,null,null,"Belimo4","Motorantrieb Fa. Belimo Typ AV230-3","On request",false,null,"Belimo4","bauseits","On request","sur demande","på forespørgsel","bauseits","Motorantrieb Fa. Belimo Typ AV230-3","Motorantrieb Fa. Belimo Typ AV230-3","Motorantrieb Fa. Belimo Typ AV230-3","Motorantrieb Fa. Belimo Typ AV230-3","Stelaandrijving Belimo type AV230-3"]
[null,"Belimo5","Heizungs-Umschaltventil","On request",null,null,null,null,null,null,null,"Belimo5","Heizungs-Umschaltventil","On request",false,null,"Belimo5","bauseits","On request","sur demande","på forespørgsel","bauseits","Heizungs-Umschaltventil","Heizungs-Umschaltventil","Heizungs-Umschaltventil","Heizungs-Umschaltventil","Verwarmings-omschakelventiel"]
[null,"Meibes1","Hydraulische Weiche Fa. Meibes Typ MHK 32","On request",null,null,null,null,null,null,null,"Meibes1","Hydraulische Weiche Fa. Meibes Typ MHK 32","On request",false,null,"Meibes1","bauseits","On request","sur demande","på forespørgsel","bauseits","Hydraulische Weiche Fa. Meibes Typ MHK 32","Hydraulische Weiche Fa. Meibes Typ MHK 32","Hydraulische Weiche Fa. Meibes Typ MHK 32","Hydraulische Weiche Fa. Meibes Typ MHK 32","Hydraulische scheiding Fa. Meibes Type MHK 32"]
[null,"SMA-01","Modulwechselrichter SB 240-10","On request",null,null,null,null,null,null,null,"SMA-01","Modulwechselrichter SB 240-10","On request",false,null,"SMA-01","bauseits","On request","sur demande","på forespørgsel","bauseits","Modulwechselrichter SB 240-10","Modulwechselrichter SB 240-10","Modulwechselrichter SB 240-10","Modulwechselrichter SB 240-10","Modulwechselrichter SB 240-10"]
[null,"SMA-02","Kommunikationseinheit Sunny Multigate","On request",null,null,null,null,null,null,null,"SMA-02","Kommunikationseinheit Sunny Multigate","On request",false,null,"SMA-02","bauseits","On request","sur demande","på forespørgsel","bauseits","Kommunikationseinheit Sunny Multigate","Kommunikationseinheit Sunny Multigate","Kommunikationseinheit Sunny Multigate","Kommunikationseinheit Sunny Multigate","Kommunikationseinheit Sunny Multigate"]
[null,"WTG-06","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 59","On request",null,null,null,null,null,null,null,"WTG-06","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 59","On request",false,null,"WTG-06","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 59","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 59","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 59","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 59","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 59"]
[null,"WTG-07","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 67","On request",null,null,null,null,null,null,null,"WTG-07","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 67","On request",false,null,"WTG-07","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 67","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 67","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 67","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 67","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 67"]
[null,"WTG-08","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 75","On request",null,null,null,null,null,null,null,"WTG-08","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 75","On request",false,null,"WTG-08","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 75","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 75","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 75","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 75","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 75"]
[null,"WTG-01","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 78","On request",null,null,null,null,null,null,null,"WTG-01","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 78","On request",false,null,"WTG-01","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 78","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 78","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 78","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 78","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 78"]
[null,"WTG-09","Wärmetauscher Fa. Alfa Laval Typ M6-FM 47","On request",null,null,null,null,null,null,null,"WTG-09","Wärmetauscher Fa. Alfa Laval Typ M6-FM 47","On request",false,null,"WTG-09","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-FM 47","Wärmetauscher Fa. Alfa Laval Typ M6-FM 47","Wärmetauscher Fa. Alfa Laval Typ M6-FM 47","Wärmetauscher Fa. Alfa Laval Typ M6-FM 47","Warmtewisselaar Fa. Alfa Laval Typ M6-FM 47"]
[null,"WTG-02","Wärmetauscher Fa. Alfa Laval Typ M6-FM 53","On request",null,null,null,null,null,null,null,"WTG-02","Wärmetauscher Fa. Alfa Laval Typ M6-FM 53","On request",false,null,"WTG-02","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-FM 53","Wärmetauscher Fa. Alfa Laval Typ M6-FM 53","Wärmetauscher Fa. Alfa Laval Typ M6-FM 53","Wärmetauscher Fa. Alfa Laval Typ M6-FM 53","Warmtewisselaar Fa. Alfa Laval Typ M6-FM 53"]
[null,"WTG-19","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 104","On request",null,null,null,null,null,null,null,"WTG-19","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 104","On request",false,null,"WTG-19","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 104","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 104","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 104","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 104","Warmtewisselaar Fa. Alfa Laval Typ M15-BFM 104"]
[null,"WTG-20","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 146","On request",null,null,null,null,null,null,null,"WTG-20","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 146","On request",false,null,"WTG-20","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 146","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 146","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 146","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 146","Warmtewisselaar Fa. Alfa Laval Typ M15-BFM 146"]
[null,"WTG-03","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 68","On request",null,null,null,null,null,null,null,"WTG-03","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 68","On request",false,null,"WTG-03","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 68","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 68","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 68","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 68","Warmtewisselaar Fa. Alfa Laval Typ TL6-BFM 68"]
[null,"WTG-04","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 92","On request",null,null,null,null,null,null,null,"WTG-04","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 92","On request",false,null,"WTG-04","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 92","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 92","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 92","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 92","Warmtewisselaar Fa. Alfa Laval Typ TL6-BFM 92"]
[null,"WTG-05","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 76","On request",null,null,null,null,null,null,null,"WTG-05","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 76","On request",false,null,"WTG-05","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 76","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 76","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 76","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 76","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 76"]
[null,"WTG-10","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 98","On request",null,null,null,null,null,null,null,"WTG-10","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 98","On request",false,null,"WTG-10","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 98","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 98","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 98","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 98","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 98"]
[null,"WTG-11","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 114","On request",null,null,null,null,null,null,null,"WTG-11","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 114","On request",false,null,"WTG-11","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 114","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 114","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 114","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 114","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 114"]
[null,"WTG-12","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 130","On request",null,null,null,null,null,null,null,"WTG-12","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 130","On request",false,null,"WTG-12","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 130","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 130","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 130","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 130","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 130"]
[null,"WTG-13","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 144","On request",null,null,null,null,null,null,null,"WTG-13","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 144","On request",false,null,"WTG-13","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 144","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 144","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 144","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 144","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 144"]
[null,"WTG-14","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 158","On request",null,null,null,null,null,null,null,"WTG-14","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 158","On request",false,null,"WTG-14","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 158","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 158","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 158","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 158","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 158"]
[null,"WTG-15","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 76","On request",null,null,null,null,null,null,null,"WTG-15","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 76","On request",false,null,"WTG-15","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 76","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 76","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 76","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 76","Warmtewisselaar Fa. Alfa Laval Typ TL6-BFM 76"]
[null,"WTG-16","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 110","On request",null,null,null,null,null,null,null,"WTG-16","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 110","On request",false,null,"WTG-16","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 110","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 110","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 110","Wärmetauscher Fa. Alfa Laval Typ TL6-BFM 110","Warmtewisselaar Fa. Alfa Laval Typ TL6-BFM 110"]
[null,"WTG-17","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 90","On request",null,null,null,null,null,null,null,"WTG-17","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 90","On request",false,null,"WTG-17","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 90","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 90","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 90","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 90","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 90"]
[null,"WTG-18","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 110","On request",null,null,null,null,null,null,null,"WTG-18","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 110","On request",false,null,"WTG-18","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 110","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 110","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 110","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 110","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 110"]
[null,"WTG-21","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 194","On request",null,null,null,null,null,null,null,"WTG-21","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 194","On request",false,null,"WTG-21","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 194","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 194","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 194","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 194","Warmtewisselaar Fa. Alfa Laval Typ M15-BFM 194"]
[null,"WTG-22","Wärmetauscher Fa. Alfa Laval Typ T20-PFG 124","On request",null,null,null,null,null,null,null,"WTG-22","Wärmetauscher Fa. Alfa Laval Typ T20-PFG 124","On request",false,null,"WTG-22","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T20-PFG 124","Wärmetauscher Fa. Alfa Laval Typ T20-PFG 124","Wärmetauscher Fa. Alfa Laval Typ T20-PFG 124","Wärmetauscher Fa. Alfa Laval Typ T20-PFG 124","Warmtewisselaar Fa. Alfa Laval Typ T20-PFG 124"]
[null,"WTP-01","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","On request",null,null,null,null,null,null,null,"WTP-01","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","On request",false,null,"WTP-01","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","Warmtewisselaar Fa. Alfa Laval Typ TL3-PFG 12"]
[null,"WTP-02","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 16","On request",null,null,null,null,null,null,null,"WTP-02","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 16","On request",false,null,"WTP-02","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 16","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 16","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 16","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 16","Warmtewisselaar Fa. Alfa Laval Typ TL3-PFG 16"]
[null,"WTP-03","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 22","On request",null,null,null,null,null,null,null,"WTP-03","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 22","On request",false,null,"WTP-03","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 22","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 22","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 22","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 22","Warmtewisselaar Fa. Alfa Laval Typ TL3-PFG 22"]
[null,"WTP-04","Wärmetauscher Fa. Alfa Laval Typ M3-FG 44","On request",null,null,null,null,null,null,null,"WTP-04","Wärmetauscher Fa. Alfa Laval Typ M3-FG 44","On request",false,null,"WTP-04","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M3-FG 44","Wärmetauscher Fa. Alfa Laval Typ M3-FG 44","Wärmetauscher Fa. Alfa Laval Typ M3-FG 44","Wärmetauscher Fa. Alfa Laval Typ M3-FG 44","Warmtewisselaar Fa. Alfa Laval Typ M3-FG 44"]
[null,"WTP-05","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 26","On request",null,null,null,null,null,null,null,"WTP-05","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 26","On request",{"$f":"IF(AND(B1702=L1702,C1702=M1702,D1702=N1702),FALSE,TRUE)","v":false},null,"WTP-05","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 26","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 26","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 26","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 26","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 26"]
[null,"WTP-06","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 34","On request",null,null,null,null,null,null,null,"WTP-06","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 34","On request",false,null,"WTP-06","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 34","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 34","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 34","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 34","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 34"]
[null,"WTP-07","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 48","On request",null,null,null,null,null,null,null,"WTP-07","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 48","On request",false,null,"WTP-07","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 48","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 48","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 48","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 48","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 48"]
[null,"WTP-08","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 47","On request",null,null,null,null,null,null,null,"WTP-08","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 47","On request",false,null,"WTP-08","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 47","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 47","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 47","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 47","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 47"]
[null,"WTP-09","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 35","On request",null,null,null,null,null,null,null,"WTP-09","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 35","On request",false,null,"WTP-09","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 35","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 35","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 35","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 35","Warmtewisselaar Fa. Alfa Laval Typ M6-MFM 35"]
[null,"WTP-10","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","On request",null,null,null,null,null,null,null,"WTP-10","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","On request",false,null,"WTP-10","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","Warmtewisselaar Fa. Alfa Laval Typ M6-MFM 46"]
[null,"WTP-11","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 58","On request",null,null,null,null,null,null,null,"WTP-11","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 58","On request",false,null,"WTP-11","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 58","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 58","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 58","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 58","Warmtewisselaar Fa. Alfa Laval Typ M6-MFM 58"]
[null,"WTP-12","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 31","On request",null,null,null,null,null,null,null,"WTP-12","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 31","On request",false,null,"WTP-12","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 31","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 31","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 31","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 31","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 31"]
[null,"WTP-13","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 36","On request",null,null,null,null,null,null,null,"WTP-13","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 36","On request",false,null,"WTP-13","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 36","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 36","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 36","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 36","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 36"]
[null,"WTP-14","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 40","On request",null,null,null,null,null,null,null,"WTP-14","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 40","On request",false,null,"WTP-14","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 40","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 40","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 40","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 40","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 40"]
[null,"WTP-15","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 38","On request",null,null,null,null,null,null,null,"WTP-15","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 38","On request",false,null,"WTP-15","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 38","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 38","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 38","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 38","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 38"]
[null,"WTP-16","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","On request",null,null,null,null,null,null,null,"WTP-16","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","On request",false,null,"WTP-16","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 42"]
[null,"WTP-17","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 48","On request",null,null,null,null,null,null,null,"WTP-17","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 48","On request",false,null,"WTP-17","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 48","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 48","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 48","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 48","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 48"]
[null,"WTP-18","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 56","On request",null,null,null,null,null,null,null,"WTP-18","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 56","On request",false,null,"WTP-18","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 56","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 56"]
[null,"WTP-19","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","On request",null,null,null,null,null,null,null,"WTP-19","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","On request",false,null,"WTP-19","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 64"]
[null,"WTP-20","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 70","On request",null,null,null,null,null,null,null,"WTP-20","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 70","On request",false,null,"WTP-20","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 70","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 70","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 70","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 70","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 70"]
[null,"WTP-21","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 78","On request",null,null,null,null,null,null,null,"WTP-21","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 78","On request",false,null,"WTP-21","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 78","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 78","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 78","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 78","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 78"]
[null,"WTP-22","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 38","On request",null,null,null,null,null,null,null,"WTP-22","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 38","On request",false,null,"WTP-22","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 38","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 38","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 38","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 38","Warmtewisselaar Fa. Alfa Laval Typ M6-MFM 38"]
[null,"WTP-23","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","On request",null,null,null,null,null,null,null,"WTP-23","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","On request",false,null,"WTP-23","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","Warmtewisselaar Fa. Alfa Laval Typ M6-MFM 56"]
[null,"WTP-24","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 44","On request",null,null,null,null,null,null,null,"WTP-24","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 44","On request",false,null,"WTP-24","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 44","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 44","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 44","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 44","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 44"]
[null,"WTP-25","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 54","On request",null,null,null,null,null,null,null,"WTP-25","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 54","On request",false,null,"WTP-25","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 54","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 54","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 54","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 54","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 54"]
[null,"WTP-26","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 58","On request",null,null,null,null,null,null,null,"WTP-26","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 58","On request",false,null,"WTP-26","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 58","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 58","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 58","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 58","Warmtewisselaar Fa. Alfa Laval Typ M15-MFM 58"]
[null,"WTP-27","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 76","On request",null,null,null,null,null,null,null,"WTP-27","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 76","On request",false,null,"WTP-27","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 76","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 76","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 76","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 76","Warmtewisselaar Fa. Alfa Laval Typ M15-MFM 76"]
[null,"WTP-28","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 186","On request",null,null,null,null,null,null,null,"WTP-28","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 186","On request",false,null,"WTP-28","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 186","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 186","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 186","Wärmetauscher Fa. Alfa Laval Typ M15-BFM 186","Warmtewisselaar Fa. Alfa Laval Typ M15-BFM 186"]
[null,"WTP-29","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 89","On request",null,null,null,null,null,null,null,"WTP-29","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 89","On request",false,null,"WTP-29","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 89","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 89","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 89","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 89","Warmtewisselaar Fa. Alfa Laval Typ M15-MFM 89"]
[null,"WTA-01","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 10","On request",null,null,null,null,null,null,null,"WTA-01","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 10","On request",false,null,"WTA-01","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 10","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 10","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 10","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 10","Warmtewisselaar Fa. Alfa Laval Typ TL3-PFG 10"]
[null,"WTA-02","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","On request",null,null,null,null,null,null,null,"WTA-02","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","On request",false,null,"WTA-02","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 12","Warmtewisselaar Fa. Alfa Laval Typ TL3-PFG 12"]
[null,"WTA-03","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 18","On request",null,null,null,null,null,null,null,"WTA-03","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 18","On request",false,null,"WTA-03","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 18","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 18","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 18","Wärmetauscher Fa. Alfa Laval Typ TL3-PFG 18","Warmtewisselaar Fa. Alfa Laval Typ TL3-PFG 18"]
[null,"WTA-04","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 18","On request",null,null,null,null,null,null,null,"WTA-04","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 18","On request",false,null,"WTA-04","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 18","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 18","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 18","Wärmetauscher Fa. Alfa Laval Typ T5-BFG 18","Warmtewisselaar Fa. Alfa Laval Typ T5-BFG 18"]
[null,"WTA-05","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 18","On request",null,null,null,null,null,null,null,"WTA-05","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 18","On request",false,null,"WTA-05","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 18","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 18","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 18","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 18","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 18"]
[null,"WTA-06","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 22","On request",null,null,null,null,null,null,null,"WTA-06","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 22","On request",false,null,"WTA-06","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 22","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 22","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 22","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 22","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 22"]
[null,"WTA-07","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","On request",null,null,null,null,null,null,null,"WTA-07","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","On request",false,null,"WTA-07","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 30"]
[null,"WTA-08","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","On request",null,null,null,null,null,null,null,"WTA-08","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","On request",false,null,"WTA-08","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 42","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 42"]
[null,"WTA-09","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 54","On request",null,null,null,null,null,null,null,"WTA-09","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 54","On request",false,null,"WTA-09","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 54","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 54","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 54","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 54","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 54"]
[null,"WTA-10","Wärmetauscher Fa. Alfa Laval Typ M6-MFG 40","On request",null,null,null,null,null,null,null,"WTA-10","Wärmetauscher Fa. Alfa Laval Typ M6-MFG 40","On request",false,null,"WTA-10","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-MFG 40","Wärmetauscher Fa. Alfa Laval Typ M6-MFG 40","Wärmetauscher Fa. Alfa Laval Typ M6-MFG 40","Wärmetauscher Fa. Alfa Laval Typ M6-MFG 40","Warmtewisselaar Fa. Alfa Laval Typ M6-MFG 40"]
[null,"WTA-11","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","On request",null,null,null,null,null,null,null,"WTA-11","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","On request",false,null,"WTA-11","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 56","Warmtewisselaar Fa. Alfa Laval Typ M6-MFM 56"]
[null,"WTA-12","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 42","On request",null,null,null,null,null,null,null,"WTA-12","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 42","On request",false,null,"WTA-12","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 42","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 42","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 42","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 42","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 42"]
[null,"WTA-13","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 26","On request",null,null,null,null,null,null,null,"WTA-13","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 26","On request",false,null,"WTA-13","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 26","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 26","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 26","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 26","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 26"]
[null,"WTA-14","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","On request",null,null,null,null,null,null,null,"WTA-14","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","On request",false,null,"WTA-14","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 30","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 30"]
[null,"WTA-15","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 34","On request",null,null,null,null,null,null,null,"WTA-15","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 34","On request",false,null,"WTA-15","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 34","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 34","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 34","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 34","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 34"]
[null,"WTA-16","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 40","On request",null,null,null,null,null,null,null,"WTA-16","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 40","On request",false,null,"WTA-16","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 40","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 40","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 40","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 40","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 40"]
[null,"WTA-17","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 46","On request",null,null,null,null,null,null,null,"WTA-17","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 46","On request",false,null,"WTA-17","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 46","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 46","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 46","Wärmetauscher Fa. Alfa Laval Typ T5-MFG 46","Warmtewisselaar Fa. Alfa Laval Typ T5-MFG 46"]
[null,"WTA-18","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 60","On request",null,null,null,null,null,null,null,"WTA-18","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 60","On request",false,null,"WTA-18","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 60","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 60","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 60","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 60","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 60"]
[null,"WTA-19","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","On request",null,null,null,null,null,null,null,"WTA-19","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","On request",false,null,"WTA-19","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 64","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 64"]
[null,"WTA-20","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 72","On request",null,null,null,null,null,null,null,"WTA-20","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 72","On request",false,null,"WTA-20","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 72","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 72","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 72","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 72","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 72"]
[null,"WTA-21","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 84","On request",null,null,null,null,null,null,null,"WTA-21","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 84","On request",false,null,"WTA-21","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 84","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 84","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 84","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 84","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 84"]
[null,"WTA-22","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 91","On request",null,null,null,null,null,null,null,"WTA-22","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 91","On request",false,null,"WTA-22","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 91","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 91","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 91","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 91","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 91"]
[null,"WTA-23","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","On request",null,null,null,null,null,null,null,"WTA-23","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","On request",false,null,"WTA-23","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","Wärmetauscher Fa. Alfa Laval Typ M6-MFM 46","Warmtewisselaar Fa. Alfa Laval Typ M6-MFM 46"]
[null,"WTA-24","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 40","On request",null,null,null,null,null,null,null,"WTA-24","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 40","On request",false,null,"WTA-24","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 40","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 40","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 40","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 40","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 40"]
[null,"WTA-25","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 57","On request",null,null,null,null,null,null,null,"WTA-25","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 57","On request",false,null,"WTA-25","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 57","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 57","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 57","Wärmetauscher Fa. Alfa Laval Typ M10-BFM 57","Warmtewisselaar Fa. Alfa Laval Typ M10-BFM 57"]
[null,"WTA-26","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 62","On request",null,null,null,null,null,null,null,"WTA-26","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 62","On request",false,null,"WTA-26","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 62","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 62","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 62","Wärmetauscher Fa. Alfa Laval Typ M10-MFM 62","Warmtewisselaar Fa. Alfa Laval Typ M10-MFM 62"]
[null,"WTA-27","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 52","On request",null,null,null,null,null,null,null,"WTA-27","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 52","On request",false,null,"WTA-27","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 52","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 52","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 52","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 52","Warmtewisselaar Fa. Alfa Laval Typ M15-MFM 52"]
[null,"WTA-28","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 72","On request",null,null,null,null,null,null,null,"WTA-28","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 72","On request",false,null,"WTA-28","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 72","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 72","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 72","Wärmetauscher Fa. Alfa Laval Typ M15-MFM 72","Warmtewisselaar Fa. Alfa Laval Typ M15-MFM 72"]
[null,"WTA-29","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 69","On request",null,null,null,null,null,null,null,"WTA-29","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 69","On request",false,null,"WTA-29","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 69","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 69","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 69","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 69","Warmtewisselaar Fa. Alfa Laval Typ T20-MFM 69"]
[null,"WTA-30","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 82","On request",null,null,null,null,null,null,null,"WTA-30","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 82","On request",false,null,"WTA-30","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 82","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 82","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 82","Wärmetauscher Fa. Alfa Laval Typ T20-MFM 82","Warmtewisselaar Fa. Alfa Laval Typ T20-MFM 82"]
[null,"WT-001","Wärmetauscher Fa. Alfa Laval Typ CB 30-10H","On request",null,null,null,null,null,null,null,"WT-001","Wärmetauscher Fa. Alfa Laval Typ CB 30-10H","On request",false,null,"WT-001","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-10H","Wärmetauscher Fa. Alfa Laval Typ CB 30-10H","Wärmetauscher Fa. Alfa Laval Typ CB 30-10H","Wärmetauscher Fa. Alfa Laval Typ CB 30-10H","Warmtewisselaar Alfa Laval Typ CB 30-10H"]
[null,"WT-002","Wärmetauscher Fa. Alfa Laval Typ CB 30-18H","On request",null,null,null,null,null,null,null,"WT-002","Wärmetauscher Fa. Alfa Laval Typ CB 30-18H","On request",false,null,"WT-002","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-18H","Wärmetauscher Fa. Alfa Laval Typ CB 30-18H","Wärmetauscher Fa. Alfa Laval Typ CB 30-18H","Wärmetauscher Fa. Alfa Laval Typ CB 30-18H","Warmtewisselaar Alfa Laval Typ CB 30-18H"]
[null,"WT-003","Wärmetauscher Fa. Alfa Laval Typ CB 30-24H","On request",null,null,null,null,null,null,null,"WT-003","Wärmetauscher Fa. Alfa Laval Typ CB 30-24H","On request",false,null,"WT-003","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-24H","Wärmetauscher Fa. Alfa Laval Typ CB 30-24H","Wärmetauscher Fa. Alfa Laval Typ CB 30-24H","Wärmetauscher Fa. Alfa Laval Typ CB 30-24H","Warmtewisselaar Alfa Laval Typ CB 30-24H"]
[null,"WT-004","Wärmetauscher Fa. Alfa Laval Typ CB 30-34H","On request",null,null,null,null,null,null,null,"WT-004","Wärmetauscher Fa. Alfa Laval Typ CB 30-34H","On request",false,null,"WT-004","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-34H","Wärmetauscher Fa. Alfa Laval Typ CB 30-34H","Wärmetauscher Fa. Alfa Laval Typ CB 30-34H","Wärmetauscher Fa. Alfa Laval Typ CB 30-34H","Warmtewisselaar Alfa Laval Typ CB 30-34H"]
[null,"WT-005","Wärmetauscher Fa. Alfa Laval Typ CB 30-18M","On request",null,null,null,null,null,null,null,"WT-005","Wärmetauscher Fa. Alfa Laval Typ CB 30-18M","On request",false,null,"WT-005","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-18M","Wärmetauscher Fa. Alfa Laval Typ CB 30-18M","Wärmetauscher Fa. Alfa Laval Typ CB 30-18M","Wärmetauscher Fa. Alfa Laval Typ CB 30-18M","Warmtewisselaar Alfa Laval Typ CB 30-18M"]
[null,"WT-006","Wärmetauscher Fa. Alfa Laval Typ CB 30-24M","On request",null,null,null,null,null,null,null,"WT-006","Wärmetauscher Fa. Alfa Laval Typ CB 30-24M","On request",false,null,"WT-006","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-24M","Wärmetauscher Fa. Alfa Laval Typ CB 30-24M","Wärmetauscher Fa. Alfa Laval Typ CB 30-24M","Wärmetauscher Fa. Alfa Laval Typ CB 30-24M","Warmtewisselaar Alfa Laval Typ CB 30-24M"]
[null,"WT-007","Wärmetauscher Fa. Alfa Laval Typ CB 30-34M","On request",null,null,null,null,null,null,null,"WT-007","Wärmetauscher Fa. Alfa Laval Typ CB 30-34M","On request",false,null,"WT-007","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-34M","Wärmetauscher Fa. Alfa Laval Typ CB 30-34M","Wärmetauscher Fa. Alfa Laval Typ CB 30-34M","Wärmetauscher Fa. Alfa Laval Typ CB 30-34M","Warmtewisselaar Alfa Laval Typ CB 30-34M"]
[null,"WT-008","Wärmetauscher Fa. Alfa Laval Typ CB 30-50M","On request",null,null,null,null,null,null,null,"WT-008","Wärmetauscher Fa. Alfa Laval Typ CB 30-50M","On request",false,null,"WT-008","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-50M","Wärmetauscher Fa. Alfa Laval Typ CB 30-50M","Wärmetauscher Fa. Alfa Laval Typ CB 30-50M","Wärmetauscher Fa. Alfa Laval Typ CB 30-50M","Warmtewisselaar Alfa Laval Typ CB 30-50M"]
[null,"WT-009","Wärmetauscher Fa. Alfa Laval Typ CB 30-10L","On request",null,null,null,null,null,null,null,"WT-009","Wärmetauscher Fa. Alfa Laval Typ CB 30-10L","On request",false,null,"WT-009","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-10L","Wärmetauscher Fa. Alfa Laval Typ CB 30-10L","Wärmetauscher Fa. Alfa Laval Typ CB 30-10L","Wärmetauscher Fa. Alfa Laval Typ CB 30-10L","Warmtewisselaar Alfa Laval Typ CB 76-20M"]
[null,"WT-010","Wärmetauscher Fa. Alfa Laval Typ CB 30-18L","On request",null,null,null,null,null,null,null,"WT-010","Wärmetauscher Fa. Alfa Laval Typ CB 30-18L","On request",{"$f":"IF(AND(B1766=L1766,C1766=M1766,D1766=N1766),FALSE,TRUE)","v":false},null,"WT-010","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-18L","Wärmetauscher Fa. Alfa Laval Typ CB 30-18L","Wärmetauscher Fa. Alfa Laval Typ CB 30-18L","Wärmetauscher Fa. Alfa Laval Typ CB 30-18L","Warmtewisselaar Alfa Laval Typ CB 76-30M"]
[null,"WT-011","Wärmetauscher Fa. Alfa Laval Typ CB 30-24L","On request",null,null,null,null,null,null,null,"WT-011","Wärmetauscher Fa. Alfa Laval Typ CB 30-24L","On request",false,null,"WT-011","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 30-24L","Wärmetauscher Fa. Alfa Laval Typ CB 30-24L","Wärmetauscher Fa. Alfa Laval Typ CB 30-24L","Wärmetauscher Fa. Alfa Laval Typ CB 30-24L","Warmtewisselaar Alfa Laval Typ CB 76-40M"]
[null,"WT-012","Wärmetauscher Fa. Alfa Laval Typ CB 76-20L","On request",null,null,null,null,null,null,null,"WT-012","Wärmetauscher Fa. Alfa Laval Typ CB 76-20L","On request",false,null,"WT-012","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 76-20L","Wärmetauscher Fa. Alfa Laval Typ CB 76-20L","Wärmetauscher Fa. Alfa Laval Typ CB 76-20L","Wärmetauscher Fa. Alfa Laval Typ CB 76-20L","Warmtewisselaar Alfa Laval Typ CB 76-60M"]
[null,"WT-013","Wärmetauscher Fa. Alfa Laval Typ CB 76-30L","On request",null,null,null,null,null,null,null,"WT-013","Wärmetauscher Fa. Alfa Laval Typ CB 76-30L","On request",false,null,"WT-013","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 76-30L","Wärmetauscher Fa. Alfa Laval Typ CB 76-30L","Wärmetauscher Fa. Alfa Laval Typ CB 76-30L","Wärmetauscher Fa. Alfa Laval Typ CB 76-30L","Warmtewisselaar Alfa Laval Typ CB 30-10L"]
[null,"WT-014","Wärmetauscher Fa. Alfa Laval Typ CB 76-40L","On request",null,null,null,null,null,null,null,"WT-014","Wärmetauscher Fa. Alfa Laval Typ CB 76-40L","On request",false,null,"WT-014","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 76-40L","Wärmetauscher Fa. Alfa Laval Typ CB 76-40L","Wärmetauscher Fa. Alfa Laval Typ CB 76-40L","Wärmetauscher Fa. Alfa Laval Typ CB 76-40L","Warmtewisselaar Alfa Laval Typ CB 30-18L"]
[null,"WT-015","Wärmetauscher Fa. Alfa Laval Typ CB 76-50L","On request",null,null,null,null,null,null,null,"WT-015","Wärmetauscher Fa. Alfa Laval Typ CB 76-50L","On request",false,null,"WT-015","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 76-50L","Wärmetauscher Fa. Alfa Laval Typ CB 76-50L","Wärmetauscher Fa. Alfa Laval Typ CB 76-50L","Wärmetauscher Fa. Alfa Laval Typ CB 76-50L","Warmtewisselaar Alfa Laval Typ CB 30-24L"]
[null,"WT-016","Wärmetauscher Fa. Alfa Laval Typ CB 76-20M","On request",null,null,null,null,null,null,null,"WT-016","Wärmetauscher Fa. Alfa Laval Typ CB 76-20M","On request",false,null,"WT-016","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 76-20M","Wärmetauscher Fa. Alfa Laval Typ CB 76-20M","Wärmetauscher Fa. Alfa Laval Typ CB 76-20M","Wärmetauscher Fa. Alfa Laval Typ CB 76-20M","Warmtewisselaar Alfa Laval Typ CB 76-20L"]
[null,"WT-017","Wärmetauscher Fa. Alfa Laval Typ CB 76-30M","On request",null,null,null,null,null,null,null,"WT-017","Wärmetauscher Fa. Alfa Laval Typ CB 76-30M","On request",false,null,"WT-017","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 76-30M","Wärmetauscher Fa. Alfa Laval Typ CB 76-30M","Wärmetauscher Fa. Alfa Laval Typ CB 76-30M","Wärmetauscher Fa. Alfa Laval Typ CB 76-30M","Warmtewisselaar Alfa Laval Typ CB 76-30L"]
[null,"WT-018","Wärmetauscher Fa. Alfa Laval Typ CB 76-40M","On request",null,null,null,null,null,null,null,"WT-018","Wärmetauscher Fa. Alfa Laval Typ CB 76-40M","On request",false,null,"WT-018","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 76-40M","Wärmetauscher Fa. Alfa Laval Typ CB 76-40M","Wärmetauscher Fa. Alfa Laval Typ CB 76-40M","Wärmetauscher Fa. Alfa Laval Typ CB 76-40M","Warmtewisselaar Alfa Laval Typ CB 76-40L"]
[null,"WT-019","Wärmetauscher Fa. Alfa Laval Typ CB 76-60M","On request",null,null,null,null,null,null,null,"WT-019","Wärmetauscher Fa. Alfa Laval Typ CB 76-60M","On request",false,null,"WT-019","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 76-60M","Wärmetauscher Fa. Alfa Laval Typ CB 76-60M","Wärmetauscher Fa. Alfa Laval Typ CB 76-60M","Wärmetauscher Fa. Alfa Laval Typ CB 76-60M","Warmtewisselaar Alfa Laval Typ CB 76-50L"]
[null,"WT-020","Wärmetauscher Fa. Alfa Laval Typ CB 200-40L","On request",null,null,null,null,null,null,null,"WT-020","Wärmetauscher Fa. Alfa Laval Typ CB 200-40L","On request",false,null,"WT-020","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 200-40L","Wärmetauscher Fa. Alfa Laval Typ CB 200-40L","Wärmetauscher Fa. Alfa Laval Typ CB 200-40L","Wärmetauscher Fa. Alfa Laval Typ CB 200-40L","Warmtewisselaar Alfa Nova Typ AN 27-18H"]
[null,"WT-021","Wärmetauscher Fa. Alfa Laval Typ CB 200-50L","On request",null,null,null,null,null,null,null,"WT-021","Wärmetauscher Fa. Alfa Laval Typ CB 200-50L","On request",false,null,"WT-021","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 200-50L","Wärmetauscher Fa. Alfa Laval Typ CB 200-50L","Wärmetauscher Fa. Alfa Laval Typ CB 200-50L","Wärmetauscher Fa. Alfa Laval Typ CB 200-50L","Warmtewisselaar Alfa Nova Typ AN 27-24H"]
[null,"WT-022","Wärmetauscher Fa. Alfa Laval Typ CB 200-64L","On request",null,null,null,null,null,null,null,"WT-022","Wärmetauscher Fa. Alfa Laval Typ CB 200-64L","On request",false,null,"WT-022","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 200-64L","Wärmetauscher Fa. Alfa Laval Typ CB 200-64L","Wärmetauscher Fa. Alfa Laval Typ CB 200-64L","Wärmetauscher Fa. Alfa Laval Typ CB 200-64L","Warmtewisselaar Alfa Nova Typ AN 27-34H"]
[null,"WT-023","Wärmetauscher Fa. Alfa Laval Typ CB 200-100L","On request",null,null,null,null,null,null,null,"WT-023","Wärmetauscher Fa. Alfa Laval Typ CB 200-100L","On request",false,null,"WT-023","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 200-100L","Wärmetauscher Fa. Alfa Laval Typ CB 200-100L","Wärmetauscher Fa. Alfa Laval Typ CB 200-100L","Wärmetauscher Fa. Alfa Laval Typ CB 200-100L","Warmtewisselaar Alfa Nova Typ AN 27-50H"]
[null,"WT-024","Wärmetauscher Fa. Alfa Laval Typ CB 300-80L","On request",null,null,null,null,null,null,null,"WT-024","Wärmetauscher Fa. Alfa Laval Typ CB 300-80L","On request",false,null,"WT-024","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 300-80L","Wärmetauscher Fa. Alfa Laval Typ CB 300-80L","Wärmetauscher Fa. Alfa Laval Typ CB 300-80L","Wärmetauscher Fa. Alfa Laval Typ CB 300-80L","Warmtewisselaar Alfa Nova Typ AN 27-70H"]
[null,"WT-025","Wärmetauscher Fa. Alfa Laval Typ CB 300-100L","On request",null,null,null,null,null,null,null,"WT-025","Wärmetauscher Fa. Alfa Laval Typ CB 300-100L","On request",false,null,"WT-025","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 300-100L","Wärmetauscher Fa. Alfa Laval Typ CB 300-100L","Wärmetauscher Fa. Alfa Laval Typ CB 300-100L","Wärmetauscher Fa. Alfa Laval Typ CB 300-100L","Warmtewisselaar Alfa Laval Typ AN 52-60H"]
[null,"WT-026","Wärmetauscher Fa. Alfa Laval Typ CB 300-124L","On request",null,null,null,null,null,null,null,"WT-026","Wärmetauscher Fa. Alfa Laval Typ CB 300-124L","On request",false,null,"WT-026","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 300-124L","Wärmetauscher Fa. Alfa Laval Typ CB 300-124L","Wärmetauscher Fa. Alfa Laval Typ CB 300-124L","Wärmetauscher Fa. Alfa Laval Typ CB 300-124L","Warmtewisselaar Alfa Laval Typ AN 76-30H"]
[null,"WT-027","Wärmetauscher Fa. Alfa Laval Typ CB 400-270L","On request",null,null,null,null,null,null,null,"WT-027","Wärmetauscher Fa. Alfa Laval Typ CB 400-270L","On request",false,null,"WT-027","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Laval Typ CB 400-270L","Wärmetauscher Fa. Alfa Laval Typ CB 400-270L","Wärmetauscher Fa. Alfa Laval Typ CB 400-270L","Wärmetauscher Fa. Alfa Laval Typ CB 400-270L","Warmtewisselaar Alfa Laval Typ AN 76-40H"]
[null,"WT-028","Wärmetauscher Fa. Alfa Nova Typ AN 27-18H","On request",null,null,null,null,null,null,null,"WT-028","Wärmetauscher Fa. Alfa Nova Typ AN 27-18H","On request",false,null,"WT-028","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 27-18H","Wärmetauscher Fa. Alfa Nova Typ AN 27-18H","Wärmetauscher Fa. Alfa Nova Typ AN 27-18H","Wärmetauscher Fa. Alfa Nova Typ AN 27-18H","Warmtewisselaar Alfa Laval Typ AN 76-50H"]
[null,"WT-029","Wärmetauscher Fa. Alfa Nova Typ AN 27-24H","On request",null,null,null,null,null,null,null,"WT-029","Wärmetauscher Fa. Alfa Nova Typ AN 27-24H","On request",false,null,"WT-029","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 27-24H","Wärmetauscher Fa. Alfa Nova Typ AN 27-24H","Wärmetauscher Fa. Alfa Nova Typ AN 27-24H","Wärmetauscher Fa. Alfa Nova Typ AN 27-24H","Warmtewisselaar Alfa Laval Typ AN 76-60H"]
[null,"WT-030","Wärmetauscher Fa. Alfa Nova Typ AN 27-34H","On request",null,null,null,null,null,null,null,"WT-030","Wärmetauscher Fa. Alfa Nova Typ AN 27-34H","On request",false,null,"WT-030","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 27-34H","Wärmetauscher Fa. Alfa Nova Typ AN 27-34H","Wärmetauscher Fa. Alfa Nova Typ AN 27-34H","Wärmetauscher Fa. Alfa Nova Typ AN 27-34H","Warmtewisselaar Alfa Laval Typ AN 76-70H"]
[null,"WT-031","Wärmetauscher Fa. Alfa Nova Typ AN 27-50H","On request",null,null,null,null,null,null,null,"WT-031","Wärmetauscher Fa. Alfa Nova Typ AN 27-50H","On request",false,null,"WT-031","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 27-50H","Wärmetauscher Fa. Alfa Nova Typ AN 27-50H","Wärmetauscher Fa. Alfa Nova Typ AN 27-50H","Wärmetauscher Fa. Alfa Nova Typ AN 27-50H","Warmtewisselaar Alfa Laval Typ AN 76-80H"]
[null,"WT-032","Wärmetauscher Fa. Alfa Nova Typ AN 27-70H","On request",null,null,null,null,null,null,null,"WT-032","Wärmetauscher Fa. Alfa Nova Typ AN 27-70H","On request",false,null,"WT-032","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 27-70H","Wärmetauscher Fa. Alfa Nova Typ AN 27-70H","Wärmetauscher Fa. Alfa Nova Typ AN 27-70H","Wärmetauscher Fa. Alfa Nova Typ AN 27-70H","Warmtewisselaar Alfa Laval Typ AN 76-110H"]
[null,"WT-033","Wärmetauscher Fa. Alfa Nova Typ AN 52-60H","On request",null,null,null,null,null,null,null,"WT-033","Wärmetauscher Fa. Alfa Nova Typ AN 52-60H","On request",false,null,"WT-033","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 52-60H","Wärmetauscher Fa. Alfa Nova Typ AN 52-60H","Wärmetauscher Fa. Alfa Nova Typ AN 52-60H","Wärmetauscher Fa. Alfa Nova Typ AN 52-60H","Warmtewisselaar Alfa Laval Typ AN 76-140H"]
[null,"WT-034","Wärmetauscher Fa. Alfa Nova Typ AN 76-30H","On request",null,null,null,null,null,null,null,"WT-034","Wärmetauscher Fa. Alfa Nova Typ AN 76-30H","On request",false,null,"WT-034","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 76-30H","Wärmetauscher Fa. Alfa Nova Typ AN 76-30H","Wärmetauscher Fa. Alfa Nova Typ AN 76-30H","Wärmetauscher Fa. Alfa Nova Typ AN 76-30H","Warmtewisselaar Alfa Laval Typ AN 400-50L"]
[null,"WT-035","Wärmetauscher Fa. Alfa Nova Typ AN 76-40H","On request",null,null,null,null,null,null,null,"WT-035","Wärmetauscher Fa. Alfa Nova Typ AN 76-40H","On request",false,null,"WT-035","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 76-40H","Wärmetauscher Fa. Alfa Nova Typ AN 76-40H","Wärmetauscher Fa. Alfa Nova Typ AN 76-40H","Wärmetauscher Fa. Alfa Nova Typ AN 76-40H","Warmtewisselaar Alfa Laval Typ AN 400-60L"]
[null,"WT-036","Wärmetauscher Fa. Alfa Nova Typ AN 76-50H","On request",null,null,null,null,null,null,null,"WT-036","Wärmetauscher Fa. Alfa Nova Typ AN 76-50H","On request",false,null,"WT-036","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 76-50H","Wärmetauscher Fa. Alfa Nova Typ AN 76-50H","Wärmetauscher Fa. Alfa Nova Typ AN 76-50H","Wärmetauscher Fa. Alfa Nova Typ AN 76-50H","Warmtewisselaar Alfa Laval Typ AN 400-80L"]
[null,"WT-037","Wärmetauscher Fa. Alfa Nova Typ AN 76-60H","On request",null,null,null,null,null,null,null,"WT-037","Wärmetauscher Fa. Alfa Nova Typ AN 76-60H","On request",false,null,"WT-037","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 76-60H","Wärmetauscher Fa. Alfa Nova Typ AN 76-60H","Wärmetauscher Fa. Alfa Nova Typ AN 76-60H","Wärmetauscher Fa. Alfa Nova Typ AN 76-60H","Warmtewisselaar Alfa Laval Typ AN 400-90L"]
[null,"WT-038","Wärmetauscher Fa. Alfa Nova Typ AN 76-70H","On request",null,null,null,null,null,null,null,"WT-038","Wärmetauscher Fa. Alfa Nova Typ AN 76-70H","On request",false,null,"WT-038","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 76-70H","Wärmetauscher Fa. Alfa Nova Typ AN 76-70H","Wärmetauscher Fa. Alfa Nova Typ AN 76-70H","Wärmetauscher Fa. Alfa Nova Typ AN 76-70H","Warmtewisselaar Alfa Laval Typ AN 400-100L"]
[null,"WT-039","Wärmetauscher Fa. Alfa Nova Typ AN 76-80H","On request",null,null,null,null,null,null,null,"WT-039","Wärmetauscher Fa. Alfa Nova Typ AN 76-80H","On request",false,null,"WT-039","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 76-80H","Wärmetauscher Fa. Alfa Nova Typ AN 76-80H","Wärmetauscher Fa. Alfa Nova Typ AN 76-80H","Wärmetauscher Fa. Alfa Nova Typ AN 76-80H","Warmtewisselaar Alfa Laval Typ AN 400-110L"]
[null,"WT-040","Wärmetauscher Fa. Alfa Nova Typ AN 76-110H","On request",null,null,null,null,null,null,null,"WT-040","Wärmetauscher Fa. Alfa Nova Typ AN 76-110H","On request",false,null,"WT-040","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 76-110H","Wärmetauscher Fa. Alfa Nova Typ AN 76-110H","Wärmetauscher Fa. Alfa Nova Typ AN 76-110H","Wärmetauscher Fa. Alfa Nova Typ AN 76-110H","Warmtewisselaar Alfa Laval Typ AN 400-120L"]
[null,"WT-041","Wärmetauscher Fa. Alfa Nova Typ AN 76-140H","On request",null,null,null,null,null,null,null,"WT-041","Wärmetauscher Fa. Alfa Nova Typ AN 76-140H","On request",false,null,"WT-041","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 76-140H","Wärmetauscher Fa. Alfa Nova Typ AN 76-140H","Wärmetauscher Fa. Alfa Nova Typ AN 76-140H","Wärmetauscher Fa. Alfa Nova Typ AN 76-140H","Warmtewisselaar Alfa Laval Typ AN 400-160L"]
[null,"WT-042","Wärmetauscher Fa. Alfa Nova Typ AN 400-50L","On request",null,null,null,null,null,null,null,"WT-042","Wärmetauscher Fa. Alfa Nova Typ AN 400-50L","On request",false,null,"WT-042","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-50L","Wärmetauscher Fa. Alfa Nova Typ AN 400-50L","Wärmetauscher Fa. Alfa Nova Typ AN 400-50L","Wärmetauscher Fa. Alfa Nova Typ AN 400-50L","Warmtewisselaar Alfa Laval Typ AN 400-190L"]
[null,"WT-043","Wärmetauscher Fa. Alfa Nova Typ AN 400-60L","On request",null,null,null,null,null,null,null,"WT-043","Wärmetauscher Fa. Alfa Nova Typ AN 400-60L","On request",false,null,"WT-043","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-60L","Wärmetauscher Fa. Alfa Nova Typ AN 400-60L","Wärmetauscher Fa. Alfa Nova Typ AN 400-60L","Wärmetauscher Fa. Alfa Nova Typ AN 400-60L","Warmtewisselaar Alfa Laval Typ AN 400-200L"]
[null,"WT-044","Wärmetauscher Fa. Alfa Nova Typ AN 400-80L","On request",null,null,null,null,null,null,null,"WT-044","Wärmetauscher Fa. Alfa Nova Typ AN 400-80L","On request",false,null,"WT-044","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-80L","Wärmetauscher Fa. Alfa Nova Typ AN 400-80L","Wärmetauscher Fa. Alfa Nova Typ AN 400-80L","Wärmetauscher Fa. Alfa Nova Typ AN 400-80L","Warmtewisselaar Alfa Laval Typ AN 400-240L"]
[null,"WT-045","Wärmetauscher Fa. Alfa Nova Typ AN 400-90L","On request",null,null,null,null,null,null,null,"WT-045","Wärmetauscher Fa. Alfa Nova Typ AN 400-90L","On request",false,null,"WT-045","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-90L","Wärmetauscher Fa. Alfa Nova Typ AN 400-90L","Wärmetauscher Fa. Alfa Nova Typ AN 400-90L","Wärmetauscher Fa. Alfa Nova Typ AN 400-90L","Warmtewisselaar Alfa Laval Typ AN 400-250L"]
[null,"WT-046","Wärmetauscher Fa. Alfa Nova Typ AN 400-100L","On request",null,null,null,null,null,null,null,"WT-046","Wärmetauscher Fa. Alfa Nova Typ AN 400-100L","On request",false,null,"WT-046","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-100L","Wärmetauscher Fa. Alfa Nova Typ AN 400-100L","Wärmetauscher Fa. Alfa Nova Typ AN 400-100L","Wärmetauscher Fa. Alfa Nova Typ AN 400-100L","Warmtewisselaar Alfa Laval Typ AN 400-270L"]
[null,"WT-047","Wärmetauscher Fa. Alfa Nova Typ AN 400-110L","On request",null,null,null,null,null,null,null,"WT-047","Wärmetauscher Fa. Alfa Nova Typ AN 400-110L","On request",false,null,"WT-047","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-110L","Wärmetauscher Fa. Alfa Nova Typ AN 400-110L","Wärmetauscher Fa. Alfa Nova Typ AN 400-110L","Wärmetauscher Fa. Alfa Nova Typ AN 400-110L","Warmtewisselaar Alfa Laval Typ CB 200-40L"]
[null,"WT-048","Wärmetauscher Fa. Alfa Nova Typ AN 400-120L","On request",null,null,null,null,null,null,null,"WT-048","Wärmetauscher Fa. Alfa Nova Typ AN 400-120L","On request",false,null,"WT-048","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-120L","Wärmetauscher Fa. Alfa Nova Typ AN 400-120L","Wärmetauscher Fa. Alfa Nova Typ AN 400-120L","Wärmetauscher Fa. Alfa Nova Typ AN 400-120L","Warmtewisselaar Alfa Laval Typ CB 200-50L"]
[null,"WT-049","Wärmetauscher Fa. Alfa Nova Typ AN 400-160L","On request",null,null,null,null,null,null,null,"WT-049","Wärmetauscher Fa. Alfa Nova Typ AN 400-160L","On request",false,null,"WT-049","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-160L","Wärmetauscher Fa. Alfa Nova Typ AN 400-160L","Wärmetauscher Fa. Alfa Nova Typ AN 400-160L","Wärmetauscher Fa. Alfa Nova Typ AN 400-160L","Warmtewisselaar Alfa Laval Typ CB 200-64L"]
[null,"WT-050","Wärmetauscher Fa. Alfa Nova Typ AN 400-190L","On request",null,null,null,null,null,null,null,"WT-050","Wärmetauscher Fa. Alfa Nova Typ AN 400-190L","On request",false,null,"WT-050","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-190L","Wärmetauscher Fa. Alfa Nova Typ AN 400-190L","Wärmetauscher Fa. Alfa Nova Typ AN 400-190L","Wärmetauscher Fa. Alfa Nova Typ AN 400-190L","Warmtewisselaar Alfa Laval Typ CB 200-100L"]
[null,"WT-051","Wärmetauscher Fa. Alfa Nova Typ AN 400-200L","On request",null,null,null,null,null,null,null,"WT-051","Wärmetauscher Fa. Alfa Nova Typ AN 400-200L","On request",false,null,"WT-051","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-200L","Wärmetauscher Fa. Alfa Nova Typ AN 400-200L","Wärmetauscher Fa. Alfa Nova Typ AN 400-200L","Wärmetauscher Fa. Alfa Nova Typ AN 400-200L","Warmtewisselaar Alfa Laval Typ CB 300-80L"]
[null,"WT-052","Wärmetauscher Fa. Alfa Nova Typ AN 400-240L","On request",null,null,null,null,null,null,null,"WT-052","Wärmetauscher Fa. Alfa Nova Typ AN 400-240L","On request",false,null,"WT-052","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-240L","Wärmetauscher Fa. Alfa Nova Typ AN 400-240L","Wärmetauscher Fa. Alfa Nova Typ AN 400-240L","Wärmetauscher Fa. Alfa Nova Typ AN 400-240L","Warmtewisselaar Alfa Laval Typ CB 300-100L"]
[null,"WT-053","Wärmetauscher Fa. Alfa Nova Typ AN 400-250L","On request",null,null,null,null,null,null,null,"WT-053","Wärmetauscher Fa. Alfa Nova Typ AN 400-250L","On request",false,null,"WT-053","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-250L","Wärmetauscher Fa. Alfa Nova Typ AN 400-250L","Wärmetauscher Fa. Alfa Nova Typ AN 400-250L","Wärmetauscher Fa. Alfa Nova Typ AN 400-250L","Warmtewisselaar Alfa Laval Typ CB 300-124L"]
[null,"WT-054","Wärmetauscher Fa. Alfa Nova Typ AN 400-270L","On request",null,null,null,null,null,null,null,"WT-054","Wärmetauscher Fa. Alfa Nova Typ AN 400-270L","On request",false,null,"WT-054","bauseits","On request","sur demande","på forespørgsel","bauseits","Wärmetauscher Fa. Alfa Nova Typ AN 400-270L","Wärmetauscher Fa. Alfa Nova Typ AN 400-270L","Wärmetauscher Fa. Alfa Nova Typ AN 400-270L","Wärmetauscher Fa. Alfa Nova Typ AN 400-270L","Warmtewisselaar Alfa Laval Typ CB 400-270L"]
[null,227492,"Durchlauferhitzer DHE 18 SLi 25A","On request",null,null,null,null,null,null,null,227492,"Durchlauferhitzer DHE 18 SLi 25A","On request",false,null,227492,"auf Anfrage","On request",960,"på forespørgsel",991,"Durchlauferhitzer DHE 18 SLi 25A","Durchlauferhitzer DHE 18 SLi 25A","Durchlauferhitzer DHE 18 SLi 25A","Durchlauferhitzer DHE 18 SLi 25A","Elektr. Doorstromer DHE 18 SLi 25 A"]
[null,227493,"Durchlauferhitzer DHE 18/21/24 SLi","On request",null,null,null,null,null,null,null,227493,"Durchlauferhitzer DHE 18/21/24 SLi","On request",false,null,227493,"auf Anfrage","On request",910,"på forespørgsel",991,"Durchlauferhitzer DHE 18/21/24 SLi","Durchlauferhitzer DHE 18/21/24 SLi","Durchlauferhitzer DHE 18/21/24 SLi","Durchlauferhitzer DHE 18/21/24 SLi","Elektr. Doorstromer DHE 18/21/24 SLi"]
[null,227494,"Durchlauferhitzer DHE 27 SLi","On request",null,null,null,null,null,null,null,227494,"Durchlauferhitzer DHE 27 SLi","On request",false,null,227494,"auf Anfrage","On request",950,"på forespørgsel",991,"Durchlauferhitzer DHE 27 SLi","Durchlauferhitzer DHE 27 SLi","Durchlauferhitzer DHE 27 SLi","Durchlauferhitzer DHE 27 SLi","Elektr. Doorstromer DHE 27 SLi"]
[null,227498,"Durchlauferhitzer DEL 18 SLi 25A","On request",null,null,null,null,null,null,null,227498,"Durchlauferhitzer DEL 18 SLi 25A","On request",false,null,227498,"auf Anfrage","On request","sur demande","på forespørgsel",626,"Durchlauferhitzer DEL 18 SLi 25A","Durchlauferhitzer DEL 18 SLi 25A","Durchlauferhitzer DEL 18 SLi 25A","Durchlauferhitzer DEL 18 SLi 25A","Elektr. Doorstromer DEL 18 SLi 25 A"]
[null,227499,"Durchlauferhitzer DEL 18/21/24 SLi","On request",null,null,null,null,null,null,null,227499,"Durchlauferhitzer DEL 18/21/24 SLi","On request",false,null,227499,"auf Anfrage","On request","sur demande","på forespørgsel",626,"Durchlauferhitzer DEL 18/21/24 SLi","Durchlauferhitzer DEL 18/21/24 SLi","Durchlauferhitzer DEL 18/21/24 SLi","Durchlauferhitzer DEL 18/21/24 SLi","Elektr. Doorstromer DEL 18/21/24 SLi"]
[null,227500,"Durchlauferhitzer DEL 27 SLi","On request",null,null,null,null,null,null,null,227500,"Durchlauferhitzer DEL 27 SLi","On request",false,null,227500,"auf Anfrage","On request","sur demande","på forespørgsel",626,"Durchlauferhitzer DEL 27 SLi","Durchlauferhitzer DEL 27 SLi","Durchlauferhitzer DEL 27 SLi","Durchlauferhitzer DEL 27 SLi","Elektr. Doorstromer DEL 27 SLi"]
[null,232013,"Durchlauferhitzer DHB-E 11 SLi","On request",null,null,null,null,null,null,null,232013,"Durchlauferhitzer DHB-E 11 SLi","On request",false,null,232013,"auf Anfrage","On request","sur demande","på forespørgsel",501,"Durchlauferhitzer DHB-E 11 SLi","Durchlauferhitzer DHB-E 11 SLi","Durchlauferhitzer DHB-E 11 SLi","Durchlauferhitzer DHB-E 11 SLi","Elektr. Doorstromer DHB-E 11 SLi"]
[null,232014,"Durchlauferhitzer DHB-E 13 SLi","On request",null,null,null,null,null,null,null,232014,"Durchlauferhitzer DHB-E 13 SLi","On request",false,null,232014,"auf Anfrage","On request","sur demande","på forespørgsel",501,"Durchlauferhitzer DHB-E 13 SLi","Durchlauferhitzer DHB-E 13 SLi","Durchlauferhitzer DHB-E 13 SLi","Durchlauferhitzer DHB-E 13 SLi","Elektr. Doorstromer DHB-E 13 SLi"]
[null,232015,"Durchlauferhitzer DHB-E 18 SLi 25A","On request",null,null,null,null,null,null,null,232015,"Durchlauferhitzer DHB-E 18 SLi 25A","On request",false,null,232015,"auf Anfrage","On request","sur demande","på forespørgsel",501,"Durchlauferhitzer DHB-E 18 SLi 25A","Durchlauferhitzer DHB-E 18 SLi 25A","Durchlauferhitzer DHB-E 18 SLi 25A","Durchlauferhitzer DHB-E 18 SLi 25A","Elektr. Doorstromer DHB-E 18 SLi 25A"]
[null,232016,"Durchlauferhitzer DHB-E 18/21/24 SLi","On request",null,null,null,null,null,null,null,232016,"Durchlauferhitzer DHB-E 18/21/24 SLi","On request",false,null,232016,"auf Anfrage","On request","sur demande","på forespørgsel",501,"Durchlauferhitzer DHB-E 18/21/24 SLi","Durchlauferhitzer DHB-E 18/21/24 SLi","Durchlauferhitzer DHB-E 18/21/24 SLi","Durchlauferhitzer DHB-E 18/21/24 SLi","Elektr. Doorstromer DHB-E 18/21/24 SLi"]
[null,232017,"Durchlauferhitzer DHB-E 27 SLi","On request",null,null,null,null,null,null,null,232017,"Durchlauferhitzer DHB-E 27 SLi","On request",false,null,232017,"auf Anfrage","On request","sur demande","på forespørgsel",501,"Durchlauferhitzer DHB-E 27 SLi","Durchlauferhitzer DHB-E 27 SLi","Durchlauferhitzer DHB-E 27 SLi","Durchlauferhitzer DHB-E 27 SLi","Elektr. Doorstromer DHB-E 27 SLi"]
[null,227612,"Durchlauferhitzer DHB 18 STi","On request",null,null,null,null,null,null,null,227612,"Durchlauferhitzer DHB 18 STi","On request",false,null,227612,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB 18 STi","Durchlauferhitzer DHB 18 STi","Durchlauferhitzer DHB 18 STi","Durchlauferhitzer DHB 18 STi","Elektr. Doorstromer DHB 18 STi"]
[null,227613,"Durchlauferhitzer DHB 21 STi","On request",null,null,null,null,null,null,null,227613,"Durchlauferhitzer DHB 21 STi","On request",false,null,227613,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB 21 STi","Durchlauferhitzer DHB 21 STi","Durchlauferhitzer DHB 21 STi","Durchlauferhitzer DHB 21 STi","Elektr. Doorstromer DHB 21 STi"]
[null,227614,"Durchlauferhitzer DHB 24 STi","On request",null,null,null,null,null,null,null,227614,"Durchlauferhitzer DHB 24 STi","On request",false,null,227614,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB 24 STi","Durchlauferhitzer DHB 24 STi","Durchlauferhitzer DHB 24 STi","Durchlauferhitzer DHB 24 STi","Elektr. Doorstromer DHB 24 STi"]
[null,227615,"Durchlauferhitzer DHB 27 STi","On request",null,null,null,null,null,null,null,227615,"Durchlauferhitzer DHB 27 STi","On request",false,null,227615,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHB 27 STi","Durchlauferhitzer DHB 27 STi","Durchlauferhitzer DHB 27 STi","Durchlauferhitzer DHB 27 STi","Elektr. Doorstromer DHB 27 STi"]
[null,232003,"Durchlauferhitzer HDB-E 12 Si","On request",null,null,null,null,null,null,null,232003,"Durchlauferhitzer HDB-E 12 Si","On request",false,null,232003,"auf Anfrage","On request","sur demande","på forespørgsel",332,"Durchlauferhitzer HDB-E 12 Si","Durchlauferhitzer HDB-E 12 Si","Durchlauferhitzer HDB-E 12 Si","Durchlauferhitzer HDB-E 12 Si","Elektr. Doorstromer HDB-E 12 Si"]
[null,232004,"Durchlauferhitzer HDB-E 18 Si","On request",null,null,null,null,null,null,null,232004,"Durchlauferhitzer HDB-E 18 Si","On request",false,null,232004,"auf Anfrage","On request","sur demande","på forespørgsel",332,"Durchlauferhitzer HDB-E 18 Si","Durchlauferhitzer HDB-E 18 Si","Durchlauferhitzer HDB-E 18 Si","Durchlauferhitzer HDB-E 18 Si","Elektr. Doorstromer HDB-E 18 Si"]
[null,232005,"Durchlauferhitzer HDB-E 21 Si","On request",null,null,null,null,null,null,null,232005,"Durchlauferhitzer HDB-E 21 Si","On request",false,null,232005,"auf Anfrage","On request","sur demande","på forespørgsel",332,"Durchlauferhitzer HDB-E 21 Si","Durchlauferhitzer HDB-E 21 Si","Durchlauferhitzer HDB-E 21 Si","Durchlauferhitzer HDB-E 21 Si","Elektr. Doorstromer HDB-E 21 Si"]
[null,232006,"Durchlauferhitzer HDB-E 24 Si","On request",null,null,null,null,null,null,null,232006,"Durchlauferhitzer HDB-E 24 Si","On request",false,null,232006,"auf Anfrage","On request","sur demande","på forespørgsel",332,"Durchlauferhitzer HDB-E 24 Si","Durchlauferhitzer HDB-E 24 Si","Durchlauferhitzer HDB-E 24 Si","Durchlauferhitzer HDB-E 24 Si","Elektr. Doorstromer HDB-E 24 Si"]
[null,182137,"Durchlauferhitzer DHF 12 C1","On request",null,null,null,null,null,null,null,182137,"Durchlauferhitzer DHF 12 C1","On request",{"$f":"IF(AND(B1830=L1830,C1830=M1830,D1830=N1830),FALSE,TRUE)","v":false},null,182137,"auf Anfrage","On request",535,"på forespørgsel","op aanvraag","Durchlauferhitzer DHF 12 C1","Durchlauferhitzer DHF 12 C1","Durchlauferhitzer DHF 12 C1","Durchlauferhitzer DHF 12 C1","Doorstromer DHF 12 C1"]
[null,185708,"Durchlauferhitzer DHF 13 C3","On request",null,null,null,null,null,null,null,185708,"Durchlauferhitzer DHF 13 C3","On request",false,null,185708,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHF 13 C3","Durchlauferhitzer DHF 13 C3","Durchlauferhitzer DHF 13 C3","Durchlauferhitzer DHF 13 C3","Doorstromer DHF 13 C3"]
[null,224201,"Durchlauferhitzer DHC-E 8/10","On request",null,null,null,null,null,null,null,224201,"Durchlauferhitzer DHC-E 8/10","On request",false,null,224201,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHC-E 8/10","Durchlauferhitzer DHC-E 8/10","Durchlauferhitzer DHC-E 8/10","Durchlauferhitzer DHC-E 8/10","Elektr. Doorstromer DHC-E 8/10"]
[null,230628,"Durchlauferhitzer DHC-E 12","On request",null,null,null,null,null,null,null,230628,"Durchlauferhitzer DHC-E 12","On request",false,null,230628,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHC-E 12","Durchlauferhitzer DHC-E 12","Durchlauferhitzer DHC-E 12","Durchlauferhitzer DHC-E 12","Doorstromer DHC-E 12"]
[null,73715,"Durchlauferhitzer DHC 4","On request",null,null,null,null,null,null,null,73715,"Durchlauferhitzer DHC 4","On request",false,null,73715,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHC 4","Durchlauferhitzer DHC 4","Durchlauferhitzer DHC 4","Durchlauferhitzer DHC 4","Elektr. Doorstromer DHC 4"]
[null,73480,"Durchlauferhitzer DHC 6","On request",null,null,null,null,null,null,null,73480,"Durchlauferhitzer DHC 6","On request",false,null,73480,"auf Anfrage","On request",320,"på forespørgsel","op aanvraag","Durchlauferhitzer DHC 6","Durchlauferhitzer DHC 6","Durchlauferhitzer DHC 6","Durchlauferhitzer DHC 6","Elektr. Doorstromer DHC 6"]
[null,73479,"Durchlauferhitzer DHC 6 U","On request",null,null,null,null,null,null,null,73479,"Durchlauferhitzer DHC 6 U","On request",false,null,73479,"auf Anfrage","On request",375,"på forespørgsel","op aanvraag","Durchlauferhitzer DHC 6 U","Durchlauferhitzer DHC 6 U","Durchlauferhitzer DHC 6 U","Durchlauferhitzer DHC 6 U","Elektr. Doorstromer DHC 6 U"]
[null,73481,"Durchlauferhitzer DHC 8","On request",null,null,null,null,null,null,null,73481,"Durchlauferhitzer DHC 8","On request",false,null,73481,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer DHC 8","Durchlauferhitzer DHC 8","Durchlauferhitzer DHC 8","Durchlauferhitzer DHC 8","Elektr. Doorstromer DHC 8"]
[null,73716,"Durchlauferhitzer DHA 4/8 L","On request",null,null,null,null,null,null,null,73716,"Durchlauferhitzer DHA 4/8 L","On request",false,null,73716,"auf Anfrage","On request",395,"på forespørgsel","op aanvraag","Durchlauferhitzer DHA 4/8 L","Durchlauferhitzer DHA 4/8 L","Durchlauferhitzer DHA 4/8 L","Durchlauferhitzer DHA 4/8 L","Elektr. Doorstromer DHA 4/8 L"]
[null,224196,"Durchlauferhitzer Tempra 12 Plus","On request",null,null,null,null,null,null,null,224196,"Durchlauferhitzer Tempra 12 Plus","On request",false,null,224196,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 12 Plus","Durchlauferhitzer Tempra 12 Plus","Durchlauferhitzer Tempra 12 Plus","Durchlauferhitzer Tempra 12 Plus","Kleine Elektr. Doorstromer Tempra 12 Plus"]
[null,224197,"Durchlauferhitzer Tempra 15 Plus","On request",null,null,null,null,null,null,null,224197,"Durchlauferhitzer Tempra 15 Plus","On request",false,null,224197,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 15 Plus","Durchlauferhitzer Tempra 15 Plus","Durchlauferhitzer Tempra 15 Plus","Durchlauferhitzer Tempra 15 Plus","Kleine Elektr. Doorstromer Tempra 15 Plus"]
[null,224198,"Durchlauferhitzer Tempra 20 Plus","On request",null,null,null,null,null,null,null,224198,"Durchlauferhitzer Tempra 20 Plus","On request",false,null,224198,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 20 Plus","Durchlauferhitzer Tempra 20 Plus","Durchlauferhitzer Tempra 20 Plus","Durchlauferhitzer Tempra 20 Plus","Kleine Elektr. Doorstromer Tempra 20 Plus"]
[null,224199,"Durchlauferhitzer Tempra 24 Plus","On request",null,null,null,null,null,null,null,224199,"Durchlauferhitzer Tempra 24 Plus","On request",false,null,224199,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 24 Plus","Durchlauferhitzer Tempra 24 Plus","Durchlauferhitzer Tempra 24 Plus","Durchlauferhitzer Tempra 24 Plus","Kleine Elektr. Doorstromer Tempra 24 Plus"]
[null,223425,"Durchlauferhitzer Tempra 29 Plus","On request",null,null,null,null,null,null,null,223425,"Durchlauferhitzer Tempra 29 Plus","On request",false,null,223425,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 29 Plus","Durchlauferhitzer Tempra 29 Plus","Durchlauferhitzer Tempra 29 Plus","Durchlauferhitzer Tempra 29 Plus","Kleine Elektr. Doorstromer Tempra 29 Plus"]
[null,223426,"Durchlauferhitzer Tempra 36 Plus","On request",null,null,null,null,null,null,null,223426,"Durchlauferhitzer Tempra 36 Plus","On request",false,null,223426,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 36 Plus","Durchlauferhitzer Tempra 36 Plus","Durchlauferhitzer Tempra 36 Plus","Durchlauferhitzer Tempra 36 Plus","Kleine Elektr. Doorstromer Tempra 36 Plus"]
[null,223420,"Durchlauferhitzer Tempra 12 B","On request",null,null,null,null,null,null,null,223420,"Durchlauferhitzer Tempra 12 B","On request",false,null,223420,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 12 B","Durchlauferhitzer Tempra 12 B","Durchlauferhitzer Tempra 12 B","Durchlauferhitzer Tempra 12 B","Kleine Elektr. Doorstromer Tempra 12"]
[null,223421,"Durchlauferhitzer Tempra 15 B","On request",null,null,null,null,null,null,null,223421,"Durchlauferhitzer Tempra 15 B","On request",false,null,223421,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 15 B","Durchlauferhitzer Tempra 15 B","Durchlauferhitzer Tempra 15 B","Durchlauferhitzer Tempra 15 B","Kleine Elektr. Doorstromer Tempra 15"]
[null,223422,"Durchlauferhitzer Tempra 20 B","On request",null,null,null,null,null,null,null,223422,"Durchlauferhitzer Tempra 20 B","On request",false,null,223422,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 20 B","Durchlauferhitzer Tempra 20 B","Durchlauferhitzer Tempra 20 B","Durchlauferhitzer Tempra 20 B","Kleine Elektr. Doorstromer Tempra 20"]
[null,223424,"Durchlauferhitzer Tempra 24 B","On request",null,null,null,null,null,null,null,223424,"Durchlauferhitzer Tempra 24 B","On request",false,null,223424,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Durchlauferhitzer Tempra 24 B","Durchlauferhitzer Tempra 24 B","Durchlauferhitzer Tempra 24 B","Durchlauferhitzer Tempra 24 B","Kleine Elektr. Doorstromer heater Tempra 24"]
[null,73125,"Warmwasser-Wandspeicher SHZ 30 F","On request",null,null,null,null,null,null,null,73125,"Warmwasser-Wandspeicher SHZ 30 F","On request",false,null,73125,"auf Anfrage","On request","1.015,00","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher SHZ 30 F","Warmwasser-Wandspeicher SHZ 30 F","Warmwasser-Wandspeicher SHZ 30 F","Warmwasser-Wandspeicher SHZ 30 F","Warmwasser-Wandspeicher SHZ 30 F"]
[null,73126,"Warmwasser-Wandspeicher SHZ 50 F","On request",null,null,null,null,null,null,null,73126,"Warmwasser-Wandspeicher SHZ 50 F","On request",false,null,73126,"auf Anfrage","On request","1.080,00","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher SHZ 50 F","Warmwasser-Wandspeicher SHZ 50 F","Warmwasser-Wandspeicher SHZ 50 F","Warmwasser-Wandspeicher SHZ 50 F","Warmwasser-Wandspeicher SHZ 50 F"]
[null,73127,"Warmwasser-Wandspeicher SHZ 80 F","On request",null,null,null,null,null,null,null,73127,"Warmwasser-Wandspeicher SHZ 80 F","On request",false,null,73127,"auf Anfrage","On request","1.165,00","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher SHZ 80 F","Warmwasser-Wandspeicher SHZ 80 F","Warmwasser-Wandspeicher SHZ 80 F","Warmwasser-Wandspeicher SHZ 80 F","Warmwasser-Wandspeicher SHZ 80 F"]
[null,73128,"Warmwasser-Wandspeicher SHZ 100 F","On request",null,null,null,null,null,null,null,73128,"Warmwasser-Wandspeicher SHZ 100 F","On request",false,null,73128,"auf Anfrage","On request","1.180,00","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher SHZ 100 F","Warmwasser-Wandspeicher SHZ 100 F","Warmwasser-Wandspeicher SHZ 100 F","Warmwasser-Wandspeicher SHZ 100 F","Warmwasser-Wandspeicher SHZ 100 F"]
[null,73129,"Warmwasser-Wandspeicher SHZ 120 F","On request",null,null,null,null,null,null,null,73129,"Warmwasser-Wandspeicher SHZ 120 F","On request",false,null,73129,"auf Anfrage","On request","1.245,00","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher SHZ 120 F","Warmwasser-Wandspeicher SHZ 120 F","Warmwasser-Wandspeicher SHZ 120 F","Warmwasser-Wandspeicher SHZ 120 F","Warmwasser-Wandspeicher SHZ 120 F"]
[null,73130,"Warmwasser-Wandspeicher SHZ 150 F","On request",null,null,null,null,null,null,null,73130,"Warmwasser-Wandspeicher SHZ 150 F","On request",false,null,73130,"auf Anfrage","On request","1.330,00","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher SHZ 150 F","Warmwasser-Wandspeicher SHZ 150 F","Warmwasser-Wandspeicher SHZ 150 F","Warmwasser-Wandspeicher SHZ 150 F","Warmwasser-Wandspeicher SHZ 150 F"]
[null,222126,"Warmwasser-Wandspeicher SHZ 200 F","On request",null,null,null,null,null,null,null,222126,"Warmwasser-Wandspeicher SHZ 200 F","On request",false,null,222126,"auf Anfrage","On request","1.420,00","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher SHZ 200 F","Warmwasser-Wandspeicher SHZ 200 F","Warmwasser-Wandspeicher SHZ 200 F","Warmwasser-Wandspeicher SHZ 200 F","Warmwasser-Wandspeicher SHZ 200 F"]
[null,231150,"Warmwasser-Wandspeicher PSH 30 Universal EL","On request",null,null,null,null,null,null,null,231150,"Warmwasser-Wandspeicher PSH 30 Universal EL","On request",false,null,231150,"auf Anfrage","On request","sur demande","på forespørgsel",832,"Warmwasser-Wandspeicher PSH 30 Universal EL","Warmwasser-Wandspeicher PSH 30 Universal EL","Warmwasser-Wandspeicher PSH 30 Universal EL","Warmwasser-Wandspeicher PSH 30 Universal EL","Wandboiler PSH 30 Universeel EL"]
[null,231151,"Warmwasser-Wandspeicher PSH 50 Universal EL","On request",null,null,null,null,null,null,null,231151,"Warmwasser-Wandspeicher PSH 50 Universal EL","On request",false,null,231151,"auf Anfrage","On request","sur demande","på forespørgsel",900,"Warmwasser-Wandspeicher PSH 50 Universal EL","Warmwasser-Wandspeicher PSH 50 Universal EL","Warmwasser-Wandspeicher PSH 50 Universal EL","Warmwasser-Wandspeicher PSH 50 Universal EL","Wandboiler PSH 50 Universeel EL"]
[null,231152,"Warmwasser-Wandspeicher PSH 80 Universal EL","On request",null,null,null,null,null,null,null,231152,"Warmwasser-Wandspeicher PSH 80 Universal EL","On request",false,null,231152,"auf Anfrage","On request","sur demande","på forespørgsel",1025,"Warmwasser-Wandspeicher PSH 80 Universal EL","Warmwasser-Wandspeicher PSH 80 Universal EL","Warmwasser-Wandspeicher PSH 80 Universal EL","Warmwasser-Wandspeicher PSH 80 Universal EL","Wandboiler PSH 80 Universeel EL"]
[null,231153,"Warmwasser-Wandspeicher PSH 100 Universal EL","On request",null,null,null,null,null,null,null,231153,"Warmwasser-Wandspeicher PSH 100 Universal EL","On request",false,null,231153,"auf Anfrage","On request","sur demande","på forespørgsel",1083,"Warmwasser-Wandspeicher PSH 100 Universal EL","Warmwasser-Wandspeicher PSH 100 Universal EL","Warmwasser-Wandspeicher PSH 100 Universal EL","Warmwasser-Wandspeicher PSH 100 Universal EL","Wandboiler PSH 100 Universeel EL_horizontaal"]
[null,231649,"Warmwasser-Wandspeicher PSH 120 Universal EL","On request",null,null,null,null,null,null,null,231649,"Warmwasser-Wandspeicher PSH 120 Universal EL","On request",false,null,231649,"auf Anfrage","On request","sur demande","på forespørgsel",1145,"Warmwasser-Wandspeicher PSH 120 Universal EL","Warmwasser-Wandspeicher PSH 120 Universal EL","Warmwasser-Wandspeicher PSH 120 Universal EL","Warmwasser-Wandspeicher PSH 120 Universal EL","Wandboiler PSH 120 Universeel EL"]
[null,231154,"Warmwasser-Wandspeicher PSH 150 Universal EL","On request",null,null,null,null,null,null,null,231154,"Warmwasser-Wandspeicher PSH 150 Universal EL","On request",false,null,231154,"auf Anfrage","On request","sur demande","på forespørgsel",1250,"Warmwasser-Wandspeicher PSH 150 Universal EL","Warmwasser-Wandspeicher PSH 150 Universal EL","Warmwasser-Wandspeicher PSH 150 Universal EL","Warmwasser-Wandspeicher PSH 150 Universal EL","Wandboiler PSH 150 Universeel EL"]
[null,231155,"Warmwasser-Wandspeicher PSH 30 EL","On request",null,null,null,null,null,null,null,231155,"Warmwasser-Wandspeicher PSH 30 EL","On request",false,null,231155,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 30 EL","Warmwasser-Wandspeicher PSH 30 EL","Warmwasser-Wandspeicher PSH 30 EL","Warmwasser-Wandspeicher PSH 30 EL","Wandboiler PSH 30 EL"]
[null,231156,"Warmwasser-Wandspeicher PSH 50 EL","On request",null,null,null,null,null,null,null,231156,"Warmwasser-Wandspeicher PSH 50 EL","On request",false,null,231156,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 50 EL","Warmwasser-Wandspeicher PSH 50 EL","Warmwasser-Wandspeicher PSH 50 EL","Warmwasser-Wandspeicher PSH 50 EL","Wandboiler PSH 50 EL"]
[null,231157,"Warmwasser-Wandspeicher PSH 80 EL","On request",null,null,null,null,null,null,null,231157,"Warmwasser-Wandspeicher PSH 80 EL","On request",false,null,231157,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 80 EL","Warmwasser-Wandspeicher PSH 80 EL","Warmwasser-Wandspeicher PSH 80 EL","Warmwasser-Wandspeicher PSH 80 EL","Wandboiler PSH 80 EL"]
[null,231158,"Warmwasser-Wandspeicher PSH 100 EL","On request",null,null,null,null,null,null,null,231158,"Warmwasser-Wandspeicher PSH 100 EL","On request",false,null,231158,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 100 EL","Warmwasser-Wandspeicher PSH 100 EL","Warmwasser-Wandspeicher PSH 100 EL","Warmwasser-Wandspeicher PSH 100 EL","Wandboiler PSH 100 EL"]
[null,231648,"Warmwasser-Wandspeicher PSH 120 EL","On request",null,null,null,null,null,null,null,231648,"Warmwasser-Wandspeicher PSH 120 EL","On request",false,null,231648,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 120 EL","Warmwasser-Wandspeicher PSH 120 EL","Warmwasser-Wandspeicher PSH 120 EL","Warmwasser-Wandspeicher PSH 120 EL","Wandboiler PSH 120 EL"]
[null,231159,"Warmwasser-Wandspeicher PSH 150 EL","On request",null,null,null,null,null,null,null,231159,"Warmwasser-Wandspeicher PSH 150 EL","On request",false,null,231159,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 150 EL","Warmwasser-Wandspeicher PSH 150 EL","Warmwasser-Wandspeicher PSH 150 EL","Warmwasser-Wandspeicher PSH 150 EL","Wandboiler PSH 150 EL"]
[null,74478,"Warmwasser-Wandspeicher PSH 30 Si","On request",null,null,null,null,null,null,null,74478,"Warmwasser-Wandspeicher PSH 30 Si","On request",false,null,74478,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 30 Si","Warmwasser-Wandspeicher PSH 30 Si","Warmwasser-Wandspeicher PSH 30 Si","Warmwasser-Wandspeicher PSH 30 Si","Wandboiler PSH 30 Si"]
[null,74479,"Warmwasser-Wandspeicher PSH 50 Si","On request",null,null,null,null,null,null,null,74479,"Warmwasser-Wandspeicher PSH 50 Si","On request",false,null,74479,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 50 Si","Warmwasser-Wandspeicher PSH 50 Si","Warmwasser-Wandspeicher PSH 50 Si","Warmwasser-Wandspeicher PSH 50 Si","Wandboiler PSH 50 Si"]
[null,74480,"Warmwasser-Wandspeicher PSH 80 Si","On request",null,null,null,null,null,null,null,74480,"Warmwasser-Wandspeicher PSH 80 Si","On request",false,null,74480,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 80 Si","Warmwasser-Wandspeicher PSH 80 Si","Warmwasser-Wandspeicher PSH 80 Si","Warmwasser-Wandspeicher PSH 80 Si","Wandboiler PSH 80 Si"]
[null,74481,"Warmwasser-Wandspeicher PSH 100 Si","On request",null,null,null,null,null,null,null,74481,"Warmwasser-Wandspeicher PSH 100 Si","On request",false,null,74481,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 100 Si","Warmwasser-Wandspeicher PSH 100 Si","Warmwasser-Wandspeicher PSH 100 Si","Warmwasser-Wandspeicher PSH 100 Si","Wandboiler PSH 100 Si"]
[null,74482,"Warmwasser-Wandspeicher PSH 120 Si","On request",null,null,null,null,null,null,null,74482,"Warmwasser-Wandspeicher PSH 120 Si","On request",false,null,74482,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 120 Si","Warmwasser-Wandspeicher PSH 120 Si","Warmwasser-Wandspeicher PSH 120 Si","Warmwasser-Wandspeicher PSH 120 Si","Wandboiler PSH 120 Si"]
[null,74483,"Warmwasser-Wandspeicher PSH 150 Si","On request",null,null,null,null,null,null,null,74483,"Warmwasser-Wandspeicher PSH 150 Si","On request",false,null,74483,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 150 Si","Warmwasser-Wandspeicher PSH 150 Si","Warmwasser-Wandspeicher PSH 150 Si","Warmwasser-Wandspeicher PSH 150 Si","Wandboiler PSH 150 Si"]
[null,232080,"Warmwasser-Wandspeicher PSH 30 Trend","On request",null,null,null,null,null,null,null,232080,"Warmwasser-Wandspeicher PSH 30 Trend","On request",false,null,232080,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 30 Trend","Warmwasser-Wandspeicher PSH 30 Trend","Warmwasser-Wandspeicher PSH 30 Trend","Warmwasser-Wandspeicher PSH 30 Trend","Warmwasser-Wandspeicher PSH 30 Trend"]
[null,232081,"Warmwasser-Wandspeicher PSH 50 Trend","On request",null,null,null,null,null,null,null,232081,"Warmwasser-Wandspeicher PSH 50 Trend","On request",false,null,232081,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 50 Trend","Warmwasser-Wandspeicher PSH 50 Trend","Warmwasser-Wandspeicher PSH 50 Trend","Warmwasser-Wandspeicher PSH 50 Trend","Warmwasser-Wandspeicher PSH 50 Trend"]
[null,232082,"Warmwasser-Wandspeicher PSH 80 Trend","On request",null,null,null,null,null,null,null,232082,"Warmwasser-Wandspeicher PSH 80 Trend","On request",false,null,232082,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 80 Trend","Warmwasser-Wandspeicher PSH 80 Trend","Warmwasser-Wandspeicher PSH 80 Trend","Warmwasser-Wandspeicher PSH 80 Trend","Warmwasser-Wandspeicher PSH 80 Trend"]
[null,232083,"Warmwasser-Wandspeicher PSH 100 Trend","On request",null,null,null,null,null,null,null,232083,"Warmwasser-Wandspeicher PSH 100 Trend","On request",false,null,232083,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 100 Trend","Warmwasser-Wandspeicher PSH 100 Trend","Warmwasser-Wandspeicher PSH 100 Trend","Warmwasser-Wandspeicher PSH 100 Trend","Warmwasser-Wandspeicher PSH 100 Trend"]
[null,232084,"Warmwasser-Wandspeicher PSH 120 Trend","On request",null,null,null,null,null,null,null,232084,"Warmwasser-Wandspeicher PSH 120 Trend","On request",false,null,232084,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 120 Trend","Warmwasser-Wandspeicher PSH 120 Trend","Warmwasser-Wandspeicher PSH 120 Trend","Warmwasser-Wandspeicher PSH 120 Trend","Warmwasser-Wandspeicher PSH 120 Trend"]
[null,232085,"Warmwasser-Wandspeicher PSH 150 Trend","On request",null,null,null,null,null,null,null,232085,"Warmwasser-Wandspeicher PSH 150 Trend","On request",false,null,232085,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 150 Trend","Warmwasser-Wandspeicher PSH 150 Trend","Warmwasser-Wandspeicher PSH 150 Trend","Warmwasser-Wandspeicher PSH 150 Trend","Warmwasser-Wandspeicher PSH 150 Trend"]
[null,232086,"Warmwasser-Wandspeicher PSH 200 Trend","On request",null,null,null,null,null,null,null,232086,"Warmwasser-Wandspeicher PSH 200 Trend","On request",false,null,232086,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 200 Trend","Warmwasser-Wandspeicher PSH 200 Trend","Warmwasser-Wandspeicher PSH 200 Trend","Warmwasser-Wandspeicher PSH 200 Trend","Warmwasser-Wandspeicher PSH 200 Trend"]
[null,222215,"Warmwasser-Wandspeicher PSH 30 TM","On request",null,null,null,null,null,null,null,222215,"Warmwasser-Wandspeicher PSH 30 TM","On request",false,null,222215,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 30 TM","Warmwasser-Wandspeicher PSH 30 TM","Warmwasser-Wandspeicher PSH 30 TM","Warmwasser-Wandspeicher PSH 30 TM","Warmwasser-Wandspeicher PSH 30 TM"]
[null,222216,"Warmwasser-Wandspeicher PSH 50 TM","On request",null,null,null,null,null,null,null,222216,"Warmwasser-Wandspeicher PSH 50 TM","On request",false,null,222216,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 50 TM","Warmwasser-Wandspeicher PSH 50 TM","Warmwasser-Wandspeicher PSH 50 TM","Warmwasser-Wandspeicher PSH 50 TM","Warmwasser-Wandspeicher PSH 50 TM"]
[null,222217,"Warmwasser-Wandspeicher PSH 80 TM","On request",null,null,null,null,null,null,null,222217,"Warmwasser-Wandspeicher PSH 80 TM","On request",false,null,222217,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 80 TM","Warmwasser-Wandspeicher PSH 80 TM","Warmwasser-Wandspeicher PSH 80 TM","Warmwasser-Wandspeicher PSH 80 TM","Warmwasser-Wandspeicher PSH 80 TM"]
[null,222218,"Warmwasser-Wandspeicher PSH 100 TM","On request",null,null,null,null,null,null,null,222218,"Warmwasser-Wandspeicher PSH 100 TM","On request",false,null,222218,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 100 TM","Warmwasser-Wandspeicher PSH 100 TM","Warmwasser-Wandspeicher PSH 100 TM","Warmwasser-Wandspeicher PSH 100 TM","Warmwasser-Wandspeicher PSH 100 TM"]
[null,222231,"Warmwasser-Wandspeicher PSH 120 TM","On request",null,null,null,null,null,null,null,222231,"Warmwasser-Wandspeicher PSH 120 TM","On request",false,null,222231,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 120 TM","Warmwasser-Wandspeicher PSH 120 TM","Warmwasser-Wandspeicher PSH 120 TM","Warmwasser-Wandspeicher PSH 120 TM","Warmwasser-Wandspeicher PSH 120 TM"]
[null,222232,"Warmwasser-Wandspeicher PSH 150 TM","On request",null,null,null,null,null,null,null,222232,"Warmwasser-Wandspeicher PSH 150 TM","On request",false,null,222232,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 150 TM","Warmwasser-Wandspeicher PSH 150 TM","Warmwasser-Wandspeicher PSH 150 TM","Warmwasser-Wandspeicher PSH 150 TM","Warmwasser-Wandspeicher PSH 150 TM"]
[null,222233,"Warmwasser-Wandspeicher PSH 200 TM","On request",null,null,null,null,null,null,null,222233,"Warmwasser-Wandspeicher PSH 200 TM","On request",false,null,222233,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wandspeicher PSH 200 TM","Warmwasser-Wandspeicher PSH 200 TM","Warmwasser-Wandspeicher PSH 200 TM","Warmwasser-Wandspeicher PSH 200 TM","Warmwasser-Wandspeicher PSH 200 TM"]
[null,73945,"Sicherheitsventil SV EX 1/2","On request",null,null,null,null,null,null,null,73945,"Sicherheitsventil SV EX 1/2","On request",false,null,73945,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sicherheitsventil SV EX 1/2","Sicherheitsventil SV EX 1/2","Sicherheitsventil SV EX 1/2","Sicherheitsventil SV EX 1/2","Veiligheidsklep SV EX 1/2"]
[null,73946,"Sicherheitsventil SV EX 3/4","On request",null,null,null,null,null,null,null,73946,"Sicherheitsventil SV EX 3/4","On request",false,null,73946,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sicherheitsventil SV EX 3/4","Sicherheitsventil SV EX 3/4","Sicherheitsventil SV EX 3/4","Sicherheitsventil SV EX 3/4","Veiligheidsklep SV EX 3/4"]
[null,221127,"Warmwasser-Kleinspeicher SN 5 SLi","On request",null,null,null,null,null,null,null,221127,"Warmwasser-Kleinspeicher SN 5 SLi","On request",false,null,221127,"auf Anfrage","On request",170,"på forespørgsel","op aanvraag","Warmwasser-Kleinspeicher SN 5 SLi","Warmwasser-Kleinspeicher SN 5 SLi","Warmwasser-Kleinspeicher SN 5 SLi","Warmwasser-Kleinspeicher SN 5 SLi","Warmwasser-Kleinspeicher SN 5 SLi"]
[null,221121,"Warmwasser-Kleinspeicher SNU 5 SLi","On request",null,null,null,null,null,null,null,221121,"Warmwasser-Kleinspeicher SNU 5 SLi","On request",false,null,221121,"auf Anfrage","On request",170,"på forespørgsel","op aanvraag","Warmwasser-Kleinspeicher SNU 5 SLi","Warmwasser-Kleinspeicher SNU 5 SLi","Warmwasser-Kleinspeicher SNU 5 SLi","Warmwasser-Kleinspeicher SNU 5 SLi","Warmwasser-Kleinspeicher SNU 5 SLi"]
[null,222193,"Warmwasser-Kleinspeicher SN 10 SLi","On request",null,null,null,null,null,null,null,222193,"Warmwasser-Kleinspeicher SN 10 SLi","On request",false,null,222193,"auf Anfrage","On request",295,"på forespørgsel","op aanvraag","Warmwasser-Kleinspeicher SN 10 SLi","Warmwasser-Kleinspeicher SN 10 SLi","Warmwasser-Kleinspeicher SN 10 SLi","Warmwasser-Kleinspeicher SN 10 SLi","Warmwasser-Kleinspeicher SN 10 SLi"]
[null,222199,"Warmwasser-Kleinspeicher SNU 10 SLi","On request",null,null,null,null,null,null,null,222199,"Warmwasser-Kleinspeicher SNU 10 SLi","On request",false,null,222199,"auf Anfrage","On request",300,"på forespørgsel","op aanvraag","Warmwasser-Kleinspeicher SNU 10 SLi","Warmwasser-Kleinspeicher SNU 10 SLi","Warmwasser-Kleinspeicher SNU 10 SLi","Warmwasser-Kleinspeicher SNU 10 SLi","Warmwasser-Kleinspeicher SNU 10 SLi"]
[null,222204,"Warmwasser-Kleinspeicher SN 15 SLi","On request",null,null,null,null,null,null,null,222204,"Warmwasser-Kleinspeicher SN 15 SLi","On request",{"$f":"IF(AND(B1894=L1894,C1894=M1894,D1894=N1894),FALSE,TRUE)","v":false},null,222204,"auf Anfrage","On request",480,"på forespørgsel","op aanvraag","Warmwasser-Kleinspeicher SN 15 SLi","Warmwasser-Kleinspeicher SN 15 SLi","Warmwasser-Kleinspeicher SN 15 SLi","Warmwasser-Kleinspeicher SN 15 SLi","Warmwasser-Kleinspeicher SN 15 SLi"]
[null,222176,"Warmwasser-Kleinspeicher UFP 5 t Si","On request",null,null,null,null,null,null,null,222176,"Warmwasser-Kleinspeicher UFP 5 t Si","On request",false,null,222176,"auf Anfrage","On request",145,"på forespørgsel","op aanvraag","Warmwasser-Kleinspeicher UFP 5 t Si","Warmwasser-Kleinspeicher UFP 5 t Si","Warmwasser-Kleinspeicher UFP 5 t Si","Warmwasser-Kleinspeicher UFP 5 t Si","Warmwasser-Kleinspeicher UFP 5 t SLi"]
[null,229476,"Warmwasser-Kleinspeicher SH 10 SLi","On request",null,null,null,null,null,null,null,229476,"Warmwasser-Kleinspeicher SH 10 SLi","On request",false,null,229476,"auf Anfrage","On request",505,"på forespørgsel",224,"Warmwasser-Kleinspeicher SH 10 SLi","Warmwasser-Kleinspeicher SH 10 SLi","Warmwasser-Kleinspeicher SH 10 SLi","Warmwasser-Kleinspeicher SH 10 SLi","Boiler SHU 10 SLi"]
[null,229478,"Warmwasser-Kleinspeicher SH 15 SLi","On request",null,null,null,null,null,null,null,229478,"Warmwasser-Kleinspeicher SH 15 SLi","On request",false,null,229478,"auf Anfrage","On request",710,"på forespørgsel","op aanvraag","Warmwasser-Kleinspeicher SH 15 SLi","Warmwasser-Kleinspeicher SH 15 SLi","Warmwasser-Kleinspeicher SH 15 SLi","Warmwasser-Kleinspeicher SH 15 SLi","Warmwasser-Kleinspeicher SH 15 SLi"]
[null,222151,"Warmwasser-Kleinspeicher SHU 5 SLi","On request",null,null,null,null,null,null,null,222151,"Warmwasser-Kleinspeicher SHU 5 SLi","On request",false,null,222151,"auf Anfrage","On request",445,"på forespørgsel",224,"Warmwasser-Kleinspeicher SHU 5 SLi","Warmwasser-Kleinspeicher SHU 5 SLi","Warmwasser-Kleinspeicher SHU 5 SLi","Warmwasser-Kleinspeicher SHU 5 SLi","SHU 5 SLi  "]
[null,229473,"Warmwasser-Kleinspeicher SHU 10 SLi","On request",null,null,null,null,null,null,null,229473,"Warmwasser-Kleinspeicher SHU 10 SLi","On request",false,null,229473,"auf Anfrage","On request",505,"på forespørgsel",224,"Warmwasser-Kleinspeicher SHU 10 SLi","Warmwasser-Kleinspeicher SHU 10 SLi","Warmwasser-Kleinspeicher SHU 10 SLi","Warmwasser-Kleinspeicher SHU 10 SLi","Boiler SHU 10 SLi"]
[null,229501,"Warmwasser-Kleinspeicher PSH 15 MINI ID","On request",null,null,null,null,null,null,null,229501,"Warmwasser-Kleinspeicher PSH 15 MINI ID","On request",false,null,229501,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Kleinspeicher PSH 15 MINI ID","Warmwasser-Kleinspeicher PSH 15 MINI ID","Warmwasser-Kleinspeicher PSH 15 MINI ID","Warmwasser-Kleinspeicher PSH 15 MINI ID","Boiler PSH 15 MINI ID"]
[null,70074,"Warmwasser-Standspeicher SHW 200 ACE","On request",null,null,null,null,null,null,null,70074,"Warmwasser-Standspeicher SHW 200 ACE","On request",false,null,70074,"auf Anfrage","On request","1.615,00","på forespørgsel",1318,"Warmwasser-Standspeicher SHW 200 ACE","Warmwasser-Standspeicher SHW 200 ACE","Warmwasser-Standspeicher SHW 200 ACE","Warmwasser-Standspeicher SHW 200 ACE","Staande boiler SHW 200 ACE"]
[null,70075,"Warmwasser-Standspeicher SHW 300 ACE","On request",null,null,null,null,null,null,null,70075,"Warmwasser-Standspeicher SHW 300 ACE","On request",false,null,70075,"auf Anfrage","On request","1.660,00","på forespørgsel",1474,"Warmwasser-Standspeicher SHW 300 ACE","Warmwasser-Standspeicher SHW 300 ACE","Warmwasser-Standspeicher SHW 300 ACE","Warmwasser-Standspeicher SHW 300 ACE","Staande boiler SHW 300 ACE"]
[null,70076,"Warmwasser-Standspeicher SHW 400 ACE","On request",null,null,null,null,null,null,null,70076,"Warmwasser-Standspeicher SHW 400 ACE","On request",false,null,70076,"auf Anfrage","On request","1.775,00","på forespørgsel",1684,"Warmwasser-Standspeicher SHW 400 ACE","Warmwasser-Standspeicher SHW 400 ACE","Warmwasser-Standspeicher SHW 400 ACE","Warmwasser-Standspeicher SHW 400 ACE","Staande boiler SHW 400 ACE"]
[null,75140,"Elektro-Heizflansch FCR 28/120 Si","On request",null,null,null,null,null,null,null,75140,"Elektro-Heizflansch FCR 28/120 Si","On request",false,null,75140,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Elektro-Heizflansch FCR 28/120 Si","Elektro-Heizflansch FCR 28/120 Si","Elektro-Heizflansch FCR 28/120 Si","Elektro-Heizflansch FCR 28/120 Si","Electrische verwarmingsflens FCR 28/120 Si"]
[null,75131,"Elektro-Heizflansch FCR 28/180 Si","On request",null,null,null,null,null,null,null,75131,"Elektro-Heizflansch FCR 28/180 Si","On request",false,null,75131,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Elektro-Heizflansch FCR 28/180 Si","Elektro-Heizflansch FCR 28/180 Si","Elektro-Heizflansch FCR 28/180 Si","Elektro-Heizflansch FCR 28/180 Si","Electrische verwarmingsflens FCR 28/180 Si"]
[null,75141,"Elektro-Heizflansch FCR 28/270 Si","On request",null,null,null,null,null,null,null,75141,"Elektro-Heizflansch FCR 28/270 Si","On request",false,null,75141,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Elektro-Heizflansch FCR 28/270 Si","Elektro-Heizflansch FCR 28/270 Si","Elektro-Heizflansch FCR 28/270 Si","Elektro-Heizflansch FCR 28/270 Si","Electrische verwarmingsflens FCR 28/270 Si"]
[null,75124,"Elektro-Heizflansch FCR 28/360 Si","On request",null,null,null,null,null,null,null,75124,"Elektro-Heizflansch FCR 28/360 Si","On request",false,null,75124,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Elektro-Heizflansch FCR 28/360 Si","Elektro-Heizflansch FCR 28/360 Si","Elektro-Heizflansch FCR 28/360 Si","Elektro-Heizflansch FCR 28/360 Si","Electrische verwarmingsflens FCR 28/360 Si"]
[null,73007,"Händetrockner HTE 4","On request",null,null,null,null,null,null,null,73007,"Händetrockner HTE 4","On request",false,null,73007,"auf Anfrage","On request",215,"på forespørgsel",252,"Händetrockner HTE 4","Händetrockner HTE 4","Händetrockner HTE 4","Händetrockner HTE 4","Handendroger HTE 4"]
[null,73008,"Händetrockner HTE 5","On request",null,null,null,null,null,null,null,73008,"Händetrockner HTE 5","On request",false,null,73008,"auf Anfrage","On request",360,"på forespørgsel",355,"Händetrockner HTE 5","Händetrockner HTE 5","Händetrockner HTE 5","Händetrockner HTE 5","Handendroger HTE 5"]
[null,232492,"Luft|Wasser-Wärmepumpe WPL 25 AS","On request",null,null,null,null,null,null,null,232492,"Luft|Wasser-Wärmepumpe WPL 25 AS","On request",false,null,232492,"auf Anfrage","On request","9.790,00","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 25 AS","Luft|Wasser-Wärmepumpe WPL 25 AS","Luft|Wasser-Wärmepumpe WPL 25 AS","Luft|Wasser-Wärmepumpe WPL 25 AS","Luft|Wasser-Wärmepumpe WPL 25 AS"]
[null,229937,"Luft|Wasser-Wärmepumpe WPL 33 HT S","On request",null,null,null,null,null,null,null,229937,"Luft|Wasser-Wärmepumpe WPL 33 HT S","On request",false,null,229937,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 33 HT S","Luft|Wasser-Wärmepumpe WPL 33 HT S","Luft|Wasser-Wärmepumpe WPL 33 HT S","Luft|Wasser-Wärmepumpe WPL 33 HT S","Lucht - Water warmtepomp WPL 33 HT S"]
[null,227995,"Luft|Wasser-Wärmepumpe WPL 10 ACS","On request",null,null,null,null,null,null,null,227995,"Luft|Wasser-Wärmepumpe WPL 10 ACS","On request",false,null,227995,"auf Anfrage","On request","7.120,00","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 10 ACS","Luft|Wasser-Wärmepumpe WPL 10 ACS","Luft|Wasser-Wärmepumpe WPL 10 ACS","Luft|Wasser-Wärmepumpe WPL 10 ACS","Lucht - Water warmtepomp WPL 10 ACS"]
[null,230385,"Luft|Wasser-Wärmepumpe WPL 13 basic","On request",null,null,null,null,null,null,null,230385,"Luft|Wasser-Wärmepumpe WPL 13 basic","On request",false,null,230385,"auf Anfrage","On request","7.400,00","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 13 basic","Luft|Wasser-Wärmepumpe WPL 13 basic","Luft|Wasser-Wärmepumpe WPL 13 basic","Luft|Wasser-Wärmepumpe WPL 13 basic","Lucht - Water warmtepomp WPL 13 basic"]
[null,230386,"Luft|Wasser-Wärmepumpe WPL 20 basic","On request",null,null,null,null,null,null,null,230386,"Luft|Wasser-Wärmepumpe WPL 20 basic","On request",false,null,230386,"auf Anfrage","On request","8.100,00","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 20 basic","Luft|Wasser-Wärmepumpe WPL 20 basic","Luft|Wasser-Wärmepumpe WPL 20 basic","Luft|Wasser-Wärmepumpe WPL 20 basic","Lucht - Water warmtepomp WPL 20 basic"]
[null,230387,"Luft|Wasser-Wärmepumpe WPL 13 basic S","On request",null,null,null,null,null,null,null,230387,"Luft|Wasser-Wärmepumpe WPL 13 basic S","On request",false,null,230387,"auf Anfrage","On request","7.400,00","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 13 basic S","Luft|Wasser-Wärmepumpe WPL 13 basic S","Luft|Wasser-Wärmepumpe WPL 13 basic S","Luft|Wasser-Wärmepumpe WPL 13 basic S","Lucht - Water warmtepomp WPL 13 basic S"]
[null,230388,"Luft|Wasser-Wärmepumpe WPL 18 basic S","On request",null,null,null,null,null,null,null,230388,"Luft|Wasser-Wärmepumpe WPL 18 basic S","On request",false,null,230388,"auf Anfrage","On request","7.700,00","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 18 basic S","Luft|Wasser-Wärmepumpe WPL 18 basic S","Luft|Wasser-Wärmepumpe WPL 18 basic S","Luft|Wasser-Wärmepumpe WPL 18 basic S","Lucht - Water warmtepomp WPL 18 basic S"]
[null,185348,"Luft|Wasser-Wärmepumpe WPL 33","On request",null,null,null,null,null,null,null,185348,"Luft|Wasser-Wärmepumpe WPL 33","On request",false,null,185348,"auf Anfrage","On request","12.910,00","på forespørgsel","op aanvraag","Luft|Wasser-Wärmepumpe WPL 33","Luft|Wasser-Wärmepumpe WPL 33","Luft|Wasser-Wärmepumpe WPL 33","Luft|Wasser-Wärmepumpe WPL 33","Lucht/water-warmtepompen WPL 33"]
[null,185368,"Verkleidung WPL 33 Innenaufstellung","On request",null,null,null,null,null,null,null,185368,"Verkleidung WPL 33 Innenaufstellung","On request",false,null,185368,"auf Anfrage","On request","1.690,00","på forespørgsel","op aanvraag","Verkleidung WPL 33 Innenaufstellung","Verkleidung WPL 33 Innenaufstellung","Verkleidung WPL 33 Innenaufstellung","Verkleidung WPL 33 Innenaufstellung","Behuizing WPL 33 binnenopstelling"]
[null,185369,"Verkleidung WPL 33 Außenaufstellung","On request",null,null,null,null,null,null,null,185369,"Verkleidung WPL 33 Außenaufstellung","On request",false,null,185369,"auf Anfrage","On request","1.980,00","på forespørgsel","op aanvraag","Verkleidung WPL 33 Außenaufstellung","Verkleidung WPL 33 Außenaufstellung","Verkleidung WPL 33 Außenaufstellung","Verkleidung WPL 33 Außenaufstellung","Behuizing WPL 33 buitenopstelling"]
[null,230384,"Verkleidung WPL basic Außenaufstellung","On request",null,null,null,null,null,null,null,230384,"Verkleidung WPL basic Außenaufstellung","On request",false,null,230384,"auf Anfrage","On request","1.300,00","på forespørgsel","op aanvraag","Verkleidung WPL basic Außenaufstellung","Verkleidung WPL basic Außenaufstellung","Verkleidung WPL basic Außenaufstellung","Verkleidung WPL basic Außenaufstellung","Accessoires WPL basic externe installatie"]
[null,232937,"Sole|Wasser-Wärmepumpe WPC 05 S","On request",null,null,null,null,null,null,null,232937,"Sole|Wasser-Wärmepumpe WPC 05 S","On request",false,null,232937,"auf Anfrage","On request","9.975,00","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPC 05 S","Sole|Wasser-Wärmepumpe WPC 05 S","Sole|Wasser-Wärmepumpe WPC 05 S","Sole|Wasser-Wärmepumpe WPC 05 S","Sole|Wasser-Wärmepumpe WPC 05 S"]
[null,232938,"Sole|Wasser-Wärmepumpe WPC 07 S","On request",null,null,null,null,null,null,null,232938,"Sole|Wasser-Wärmepumpe WPC 07 S","On request",false,null,232938,"auf Anfrage","On request","10.350,00","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPC 07 S","Sole|Wasser-Wärmepumpe WPC 07 S","Sole|Wasser-Wärmepumpe WPC 07 S","Sole|Wasser-Wärmepumpe WPC 07 S","Sole|Wasser-Wärmepumpe WPC 07 S"]
[null,232939,"Sole|Wasser-Wärmepumpe WPC 10 S","On request",null,null,null,null,null,null,null,232939,"Sole|Wasser-Wärmepumpe WPC 10 S","On request",false,null,232939,"auf Anfrage","On request","10.785,00","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPC 10 S","Sole|Wasser-Wärmepumpe WPC 10 S","Sole|Wasser-Wärmepumpe WPC 10 S","Sole|Wasser-Wärmepumpe WPC 10 S","Sole|Wasser-Wärmepumpe WPC 10 S"]
[null,232940,"Sole|Wasser-Wärmepumpe WPC 13 S","On request",null,null,null,null,null,null,null,232940,"Sole|Wasser-Wärmepumpe WPC 13 S","On request",false,null,232940,"auf Anfrage","On request","11.030,00","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPC 13 S","Sole|Wasser-Wärmepumpe WPC 13 S","Sole|Wasser-Wärmepumpe WPC 13 S","Sole|Wasser-Wärmepumpe WPC 13 S","Sole|Wasser-Wärmepumpe WPC 13 S"]
[null,232922,"Sole|Wasser-Wärmepumpe WPF 05 S","On request",null,null,null,null,null,null,null,232922,"Sole|Wasser-Wärmepumpe WPF 05 S","On request",false,null,232922,"auf Anfrage","On request","8.295,00","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 05 S","Sole|Wasser-Wärmepumpe WPF 05 S","Sole|Wasser-Wärmepumpe WPF 05 S","Sole|Wasser-Wärmepumpe WPF 05 S","Sole|Wasser-Wärmepumpe WPF 05 S"]
[null,232923,"Sole|Wasser-Wärmepumpe WPF 07 S","On request",null,null,null,null,null,null,null,232923,"Sole|Wasser-Wärmepumpe WPF 07 S","On request",false,null,232923,"auf Anfrage","On request","8.665,00","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 07 S","Sole|Wasser-Wärmepumpe WPF 07 S","Sole|Wasser-Wärmepumpe WPF 07 S","Sole|Wasser-Wärmepumpe WPF 07 S","Sole|Wasser-Wärmepumpe WPF 07 S"]
[null,232924,"Sole|Wasser-Wärmepumpe WPF 10 S","On request",null,null,null,null,null,null,null,232924,"Sole|Wasser-Wärmepumpe WPF 10 S","On request",false,null,232924,"auf Anfrage","On request","9.010,00","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 10 S","Sole|Wasser-Wärmepumpe WPF 10 S","Sole|Wasser-Wärmepumpe WPF 10 S","Sole|Wasser-Wärmepumpe WPF 10 S","Sole|Wasser-Wärmepumpe WPF 10 S"]
[null,232925,"Sole|Wasser-Wärmepumpe WPF 13 S","On request",null,null,null,null,null,null,null,232925,"Sole|Wasser-Wärmepumpe WPF 13 S","On request",false,null,232925,"auf Anfrage","On request","9.322,00","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 13 S","Sole|Wasser-Wärmepumpe WPF 13 S","Sole|Wasser-Wärmepumpe WPF 13 S","Sole|Wasser-Wärmepumpe WPF 13 S","Sole|Wasser-Wärmepumpe WPF 13 S"]
[null,74425,"Sole|Wasser-Wärmepumpe WPF 5 S basic","On request",null,null,null,null,null,null,null,74425,"Sole|Wasser-Wärmepumpe WPF 5 S basic","On request",false,null,74425,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 5 S basic","Sole|Wasser-Wärmepumpe WPF 5 S basic","Sole|Wasser-Wärmepumpe WPF 5 S basic","Sole|Wasser-Wärmepumpe WPF 5 S basic","Brine|water warmtepomp WPF 5 S"]
[null,74426,"Sole|Wasser-Wärmepumpe WPF 7 S basic","On request",null,null,null,null,null,null,null,74426,"Sole|Wasser-Wärmepumpe WPF 7 S basic","On request",false,null,74426,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 7 S basic","Sole|Wasser-Wärmepumpe WPF 7 S basic","Sole|Wasser-Wärmepumpe WPF 7 S basic","Sole|Wasser-Wärmepumpe WPF 7 S basic","Brine|water warmtepomp WPF 7 S"]
[null,220819,"Sole|Wasser-Wärmepumpe WPF 10 S basic","On request",null,null,null,null,null,null,null,220819,"Sole|Wasser-Wärmepumpe WPF 10 S basic","On request",false,null,220819,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 10 S basic","Sole|Wasser-Wärmepumpe WPF 10 S basic","Sole|Wasser-Wärmepumpe WPF 10 S basic","Sole|Wasser-Wärmepumpe WPF 10 S basic","Brine|water warmtepomp WPF 10 S"]
[null,222553,"Sole|Wasser-Wärmepumpe WPF 7 MS","On request",null,null,null,null,null,null,null,222553,"Sole|Wasser-Wärmepumpe WPF 7 MS","On request",false,null,222553,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 7 MS","Sole|Wasser-Wärmepumpe WPF 7 MS","Sole|Wasser-Wärmepumpe WPF 7 MS","Sole|Wasser-Wärmepumpe WPF 7 MS","Brine|water warmtepomp WPF 7 MS"]
[null,222552,"Sole|Wasser-Wärmepumpe WPF 10 MS","On request",null,null,null,null,null,null,null,222552,"Sole|Wasser-Wärmepumpe WPF 10 MS","On request",false,null,222552,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 10 MS","Sole|Wasser-Wärmepumpe WPF 10 MS","Sole|Wasser-Wärmepumpe WPF 10 MS","Sole|Wasser-Wärmepumpe WPF 10 MS","Brine|water warmtepomp WPF 10 MS"]
[null,223416,"Sole|Wasser-Wärmepumpe WPF 14 Set S","On request",null,null,null,null,null,null,null,223416,"Sole|Wasser-Wärmepumpe WPF 14 Set S","On request",false,null,223416,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 14 Set S","Sole|Wasser-Wärmepumpe WPF 14 Set S","Sole|Wasser-Wärmepumpe WPF 14 Set S","Sole|Wasser-Wärmepumpe WPF 14 Set S","Brine|water warmtepomp WPF 14 Set S"]
[null,223417,"Sole|Wasser-Wärmepumpe WPF 17 Set S","On request",null,null,null,null,null,null,null,223417,"Sole|Wasser-Wärmepumpe WPF 17 Set S","On request",false,null,223417,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 17 Set S","Sole|Wasser-Wärmepumpe WPF 17 Set S","Sole|Wasser-Wärmepumpe WPF 17 Set S","Sole|Wasser-Wärmepumpe WPF 17 Set S","Brine|water warmtepomp WPF 17 Set S"]
[null,223418,"Sole|Wasser-Wärmepumpe WPF 20 Set S","On request",null,null,null,null,null,null,null,223418,"Sole|Wasser-Wärmepumpe WPF 20 Set S","On request",false,null,223418,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Sole|Wasser-Wärmepumpe WPF 20 Set S","Sole|Wasser-Wärmepumpe WPF 20 Set S","Sole|Wasser-Wärmepumpe WPF 20 Set S","Sole|Wasser-Wärmepumpe WPF 20 Set S","Brine|water warmtepomp WPF 20 Set S"]
[null,222422,"Warmwasser-Wärmepumpe WWK 300 A","On request",null,null,null,null,null,null,null,222422,"Warmwasser-Wärmepumpe WWK 300 A","On request",false,null,222422,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 300 A","Warmwasser-Wärmepumpe WWK 300 A","Warmwasser-Wärmepumpe WWK 300 A","Warmwasser-Wärmepumpe WWK 300 A","Warmtepompboiler WWK 300 A"]
[null,227070,"Warmwasser-Wärmepumpe WWK 300 AH","On request",null,null,null,null,null,null,null,227070,"Warmwasser-Wärmepumpe WWK 300 AH","On request",false,null,227070,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 300 AH","Warmwasser-Wärmepumpe WWK 300 AH","Warmwasser-Wärmepumpe WWK 300 AH","Warmwasser-Wärmepumpe WWK 300 AH","Warmtepompboiler WWK 300 AH"]
[null,227072,"Warmwasser-Wärmepumpe WWK 300 GP","On request",null,null,null,null,null,null,null,227072,"Warmwasser-Wärmepumpe WWK 300 GP","On request",false,null,227072,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe WWK 300 GP","Warmwasser-Wärmepumpe WWK 300 GP","Warmwasser-Wärmepumpe WWK 300 GP","Warmwasser-Wärmepumpe WWK 300 GP","Warmtepompboiler WWK 300 GP"]
[null,222423,"Warmwasser-Wärmepumpe Accelera 300","On request",null,null,null,null,null,null,null,222423,"Warmwasser-Wärmepumpe Accelera 300","On request",false,null,222423,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Warmwasser-Wärmepumpe Accelera 300","Warmwasser-Wärmepumpe Accelera 300","Warmwasser-Wärmepumpe Accelera 300","Warmwasser-Wärmepumpe Accelera 300","Warmwasser-Wärmepumpe Accelera 300"]
[null,185350,"Warmwasser-Wärmepumpe WM 300","On request",null,null,null,null,null,null,null,185350,"Warmwasser-Wärmepumpe WM 300","On request",false,null,185350,"auf Anfrage","On request","sur demande","på forespørgsel",3696,"Warmwasser-Wärmepumpe WM 300","Warmwasser-Wärmepumpe WM 300","Warmwasser-Wärmepumpe WM 300","Warmwasser-Wärmepumpe WM 300","Centraal ventilatietoestel WM 300"]
[null,234921,"Wärmepumpen-Manager WPMW 3 International","On request",null,null,null,null,null,null,null,234921,"Wärmepumpen-Manager WPMW 3 International","On request",false,null,234921,"auf Anfrage","On request","sur demande","på forespørgsel",866,"Wärmepumpen-Manager WPMW 3 International","Wärmepumpen-Manager WPMW 3 International","Wärmepumpen-Manager WPMW 3 International","Wärmepumpen-Manager WPMW 3 International","Warmtepompmanager WPMS 3 international"]
[null,234922,"Wärmepumpen-Manager WPMS 3 International","On request",null,null,null,null,null,null,null,234922,"Wärmepumpen-Manager WPMS 3 International","On request",false,null,234922,"auf Anfrage","On request","sur demande","på forespørgsel",942,"Wärmepumpen-Manager WPMS 3 International","Wärmepumpen-Manager WPMS 3 International","Wärmepumpen-Manager WPMS 3 International","Wärmepumpen-Manager WPMS 3 International","Warmtepompmanager WPMW 3 international"]
[null,220833,"Anlaufstrombegrenzer WPAB 25","On request",null,null,null,null,null,null,null,220833,"Anlaufstrombegrenzer WPAB 25","On request",false,null,220833,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Anlaufstrombegrenzer WPAB 25","Anlaufstrombegrenzer WPAB 25","Anlaufstrombegrenzer WPAB 25","Anlaufstrombegrenzer WPAB 25","Soft starter WPAB"]
[null,232412,"Anlaufstrombegrenzer WPAB 32","On request",null,null,null,null,null,null,null,232412,"Anlaufstrombegrenzer WPAB 32","On request",false,null,232412,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Anlaufstrombegrenzer WPAB 32","Anlaufstrombegrenzer WPAB 32","Anlaufstrombegrenzer WPAB 32","Anlaufstrombegrenzer WPAB 32","Anlaufstrombegrenzer WPAB 32"]
[null,182059,"Wärmespeicher ETC 085 M","On request",null,null,null,null,null,null,null,182059,"Wärmespeicher ETC 085 M","On request",false,null,182059,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher ETC 085 M","Wärmespeicher ETC 085 M","Wärmespeicher ETC 085 M","Wärmespeicher ETC 085 M","Accumulatiekachel ETC 085 M"]
[null,182060,"Wärmespeicher ETC 170 M","On request",null,null,null,null,null,null,null,182060,"Wärmespeicher ETC 170 M","On request",false,null,182060,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher ETC 170 M","Wärmespeicher ETC 170 M","Wärmespeicher ETC 170 M","Wärmespeicher ETC 170 M","Accumulatiekachel ETC 170 M"]
[null,182061,"Wärmespeicher ETC 250 M","On request",null,null,null,null,null,null,null,182061,"Wärmespeicher ETC 250 M","On request",false,null,182061,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher ETC 250 M","Wärmespeicher ETC 250 M","Wärmespeicher ETC 250 M","Wärmespeicher ETC 250 M","Accumulatiekachel ETC 250 M"]
[null,182062,"Wärmespeicher ETC 340 M ","On request",null,null,null,null,null,null,null,182062,"Wärmespeicher ETC 340 M ","On request",false,null,182062,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher ETC 340 M ","Wärmespeicher ETC 340 M ","Wärmespeicher ETC 340 M ","Wärmespeicher ETC 340 M ","Accumulatiekachel ETC 340 M "]
[null,182063,"Wärmespeicher ETC 170 A ","On request",null,null,null,null,null,null,null,182063,"Wärmespeicher ETC 170 A ","On request",false,null,182063,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher ETC 170 A ","Wärmespeicher ETC 170 A ","Wärmespeicher ETC 170 A ","Wärmespeicher ETC 170 A ","Accumulatiekachel ETC 170 A "]
[null,182064,"Wärmespeicher ETC 250 A ","On request",null,null,null,null,null,null,null,182064,"Wärmespeicher ETC 250 A ","On request",false,null,182064,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher ETC 250 A ","Wärmespeicher ETC 250 A ","Wärmespeicher ETC 250 A ","Wärmespeicher ETC 250 A ","Accumulatiekachel ETC 250 A "]
[null,182065,"Wärmespeicher ETC 340 A","On request",null,null,null,null,null,null,null,182065,"Wärmespeicher ETC 340 A","On request",false,null,182065,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wärmespeicher ETC 340 A","Wärmespeicher ETC 340 A","Wärmespeicher ETC 340 A","Wärmespeicher ETC 340 A","Accumulatiekachel ETC 340 A"]
[null,220725,"Wandkonvektor CNS 50 U","On request",null,null,null,null,null,null,null,220725,"Wandkonvektor CNS 50 U","On request",false,null,220725,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 50 U","Wandkonvektor CNS 50 U","Wandkonvektor CNS 50 U","Wandkonvektor CNS 50 U","Wandconvector CNS 50 U"]
[null,220726,"Wandkonvektor CNS 75 U","On request",null,null,null,null,null,null,null,220726,"Wandkonvektor CNS 75 U","On request",false,null,220726,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 75 U","Wandkonvektor CNS 75 U","Wandkonvektor CNS 75 U","Wandkonvektor CNS 75 U","Wandconvector CNS 75 U"]
[null,220727,"Wandkonvektor CNS 100 U","On request",null,null,null,null,null,null,null,220727,"Wandkonvektor CNS 100 U","On request",false,null,220727,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 100 U","Wandkonvektor CNS 100 U","Wandkonvektor CNS 100 U","Wandkonvektor CNS 100 U","Wandconvector CNS 100 U"]
[null,220729,"Wandkonvektor CNS 150 U","On request",null,null,null,null,null,null,null,220729,"Wandkonvektor CNS 150 U","On request",false,null,220729,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 150 U","Wandkonvektor CNS 150 U","Wandkonvektor CNS 150 U","Wandkonvektor CNS 150 U","Wandconvector CNS 150 U"]
[null,220731,"Wandkonvektor CNS 200 U","On request",null,null,null,null,null,null,null,220731,"Wandkonvektor CNS 200 U","On request",false,null,220731,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 200 U","Wandkonvektor CNS 200 U","Wandkonvektor CNS 200 U","Wandkonvektor CNS 200 U","Wandconvector CNS 200 U"]
[null,220732,"Wandkonvektor CNS 250 U","On request",null,null,null,null,null,null,null,220732,"Wandkonvektor CNS 250 U","On request",{"$f":"IF(AND(B1958=L1958,C1958=M1958,D1958=N1958),FALSE,TRUE)","v":false},null,220732,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 250 U","Wandkonvektor CNS 250 U","Wandkonvektor CNS 250 U","Wandkonvektor CNS 250 U","Wandconvector CNS 250 U"]
[null,220733,"Wandkonvektor CNS 300 U","On request",null,null,null,null,null,null,null,220733,"Wandkonvektor CNS 300 U","On request",false,null,220733,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 300 U","Wandkonvektor CNS 300 U","Wandkonvektor CNS 300 U","Wandkonvektor CNS 300 U","Wandconvector CNS 300 U"]
[null,229749,"Wandkonvektor CNS 50 UE","On request",null,null,null,null,null,null,null,229749,"Wandkonvektor CNS 50 UE","On request",false,null,229749,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 50 UE","Wandkonvektor CNS 50 UE","Wandkonvektor CNS 50 UE","Wandkonvektor CNS 50 UE","Wandconvector CNS 50 UE"]
[null,229750,"Wandkonvektor CNS 75 UE","On request",null,null,null,null,null,null,null,229750,"Wandkonvektor CNS 75 UE","On request",false,null,229750,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 75 UE","Wandkonvektor CNS 75 UE","Wandkonvektor CNS 75 UE","Wandkonvektor CNS 75 UE","Wandconvector CNS 75 UE"]
[null,229751,"Wandkonvektor CNS 100 UE","On request",null,null,null,null,null,null,null,229751,"Wandkonvektor CNS 100 UE","On request",false,null,229751,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 100 UE","Wandkonvektor CNS 100 UE","Wandkonvektor CNS 100 UE","Wandkonvektor CNS 100 UE","Wandconvector CNS 100 UE"]
[null,229753,"Wandkonvektor CNS 150 UE","On request",null,null,null,null,null,null,null,229753,"Wandkonvektor CNS 150 UE","On request",false,null,229753,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 150 UE","Wandkonvektor CNS 150 UE","Wandkonvektor CNS 150 UE","Wandkonvektor CNS 150 UE","Wandconvector CNS 150 UE"]
[null,229755,"Wandkonvektor CNS 200 UE","On request",null,null,null,null,null,null,null,229755,"Wandkonvektor CNS 200 UE","On request",false,null,229755,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 200 UE","Wandkonvektor CNS 200 UE","Wandkonvektor CNS 200 UE","Wandkonvektor CNS 200 UE","Wandconvector CNS 200 UE"]
[null,229756,"Wandkonvektor CNS 250 UE","On request",null,null,null,null,null,null,null,229756,"Wandkonvektor CNS 250 UE","On request",false,null,229756,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 250 UE","Wandkonvektor CNS 250 UE","Wandkonvektor CNS 250 UE","Wandkonvektor CNS 250 UE","Wandconvector CNS 250 UE"]
[null,229757,"Wandkonvektor CNS 300 UE","On request",null,null,null,null,null,null,null,229757,"Wandkonvektor CNS 300 UE","On request",false,null,229757,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 300 UE","Wandkonvektor CNS 300 UE","Wandkonvektor CNS 300 UE","Wandkonvektor CNS 300 UE","Wandconvector CNS 300 UE"]
[null,229789,"Wandkonvektor CNS 75 F","On request",null,null,null,null,null,null,null,229789,"Wandkonvektor CNS 75 F","On request",false,null,229789,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 75 F","Wandkonvektor CNS 75 F","Wandkonvektor CNS 75 F","Wandkonvektor CNS 75 F","Wandconvector CNS 75 F "]
[null,229790,"Wandkonvektor CNS 100 F","On request",null,null,null,null,null,null,null,229790,"Wandkonvektor CNS 100 F","On request",false,null,229790,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 100 F","Wandkonvektor CNS 100 F","Wandkonvektor CNS 100 F","Wandkonvektor CNS 100 F","Wandconvector CNS 100 F "]
[null,229792,"Wandkonvektor CNS 150 F","On request",null,null,null,null,null,null,null,229792,"Wandkonvektor CNS 150 F","On request",false,null,229792,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 150 F","Wandkonvektor CNS 150 F","Wandkonvektor CNS 150 F","Wandkonvektor CNS 150 F","Wandconvector CNS 150 F "]
[null,229794,"Wandkonvektor CNS 200 F","On request",null,null,null,null,null,null,null,229794,"Wandkonvektor CNS 200 F","On request",false,null,229794,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 200 F","Wandkonvektor CNS 200 F","Wandkonvektor CNS 200 F","Wandkonvektor CNS 200 F","Wandconvector CNS 200 F "]
[null,229795,"Wandkonvektor CNS 250 F","On request",null,null,null,null,null,null,null,229795,"Wandkonvektor CNS 250 F","On request",false,null,229795,"auf Anfrage","On request","sur demande","på forespørgsel","op aanvraag","Wandkonvektor CNS 250 F","Wandkonvektor CNS 250 F","Wandkonvektor CNS 250 F","Wandkonvektor CNS 250 F","Wandconvector CNS 250 F "]

{"sheet":"Ausdruck","index":6,"n_rows":610,"n_cols":115,"rows_kept":610,"cut":false,"hidden":true,"merged":[[600,58,600,82],[601,58,601,82],[602,58,602,82],[603,58,603,82],[593,30,593,54],[594,30,594,54],[594,86,594,110],[584,30,584,54],[585,30,585,54],[586,30,586,54],[587,30,587,54],[588,30,588,54],[589,30,589,54],[590,30,590,54],[591,30,591,54],[592,30,592,54],[592,86,592,110],[593,86,593,110],[591,58,591,82],[592,58,592,82],[593,58,593,82],[594,58,594,82],[595,58,595,82],[596,58,596,82],[573,30,573,54],[574,30,574,54],[588,86,588,110],[569,86,569,110],[570,86,570,110],[571,86,571,110],[554,30,554,54],[559,30,559,54],[560,30,560,54],[561,30,561,54],[562,30,562,54],[563,30,563,54],[564,30,564,54],[565,30,565,54],[566,30,566,54],[575,30,575,54],[576,30,576,54],[577,30,577,54],[578,30,578,54],[579,30,579,54],[580,30,580,54],[581,30,581,54],[582,30,582,54],[583,30,583,54],[565,86,565,110],[566,86,566,110],[568,86,568,110],[567,30,567,54],[568,30,568,54],[569,30,569,54],[570,30,570,54],[571,30,571,54],[572,30,572,54],[567,86,567,110],[572,86,572,110],[567,58,567,82],[568,58,568,82],[569,58,569,82],[570,58,570,82],[571,58,571,82],[572,58,572,82],[577,86,577,110],[580,86,580,110],[589,86,589,110],[590,86,590,110],[591,86,591,110],[579,86,579,110],[581,86,581,110],[582,86,582,110],[583,86,583,110],[584,86,584,110],[585,86,585,110],[586,86,586,110],[587,86,587,110],[573,86,573,110],[574,86,574,110],[575,86,575,110],[576,86,576,110],[578,86,578,110],[563,86,563,110],[564,86,564,110],[392,15,392,25],[393,15,393,25],[394,15,394,25],[395,15,395,25],[396,15,396,25],[397,15,397,25],[398,15,398,25],[474,12,474,18],[474,19,474,25],[483,12,483,25],[484,12,484,25],[485,12,485,25],[520,22,520,25],[521,22,521,25],[522,22,522,25],[519,22,519,25],[512,22,512,25],[520,16,520,18],[554,86,554,110],[383,15,383,25],[384,15,384,25],[385,15,385,25],[386,15,386,25],[387,15,387,25],[559,86,559,110],[560,86,560,110],[390,15,390,25],[391,15,391,25],[520,19,520,21],[521,16,521,18],[521,19,521,21],[522,16,522,18],[522,19,522,21],[513,16,513,18],[513,19,513,21],[514,16,514,18],[514,19,514,21],[515,16,515,18],[515,19,515,21],[516,16,516,18],[516,19,516,21],[561,86,561,110],[562,86,562,110],[385,2,385,12],[386,2,386,12],[387,2,387,12],[388,2,388,12],[389,2,389,12],[315,1,315,25],[404,1,404,25],[356,2,356,12],[357,2,357,12],[358,2,358,12],[359,2,359,12],[360,2,360,12],[361,2,361,12],[362,2,362,12],[363,2,363,12],[364,2,364,12],[365,2,365,12],[366,2,366,12],[367,2,367,12],[368,2,368,12],[369,2,369,12],[370,2,370,12],[371,2,371,12],[372,2,372,12],[373,2,373,12],[374,2,374,12],[375,2,375,12],[376,2,376,12],[377,2,377,12],[378,2,378,12],[373,15,373,25],[374,15,374,25],[375,15,375,25],[376,15,376,25],[377,15,377,25],[378,15,378,25],[379,15,379,25],[380,15,380,25],[381,15,381,25],[382,15,382,25],[388,15,388,25],[389,15,389,25],[381,2,381,12],[382,2,382,12],[383,2,383,12],[384,2,384,12],[609,1,609,25],[213,1,213,10],[213,11,213,25],[220,1,220,10],[220,11,220,25],[227,1,227,10],[227,11,227,25],[234,1,234,10],[234,11,234,25],[304,1,304,25],[354,1,354,25],[218,1,218,10],[218,11,218,25],[219,1,219,10],[219,11,219,25],[222,1,222,10],[223,1,223,10],[223,11,223,25],[224,1,224,10],[224,11,224,25],[225,1,225,10],[225,11,225,25],[390,2,390,12],[391,2,391,12],[211,11,211,25],[211,1,211,10],[212,1,212,10],[212,11,212,25],[215,1,215,10],[216,1,216,10],[216,11,216,25],[217,1,217,10],[217,11,217,25],[110,1,110,8],[110,9,110,25],[111,1,111,8],[111,9,111,25],[116,1,116,8],[113,9,113,25],[117,1,117,8],[117,9,117,25],[118,1,118,8],[118,9,118,25],[60,1,60,8],[60,9,60,25],[61,1,61,8],[61,9,61,25],[62,1,62,8],[62,9,62,25],[109,1,109,8],[66,1,66,8],[66,9,66,25],[63,1,63,8],[63,9,63,25],[64,1,64,8],[64,9,64,25],[65,1,65,8],[65,9,65,25],[104,1,104,25],[18,1,18,8],[19,1,19,8],[19,9,19,25],[20,1,20,8],[20,9,20,25],[21,1,21,8],[21,9,21,25],[59,1,59,8],[22,1,22,8],[22,9,22,25],[24,1,24,8],[25,1,25,8],[25,9,25,25],[26,1,26,8],[26,9,26,25],[27,1,27,8],[27,9,27,25],[2,20,2,26],[122,1,122,8],[123,1,123,8],[123,9,123,25],[124,1,124,8],[124,9,124,25],[112,1,112,8],[112,9,112,25],[113,1,113,8],[114,1,114,8],[114,9,114,25],[119,1,119,8],[119,9,119,25],[120,1,120,8],[120,9,120,25],[13,1,13,8],[14,1,14,8],[13,9,13,25],[14,9,14,25],[12,1,12,8],[15,1,15,8],[16,1,16,8],[15,9,15,25],[16,9,16,25],[171,23,171,25],[163,3,163,4],[163,5,163,7],[163,8,163,19],[160,8,160,19],[160,20,160,22],[160,23,160,25],[161,1,161,2],[161,3,161,4],[161,5,161,7],[161,8,161,19],[161,20,161,22],[161,23,161,25],[163,20,163,22],[163,23,163,25],[167,1,167,2],[167,3,167,4],[167,5,167,7],[167,8,167,19],[167,20,167,22],[167,23,167,25],[168,1,168,2],[168,3,168,4],[168,5,168,7],[168,8,168,19],[168,20,168,22],[164,1,164,2],[164,3,164,4],[164,5,164,7],[164,8,164,19],[164,20,164,22],[164,23,164,25],[159,1,159,2],[159,5,159,7],[159,20,159,22],[159,3,159,4],[159,23,159,25],[159,8,159,19],[160,1,160,2],[160,3,160,4],[160,5,160,7],[162,1,162,2],[162,3,162,4],[162,5,162,7],[162,8,162,19],[162,20,162,22],[162,23,162,25],[163,1,163,2],[165,23,165,25],[166,1,166,2],[166,3,166,4],[166,5,166,7],[166,8,166,19],[166,20,166,22],[166,23,166,25],[165,1,165,2],[165,3,165,4],[165,5,165,7],[165,8,165,19],[165,20,165,22],[172,1,172,2],[172,3,172,4],[172,5,172,7],[172,8,172,19],[172,20,172,22],[172,23,172,25],[168,23,168,25],[169,1,169,2],[169,3,169,4],[169,5,169,7],[169,8,169,19],[169,20,169,22],[169,23,169,25],[170,1,170,2],[170,3,170,4],[170,5,170,7],[170,8,170,19],[170,20,170,22],[170,23,170,25],[171,1,171,2],[171,3,171,4],[171,5,171,7],[171,8,171,19],[171,20,171,22],[173,23,173,25],[174,1,174,2],[174,3,174,4],[174,5,174,7],[174,8,174,19],[174,20,174,22],[174,23,174,25],[173,1,173,2],[173,3,173,4],[173,5,173,7],[173,8,173,19],[173,20,173,22],[175,23,175,25],[176,1,176,2],[176,3,176,4],[176,5,176,7],[176,8,176,19],[176,20,176,22],[176,23,176,25],[175,1,175,2],[175,3,175,4],[175,5,175,7],[175,8,175,19],[175,20,175,22],[177,23,177,25],[178,1,178,2],[178,3,178,4],[178,5,178,7],[178,8,178,19],[178,20,178,22],[178,23,178,25],[177,1,177,2],[177,3,177,4],[177,5,177,7],[177,8,177,19],[177,20,177,22],[179,23,179,25],[180,1,180,2],[180,3,180,4],[180,5,180,7],[180,8,180,19],[180,20,180,22],[180,23,180,25],[179,1,179,2],[179,3,179,4],[179,5,179,7],[179,8,179,19],[179,20,179,22],[181,23,181,25],[182,1,182,2],[182,3,182,4],[182,5,182,7],[182,8,182,19],[182,20,182,22],[182,23,182,25],[181,1,181,2],[181,3,181,4],[181,5,181,7],[181,8,181,19],[181,20,181,22],[183,23,183,25],[184,1,184,2],[184,3,184,4],[184,5,184,7],[184,8,184,19],[184,20,184,22],[184,23,184,25],[183,1,183,2],[183,3,183,4],[183,5,183,7],[183,8,183,19],[183,20,183,22],[185,23,185,25],[186,1,186,2],[186,3,186,4],[186,5,186,7],[186,8,186,19],[186,20,186,22],[186,23,186,25],[185,1,185,2],[185,3,185,4],[185,5,185,7],[185,8,185,19],[185,20,185,22],[187,23,187,25],[188,1,188,2],[188,3,188,4],[188,5,188,7],[188,8,188,19],[188,20,188,22],[188,23,188,25],[187,1,187,2],[187,3,187,4],[187,5,187,7],[187,8,187,19],[187,20,187,22],[189,23,189,25],[190,1,190,2],[190,3,190,4],[190,5,190,7],[190,8,190,19],[190,20,190,22],[190,23,190,25],[189,1,189,2],[189,3,189,4],[189,5,189,7],[189,8,189,19],[189,20,189,22],[193,1,193,2],[193,3,193,4],[193,5,193,7],[193,8,193,19],[193,20,193,22],[191,23,191,25],[192,1,192,2],[192,3,192,4],[192,5,192,7],[192,8,192,19],[192,20,192,22],[192,23,192,25],[191,1,191,2],[191,3,191,4],[191,5,191,7],[191,8,191,19],[191,20,191,22],[197,3,197,4],[197,5,197,7],[197,8,197,19],[197,20,197,22],[209,1,209,10],[210,1,210,10],[210,11,210,25],[194,3,194,4],[194,5,194,7],[194,8,194,19],[194,20,194,22],[194,23,194,25],[154,1,154,25],[198,1,198,19],[198,20,198,25],[204,1,204,25],[0,2,0,17],[1,2,1,17],[7,1,7,25],[54,1,54,25],[195,23,195,25],[196,1,196,2],[196,3,196,4],[196,5,196,7],[196,8,196,19],[196,20,196,22],[196,23,196,25],[195,1,195,2],[195,3,195,4],[195,5,195,7],[195,8,195,19],[195,20,195,22],[193,23,193,25],[194,1,194,2],[197,23,197,25],[197,1,197,2],[604,1,604,25],[275,3,275,23],[254,1,254,25],[229,1,229,10],[230,1,230,10],[230,11,230,25],[231,1,231,10],[231,11,231,25],[232,1,232,10],[232,11,232,25],[233,1,233,10],[233,11,233,25],[454,1,454,25],[379,2,379,12],[380,2,380,12],[392,2,392,12],[393,2,393,12],[394,2,394,12],[395,2,395,12],[396,2,396,12],[397,2,397,12],[398,2,398,12],[356,15,356,25],[357,15,357,25],[463,1,463,11],[463,12,463,18],[463,19,463,25],[464,1,464,11],[464,12,464,18],[464,19,464,25],[226,1,226,10],[226,11,226,25],[296,3,296,23],[358,15,358,25],[359,15,359,25],[360,15,360,25],[361,15,361,25],[362,15,362,25],[363,15,363,25],[364,15,364,25],[365,15,365,25],[366,15,366,25],[367,15,367,25],[368,15,368,25],[369,15,369,25],[370,15,370,25],[371,15,371,25],[372,15,372,25],[459,1,459,11],[460,1,460,11],[460,12,460,18],[460,19,460,25],[461,1,461,11],[461,12,461,18],[461,19,461,25],[462,1,462,11],[462,12,462,18],[462,19,462,25],[459,12,459,25],[465,1,465,11],[465,12,465,18],[465,19,465,25],[466,1,466,11],[466,12,466,18],[466,19,466,25],[467,1,467,11],[467,12,467,18],[467,19,467,25],[468,1,468,11],[468,12,468,18],[468,19,468,25],[469,1,469,11],[469,12,469,18],[469,19,469,25],[470,1,470,11],[470,12,470,18],[470,19,470,25],[475,1,475,11],[475,12,475,18],[475,19,475,25],[476,1,476,11],[476,12,476,18],[476,19,476,25],[472,1,472,11],[482,1,482,11],[473,1,473,11],[473,12,473,18],[473,19,473,25],[482,12,482,25],[474,1,474,11],[472,12,472,25],[483,1,483,11],[484,1,484,11],[485,1,485,11],[480,1,480,11],[480,12,480,18],[480,19,480,25],[477,1,477,11],[477,12,477,18],[477,19,477,25],[478,1,478,11],[478,12,478,18],[478,19,478,25],[479,1,479,11],[479,12,479,18],[479,19,479,25],[568,1,568,25],[569,1,569,25],[570,1,570,25],[486,1,486,25],[504,1,504,25],[554,1,554,25],[559,1,559,25],[560,1,560,25],[561,1,561,25],[512,1,512,9],[515,1,515,9],[516,1,516,9],[513,1,513,9],[562,1,562,25],[563,1,563,25],[564,1,564,25],[565,1,565,25],[566,1,566,25],[567,1,567,25],[537,1,537,9],[538,1,538,9],[536,1,536,9],[535,1,535,9],[531,1,531,9],[579,1,579,25],[594,1,594,25],[580,1,580,25],[581,1,581,25],[582,1,582,25],[583,1,583,25],[584,1,584,25],[585,1,585,25],[586,1,586,25],[587,1,587,25],[588,1,588,25],[589,1,589,25],[590,1,590,25],[591,1,591,25],[592,1,592,25],[593,1,593,25],[532,1,532,9],[529,1,529,9],[530,1,530,9],[527,1,527,9],[528,1,528,9],[524,1,524,9],[512,10,512,12],[513,10,513,12],[514,10,514,12],[526,1,526,9],[522,1,522,9],[523,1,523,9],[520,1,520,9],[521,1,521,9],[517,1,517,9],[518,1,518,9],[519,1,519,9],[514,1,514,9],[526,10,526,15],[530,10,530,15],[531,10,531,15],[532,10,532,15],[517,16,517,18],[513,22,513,25],[514,22,514,25],[515,22,515,25],[516,22,516,25],[509,1,509,9],[511,1,511,9],[512,13,512,15],[511,10,511,12],[511,13,511,15],[511,16,511,18],[511,19,511,21],[509,22,509,25],[511,22,511,25],[512,16,512,18],[512,19,512,21],[510,1,510,9],[510,10,510,12],[510,13,510,15],[510,16,510,18],[510,19,510,21],[510,22,510,25],[509,10,509,15],[509,16,509,21],[539,1,539,9],[513,13,513,15],[514,13,514,15],[515,10,515,12],[515,13,515,15],[516,10,516,12],[516,13,516,15],[517,10,517,12],[517,13,517,15],[518,10,518,12],[518,13,518,15],[519,10,519,12],[519,13,519,15],[520,10,520,12],[520,13,520,15],[521,10,521,12],[521,13,521,15],[522,10,522,12],[522,13,522,15],[523,10,523,12],[523,13,523,15],[524,10,524,12],[524,13,524,15],[533,1,533,9],[526,16,526,21],[527,22,527,25],[523,16,523,18],[523,19,523,21],[524,16,524,18],[524,19,524,21],[524,22,524,25],[527,10,527,15],[527,16,527,21],[523,22,523,25],[526,22,526,25],[571,1,571,25],[572,1,572,25],[573,1,573,25],[574,1,574,25],[575,1,575,25],[576,1,576,25],[577,1,577,25],[578,1,578,25],[517,22,517,25],[518,22,518,25],[518,16,518,18],[518,19,518,21],[519,16,519,18],[519,19,519,21],[517,19,517,21],[539,10,539,15],[539,16,539,21],[535,10,535,15],[535,16,535,21],[535,22,535,25],[528,22,528,25],[529,22,529,25],[530,22,530,25],[531,22,531,25],[554,58,554,82],[537,10,537,15],[537,16,537,21],[538,10,538,15],[538,16,538,21],[533,10,533,15],[528,16,528,21],[529,16,529,21],[530,16,530,21],[531,16,531,21],[532,16,532,21],[533,16,533,21],[536,10,536,15],[536,16,536,21],[532,22,532,25],[533,22,533,25],[536,22,536,25],[537,22,537,25],[538,22,538,25],[539,22,539,25],[528,10,528,15],[529,10,529,15],[597,58,597,82],[598,58,598,82],[599,58,599,82],[583,58,583,82],[584,58,584,82],[585,58,585,82],[586,58,586,82],[587,58,587,82],[588,58,588,82],[589,58,589,82],[590,58,590,82],[559,58,559,82],[560,58,560,82],[561,58,561,82],[562,58,562,82],[563,58,563,82],[564,58,564,82],[565,58,565,82],[566,58,566,82],[582,58,582,82],[573,58,573,82],[574,58,574,82],[575,58,575,82],[576,58,576,82],[577,58,577,82],[578,58,578,82],[579,58,579,82],[580,58,580,82],[581,58,581,82],[566,114,566,138],[567,114,567,138],[568,114,568,138],[569,114,569,138],[570,114,570,138],[554,114,554,138],[559,114,559,138],[560,114,560,138],[561,114,561,138],[562,114,562,138],[563,114,563,138],[564,114,564,138],[565,114,565,138],[571,114,571,138],[572,114,572,138],[573,114,573,138],[580,114,580,138],[581,114,581,138],[582,114,582,138],[583,114,583,138],[584,114,584,138],[574,114,574,138],[575,114,575,138],[576,114,576,138],[577,114,577,138],[578,114,578,138],[579,114,579,138],[594,114,594,138],[585,114,585,138],[586,114,586,138],[587,114,587,138],[588,114,588,138],[589,114,589,138],[590,114,590,138],[591,114,591,138],[592,114,592,138],[593,114,593,138]]}
[null,null,{"$f":"UPPER(Translation!$A$311)&\".\"","v":"DESIGN."}]
[null,null,{"$f":"UPPER(Translation!$A$5)","v":"SOLAR SYSTEM"}]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A300","v":"Project"}]
[]
[]
[]
[]
[null,{"$f":"Translation!$A$10","v":"Project"}]
[null,{"$f":"Translation!$A$11","v":"Name"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B6","v":"Beispielprojekt"}]
[null,{"$f":"Translation!$A$12","v":"Street"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B7","v":""}]
[null,{"$f":"Translation!$A$13","v":"Postcode/Town"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B8","v":""}]
[null,{"$f":"Translation!$A$14","v":"Phone"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B9","v":""}]
[]
[null,{"$f":"Translation!$A$15","v":"Customer"}]
[null,{"$f":"Translation!$A$11","v":"Name"},null,null,null,null,"Stiebel Eltron GmbH & Co. KG",null,null,{"$f":"Zwischenwerte!D6","v":"Stiebel Eltron GmbH & Co. KG"}]
[null,{"$f":"Translation!$A$12","v":"Street"},null,null,null,null,"Dr.-Stiebel-Straße",null,null,{"$f":"Zwischenwerte!D7","v":"Dr.-Stiebel-Straße"}]
[null,{"$f":"Translation!$A$13","v":"Postcode/Town"},null,null,null,null,"37603 Holzminden",null,null,{"$f":"Zwischenwerte!D8","v":"37603 Holzminden"}]
[null,{"$f":"Translation!$A$14","v":"Phone"},null,null,null,null,"05531 / 702 110",null,null,{"$f":"Zwischenwerte!D9","v":"05531 / 702 110"}]
[]
[null,{"$f":"Translation!$A$16","v":"Climate zone"}]
[null,{"$f":"Translation!A312","v":"Country"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!A14","v":"Germany"}]
[null,{"$f":"Translation!A313","v":"City"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B14","v":"Aachen"}]
[null,{"$f":"Translation!A16","v":"Climate zone"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!L112","v":"I"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A301","v":"Description solar system"}]
[]
[]
[]
[]
[null,{"$f":"Translation!A65","v":"Collector details"}]
[null,{"$f":"Translation!A66","v":"Collector type"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!N14","v":"Rooftop SOL 27 Premium"}]
[null,{"$f":"Translation!A69","v":"Collector number"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B81","v":2}]
[null,{"$f":"Translation!A71","v":"Collector inclination"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!P14","v":"45 °"}]
[null,{"$f":"Translation!A72","v":"Collector orientation"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!Q14","v":"South"}]
[null,{"$f":"Translation!A78","v":"Arrangement"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!M14","v":"On end next to each other"}]
[null,{"$f":"Translation!A83","v":"Shape of roof"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!R39","v":"Tiled roof"}]
[null,{"$f":"Translation!A86","v":"Fixing type"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!S14","v":"Standard fixings"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A302","v":"Type of utilisation"}]
[]
[]
[]
[]
[null,{"$f":"Translation!A43","v":"Solar DHW heating"}]
[null,{"$f":"Translation!A44","v":"Number of occupants"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!C14=FALSE,\"---\",Zwischenwerte!F14)","v":"4"}]
[null,{"$f":"Translation!A45","v":"DHW demand"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!C14=FALSE,\"---\",Zwischenwerte!G14)","v":"Standard demand (40 litres)"}]
[null,{"$f":"Translation!A167","v":"Cold water temperature"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!C14=FALSE,\"---\",Zwischenwerte!U14)","v":"10 °C"}]
[null,{"$f":"Translation!A168","v":"Cylinder temperature"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!C14=FALSE,\"---\",Zwischenwerte!V14)","v":"45 °C"}]
[null,{"$f":"Translation!A169","v":"System losses DHW"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!C14=FALSE,\"---\",Zwischenwerte!W14)","v":"20 %"}]
[]
[null,{"$f":"Translation!A51","v":"Solar central heating backup"}]
[null,{"$f":"Translation!A52","v":"Heat demand building"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!D14=FALSE,\"---\",Zwischenwerte!H14)","v":"---"}]
[null,{"$f":"Translation!A53","v":"Cylinder type"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!D14=FALSE,\"---\",Zwischenwerte!I14)","v":"---"}]
[null,{"$f":"Translation!A170","v":"Standard outside temperature"},null,null,null,null,null,null,null,{"$f":"IF(OR(Zwischenwerte!A39=FALSE,Zwischenwerte!D14=FALSE),\"---\",Zwischenwerte!X14)","v":"---"}]
[null,{"$f":"Translation!A171","v":"Heating limit temperature"},null,null,null,null,null,null,null,{"$f":"IF(OR(Zwischenwerte!A39=FALSE,Zwischenwerte!D14=FALSE),\"---\",Zwischenwerte!Y14)","v":"---"}]
[]
[null,{"$f":"Translation!A57","v":"Solar swimming pool heating"}]
[null,{"$f":"Translation!A58","v":"Swimming pool type"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!E14=FALSE,\"---\",Zwischenwerte!J14)","v":"---"}]
[null,{"$f":"Translation!A314","v":"Volume"},null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!E14=FALSE,\"---\",Zwischenwerte!K14&\" m³\")","v":"---"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A303","v":"Material composition"}]
[]
[]
[]
[]
[null,{"$f":"Translation!A96","v":"Position"},null,{"$f":"Translation!A97","v":"Number"},null,{"$f":"Translation!A98","v":"ID"},null,null,{"$f":"Translation!A99","v":"Description"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!F9=FALSE,\"\",Translation!A100)","v":"Price each"},null,null,{"$f":"IF(Zwischenwerte!F9=FALSE,\"\",Translation!A101)","v":"Total price"}]
[null,{"$f":"Auswahl!C154","v":1},null,{"$f":"Auswahl!E154","v":2},null,{"$f":"Auswahl!H154","v":230016},null,null,{"$f":"Auswahl!K154","v":"Solar flat-plate collector SOL 27 premium S"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V154)","v":809},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y154)","v":1618}]
[null,{"$f":"Auswahl!C155","v":2},null,{"$f":"Auswahl!E155","v":1},null,{"$f":"Auswahl!H155","v":230170},null,null,{"$f":"Auswahl!K155","v":"Mounting frame SOL R2"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V155)","v":160},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y155)","v":160}]
[null,{"$f":"Auswahl!C156","v":3},null,{"$f":"Auswahl!E156","v":2},null,{"$f":"Auswahl!H156","v":230175},null,null,{"$f":"Auswahl!K156","v":"Fixing Kit - tiled roof SOL BP"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V156)","v":80},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y156)","v":160}]
[null,{"$f":"Auswahl!C157","v":4},null,{"$f":"Auswahl!E157","v":1},null,{"$f":"Auswahl!H157","v":230185},null,null,{"$f":"Auswahl!K157","v":"Push-fit connection SOL SV-A"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V157)","v":49},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y157)","v":49}]
[null,{"$f":"Auswahl!C158","v":5},null,{"$f":"Auswahl!E158","v":1},null,{"$f":"Auswahl!H158","v":230186},null,null,{"$f":"Auswahl!K158","v":"Push-fit connection SOL SV-D"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V158)","v":299},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y158)","v":299}]
[null,{"$f":"Auswahl!C159","v":6},null,{"$f":"Auswahl!E159","v":1},null,{"$f":"Auswahl!H159","v":232945},null,null,{"$f":"Auswahl!K159","v":"Flexible solar pipe SFR 15, DN 20 15m"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V159)","v":585},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y159)","v":585}]
[null,{"$f":"Auswahl!C160","v":7},null,{"$f":"Auswahl!E160","v":1},null,{"$f":"Auswahl!H160","v":234784},null,null,{"$f":"Auswahl!K160","v":"Solar compact installation SOKI 7 E trend"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V160)","v":540},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y160)","v":540}]
[null,{"$f":"Auswahl!C161","v":8},null,{"$f":"Auswahl!E161","v":1},null,{"$f":"Auswahl!H161","v":187873},null,null,{"$f":"Auswahl!K161","v":"Warm water cylinder SBB 300 plus"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V161)","v":1692},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y161)","v":1692}]
[null,{"$f":"Auswahl!C162","v":9},null,{"$f":"Auswahl!E162","v":1},null,{"$f":"Auswahl!H162","v":73222},null,null,{"$f":"Auswahl!K162","v":"Heat transfer liquid H30-L, 20 l"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V162)","v":79},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y162)","v":79}]
[null,{"$f":"Auswahl!C163","v":10},null,{"$f":"Auswahl!E163","v":1},null,{"$f":"Auswahl!H163","v":74031},null,null,{"$f":"Auswahl!K163","v":"Solar expansion vessel 25 l"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V163)","v":80},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y163)","v":80}]
[null,{"$f":"Auswahl!C164","v":11},null,{"$f":"Auswahl!E164","v":1},null,{"$f":"Auswahl!H164","v":231905},null,null,{"$f":"Auswahl!K164","v":"DEV connection set AGWH"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V164)","v":46},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y164)","v":46}]
[null,{"$f":"Auswahl!C165","v":12},null,{"$f":"Auswahl!E165","v":0},null,{"$f":"Auswahl!H165","v":0},null,null,{"$f":"Auswahl!K165","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V165)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y165)","v":""}]
[null,{"$f":"Auswahl!C166","v":13},null,{"$f":"Auswahl!E166","v":0},null,{"$f":"Auswahl!H166","v":0},null,null,{"$f":"Auswahl!K166","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V166)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y166)","v":""}]
[null,{"$f":"Auswahl!C167","v":14},null,{"$f":"Auswahl!E167","v":0},null,{"$f":"Auswahl!H167","v":0},null,null,{"$f":"Auswahl!K167","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V167)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y167)","v":""}]
[null,{"$f":"Auswahl!C168","v":15},null,{"$f":"Auswahl!E168","v":0},null,{"$f":"Auswahl!H168","v":0},null,null,{"$f":"Auswahl!K168","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V168)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y168)","v":""}]
[null,{"$f":"Auswahl!C169","v":16},null,{"$f":"Auswahl!E169","v":0},null,{"$f":"Auswahl!H169","v":0},null,null,{"$f":"Auswahl!K169","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V169)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y169)","v":""}]
[null,{"$f":"Auswahl!C170","v":17},null,{"$f":"Auswahl!E170","v":0},null,{"$f":"Auswahl!H170","v":0},null,null,{"$f":"Auswahl!K170","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V170)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y170)","v":""}]
[null,{"$f":"Auswahl!C171","v":18},null,{"$f":"Auswahl!E171","v":0},null,{"$f":"Auswahl!H171","v":0},null,null,{"$f":"Auswahl!K171","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V171)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y171)","v":""}]
[null,{"$f":"Auswahl!C172","v":19},null,{"$f":"Auswahl!E172","v":0},null,{"$f":"Auswahl!H172","v":0},null,null,{"$f":"Auswahl!K172","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V172)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y172)","v":""}]
[null,{"$f":"Auswahl!C173","v":20},null,{"$f":"Auswahl!E173","v":0},null,{"$f":"Auswahl!H173","v":0},null,null,{"$f":"Auswahl!K173","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V173)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y173)","v":""}]
[null,{"$f":"Auswahl!C174","v":21},null,{"$f":"Auswahl!E174","v":0},null,{"$f":"Auswahl!H174","v":0},null,null,{"$f":"Auswahl!K174","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V174)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y174)","v":""}]
[null,{"$f":"Auswahl!C175","v":22},null,{"$f":"Auswahl!E175","v":0},null,{"$f":"Auswahl!H175","v":0},null,null,{"$f":"Auswahl!K175","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V175)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y175)","v":""}]
[null,{"$f":"Auswahl!C176","v":23},null,{"$f":"Auswahl!E176","v":0},null,{"$f":"Auswahl!H176","v":0},null,null,{"$f":"Auswahl!K176","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V176)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y176)","v":""}]
[null,{"$f":"Auswahl!C177","v":24},null,{"$f":"Auswahl!E177","v":0},null,{"$f":"Auswahl!H177","v":0},null,null,{"$f":"Auswahl!K177","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V177)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y177)","v":""}]
[null,{"$f":"Auswahl!C178","v":25},null,{"$f":"Auswahl!E178","v":0},null,{"$f":"Auswahl!H178","v":0},null,null,{"$f":"Auswahl!K178","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V178)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y178)","v":""}]
[null,{"$f":"Auswahl!C179","v":26},null,{"$f":"Auswahl!E179","v":0},null,{"$f":"Auswahl!H179","v":0},null,null,{"$f":"Auswahl!K179","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V179)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y179)","v":""}]
[null,{"$f":"Auswahl!C180","v":27},null,{"$f":"Auswahl!E180","v":0},null,{"$f":"Auswahl!H180","v":0},null,null,{"$f":"Auswahl!K180","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V180)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y180)","v":""}]
[null,{"$f":"Auswahl!C181","v":28},null,{"$f":"Auswahl!E181","v":0},null,{"$f":"Auswahl!H181","v":0},null,null,{"$f":"Auswahl!K181","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V181)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y181)","v":""}]
[null,{"$f":"Auswahl!C182","v":29},null,{"$f":"Auswahl!E182","v":0},null,{"$f":"Auswahl!H182","v":0},null,null,{"$f":"Auswahl!K182","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V182)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y182)","v":""}]
[null,{"$f":"Auswahl!C183","v":30},null,{"$f":"Auswahl!E183","v":0},null,{"$f":"Auswahl!H183","v":0},null,null,{"$f":"Auswahl!K183","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V183)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y183)","v":""}]
[null,{"$f":"Auswahl!C184","v":31},null,{"$f":"Auswahl!E184","v":0},null,{"$f":"Auswahl!H184","v":0},null,null,{"$f":"Auswahl!K184","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V184)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y184)","v":""}]
[null,{"$f":"Auswahl!C185","v":32},null,{"$f":"Auswahl!E185","v":0},null,{"$f":"Auswahl!H185","v":0},null,null,{"$f":"Auswahl!K185","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V185)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y185)","v":""}]
[null,{"$f":"Auswahl!C186","v":33},null,{"$f":"Auswahl!E186","v":0},null,{"$f":"Auswahl!H186","v":0},null,null,{"$f":"Auswahl!K186","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V186)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y186)","v":""}]
[null,{"$f":"Auswahl!C187","v":34},null,{"$f":"Auswahl!E187","v":0},null,{"$f":"Auswahl!H187","v":0},null,null,{"$f":"Auswahl!K187","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V187)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y187)","v":""}]
[null,{"$f":"Auswahl!C188","v":35},null,{"$f":"Auswahl!E188","v":0},null,{"$f":"Auswahl!H188","v":0},null,null,{"$f":"Auswahl!K188","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V188)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y188)","v":""}]
[null,{"$f":"Auswahl!C189","v":36},null,{"$f":"Auswahl!E189","v":0},null,{"$f":"Auswahl!H189","v":0},null,null,{"$f":"Auswahl!K189","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V189)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y189)","v":""}]
[null,{"$f":"Auswahl!C190","v":37},null,{"$f":"Auswahl!E190","v":0},null,{"$f":"Auswahl!H190","v":0},null,null,{"$f":"Auswahl!K190","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V190)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y190)","v":""}]
[null,{"$f":"Auswahl!C191","v":38},null,{"$f":"Auswahl!E191","v":0},null,{"$f":"Auswahl!H191","v":0},null,null,{"$f":"Auswahl!K191","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!V191)","v":""},null,null,{"$f":"IF(Zwischenwerte!$F$9=FALSE,\"\",Auswahl!Y191)","v":""}]
[null,{"$f":"IF(Zwischenwerte!F9=FALSE,\"\",Translation!A102)","v":"Recommended retail price excl. VAT"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zwischenwerte!F9=FALSE,\"\",Auswahl!Y192)","v":5308}]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A135","v":"Solar yield"}]
[]
[]
[]
[]
[null,{"$f":"Translation!A65","v":"Collector details"}]
[null,{"$f":"Translation!A66&\" | \"&Translation!A315","v":"Collector type | Total area"},null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B81&\" x \"&Zwischenwerte!N14&\"  |  \"&FIXED(Zwischenwerte!B103,1)&\" m²\"","v":"2 x Rooftop SOL 27 Premium  |  4,8 m²"}]
[null,{"$f":"Translation!A316","v":"Location"},null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!A14&\" | \"&Zwischenwerte!B14&\" (\"&Translation!A16&\" \"&Zwischenwerte!L112&\")\"","v":"Germany | Aachen (Climate zone I)"}]
[null,{"$f":"Translation!A71&\" | \"&Translation!A72","v":"Collector inclination | Collector orientation"},null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!P14&\"  |  \"&Zwischenwerte!Q14","v":"45 °  |  South"}]
[null,{"$f":"Translation!A317","v":"Insolation, collector area"},null,null,null,null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C319,0)&IF(Zwischenwerte!$F$6=6,\" kWh/r\",\" kWh/a\")","v":"5.330 kWh/a"}]
[]
[null,{"$f":"Translation!A43","v":"Solar DHW heating"}]
[null,{"$f":"Translation!A45","v":"DHW demand"},null,null,null,null,null,null,null,{"$f":"Auswahl!Q256","v":"4 Occupants x 40 l/day"},null,{"$f":"Auswahl!Q256","v":"4 Occupants x 40 l/day"}]
[null,{"$f":"Translation!$A$139","v":"Heat demand"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q260","v":"2.853 kWh/a"}]
[null,{"$f":"Translation!$A$138","v":"Recommended cylinder"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q258","v":"SBB 300 Plus"}]
[null,{"$f":"Translation!$A$135","v":"Solar yield"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q262","v":"2.013 kWh/a"}]
[null,{"$f":"Translation!A140","v":"Solar coverage DHW heating"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q264","v":"70,6 %"}]
[]
[null,{"$f":"Translation!A51","v":"Solar central heating backup"}]
[null,{"$f":"Translation!A52","v":"Heat demand building"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q268","v":""}]
[null,{"$f":"Translation!A141","v":"Annual heat demand"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q270","v":{"$error":"#VALUE!"}}]
[null,{"$f":"Translation!A142","v":"Heating water buffer cylinder"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q272","v":"SBB 300 Plus"}]
[null,{"$f":"Translation!A143","v":"Solar yield heating backup"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q274","v":{"$error":"#VALUE!"}}]
[null,{"$f":"Translation!A144","v":"Coverage DHW | Heating backup"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q276","v":{"$error":"#VALUE!"}}]
[]
[null,{"$f":"Translation!A57","v":"Solar swimming pool heating"}]
[null,{"$f":"Translation!A145","v":"Swimming pool type | Volume"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!A211","v":0},null,{"$f":"Auswahl!Q280","v":"  |  0 m³"}]
[null,{"$f":"Translation!A146","v":"Duration of use | Cooling"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B211","v":0},null,{"$f":"Auswahl!Q282","v":{"$error":"#N/A"}}]
[null,{"$f":"Translation!A147","v":"Heat demand for reheating"},null,null,null,null,null,null,null,{"$f":"Zwischenwerte!L309","v":{"$error":"#VALUE!"}},null,{"$f":"Auswahl!Q284","v":{"$error":"#N/A"}}]
[null,{"$f":"Translation!A148","v":"Solar yield swimming pool"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q286","v":{"$error":"#N/A"}}]
[null,{"$f":"Translation!A149","v":"Coverage heat loss swimming pool"},null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!Q288","v":{"$error":"#N/A"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A135","v":"Solar yield"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"Auswahl!$C$298","v":"Solar yield DHW heating [kWh/d]"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"Auswahl!$S$298","v":"Solar coverage DHW heating [%]"}]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A175","v":"Hydraulical scetch"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A176","v":"Scheme is not available yet."}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A175","v":"Hydraulical scetch"}]
[]
[null,{"$f":"Auswahl!E353","v":1},{"$f":"Auswahl!F353","v":"Heat pump"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R353","v":10},{"$f":"Auswahl!S353","v":"Fill & drain valve"}]
[null,{"$f":"Auswahl!E354","v":"1-1"},{"$f":"Auswahl!F354","v":"Exhaust air module: LWM 250"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R354","v":11},{"$f":"Auswahl!S354","v":"Oil fired boiler / Gas fired boiler"}]
[null,{"$f":"Auswahl!E355","v":"1-2"},{"$f":"Auswahl!F355","v":"Cooling module: WPAC"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R355","v":12},{"$f":"Auswahl!S355","v":"Electric central heating"}]
[null,{"$f":"Auswahl!E356","v":2},{"$f":"Auswahl!F356","v":"Control unit: WPMW"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R356","v":13},{"$f":"Auswahl!S356","v":"Mixing valve"}]
[null,{"$f":"Auswahl!E357","v":"2-1"},{"$f":"Auswahl!F357","v":"Swimming pool module: MSMW"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R357","v":14},{"$f":"Auswahl!S357","v":"Mixing valve actuator"}]
[null,{"$f":"Auswahl!E358","v":"2-2"},{"$f":"Auswahl!F358","v":"Remote control: FE 7"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R358","v":15},{"$f":"Auswahl!S358","v":"Heating control unit"}]
[null,{"$f":"Auswahl!E359","v":"2-3"},{"$f":"Auswahl!F359","v":"Remote control cooling: FEK"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R359","v":16},{"$f":"Auswahl!S359","v":"Remote set value selector"}]
[null,{"$f":"Auswahl!E360","v":"2 a"},{"$f":"Auswahl!F360","v":"Temperature sensor: Outside temperature"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R360","v":17},{"$f":"Auswahl!S360","v":"Temperature sensor: Outside temperature"}]
[null,{"$f":"Auswahl!E361","v":"2 b"},{"$f":"Auswahl!F361","v":"Temperature sensor: Return temperature"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R361","v":18},{"$f":"Auswahl!S361","v":"Temperature sensor: Flow temperature"}]
[null,{"$f":"Auswahl!E362","v":"2 c"},{"$f":"Auswahl!F362","v":"Temperature sensor: Flow temperature, DHW \"off\""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R362","v":19},{"$f":"Auswahl!S362","v":"Air vent valve"}]
[null,{"$f":"Auswahl!E363","v":"2 d"},{"$f":"Auswahl!F363","v":"Temperature sensor: Flow temperature, DHW \"on\""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R363","v":20},{"$f":"Auswahl!S363","v":"Solid fuel boiler"}]
[null,{"$f":"Auswahl!E364","v":"2 e"},{"$f":"Auswahl!F364","v":"Temperature sensor: Mixer control"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R364","v":21},{"$f":"Auswahl!S364","v":"Motorised valve / Solenoid valve"}]
[null,{"$f":"Auswahl!E365","v":"2 f"},{"$f":"Auswahl!F365","v":"Temperature sensor: Heat source 2"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R365","v":22},{"$f":"Auswahl!S365","v":"Diverter valve"}]
[null,{"$f":"Auswahl!E366","v":"2 g"},{"$f":"Auswahl!F366","v":"Temperature sensor: Heat source "},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R366","v":23},{"$f":"Auswahl!S366","v":"Threaded immersion heater"}]
[null,{"$f":"Auswahl!E367","v":"2 h"},{"$f":"Auswahl!F367","v":"Temperature sensor: Swimming pool water heating"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R367","v":24},{"$f":"Auswahl!S367","v":"Heat exchanger"}]
[null,{"$f":"Auswahl!E368","v":"2 k"},{"$f":"Auswahl!F368","v":"Temperature sensor: solar panel"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R368","v":25},{"$f":"Auswahl!S368","v":"Combi cylinder"}]
[null,{"$f":"Auswahl!E369","v":"2 ko"},{"$f":"Auswahl!F369","v":"Temperature sensor: solar panel East"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R369","v":26},{"$f":"Auswahl!S369","v":"DHW cylinder"}]
[null,{"$f":"Auswahl!E370","v":"2 kw"},{"$f":"Auswahl!F370","v":"Temperature sensor: solar panel West"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R370","v":27},{"$f":"Auswahl!S370","v":"Central control thermostat"}]
[null,{"$f":"Auswahl!E371","v":"2 l"},{"$f":"Auswahl!F371","v":"Temperature sensor 1:  return flow temperature increase"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R371","v":28},{"$f":"Auswahl!S371","v":"Cold water - safety equipment assembly"}]
[null,{"$f":"Auswahl!E372","v":"2 m"},{"$f":"Auswahl!F372","v":"Temperature sensor 2:  return flow temperature increase"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R372","v":29},{"$f":"Auswahl!S372","v":"Controller: Swimming pool water"}]
[null,{"$f":"Auswahl!E373","v":"2 p"},{"$f":"Auswahl!F373","v":"Temperature sensor: solar buffer cylinder"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R373","v":30},{"$f":"Auswahl!S373","v":"Control thermostat"}]
[null,{"$f":"Auswahl!E374","v":"2 r"},{"$f":"Auswahl!F374","v":"Temperature sensor: additional solar buffer cylinder"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R374","v":31},{"$f":"Auswahl!S374","v":"Overflow valve"}]
[null,{"$f":"Auswahl!E375","v":"2 s"},{"$f":"Auswahl!F375","v":"Temperature sensor: solar system hot water/ cooling"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R375","v":32},{"$f":"Auswahl!S375","v":"cap valve"}]
[null,{"$f":"Auswahl!E376","v":3},{"$f":"Auswahl!F376","v":"Circulation pump: Heat pump - heat source"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R376","v":33},{"$f":"Auswahl!S376","v":"Line regulating valve"}]
[null,{"$f":"Auswahl!E377","v":"3 a"},{"$f":"Auswahl!F377","v":"Circulation pump: Heat pump - heating side"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R377","v":34},{"$f":"Auswahl!S377","v":"Temperature differential controller"}]
[null,{"$f":"Auswahl!E378","v":"3 b"},{"$f":"Auswahl!F378","v":"Circulation pump: DHW heating"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R378","v":35},{"$f":"Auswahl!S378","v":"Flow limiter"}]
[null,{"$f":"Auswahl!E379","v":"3 c"},{"$f":"Auswahl!F379","v":"Circulation pump: Heating circuit 1"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R379","v":36},{"$f":"Auswahl!S379","v":"High limit thermostat - underfloor heating system "}]
[null,{"$f":"Auswahl!E380","v":"3 d "},{"$f":"Auswahl!F380","v":"Circulation pump: Heating circuit 2"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R380","v":37},{"$f":"Auswahl!S380","v":"Zone valve"}]
[null,{"$f":"Auswahl!E381","v":"3 e"},{"$f":"Auswahl!F381","v":"Circulation pump: Swimming pool"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R381","v":38},{"$f":"Auswahl!S381","v":"Inflow tube"}]
[null,{"$f":"Auswahl!E382","v":"3 f"},{"$f":"Auswahl!F382","v":"Circulation pump: Solar DHE heating"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R382","v":39},{"$f":"Auswahl!S382","v":"Filter / strainer"}]
[null,{"$f":"Auswahl!E383","v":"3 f.1"},{"$f":"Auswahl!F383","v":"Circulation pump: Solar heating system"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R383","v":40},{"$f":"Auswahl!S383","v":"Fancoil "}]
[null,{"$f":"Auswahl!E384","v":"3 f.2"},{"$f":"Auswahl!F384","v":"Circulation pump: Solar Swimming pool"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R384","v":41},{"$f":"Auswahl!S384","v":"Instantaneous water heater DHE"}]
[null,{"$f":"Auswahl!E385","v":"3 fo"},{"$f":"Auswahl!F385","v":"Circulation pump: Solar panel East"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R385","v":42},{"$f":"Auswahl!S385","v":"Solar panel"}]
[null,{"$f":"Auswahl!E386","v":"3 fw"},{"$f":"Auswahl!F386","v":"Circulation pump: Solar panel West"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R386","v":43},{"$f":"Auswahl!S386","v":"Electrical heating flang"}]
[null,{"$f":"Auswahl!E387","v":"3 g"},{"$f":"Auswahl!F387","v":"Circulation pump: Solid fuel boiler"}]
[null,{"$f":"Auswahl!E388","v":"3 x"},{"$f":"Auswahl!F388","v":"Circulation pump: Cooling - hest source"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R388","v":"I"},{"$f":"Auswahl!S388","v":"Heat utilisation system"}]
[null,{"$f":"Auswahl!E389","v":"3 y"},{"$f":"Auswahl!F389","v":"Circulation pump: Heat pump - heat source"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R389","v":"II"},{"$f":"Auswahl!S389","v":"Heat source system "}]
[null,{"$f":"Auswahl!E390","v":4},{"$f":"Auswahl!F390","v":"Compact installation: WPKI"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R390","v":"III"},{"$f":"Auswahl!S390","v":"Solar panel"}]
[null,{"$f":"Auswahl!E391","v":5},{"$f":"Auswahl!F391","v":"Safety valve"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R391","v":"IV"},{"$f":"Auswahl!S391","v":"Cooling system"}]
[null,{"$f":"Auswahl!E392","v":6},{"$f":"Auswahl!F392","v":"Expansion vessel"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R392","v":"V"},{"$f":"Auswahl!S392","v":"Radiator heating system "}]
[null,{"$f":"Auswahl!E393","v":7},{"$f":"Auswahl!F393","v":"Buffer cylinder/ low loss header"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R393","v":"VI"},{"$f":"Auswahl!S393","v":"Underfloor heating system"}]
[null,{"$f":"Auswahl!E394","v":8},{"$f":"Auswahl!F394","v":"Anti-vibration mount"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R394","v":"VII"},{"$f":"Auswahl!S394","v":"DHW"}]
[null,{"$f":"Auswahl!E395","v":9},{"$f":"Auswahl!F395","v":"Non-return valve"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"Auswahl!R395","v":"VIII"},{"$f":"Auswahl!S395","v":"Swimming pool water "}]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A305","v":"Pipework installation"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A273","v":"Expansion vessel"}]
[]
[]
[]
[]
[null,{"$f":"Translation!A293","v":"System volume"}]
[null,{"$f":"Zwischenwerte!B390&\"  x  \"&Zwischenwerte!A390","v":"2  x  Rooftop SOL 27 Premium S"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B390&\"  x  \"&FIXED(VLOOKUP(Zwischenwerte!A390,Zwischenwerte!A392:C413,3,FALSE),2)&\" \"&Translation!A287","v":"2  x  1,50 Litres"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C390,1)&\" \"&Translation!A287","v":"3,0 Litres"}]
[null,{"$f":"FIXED(Zwischenwerte!D390/0.13,0)&\"  x  Kollektorverbindung\"","v":"1  x  Kollektorverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!D390/0.13,0)&\"  x  0,13 \"&Translation!A287","v":"1  x  0,13 Litres"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!D390,1)&\" \"&Translation!A287","v":"0,1 Litres"}]
[null,{"$f":"Zwischenwerte!G390&\"  x  \"&Zwischenwerte!E390","v":"1  x  SBB 300 Plus"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!G390&\"  x  \"&FIXED(Zwischenwerte!F390/Zwischenwerte!G390,2)&\" \"&Translation!A287","v":"1  x  10,10 Litres"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!F390,1)&\" \"&Translation!A287","v":"10,1 Litres"}]
[null,{"$f":"Zwischenwerte!J390&\"  x  \"&Zwischenwerte!H390","v":"---  x  SBP 700 E SOL"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!J390&\"  x  \"&FIXED(Zwischenwerte!I390/Zwischenwerte!J390,2)&\" \"&Translation!A287","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!I390,1)&\" \"&Translation!A287","v":"0,0 Litres"}]
[null,{"$f":"Zwischenwerte!M390&\"  x  \"&Zwischenwerte!K390","v":"---  x  WT 10"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!M390&\"  x  \"&FIXED(Zwischenwerte!L390/Zwischenwerte!M390,2)&\" \"&Translation!A287","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!L390,1)&\" \"&Translation!A287","v":"0,0 Litres"}]
[null,{"$f":"Translation!A279","v":"Flexible solar pipe"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!B433&\"  x  \"&FIXED(Zwischenwerte!B437,2)&\" l/m\"","v":"---  x  0,31 l/m"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!B435,1)&\" \"&Translation!$A$287","v":"0,0 Litres"}]
[null,{"$f":"Translation!A280","v":"Copper pipe 18 x 1.0"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!C433&\"  x  \"&FIXED(Zwischenwerte!C437,2)&\" l/m\"","v":"---  x  0,20 l/m"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C435,1)&\" \"&Translation!$A$287","v":"0,0 Litres"}]
[null,{"$f":"Translation!A281","v":"Copper pipe 22 x 1.0"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!D433&\"  x  \"&FIXED(Zwischenwerte!D437,2)&\" l/m\"","v":"---  x  0,31 l/m"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!D435,1)&\" \"&Translation!$A$287","v":"0,0 Litres"}]
[null,{"$f":"Translation!A282","v":"Copper pipe 28 x 1.5"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!E433&\"  x  \"&FIXED(Zwischenwerte!E437,2)&\" l/m\"","v":"---  x  0,49 l/m"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!E435,1)&\" \"&Translation!$A$287","v":"0,0 Litres"}]
[null,{"$f":"Translation!A283","v":"Copper pipe 35 x 1.5"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!F433&\"  x  \"&FIXED(Zwischenwerte!F437,2)&\" l/m\"","v":"---  x  0,80 l/m"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!F435,1)&\" \"&Translation!$A$287","v":"0,0 Litres"}]
[null,{"$f":"Translation!A284","v":"Other installations"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"1  x  \"&FIXED(Zwischenwerte!O390,2)&\" \"&Translation!A287","v":"1  x  0,00 Litres"},null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!O390,1)&\" \"&Translation!A287","v":"0,0 Litres"}]
[]
[null,{"$f":"Translation!A318","v":"Calculation"}]
[null,{"$f":"Translation!A293","v":"System volume"},null,null,null,null,null,null,null,null,null,null,"VA",null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C454,1)&\" \"&Translation!A287","v":"13,2 Litres"}]
[null,{"$f":"Translation!A294","v":"Liquid seal (min. 3 l)"},null,null,null,null,null,null,null,null,null,null,"VV = 0,005  x  VA",null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C455,1)&\" \"&Translation!A287","v":"3,0 Litres"}]
[null,{"$f":"Translation!A319","v":"Total volume"},null,null,null,null,null,null,null,null,null,null,"VG = VA + VV",null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C456,1)&\" \"&Translation!A287","v":"16,2 Litres"}]
[null,{"$f":"Translation!A320","v":"Heat transfer medium expansion"},null,null,null,null,null,null,null,null,null,null,"Ve = 0,0849  x  (VG - VKoll)",null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C457,1)&\" \"&Translation!A287","v":"1,1 Litres"}]
[null,{"$f":"Translation!A321","v":"Volume evaporation"},null,null,null,null,null,null,null,null,null,null,"VD = 1,0  x  VKoll",null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C458,1)&\" \"&Translation!A287","v":"3,1 Litres"}]
[null,{"$f":"Translation!A286","v":"Expansion volume"},null,null,null,null,null,null,null,null,null,null,"V0 = VV + Ve + VD",null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C459,1)&\" \"&Translation!A287","v":"7,3 Litres"}]
[null,{"$f":"Translation!A288","v":"Pressure factor"},null,null,null,null,null,null,null,null,null,null,"Df = 0,385"]
[null,{"$f":"Translation!A322","v":"Nominal volume, expansion vessel"},null,null,null,null,null,null,null,null,null,null,"VN = V0 / Df",null,null,null,null,null,null,{"$f":"FIXED(Zwischenwerte!C460,1)&\" \"&Translation!A287","v":"19,0 Litres"}]
[]
[null,{"$f":"Translation!A291","v":"Recommendation"}]
[null,{"$f":"Translation!A292","v":"Heat transfer medium"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!C478","v":"1 x 20 Litres H-30L"}]
[null,{"$f":"Translation!A273","v":"Expansion vessel"},null,null,null,null,null,null,null,null,null,null,{"$f":"Zwischenwerte!C473","v":"AG 25"}]
[null,{"$f":"Translation!A323","v":"Pre-charge pressure, expansion vessel"},null,null,null,null,null,null,null,null,null,null,"3 bar"]
[null,{"$f":"Translation!A296","v":"Applicable for up to 20 m height differential (collector - DEV), safety valve response pressure 6 bar"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A65","v":"Collector details"}]
[]
[]
[]
[]
[null,{"$f":"Translation!A338","v":"Specification"},null,null,null,null,null,null,null,null,"SOL 27 Premium",null,null,null,null,null,"SOL 27  basic",null,null,null,null,null,"SOL 23 premium"]
[null,{"$f":"Translation!A339","v":"Version"},null,null,null,null,null,null,null,null,{"$f":"Translation!A358","v":"Vertical"},null,null,{"$f":"Translation!A359","v":"Horizontal"},null,null,{"$f":"Translation!A358","v":"Vertical"},null,null,{"$f":"Translation!A359","v":"Horizontal"},null,null,{"$f":"Translation!A358","v":"Vertical"}]
[null,{"$f":"Translation!A83","v":"Shape of roof"},null,null,null,null,null,null,null,null,{"$f":"Translation!A67","v":"Rooftop"},null,null,{"$f":"Translation!A67","v":"Rooftop"},null,null,{"$f":"Translation!A67","v":"Rooftop"},null,null,{"$f":"Translation!A67","v":"Rooftop"},null,null,{"$f":"Translation!A68","v":"Roof integration"}]
[null,{"$f":"Translation!A340","v":"Overall area [m²]"},null,null,null,null,null,null,null,null,2.5499999999999998,null,null,2.5499999999999998,null,null,2.5299999999999998,null,null,2.5299999999999998,null,null,2.63]
[null,{"$f":"Translation!A341","v":"Aperture area [m²]"},null,null,null,null,null,null,null,null,2.39,null,null,2.39,null,null,2.39,null,null,2.39,null,null,2.04]
[null,{"$f":"Translation!A342","v":"Subsidides area [m²]"},null,null,null,null,null,null,null,null,2.5499999999999998,null,null,2.5499999999999998,null,null,2.5299999999999998,null,null,2.5299999999999998,null,null,2.33]
[null,{"$f":"Translation!A343","v":"Height [mm]"},null,null,null,null,null,null,null,null,2171,null,null,1171,null,null,2168,null,null,1168,null,null,2340]
[null,{"$f":"Translation!A344","v":"Width [mm]"},null,null,null,null,null,null,null,null,1171,null,null,2171,null,null,1168,null,null,2168,null,null,1155]
[null,{"$f":"Translation!A345","v":"Depth [mm]"},null,null,null,null,null,null,null,null,96,null,null,96,null,null,93,null,null,93,null,null,102]
[null,{"$f":"Translation!A346","v":"Weight, dry [kg]"},null,null,null,null,null,null,null,null,40,null,null,40.5,null,null,38.5,null,null,39.200000000000003,null,null,54]
[null,{"$f":"Translation!A347","v":"Capacity [l]"},null,null,null,null,null,null,null,null,1.5,null,null,1.83,null,null,1.3,null,null,1.7,null,null,1.2]
[null,{"$f":"Translation!A348","v":"Permissible operating pressure [bar]"},null,null,null,null,null,null,null,null,6,null,null,6,null,null,6,null,null,6,null,null,6]
[null,{"$f":"Translation!A349","v":"Conversion factor Eta-0"},null,null,null,null,null,null,null,null,0.82299999999999995,null,null,0.82499999999999996,null,null,0.79,null,null,0.78,null,null,"> 0,82"]
[null,{"$f":"Translation!A350","v":"Heat loss coefficient a0"},null,null,null,null,null,null,null,null,3.46,null,null,3.46,null,null,3.42,null,null,3.42,null,null,3.46]
[null,{"$f":"Translation!A351","v":"Heat loss coefficient a1"},null,null,null,null,null,null,null,null,1.5299999999999999E-2,null,null,1.5299999999999999E-2,null,null,1.4200000000000001E-2,null,null,1.4200000000000001E-2,null,null,1.5299999999999999E-2]
[null,{"$f":"Translation!A352","v":"Connection"},null,null,null,null,null,null,null,null,"22 mm",null,null,"22 mm",null,null,{"$f":"Translation!A354","v":"G ¾\" male"},null,null,{"$f":"Translation!A354","v":"G ¾\" male"},null,null,"22 mm"]
[]
[null,{"$f":"Translation!A353","v":"Application range"},null,null,null,null,null,null,null,null,"SOL 27 Premium",null,null,null,null,null,"SOL 27  basic",null,null,null,null,null,"SOL 23 premium"]
[null,{"$f":"Translation!$A$89","v":"Quick assembly fixings"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"P",null,null,null,null,null,"O"]
[null,{"$f":"Translation!A84","v":"Tiled roof"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"P",null,null,null,null,null,"P"]
[null,{"$f":"Translation!A85","v":"Corrugated roof"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"P",null,null,null,null,null,"O"]
[null,{"$f":"Translation!A355","v":"Flat roof"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"P",null,null,null,null,null,"O"]
[null,{"$f":"Translation!A356","v":"Wall mounting"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"P",null,null,null,null,null,"O"]
[null,{"$f":"Translation!A357","v":"Roof integration"},null,null,null,null,null,null,null,null,"O",null,null,null,null,null,"O",null,null,null,null,null,"P"]
[null,{"$f":"Translation!A88","v":"Support stands 15°- 30°"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"P",null,null,null,null,null,"O"]
[]
[null,{"$f":"Translation!A78","v":"Arrangement"},null,null,null,null,null,null,null,null,"SOL 27 Premium",null,null,null,null,null,"SOL 27  basic",null,null,null,null,null,"SOL 23 premium"]
[null,{"$f":"Translation!A79","v":"On end next to each other"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"P",null,null,null,null,null,"P"]
[null,{"$f":"Translation!A82","v":"On end above each other"},null,null,null,null,null,null,null,null,"O",null,null,null,null,null,"O",null,null,null,null,null,"P"]
[null,{"$f":"Translation!A81","v":"Across next to each other"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"P",null,null,null,null,null,"O"]
[null,{"$f":"Translation!A80","v":"Across above each other"},null,null,null,null,null,null,null,null,"P",null,null,null,null,null,"O",null,null,null,null,null,"O"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A306","v":"Installation information"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Deutsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Englisch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tschechisch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Niederlande"]
[]
[]
[]
[]
[">>","Die Installation der Kollektoren hat für jedes Befestigungssystem stets gemäß Montageanweisung zu erfolgen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Die Installation der Kollektoren hat für jedes Befestigungssystem stets gemäß Montageanweisung zu erfolgen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","The installation of the collectors onto the different roof types always is to be made in compliance with the manual ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Kolektory je nutno instalovat pro každý upevňovací systém vždy podle pokynů k montáži.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","De installatie van de collectoren moet bij elk bevestigingssysteem worden uitgevoerd conform de montagemogelijkheid."]
[">>","Für die Verbindung der einzelnen Kollektoren dürfen ausschließlich beiliegende Kompensatoren,",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Für die Verbindung der einzelnen Kollektoren dürfen ausschließlich beiliegende Kompensatoren,",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","The connection between the collectores is only allowed to be done with the destined compensator elements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Pro spojování jednotlivých kolektorů se smí používat výhradně přiložené kompenzátory se začleněnými odvzdušňovacími šrouby.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Voor de aansluiting van de afzonderlijk collectoren mogen alleen de meegeleverde"]
[null,"oder die integreierten Anschlüsse eingesetzt werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"oder die integreierten Anschlüsse eingesetzt werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"or with the prepared connections of the panels  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Automatické odvzdušňovače k odvzdušňování soustavy nejsou přípustné",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"compensatoren of de geïntegreerde aansluitingen worden gebruikt. "]
[">>","Automatische Entlüfter zur Entlüftung der Anlage sind nicht zulässig (Ausnahme: absperrbare Entlüfter nach DIN 12977).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Automatische Entlüfter zur Entlüftung der Anlage sind nicht zulässig (Ausnahme: absperrbare Entlüfter nach DIN 12977).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Automatical bleeding devices are generally not allowed to be installed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(výjimka: odvzdušňovače s možností blokování podle normy DIN 12977).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Automatische ontluchters voor het ontluchten van de installatie zijn niet toegestaan (uitzondering: afsluitbare ontluchters conform DIN 12977). "]
[">>","Zur Vermeidung überhöhter Temperaturen und Druckverluste dürfen nicht mehr als 5 Kollektoren zu einer ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Zur Vermeidung überhöhter Temperaturen und Druckverluste dürfen nicht mehr als 5 Kollektoren zu einer ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(Exception: closeable bleeding devices refer to DIN EN 12977)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Aby se zamezilo nadměrným teplotám a ztrátám tlaku, nesmí se sdružit více než 5 kolektorů do jedné hydraulické skupiny.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Ter voorkoming van te hoge temperaturen en drukverliezen mogen niet meer dan 5 collectoren"]
[null,"hydraulischen Gruppe zusammengefasst werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"hydraulischen Gruppe zusammengefasst werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","To avoid high temperatures and pressure losses you should not connect more then 5 panels in series ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","U soustav s více než 5 kolektory je nutné paralelní zapojení několika skupin.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"worden ondergebracht in één hydraulische groep. "]
[">>","Bei Anlagen mit mehr als 5 Kollektoren ist eine Parallelschaltung mehrerer Gruppen erforderlich.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bei Anlagen mit mehr als 5 Kollektoren ist eine Parallelschaltung mehrerer Gruppen erforderlich.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","In case of solar plants with more then 5 collectors it is recommended to divide into several parallel groups ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>"," Veškeré práce při instalaci včetně hydraulického propojení smí provádět výhradně oprávněný odborný personál.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bij installaties met meer dan 5 collectoren moeten meerdere groepen parallel worden geschakeld. "]
[">>","Alle Installationsarbeiten inklusive Verrohrung sind ausschließlich von zugelassenem Fachpersonal durchzuführen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Alle Installationsarbeiten inklusive Verrohrung sind ausschließlich von zugelassenem Fachpersonal durchzuführen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","All installations and mountings, including the piping, generally has to be performed by accredited technical staff   ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Pro výstupní a vratná potrubí se musejí použít měděné trubky podle normy DIN EN 1057 nebo alternativně",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Alle installatiewerkzaamheden inclusief het leggen van leidingen, moeten door bevoegde installatiemonteurs worden uitgevoerd. "]
[">>","Vor-und Rücklaufleitungen sind mit Kupferrohr nach DIN EN 1057 oder alternativ mit vorisolierten Edelstahlwellrohr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Vor-und Rücklaufleitungen sind mit Kupferrohr nach DIN EN 1057 oder alternativ mit vorisolierten Edelstahlwellrohr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Flow and return preferably should be done in cupper refer to DIN EN 1057 or alternatively in ready insulated ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"předem izolované vlnité trubky z ušlechtilé oceli z výrobního programu STIEBEL ELTRON. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Aanvoer- en retourleidingen moeten worden uitgevoerd met koperen buis conform DIN EN 1057 of met vooraf geïsoleerde"]
[null,"aus dem STIEBEL ELTRON Produktprogramm auszuführen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"aus dem STIEBEL ELTRON Produktprogramm auszuführen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"corrugated stainless steel tubes of STIEBEL ELTRON product range",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Měděné trubky je nutno pájet natvrdo se zřetelem k pracovnímu listu DVGW GW 2, pájka podle normy DIN EN 1044",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"gegolfde geribbelde buizen van roestvrij staal roestvaststaal uit het productassortiment van STIEBEL ELTRON. "]
[">>","Kupferrohr ist  unter Beachtung des DVGW-Arbeitsblattes GW 2 hartzulöten, Lote gemäß DIN EN 1044 CP und CP 203 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Kupferrohr ist  unter Beachtung des DVGW-Arbeitsblattes GW 2 hartzulöten, Lote gemäß DIN EN 1044 CP und CP 203 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Cupper tubes have to be hard soldered according to the common technical regulations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CP a CP 203 bez tavidla. S použitím tavidla F-SH-1 podle normy DIN 8511 se pájí fitinky z červeného kovu a mosazi.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Koperenbuis moet met inachtneming van DVGW-werkblad GW 2 met hardsoldeer worden gesoldeerd, soldeermiddelen conform EN 1044 CP en CP 203"]
[null,"ohne Flussmittel. Rotguss- und Messingfittings sind mit Flussmittel F-SH-I nach DIN 8511 zu löten.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ohne Flussmittel. Rotguss- und Messingfittings sind mit Flussmittel F-SH-I nach DIN 8511 zu löten.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","In case of utilisation of the ready insulated corrugated stainless steel hose please observe the maximal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Při použití předem izolované vlnité trubky z ušlechtilé oceli STIEBEL ELTRON je nutno dodržovat maximálně přípustnou",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"zonder vloeimiddel. Roodkoperen messingfittingen moeten met vloeimiddel F-SH-1 volgens DIN 8511 worden gesoldeerd. "]
[">>","Bei Einsatz des vorisolierten STIEBEL ELTRON Edelstahlwellrohres ist die maximal zulässige Rohrlänge zwischen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bei Einsatz des vorisolierten STIEBEL ELTRON Edelstahlwellrohres ist die maximal zulässige Rohrlänge zwischen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"permitted distance between storages and collector field",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"délku trubky mezi zásobníkem teplé vody a kolektorovým polem.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bij toepassing van vooraf geïsoleerde geribbelde buizen van  roestvasstaal uit het productassortiment van STIEBEL "]
[null,"Speicher und Kollektorfeld zu beachten.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Speicher und Kollektorfeld zu beachten.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","The insulation of the piping should comply to the national regulations for energy savings",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Na podkladě nařízení o úspoře energie (tepelná vodivost λ = 0,035 W/mK) je třeba všechny části potrubí tepelně izolovat. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELTRON moet rekening worden gehouden met de maximaal toelaatbare leidinglengte tussen boiler en collectorveld."]
[">>","Alle Rohrleitungen sind nach Energieeinsparverordnung zu dämmen (Wärmeleitfähigkeit λ = 0,035 W/(mK)).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Alle Rohrleitungen sind nach Energieeinsparverordnung zu dämmen (Wärmeleitfähigkeit λ = 0,035 W/(mK)).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(Recommendation: Thermal conductivity λ=0,035 W/mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Veškeré součásti soustavy musejí být odolné proti působení glykolu a provedeny s odolností proti teplotě až 180 °C.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Alle buizen moeten conform richtlijnen voor energiebesparing worden geïsoleerd (warmtegeleidend vermogen λ = 0,035 W/(mK))."]
[">>","Sämtliche Anlagenkomponenten müssen glykolbeständig und bis 180°C temperaturbeständig ausgeführt werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Sämtliche Anlagenkomponenten müssen glykolbeständig und bis 180°C temperaturbeständig ausgeführt werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","All the components have to be resistant against glycol and glycol mixes and should be thermal resitant up to 180 °C ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Mezi kolektorovým polem a pojistným ventilem nesmějí být instalované žádné uzavírací orgány.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Alle onderdelen van de installatie moeten bestand zijn tegen glycol en tegen temperaturen tot 180 °C. "]
[">>","Zwischen Kollektorfeld und Sicherheitsventil dürfen keine Absperrorgane vorgesehen werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Zwischen Kollektorfeld und Sicherheitsventil dürfen keine Absperrorgane vorgesehen werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","It is not allowed to install any closing valves between pressure relieve valve and collector field",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Otevírací přetlak pojistného ventilu, instalovaného v solární kompaktní instalační skupině (SOKI), je 6 bar.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Tussen de collectoren en het veiligheidsventiel mogen geen afsluiters worden gemonteerd. "]
[">>","Der Ansprechdruck des in der Solar-Kompaktinstallationsgruppe (SOKI) enthaltenem Sicherheitsventils beträgt 6 bar. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Der Ansprechdruck des in der Solar-Kompaktinstallationsgruppe (SOKI) enthaltenem Sicherheitsventils beträgt 6 bar. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","The popping pressure of the pressure relieve valve should be 6 bar",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Při použití cizího produktu je nutno zkontrolovat správný otevírací přetlak pojistného ventilu, ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","De aanspreekdruk van de in de compacte zonne-installatie (SOKI) geïntegreerde veiligheidsklep is 6 bar.  "]
[null,"Bei Einsatz eines Fremdproduktes ist auf den korrekten Ansprechdruck des SV sowie das Vorhandensein eines",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bei Einsatz eines Fremdproduktes ist auf den korrekten Ansprechdruck des SV sowie das Vorhandensein eines",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Please proof the existence of a non-return valve to avoid heat losses because of thermal roll out  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a dále přítomnost zpětného ventilu k zamezení nepřípustného výdeje tepla.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bij toepassing van een product van derden moet op de juiste aanspreekdruk van het veiligheidsventiel en de "]
[null,"Rückschlagventils zu Vermeidung der Wärmeausspeicherung zu prüfen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rückschlagventils zu Vermeidung der Wärmeausspeicherung zu prüfen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","The compact installation pump groups are serially fittet with solar pumps, the application should be proofed ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Kompaktní instalační skupiny SOKI Plus jsou sériově vybaveny oběhovým čerpadlem ST 15/6 ECO (WILO).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"aanwezigheid van een terugslagklep worden gelet om warmteverlies  door thermosifon werking te voorkomen. "]
[">>","Die Kompaktinstallationsgruppen sind serienmäßig mit gängigen Solar - Umwälzpumpen ausgestattet.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Die Kompaktinstallationsgruppen sind serienmäßig mit gängigen Solar - Umwälzpumpen ausgestattet.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"according to there capacity",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," To dovoluje provoz maximálně 16 kolektorů (4 x 4). Součástí kompaktní instalační skupiny SOKI SBK-M",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","De compacte installaties zijn standaard uitgerust met gangbare zone-circulatiepompen. "]
[null,"Der Einsatz muss entsprechend den tatsächlichen Installationen hinsichtlich der Leistungsgrenzen geprüft werden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Der Einsatz muss entsprechend den tatsächlichen Installationen hinsichtlich der Leistungsgrenzen geprüft werden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","The volume of the delivered expansion vessel has to be checked with the factual installation ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," je oběhové čerpadlo UP 25-40, které je možno použít až do max. 8 kolektorů.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Het gebruik moet overeenkomstig de vermogensgrenzen van de werkelijke installatie worden gecontroleerd."]
[">>","Die Größe des gelieferten Ausdehnungsgefäßes ist entsprechend der tatsächlichen Bauausführung gemäß ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Die Größe des gelieferten Ausdehnungsgefäßes ist entsprechend der tatsächlichen Bauausführung gemäß ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"in accordance to DIN EN 12828. In cases of differences it should be adapted.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Podle normy DIN EN 12828 je nutno přezkoušet a případně přizpůsobit velikost dodané tlakové expanzní",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","De grootte van het meegeleverde expansievat moet in de daadwerkelijke installatie worden"]
[null,"DIN EN 12828 zu prüfen und gegebenenfalls anzupassen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIN EN 12828 zu prüfen und gegebenenfalls anzupassen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","In use of heat exchangers for thermal supply of swimming pools, please observe there technical limitations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nádoby v souladu se skutečným provedením soustavy.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"gecontroleerd conform DIN EN 12828; zo nodig moet een groter expansievat worden gemonteerd."]
[">>","Bei Einsatz eines STIEBEL ELTRON Plattenwärmetauschers in einer Solaranlage zur Schwimmbad-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bei Einsatz eines STIEBEL ELTRON Plattenwärmetauschers in einer Solaranlage zur Schwimmbad-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"in view of chlorination of the pool water",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Při použití deskového tepelného výměníku STIEBEL ELTRON WT 10 / 20 / 30 / 40 v solární soustavě  k ohřevu vody",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bij toepassing van een platenwarmtewisselaar van STIEBEL ELTRON in een zonne-installatie voor het verwarmen "]
[null,"wassererwärmung sind die Einsatzgrenzen hinsichtlich der zulässigen Chlorierung zu berücksichtigen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"wassererwärmung sind die Einsatzgrenzen hinsichtlich der zulässigen Chlorierung zu berücksichtigen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","If a lightning protection system is excisting the collector and mounting devices should be included into the concept ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pro bazén je třeba mít na zřeteli meze použití pokud se týká přípustného chlórování.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," van zwembadwater moeten de werkingsgrenzen op het vlak van toelaatbare chlorering in acht worden genomen. "]
[">>","Bei eventuell vorhandenen Blitzschutzanlagen sind Kollektorgehäuse, Montagerahmen sowie Rohrleitungen ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bei eventuell vorhandenen Blitzschutzanlagen sind Kollektorgehäuse, Montagerahmen sowie Rohrleitungen ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","According to the expected snow load please observe the details for the minimal inclination of the collectores",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Pokud případně existují zařízení na ochranu proti úderu blesku, je třeba do koncepce této ochrany",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bij een eventueel aanwezige bliksembeveiliging moeten de collectorbehuizing, montageframes en leidingen"]
[null,"in das Blitzschutzkonzept einzubeziehen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"in das Blitzschutzkonzept einzubeziehen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"into the manual ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"zahrnout i skříně kolektorů, montážní rámy a potrubí.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"worden opgenomen in de beveiliging. "]
[">>","Je nach Schneelastzone ist der in der Montageanweisung angegebene Mindestaufstellwinkel einzuhalten.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Je nach Schneelastzone ist der in der Montageanweisung angegebene Mindestaufstellwinkel einzuhalten.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Please always observe the requirements of DIN EN 12977 when installating a thermal solar plant   ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Podle zóny zatížení sněhem je třeba dodržovat v montážních instrukcích uvedený minimální úhel instalace kolektorů.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Afhankelijk van de sneeuwbelastingszone moet de, in de montagehandleiding aangegeven minimale, opstelhoek in acht worden genomen. "]
[">>","Bei der Installation einer Solaranlage sind stets die Anforderungen nach DIN 12977 'Thermische Solaranlagen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bei der Installation einer Solaranlage sind stets die Anforderungen nach DIN 12977 'Thermische Solaranlagen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","A yearly technical inspect of the whole system is recommended",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Při instalací solární soustavy se musejí stále dodržovat požadavky podle normy DIN 12977",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bij de installatie van een zonne-installatie moeten steeds de eisen van DIN 12977 'Thermische zonne-"]
[null,"und ihre Bauteile' einzuhalten.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"und ihre Bauteile' einzuhalten.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","To avoid critical operating conditions the controler and the pump never should be cutt off ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"„Tepelné solární soustavy a jejich konstrukční díly“.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"installaties en de betrokken componenten' in acht worden genomen. "]
[">>","Von Fachpersonal ist jährlich eine Überprüfung der Solar-Anlage auf einwandfreie Funktion der Anlage einschließlich",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Von Fachpersonal ist jährlich eine Überprüfung der Solar-Anlage auf einwandfreie Funktion der Anlage einschließlich",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","In systems for solar supply of the hotwater production please make sure that it is impossible to scald. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Jednou ročně musí přezkoušet odborný personál dokonalou funkci solární soustavy, včetně regulátoru,",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Jaarlijks dient door deskundig personeel een controle van de zonne-installatie op het probleemloos"]
[null,"Regelung, Sicherheitseinrichtungen und Speicher durchzuführen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regelung, Sicherheitseinrichtungen und Speicher durchzuführen.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A central mixing valve is recommended. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bezpečnostních zařízení a zásobníku teplé vody.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"functioneren van de regeling, veiligheidsvoorzieningen en boiler te worden uitgevoerd."]
[">>","Um eine Überhitzung der Anlage auszuschließen, dürfen die Regelung und die Pumpe nicht ausgeschaltet werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Um eine Überhitzung der Anlage auszuschließen, dürfen die Regelung und die Pumpe nicht ausgeschaltet werden.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Aby se vyloučilo přehřátí soustavy, nesmí se vypínat regulátor a čerpadlo.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","De regeling en de pomp mogen niet worden uitgeschakeld, om oververhitting van de installatie te voorkomen. "]
[">>","Bei Anlagen zur solaren Warmwasserbereitung sollte ein wirksamer Verbrühschutz in der Warmwasserleitung vorgesehen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bei Anlagen zur solaren Warmwasserbereitung sollte ein wirksamer Verbrühschutz in der Warmwasserleitung vorgesehen",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","V potrubí teplé vody je vhodné instalovat účinnou ochranu proti opaření (např. centrální termostatickou armaturu).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">>","Bij installaties met warmwaterbereiding moet een werkende temperatuurbeveiliging  worden"]
[null,"werden (z.B. Zentral-Thermostatarmatur)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"werden (z.B. Zentral-Thermostatarmatur)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," gemonteerd in de warmwaterleiding (bijv. een centrale thermostaatkraan)."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translation!A329","v":"Legal note"}]
[]
[]
[]
[]
[null,{"$f":"Translation!A330","v":"Stiebel Eltron shall not provide any guarantees that the information, values and data provided, or values, information and recommendations determined with the aid or on the basis of such information, values and data, are complete, accurate, correct or current in every respect.\nStiebel Eltron shall reserve the right to make changes to the data, values and information provided at any time and without prior notification.\nErrors excepted. Subject to changes.\nNone of the information, values and data provided or the values, information and recommendations determined with the aid or on the basis of such information, values and data constitutes any basis for a financial decision or for any other purpose, but rather is merely initial non-binding information as an initial guide.\nUnder no circumstances should the following design tool be considered a substitute for consultation with Stiebel Eltron or another authorised expert engineer.\nPlease contact Stiebel Eltron or another authorised expert engineer in relation to specific project design.\nStiebel Eltron shall accept no liability for losses of any kind that may arise from the use of information, values and data provided, or values, information and recommendations determined with the aid or on the basis of such information, values and data. This exclusion of liability shall not apply if the loss is due to intent or gross negligence on the part of Stiebel Eltron or in the event of a fatality, physical injury or damage to health.\n"}]